
**** 08/25/22 12:08:40 ******* PSpice 17.4.0 (Nov 2018) ******* ID# 0 ********

 ** Profile: "Startup-trans"  [ C:\work\LM2735\SNVM297\LM2735Y_PSPICE_TRANS\lm2735y_trans-pspicefiles\startup\trans.sim ] 


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "trans.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
.LIB "../../../LM2735Y_trans.lib" 
* From [PSPICE NETLIST] section of C:\cds_spb_home\cdssetup\OrCAD_PSpiceTIPSpice_Install\17.4.0\PSpice.ini file:
.lib "nom_pspti.lib" 
.lib "nom.lib" 

*Analysis directives: 
.TRAN  0 5m 0 15n SKIPBP 
.OPTIONS ADVCONV
.OPTIONS FILEMODELSEARCH
.OPTIONS ITL1= 1000
.OPTIONS ITL2= 400
.OPTIONS ITL4= 400
.PROBE64 V(alias(*)) I(alias(*)) 
.INC "..\Startup.net" 



**** INCLUDING Startup.net ****
* source LM2735Y_TRANS
X_U1         VIN N168163383 SW N16819839 0 LM2735Y_TRANS
R_R3         VIN N168163383  10k TC=0,0 
D_D1         SW VOUT myD30880 
R_R1         0 N16819839  10k TC=0,0 
R_R2         N16819839 VOUT  69.8k TC=0,0 
C_C3         VOUT N16819839  330p  TC=0,0 
R_Rs         N168305351 VIN  10m TC=0,0 
V_VIN         N168305351 0  
+PULSE 0 5 40u 40u 40u 1 3
X_C2         VOUT 0 CESR PARAMS: C=10u ESR=4.6m
X_L1         VIN SW LDCR PARAMS:  L=33u  DCR=80m IC=0
X_C1         VIN 0 CESR PARAMS: C=20u ESR=2.3m
I_Iload         VOUT 0 DC 0Adc AC 0Aac
+PULSE 0 0.03 700u 10u 10u 750u 1500u

**** RESUMING trans.cir ****
.END

WARNING(ORPSIM-15256): <X_L1.IC> not a subcircuit param

**** 08/25/22 12:08:40 ******* PSpice 17.4.0 (Nov 2018) ******* ID# 0 ********

 ** Profile: "Startup-trans"  [ C:\work\LM2735\SNVM297\LM2735Y_PSPICE_TRANS\lm2735y_trans-pspicefiles\startup\trans.sim ] 


 ****     Diode MODEL PARAMETERS


******************************************************************************




               myD30880        X_U1.DCLAMP     
          IS    9.000000E-06   10.000000E-15 
           N    1.442                        
          BV  200                            
         IBV    1.000000E-06                 
          RS     .06                         
         CJO  470.000000E-12                 
           M     .8                          
          EG     .69                         
         XTI    2                            


               X_U1.XDRIVER.DCGD 
          IS   10.000000E-15 
         CJO   59.000000E-12 
          VJ     .6          
           M     .68         


               X_U1.XDRIVER.DSUB 
          IS   10.400000E-09 
           N    1.5          
          BV   25            
          RS     .1          
          TT   86.000000E-09 
         CJO  217.000000E-12 
          VJ     .8          
           M     .42         


               X_U1.XDRIVER.DLIM 
          IS  100.000000E-06 


**** 08/25/22 12:08:40 ******* PSpice 17.4.0 (Nov 2018) ******* ID# 0 ********

 ** Profile: "Startup-trans"  [ C:\work\LM2735\SNVM297\LM2735Y_PSPICE_TRANS\lm2735y_trans-pspicefiles\startup\trans.sim ] 


 ****     MOSFET MODEL PARAMETERS


******************************************************************************




               X_U1.XDRIVER.DMOS 
               NMOS            
       LEVEL    3            
           L  100.000000E-06 
           W  100.000000E-06 
         VTO    3.1          
          KP   10.69         
       GAMMA    0            
         PHI     .6          
      LAMBDA    0            
          IS   10.000000E-15 
          JS    0            
          PB     .8          
        PBSW     .8          
          CJ    0            
        CJSW    0            
        CGSO    0            
        CGDO    0            
        CGBO    0            
         TOX  100.000000E-09 
          XJ    0            
       UCRIT   10.000000E+03 
        VMAX   52.100000E+03 
       THETA     .0581       
         ETA    2.000000E-03 
      DIOMOD    1            
         VFB    0            
        LETA    0            
        WETA    0            
          U0    0            
        TEMP    0            
         VDD    5            
       XPART    0            


**** 08/25/22 12:08:40 ******* PSpice 17.4.0 (Nov 2018) ******* ID# 0 ********

 ** Profile: "Startup-trans"  [ C:\work\LM2735\SNVM297\LM2735Y_PSPICE_TRANS\lm2735y_trans-pspicefiles\startup\trans.sim ] 


 ****     Voltage Controlled Switch MODEL PARAMETERS


******************************************************************************




               X_U1._S1_MOD    X_U1._S2_MOD    
         RON    1               1            
        ROFF    1.000000E+06    1.000000E+06 
          VT    1.1             2.1          
          VH     .7              .2          
          TD    0               0            


               X_U1.XSSFA.SMOOTH 
         RON    1.000000E-03 
        ROFF    1.000000E+09 
         VON     .75         
        VOFF     .25         


               X_U1.XAMP.SMOOTH 
         RON    1.000000E-03 
        ROFF  500.000000E+06 
         VON     .75         
        VOFF     .25         


               X_U1.XMEASS.SMOOTH 
         RON    1            
        ROFF    1.000000E+06 
         VON     .75         
        VOFF     .25         


               X_U1.XOSC.SMOOTH 
         RON    1            
        ROFF    1.000000E+09 
         VON     .75         
        VOFF     .25         


               X_U1.XSHOTAMP.SMOOTH 
         RON    1            
        ROFF    1.000000E+09 
         VON     .75         
        VOFF     .25         


WARNING(ORPSIM-16534): Using high values of ITL4 for Speed Level > 0 may increase total simulation job time.


          JOB CONCLUDED

**** 08/25/22 12:08:40 ******* PSpice 17.4.0 (Nov 2018) ******* ID# 0 ********

 ** Profile: "Startup-trans"  [ C:\work\LM2735\SNVM297\LM2735Y_PSPICE_TRANS\lm2735y_trans-pspicefiles\startup\trans.sim ] 


 ****     JOB STATISTICS SUMMARY


******************************************************************************



  License check-out time            =      811.61
  Total job time (using Solver 1)   =       92.91
