{"text_format":"1","workbook":"xlsx","n_sheets":12,"sheets":["Instructions","Design Converter","BOM & Schematic","Fsw & Ripple","Losses","EVM","Design EMI Filter","Variable Mgmt","Standard Value Calculator","Efficiency","Schematic Mgmt","Efficiency Plots"],"not_rendered":{"charts":6,"images":26,"macros":1,"external_links":0,"defined_names":205,"comments":4,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Instructions","index":0,"n_rows":74,"n_cols":3,"rows_kept":74,"cut":false,"hidden":true,"merged":[[0,0,0,16],[7,1,9,15],[16,2,17,15],[11,1,14,15],[18,2,19,15],[65,1,66,15],[69,1,70,15],[73,1,74,15],[77,1,78,15],[20,2,21,15],[50,1,52,15],[54,1,55,15],[56,1,57,15],[60,1,62,15],[24,1,26,15],[38,1,39,15],[41,1,43,15],[46,1,47,15],[28,1,28,15],[29,1,31,15],[33,1,35,15]]}
["                         LM5164 Low IQ DC/DC Converter Design Tool  "]
[]
[]
[null,"Design Regulator tab"]
[null,"Start with Step 1, and then work down towards the bottom of the worksheet."]
[]
[null,"Step 1. Operating Specifications"]
[null,"First, enter the values in the yellow shaded cells to define the power supply parameters.  If a particular specification is not known, enter an estimate. It can be changed later, if necessary, to optimize component values.  Cells  with a red mark in the upper right corner have a comment to provide additional information.  Hold the cursor over the cell to read the comment.  A red font indicates an erroneous entry and requires an adjustment to the entry.  Consult the entry's comments for the entry specific requirements."]
[]
[]
[]
[null,"Second, select a desired mode of operation. PFM mode requires the fewest external components and the lowest inductance.  As a result, it can provide the smallest solution size. At light loads, a PFM converter has a relatively longer sleep time interval and thus operates at lower input quiescent current levels.  COT mode offers nearly constant switching frequency, relatively higher conversion efficiencies at medium to heavy loads, and enables the lowest output voltage ripple.  Options COT1, COT2, and COT3 enable you to select a ripple generation method (a requirement for the stable operation in COT mode):"]
[]
[]
[]
[]
[null,"-COT1: ","Type 1 ripple generation method requires a single resistor in series with the output capacitor.  It is the simplest, the most compact, and the most economical method that works with fixed and adjustable device options, however, the output voltage ripple is the highest."]
[]
[null,"-COT2: ","Type 2 ripple generation method requires a feedforward capacitor in addition to the series resistor.  The feedforward capacitor reduces the required minimum value of the series resistor and ultimately the output voltage ripple by the VOUT / 1.223V factor.  It only works with an adjustable device option (i.e. external feedback resistor network)."]
[]
[null,"-COT3:","Type 3 ripple generation method three external components to generate and inject required voltage ripple into the FB node.  In return, it provides the lowest output voltage ripple. It also only works with an adjustable device option (i.e. external feedback resistor network)."]
[]
[]
[null,"Step 2. Filter Inductor"]
[null,"First, select an inductor current limit level.  In PFM Mode, 1.25A, 0.75A, 0.5A, and 1.25A - MOD options are available.  For the 500mA max load, select either 1.25A or 1.25A - MOD option.  The 1.25A - MOD option enables higher efficiency at the expense of slightly worse transient operation.  For the 300mA and 200mA max loads, select 0.75A and 0.5A options respectively. In COT Mode, 0.75A and 0.5A options are available.   For the 500mA and 300mA max loads, select 0.75A and 0.5A options respectively."]
[]
[]
[]
[null,"Second, select the filter inductance value based on the suggested value. Enter the inductor RDC for accurate efficiency estimates."]
[null,"In PFM mode, selected inductance defines the switching frequency.  You may select lower or higher inductance to increase or decrease the switching frequency.  Watch the minimum output capacitance.  At very low switching frequencies, the required minimum capacitance may become excessive."]
[]
[]
[]
[null,"In COT mode, the suggested inductance is  derived based on the target inductor (peak-to-peak) ripple current of 40% of the DC full load output current at nominal input voltage. It may be acceptable to use higher ripple current with the proviso that peak inductor current remains below the ILIM setting.  Pk-to-Pk Ripple Current value will turn red if this is violated.  If this happens, increase the selected inductance or decrease the Input Voltage (max) or both."]
[]
[]
[]
[null,"Step 3. Output Capacitors and Ripple Generation"]
[null,"First, select the output capacitance based on the minimum recommended value.  Make sure that the nominal capacitance is appropriately derated for applied voltage, especially with ceramics.  For PFM and COT3 modes, ensure that the capacitor ESR does not exceed the maximum allowable value.  "]
[]
[]
[null,"Second, for COT modes, select the values for the ripple generation components based on the minimum recommended values.  Ensure that the output voltage ripple meets any of your minimum ripple requirements by reviewing the VOUT Ripple vs. IOUT plot in the fSW&Ripple tab.  For accurate output voltage ripple estimates in COT3 mode, ensure that the Output Capacitor ESR is set to the levels of a typical ceramic capacitor ESR (e.g. 10 mW)."]
[]
[]
[]
[null,"Step 4. Input Capacitors"]
[null,"Select the input capacitance based on the minimum recommended value.  Make sure that the nominal capacitance is appropriately derated for applied voltage, especially with ceramics.  "]
[]
[]
[null,"Step 5. Feedback, Soft-Start, UVLO"]
[null,"First, review the feedback resistor network. With an adjustable device option, an external feedback resistor network is required. The resistor values are automatically calculated based on the selected VOUT in Step 1.  For lowering the leakage current through the resistors, adjust the upper FB resistor (R1) until the lower FB resistor (R2) reaches its upper end of the range (100kW).  Keeping the upper FB resistor below 1MW is recommended."]
[]
[]
[]
[null,"Second, select one out of three soft-start configurations.  If the external soft-start option is selected, enter a desired soft start time.  "]
[]
[null,"Third, select one out of the two UVLO options.  If the external UVLO option is selected, define desired UVLO thresholds and hysteresis.  Keeping the upper UVLO resistor at 1MW or higher is recommended for the minimum leakage current."]
[]
[]
[null,"Step 6. Efficiency and Thermals"]
[null,"Enter the LM5166's junction-to-ambient thermal impedance (dependent on your PCB design, air flow, etc.) and ambient temperature. Device power dissipation and junction temperature are derived at the maximum load.  Ensure that the junction temperature is within the recommended range."]
[]
[]
[]
[null,"BOM & Schematic tab"]
[null,"This tab summarizes the converter schematic and BOM.  It also helps you estimate the total solution size. Select a package size for each external component (i.e. inductor, capacitors, and resistors) for accurate solution size estimates."]
[]
[]
[null,"Design EMI Filter tab"]
[null,"In case an EMI filter is needed, a simple EMI filter design aid is given in this tab.  It is based on the guidelines documented in TI's literature number SNVA489C (aka AN-2162).  Suggest reviewing the note before using the design aid."]
[]
[]
[null,"fSW & Ripple tab"]
[null,"In this tab, the switching/burst frequency (COT/PFM mode) and the output voltage ripple as a function of the load current are plotted."]

{"sheet":"Design Converter","index":1,"n_rows":58,"n_cols":17,"rows_kept":58,"cut":false,"hidden":false,"merged":[[2,14,2,15],[0,0,0,16]]}
["                          LM5163/4 Low IQ DC/DC Converter Design Tool  "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"http://www.ti.com/ww/en/analog/power_management/widevin"]
["About",null,"xx",null,null,"= Input Box",null,null,null,null,null,null,null,null,"Terms Of Use",null,"                "]
[]
["Step 1: Operating Specifications"]
[null,null,null,"Input Voltage - Min, VIN(min) ",40,"V"]
[null,null,null,"Input Voltage - Nom, VIN(nom)",51.2,"V"]
[null,null,null,"Input Voltage - Max, VIN(max)",58,"V"]
[null,null,null,"Output Voltage, VOUT ",5,"V"]
[null,null,null,"Full Load Current, IOUT",0.5,"A"]
[null,null,null,"Mode of Operation",null,null,{"$f":"MODE","v":3}]
[null,null,null,"Switching Frequency at VIN(nom)",400,"kHz"]
[null,null,null,"Timing Resistance, RT",{"$f":"'Standard Value Calculator'!J4/1000","v":30.9},"kΩ"]
[]
["Step 2: Buck Inductor"]
[null,null,null,"Recommended Buck Inductance ",{"$f":"Lopt*1000000","v":56.396484375},"µH"]
[null,null,null,"Inductance, LF ",68,"µH"]
[null,null,null,"Inductor DCR ",120,"mΩ"]
[null,null,null,{"$f":"CHOOSE(MODE, \"Pk-to-Pk Ripple Current\",\"Pk-to-Pk Ripple Current\",\"Pk-to-Pk Ripple Current\", \"Resulting PFM Switching Frequency\")","v":"Pk-to-Pk Ripple Current"},{"$f":"Iripple_Vinnom*1000","v":171.3770141318476},"mApk-pk"]
[null,null,null,{"$f":"CHOOSE(MODE, 'Variable Mgmt'!H88,'Variable Mgmt'!H88,'Variable Mgmt'!H88, 'Variable Mgmt'!H89)","v":"% Ripple Current at Nom VIN"},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), 'Variable Mgmt'!B96*100, Ilim/2*1000)","v":34.275402826369522},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), \"%\", \"mA\")","v":"%"}]
[]
[{"$f":"IF(MODE=4, \"Step 3: Output Capacitors\", \"Step 3: Output Capacitors, Ripple Generation\")","v":"Step 3: Output Capacitors, Ripple Generation"}]
[null,null,null,"Minimum Output Capacitance ",{"$f":"'Variable Mgmt'!B116","v":9.1028721393246919},"µF"]
[null,null,null,"Output Capacitance, COUT ",33,"µF"]
[null,null,null,{"$f":"IF(OR(MODE=1,MODE=2),\"Recommended Series Resistance\",IF(MODE=3,\"Maximum Allowable ESR\",\"*Higher Cout Improves Light-Load Eff\"))","v":"Maximum Allowable ESR"},{"$f":"'Variable Mgmt'!B272","v":0.14599999999999999},"Ω"]
[null,null,null,{"$f":"IF(OR(MODE=1,MODE=2),\"Total ESR & Series Resistance, Rser\",IF(MODE=3,\"Output Capacitor ESR\",\"*PFM Hysteresis Sets Output Ripple\"))","v":"Output Capacitor ESR"},5.0000000000000001E-3,"Ω"]
[null,null,null,{"$f":"CHOOSE(MODE, \"Resulting Output Voltage Ripple\",\"Resulting Output Voltage Ripple\", \"Output Voltage Ripple\",\"Output Voltage Ripple\")","v":"Output Voltage Ripple"},{"$f":"CHOOSE(MODE, Vripple2*1000,Vripple2*1000,Vripple2*1000, PFM_Ripple)","v":1.835216269342608},"mVpk-pk"]
[null,null,null,{"$f":"IF(MODE=1,\"\",IF(MODE=2,\"Minimum Feedforward Capacitance\", IF(MODE=3,\"Minimum Coupling Capacitance\",\"\")))","v":"Minimum Coupling Capacitance"},{"$f":"'Variable Mgmt'!B140","v":">47"},"pF"]
[null,null,null,{"$f":"IF(MODE=1,\"\",IF(MODE=2,\"Feedforward Capacitance, Cff\", IF(MODE=3,\"Coupling Capacitance, Cb\",\"\")))","v":"Coupling Capacitance, Cb"},56,"pF",null,null,null,null,null,"** Specify Inductor Core Loss **",100,"mW"]
[null,null,null,{"$f":"IF(MODE=3,\"Minimum Ripple Generation Capacitance\",\"\")","v":"Minimum Ripple Generation Capacitance"},{"$f":"'Variable Mgmt'!B144","v":">230"},"pF"]
[null,null,null,{"$f":"IF(MODE=3,\"Ripple Generation Capacitance, Ca\",\"\")","v":"Ripple Generation Capacitance, Ca"},2200,"pF"]
[null,null,null,{"$f":"IF(MODE=3,\"Ripple Generation Resistance, Ra\",\"\")","v":"Ripple Generation Resistance, Ra"},{"$f":"Ra","v":255},"kΩ"]
[null,null,null,{"$f":"IF(MODE=3,\"Amplitude of Injected Ripple\",\"\")","v":"Amplitude of Injected Ripple"},20,"mVpk-pk"]
[]
["Step 4: Input Capacitors"]
[null,null,null,"Minimum Input Capacitance ",{"$f":"'Variable Mgmt'!B157","v":2.2000000000000002},"µF"]
[null,null,null,"Input Capacitance, CIN ",2.2000000000000002,"µF"]
[null,null,null,"Maximum Allowable ESR",{"$f":"'Variable Mgmt'!B159","v":4.28227996240709},"Ω"]
[null,null,null,"Input Capacitor ESR ",3,"mΩ"]
[null,null,null,"Resulting Input Voltage Ripple ",{"$f":"CHOOSE(MODE, Vinripple2*1000,Vinripple2*1000,Vinripple2*1000, 'Variable Mgmt'!B165*1000)","v":53.674907500669718},"mVpk-pk"]
[]
["Step 5: Feedback, PGOOD, UVLO"]
[null,null,null,"Upper Feedback Resistor, RFB1 ",453,"kΩ"]
[null,null,null,"Lower Feedback Resistor, RFB2",{"$f":"IF(Vout=Vref,\"OPEN\",Rfb2_u/1000)","v":143},{"$f":"IF(Vout=Vref,\"\",\"kΩ\")","v":"kΩ"}]
[null,null,null,"Acutal Output Voltage Setpoint",{"$f":"'Variable Mgmt'!B201","v":5.0013986013986012},"V"]
[null,null,null,"PGOOD Pull-up Resistance",20,{"$f":"\"kΩ\"","v":"kΩ"},null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,"BST Capacitance, CBST ",2.2000000000000002,"nF"]
[null,null,null,{"$f":"\"Required Input Voltage UVLO Turn-on\"","v":"Required Input Voltage UVLO Turn-on"},6,"V"]
[null,null,null,"Upper UVLO Resistor, RUV1",1,"MΩ"]
[null,null,null,"Lower UVLO Resistor, RUV2",{"$f":"'Variable Mgmt'!F276","v":332},{"$f":"'Variable Mgmt'!G276","v":"kΩ"}]
[null,null,null,"Actual UVLO Turn-on Threshold",{"$f":"'Variable Mgmt'!B186","v":6.0180722891566267},"V"]
[null,null,null,"Actual UVLO Turn-off Threshold",{"$f":"'Variable Mgmt'!B187","v":5.6168674698795176},"V"]
[]
["Step 6: Efficiency & Thermals"]
[null,null,null,"Estimated Thermal Impedance, JJA",41,"°C/W"]
[null,null,null,"Ambient Temp, TA",25,"°C"]
[null,null,null,"IC Power Dissipation at Full Load, PD",{"$f":"'Variable Mgmt'!B26","v":0.59420337828422776},"W"]
[null,null,null,"IC Junction Temp at Full Load, TJ",{"$f":"E56+E55*'Variable Mgmt'!B26","v":49.362338509653341},"°C"]

{"sheet":"BOM & Schematic","index":2,"n_rows":53,"n_cols":13,"rows_kept":53,"cut":false,"hidden":false,"merged":[[33,3,33,5],[0,0,0,16],[29,3,29,5],[41,3,41,5],[47,7,47,9],[30,3,30,5],[43,3,43,5],[44,3,44,5],[42,3,42,5],[39,3,39,5],[40,3,40,5],[38,3,38,5],[37,3,37,5],[36,3,36,5],[31,3,31,5],[34,3,34,5],[32,3,32,5]]}
["                         LM5163/4 100V Low IQ DC/DC Converter Design Tool  "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[{"$f":"\"VIN = \"&Vin&\" V, VOUT = \"&Vout&\" V, IOUT = \"&Iout&\" A \"&'Variable Mgmt'!B35&\" Converter\"","v":"VIN = 51.2 V, VOUT = 5 V, IOUT = 0.5 A COT Converter"}]
["Low IQ, High Efficiency, Synchronous Buck Converter BOM"]
["Count","Ref Des","Value","Description",null,null,"Size","Part Number","MFR","Footprint (mm)","Area (mm2)"]
[{"$f":"ROUNDUP('Design Converter'!E37/10,0)","v":1},"CIN",{"$f":"Cin*1000000","v":2.2000000000000002},{"$f":"IF(VIN_max>35, \"Capacitor, Ceramic, \"&'Variable Mgmt'!B257&\", 100V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B257&\", 50V, X7R, 10%\")","v":"Capacitor, Ceramic, 2.2µF, 100V, X7R, 10%"},null,null,5,"Std","Std",{"$f":"CHOOSE(G31,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)","v":"3.2 x 2.5"},{"$f":"CHOOSE(G31,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45)","v":8}]
[{"$f":"'Variable Mgmt'!D252","v":1},"COUT",{"$f":"'Variable Mgmt'!F253","v":"47µF"},{"$f":"CHOOSE(Cout_Voltage_Rating, \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 6.3V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 10V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 16V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 25V, X7R, 10%\",  \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 50V, X7R, 10%\")","v":"Capacitor, Ceramic, 47µF, 6.3V, X7R, 10%"},null,null,5,"Std","Std",{"$f":"CHOOSE(G32,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)","v":"3.2 x 2.5"},{"$f":"(CHOOSE(G32,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45))*A32","v":8}]
[{"$f":"CHOOSE(MODE, \"-\", \"-\", \"1\",\"-\")","v":"1"},{"$f":"CHOOSE(MODE,\"-\",\"-\",\"Ca\",\"-\")","v":"Ca"},{"$f":"CHOOSE(MODE, \"-\",\"-\",'Variable Mgmt'!B293, \"-\")","v":"2200pF"},{"$f":"CHOOSE(MODE,\"-\",\"-\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B293&\", 16V, X7R, 10%\", \"-\")","v":"Capacitor, Ceramic, 2200pF, 16V, X7R, 10%"},null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"-\", \"Std\", \"-\")","v":"Std"},{"$f":"H33","v":"Std"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G33,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G33,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[{"$f":"CHOOSE(MODE, \"-\", \"1\", \"1\",\"-\")","v":"1"},{"$f":"CHOOSE(MODE,\"-\",\"Cff\",\"Cb\",\"-\")","v":"Cb"},{"$f":"CHOOSE(MODE, \"-\",'Variable Mgmt'!B290,'Variable Mgmt'!B290, \"-\")","v":"56pF"},{"$f":"CHOOSE(MODE,\"-\",\"Capacitor, Ceramic, \"&'Variable Mgmt'!B290&\", 50V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B290&\", 50V, X7R, 10%\", \"-\")","v":"Capacitor, Ceramic, 56pF, 50V, X7R, 10%"},null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"Std\", \"Std\", \"-\")","v":"Std"},{"$f":"H34","v":"Std"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G34,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G34,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G34,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G34,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"CBST","2.2nF","Capacitor, Ceramic, 2.2nF, 25V, X7R, 10%",null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"Std\", \"Std\", \"-\")","v":"Std"},{"$f":"H35","v":"Std"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G35,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G35,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G35,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G35,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[]
[1,"LF",{"$f":"'Design Converter'!E17","v":68},{"$f":"\"Inductor, \"&Lf*1000000&\" µH, \"&Rdcr*1000&\" mΩ, >\"&ROUNDUP(Isat_min,2)&\"A\"","v":"Inductor, 68 µH, 120 mΩ, >0.9A"},null,null,4,"Various","Various",{"$f":"CHOOSE(G37,'Variable Mgmt'!T50,'Variable Mgmt'!T51,'Variable Mgmt'!T52,'Variable Mgmt'!T53,'Variable Mgmt'!T54,'Variable Mgmt'!T55,'Variable Mgmt'!T56)","v":"6.0 x 6.0"},{"$f":"CHOOSE(G37,'Variable Mgmt'!U50,'Variable Mgmt'!U51,'Variable Mgmt'!U52,'Variable Mgmt'!U53,'Variable Mgmt'!U54,'Variable Mgmt'!U55,'Variable Mgmt'!U56)","v":36}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(MODE_RSET=2,CHOOSE(G38,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":""}]
[{"$f":"CHOOSE(MODE, \"1\",\"1\",\"1\", \"-\")","v":"1"},"RT",{"$f":"CHOOSE(MODE, 'Design Converter'!E13, 'Design Converter'!E13,'Design Converter'!E13,\"-\")","v":30.9},{"$f":"C39","v":30.9},null,null,1,{"$f":"CHOOSE(MODE, \"Std\",\"Std\",\"Std\",\"-\")","v":"Std"},{"$f":"H39","v":"Std"},{"$f":"CHOOSE(MODE,CHOOSE(G39,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G39,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G39,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,CHOOSE(G39,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G39,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G39,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"RFB1",{"$f":"Rfb1_/1000","v":453},453,null,null,1,{"$f":"CHOOSE(MODE_VOUT,\"-\",\"Std\")","v":"Std"},{"$f":"H40","v":"Std"},{"$f":"(CHOOSE(MODE_VOUT,\"\",CHOOSE(G40,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)))","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE_VOUT,\"\",CHOOSE(G40,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45))","v":0.5}]
[1,"RFB2",{"$f":"Rfb2_u/1000","v":143},143,null,null,1,{"$f":"CHOOSE(MODE_VOUT,\"-\",\"Std\")","v":"Std"},{"$f":"H41","v":"Std"},{"$f":"CHOOSE(MODE_VOUT,\"\",CHOOSE(G41,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45))","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE_VOUT,\"\",CHOOSE(G41,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45))","v":0.5}]
[{"$f":"IF(MODE=3,\"1\",\"-\")","v":"1"},{"$f":"CHOOSE(MODE,\"-\",\"-\",\"Ra\",\"-\")","v":"Ra"},{"$f":"'Variable Mgmt'!F296","v":"255k"},{"$f":"\"Resistor, Chip, \"&'Variable Mgmt'!B296&\", 1/16W, 1%\"","v":"Resistor, Chip, 255kΩ, 1/16W, 1%"},null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"-\", \"Std\", \"-\")","v":"Std"},{"$f":"H42","v":"Std"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G42,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G42,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"RPGOOD",100,100,null,null,1,"Std","Std",{"$f":"CHOOSE(G43,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)","v":"1.0 x 0.5"},{"$f":"CHOOSE(G43,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45)","v":0.5}]
[{"$f":"CHOOSE(MODE_UVLO, \"1\", \"-\")","v":"1"},"RUV1",{"$f":"CHOOSE(MODE_UVLO, 'Variable Mgmt'!H275, \"-\")","v":"1M"},{"$f":"CHOOSE(MODE_UVLO, \"Resistor, Chip, \"&'Variable Mgmt'!C275&\", 1/16W, 1%\", \"-\")","v":"Resistor, Chip, 1MΩ, 1/16W, 1%"},null,null,2,{"$f":"CHOOSE(MODE_UVLO,\"Std\",\"-\")","v":"Std"},{"$f":"H44","v":"Std"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G44,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.6 x 0.8"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G44,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":1.3}]
[{"$f":"CHOOSE(MODE_UVLO, \"1\", \"-\")","v":"1"},"RUV2",{"$f":"CHOOSE(MODE_UVLO, 'Variable Mgmt'!H276, \"-\")","v":"332k"},{"$f":"CHOOSE(MODE_UVLO, \"Resistor, Chip, \"&'Variable Mgmt'!C276&\", 1/16W, 1%\", \"-\")","v":"Resistor, Chip, 332kΩ, 1/16W, 1%"},null,null,1,{"$f":"CHOOSE(MODE_UVLO,\"Std\",\"-\")","v":"Std"},{"$f":"H45","v":"Std"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G45,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G45,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"U1",{"$f":"CHOOSE(VARIANT, \"LM5163-Q1\", \"LM5164-Q1\")","v":"LM5163-Q1"},{"$f":"CHOOSE(VARIANT, \"IC, LM51643-Q1, Buck Converter, 6V–100V Input\", \"IC, LM5164-Q1, Buck Converter, 6V–100V Input\")","v":"IC, LM51643-Q1, Buck Converter, 6V–100V Input"},null,null,"SOIC-8",{"$f":"CHOOSE(VARIANT, \"LM5163QDDATQ1\", \"LM5164QDDATQ1\")","v":"LM5163QDDATQ1"},"TI","5.0 x 6.0",30]
[]
[null,{"$f":"\"Total Solution Size (padded by 15%) = \"&ROUND(K48,1)&\" mm^2 = \"&ROUND(M48,3)&\" in^2\"","v":"Total Solution Size (padded by 15%) = 101 mm^2 = 0.157 in^2"},null,null,null,null,null,null,null,null,{"$f":"SUM(K31:K46)*1.15","v":100.96999999999998},null,{"$f":"K48/25.4/25.4","v":0.156503813007626}]
[]
["NOTES:"]
["* Inductor saturation current should be higher than the peak inductor current setting for all operating temperatures *"]
["** Effective input and output capacitances should be appropriately derated for applied voltage and temperature, particularly with ceramics **"]
["***Estimated total solution size does not include EMI filter***"]

{"sheet":"Fsw & Ripple","index":3,"n_rows":1,"n_cols":1,"rows_kept":1,"cut":false,"hidden":true,"merged":[[0,0,0,16]]}
["                         LM5164 Low IQ DC/DC Converter Design Tool  "]

{"sheet":"Losses","index":4,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":true,"merged":[[0,0,0,16]]}
["                         LM5166 Low IQ DC/DC Converter Design Tool  "]
[]
[]
[]
[null,null,null,"Load Current",500,"mA"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"Inductor Core Loss Constant",0]

{"sheet":"EVM","index":5,"n_rows":85,"n_cols":15,"rows_kept":85,"cut":false,"hidden":false,"merged":[[0,0,0,16]]}
["LM5163/4 100V, Low IQ DC/DC Converter Design Tool  "]
[]
[null,"LM5164-Q1EVM-041 PCB Layout"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Top"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer 2"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer 3"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bottom"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer"]

{"sheet":"Design EMI Filter","index":6,"n_rows":33,"n_cols":15,"rows_kept":33,"cut":false,"hidden":false,"merged":[[0,0,0,22],[32,10,32,12],[29,10,29,12],[31,10,31,12]]}
["                         LM5163/4 100V, Low IQ DC/DC Converter Design Tool  "]
[]
[]
[]
[]
[]
["Step 7: EMI Filter (Optional)"]
[null,null,null,"Desired Maximum Noise Level, Vnoise(MAX)",50,"dBmV"]
[null,null,null,"EMI Filter Inductance, LF(EMI)",22,"mH"]
[null,null,null,"Minimum EMI Filter Capacitance",{"$f":"'Variable Mgmt'!M164","v":0.50516181006850647},"mF"]
[null,null,null,"EMI Filter Capacitance, CF(EMI)",4.7,"mF"]
[null,null,null,"Minimum EMI Filter Damping Capacitance",{"$f":"'Variable Mgmt'!M168","v":8.8000000000000007},"mF"]
[null,null,null,"EMI Filter Damping Capacitance, CD(EMI)",10,"mF"]
[null,null,null,"Minimum Damping Capacitor ESR",{"$f":"'Variable Mgmt'!M169","v":3.1622776601683795},"Ω"]
[null,null,null,"Damping Capacitor ESR, ESR CD(EMI)",3.3,"Ω"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"EMI Filter BOM"]
[null,null,null,null,null,null,null,"Count","Ref Des","Value","Description",null,null,"Part Number","MFR"]
[null,null,null,null,null,null,null,1,"LF(EMI)",{"$f":"'Variable Mgmt'!B298","v":"22µH"},{"$f":"\"Inductor, \"&Lf_emi*1000000&\" µH, \"&ROUNDUP(Isat_min,2)&\"A\"","v":"Inductor, 22 µH, 0.9A"},null,null,"Std","Std"]
[null,null,null,null,null,null,null,1,"CF(EMI)",{"$f":"'Variable Mgmt'!B299","v":"4.7µF"},{"$f":"IF(VIN_max>35, \"Capacitor, Ceramic, \"&'Variable Mgmt'!B299&\", 100V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B299&\", 50V, X7R, 10%\")","v":"Capacitor, Ceramic, 4.7µF, 100V, X7R, 10%"},null,null,"Std","Std"]
[null,null,null,null,null,null,null,1,"CD(EMI)",{"$f":"'Variable Mgmt'!B300","v":"10µF"},{"$f":"IF(VIN_max>35, \"Capacitor, Electrolytic, \"&'Variable Mgmt'!B300&\", 100V, ESR>\"&ESR_Cd&ohm, \"Capacitor, Electrolytic, \"&'Variable Mgmt'!B300&\", 50V, ESR>\"&ESR_Cd&ohm)","v":"Capacitor, Electrolytic, 10µF, 100V, ESR>3.3Ω"},null,null,"Std","Std"]

{"sheet":"Variable Mgmt","index":7,"n_rows":320,"n_cols":21,"rows_kept":320,"cut":false,"hidden":true,"merged":[[4,4,4,7],[0,0,0,8]]}
["EXCEL Variables Names/Calculations",null,null,null,null,null,null,null,null,null,null,"LM5166"]
[null,"Input from user ="]
[null,"Output ="]
[null,"Constant"]
["Variable Name","Value","STD Units",null,"Notes",null,null,null,"Iteration"]
["Step 1: Operational Specs"]
["VIN_min",{"$f":"'Design Converter'!E6","v":40},"V","Minimum input voltage",null,null,null,null,1]
["VIN_nom",{"$f":"'Design Converter'!E7","v":51.2},"V","Nominal input voltage"]
["VIN_max",{"$f":"'Design Converter'!E8","v":58},"V","Maximum input voltage"]
[]
["Vout",{"$f":"'Design Converter'!E9","v":5},"V","Output Voltage",null,null,null,null,1]
["Iout",{"$f":"'Design Converter'!E10","v":0.5},"A","Maximum Output Current",null,null,null,null,1]
["Rout",{"$f":"Vout/Iout","v":10},"W","Load resistance"]
["Pout",{"$f":"Vout*Iout","v":2.5},"W","Output power"]
[]
["Efficiency",0.9,null,"Estimate of efficiency"]
["Pin",{"$f":"Pout/Efficiency","v":2.7777777777777777},"W","Calculate input power assuming 90% efficiency"]
["Iin_Vinmin",{"$f":"Pin/VIN_min","v":6.9444444444444448E-2},"A"]
["Iin_Vinnom",{"$f":"Pin/VIN_nom","v":5.4253472222222217E-2},"A","Input currents at min, nom, max Vin"]
["Iin_Vinmax",{"$f":"Pin/VIN_max","v":4.7892720306513412E-2},"A"]
[]
["Fsw",{"$f":"'Design Converter'!E12*1000","v":400000},"Hz","Nominal Switching Frequency",null,null,null,null,1]
["Vref",1.2,"V","Reference Voltage"]
["Rt",{"$f":"Vout*2500000000/Fsw","v":31250},"W","Frequency Set Resistor"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"B34&\"_\"&F35&\"_\"&F39&\"_\"&I41&\"_\"&I36","v":"COT3_VOUTadj_UVLOadj_SSAdj_RsetGND"},null,null,null,null,null,"Vout<5V",100,1]
["Internal PD at Full Load",{"$f":" IF(OR(MODE=1,MODE=2,MODE=3), Efficiency!AZ106,#REF!)","v":0.59420337828422776},"W",null,null,null,null,null,null,null,null,null,null,null,null,null,"Vout<=8V",47,2]
[null,null,null,null,null,null,null,null,null,null,{"$f":"\"SCH_\"&B34&\"_\"&B41","v":"SCH_COT3_LM5163"},null,null,null,null,null,"Vout<=12V",22,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vout<=20V",22,4]
["Step 2: Circuit Configuration for COT / PFM, Fixed / Adj Vout, ILIM, UVLO, SS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vout>20V",10,5]
[null,"COT Type I",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cout Capacitance",{"$f":"CHOOSE(S30,\"100\", \"47\",\"22\",\"22\",\"10\")","v":"47"},{"$f":"IF(Vout<5, 1, IF(Vout<=8, 2, IF(Vout<=12, 3, IF(Vout<=20, 4, 5))))","v":2}]
[null,"COT Type II",2]
["COT/PFM ","COT Type III",3]
[null,null,null,null,"VOUT Fixed/Adjustable","Fixed",1,null,"ILIM shorted",1,{"$f":"B34&\", \"&F35&\", \"&I36&\", \"&F39&\", \"&I41","v":"COT3, VOUTadj, RsetGND, UVLOadj, SSAdj"},null,null,null,null,null,"Vout<=5V","6.3V",1]
["MODE",{"$f":"CHOOSE(C34, \"COT1\", \"COT2\",\"COT3\")","v":"COT3"},3,null,null,"Adjustable",2,null,"ILIM resistor needed",2,{"$f":"C34&\", \"&G35&\", \"&J36&\", \"&G39&\", \"&J41","v":"3, 2, 1, 1, 1"},null,null,null,null,null,"Vout<=8V","10V",2]
[null,{"$f":"IF(MODE=4, \"PFM\", \"COT\")","v":"COT"},null,null,"MODE_VOUT",{"$f":"CHOOSE(G35, \"VOUTfixed\", \"VOUTadj\")","v":"VOUTadj"},{"$f":"IF(AND(OR(MODE=1,MODE=4),OR(Vout=3.3,Vout=5)),1,2)","v":2},null,null,null,{"$f":"C34&G35&J36&G39&J41","v":"32111"},null,null,null,null,null,"Vout<=12V","16V",3]
[null,null,null,null,null,null,null,"MODE_RSET",{"$f":"CHOOSE(J36, \"RsetGND\",\"Rset\")","v":"RsetGND"},1,null,null,null,null,null,null,"Vout<=20V","25V",4]
[null,null,null,null,"UVLO","Adjustable",1,null,null,null,null,null,null,null,null,null,"Vout>20V","50V",5]
[null,null,null,null,null,"Internal",2,"Soft Start","Adjustable",1,null,"Iout Linear Axis",1,null,null,null,"Cout Voltage Rating",{"$f":"CHOOSE(S38,\"6.3V\", \"10V\",\"16V\",\"25V\",\"50V\")","v":"6.3V"},{"$f":"IF(Vout<=5, 1, IF(Vout<=8, 2, IF(Vout<=12, 3, IF(Vout<=20, 4, 5))))","v":1}]
[null,"LM5163",1,null,"MODE_UVLO",{"$f":"CHOOSE(G39, \"UVLOadj\", \"UVLOint\")","v":"UVLOadj"},1,null,"3ms Fixed",2,null,"Iout Log Axis",2]
[null,"LM5164",2,null,null,null,null,null,null,null,null,"PLOT_TYPE",1]
["VARIANT",{"$f":"CHOOSE(VARIANT, \"LM5163\", \"LM5164\")","v":"LM5163"},1,null,"ESR","NO",1,"MODE_SS",{"$f":"CHOOSE(J41, \"SSAdj\", \"SSfix\")","v":"SSAdj"},1,null,null,null,null,null,null,null,"0402",1,"1.0 x 0.5",0.5]
[null,null,null,null,null,"YES",2,null,null,null,null,null,null,null,null,null,null,"0603",2,"1.6 x 0.8",1.3]
[null,null,null,null,"MODE_ESR",null,2,null,null,null,null,null,null,null,null,null,null,"0805",3,"2.0 x 1.25",2.5]
[null,null,null,null,null,{"$f":"CHOOSE(G44, \"\", \"_ESR\")","v":"_ESR"},{"$f":"IF(MODE=2, 1, MODE_ESR)","v":2},null,null,null,null,null,null,null,null,null,null,"1206",4,"3.2 x 1.6",5.0999999999999996]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1210",5,"3.2 x 2.5",8]
["Step 3: Buck Inductor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Component Size",{"$f":"CHOOSE(S46,\"0402\", \"0603\",\"0805\",\"1206\",\"1210\")","v":"1210"},5,{"$f":"CHOOSE(S46,T41,T42,T43,T44,T45)","v":"3.2 x 2.5"}]
["Don1",{"$f":"Vout/VIN_nom","v":9.765625E-2},{"$f":"(Vout-VIN_nom)/Vout","v":-9.24},null,"Ideal Duty Cycle at VIN(nom)",null,null,null,1]
["Doff1",{"$f":"1-47:47","v":0.90234375},null,null,"Ideal 1- Duty Cycle at VIN(nom)",null,null,null,1]
[]
["Don_Vinmin",{"$f":"Vout/VIN_min","v":0.125},{"$f":"IF(VIN_min>Vout, \"BUCK\", \"BOOST\")","v":"BUCK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3mm x 3mm",1,"3.0 x 3.0",9]
["Don_Vinnom",{"$f":"Vout/VIN_nom","v":9.765625E-2},{"$f":"IF(VIN_nom>Vout, \"BUCK\", \"BOOST\")","v":"BUCK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4mm x 4mm",2,"4.0 x 4.0",16]
["Don_Vinmax",{"$f":"Vout/VIN_max","v":8.6206896551724144E-2},{"$f":"IF(VIN_max>Vout, \"BUCK\", \"BOOST\")","v":"BUCK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5mm x 5mm",3,"5.0 x 5.0",25]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6mm x 6mm",4,"6.0 x 6.0",36]
["Lf_Vinmin",{"$f":"(VIN_min-Vout)*Don_Vinmin/(Fsw*Iout*0.4)","v":5.4687500000000001E-5},"H","COT",null,null,null,null,null,null,null,null,null,null,null,null,null,"7mm x 7mm",5,"7.0 x 7.0",49]
["Lf_Vinnom",{"$f":"(VIN_nom-Vout)*Don_Vinnom/(Fsw*Iout*0.4)","v":5.6396484375000003E-5},"H","COT",null,null,null,null,1,null,null,null,null,null,null,null,"Inductor Size","8mm x 8mm",6,"8.0 x 8.0",64]
["Lf_Vinmax",{"$f":"(VIN_max-Vout)*Don_Vinmax/(Fsw*Iout*0.7)","v":3.2635467980295569E-5},"H","COT",null,null,null,null,null,null,null,null,null,null,null,null,null,"10mm x 10mm",7,"10.0 x 10.0",100]
[]
["L_Vinmin_COT",{"$f":"(VIN_min-Vout)*Don_Vinmin/(Fsw*Iout*0.3)","v":7.2916666666666673E-5},"H","COT","Calculated Inductance for 30% ripple at VIN(min)"]
["L_Vinnom_COT",{"$f":"(VIN_nom-Vout)*Don_Vinnom/(Fsw*Iout*0.4)","v":5.6396484375000003E-5},"H","COT","Calculated Inductance for 40% ripple at VIN(nom)",null,null,null,null,null,"Pk-to-Pk Ripple Current at VIN(nom), DIL"]
["L_Vinmax_COT",{"$f":"(VIN_max-Vout)*Don_Vinmax/(Fsw*Iout*0.7)","v":3.2635467980295569E-5},"H","COT","Calculated Inductance for 70% ripple at VIN(max)"]
[]
[]
["Lopt",{"$f":"B59","v":5.6396484375000003E-5},"H"]
[]
["Lf",{"$f":"'Design Converter'!E17/1000000","v":6.7999999999999999E-5},"H",null,"Chosen Inductance"]
["Rdcr",{"$f":"'Design Converter'!E18/1000","v":0.12},"W",null,"Chosen Inductor DCR"]
[]
["Don2",{"$f":"(Vout+Iout*Rdcr)/Vin","v":9.8828124999999989E-2},null,null,"**Edit to add Rdson**"]
["Doff2",{"$f":"1-_Don2","v":0.90117187499999996}]
[]
["Rdson1",0.75,"W"]
["Rdson2",0.33,"W"]
[]
["Don_Vinmin_2",{"$f":"(Vout+Iout*(Rdcr+Rdson2))/(VIN_min+Iout*Rdson2)","v":0.130088385410183},null,null,"Duty cycles adjusted for DCR and shunt voltage drops"]
["Don_Vinnom_2",{"$f":"(Vout+Iout*(Rdcr+Rdson2))/(VIN_nom+Iout*Rdson2)","v":0.10172296310717413},null,null,"need to include RDS(on) later"]
["Don_Vinmax_2",{"$f":"(Vout+Iout*(Rdcr+Rdson2))/(VIN_max+Iout*Rdson2)","v":8.983065417347201E-2}]
[]
["Iripple_Vinmin",{"$f":"(VIN_min-Vout-Rdson1*Iout)*Don_Vinmin_2/(Fsw*Lf)","v":0.16559964503042598},"A","COT"]
["Iripple_Vinnom",{"$f":"(VIN_nom-Vout-Rdson1*Iout)*Don_Vinnom_2/(Fsw*Lf)","v":0.17137701413184761},"A","COT"]
["Iripple_Vinmax",{"$f":"(VIN_max-Vout)*Don_Vinmax_2/(Fsw*Lf)","v":0.17503767173507415},"A","COT"]
[]
["ILpk_Vinmin",{"$f":"Iout+Iripple_Vinmin/2","v":0.58279982251521301},"A","COT"]
["ILpk_Vinnom",{"$f":"Iout+Iripple_Vinnom/2","v":0.58568850706592379},"A","COT"]
["ILpk_Vinmax",{"$f":"Iout+Iripple_Vinmax/2","v":0.58751883586753706},"A","COT"]
[]
["ILIM_Typ",{"$f":"CHOOSE(VARIANT, 0.75, 1.5)","v":0.75},"A",null,"Isat_min",{"$f":"B86*1.2","v":0.89999999999999991}]
[]
["Ripple current",{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), Iripple_Vinnom, Iripple)","v":0.17137701413184761},"A",null,null,null,null,"% Ripple Current at Nom VIN"]
[null,null,null,null,null,null,null,"Maximum Load Current"]
["Max inductor ripple current",{"$f":"MAX(B78:B80)","v":0.17503767173507415},"A"]
[null,null,null,null,null,"Ripple I","Iin"]
["% Ripple Current",{"$f":"B78/Iout","v":0.33119929006085197},null,"COT",null,{"$f":"B78","v":0.16559964503042598},{"$f":"Iin_Vinmin","v":6.9444444444444448E-2}]
[null,{"$f":"B79/Iout","v":0.34275402826369522},null,"COT",null,{"$f":"B79","v":0.17137701413184761},{"$f":"Iin_Vinnom","v":5.4253472222222217E-2}]
[null,{"$f":"B80/Iout","v":0.35007534347014829},null,"COT",null,{"$f":"B80","v":0.17503767173507415},{"$f":"Iin_Vinmax","v":4.7892720306513412E-2}]
[]
[null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3), B93, Ilim/Iout)","v":0.34275402826369522}]
[]
["Iripple1",{"$f":"(Vin-Vout)*Don_Vinnom_2/(Fsw*Lf)","v":0.17277944468939135},"A","inductor ripple current with chosen inductance (pk-pk)",null,null,null,null,1]
["Temp",100]
["DCR at hot",{"$f":"Rdcr*(1+0.0039*(B99-25))","v":0.15509999999999999},"W"]
[]
[]
[]
["Step 4: Output Capacitor"]
["Icoutrms_VINmin",{"$f":"Iripple_Vinmin/SQRT(12)","v":4.7804499818011457E-2},"A","Output Cap RMS current"]
["Icoutrms_VINnom",{"$f":"Iripple_Vinnom/SQRT(12)","v":4.9472282620968262E-2},"A"]
["Icoutrms_VINmax",{"$f":"Iripple_Vinmax/SQRT(12)","v":5.0529023447285208E-2},"A",null,null,null,{"$f":"Vripple1","v":2.5000000000000001E-2}]
[]
["Output Ripple Spec (pk-pk)",{"$f":"Vout*0.005","v":2.5000000000000001E-2},"V","Vout capacitive ripple spec at Vin(nom) = Vripple1"]
[]
["Coutmin"]
["COT",{"$f":"Iripple_Vinnom/(Fsw*8*Vripple1)","v":2.1422126766480952E-6},"F","COT","Min recommended Cout based on ripple spec above",null,null,null,1]
[null,{"$f":"Lf*B83^2/((1.05*Vout)^2-Vout^2)","v":9.1028721393246927E-6},"F","COT","Min recommended Cout based on 5% load-off transient spec"]
["CoutMinCOT",{"$f":"MAX(B112:B113, 0.0000022)","v":9.1028721393246927E-6},"F","COT","max of 2 results and 2.2uF"]
[]
["Reported Countmin",{"$f":"CoutMinCOT*1000000","v":9.1028721393246919},"µF"]
[]
["Cout",{"$f":"'Design Converter'!E24/1000000","v":3.3000000000000003E-5},"F","Chosen Output Capacitance",null,null,null,null,1]
["Resrmax",{"$f":"SQRT((Vripple1/Iripple_Vinnom)^2-(1/(Fsw*Cout*8))^2)","v":0.14556951631293774},"W","Max ESR before ripple exceeds Vripple1",null,null,null,null,1]
["Type1 ESR for sufficient (20mV) COT ripple at FB pin",{"$f":"0.02*Vout/Vref/Iripple_Vinnom","v":0.48625735344660326},"W","(a)"]
["Type2 ESR for sufficient (20mV) COT ripple at FB pin",{"$f":"0.02/Iripple_Vinnom","v":0.11670176482718476},"W","(b)"]
[]
["Type 1 Output Cap RC Time Constant",{"$f":"Cout*B130*1000000","v":0},"µs"]
["Type 2 Output Cap RC Time Constant",{"$f":"Cout*B131*1000000","v":0},"µs"]
["Ton @ Vin(min)",{"$f":"Vout/VIN_min/(Fsw)","v":3.1250000000000003E-7},"s"]
["Ton @ Vin(nom)",{"$f":"Vout/VIN_nom/(Fsw)","v":2.4414062500000001E-7},"s"]
["ESR so that RC > Ton/2",{"$f":"B125/2/Cout","v":4.734848484848485E-3},"W","(c)"]
[]
[]
["Type1: Need ESR of…",{"$f":"IF(MODE=1, MAX(B120,B127), 0)","v":0},"W","Max of (a) and (c)"]
["Type2: Need ESR of…",{"$f":"IF(MODE=2, MAX(B121,B127), 0)","v":0},"W","Max of (b) and (c)"]
[]
["Reported Cout ESR max",{"$f":"IF(OR(CoutEsrMax>0.5, CoutEsrMax<0, (ISERROR(CoutEsrMax))), \"N/A\", CoutEsrMax*1000)","v":145.56951631293774},"mW"]
[]
["CoutEsr",{"$f":" 'Design Converter'!E26","v":5.0000000000000001E-3},"W","Chosen ESR",null,null,null,null,1]
[]
["Actual Output Ripple",{"$f":"Iripple_Vinnom*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2)","v":1.8352162693426079E-3},"Vp-p","Vripple2"]
[]
["Minimum Feedforward / Coupling Capacitance",{"$f":"MAX(1000000000000*0.00005/(3*Rfb1_),47)","v":47},"pF",null,null,null,null,{"$f":"0.00005/3/Rfb1_","v":3.6791758646063281E-11}]
["Recommended Cff / Cb",{"$f":"IF(OR(MODE=2,MODE=3), \">\"&ROUND(B139,0),\"\")","v":">47"},"pF"]
["Selected Cff / Cb",{"$f":"'Design Converter'!$E$29","v":56},"pF"]
[]
["Minimum Ripple Generation Capacitance",{"$f":"10/(Fsw*Rfb)","v":2.3001281279426974E-10},"F",{"$f":"1000000000000*B143","v":230.01281279426973},"pF",{"$f":"Rfb","v":108689.59731543624}]
["Recommended Ca",{"$f":"IF(MODE=3, \">\"&ROUND(D143,0),\"\")","v":">230"},"pF"]
["Selected Ca",{"$f":"'Design Converter'!E31","v":2200},"pF",{"$f":"B145/1000000000000","v":2.1999999999999998E-9},"F"]
[]
["Maximum Ripple Generation Resistance",{"$f":"(VIN_nom-Vout)*B126/((B149/1000)*Ca)","v":256347.65625000006},"W",{"$f":"B147/1000","v":256.34765625000006},"kW"]
["Recommended Ra",{"$f":"IF(MODE=3, \"<\"&ROUND(D147,0),\"\")","v":"<256"},"kW",null,null,null,null,null,null,null,null,"Lf_emi",{"$f":"'Design EMI Filter'!$E$9","v":22},"uH",{"$f":"M148/1000000","v":2.1999999999999999E-5},"H"]
["Ripple amplitude",{"$f":"'Design Converter'!E33","v":20},"mVp-p",null,null,null,null,null,null,null,null,"Cf_emi",{"$f":"'Design EMI Filter'!$E$11","v":4.7},"uF",{"$f":"M149/1000000","v":4.6999999999999999E-6},"F"]
[null,null,null,null,null,null,null,null,null,null,null,"Cd_emi",{"$f":"'Design EMI Filter'!$E$13","v":10},"uF",{"$f":"M150/1000000","v":1.0000000000000001E-5},"F"]
[null,null,null,null,null,null,null,null,null,null,null,"ESR_Cd",{"$f":"'Design EMI Filter'!$E$15","v":3.3},"Ω",{"$f":"M151","v":3.3},"Ω",{"$f":"ESR_Cd&ohm","v":"3.3Ω"}]
["Step 5: Input Capacitor",null,null,null,null,null,null,null,null,null,null,"Min Noise",{"$f":"'Design EMI Filter'!$E$8","v":50},"dB","noise limit"]
["Vinripple1",{"$f":"0.05*VIN_nom","v":2.5600000000000005},"Vp-p","Input voltage ripple spec (pk-pk) at Vin(nom)",null,null,null,null,null,null,null,"Duty Cycle",{"$f":"Vout/VIN_nom/Efficiency_COT_Full_Load","v":0.12600806451612903},null,"calculated duty cycle"]
[null,null,null,null,null,null,null,null,null,null,null,"Target Atten.",{"$f":"20*LOG(Iout/(PI()^2*Fsw*Cin)*SIN(PI()*Duty_Cycle)/0.000001) - Min_Noise","v":36.926658218297746},"dB","calculated attenuation"]
["Icinrms",{"$f":"Iout*SQRT(Don_Vinnom_2*(1-Don_Vinnom_2))","v":0.15114182237543536},"A"]
["Cinmin",{"$f":"Iout*Don_Vinnom_2*(1-Don_Vinnom_2)/(Vinripple1*Fsw-Iout*RCinEsr)*1000000","v":4.4616895516465471E-2},"µF"]
["Reported Cinmin",{"$f":"IF(Cinmin<2.2, 2.2,Cinmin)","v":2.2000000000000002},"µF",null,null,null,null,null,null,null,null,"Filter Inductor"]
["Cin",{"$f":"'Design Converter'!E37/1000000","v":2.2000000000000001E-6},"F","Input capacitance",null,null,null,null,null,null,null,"Irms rating",{"$f":"Iout*1.5","v":0.75},"A","calculated suggested IRMS rating"]
["CinEsrMax",{"$f":"-(Iout*Don_Vinnom_2*(1-Don_Vinnom_2)/(Cin*Fsw)-Vinripple1)/(Iout+Iripple_Vinnom/2)","v":4.28227996240709},"W"]
["RCinEsr",{"$f":"'Design Converter'!E39/1000","v":3.0000000000000001E-3},"W","Input capacitance series resistance (ESR)"]
["Reported Cin ESR max",{"$f":"IF(OR(CinEsrMax>12, CinEsrMax<0), \"N/A\",CinEsrMax*1000)","v":4282.2799624070904},"mΩ",null,null,null,null,null,null,null,null,"Filter Capacitor"]
[null,null,null,null,null,null,null,null,null,null,null,"Cfa calculation",{"$f":"Cin/(Cin*Lf_emi*0.000001*(2*PI()*Fsw/10)^2 - 1) / 0.000001","v":-2.2000067258796125},"uF","calculated value"]
["COT input voltage ripple - Vinripple2",{"$f":"Iout*Don_Vinnom_2*(1-Don_Vinnom_2)/(Cin*Fsw)+(Iout +Iripple_Vinnom/2)*RCinEsr","v":5.3674907500669722E-2},"Vp-p",null,{"$f":"Iout*Don_Vinmax_2*(1-Don_Vinmax_2)/(Cin*Fsw)","v":4.6455174854680731E-2},"Vp-p",null,null,null,null,null,"Cfb calculation",{"$f":"1/(Lf_emi)*(10^(Target_Att/40)/(2*PI()*Fsw))^2/0.000001","v":0.50516181006850647},"uF","calculated value"]
[null,null,null,null,null,null,null,null,null,null,null,"Cf",{"$f":"MAX(M162,M163)","v":0.50516181006850647},"uF","calculated value"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Damping Capacitor"]
["Step 6: Soft Start",null,null,null,null,null,null,null,null,null,null,"Cd ≥",{"$f":"4*Cin*1000000","v":8.8000000000000007},"uF","calculated value"]
["Tss",{"$f":"'Design Converter'!#REF!/1000","v":{"$error":"#REF!"}},"s","Soft-start time",null,null,null,null,null,null,null,"Cd ESR ≥",{"$f":"SQRT(Lf_emi/Cin)","v":3.1622776601683795},"Ω","calculated value"]
["Iss",1.0000000000000001E-5,"A","Soft-start current"]
["Css",{"$f":"8.16*Tss/1000000","v":{"$error":"#NAME?"}},"F","Required soft-start cap"]
["Css_u",{"$f":"'Standard Value Calculator'!B4","v":{"$error":"#NAME?"}},"F","User selected SS cap",null,null,null,null,null,null,null,"CIN and Cd Capacitors Current Sharing and Rating"]
[null,null,null,null,null,null,null,null,null,null,null,"Cd impedance",{"$f":" 1/(2*PI()*Fsw*Cd_emi) + ESR_Cd","v":3.3397887357729736},"Ω","calculated Cd impedance at the sw. frequency"]
["Step 7: Other Components - UVLO, PGOOD",null,null,null,null,null,null,null,null,null,null,"Cin impedance",{"$f":" 1/(2*PI()*Fsw*Cin) + RCinEsr","v":0.18385788987715382},"Ω","calculated CIN impedance at the sw. frequency"]
[]
["Rising UVLO/EN Threshold",1.5,"V",null,null,null,null,null,null,null,null,"IRMS Total Input Cap",{"$f":"Iout*SQRT(Duty_Cycle*(1-Duty_Cycle))","v":0.16592922602199114},"A","calculated total IRMS current for CIN and Cd combined"]
["Falling UVLO/EN Threshold",1.4,"V",null,null,null,null,null,null,null,null,"IRMS Cd Act",{"$f":"IRMSTOT*(ZCIN/(ZCIN+ZCd))","v":8.6579048941162959E-3},"A","Calculated min IRMS current rating for Cd"]
["Voltage Hysteresis",{"$f":"B176-B177","v":0.10000000000000009},"V",null,null,null,null,null,null,null,null,"IRMS CIN",{"$f":"IRMSTOT*(ZCd/(ZCIN+ZCd))","v":0.15727132112787484},"A","Calculated min IRMS current rating for CIN"]
[]
["VINUVLO_ON",{"$f":"'Design Converter'!E48","v":6},"V"]
["VINUVLO_OFF",null,"V"]
[]
["RUV1",{"$f":"'Design Converter'!E49*1000","v":1000},"kΩ",{"$f":"'Standard Value Calculator'!J16","v":1000},"kΩ",{"$f":"IF(Ruvlo1<0,\"N/A\",D183)","v":1000},{"$f":"IF(Ruvlo1<0,\"N/A\",D183&\"kΩ\")","v":"1000kΩ"}]
["RUV2",{"$f":"Vuvlo_on*Ruvlo1/(VINuvlo_on-Vuvlo_on)","v":333.33333333333331},"kΩ",{"$f":"'Standard Value Calculator'!J17","v":332},"kΩ",{"$f":"IF(F183=\"N/A\",\"N/A\",D184)","v":332},{"$f":"IF(G183=\"N/A\",\"N/A\",D184&\"kΩ\")","v":"332kΩ"}]
[]
["VINUVLO_ON_ACTUAL",{"$f":"(D183+D184)/D184*Vuvlo_on","v":6.0180722891566267},"V"]
["VINUVLO_OFF_ACTUAL",{"$f":"(D183+D184)/D184*Vuvlo_off","v":5.6168674698795176},"V"]
[]
["RPG",20,"kΩ"]
[]
[]
["Step 8: FB Divider"]
["Pi",3.1415926500000002,null,"p"]
["Toff_Vinmax",{"$f":"(1-Don_Vinmax_2)/Fsw","v":2.2754233645663198E-6},"sec"]
["Ton_Vinmin",{"$f":"IF(VIN_min>Vout, (1-Don_Vinmin_2)/Fsw, Don_Vinmin_2/Fsw)","v":2.1747790364745427E-6},"sec"]
[]
["Rfb1",{"$f":"'Design Converter'!E43*1000","v":453000},"W","Lower Feedback Resistance - chosen by user",null,null,null,null,1]
["Rfb2",{"$f":"IF(Vout=Vref,100000000,Vref*B197/((Vout-Vref)))","v":143052.63157894739},"W","Upper Feedback Resistance"]
["Rfb2_u",{"$f":"IF(Vout=Vref,\"N/A\",'Standard Value Calculator'!J10)","v":143000},"W","Std Value Upper Feedback Resistance"]
["Rfb",{"$f":"Rfb1_*Rfb2_u/(Rfb1_+Rfb2_u)","v":108689.59731543624},"W","Rfb1 || Rfb2_u"]
[null,{"$f":"1.2/Rfb2_u*(Rfb2_u+Rfb1_)","v":5.0013986013986012},"V"]
["Ifb",{"$f":"CHOOSE(MODE_VOUT, IF(Vout=5, 0.000007, 0.0000038), Vout/(Rfb1_+Rfb2_u))","v":8.3892617449664422E-6}]
[]
["Other Input Variables"]
["Rfets",0,"W","Series resistance due to FETs",null,null,null,{"$f":"_Don2*RdsonTop+Doff2*RdsonBot+B209*Vin^2*Fsw/2/(((Iripple1/SQRT(3))^2))","v":263.77900702892629}]
["Diode loss eq res",{"$f":"0.00000002*Fsw*0.6*4/Iripple1","v":0.11112432983284659}]
["Fet loss eq res",{"$f":"_Don2*RdsonTop+Doff2*RdsonBot","v":0.34185117187499997}]
["cap loss eq res",{"$f":"B209*Vin^2*Fsw/2/(((Iripple1/SQRT(3))^2))","v":263.43715585705127}]
["Sw cap",5.0000000000000001E-9]
[]
["Step 8: Efficiency"]
[]
["Design"]
["Ta",25,"°C","Ambient Temperature"]
["Components"]
["LTc",{"$f":"4000/1000000","v":4.0000000000000001E-3},"%/°C","Inductor DCR Temp Co"]
["θCA",40,"°C/W","Inductor Core to Ambient Thermal Resistance"]
["RCinEsr",{"$f":"RCinEsr","v":3.0000000000000001E-3},"W","Input Capacitor ESR"]
["Part Characteristics"]
["Vcc",{"$f":"IF(Vin>7.7,7.5,Vin-0.2)","v":7.5},"V"]
["Deadtime"]
["Deadtime",2E-8,"s","Total Deadtime",null,null,"20ns for LM5166"]
["IQ"]
["IQ ",1.0000000000000001E-5,"A","Quiescent Current Of Controller (Not Switching!)"]
[]
[]
["IC Power Disipation","Value","Units"]
["Power Dis",{"$f":"Efficiency!AZ106","v":0.59420337828422776},"W"]
["Temp rise",{"$f":"B228*ThetaJA","v":24.421758847481762},"°C"]
["Current (switching)",{"$f":"(Qg_Q1+Qg_Q2)*Fsw+Iq","v":{"$error":"#NAME?"}},"A"]
["Qrr Current",{"$f":"Qrr_Q2*Fsw","v":{"$error":"#NAME?"}},"A"]
["Diode Current",{"$f":"C232/Vin","v":{"$error":"#NAME?"}},{"$f":"Deadtime*Fsw*(Ipp/2)*(Vsd_Q1+Vsd_Q2)","v":{"$error":"#NAME?"}}]
["Total Application Switching IQ",{"$f":"SUM(B230:B232)","v":{"$error":"#NAME?"}},"A"]
[]
[]
["SCHEMATIC LABELS"]
[]
[]
[{"$f":"\"RUV1 = \"&'Design Converter'!E49&\"MΩ\"","v":"RUV1 = 1MΩ"},{"$f":"C275","v":"1MΩ"}]
[{"$f":"\"RUV2 = \"&'Design Converter'!E50&\"kΩ\"","v":"RUV2 = 332kΩ"},{"$f":"C276","v":"332kΩ"}]
[{"$f":"\"Rhys = \"&'Design Converter'!E52&\"kΩ\"","v":"Rhys = 5.61686746987952kΩ"},{"$f":"C277","v":{"$error":"#REF!"}}]
[]
[{"$f":"\"LF = \"&'Design Converter'!E17&\"µH\"","v":"LF = 68µH"},{"$f":"'Design Converter'!E17&\"µH\"","v":"68µH"}]
[{"$f":"\"Rdcr = \"&Rdcr*1000&\"mΩ\"","v":"Rdcr = 120mΩ"},{"$f":"Rdcr*1000&\"mΩ\"","v":"120mΩ"}]
[{"$f":"\"Rt = \"&'Design Converter'!I43&\"kΩ\"","v":"Rt = kΩ"},{"$f":"'Design Converter'!I43&\"kΩ\"","v":"kΩ"}]
[{"$f":"\"Css = \"&ROUND(Css_u*1000000000,1)&\"nF\"","v":{"$error":"#NAME?"}},{"$f":"ROUND(Css_u*1000000000,1)&\"nF\"","v":{"$error":"#NAME?"}}]
[]
["VIN",{"$f":"VIN_nom&\"V\"","v":"51.2V"}]
["VIN range",{"$f":"VIN_min&\"V...\"&VIN_max&\"V\"","v":"40V...58V"}]
[]
[{"$f":"\"VOUT = \"&'Design Converter'!E9&\"V\"","v":"VOUT = 5V"},{"$f":"'Design Converter'!E9&\"V\"","v":"5V"}]
[null,null,{"$f":"R30","v":"47"},{"$f":"ROUNDUP('Design Converter'!$E$24/C252,0)","v":1}]
[{"$f":"\"COUT = \"&'Design Converter'!$E$24&\"µF\"","v":"COUT = 33µF"},{"$f":"'Design Converter'!$E$24&\"µF\"","v":"33µF"},{"$f":"IF('Design Converter'!$E$24=OR(10, 22, 47, 100), 'Design Converter'!$E$24,C252)","v":"47"},{"$f":"IF(D252=1, \"\",B255)","v":""},{"$f":"D253&C253&\"µF\"","v":"47µF"},{"$f":"C253&\"µF\"","v":"47µF"}]
["Capacitance per component (Cout)",{"$f":"C252&\"µF\"","v":"47µF"}]
["# of output caps",{"$f":"D252&\" x \"","v":"1 x "}]
[]
["CIN",{"$f":"Cin*1000000&\"µF\"","v":"2.2µF"}]
["Capacitance per component (Cin)",{"$f":"\"2.2µF\"","v":"2.2µF"}]
["# of input caps",{"$f":"ROUNDUP(Cin*1000000/2.2,0)&\" x \"","v":"1 x "}]
[]
["Fixed VOUT?",{"$f":"IF(MODE_VOUT=1, \"YES\", \"NO\")","v":"NO"}]
["FB resistor ref des shown or not?",{"$f":"IF(MODE_VOUT=2, \"YES\", \"NO\")","v":"YES"},{"$f":"IF(MODE_VOUT=2, \"R1\", \"\")","v":"R1"},{"$f":"IF(MODE_VOUT=2, \"R2\", \"\")","v":"R2"}]
[{"$f":"\"RFB1 = \"&'Design Converter'!E43&\"kΩ\"","v":"RFB1 = 453kΩ"},{"$f":"'Design Converter'!E43&\"kΩ\"","v":"453kΩ"},{"$f":"IF(MODE=1,'Design Converter'!E43&\"kΩ\", \"\")","v":""}]
[{"$f":"\"RFB2 = \"&IF(Vout=Vref,\"OPEN\",'Design Converter'!E44&\"kΩ\")","v":"RFB2 = 143kΩ"},{"$f":"IF(Vout=Vref,\"OPEN\",Rfb2_u/1000&\"kΩ\")","v":"143kΩ"},{"$f":"IF(MODE=1, IF(Vout=Vref, \"OPEN\",Rfb2_u/1000&\"kΩ\" ), \"\")","v":""}]
[]
[]
["Show Rt resistor ref des?",{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), \"YES\", \"NO\")","v":"YES"},{"$f":"IF(MODE=4,\"\", \"Rt\")","v":"Rt"}]
["Rt",{"$f":"IF(MODE=4, \"\", 'Standard Value Calculator'!J4/1000&\"kΩ\")","v":"30.9kΩ"}]
[]
["Show ESR resistor ref des?",{"$f":"IF(OR(MODE=3, MODE=4), \"NO\", \"YES\")","v":"NO"},{"$f":"IF(OR(MODE=3, MODE=4),\"\",\"Resr\")","v":""}]
[{"$f":"\"RESR = \"&'Design Converter'!E26&\"mΩ\"","v":"RESR = 0.005mΩ"},{"$f":"IF(OR(MODE=3,MODE=4), \"\", 'Design Converter'!E26&\"Ω\")","v":""},null,null,null,{"$f":"B120","v":0.48625735344660326}]
["Resr",{"$f":"IF(MODE=1, \">\"&ROUND(B130,3), IF(MODE=2,  \">\"&ROUND(B131,3),IF(MODE=3,ROUND(B119,3),\"\")))","v":0.14599999999999999}]
[]
["Adjustable UVLO?",{"$f":"IF(MODE_UVLO=1, \"YES\", \"NO\")","v":"YES"},{"$f":"IF(MODE_UVLO=1,\"Ren1\", \"\")","v":"Ren1"},{"$f":"IF(MODE_UVLO=1, \"Ren2\", \"\")","v":"Ren2"},{"$f":"IF(MODE_UVLO=1, \"Rhys\", \"\")","v":"Rhys"},"Value","Units","BOM display"]
[{"$f":"\"RUV1 = \"&C275","v":"RUV1 = 1MΩ"},{"$f":"'Design Converter'!E49&\" MΩ\"","v":"1 MΩ"},{"$f":"IF(MODE_UVLO=1,'Design Converter'!E49&\"MΩ\", \"\")","v":"1MΩ"},null,null,{"$f":"IF(MODE_UVLO=1,'Design Converter'!E49, \"\")","v":1},{"$f":"IF(MODE_UVLO=1,\"MΩ\", \"\")","v":"MΩ"},{"$f":"IF(MODE_UVLO=1,'Design Converter'!E49&\"M\", \"\")","v":"1M"}]
[{"$f":"\"RUV2 = \"&C276","v":"RUV2 = 332kΩ"},{"$f":"IF(D184>=1000, D184/1000&\" MΩ\", D184&\" kΩ\")","v":"332 kΩ"},{"$f":"IF(MODE_UVLO=1, IF(D184<1, D184*1000&\"Ω\", IF(D184<1000, D184&\"kΩ\", D184/1000&\"MΩ\")), \"\")","v":"332kΩ"},null,null,{"$f":"IF(MODE_UVLO=1, IF(D184<1, D184*1000, IF(D184<1000, D184, D184/1000)), \"\")","v":332},{"$f":"IF(MODE_UVLO=1, IF(D184<1, \"Ω\", IF(D184<1000,\"kΩ\", \"MΩ\")), \"\")","v":"kΩ"},{"$f":"IF(MODE_UVLO=1, IF(D184<1, D184*1000, IF(D184<1000, D184&\"k\", D184/1000&\"M\")), \"\")","v":"332k"}]
[{"$f":"\"RHYS = \"&C277","v":{"$error":"#REF!"}},{"$f":"IF(#REF!<1000,#REF!& \" kΩ\",#REF!& \" MΩ\")","v":{"$error":"#REF!"}},{"$f":"IF(MODE_UVLO=1, IF(#REF!<1,#REF!* 1000&\"Ω\", IF(#REF!<1000,#REF!& \"kΩ\",#REF!/ 1000&\"MΩ\")), \"\")","v":{"$error":"#REF!"}},null,null,{"$f":"IF(MODE_UVLO=1, IF(#REF!<1,#REF!* 1000, IF(#REF!<1000,#REF!,#REF!/ 1000)), \"\")","v":{"$error":"#REF!"}},{"$f":"IF(MODE_UVLO=1, IF(#REF!<1, \"Ω\", IF(#REF!<1000,\"kΩ\", \"MΩ\")), \"\")","v":{"$error":"#REF!"}},{"$f":"IF(MODE_UVLO=1, IF(#REF!<1,#REF!* 1000, IF(#REF!<1000,#REF!& \"k\",#REF!& \"M\")), \"\")","v":{"$error":"#REF!"}}]
[]
[{"$f":"\"Css = \"&Css*1000000000&\"nF\"","v":{"$error":"#NAME?"}},{"$f":"Css*1000000000&\"nF\"","v":{"$error":"#NAME?"}}]
["Cbst",{"$f":"\"2.2nF\"","v":"2.2nF"},null,{"$f":"B280","v":"2.2nF"}]
[]
[]
["Rset resistor ref des?",{"$f":"IF(MODE_RSET=2, \"YES\", \"NO\")","v":"NO"},{"$f":"IF(MODE_RSET=2, \"R3\", \"\")","v":""},null,null,{"$f":"MODE_RSET","v":1}]
["Rset",{"$f":"IF(MODE_RSET=2, C284&\"kΩ\", \"\")","v":""},{"$f":"IF(MODE_ILIM=3,100,IF(MODE_ILIM=2,56.2,IF(MODE_ILIM=4,24.9,0)))","v":{"$error":"#REF!"}}]
[]
[]
["Rpgood","100kΩ"]
[]
["Cff / Cb?",{"$f":"IF(MODE=2, \"Cff\", IF(MODE=3,\"Cb\",\"\"))","v":"Cb"}]
[{"$f":"\"Cff / Cb=\"&B290","v":"Cff / Cb=56pF"},{"$f":"IF(OR(MODE=2,MODE=3),B141&\"pF\",\"\")","v":"56pF"}]
[]
["Ca?",{"$f":"IF(MODE=3, \"Ca\",\"\")","v":"Ca"},null,{"$f":"Ca","v":2.1999999999999998E-9},{"$f":"Ton_Vinmin","v":2.1747790364745427E-6}]
["Ca=",{"$f":"IF(MODE=3,B145&\"pF\",\"\")","v":"2200pF"}]
[]
["Ra?",{"$f":"IF(MODE=3, \"Ra\",\"\")","v":"Ra"},"Injected Ripple"]
["Ra=",{"$f":"IF(MODE=3,Ra&\"kΩ\",\"\")","v":"255kΩ"},{"$f":"(VIN_nom-Vout)*Ton_Vin_nom/(Ra*Ca)/1000","v":2.010569852941177E-2},{"$f":"ROUNDUP(1000*C296,0)","v":21},null,{"$f":"IF(MODE=3,Ra&\"k\",\"\")","v":"255k"}]
[]
["Lf(emi)",{"$f":"M148&\"µH\"","v":"22µH"}]
["Cf(emi)",{"$f":"M149&\"µF\"","v":"4.7µF"}]
["Df(emi)",{"$f":"M150&\"µF\"","v":"10µF"}]
[]
["Full-load efficiency",{"$f":"ROUND(Efficiency!CE106,1)&\"%\"","v":"77.5%"}]
["Full-load efficiency",{"$f":"ROUND(Efficiency!CE107,1)&\"%\"","v":"77.5%"}]
["10% load efficiency",{"$f":"ROUND(Efficiency!CE16,1)&\"%\"","v":"52.3%"},"linear scale only"]
["1% load efficiency",{"$f":"ROUND(Efficiency!CE56,1)&\"%\"","v":"71.8%"},"log scale only"]
[]
["Blank out",{"$f":"IF(C307=\"y\",\"\",\"|\")","v":"|"},"n"]
[]
["OUTPUT CURRENT",{"$f":"'Design Converter'!$E$10&\"A\"","v":"0.5A"}]
[]
["VIN ",2]
["RT",5]
["EN",7]
["PGOOD",6]
["SS",4]
["ILIM",3]
["GND",10]
["FB",8]
["SW",1]
["HYS",9]

{"sheet":"Standard Value Calculator","index":8,"n_rows":159,"n_cols":11,"rows_kept":159,"cut":false,"hidden":true,"merged":[]}
[]
["Capacitors","Css","Cout","Cin","Cb"]
["Inputs",{"$f":"Css","v":{"$error":"#NAME?"}},{"$f":"Cout","v":3.3000000000000003E-5},{"$f":"Cin","v":2.2000000000000001E-6},{"$f":"Cb","v":0},null,null,"Resistors","inputs","Standard Result"]
["Standard Result",{"$f":"SUM(B6:B158)/1000000000000","v":{"$error":"#NAME?"}},{"$f":"SUM(C6:C158)/1000000000000","v":3.3000000000000003E-5},{"$f":"SUM(D6:D158)/1000000000000","v":2.2000000000000001E-6},{"$f":"IF(E3=\"OPEN\",\"OPEN\",SUM(E6:E158)/1000000000000)","v":0},null,null,"Rt",{"$f":"Rt","v":31250},{"$f":"IF(I4>(INT(0.5+100*POWER(10,IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))/96))*POWER(10,INT(LOG(I4))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))+1)/96))*POWER(10,INT(LOG(I4))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))+1)/96))*POWER(10,INT(LOG(I4))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))/96))*POWER(10,INT(LOG(I4))-2))","v":30900},"Ω"]
["(pF)"]
[0.47,{"$f":"IF(IF((B$3*10^12-$A7)*(B$3*10^12-$A6)*-1<0,0,1)*IF(ABS(B$3*10^12-$A7)>(B$3*10^12-$A6),$A6,$A7)=B7,0,IF((B$3*10^12-$A7)*(B$3*10^12-$A6)*-1<0,0,1)*IF(ABS(B$3*10^12-$A7)>(B$3*10^12-$A6),$A6,$A7))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A7)*(C$3*10^12-$A6)*-1<0,0,1)*IF(ABS(C$3*10^12-$A7)>(C$3*10^12-$A6),$A6,$A7)=C7,0,IF((C$3*10^12-$A7)*(C$3*10^12-$A6)*-1<0,0,1)*IF(ABS(C$3*10^12-$A7)>(C$3*10^12-$A6),$A6,$A7))","v":0},{"$f":"IF(IF((D$3*10^12-$A7)*(D$3*10^12-$A6)*-1<0,0,1)*IF(ABS(D$3*10^12-$A7)>(D$3*10^12-$A6),$A6,$A7)=D7,0,IF((D$3*10^12-$A7)*(D$3*10^12-$A6)*-1<0,0,1)*IF(ABS(D$3*10^12-$A7)>(D$3*10^12-$A6),$A6,$A7))","v":0},{"$f":"IF(IF((E$3*10^12-$A7)*(E$3*10^12-$A6)*-1<0,0,1)*IF(ABS(E$3*10^12-$A7)>(E$3*10^12-$A6),$A6,$A7)=E7,0,IF((E$3*10^12-$A7)*(E$3*10^12-$A6)*-1<0,0,1)*IF(ABS(E$3*10^12-$A7)>(E$3*10^12-$A6),$A6,$A7))","v":0},null,null,"Rshunt",{"$f":"Rshunt","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},"Ω"]
[0.56000000000000005,{"$f":"IF(IF((B$3*10^12-$A8)*(B$3*10^12-$A7)*-1<0,0,1)*IF(ABS(B$3*10^12-$A8)>(B$3*10^12-$A7),$A7,$A8)=B8,0,IF((B$3*10^12-$A8)*(B$3*10^12-$A7)*-1<0,0,1)*IF(ABS(B$3*10^12-$A8)>(B$3*10^12-$A7),$A7,$A8))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A8)*(C$3*10^12-$A7)*-1<0,0,1)*IF(ABS(C$3*10^12-$A8)>(C$3*10^12-$A7),$A7,$A8)=C8,0,IF((C$3*10^12-$A8)*(C$3*10^12-$A7)*-1<0,0,1)*IF(ABS(C$3*10^12-$A8)>(C$3*10^12-$A7),$A7,$A8))","v":0},{"$f":"IF(IF((D$3*10^12-$A8)*(D$3*10^12-$A7)*-1<0,0,1)*IF(ABS(D$3*10^12-$A8)>(D$3*10^12-$A7),$A7,$A8)=D8,0,IF((D$3*10^12-$A8)*(D$3*10^12-$A7)*-1<0,0,1)*IF(ABS(D$3*10^12-$A8)>(D$3*10^12-$A7),$A7,$A8))","v":0},{"$f":"IF(IF((E$3*10^12-$A8)*(E$3*10^12-$A7)*-1<0,0,1)*IF(ABS(E$3*10^12-$A8)>(E$3*10^12-$A7),$A7,$A8)=E8,0,IF((E$3*10^12-$A8)*(E$3*10^12-$A7)*-1<0,0,1)*IF(ABS(E$3*10^12-$A8)>(E$3*10^12-$A7),$A7,$A8))","v":0},null,null,"Rc1ea",{"$f":"Rcea1","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},"Ω"]
[0.68,{"$error":"#NAME?"},0,0,0]
[0.82,{"$error":"#NAME?"},0,0,0,null,null,"Rfb1",{"$f":"Rfb1_","v":453000},453000,"Ω"]
[1,{"$error":"#NAME?"},0,0,0,null,null,"Rfb2",{"$f":"Rfb2_","v":143052.63157894739},{"$f":"IF(I10=\"OPEN\",\"OPEN\",IF(I10>(INT(0.5+100*POWER(10,IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))/96))*POWER(10,INT(LOG(I10))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))+1)/96))*POWER(10,INT(LOG(I10))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))+1)/96))*POWER(10,INT(LOG(I10))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))/96))*POWER(10,INT(LOG(I10))-2)))","v":143000},"Ω"]
[1.2,{"$error":"#NAME?"},0,0,0]
[1.5,{"$error":"#NAME?"},0,0,0]
[1.8,{"$error":"#NAME?"},0,0,0,null,null,"Rs",{"$f":"Rs_ideal*1000","v":{"$error":"#NAME?"}},{"$f":"IF(I13=0,0,IF(I13>(INT(0.5+100*POWER(10,IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))/96))*POWER(10,INT(LOG(I13))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))+1)/96))*POWER(10,INT(LOG(I13))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))+1)/96))*POWER(10,INT(LOG(I13))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))/96))*POWER(10,INT(LOG(I13))-2)))","v":{"$error":"#NAME?"}},"mΩ"]
[2.2000000000000002,{"$f":"IF(IF((B$3*10^12-$A15)*(B$3*10^12-$A14)*-1<0,0,1)*IF(ABS(B$3*10^12-$A15)>(B$3*10^12-$A14),$A14,$A15)=B15,0,IF((B$3*10^12-$A15)*(B$3*10^12-$A14)*-1<0,0,1)*IF(ABS(B$3*10^12-$A15)>(B$3*10^12-$A14),$A14,$A15))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A15)*(C$3*10^12-$A14)*-1<0,0,1)*IF(ABS(C$3*10^12-$A15)>(C$3*10^12-$A14),$A14,$A15)=C15,0,IF((C$3*10^12-$A15)*(C$3*10^12-$A14)*-1<0,0,1)*IF(ABS(C$3*10^12-$A15)>(C$3*10^12-$A14),$A14,$A15))","v":0},{"$f":"IF(IF((D$3*10^12-$A15)*(D$3*10^12-$A14)*-1<0,0,1)*IF(ABS(D$3*10^12-$A15)>(D$3*10^12-$A14),$A14,$A15)=D15,0,IF((D$3*10^12-$A15)*(D$3*10^12-$A14)*-1<0,0,1)*IF(ABS(D$3*10^12-$A15)>(D$3*10^12-$A14),$A14,$A15))","v":0},{"$f":"IF(IF((E$3*10^12-$A15)*(E$3*10^12-$A14)*-1<0,0,1)*IF(ABS(E$3*10^12-$A15)>(E$3*10^12-$A14),$A14,$A15)=E15,0,IF((E$3*10^12-$A15)*(E$3*10^12-$A14)*-1<0,0,1)*IF(ABS(E$3*10^12-$A15)>(E$3*10^12-$A14),$A14,$A15))","v":0},null,null,"Cslope_ideal",{"$f":"Cslope_ideal","v":{"$error":"#NAME?"}},{"$f":"#REF!*1000000000000","v":{"$error":"#REF!"}},"pF"]
[2.7,{"$error":"#NAME?"},0,0,0]
[3.3,{"$error":"#NAME?"},0,0,0,null,null,"Ruv1",{"$f":"Ruvlo1","v":1000},{"$f":"IF(I16=\"OPEN\",\"OPEN\",IF(I16>(INT(0.5+100*POWER(10,IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))/96))*POWER(10,INT(LOG(I16))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))+1)/96))*POWER(10,INT(LOG(I16))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))+1)/96))*POWER(10,INT(LOG(I16))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))/96))*POWER(10,INT(LOG(I16))-2)))","v":1000},"kΩ"]
[3.9,{"$error":"#NAME?"},0,0,0,null,null,"Ruv2",{"$f":"Ruvlo2","v":333.33333333333331},{"$f":"IF(I17=\"OPEN\",\"OPEN\",IF(I17>(INT(0.5+100*POWER(10,IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))/96))*POWER(10,INT(LOG(I17))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))+1)/96))*POWER(10,INT(LOG(I17))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))+1)/96))*POWER(10,INT(LOG(I17))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))/96))*POWER(10,INT(LOG(I17))-2)))","v":332},"kΩ"]
[4.7,{"$error":"#NAME?"},0,0,0,null,null,"Rhys",{"$f":"Rhys","v":{"$error":"#NAME?"}},{"$f":"IF(I18=\"OPEN\",\"OPEN\",IF(I18>(INT(0.5+100*POWER(10,IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))/96))*POWER(10,INT(LOG(I18))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))+1)/96))*POWER(10,INT(LOG(I18))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))+1)/96))*POWER(10,INT(LOG(I18))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))/96))*POWER(10,INT(LOG(I18))-2)))","v":{"$error":"#NAME?"}},"kΩ"]
[5.6,{"$error":"#NAME?"},0,0,0]
[6.8,{"$error":"#NAME?"},0,0,0,null,null,"Ra",{"$f":"'Variable Mgmt'!D147","v":256.34765625000006},{"$f":"IF(I20=\"OPEN\",\"OPEN\",IF(I20>(INT(0.5+100*POWER(10,IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))/96))*POWER(10,INT(LOG(I20))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))+1)/96))*POWER(10,INT(LOG(I20))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))+1)/96))*POWER(10,INT(LOG(I20))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))/96))*POWER(10,INT(LOG(I20))-2)))","v":255},"kΩ"]
[8.1999999999999993,{"$error":"#NAME?"},0,0,0]
[10,{"$error":"#NAME?"},0,0,0]
[12,{"$error":"#NAME?"},0,0,0]
[15,{"$error":"#NAME?"},0,0,0]
[18,{"$error":"#NAME?"},0,0,0]
[22,{"$error":"#NAME?"},0,0,0]
[27,{"$error":"#NAME?"},0,0,0]
[33,{"$error":"#NAME?"},0,0,0]
[39,{"$error":"#NAME?"},0,0,0]
[47,{"$error":"#NAME?"},0,0,0]
[56,{"$error":"#NAME?"},0,0,0]
[68,{"$error":"#NAME?"},0,0,0]
[82,{"$error":"#NAME?"},0,0,0]
[{"$f":"A22*10","v":100},{"$error":"#NAME?"},0,0,0]
[{"$f":"A23*10","v":120},{"$error":"#NAME?"},0,0,0]
[150,{"$error":"#NAME?"},0,0,0]
[180,{"$error":"#NAME?"},0,0,0]
[220,{"$error":"#NAME?"},0,0,{"$f":"IF(IF((E$3*10^12-$A39)*(E$3*10^12-$A38)*-1<0,0,1)*IF(ABS(E$3*10^12-$A39)>(E$3*10^12-$A38),$A38,$A39)=E39,0,IF((E$3*10^12-$A39)*(E$3*10^12-$A38)*-1<0,0,1)*IF(ABS(E$3*10^12-$A39)>(E$3*10^12-$A38),$A38,$A39))","v":0}]
[270,{"$error":"#NAME?"},0,0,0]
[330,{"$error":"#NAME?"},0,0,0]
[390,{"$error":"#NAME?"},0,0,0]
[470,{"$error":"#NAME?"},0,0,0]
[560,{"$error":"#NAME?"},0,0,0]
[680,{"$error":"#NAME?"},0,0,0]
[{"$f":"A33*10","v":820},{"$error":"#NAME?"},0,0,0]
[1000,{"$error":"#NAME?"},0,0,0]
[1200,{"$error":"#NAME?"},0,0,0]
[1500,{"$error":"#NAME?"},0,0,0]
[1800,{"$error":"#NAME?"},0,0,0]
[2200,{"$error":"#NAME?"},0,0,0]
[2700,{"$error":"#NAME?"},0,0,0]
[3300,{"$error":"#NAME?"},0,0,0]
[3900,{"$error":"#NAME?"},0,0,0]
[4700,{"$error":"#NAME?"},0,0,0]
[5600,{"$error":"#NAME?"},0,0,0]
[6800,{"$error":"#NAME?"},0,0,0]
[8200,{"$error":"#NAME?"},0,0,0]
[10000,{"$error":"#NAME?"},0,0,0]
[12000,{"$error":"#NAME?"},0,0,0]
[15000,{"$error":"#NAME?"},0,0,0]
[18000,{"$error":"#NAME?"},0,0,0]
[22000,{"$error":"#NAME?"},0,0,0]
[27000,{"$error":"#NAME?"},0,0,0]
[33000,{"$error":"#NAME?"},0,0,0]
[39000,{"$error":"#NAME?"},0,0,0]
[47000,{"$error":"#NAME?"},0,0,0]
[56000,{"$error":"#NAME?"},0,0,0]
[68000,{"$error":"#NAME?"},0,0,0]
[82000,{"$error":"#NAME?"},0,0,0]
[100000,{"$error":"#NAME?"},{"$f":"IF(IF((C$3*10^12-$A71)*(C$3*10^12-$A70)*-1<0,0,1)*IF(ABS(C$3*10^12-$A71)>(C$3*10^12-$A70),$A70,$A71)=C71,0,IF((C$3*10^12-$A71)*(C$3*10^12-$A70)*-1<0,0,1)*IF(ABS(C$3*10^12-$A71)>(C$3*10^12-$A70),$A70,$A71))","v":0},{"$f":"IF(IF((D$3*10^12-$A71)*(D$3*10^12-$A70)*-1<0,0,1)*IF(ABS(D$3*10^12-$A71)>(D$3*10^12-$A70),$A70,$A71)=D71,0,IF((D$3*10^12-$A71)*(D$3*10^12-$A70)*-1<0,0,1)*IF(ABS(D$3*10^12-$A71)>(D$3*10^12-$A70),$A70,$A71))","v":0},{"$f":"IF(IF((E$3*10^12-$A71)*(E$3*10^12-$A70)*-1<0,0,1)*IF(ABS(E$3*10^12-$A71)>(E$3*10^12-$A70),$A70,$A71)=E71,0,IF((E$3*10^12-$A71)*(E$3*10^12-$A70)*-1<0,0,1)*IF(ABS(E$3*10^12-$A71)>(E$3*10^12-$A70),$A70,$A71))","v":0}]
[120000,{"$f":"IF(IF((B$3*10^12-$A72)*(B$3*10^12-$A71)*-1<0,0,1)*IF(ABS(B$3*10^12-$A72)>(B$3*10^12-$A71),$A71,$A72)=B72,0,IF((B$3*10^12-$A72)*(B$3*10^12-$A71)*-1<0,0,1)*IF(ABS(B$3*10^12-$A72)>(B$3*10^12-$A71),$A71,$A72))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A72)*(C$3*10^12-$A71)*-1<0,0,1)*IF(ABS(C$3*10^12-$A72)>(C$3*10^12-$A71),$A71,$A72)=C72,0,IF((C$3*10^12-$A72)*(C$3*10^12-$A71)*-1<0,0,1)*IF(ABS(C$3*10^12-$A72)>(C$3*10^12-$A71),$A71,$A72))","v":0},{"$f":"IF(IF((D$3*10^12-$A72)*(D$3*10^12-$A71)*-1<0,0,1)*IF(ABS(D$3*10^12-$A72)>(D$3*10^12-$A71),$A71,$A72)=D72,0,IF((D$3*10^12-$A72)*(D$3*10^12-$A71)*-1<0,0,1)*IF(ABS(D$3*10^12-$A72)>(D$3*10^12-$A71),$A71,$A72))","v":0},0]
[150000,{"$error":"#NAME?"},0,0,0]
[180000,{"$error":"#NAME?"},0,0,0]
[220000,{"$error":"#NAME?"},0,0,0]
[270000,{"$error":"#NAME?"},0,0,0]
[330000,{"$error":"#NAME?"},0,0,0]
[390000,{"$error":"#NAME?"},0,0,0]
[470000,{"$error":"#NAME?"},0,0,0]
[560000,{"$error":"#NAME?"},0,0,0]
[680000,{"$error":"#NAME?"},0,0,0]
[820000,{"$error":"#NAME?"},0,0,0]
[1000000,{"$error":"#NAME?"},0,0,0]
[1200000,{"$error":"#NAME?"},0,0,0]
[1500000,{"$error":"#NAME?"},0,0,0]
[1800000,{"$error":"#NAME?"},0,0,0]
[2200000,{"$error":"#NAME?"},0,2200000,0]
[2700000,{"$error":"#NAME?"},0,0,0]
[3300000,{"$error":"#NAME?"},0,0,0]
[3900000,{"$error":"#NAME?"},0,0,0]
[4700000,{"$error":"#NAME?"},0,0,0]
[5600000,{"$error":"#NAME?"},0,0,0]
[6800000,{"$error":"#NAME?"},0,0,0]
[8200000,{"$error":"#NAME?"},0,0,0]
[10000000,{"$error":"#NAME?"},0,0,0]
[12000000,{"$error":"#NAME?"},0,0,0]
[15000000,{"$error":"#NAME?"},0,0,0]
[18000000,{"$error":"#NAME?"},0,0,0]
[22000000,{"$error":"#NAME?"},0,0,0]
[{"$f":"A87*10","v":27000000},{"$error":"#NAME?"},0,0,0]
[33000000,{"$error":"#NAME?"},33000000,0,0]
[39000000,{"$error":"#NAME?"},0,0,0]
[47000000,{"$error":"#NAME?"},0,0,{"$f":"IF(IF((E$3*10^12-$A103)*(E$3*10^12-$A102)*-1<0,0,1)*IF(ABS(E$3*10^12-$A103)>(E$3*10^12-$A102),$A102,$A103)=E103,0,IF((E$3*10^12-$A103)*(E$3*10^12-$A102)*-1<0,0,1)*IF(ABS(E$3*10^12-$A103)>(E$3*10^12-$A102),$A102,$A103))","v":0}]
[56000000,{"$error":"#NAME?"},0,{"$f":"IF(IF((D$3*10^12-$A104)*(D$3*10^12-$A103)*-1<0,0,1)*IF(ABS(D$3*10^12-$A104)>(D$3*10^12-$A103),$A103,$A104)=D104,0,IF((D$3*10^12-$A104)*(D$3*10^12-$A103)*-1<0,0,1)*IF(ABS(D$3*10^12-$A104)>(D$3*10^12-$A103),$A103,$A104))","v":0},0]
[68000000,{"$error":"#NAME?"},0,0,0]
[82000000,{"$error":"#NAME?"},0,0,0]
[100000000,{"$error":"#NAME?"},0,0,0]
[120000000,{"$error":"#NAME?"},0,0,0]
[150000000,{"$error":"#NAME?"},0,0,0]
[180000000,{"$error":"#NAME?"},0,0,0]
[220000000,{"$error":"#NAME?"},0,0,0]
[270000000,{"$error":"#NAME?"},0,0,0]
[330000000,{"$error":"#NAME?"},0,0,0]
[390000000,{"$error":"#NAME?"},0,0,0]
[470000000,{"$error":"#NAME?"},0,0,0]
[560000000,{"$error":"#NAME?"},0,0,0]
[680000000,{"$error":"#NAME?"},0,0,0]
[820000000,{"$error":"#NAME?"},0,0,0]
[1000000000,{"$error":"#NAME?"},0,0,0]
[1200000000,{"$error":"#NAME?"},0,0,0]
[1500000000,{"$error":"#NAME?"},0,0,0]
[1800000000,{"$error":"#NAME?"},0,0,0]
[2200000000,{"$error":"#NAME?"},0,0,0]
[2700000000,{"$error":"#NAME?"},0,0,0]
[3300000000,{"$error":"#NAME?"},0,0,0]
[3900000000,{"$error":"#NAME?"},0,0,0]
[4700000000,{"$error":"#NAME?"},0,0,0]
[5600000000,{"$error":"#NAME?"},0,0,0]
[6800000000,{"$error":"#NAME?"},0,0,0]
[8200000000,{"$error":"#NAME?"},0,0,0]
[10000000000,{"$error":"#NAME?"},0,0,0]
[12000000000,{"$error":"#NAME?"},0,0,0]
[15000000000,{"$error":"#NAME?"},0,0,0]
[18000000000,{"$error":"#NAME?"},0,0,0]
[22000000000,{"$error":"#NAME?"},{"$f":"IF(IF((C$3*10^12-$A135)*(C$3*10^12-$A134)*-1<0,0,1)*IF(ABS(C$3*10^12-$A135)>(C$3*10^12-$A134),$A134,$A135)=C135,0,IF((C$3*10^12-$A135)*(C$3*10^12-$A134)*-1<0,0,1)*IF(ABS(C$3*10^12-$A135)>(C$3*10^12-$A134),$A134,$A135))","v":0},0,{"$f":"IF(IF((E$3*10^12-$A135)*(E$3*10^12-$A134)*-1<0,0,1)*IF(ABS(E$3*10^12-$A135)>(E$3*10^12-$A134),$A134,$A135)=E135,0,IF((E$3*10^12-$A135)*(E$3*10^12-$A134)*-1<0,0,1)*IF(ABS(E$3*10^12-$A135)>(E$3*10^12-$A134),$A134,$A135))","v":0}]
[27000000000,{"$f":"IF(IF((B$3*10^12-$A136)*(B$3*10^12-$A135)*-1<0,0,1)*IF(ABS(B$3*10^12-$A136)>(B$3*10^12-$A135),$A135,$A136)=B136,0,IF((B$3*10^12-$A136)*(B$3*10^12-$A135)*-1<0,0,1)*IF(ABS(B$3*10^12-$A136)>(B$3*10^12-$A135),$A135,$A136))","v":{"$error":"#NAME?"}},0,0,0]
[33000000000,{"$error":"#NAME?"},0,0,0]
[39000000000,{"$error":"#NAME?"},0,0,0]
[47000000000,{"$error":"#NAME?"},0,0,0]
[56000000000,{"$error":"#NAME?"},0,0,0]
[68000000000,{"$error":"#NAME?"},0,0,0]
[82000000000,{"$error":"#NAME?"},0,0,0]
[100000000000,{"$error":"#NAME?"},0,0,0]
[120000000000,{"$error":"#NAME?"},0,0,0]
[150000000000,{"$error":"#NAME?"},0,0,0]
[180000000000,{"$error":"#NAME?"},0,0,0]
[220000000000,{"$error":"#NAME?"},0,0,0]
[270000000000,{"$error":"#NAME?"},0,0,0]
[330000000000,{"$error":"#NAME?"},0,0,0]
[390000000000,{"$error":"#NAME?"},0,0,0]
[470000000000,{"$error":"#NAME?"},0,0,0]
[560000000000,{"$error":"#NAME?"},0,0,0]
[680000000000,{"$error":"#NAME?"},0,0,0]
[820000000000,{"$error":"#NAME?"},0,0,0]
[1000000000000,{"$error":"#NAME?"},0,0,0]
[1200000000000,{"$error":"#NAME?"},0,0,0]
[1500000000000,{"$error":"#NAME?"},0,0,0]
[1800000000000,{"$error":"#NAME?"},0,0,0]
[2200000000000,{"$error":"#NAME?"},0,0,0]
[2700000000000,{"$error":"#NAME?"},2700000000000,2700000000000,2700000000000]

{"sheet":"Efficiency","index":9,"n_rows":114,"n_cols":88,"rows_kept":114,"cut":false,"hidden":true,"merged":[[0,0,2,4],[1,6,1,7],[3,0,3,4],[3,10,3,21]]}
["LM5164 (COT) Efficiency Calculator"]
[null,null,null,null,null,null,"TERMS OF USE",null,null,{"$f":"CoutEsr","v":5.0000000000000001E-3}]
[]
[null,null,null,null,null,null,null,"Currents",null,null,"Miscellaneous",null,null,null,null,null,null,null,null,null,null,null,"Inductor",null,null,null,"Cout",null,null,"Cin",null,null,"High-side MOSFET Losses ",null,null,null,null,null,null,null,null,"Low-side MOSFET Losses ",null,null,"Diode",null,null,null,null,null,null,null,"RESULTS"]
["Input Parameters",null,null,null,null,null,null,"Step","Iout (A)","Ripple Current pk-pk (A)","Peak Current (A)","Valley Current (A)","VOUT Hysteresis +Undershoot (2us Delay) (mV)","Vout Rise per Pulse (mV)","Number of Pulses in DCM","VOUT Ripple (mV)","Off Time (sec)","Duty Cycle","Switching Frequency (Hz)","Active Mode Duration (sec)","Sleep Mode Duration (sec)","Operating Quiescent Current (A)","Irms (A)","Inductor DCR Loss @ 25°C (W)","Inductor Core Loss  (W)","Total Inductor Loss (W)","Irms (A)","Cout ESR Loss (W)","Total Cout Loss (W)","Irms (A)","Cin ESR Loss (W)","Total Cin Loss (W)","Irms (A)","Rdson HS Loss @ 25°C (W)","HS Gate Qg Loss (W)     ","SW Rise Time (ns)","SW Fall Time (ns)","HS Switching  Loss (W)","Coss Loss (W)","Total HS FET AC Loss (W)","Total HS FET Loss (W)","Irms (A)","Rdson LS Loss @ 25°C (W)","LS Gate Qg Loss (W)","Reverse Recovery & Leakage Losses","DeadTime Loss @ 25°C (W)","Total LS FET AC Loss (W)","Total LS FET Loss (W)","Quiescent Loss (W)","LDO + Quiescent Loss (W)","Total Gate Drive Loss (W)","Total Power Loss in IC (W)","Total Converter Power Loss (W)","Pout (W)","EFF (%)","High-side MOSFET Rdson %","Low-side MOSFET Rdson %","Gate Drive (Qg) Loss from Vin %","High-side MOSFET AC Loss %","Reverse Recovery & Leakage Loss %","Deadtime Loss %","Low-side MOSFET AC Loss %","Inductor Cu Loss %","Inductor Core Loss %","Cin ESR %","Cout ESR %","LDO + Quiescent Current Loss %","Total Loss %","Overall Eff %","Overall Eff","Current (mA)","Keep for \"previous\" data series","Keep for \"previous\" data series","Frequency (kHz)",null,"Coss",null,"Total Power Loss in IC (mW)","LDO + Quiescent Loss (mW)","Total Inductor Loss (mW)",null,null,"Overall Eff","Total Power Loss in IC (W)","LDO + Quiescent Loss (mW)","Total Inductor Loss (mW)","Fsw (kHz)","Ripple (mV)"]
["Design","Input Value","Units","Std Units","Description",null,null,0.04,{"$f":"IF(PLOT_TYPE=1, H6/100*Iout, min_I*EXP(H6*rr/100))","v":2.0000000000000001E-4},{"$f":"IF(I6<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I6-Vout)/L*OnTime)","v":0.16563381487020262},{"$f":"IF(I6<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I6+((Vin-(Rdcr+RdsonTop)*J6-Vout)/L*OnTime)/2)","v":0.16563381487020262},{"$f":"IF(I6<Icrit, 0, I6-((Vin-(Rdcr+RdsonTop)*K6-Vout)/L*OnTime)/2)","v":0},{"$f":"1000*((((J6/2)-I6)*0.000002/Cout+Vout/306))","v":21.3469545801428},{"$f":"IF(I6<Icrit, 1000*SQRT((J6*CoutEsr)^2+(((J6/2)-I6)*(OnTime+OffTime)/Cout)^2), 1000*J6*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":6.0388748974240434},{"$f":"ROUNDUP(M6/N6,0)","v":4},{"$f":"IF(I6<Icrit, 1000*((N6/1000)*O6), 1000*J6*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":24.155499589696174},{"$f":"IF(I6<Icrit, L*J6/(Vout+J6/2*(RdsonBot+Rdcr)), L*J6/(Vout+I6*(RdsonBot+Rdcr)))","v":2.2369103433025619E-6},{"$f":"OnTime*S6","v":2.3763770672170735E-4},{"$f":"IF(I6<Icrit,I6/((OnTime+Q6)*J6/2),1/(OnTime+Q6))","v":973.36404673211325},{"$f":"IF(1/S6-OnTime-Q6>Tsleep, OnTime+Q6+Tsleep, 1/S6)","v":7.4810509683025621E-6},{"$f":"IF(1/S6-OnTime-Q6>Tsleep, 1/S6-OnTime-Q6-Tsleep, 0)","v":1.0198837909501058E-3},{"$f":"S6*(T6*Iq_active+U6*Iq_sleep)","v":1.4733160928805513E-5},{"$f":"IF(I6<Icrit,Iripple*SQRT((OnTime+OffTime)*S6/3), SQRT(I6^2+Iripple^2/12))","v":4.5780396453738376E-3},{"$f":"W6^2*Rdcr","v":2.5150136393537537E-6},{"$f":"Core_Loss/1000*S6/$S$106","v":2.3256989568906777E-4},{"$f":"(Y6+X6*(1+Ltc*(Ta-25)))/(1-X6*Ltc*ThetaCa)","v":2.3508500392714011E-4},{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q6)*S6)","v":2.3325356919394608E-3},{"$f":"RCoutEsr*AA6^2","v":2.7203613770857497E-8},{"$f":"AB6","v":2.7203613770857497E-8},{"$f":"SQRT($R6)*SQRT($I6^2*(1-R6)+(Iripple^2)/12)","v":7.317021571018557E-4},{"$f":"RCinEsr*AD6^2","v":1.6061641401225263E-9},{"$f":"AE6","v":1.6061641401225263E-9},{"$f":"IF(I6<Icrit,Iripple*SQRT((OnTime)*S6/3), SQRT(OnTime*S6*(I6^2+Iripple^2/12)))","v":1.4633913262803041E-3},{"$f":"RdsonTop*AG6^2","v":1.4712202374228776E-6},{"$f":"QgTop*S6*Vdd","v":3.9080566476294351E-6},{"$f":"20*VIN_nom/24","v":42.666666666666664},{"$f":"IF(I6<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I6+Iripple/2)*1000000000)","v":49.822614741301194},{"$f":"IF(I6<Icrit, Vin*(I6+Iripple/2)*AK6/1000000000/2*S6, Vin*(I6-Iripple/2)*AJ6/1000000000/2*S6 + Vin*(I6+Iripple/2)*AK6/1000000000/2*S6)","v":1.0231291504116249E-4},{"$f":"IF(I6<Icrit, Csw*(Vin)^2*S6/2, Csw*Vin^2*S6/2)","v":2.041292357332345E-4},{"$f":"AI6+AL6+AM6","v":3.1035020742202642E-4},{"$f":"(AI6+AL6+AM6+AH6*(1+RdsonTopTc*(Ta-25)))/(1-AH6*RdsonTopTc*ThetaJA)","v":3.1182151250676353E-4},{"$f":"IF(I6<Icrit,Iripple*SQRT((OffTime)*S6/3), SQRT(OffTime*S6*(I6^2+Iripple^2/12)))","v":4.3378488702100022E-3},{"$f":"RdsonBot*AP6^2","v":5.7203475775177864E-6},{"$f":"QgBot*S6*Vdd","v":1.0707004514053247E-5},{"$f":"IF(I6<Icrit, Vin*Idss*R6, QrrBot*(I6-Iripple/2)/1*S6*Vin+Vin*Idss*R6)","v":0},{"$f":"IF(I6<Icrit, dead1*S6*(I6+Iripple/2)*((I6+Iripple/2)*BDserR+VSD), dead1*S6*(I6+Iripple/2)*((I6+Iripple/2)*BDserR+VSD)+dead2*S6*(I6-Iripple/2)*((I6-Iripple/2)*BDserR+VSD))","v":1.2966863511547478E-6},{"$f":"AR6+AS6+AT6","v":1.2003690865207995E-5},{"$f":"(AR6+AS6+AT6+AQ6*(1+RdsonBotTc*(Ta-25)))/(1-AQ6*RdsonBotTc*ThetaJA)","v":1.7724057194393405E-5},{"$f":"Vin*V6+Vout*Ifb/0.8","v":8.0677072546088261E-4},{"$f":"(Vin-Vdd)*(S6*QgBot+S6*QgTop)+AW6","v":9.4181389059483063E-4},{"$f":"AI6+AR6","v":1.4615061161682682E-5},{"$f":"AO6+AV6+AX6+AY6","v":1.2859745214576703E-3},{"$f":"SUM(Z6,AC6,AF6,AZ6)","v":1.5210883351627214E-3},{"$f":"Vout*I6","v":1E-3},{"$f":"BB6/(BB6+BA6)","v":0.39665409024053727},{"$f":"(AO6-AN6)/($BB6+$BA6)","v":5.835991798526746E-4},{"$f":"(AV6-AU6)/($BB6+$BA6)","v":2.2690067021456403E-3},{"$f":"Vin*S6*(QgBot+QgTop)/($BB6+$BA6)","v":5.9362547598305844E-2},{"$f":"AN6/($BB6+$BA6)","v":0.12310167918094592},{"$f":"AS6/(BA6+BB6)","v":0},{"$f":"AT6/($BB6+$BA6)","v":5.1433594494460833E-4},{"$f":"AU6/($BB6+$BA6)","v":4.7613130796677243E-3},{"$f":"X6/($BB6+$BA6)","v":9.9759044706040586E-4},{"$f":"Y6/($BB6+$BA6)","v":9.2249800391883824E-2},{"$f":"(AF6)/($BB6+$BA6)","v":6.3709157577727549E-7},{"$f":"(AC6)/($BB6+$BA6)","v":1.0790424671534431E-5},{"$f":"AX6/($BB6+$BA6)","v":0.37357433194979339},{"$f":"SUM(BD6:BO6)","v":0.65742563199084736},{"$f":"BC6","v":0.39665409024053727},{"$f":"100*BQ6","v":39.66540902405373},{"$f":"I6*1000","v":0.2},8.7924221262065743,{"$f":"BT6/100","v":8.7924221262065741E-2},{"$f":"S6/1000","v":0.9733640467321133},null,{"$f":"AM6/($BB6+$BA6)","v":8.0968696291262299E-2},null,{"$f":"AZ6","v":1.2859745214576703E-3},{"$f":"AX6","v":9.4181389059483063E-4},{"$f":"Z6","v":2.3508500392714011E-4},null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR6, IF(MODE_ILIM=4,#REF!,#REF!))","v":39.66540902405373},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ6, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.2859745214576703E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA6, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.4181389059483063E-4},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB6, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.3508500392714011E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S6, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":0.9733640467321133},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P6, IF(MODE_ILIM=4,#REF!,#REF!))","v":24.155499589696174}]
[null,null,null,null,null,null,null,1,5.0000000000000001E-3,0.16563381487020262,0.16563381487020262,0,{"$f":"IF(I7<Icrit, 1000*((((J7/2)-I7)*0.000002/Cout+Vout/306)), 1000*J7*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":21.056045489233711},5.6948174474949225,{"$f":"ROUNDUP(M7/N7,0)","v":4},22.77926978997969,2.2369103433025619E-6,{"$f":"OnTime*S7","v":5.9409426680426831E-3},24334.10116830283,{"$f":"IF(1/S7-OnTime-Q7>Tsleep, OnTime+Q7+Tsleep, 1/S7)","v":7.4810509683025621E-6},{"$f":"IF(1/S7-OnTime-Q7>Tsleep, 1/S7-OnTime-Q7-Tsleep, 0)","v":3.3613542708433787E-5},1.2832902322013786E-4,{"$f":"IF(I7<Icrit,Iripple*SQRT((OnTime+OffTime)*S7/3), SQRT(I7^2+Iripple^2/12))","v":2.2890198226869187E-2},6.2875340983843832E-5,5.8142473922266937E-3,5.877181857980673E-3,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q7)*S7)","v":1.1662678459697304E-2},{"$f":"RCoutEsr*AA7^2","v":6.8009034427143729E-7},{"$f":"AB7","v":6.8009034427143729E-7},{"$f":"SQRT($R7)*SQRT($I7^2*(1-R7)+(Iripple^2)/12)","v":3.678600927412365E-3},{"$f":"RCinEsr*AD7^2","v":4.0596314349477339E-8},{"$f":"AE7","v":4.0596314349477339E-8},{"$f":"IF(I7<Icrit,Iripple*SQRT((OnTime)*S7/3), SQRT(OnTime*S7*(I7^2+Iripple^2/12)))","v":7.3169566314015199E-3},{"$f":"RdsonTop*AG7^2","v":3.6780505935571937E-5},{"$f":"QgTop*S7*Vdd","v":9.7701416190735865E-5},42.666666666666664,49.822614741301194,2.706801180756209E-3,5.1032308933308627E-3,{"$f":"AI7+AL7+AM7","v":7.9077334902778081E-3},7.9445680395710261E-3,2.1689244351050008E-2,{"$f":"RdsonBot*AP7^2","v":1.4300868943794464E-4},2.6767511285133119E-4,0,3.4325643007757195E-5,{"$f":"AR7+AS7+AT7","v":3.020007558590884E-4},4.4502121586659579E-4,6.6228788747770993E-3,9.9989580031257987E-3,3.6537652904206704E-4,{"$f":"AO7+AV7+AX7+AY7","v":1.8753923787605487E-2},2.4631826332244779E-2,2.5000000000000001E-2,{"$f":"BB7/(BB7+BA7)","v":0.50370904815481299},{"$f":"(AO7-AN7)/($BB7+$BA7)","v":7.4215583054793564E-4},{"$f":"(AV7-AU7)/($BB7+$BA7)","v":2.881627991081802E-3},7.5384202715909732E-2,{"$f":"AN7/($BB7+$BA7)","v":0.15932787637799087},{"$f":"AS7/(BA7+BB7)","v":0},{"$f":"AT7/($BB7+$BA7)","v":6.9160547866957151E-4},{"$f":"AU7/($BB7+$BA7)","v":6.0848205310326193E-3},1.2668351263752512E-3,0.11714756078700446,{"$f":"(AF7)/($BB7+$BA7)","v":8.1794923438275229E-7},{"$f":"(AC7)/($BB7+$BA7)","v":1.370270639888979E-5},{"$f":"AX7/($BB7+$BA7)","v":0.20146262473177784},{"$f":"SUM(BD7:BO7)","v":0.56500383022602341},0.50370904815481299,{"$f":"100*BQ7","v":50.370904815481296},5,9.5725635821403898,{"$f":"BT7/100","v":9.5725635821403893E-2},24.33410116830283,null,0.10282174303175699,null,{"$f":"AZ7","v":1.8753923787605487E-2},{"$f":"AX7","v":9.9989580031257987E-3},{"$f":"Z7","v":5.877181857980673E-3},null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR7, IF(MODE_ILIM=4,#REF!,#REF!))","v":50.370904815481296},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ7, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.8753923787605487E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA7, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9989580031257987E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB7, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.877181857980673E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S7, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":24.33410116830283},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P7, IF(MODE_ILIM=4,#REF!,#REF!))","v":22.77926978997969}]
["Vin",{"$f":"Vin","v":51.2},"V",{"$f":"B8","v":51.2},"Vin",null,null,2,0.01,0.16563381487020262,0.16563381487020262,0,20.753015186203406,5.3369042630402914,4,21.347617052161166,2.2369103433025619E-6,{"$f":"OnTime*S8","v":1.1881885336085366E-2},48668.20233660566,7.4810509683025621E-6,1.3066245870065613E-5,2.4665804644027569E-4,3.2371628777846981E-2,1.2575068196768769E-4,1.1628494784453387E-2,1.1754481967880858E-2,1.6493518051300483E-2,1.3601806885428744E-6,{"$f":"AB8","v":1.3601806885428744E-6},5.2861136751492475E-3,8.3828993359799655E-8,{"$f":"AE8","v":8.3828993359799655E-8},1.0347739303423784E-2,7.3561011871143861E-5,1.9540283238147173E-4,42.666666666666664,49.822614741301194,5.7239738296939726E-3,1.0206461786661725E-2,1.6125838448737169E-2,1.61996198582046E-2,3.0673223518878964E-2,2.8601737887588928E-4,5.3535022570266237E-4,0,7.2632064309527733E-5,6.0798229001219012E-4,8.9404696300168665E-4,1.2681324863648157E-2,1.9433483120345558E-2,7.3075305808413408E-4,{"$f":"AO8+AV8+AX8+AY8","v":3.7257902999635981E-2},4.9013828977198741E-2,0.05,{"$f":"BB8/(BB8+BA8)","v":0.50497996609659634},7.4516267302844423E-4,2.8891385773533972E-3,7.5574406040844311E-2,0.16286450706244968,0,7.3355474745102228E-4,6.1403775239537344E-3,1.2700315023333358E-3,0.11744313804015437,8.4663924449486844E-7,1.3737279959712514E-5,0.19627039294501752,0.56394529303179008,0.50497996609659634,{"$f":"100*BQ8","v":50.497996609659637},10,10.507357436577642,0.10507357436577643,48.66820233660566,null,0.10308117453989286,null,3.7257902999635981E-2,1.9433483120345558E-2,1.1754481967880858E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR8, IF(MODE_ILIM=4,#REF!,#REF!))","v":50.497996609659637},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ8, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7257902999635981E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA8, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.9433483120345558E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB8, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1754481967880858E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S8, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":48.66820233660566},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P8, IF(MODE_ILIM=4,#REF!,#REF!))","v":21.347617052161166}]
["Vout",{"$f":"Vout","v":5},"V",{"$f":"B9","v":5},"Vout",null,null,3,1.4999999999999999E-2,0.16563381487020262,0.16563381487020262,0,20.449984883173105,4.9795850706400886,5,24.897925353200442,2.2369103433025619E-6,1.7822828004128047E-2,73002.303504908487,7.4810509683025621E-6,6.2171469239428868E-6,3.649870696604135E-4,3.9646986324260461E-2,1.8862602295153152E-4,1.7442742176680077E-2,1.7631900333269519E-2,2.0200351644534865E-2,2.0402710328143122E-6,2.0402710328143122E-6,6.6401848687157984E-3,1.3227616527216672E-7,1.3227616527216672E-7,1.2673340642365454E-2,1.1034151780671581E-4,2.9310424857220755E-4,42.666666666666664,49.822614741301194,9.0515179468132912E-3,1.5309692679992586E-2,2.4654314875378086E-2,2.4765161792278587E-2,3.7566873193794877E-2,4.2902606831383386E-4,8.030253385539934E-4,0,1.1492656413566212E-4,9.1795190268965552E-4,1.3470848599931794E-3,1.8739770852519214E-2,2.8868008237565312E-2,1.0961295871262009E-3,5.6076384476963281E-2,7.3710457357430884E-2,7.4999999999999997E-2,{"$f":"BB9/(BB9+BA9)","v":0.50433574970275852},7.4538750583004866E-4,2.8856945565844611E-3,7.5477993757991968E-2,0.16578736501442237,0,7.728209984549509E-4,6.1727461471208136E-3,1.2684112893161384E-3,0.11729331270063829,8.8948798640458926E-7,1.37197549457497E-5,0.19412224769223879,0.56454058890552994,0.50433574970275852,50.433574970275849,15,11.516667783884284,0.11516667783884284,73.002303504908483,null,0.10294967113977194,null,5.6076384476963281E-2,2.8868008237565312E-2,1.7631900333269519E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR9, IF(MODE_ILIM=4,#REF!,#REF!))","v":50.433574970275849},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ9, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.6076384476963281E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA9, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.8868008237565312E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB9, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7631900333269519E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S9, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":73.002303504908483},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P9, IF(MODE_ILIM=4,#REF!,#REF!))","v":24.897925353200442}]
["Iout",{"$f":"Iout","v":0.5},"A",{"$f":"B10","v":0.5},"Iout(max)",null,null,4,0.02,0.16563381487020262,0.16563381487020262,0,20.1469545801428,4.622997604254695,5,23.114988021273476,2.2369103433025619E-6,2.3763770672170732E-2,97336.40467321132,7.4810509683025621E-6,2.792597450881525E-6,4.8331609288055141E-4,4.5780396453738374E-2,2.5150136393537533E-4,2.3256989568906775E-2,2.3509436957715787E-2,2.3325356919394608E-2,2.7203613770857492E-6,2.7203613770857492E-6,7.9257476553354356E-3,1.8845242768816547E-7,1.8845242768816547E-7,1.463391326280304E-2,1.4712202374228775E-4,3.9080566476294346E-4,42.666666666666664,49.822614741301194,1.2689433532114169E-2,2.0412923573323451E-2,3.3493162770200563E-2,3.3641200178343274E-2,4.3378488702100017E-2,5.7203475775177855E-4,1.0707004514053247E-3,0,1.6121644271651088E-4,1.2319168941218356E-3,1.8041425262350973E-3,2.4798216841390275E-2,3.8302533354785076E-2,1.4615061161682682E-3,7.5209382175531719E-2,9.8721727947052279E-2,0.1,0.5032162362569842,7.4494827350813937E-4,2.879532288818092E-3,7.5310449361383286E-2,0.16854303309562874,0,8.1126731526542299E-4,6.1992058284138377E-3,1.265595697730576E-3,0.11703294757533209,9.4832321374730108E-7,1.3689300134359572E-5,0.19274456673902543,0.56554618379845367,0.5032162362569842,50.321623625698422,20,12.603144523181673,0.12603144523181672,97.33640467321132,null,0.10272114571569295,null,7.5209382175531719E-2,3.8302533354785076E-2,2.3509436957715787E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR10, IF(MODE_ILIM=4,#REF!,#REF!))","v":50.321623625698422},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ10, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.5209382175531719E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA10, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.8302533354785076E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB10, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.3509436957715787E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S10, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":97.33640467321132},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P10, IF(MODE_ILIM=4,#REF!,#REF!))","v":23.114988021273476}]
["Rt",{"$f":"Vout*2500/(Fsw/1000)","v":31.25},"kW",{"$f":"B11*1000","v":31250},"RT pin resistance to get Fsw",null,null,5,2.5000000000000001E-2,0.16563381487020262,0.16563381487020262,0,19.8439242771125,4.2673253019270296,5,21.336626509635153,2.2369103433025619E-6,2.9704713340213417E-2,121670.50584151415,7.4810509683025621E-6,7.3786776704470622E-7,6.0164511610068922E-4,5.118403925372466E-2,3.1437670491921919E-4,2.9071236961133472E-2,2.9387091844788903E-2,2.6078541835605713E-2,3.400451721357187E-6,3.400451721357187E-6,9.2160882441118478E-3,2.5480884756976983E-7,2.5480884756976983E-7,1.6361212416231671E-2,1.8390252967785968E-4,4.8850708095367931E-4,42.666666666666664,49.822614741301194,1.6637720585596597E-2,2.5516154466654312E-2,4.2642382133204593E-2,4.2827741353121368E-2,4.8498624749551134E-2,7.1504344718972324E-4,1.3383755642566559E-3,0,2.1150900028242453E-4,1.5498845645390805E-3,2.2652275819276843E-3,3.0856662830261332E-2,4.773705847200483E-2,1.8268826452103352E-3,9.4656910052264204E-2,0.12404765715762203,0.125,0.50191196908504787,7.442720884519769E-4,2.8723137794300305E-3,7.5115255049815699E-2,0.17122177586363027,0,8.4927119048769319E-4,6.2232449091386552E-3,1.2623154480037951E-3,0.1167296142952042,1.02313288339228E-6,1.3653819353960212E-5,0.19167840812809611,0.56671114770449593,0.50191196908504787,50.191196908504786,25,13.76888730592373,0.1376888730592373,121.67050584151416,null,0.10245490665469364,null,9.4656910052264204E-2,4.773705847200483E-2,2.9387091844788903E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR11, IF(MODE_ILIM=4,#REF!,#REF!))","v":50.191196908504786},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ11, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.4656910052264204E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA11, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.773705847200483E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB11, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.9387091844788903E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S11, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":121.67050584151416},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P11, IF(MODE_ILIM=4,#REF!,#REF!))","v":21.336626509635153}]
["Tamb",{"$f":"'Design Converter'!E56","v":25},"°C",{"$f":"B12","v":25},"Ambient temperature",null,null,6,0.03,0.16563381487020262,0.16563381487020262,0,19.540893974082199,3.9128177348692805,5,19.564088674346404,2.2369103433025619E-6,3.5645656008256095E-2,146004.60700981697,6.8490989461227245E-6,0,6.6E-4,5.606930576698977E-2,3.772520459030631E-4,3.4885484353360155E-2,3.5264864998058254E-2,2.8567611260406859E-2,4.0805420656286244E-6,4.0805420656286244E-6,1.0547242313188479E-2,3.3373296123934033E-7,3.3373296123934033E-7,1.7922810217007378E-2,2.2068303561343164E-4,5.8620849714441511E-4,42.666666666666664,49.822614741301194,2.0896379107260575E-2,3.0619385359985173E-2,5.2101972964390161E-2,5.2324791653507986E-2,5.3127581566614984E-2,8.5805213662766783E-4,1.6060506771079868E-3,0,2.658115370637533E-4,1.87186221417174E-3,2.7303476480775124E-3,3.3844432885906044E-2,5.4100907655998239E-2,2.1922591742524018E-3,0.11134830613183615,0.14661758540492126,0.15,0.5057016420494107,7.5119851310787489E-4,2.8942499573443334E-3,7.5682410783902726E-2,0.17565368854737407,0,8.9614220512545238E-4,6.3106919693126312E-3,1.2718465271978579E-3,0.11761097814122172,1.1251287100316451E-6,1.3756912153600599E-5,0.18239278558667898,0.56347887427212928,0.5057016420494107,50.570164204941072,30,15.015319606822954,0.15015319606822955,146.00460700981697,null,0.10322848970058793,null,0.11134830613183615,5.4100907655998239E-2,3.5264864998058254E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR12, IF(MODE_ILIM=4,#REF!,#REF!))","v":50.570164204941072},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ12, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11134830613183615},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA12, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.4100907655998239E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB12, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.5264864998058254E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S12, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":146.00460700981697},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P12, IF(MODE_ILIM=4,#REF!,#REF!))","v":19.564088674346404}]
["VDD",5,"V",{"$f":"B13","v":5},"Gate drive rail",null,null,7,3.5000000000000003E-2,0.16563381487020262,0.16563381487020262,0,19.23786367105189,3.5598228931321128,6,21.358937358792677,2.2369103433025619E-6,4.1586598676298783E-2,170338.70817811982,5.8706562395337635E-6,0,6.600000000000001E-4,6.0561771969267528E-2,4.4012738688690696E-4,4.0699731745586852E-2,4.1142756421093434E-2,3.0856546825268904E-2,4.7606324099000631E-6,4.7606324099000631E-6,1.1938017344875231E-2,4.2754877437962565E-7,4.2754877437962565E-7,1.9358847600533323E-2,2.574635415490036E-4,6.8390991333515112E-4,42.666666666666664,49.822614741301194,2.5465409097106116E-2,3.572261625331604E-2,6.1871935263757311E-2,6.2132357416570749E-2,5.7384346677790826E-2,1.0010608260656124E-3,1.8737257899593181E-3,0,3.2413135329084815E-4,2.1978571432501662E-3,3.1995103464975919E-3,3.3844432885906051E-2,5.7476986784346942E-2,2.5576357032944695E-3,0.12536649025070976,0.16651443485298748,0.17500000000000002,0.51242343555795133,7.6255093851462894E-4,2.9329747179752731E-3,7.6688382477916386E-2,0.1811693121855639,0,9.4910000928768274E-4,6.4356200469133399E-3,1.2887519295527571E-3,0.11917426495634646,1.2519200676354239E-6,1.3939769228054397E-5,0.16830031447745158,0.55771646342881764,0.51242343555795133,51.242343555795131,35,16.343061169118954,0.16343061169118955,170.33870817811982,null,0.10460060427224295,null,0.12536649025070976,5.7476986784346942E-2,4.1142756421093434E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR13, IF(MODE_ILIM=4,#REF!,#REF!))","v":51.242343555795131},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ13, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12536649025070976},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA13, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.7476986784346942E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB13, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.1142756421093434E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S13, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":170.33870817811982},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P13, IF(MODE_ILIM=4,#REF!,#REF!))","v":21.358937358792677}]
["K1",400,"pC",4,"RT constant",null,null,8,0.04,0.16563381487020262,0.16563381487020262,0,18.934833368021589,3.2088400466440197,6,19.253040279864116,2.2369103433025619E-6,4.7527541344341465E-2,194672.80934642264,5.1368242095920436E-6,0,6.600000000000001E-4,6.4743257555693962E-2,5.0300272787075077E-4,4.6513979137813549E-2,4.7020766117464086E-2,3.2987036102600967E-2,5.4407227541714975E-6,5.4407227541714975E-6,1.3397969523199655E-2,5.3851676203376034E-7,5.3851676203376034E-7,2.0695478606847569E-2,2.9424404748457545E-4,7.8161132952588692E-4,42.666666666666664,49.822614741301194,3.0344810555133203E-2,4.0825847146646901E-2,7.1952269031305999E-2,7.2250444979549619E-2,6.1346447037757927E-2,1.1440695155035571E-3,2.1414009028106495E-3,0,3.8647574919405906E-4,2.5278766520047086E-3,3.6727232998074724E-3,3.3844432885906051E-2,6.0853065912695653E-2,2.9230122323365363E-3,0.1396992464243893,0.18672599178136959,0.2,0.51716203268040839,7.710263974503945E-4,2.9603560974251447E-3,7.7397552518392906E-2,0.18605490854098905,0,9.9935292017441649E-4,6.5366091385805026E-3,1.3006695659471389E-3,0.12027631999482882,1.3925021164292565E-6,1.4068676193989407E-5,0.15735447631122279,0.55366673266332156,0.51716203268040839,51.716203268040836,40,17.75180413241851,0.17751804132418511,194.67280934642264,null,0.10556789048129782,null,0.1396992464243893,6.0853065912695653E-2,4.7020766117464086E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR14, IF(MODE_ILIM=4,#REF!,#REF!))","v":51.716203268040836},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ14, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1396992464243893},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA14, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.0853065912695653E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB14, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.7020766117464086E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S14, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":194.67280934642264},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P14, IF(MODE_ILIM=4,#REF!,#REF!))","v":19.253040279864116}]
["Outputs",null,null,null,null,null,null,9,4.4999999999999998E-2,0.16563381487020262,0.16563381487020262,0,18.631803064991285,2.860609877236719,7,20.024269140657033,2.2369103433025619E-6,5.3468484012384146E-2,219006.91051472546,4.5660659640818166E-6,0,6.6E-4,6.8670594680607572E-2,5.6587806885459457E-4,5.2328226530040239E-2,5.2898894090740056E-2,3.4988035379091911E-2,6.120813098442937E-6,6.120813098442937E-6,1.4931330244436434E-2,6.6883386860526655E-7,6.6883386860526655E-7,2.1950869894204559E-2,3.310245534201474E-4,8.7931274571662272E-4,42.666666666666664,49.822614741301194,3.553458348134185E-2,4.5929078039977762E-2,8.234297426703624E-2,8.26790606798571E-2,6.5067733053150029E-2,1.2870782049415018E-3,2.4090760156619804E-3,0,4.5285202500373699E-4,2.8619280406657174E-3,4.1499941314333518E-3,3.3844432885906044E-2,6.4229145041044336E-2,3.2883887613786031E-3,0.15434658861371339,0.20725227235142049,0.22499999999999998,0.52052936304074604,7.7752376174351811E-4,2.9798943190296021E-3,7.7901501207472454E-2,0.19049749309378186,0,1.0476567827862543E-3,6.6209670225607833E-3,1.3091384477315979E-3,0.12105945966548318,1.5473229671341219E-6,1.4160279748550922E-5,0.14859180425274002,0.55080114615604492,0.52052936304074604,52.052936304074606,45,19.240199150848532,0.19240199150848533,219.00691051472546,null,0.10625526105421486,null,0.15434658861371339,6.4229145041044336E-2,5.2898894090740056E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR15, IF(MODE_ILIM=4,#REF!,#REF!))","v":52.052936304074606},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ15, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15434658861371339},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA15, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.4229145041044336E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB15, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.2898894090740056E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S15, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":219.00691051472546},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P15, IF(MODE_ILIM=4,#REF!,#REF!))","v":20.024269140657033}]
["Design","Value","Units","Std Units","Description",null,null,10,0.05,0.16563381487020262,0.16563381487020262,0,18.328772761960984,2.5162754827047715,8,20.130203861638172,2.2369103433025619E-6,5.9409426680426834E-2,243341.01168302831,4.1094593676736342E-6,0,6.5999999999999989E-4,7.2385162489654278E-2,6.2875340983843838E-4,5.8142473922266943E-2,5.8777140344491323E-2,3.6880627550827751E-2,6.8009034427143748E-6,6.8009034427143748E-6,1.6539180832778607E-2,8.2063350785805383E-7,8.2063350785805383E-7,2.3138248495901906E-2,3.6780505935571942E-4,9.7701416190735862E-4,42.666666666666664,49.822614741301194,4.1034727875732056E-2,5.1032308933308623E-2,9.3044050970948033E-2,9.3418210855078079E-2,6.8587412877258669E-2,1.4300868943794467E-3,2.6767511285133118E-3,0,5.2326748095023212E-4,3.2000186094635437E-3,4.6313304656081852E-3,3.3844432885906037E-2,6.7605224169393033E-2,3.6537652904206704E-3,0.16930853078049996,0.22809329266194184,0.25,0.52291049432641623,7.8260851987022766E-4,2.9937919609274197E-3,7.8257857092262906E-2,0.19461484274940283,0,1.0944882285144979E-3,6.6932932517132513E-3,1.3151270253921503E-3,0.12161323912021349,1.7164714930195036E-6,1.4225055124383999E-5,0.14140592475786198,0.54878711423277615,0.52291049432641623,52.291049432641621,50,20.80575856495858,0.20805758564958579,243.34101168302831,null,0.1067413195637392,null,0.16930853078049996,6.7605224169393033E-2,5.8777140344491323E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR16, IF(MODE_ILIM=4,#REF!,#REF!))","v":52.291049432641621},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ16, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16930853078049996},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA16, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.7605224169393033E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB16, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8777140344491323E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S16, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":243.34101168302831},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P16, IF(MODE_ILIM=4,#REF!,#REF!))","v":20.130203861638172}]
["On-Time",{"$f":"(Rt*k_RT/10000)/Vin","v":0.244140625},"µs",{"$f":"B17/1000000","v":2.4414062500000001E-7},"On Time - fixed",null,null,11,5.5E-2,0.16563381487020262,0.16563381487020262,0,18.025742458930679,2.1776856408345466,9,19.599170767510923,2.2369103433025619E-6,6.5350369348469509E-2,267675.11285133113,3.7358721524305768E-6,0,6.6E-4,7.5918198895383579E-2,6.916287508222824E-4,6.3956721314493634E-2,6.4655504882287995E-2,3.8680728501376008E-2,7.480993786985811E-6,7.480993786985811E-6,1.8220735101493735E-2,9.9598556291641787E-7,9.9598556291641787E-7,2.4267599753661617E-2,4.0458556529129126E-4,1.0747155780980945E-3,42.666666666666664,49.822614741301194,4.6845243738303816E-2,5.6135539826639484E-2,0.10405549914304139,0.10446790184296997,7.1935085498768273E-2,1.5730955838173907E-3,2.9444262413646427E-3,0,5.9772941726389485E-4,3.5421556586285375E-3,5.1167399273717882E-3,3.3844432885906044E-2,7.0981303297741744E-2,4.0191418194627376E-3,0.18458508688754621,0.24924906874918412,0.27500000000000002,0.5245598254587801,7.8665413924823764E-4,3.0035041788440018E-3,7.8504693064106637E-2,0.19848485261272739,0,1.1401630501510073E-3,6.756627469229148E-3,1.3192751156858565E-3,0.12199682388962407,1.8998327747014581E-6,1.4269922891489074E-5,0.13539614570436415,0.54740490897964666,0.5245598254587801,52.455982545878008,55,22.444784059665849,0.22444784059665848,267.67511285133111,null,0.10707799626725965,null,0.18458508688754621,7.0981303297741744E-2,6.4655504882287995E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR17, IF(MODE_ILIM=4,#REF!,#REF!))","v":52.455982545878008},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ17, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.18458508688754621},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA17, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0981303297741744E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB17, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.4655504882287995E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S17, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":267.67511285133111},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P17, IF(MODE_ILIM=4,#REF!,#REF!))","v":19.599170767510923}]
["Off Time",{"$f":"L*Iripple*1000000/(Vout+(Rdcr+RdsonBot)*Iout)","v":2.1452007161957987},"µs",{"$f":"B18/1000000","v":2.1452007161957987E-6},"Off Time - depends on Vout, L, Iout, DCR, etc.",null,null,12,0.06,0.16563381487020262,0.16563381487020262,0,17.722712155900378,1.8480005968753868,10,18.480005968753868,2.2369103433025619E-6,7.129131201651219E-2,292009.21401963395,3.4245494730613622E-6,0,6.6E-4,7.9293972648520922E-2,7.5450409180612609E-4,6.977096870672031E-2,7.0533987707700321E-2,4.040070328906973E-2,8.1610841312572488E-6,8.1610841312572488E-6,1.9974119807599718E-2,1.1968963862650423E-6,1.1968963862650423E-6,2.5346681284730908E-2,4.4136607122686322E-4,1.1724169942888302E-3,42.666666666666664,49.822614741301194,5.2966131069057128E-2,6.1238770719970345E-2,0.11537731878331631,0.11582813998146262,7.5133746387589753E-2,1.7161042732553354E-3,3.2121013542159736E-3,0,6.7624513417507601E-4,3.8883464883910498E-3,5.6062301425709457E-3,3.3844432885906044E-2,7.435738242609044E-2,4.3845183485048036E-3,0.2001762708986288,0.27071961658684662,0.3,0.52565216137852666,7.899171240028811E-4,3.0100308527216792E-3,7.8668170120374914E-2,0.202161123308365,0,1.1848990546694683E-3,6.8130591193711985E-3,1.3220223554227749E-3,0.12225086834053693,2.0971705746212248E-6,1.4299638375957895E-5,0.13028706262241371,0.54650354970682913,0.52565216137852666,52.565216137852666,60,24.152326085424395,0.24152326085424394,292.00921401963393,null,0.10730097396372149,null,0.2001762708986288,7.435738242609044E-2,7.0533987707700321E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR18, IF(MODE_ILIM=4,#REF!,#REF!))","v":52.565216137852666},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ18, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.2001762708986288},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA18, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.435738242609044E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB18, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0533987707700321E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S18, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":292.00921401963393},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P18, IF(MODE_ILIM=4,#REF!,#REF!))","v":18.480005968753868}]
["DIL",{"$f":"(Vin-Vout-(Rdcr+RdsonTop)*Iout)/L*OnTime*1000","v":164.42332548253677},"mA",{"$f":"B19/1000","v":0.16442332548253677},"Inductor pk-pk ripple current in CCM",null,null,13,6.5000000000000002E-2,0.16563381487020262,0.16563381487020262,0,17.419681852870074,1.5329764095137204,12,18.395716914164645,2.2369103433025619E-6,7.7232254684554885E-2,316343.31518793682,3.1611225905181801E-6,0,6.6E-4,8.2531783412511758E-2,8.1737943278997012E-4,7.5585216098947014E-2,7.6412588824298772E-2,4.2050385195688003E-2,8.8411744755286841E-6,8.8411744755286841E-6,2.1796856040485882E-2,1.4253087997489978E-6,1.4253087997489978E-6,2.6381662314864444E-2,4.7814657716243513E-4,1.2701184104795663E-3,42.666666666666664,49.822614741301194,5.9397389867992006E-2,6.6342001613301213E-2,0.12700950989177279,0.12749893160865833,7.8201682633778496E-2,1.8591129626932808E-3,3.4797764670673054E-3,0,7.5882193191412618E-4,4.2385983989814318E-3,6.0998087378595208E-3,3.3844432885906044E-2,7.7733461554439137E-2,4.7498948775468713E-3,0.21608209677850385,0.29250495208607791,0.32500000000000001,0.52631156867985118,7.9257942018466144E-4,3.0140816403017982E-3,7.8766855847497541E-2,0.20568176734891694,0,1.2288515733366121E-3,6.8640719149902244E-3,1.3236807737794958E-3,0.12240422662782259,2.3081738776895104E-6,1.4317576637500807E-5,0.12588313873732851,0.54597587963467353,0.52631156867985118,52.631156867985119,65,25.922181532084487,0.25922181532084487,316.34331518793681,null,0.10743557827217778,null,0.21608209677850385,7.7733461554439137E-2,7.6412588824298772E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR19, IF(MODE_ILIM=4,#REF!,#REF!))","v":52.631156867985119},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ19, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21608209677850385},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA19, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.7733461554439137E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB19, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.6412588824298772E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S19, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":316.34331518793681},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P19, IF(MODE_ILIM=4,#REF!,#REF!))","v":18.395716914164645}]
["CCM Freq",{"$f":"'Design Converter'!E12","v":400},"kHz",{"$f":"B20*1000","v":400000},"Frequency in CCM",{"$f":"10000*Vout/(k_RT*Rt/1000+Vin*0.75)","v":305.99755201958385},null,14,7.0000000000000007E-2,0.16563381487020262,0.16563381487020262,0,17.116651549839769,1.2438030987734141,14,17.413243382827794,2.2369103433025619E-6,8.3173197352597567E-2,340677.41635623964,2.9353281197668817E-6,0,6.600000000000001E-4,8.5647279280284871E-2,8.802547737738137E-4,8.1399463491173704E-2,8.2291308235653851E-2,4.3637747008295751E-2,9.5212648198001244E-6,9.5212648198001244E-6,2.3686156959806297E-2,1.6831020945737407E-6,1.6831020945737407E-6,2.737754482858807E-2,5.1492708309800708E-4,1.3678198266703022E-3,42.666666666666664,49.822614741301194,6.6139020135108431E-2,7.1445232506632081E-2,0.13895207246841082,0.13948028306283189,8.115372133965125E-2,2.0021216521312248E-3,3.7474515799186363E-3,0,8.4546711071139527E-4,4.592918690630032E-3,6.5974833406985522E-3,3.3844432885906051E-2,8.1109540682787834E-2,5.115271406588939E-3,0.2323025784929072,0.31460509109547541,0.35000000000000003,0.52662852675878746,7.9477362045243154E-4,3.0161740813095116E-3,7.8814291231401198E-2,0.20907464346891275,0,1.2721345683912879E-3,6.9107485816268365E-3,1.3244779276711236E-3,0.12247794153517862,2.5324845041428525E-6,1.4326199042661747E-5,0.12204170833102426,0.54574375202951486,0.52662852675878746,52.662852675878746,70,27.746934669307642,0.27746934669307644,340.67741635623963,null,0.10750027868259053,null,0.2323025784929072,8.1109540682787834E-2,8.2291308235653851E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR20, IF(MODE_ILIM=4,#REF!,#REF!))","v":52.662852675878746},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ20, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.2323025784929072},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA20, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.1109540682787834E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB20, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.2291308235653851E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S20, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":340.67741635623963},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P20, IF(MODE_ILIM=4,#REF!,#REF!))","v":17.413243382827794}]
["Icrit_Skip",{"$f":"1000*Iripple/2","v":82.211662741268384},"mA",{"$f":"Iripple/2","v":8.2211662741268385E-2},"CCM-DCM (critical conduction) boundary",null,null,15,7.4999999999999997E-2,0.16563381487020262,0.16563381487020262,0,16.813621246809468,1.0030925357264386,17,17.052573107349456,2.2369103433025619E-6,8.9114140020640248E-2,365011.51752454246,2.7396395784490894E-6,0,6.5999999999999989E-4,8.8653356524050916E-2,9.4313011475765784E-4,8.7213710883400408E-2,8.8170145945336245E-2,4.5169359446579627E-2,1.0201355164071561E-5,1.0201355164071561E-5,2.563911095250845E-2,1.9720920313051167E-6,1.9720920313051167E-6,2.833845117834001E-2,5.517075890335791E-4,1.4655212428610381E-3,42.666666666666664,49.822614741301194,7.3191021870406395E-2,7.6548463399962935E-2,0.15120500651323038,0.15177220068243058,8.4002082163439989E-2,2.14513034156917E-3,4.0151266927699672E-3,0,9.3618797079723394E-4,4.9513146635672012E-3,7.0992615793563744E-3,3.3844432885906037E-2,8.4485619811136531E-2,5.4806479356310049E-3,0.24883773000855447,0.3370200494010861,0.375,0.52667056259922784,7.9659859252179273E-4,3.0166944281918937E-3,7.8820582240722373E-2,0.21236060226171452,0,1.3148337207424231E-3,6.9538978119113182E-3,1.3245836483831732E-3,0.12248771780620504,2.7697141856664528E-6,1.4327342569429619E-5,0.11865623711326866,0.54574884468041629,0.52667056259922784,52.667056259922788,75,29.618044224570543,0.29618044224570544,365.01151752454246,null,0.10750885942657301,null,0.24883773000855447,8.4485619811136531E-2,8.8170145945336245E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR21, IF(MODE_ILIM=4,#REF!,#REF!))","v":52.667056259922788},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ21, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.24883773000855447},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA21, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.4485619811136531E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB21, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.8170145945336245E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S21, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":365.01151752454246},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P21, IF(MODE_ILIM=4,#REF!,#REF!))","v":17.052573107349456}]
["Tr",null,"ns",{"$f":"B22/1000000000","v":0},"Switch rise time",null,null,16,0.08,0.16563381487020262,0.16563381487020262,0,16.510590943779164,0.85291390671088374,20,17.058278134217673,2.2369103433025619E-6,9.5055082688682929E-2,389345.61869284528,2.5684121047960218E-6,0,6.600000000000001E-4,9.1560792907476748E-2,1.0060054557415013E-3,9.3027958275627098E-2,9.4049101956916806E-2,4.6650713838789215E-2,1.0881445508342997E-5,1.0881445508342997E-5,2.765279274545554E-2,2.2940308398693558E-6,2.2940308398693558E-6,2.926782652560608E-2,5.88488094969151E-4,1.5632226590517738E-3,42.666666666666664,49.822614741301194,8.0553395073885939E-2,8.1651694293293803E-2,0.16376831202623152,0.16437469080607414,8.6756977404200034E-2,2.2881390310071142E-3,4.282801805621299E-3,0,1.0309918124019933E-3,5.3137936180232921E-3,7.6051510829087138E-3,3.3844432885906051E-2,8.7861698939485255E-2,5.8460244646730726E-3,0.26568756529314119,0.3597498427264062,0.4,0.52648908562399555,7.9812952335284518E-4,3.0159367413131054E-3,7.8793422718495584E-2,0.21555557213218954,0,1.3570148414933784E-3,6.9941358578692646E-3,1.3241272313152348E-3,0.12244551172500528,3.0194554981901591E-6,1.4322405739887093E-5,0.11564556384005092,0.54594675647232327,0.52648908562399555,52.648908562399555,80,31.525976771075946,0.31525976771075948,389.34561869284528,null,0.10747181467031566,null,0.26568756529314119,8.7861698939485255E-2,9.4049101956916806E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR22, IF(MODE_ILIM=4,#REF!,#REF!))","v":52.648908562399555},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ22, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.26568756529314119},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA22, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.7861698939485255E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB22, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.4049101956916806E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S22, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":389.34561869284528},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P22, IF(MODE_ILIM=4,#REF!,#REF!))","v":17.058278134217673}]
["Tf",null,"ns",{"$f":"B23/1000000000","v":0},"Switch fall time",null,null,17,8.5000000000000006E-2,0.16562573601217834,0.1676960665194131,2.3069327422757524E-3,1.7736278513846961,1.7736278513846961,1,1.7736278513846961,2.2363901098537994E-6,9.8422737347936745E-2,403139.53217714891,2.4805307348537992E-6,0,6.6E-4,9.7354605250914314E-2,1.1373502996273623E-3,9.6323795050119579E-2,9.7478884171846164E-2,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,2.9374375209094413E-2,2.5885617567739813E-6,2.5885617567739813E-6,3.054247449765941E-2,6.4086296817840059E-4,1.618605221691253E-3,42.666666666666664,48.99179797449731,8.5772292539514614E-2,8.4544487618437233E-2,0.17193538537964309,0.17259670582215997,9.0535344930500319E-2,2.4917811992321397E-3,4.4345348539486388E-3,1.7266006702651082E-4,1.1190891493333373E-3,5.7262840703084872E-3,8.2218543516753423E-3,3.3844432885906044E-2,8.9775447184818641E-2,6.0531400756398922E-3,0.27664714743429381,0.37413988476371457,0.42500000000000004,0.53182178502536115,8.2754027814844078E-4,3.1228203333947373E-3,7.7563584994734244E-2,0.21515054955676507,2.1605737658502932E-4,1.4003670329434548E-3,7.1655590960794111E-3,1.423218038934007E-3,0.1205343355858156,3.2391847862021723E-6,1.4095899895094609E-5,0.11234009076065947,0.53976145813874077,0.53182178502536115,53.182178502536118,85,33.460383546927204,0.33460383546927203,403.13953217714891,null,0.10579435369245135,null,0.27664714743429381,8.9775447184818641E-2,9.7478884171846164E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR23, IF(MODE_ILIM=4,#REF!,#REF!))","v":53.182178502536118},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ23, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.27664714743429381},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA23, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.9775447184818641E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB23, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.7478884171846164E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S23, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":403.13953217714891},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P23, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7736278513846961}]
[null,null,null,null,null,null,null,18,0.09,0.16561124913832723,0.17269608750636448,7.3141762096048391E-3,1.7734727165393485,1.7734727165393485,1,1.7734727165393485,2.2352535333149903E-6,9.8467855214242866E-2,403324.33495753875,2.4793941583149901E-6,0,6.6E-4,0.10174929564159819,1.2423502996273623E-3,9.6367950742434927E-2,9.7629707489478634E-2,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,3.0673976027038384E-2,2.8226784159219766E-6,2.8226784159219766E-6,3.1928509912652038E-2,7.0034823498147357E-4,1.619347204854518E-3,42.666666666666664,47.569368239058818,8.8014299963010148E-2,8.4583243570487243E-2,0.17421689073835189,0.17493989883452557,9.4643892009482519E-2,2.7230697535895873E-3,4.4365676845329275E-3,4.8249230519853284E-4,1.1855456786106135E-3,6.1046056683420735E-3,8.832123559784473E-3,3.3844432885906044E-2,8.9801086463846033E-2,6.0559148893874456E-3,0.2796290237475435,0.37727281851125588,0.44999999999999996,0.5439559839640461,8.7396573415138756E-4,3.2969992853757579E-3,7.4960239330628634E-2,0.21059182272163762,5.8323239250966403E-4,1.4330770358732426E-3,7.379192851190014E-3,1.5017419548040655E-3,0.11648871881933316,3.4120284781042531E-6,1.3616542893405237E-5,0.10855075188551502,0.52567677058239015,0.5439559839640461,54.395598396404608,90,35.410314704487,0.35410314704487,403.32433495753878,null,0.10224346996278882,null,0.2796290237475435,8.9801086463846033E-2,9.7629707489478634E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR24, IF(MODE_ILIM=4,#REF!,#REF!))","v":54.395598396404608},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ24, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.2796290237475435},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA24, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.9801086463846033E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB24, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.7629707489478634E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S24, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":403.32433495753878},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P24, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7734727165393485}]
["Components","Input Value","Units","Std Units","Description",null,null,19,9.5000000000000001E-2,0.16559676226447612,0.17769610849331588,1.2321419676933912E-2,1.773317581694001,1.773317581694001,1,1.773317581694001,2.2341179128906281E-6,9.851297645797702E-2,403509.15157187387,2.4782585378906284E-6,0,6.6E-4,0.10619754782273154,1.3533502996273623E-3,9.6412109740151991E-2,9.7786634371127473E-2,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,3.1991178567163367E-2,3.0703065183483984E-6,3.0703065183483984E-6,3.3331987415317552E-2,7.6327169153270788E-4,1.6200892435610736E-3,42.666666666666664,46.227205779116467,9.0258329020099864E-2,8.4622002423725862E-2,0.17650042068738681,0.17728871971322871,9.880414169114328E-2,2.9677265582583492E-3,4.4386006672906134E-3,7.9260842761509566E-4,1.2521433831532251E-3,6.483352478058934E-3,9.4562694031784141E-3,3.3844432885906044E-2,8.9826727662175629E-2,6.0586899108516865E-3,0.28263040668943445,0.38043137596289811,0.47499999999999998,0.5552754006308529,9.215222260868936E-4,3.4753423929220267E-3,7.2525963426681855E-2,0.2063291406499006,9.2655992039444759E-4,1.4637566710056392E-3,7.5790445151267529E-3,1.5820676417251968E-3,0.11270583760342874,3.5891909095482656E-6,1.3168322011952168E-5,0.10500752039994335,0.51253351296013694,0.5552754006308529,55.52754006308529,95,37.364462120689176,0.37364462120689174,403.50915157187387,null,9.8923192206356605E-2,null,0.28263040668943445,8.9826727662175629E-2,9.7786634371127473E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR25, IF(MODE_ILIM=4,#REF!,#REF!))","v":55.52754006308529},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ25, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.28263040668943445},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA25, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.9826727662175629E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB25, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.7786634371127473E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S25, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":403.50915157187387},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P25, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.773317581694001}]
["L",{"$f":"'Design Converter'!E17","v":68},"µH",{"$f":"B26/1000000","v":6.7999999999999999E-5},"Filter inductance",null,null,20,0.1,0.16558227539062501,0.18269612948026728,1.7328663144263012E-2,1.7731624468486533,1.7731624468486533,1,1.7731624468486533,2.2329832473747621E-6,9.8558101079518484E-2,403693.98202170769,2.4771238723747618E-6,0,6.6E-4,0.11069290475708619,1.4703502996273625E-3,9.6456272043641961E-2,9.7949665594494167E-2,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,3.3323977141953558E-2,3.3314623576723298E-6,3.3314623576723298E-6,3.4750891289885635E-2,8.2963799401827582E-4,1.6208313378171565E-3,42.666666666666664,44.95870284457169,9.2504379937795131E-2,8.4660764178478842E-2,0.17878597545409114,0.1796431781752755,0.10301011890222646,3.2257697172602532E-3,4.4406338022387852E-3,1.1030084661538524E-3,1.3188823806500663E-3,6.8625246490427042E-3,1.0094316697312849E-2,3.3844432885906044E-2,8.985237078002295E-2,6.0614651400559419E-3,0.28565133079266725,0.38361559244533688,0.5,0.56585692271034882,9.7010818789664216E-4,3.6574638065478378E-3,7.0244802790770861E-2,0.20233456378843992,1.2482899527625616E-3,1.4925974506630906E-3,7.766414159862442E-3,1.6640157917067573E-3,0.10916089854945497,3.7702620756756556E-6,1.2748299050079998E-5,0.10168717205562609,0.50024284509485695,0.56585692271034882,56.58569227103488,100,39.311419610679415,0.39311419610679416,403.69398202170771,null,9.5811758984681125E-2,null,0.28565133079266725,8.985237078002295E-2,9.7949665594494167E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR26, IF(MODE_ILIM=4,#REF!,#REF!))","v":56.58569227103488},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ26, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.28565133079266725},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA26, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.985237078002295E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB26, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.7949665594494167E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S26, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":403.69398202170771},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P26, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7731624468486533}]
["Rdcr",{"$f":"'Design Converter'!E18","v":120},"mW",{"$f":"B27/1000","v":0.12},"Inductor DCR at 25°C",null,null,21,0.105,0.16556778851677389,0.18769615046721869,2.2335906611592085E-2,1.7730073120033059,1.7730073120033059,1,1.7730073120033059,2.2318495355634677E-6,9.8603229079246513E-2,403878.82630859374,2.4759901605634679E-6,0,6.6E-4,0.11522985361251377,1.5933502996273623E-3,9.6500437653276039E-2,9.8118801972506914E-2,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,3.4670651499897398E-2,3.6061622262820131E-6,3.6061622262820131E-6,3.6183500452282906E-2,8.9945179932150547E-4,1.6215734876290039E-3,42.666666666666664,43.75795759755399,9.4752452943141177E-2,8.4699528835072008E-2,0.18107355526584218,0.18200328396853546,0.10725672192969798,3.497217337327785E-3,4.4426670893945317E-3,1.4136924526972296E-3,1.3857627888076516E-3,7.242122330899413E-3,1.0746290480096636E-2,3.3844432885906044E-2,8.9878015817603518E-2,6.0642405770235351E-3,0.28869183084325917,0.38682550357381018,0.52500000000000002,0.57576805862779035,1.0196344575242775E-3,3.8430249378449952E-3,6.8102749117385633E-2,0.19858356073189687,1.5503980171166537E-3,1.5197675250103128E-3,7.9424432662989E-3,1.7474289690103894E-3,0.10583213265592165,3.9548819507109808E-6,1.2353894219514906E-5,9.8569315582132208E-2,0.4887267640363121,0.57576805862779035,57.576805862779032,105,41.239947953148963,0.41239947953148964,403.87882630859372,null,9.289006339820563E-2,null,0.28869183084325917,8.9878015817603518E-2,9.8118801972506914E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR27, IF(MODE_ILIM=4,#REF!,#REF!))","v":57.576805862779032},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ27, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.28869183084325917},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA27, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.9878015817603518E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB27, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.8118801972506914E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S27, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":403.87882630859372},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P27, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7730073120033059}]
["Kcore",0,null,{"$f":"B28","v":0},"Core loss constant - consult inductor vendor",null,null,22,0.11,0.16555330164292281,0.19269617145417006,2.7343150078921172E-2,1.7728521771579584,1.7728521771579584,1,1.7728521771579584,2.2307167762548451E-6,9.8648360457540551E-2,404063.68443408608,2.4748574012548449E-6,0,6.6E-4,0.11980366924080979,1.7223502996273625E-3,9.6544606569425512E-2,9.8294044353331847E-2,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,3.602972113563073E-2,3.894422415333947E-6,3.894422415333947E-6,3.7628339629392916E-2,9.7271776502301488E-4,1.6223156930028557E-3,42.666666666666664,42.619682297983445,9.7002548263217428E-2,8.4738296393831264E-2,0.18336316035005154,0.18436904687185651,0.11153957770416315,3.7820875279046067E-3,4.4447005287749477E-3,1.72466041913243E-3,1.4527847253501221E-3,7.6221456732575004E-3,1.1412216013034115E-2,3.3844432885906044E-2,8.9903662775132953E-2,6.0670162217778033E-3,0.29175194188180137,0.39006114525336633,0.55000000000000004,0.58506832537128572,1.0700224415017856E-3,4.0317274667863333E-3,6.6087452315945219E-2,0.19505450392871124,1.8346257877380917E-3,1.5454151388828712E-3,8.1081381905250115E-3,1.832168373646751E-3,0.10270034779855165,4.1427330924142359E-6,1.1982833111106528E-5,9.563597349925787E-2,0.47791650050775025,0.58506832537128572,58.506832537128574,110,43.139231734149426,0.43139231734149425,404.0636844340861,null,9.0141260301735485E-2,null,0.29175194188180137,8.9903662775132953E-2,9.8294044353331847E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR28, IF(MODE_ILIM=4,#REF!,#REF!))","v":58.506832537128574},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ28, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.29175194188180137},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA28, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.9903662775132953E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB28, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.8294044353331847E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S28, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":404.0636844340861},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P28, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7728521771579584}]
["Cin",{"$f":"'Design Converter'!E37","v":2.2000000000000002},"µF",{"$f":"B29/1000000","v":2.2000000000000001E-6},"Input capacitance",null,null,23,0.115,0.1655388147690717,0.19769619244112147,3.2350393546250258E-2,1.7726970423126109,1.7726970423126109,1,1.7726970423126109,2.2295849682490111E-6,9.8693495214779964E-2,404248.55639973871,2.4737255932490113E-6,0,6.6E-4,0.12441028560196039,1.8573502996273624E-3,9.6588778792461721E-2,9.8475393620384558E-2,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,3.73999073740027E-2,4.1962592147519446E-6,4.1962592147519446E-6,3.908413924987595E-2,1.0494405494008378E-3,1.623057953944951E-3,42.666666666666664,41.539125456020741,9.9254666125137073E-2,8.4777066855082503E-2,0.18565479093416454,0.18674047669517876,0.11585492290647223,4.0803984011460459E-3,4.4467341203971262E-3,2.0359123973514278E-3,1.5199483080192446E-3,8.0025948257677979E-3,1.2092118782377762E-2,3.3844432885906044E-2,8.9929311652826832E-2,6.0697920743420768E-3,0.29483169920472541,0.39332255368014252,0.57500000000000007,0.59381039697432758,1.1212025960647529E-3,4.2233075549749314E-3,6.4187982201841687E-2,0.19172825235617744,2.1025146936977496E-3,1.5696714924615044E-3,8.2643895831545668E-3,1.9181111630297569E-3,9.9748558396551654E-2,4.3335345219461429E-6,1.1633102807525536E-5,9.2871235221205425E-2,0.467751191896489,0.59381039697432758,59.381039697432755,115,44.999115697666738,0.44999115697666736,404.24855639973873,null,8.7550441258322856E-2,null,0.29483169920472541,8.9929311652826832E-2,9.8475393620384558E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR29, IF(MODE_ILIM=4,#REF!,#REF!))","v":59.381039697432755},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ29, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.29483169920472541},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA29, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.9929311652826832E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB29, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.8475393620384558E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S29, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":404.24855639973873},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P29, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7726970423126109}]
["RCinESR",{"$f":"'Design Converter'!E39","v":3},"mW",{"$f":"B30/1000","v":3.0000000000000001E-3},"Input capacitor ESR",null,null,24,0.12,0.16552432789522062,0.20269621342807287,3.7357637013579331E-2,1.7725419074672635,1.7725419074672635,1,1.7725419074672635,2.228454110348098E-6,9.8738633351344279E-2,404433.44220710616,2.4725947353480983E-6,0,6.6E-4,0.12904619003892115,1.9983502996273619E-3,9.6632954322756065E-2,9.8662850692342319E-2,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,3.8780101913336251E-2,4.5116889132262385E-6,4.5116889132262385E-6,4.0549802459697123E-2,1.1296248114305554E-3,1.6238002704615313E-3,42.666666666666664,40.512005533932708,0.10150880675604754,8.4815840219151728E-2,0.18794844724566079,0.18911758327965048,0.12019950619369978,4.3921680719196179E-3,4.4487678642781683E-3,2.3474484192509753E-3,1.5872536545744184E-3,8.3834699381035611E-3,1.2786024500291489E-2,3.3844432885906044E-2,8.9954962450900872E-2,6.0725681347396998E-3,0.29793113836558255,0.39660976534265591,0.6,0.60204106046834394,1.1731131628915086E-3,4.4175310289822764E-3,6.2394630137258031E-2,0.18858780415526039,2.3554338928676584E-3,1.5926531223870624E-3,8.4119885532339175E-3,2.0051482226248166E-3,9.696167716110185E-2,4.5270366297033251E-6,1.1302915353166092E-5,9.0260968313884041E-2,0.45817677770247434,0.60204106046834394,60.204106046834397,120,46.810309970062292,0.46810309970062292,404.43344220710617,null,8.5104363983419543E-2,null,0.29793113836558255,8.9954962450900872E-2,9.8662850692342319E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR30, IF(MODE_ILIM=4,#REF!,#REF!))","v":60.204106046834397},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ30, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.29793113836558255},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA30, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.9954962450900872E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB30, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.8662850692342319E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S30, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":404.43344220710617},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P30, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7725419074672635}]
["Cout",{"$f":"'Design Converter'!E24","v":33},"µF",{"$f":"B31/1000000","v":3.3000000000000003E-5},"Output capacitance",null,null,25,0.125,0.16550984102136948,0.20769623441502427,4.2364880480908418E-2,1.7723867726219158,1.7723867726219158,1,1.7723867726219158,2.2273242013562488E-6,9.8783774867613042E-2,404618.34185774298,2.4714648263562486E-6,0,6.6E-4,0.13370833617827033,2.1453502996273623E-3,9.6677133160679982E-2,9.8856416523156632E-2,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,4.0169340705785997E-2,4.8407277982125472E-6,4.8407277982125472E-6,4.2024377946075886E-2,1.2132752107854303E-3,1.624542642558838E-3,42.666666666666664,39.534454246568217,0.10376497038313011,8.4854616486364956E-2,0.19024412951205388,0.19150037649774357,0.12457050764270131,4.7174146578055328E-3,4.4508017604351731E-3,2.6592685167326014E-3,1.6547008827926778E-3,8.7647711599604522E-3,1.3493959106024498E-2,3.3844432885906044E-2,8.9980615169570718E-2,6.0753444029940113E-3,0.30105029517633281,0.39992281702310545,0.625,0.60980201593649386,1.225699111020342E-3,4.6141893492038753E-3,6.0698743020818326E-2,0.18561800591445424,2.5946036838719842E-3,1.6144638945581936E-3,8.5516401961054818E-3,2.0931823001643628E-3,9.4326257114149631E-2,4.7230169119197384E-6,1.0990677181453378E-5,8.7792576840976147E-2,0.44914507511941598,0.60980201593649386,60.980201593649383,125,48.564555994658186,0.48564555994658187,404.61834185774296,null,8.2791225911845442E-2,null,0.30105029517633281,8.9980615169570718E-2,9.8856416523156632E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR31, IF(MODE_ILIM=4,#REF!,#REF!))","v":60.980201593649383},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ31, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.30105029517633281},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA31, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.9980615169570718E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB31, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.8856416523156632E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S31, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":404.61834185774296},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P31, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7723867726219158}]
["RCoutESR",{"$f":"'Design Converter'!E26","v":5.0000000000000001E-3},"mW",{"$f":"B32","v":5.0000000000000001E-3},"Output capacitor ESR",null,null,26,0.13,0.16549535414751843,0.21269625540197568,4.7372123948237504E-2,1.7722316377765688,1.7722316377765688,1,1.7722316377765688,2.2261952400796131E-6,9.8828919763965739E-2,404803.25535320368,2.4703358650796133E-6,0,6.6E-4,0.13839407199573742,2.2983502996273622E-3,9.672131530660491E-2,9.9056092102066298E-2,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,4.1566782234259934E-2,5.1833921559311618E-6,5.1833921559311618E-6,4.3507037491207406E-2,1.3003964078365316E-3,1.6252850702431129E-3,42.666666666666664,38.602967877348981,0.10602315723360006,8.489339565704819E-2,0.19254183796089136,0.19388886625336976,0.12896547221386817,5.0561562790971846E-3,4.4528358088852414E-3,2.9713727217026082E-3,1.7222901104686913E-3,9.1464986410565406E-3,1.4215948767095879E-2,3.3844432885906044E-2,9.0006269809052047E-2,6.0781208791283545E-3,0.30418920570864599,0.40326174579868601,0.65,0.61713054954550406,1.2789112467546748E-3,4.8130962187325869E-3,5.909258363416392E-2,0.18280530810970197,2.8211152009982314E-3,1.6351966805389696E-3,8.6839749734960447E-3,2.182126436087858E-3,9.1830274566044701E-2,4.9212763841533118E-6,1.0694963396078573E-5,8.5454798076617225E-2,0.44061300138291637,0.61713054954550406,61.713054954550408,130,50.254747979561841,0.50254747979561842,404.80325535320367,null,8.0600473714797005E-2,null,0.30418920570864599,9.0006269809052047E-2,9.9056092102066298E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR32, IF(MODE_ILIM=4,#REF!,#REF!))","v":61.713054954550408},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ32, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.30418920570864599},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA32, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0006269809052047E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB32, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9056092102066298E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S32, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":404.80325535320367},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P32, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7722316377765688}]
["Controller",null,"Units","Std Units","Description",null,null,27,0.13500000000000001,0.16548086727366729,0.21769627638892708,5.2379367415566605E-2,1.7720765029312209,1.7720765029312209,1,1.7720765029312209,2.225067225326339E-6,9.8874068040782193E-2,404988.18269504386,2.4692078503263392E-6,0,6.6E-4,0.1431010802319862,2.4573502996273621E-3,9.6765500760902526E-2,9.9261878453611424E-2,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,4.2971689406577265E-2,5.539698271366035E-6,5.539698271366035E-6,4.4997057378362008E-2,1.3909930636528715E-3,1.6260275535206013E-3,42.666666666666664,37.714365318209907,0.10828336753470694,8.4932177731527669E-2,0.19484157281975523,0.19628306248199778,0.13338225463427045,5.4084110588016937E-3,4.4548700096454829E-3,3.2837610660720845E-3,1.7900214554147731E-3,9.5286525311323398E-3,1.4952019880490067E-2,3.3844432885906044E-2,9.0031926369560672E-2,6.0808975631660841E-3,0.30734790629521458,0.40662658904291515,0.67500000000000004,0.62406010247702803,1.3327054612424687E-3,5.0140847167566682E-3,5.7569212589271973E-2,0.1801375583713804,3.0359470628192886E-3,1.6549347746699587E-3,8.8095583334021343E-3,2.271902636751714E-3,8.9462945660873719E-2,5.1216365495118558E-6,1.0414496030255984E-5,8.323753066132189E-2,0.43254191640106993,0.62406010247702803,62.406010247702802,135,51.875007795911799,0.51875007795911798,404.98818269504386,null,7.8522642279606397E-2,null,0.30734790629521458,9.0031926369560672E-2,9.9261878453611424E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR33, IF(MODE_ILIM=4,#REF!,#REF!))","v":62.406010247702802},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ33, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.30734790629521458},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA33, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0031926369560672E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB33, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9261878453611424E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S33, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":404.98818269504386},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P33, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7720765029312209}]
["Deadtime1",20,"ns",{"$f":"B34/1000000000","v":2E-8},"PMOS off to NMOS on deadtime",null,null,28,0.14000000000000001,0.1654663803998162,0.22269629737587848,5.7386610882895678E-2,1.7719213680858739,1.7719213680858739,1,1.7719213680858739,2.2239401559065773E-6,9.8919219698442015E-2,405173.12388481846,2.4680807809065771E-6,0,6.6E-4,0.14782732887920744,2.6223502996273627E-3,9.6809689523944364E-2,9.947377663764706E-2,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,4.438341442575082E-2,5.9096624282638381E-6,5.9096624282638381E-6,4.6493802939667338E-2,1.4850698400015294E-3,1.6267700923975463E-3,42.666666666666664,36.865751774416694,0.11054560151373402,8.4970962710129494E-2,0.19714333431626108,0.19868297515076977,0.13781897359351386,5.7741971226403796E-3,4.4569043627330036E-3,3.5964335817568888E-3,1.8578950354608782E-3,9.9112329799507723E-3,1.5702199073863127E-2,3.3844432885906044E-2,9.0057584851312322E-2,6.0836744551305503E-3,0.31052643353107573,0.41001738442696889,0.70000000000000007,0.63062075407167184,1.387042091510586E-3,5.2170048642092761E-3,5.612238807655856E-2,0.17760382592389179,3.2399795104231612E-3,1.6737530974976493E-3,8.9288988794236843E-3,2.3624407477015456E-3,8.72145705843346E-2,5.3239368240296696E-6,1.0148125584197001E-5,8.1131688669725921E-2,0.42489706450768494,0.63062075407167184,63.062075407167185,140,53.420714247122767,0.53420714247122769,405.17312388481844,null,7.6549217969225383E-2,null,0.31052643353107573,9.0057584851312322E-2,9.947377663764706E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR34, IF(MODE_ILIM=4,#REF!,#REF!))","v":63.062075407167185},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ34, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.31052643353107573},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA34, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0057584851312322E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB34, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.947377663764706E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S34, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":405.17312388481844},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P34, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7719213680858739}]
["Deadtime2",20,"ns",{"$f":"B35/1000000000","v":2E-8},"NMOS off to PMOS on deadtime",null,null,29,0.14499999999999999,0.16545189352596509,0.22769631836282983,6.2393854350224751E-2,1.7717662332405262,1.7717662332405262,1,1.7717662332405262,2.2228140306324685E-6,9.8964374737324945E-2,405358.07892408298,2.4669546556324683E-6,0,6.6E-4,0.15257102989611543,2.793350299627362E-3,9.6853881596102087E-2,9.969178774935826E-2,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,4.5801386111241446E-2,6.2933009091330623E-6,6.2933009091330623E-6,4.7996715671052355E-2,1.5826313993477883E-3,1.6275126868801934E-3,42.666666666666664,36.054487261635146,0.1128098593979988,8.5009750593179861E-2,0.19944712267805886,0.20108861425861965,0.14227397354929053,6.153532599049283E-3,4.4589388681649132E-3,3.9093903006776638E-3,1.92591096845461E-3,1.0294240137297185E-2,1.6466513206760115E-2,3.3844432885906044E-2,9.0083245254522826E-2,6.0864515550451068E-3,0.31372482427494769,0.41343416992103288,0.72499999999999998,0.63683963390723708,1.4418853754843376E-3,5.4217215474927872E-3,5.4746480359057624E-2,0.17519425184847837,3.4340064660469891E-3,1.6917192221911259E-3,9.042455338468312E-3,2.4536774926749798E-3,8.5076400687112474E-2,5.5280323407453545E-6,9.8948152782414512E-6,7.9129077143539547E-2,0.41764709832816554,0.63683963390723708,63.683963390723704,145,54.888490199331855,0.54888490199331852,405.35807892408297,null,7.4672521994905094E-2,null,0.31372482427494769,9.0083245254522826E-2,9.969178774935826E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR35, IF(MODE_ILIM=4,#REF!,#REF!))","v":63.683963390723704},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ35, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.31372482427494769},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA35, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0083245254522826E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB35, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.969178774935826E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S35, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":405.35807892408297},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P35, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7717662332405262}]
["Sleep delay",5,"µs",{"$f":"B36/1000000","v":5.0000000000000004E-6},"Delay time to enter sleep mode",null,null,30,0.15,0.16543740665211398,0.23269633934978123,6.7401097817553823E-2,1.7716110983951787,1.7716110983951787,1,1.7716110983951787,2.2216888483181431E-6,9.9009533157810886E-2,405543.04781439336,2.4658294733181429E-6,0,6.6E-4,0.15733060466279708,2.9703502996273616E-3,9.6898076977747452E-2,9.9915912919275179E-2,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,4.7225099241974787E-2,6.6906299952431031E-6,6.6906299952431031E-6,4.9505302450113767E-2,1.683682404855264E-3,1.6282553369747893E-3,42.666666666666664,35.27815917294204,0.11507614141485278,8.504854138100508E-2,0.20175293813283265,0.20349998983639131,0.14674579276650504,6.5464356191796925E-3,4.4609735259583273E-3,4.2226312547598375E-3,1.9940693722612251E-3,1.0677674152979389E-2,1.7244989371843544E-2,3.3844432885906044E-2,9.0108907579408037E-2,6.0892288629331168E-3,0.31694311565057603,0.41687698379566429,0.75,0.64274127471464038,1.4972029852502321E-3,5.6281127403008053E-3,5.343639854272255E-2,0.17289992084389444,3.6187458604456254E-3,1.70889425359547E-3,9.1506425280980536E-3,2.545555650575339E-3,8.3040524685432993E-2,5.7337920690487467E-6,9.6536275667764324E-6,7.7222285494309914E-2,0.41076367100426125,0.64274127471464038,64.274127471464041,150,56.276153038808332,0.5627615303880833,405.54304781439333,null,7.2885610533130724E-2,null,0.31694311565057603,9.0108907579408037E-2,9.9915912919275179E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR36, IF(MODE_ILIM=4,#REF!,#REF!))","v":64.274127471464041},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ36, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.31694311565057603},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA36, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0108907579408037E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB36, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9915912919275179E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S36, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":405.54304781439333},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P36, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7716110983951787}]
["IQ(active)",660,"µA",{"$f":"B37/1000000","v":6.6E-4},"LM5164 quiescent current - active state ",null,null,31,0.155,0.1654229197782629,0.23769636033673264,7.2408341284882924E-2,1.7714559635498313,1.7714559635498313,1,1.7714559635498313,2.2205646077797188E-6,9.9054694960279605E-2,405728.03055730526,2.464705232779719E-6,0,6.6E-4,0.16210465497190804,3.1533502996273616E-3,9.6942275669252176E-2,0.10014615331328866,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,4.8654105570593277E-2,7.1016659666233067E-6,7.1016659666233067E-6,5.1019126481521182E-2,1.7882275203860325E-3,1.6289980426875809E-3,42.666666666666664,34.534558315267923,0.11734444779168149,8.5087335073931403E-2,0.20406078090830049,0.20591711194695705,0.1512331364772464,6.9529243168986125E-3,4.4630083361303589E-3,4.5361564759336098E-3,2.0623703647636299E-3,1.1061535176827599E-2,1.8037654896132963E-2,3.3844432885906044E-2,9.0134571826183812E-2,6.0920063788179393E-3,0.32018134504809176,0.42034586462316487,0.77500000000000002,0.64834791580955542,1.5529656257620289E-3,5.8360679747736441E-3,5.2187527614663894E-2,0.17071275096821542,3.794848512203321E-3,1.7253335840282478E-3,9.2538364871616197E-3,2.6380233478462416E-3,8.1099770818058095E-2,5.9410971977237071E-6,9.4237125431123203E-6,7.5404595852765099E-2,0.40422108559521841,0.64834791580955542,64.834791580955539,155,57.582635216683897,0.57582635216683897,405.72803055730526,null,7.1182188847706718E-2,null,0.32018134504809176,9.0134571826183812E-2,0.10014615331328866,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR37, IF(MODE_ILIM=4,#REF!,#REF!))","v":64.834791580955539},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ37, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.32018134504809176},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA37, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0134571826183812E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB37, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10014615331328866},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S37, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":405.72803055730526},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P37, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7714559635498313}]
["IQ(sleep)",10,"µA",{"$f":"B38/1000000","v":1.0000000000000001E-5},"LM5164 quiescent current - sleep state",null,null,32,{"$f":"IF(PLOT_TYPE=1, H38/100*Iout, min_I*EXP(H38*rr/100))","v":0.16},{"$f":"IF(I38<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I38-Vout)/L*OnTime)","v":0.16540843290441176},{"$f":"IF(I38<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I38+((Vin-(Rdcr+RdsonTop)*J38-Vout)/L*OnTime)/2)","v":0.24269638132368404},{"$f":"IF(I38<Icrit, 0, I38-((Vin-(Rdcr+RdsonTop)*K38-Vout)/L*OnTime)/2)","v":7.7415584752212011E-2},1.7713008287044836,{"$f":"IF(I38<Icrit, 1000*SQRT((J38*CoutEsr)^2+(((J38/2)-I38)*(OnTime+OffTime)/Cout)^2), 1000*J38*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":1.7713008287044836},1,{"$f":"IF(I38<Icrit, 1000*((N38/1000)*O38), 1000*J38*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":1.7713008287044836},{"$f":"IF(I38<Icrit, L*J38/(Vout+J38/2*(RdsonBot+Rdcr)), L*J38/(Vout+I38*(RdsonBot+Rdcr)))","v":2.2194413078352909E-6},9.9099860145111171E-2,{"$f":"IF(I38<Icrit,I38/((OnTime+Q38)*J38/2),1/(OnTime+Q38))","v":405913.02715437533},2.4635819328352911E-6,0,{"$f":"S38*(T38*Iq_active+U38*Iq_sleep)","v":6.6E-4},0.16689193858171028,{"$f":"W38^2*Rdcr","v":3.3423502996273624E-3},{"$f":"Core_Loss/1000*S38/$S$106","v":9.6986477670988183E-2},{"$f":"(Y38+X38*(1+Ltc*(Ta-25)))/(1-X38*Ltc*ThetaCa)","v":0.10038251013266662},4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,5.0088006222588195E-2,7.5264251020621022E-6,7.5264251020621022E-6,5.2537799665973987E-2,1.8962714105007653E-3,1.6297408040248172E-3,{"$f":"20*VIN_nom/24","v":42.666666666666664},{"$f":"IF(I38<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I38+Iripple/2)*1000000000)","v":33.821657913932626},{"$f":"IF(I38<Icrit, Vin*(I38+Iripple/2)*AK38/1000000000/2*S38, Vin*(I38-Iripple/2)*AJ38/1000000000/2*S38 + Vin*(I38+Iripple/2)*AK38/1000000000/2*S38)","v":0.11961477875590464},{"$f":"IF(I38<Icrit, Csw*(Vin)^2*S38/2, Csw*Vin^2*S38/2)","v":8.5126131672285263E-2},0.20637065123221471,{"$f":"(AI38+AL38+AM38+AH38*(1+RdsonTopTc*(Ta-25)))/(1-AH38*RdsonTopTc*ThetaJA)","v":0.20833999068533718},{"$f":"IF(I38<Icrit,Iripple*SQRT((OffTime)*S38/3), SQRT(OffTime*S38*(I38^2+Iripple^2/12)))","v":0.15573485426051487},7.3730168287893172E-3,{"$f":"QgBot*S38*Vdd","v":4.4650432986981289E-3},{"$f":"IF(I38<Icrit, Vin*Idss*R38, QrrBot*(I38-Iripple/2)/1*S38*Vin+Vin*Idss*R38)","v":4.849965996133976E-3},{"$f":"IF(I38<Icrit, dead1*S38*(I38+Iripple/2)*((I38+Iripple/2)*BDserR+VSD), dead1*S38*(I38+Iripple/2)*((I38+Iripple/2)*BDserR+VSD)+dead2*S38*(I38-Iripple/2)*((I38-Iripple/2)*BDserR+VSD))","v":2.1308140638623936E-3},1.1445823358694499E-2,{"$f":"(AR38+AS38+AT38+AQ38*(1+RdsonBotTc*(Ta-25)))/(1-AQ38*RdsonBotTc*ThetaJA)","v":1.8844537342255982E-2},{"$f":"Vin*V38+Vout*Ifb/0.8","v":3.3844432885906044E-2},{"$f":"(Vin-Vdd)*(S38*QgBot+S38*QgTop)+AW38","v":9.0160237995066075E-2},{"$f":"AI38+AR38","v":6.0947841027229463E-3},0.32343955012538217,{"$f":"SUM(Z38,AC38,AF38,AZ38)","v":0.42384085127896864},{"$f":"Vout*I38","v":0.8},0.65367976494980051,1.6091466885293315E-3,6.0454870221315904E-3,{"$f":"Vin*S38*(QgBot+QgTop)/($BB38+$BA38)","v":5.0995674108002778E-2},0.16862539848751421,3.9629057904592277E-3,1.7410875455216234E-3,9.3523789034604451E-3,{"$f":"X38/($BB38+$BA38)","v":2.7310334478003869E-3},{"$f":"Y38/($BB38+$BA38)","v":7.9247622409100785E-2},6.1498397395352912E-6,9.2042979330480379E-6,7.3669903975541073E-2,0.39799599251573398,{"$f":"BC38","v":0.65367976494980051},65.367976494980056,{"$f":"I38*1000","v":160},58.807882255999409,0.58807882255999411,{"$f":"S38/1000","v":405.91302715437536},null,{"$f":"AM38/($BB38+$BA38)","v":6.9556537178281502E-2},null,0.32343955012538217,9.0160237995066075E-2,0.10038251013266662,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR38, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.367976494980056},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ38, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.32343955012538217},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA38, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0160237995066075E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB38, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10038251013266662},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S38, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":405.91302715437536},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P38, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7713008287044836}]
["High-side N-ch MOSFET",null,"Units","Std Units","Description",null,null,33,0.16500000000000001,0.16539394603056068,0.24769640231063544,8.2422828219541097E-2,{"$f":"IF(I39<Icrit, 1000*((((J39/2)-I39)*0.000002/Cout+Vout/306)), 1000*J39*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":1.7711456938591361},1.7711456938591361,1,1.7711456938591361,2.2183189473049346E-6,9.9145028712685504E-2,406098.03760715981,{"$f":"IF(1/S39-OnTime-Q39>Tsleep, OnTime+Q39+Tsleep, 1/S39)","v":2.4624595723049344E-6},{"$f":"IF(1/S39-OnTime-Q39>Tsleep, 1/S39-OnTime-Q39-Tsleep, 0)","v":0},6.6E-4,{"$f":"IF(I39<Icrit,Iripple*SQRT((OnTime+OffTime)*S39/3), SQRT(I39^2+Iripple^2/12))","v":0.17169134854022597},3.5373502996273623E-3,9.7030682983327315E-2,0.10062498461407061,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q39)*S39)","v":4.7464925614198031E-2},1.1264595817806762E-5,1.1264595817806762E-5,{"$f":"SQRT($R39)*SQRT($I39^2*(1-R39)+(Iripple^2)/12)","v":5.1526445246125839E-2},7.9649236791060127E-6,7.9649236791060127E-6,{"$f":"IF(I39<Icrit,Iripple*SQRT((OnTime)*S39/3), SQRT(OnTime*S39*(I39^2+Iripple^2/12)))","v":5.4060976146028963E-2},{"$f":"RdsonTop*AG39^2","v":2.0078187404588593E-3},{"$f":"QgTop*S39*Vdd","v":1.6304836209927467E-3},42.666666666666664,33.137595165053938,0.12188713453497582,8.5164931176393052E-2,0.20868254933236163,0.21076863617881944,0.16024992091048032,{"$f":"RdsonBot*AP39^2","v":7.80673129415182E-3},4.4670784136787581E-3,5.1640598473007048E-3,2.199400587475741E-3,1.1830538848455203E-2,1.966566450971052E-2,3.3844432885906044E-2,9.0185906086270751E-2,6.0975620346715043E-3,0.32671776880947223,0.42736198294303973,0.82500000000000007,0.65875522511571072,1.6657219516960434E-3,6.2562787500486383E-3,4.9857019045168573E-2,0.1666311754704973,4.1234562511752457E-3,1.7562019746935854E-3,9.4465809483082024E-3,2.8245430217504843E-3,7.747814474159144E-2,6.3599213227381036E-6,8.9946804288445895E-6,7.2012650746818938E-2,0.39206712750350009,0.65875522511571072,65.875522511571077,165,59.95273560232264,0.59952735602322638,406.09803760715982,null,6.8003446556447036E-2,null,0.32671776880947223,9.0185906086270751E-2,0.10062498461407061,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR39, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.875522511571077},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ39, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.32671776880947223},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA39, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0185906086270751E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB39, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10062498461407061},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S39, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":406.09803760715982},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P39, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7711456938591361}]
["RdsonTop",687,"mW",{"$f":"B40/1000","v":0.68700000000000006},"Drain-source resistance of high-side MOSFET @ VDD, 25°C",null,null,34,0.17,0.16537945915670957,0.25269642329758685,8.7430071686870184E-2,1.7709905590137887,1.7709905590137887,1,1.7709905590137887,2.2171975250106963E-6,9.9190200663382647E-2,406283.06191721529,2.4613381500106965E-6,0,6.6E-4,0.17650189563730287,3.7383502996273621E-3,9.7074891606641484E-2,0.10087357802957306,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,5.2969104120731865E-2,8.4171779740588006E-6,8.4171779740588006E-6,5.5588346828123879E-2,2.1228741762185639E-3,1.6312264935976195E-3,42.666666666666664,32.480654982255011,0.12416151535638278,8.5203733586581204E-2,0.21099647543656161,0.21320305858707939,0.16477742019842417,8.2540858550034062E-3,4.4691136810893683E-3,5.4784380613783516E-3,2.2681300535395657E-3,1.2215681796007285E-2,2.0501064436138739E-2,3.3844432885906044E-2,9.0211576100013818E-2,6.1003401746869881E-3,0.3300160392979189,0.43090929910128384,0.85000000000000009,0.66359109157563301,1.722669319417048E-3,6.4683601297489774E-3,4.8768077047003575E-2,0.16472397818065782,4.2769914038583001E-3,1.7707187036044931E-3,9.5367266086506617E-3,2.9185128894374302E-3,7.5785921512749974E-2,6.5712521409318283E-6,8.7942181587019993E-6,7.0427762655254647E-2,0.38641508392068247,0.66359109157563301,66.359109157563296,170,61.018807215515402,0.61018807215515403,406.28306191721532,null,6.6518163031810407E-2,null,0.3300160392979189,9.0211576100013818E-2,0.10087357802957306,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR40, IF(MODE_ILIM=4,#REF!,#REF!))","v":66.359109157563296},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ40, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.3300160392979189},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA40, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0211576100013818E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB40, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10087357802957306},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S40, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":406.28306191721532},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P40, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7709905590137887}]
["RdsonTopTc",4500,"ppm/°C",{"$f":"B41/1000000","v":4.4999999999999997E-3},"Drain to Source Resistance Temp Co",null,null,35,0.17499999999999999,0.16536497228285849,0.25769644428453825,9.2437315154199243E-2,1.7708354241684412,1.7708354241684412,1,1.7708354241684412,2.2160770397765908E-6,9.9235375997582767E-2,406468.100086099,2.4602176647765906E-6,0,6.6E-4,0.18132269345992341,3.9453502996273622E-3,9.7119103541302793E-2,0.10112829168667524,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,5.4415697067361268E-2,8.8832042619804898E-6,8.8832042619804898E-6,5.7119634717093054E-2,2.2414423844371156E-3,1.6319694218456875E-3,42.666666666666664,31.849255639081999,0.12643792144764746,8.5242538903176276E-2,0.2133124297726694,0.21564326810230142,0.16931653104310529,8.7150986560791347E-3,4.471149100947089E-3,5.7931006703162624E-3,2.3370025800074257E-3,1.2601252351270777E-2,2.1350765398612435E-2,3.3844432885906044E-2,9.02372480365113E-2,6.1031185227927763E-3,0.33333440006021792,0.43448283954697298,0.875,0.66820272368190325,1.7799685946540483E-3,6.6816553704274811E-3,4.7725660685266451E-2,0.16289822465063133,4.4239607388214695E-3,1.7846759876715393E-3,9.6230755919109959E-3,3.0129072183888192E-3,7.4165999437535199E-2,6.7837500375749195E-6,8.6023241218677204E-6,6.891059990349295E-2,0.38102211425295979,0.66820272368190325,66.820272368190331,175,62.00835196729512,0.62008351967295117,406.46810008609901,null,6.5096339049900559E-2,null,0.33333440006021792,9.02372480365113E-2,0.10112829168667524,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR41, IF(MODE_ILIM=4,#REF!,#REF!))","v":66.820272368190331},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ41, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.33333440006021792},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA41, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.02372480365113E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB41, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10112829168667524},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S41, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":406.46810008609901},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P41, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7708354241684412}]
["QgTop",0.80300000000000005,"nC",{"$f":"B42/1000000000","v":8.0300000000000002E-10},"Gate charge of high-side MOSFET @ VDD",null,null,36,0.18,0.16535048540900738,0.26269646527148965,9.7444558621528329E-2,1.7706802893230937,1.7706802893230937,1,1.7706802893230937,2.214957490428598E-6,9.9280554715665992E-2,406653.15211536788,2.4590981154285978E-6,0,6.6E-4,0.18615294562150056,4.158350299627361E-3,9.7163318787683223E-2,0.10138912692832519,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,5.5865967030284472E-2,9.3630188166864953E-6,9.3630188166864953E-6,5.8654590929231643E-2,2.3635280324708703E-3,1.6327124057432022E-3,42.666666666666664,31.241936054092591,0.1287163530363257,8.5281347126504814E-2,0.21563041256857371,0.21808927494929975,0.17386651569250988,9.1897878448323495E-3,4.4731846732690471E-3,6.1080477060685649E-3,2.4060182848505514E-3,1.2987250664188165E-2,2.2214795914930217E-2,3.3844432885906044E-2,9.0262921895979231E-2,6.1058970790122489E-3,0.33667288983922145,0.43808264438218114,0.89999999999999991,0.67260419509853786,1.8376012804959033E-3,6.8960951623452159E-3,4.6726849310532823E-2,0.16114880009383464,4.5647761232930203E-3,1.7981088798602999E-3,9.7058658661435919E-3,3.1076931735762501E-3,7.2613839806991473E-2,6.9973397054332059E-6,8.4184604479403041E-6,6.7456911032319225E-2,0.3758719565295458,0.67260419509853786,67.26041950985379,180,62.924142868481049,0.62924142868481048,406.6531521153679,null,6.3733990934379758E-2,null,0.33667288983922145,9.0262921895979231E-2,0.10138912692832519,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR42, IF(MODE_ILIM=4,#REF!,#REF!))","v":67.26041950985379},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ42, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.33667288983922145},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA42, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0262921895979231E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB42, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10138912692832519},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S42, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":406.6531521153679},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P42, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7706802893230937}]
["Coss",100,"pF",{"$f":"B43/1000000000000","v":1E-10},"Capacitance (Coss)",null,null,37,0.185,0.16533599853515626,0.26769648625844106,0.10245180208885742,1.7705251544777463,1.7705251544777463,1,1.7705251544777463,2.2138388757946588E-6,9.9325736818012489E-2,406838.21800657915,2.457979500794659E-6,0,6.6E-4,0.19099193481286414,4.3773502996273606E-3,9.7207537346154865E-2,0.10165608513293672,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,5.7319682223900041E-2,9.856637910746648E-6,9.856637910746648E-6,6.0192991273973324E-2,2.4891357883754283E-3,1.6334554452964152E-3,42.666666666666664,30.657344503454638,0.13099681035000743,8.5320158256893361E-2,0.21795042405219722,0.22054108938564018,0.1784267095911104,9.6781715714351745E-3,4.4752203980723713E-3,6.423279200594172E-3,2.4751772860578435E-3,1.3373676884724385E-2,2.3093184744926422E-2,3.3844432885906044E-2,9.0288597678633634E-2,6.1086758433687863E-3,0.34003154765256899,0.44170875401923426,0.92500000000000004,0.67680842555500464,1.8955504059107683E-3,7.1116160130084679E-3,4.5768961713415685E-2,0.15947100902898725,4.6998156569236218E-3,1.8110495588608848E-3,9.7853158878180215E-3,3.2028406101551584E-3,7.1125276003600413E-2,7.2119519844737396E-6,8.242133362122469E-6,6.6062793124805702E-2,0.37094968208883261,0.67680842555500464,67.680842555500462,185,63.769353027551922,0.63769353027551923,406.83821800657915,null,6.2427461597785755E-2,null,0.34003154765256899,9.0288597678633634E-2,0.10165608513293672,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR43, IF(MODE_ILIM=4,#REF!,#REF!))","v":67.680842555500462},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ43, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.34003154765256899},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA43, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0288597678633634E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB43, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10165608513293672},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S43, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":406.83821800657915},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P43, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7705251544777463}]
["Low-side N-ch MOSFET",null,"Units","Std Units","Description",null,null,38,0.19,0.16532151166130518,0.27269650724539246,0.10745904555618652,1.7703700196323988,1.7703700196323988,1,1.7703700196323988,2.2127211947046688E-6,9.9370922305002635E-2,407023.2977612908,2.4568618197046685E-6,0,6.6E-4,0.19583901338487525,4.602350299627361E-3,9.725175921708995E-2,0.1019291677144087,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,5.8776633156054789E-2,1.0364077815484317E-5,1.0364077815484317E-5,6.1734633313661968E-2,2.6182703209057718E-3,1.6341985405115827E-3,42.666666666666664,30.094228577510762,0.13327929361631696,8.535897229466867E-2,0.22027246445149723,0.22299872170176313,0.18299651266431152,1.0180267988779057E-2,4.4772562753741989E-3,6.7387951858567932E-3,2.5444797016358871E-3,1.3760531162866879E-2,2.3985960891792106E-2,3.3844432885906044E-2,9.0314275384690668E-2,6.1114548158857813E-3,0.3434104127941317,0.4453612091821737,0.95,0.68082729672326092,1.9538003724954992E-3,7.3281596633450836E-3,4.4849532080191289E-2,0.15786053317377208,4.8294270626932688E-3,1.823527617717864E-3,9.8616265611482616E-3,3.2983218032303016E-3,6.9696476136160881E-2,7.4275232443639028E-6,8.0728887571763455E-6,6.4724656805977998E-2,0.36624156168873401,0.68082729672326092,68.082729672326096,190,64.547447140017496,0.645474471400175,407.02329776129079,null,6.117338774574211E-2,null,0.3434104127941317,9.0314275384690668E-2,0.1019291677144087,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR44, IF(MODE_ILIM=4,#REF!,#REF!))","v":68.082729672326096},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ44, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.3434104127941317},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA44, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0314275384690668E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB44, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1019291677144087},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S44, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":407.02329776129079},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P44, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7703700196323988}]
["RdsonBot",304,"mW",{"$f":"B45/1000","v":0.30399999999999999},"Drain-source resistance of low-side MOSFET @ VDD, 25°C",null,null,39,0.19500000000000001,0.16530702478745407,0.27769652823234386,0.11246628902351559,1.7702148847870514,1.7702148847870514,1,1.7702148847870514,2.2116044459904768E-6,9.9416111177016708E-2,407208.39138106041,2.4557450709904766E-6,0,6.6E-4,0.20069359522306973,4.833350299627363E-3,9.7295984400860652E-2,0.10220837612214471,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,6.0236630054520422E-2,1.088535480097546E-5,1.088535480097546E-5,6.3279333826641276E-2,2.7509362995163894E-3,1.6349416913949576E-3,42.666666666666664,29.551426224249038,0.1355638030629123,8.5397789240157368E-2,0.22259653399446463,0.22546218222110542,0.18757538179842903,1.0696095252475231E-2,4.4792923051916646E-3,7.0545956938249154E-3,2.6139256496089409E-3,1.4147813648625522E-2,2.4893153603407811E-2,3.3844432885906044E-2,9.0339955014366438E-2,6.1142339965866224E-3,0.34680952483546629,0.44904005090822979,0.97500000000000009,0.68467175440617756,2.012336819328307E-3,7.5456725728529081E-3,4.3966288788798831E-2,0.15631339431253788,4.9539306772485841E-3,1.8355703183641648E-3,9.9349829659652299E-3,3.3941112095440926E-3,6.8323910088629064E-2,7.6439948399154618E-6,7.9103082884658926E-6,6.3439195377088642E-2,0.36173494743348611,0.68467175440617756,68.467175440617751,195,65.262084299350803,0.65262084299350809,407.20839138106044,null,5.9968670955351314E-2,null,0.34680952483546629,9.0339955014366438E-2,0.10220837612214471,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR45, IF(MODE_ILIM=4,#REF!,#REF!))","v":68.467175440617751},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ45, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.34680952483546629},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA45, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0339955014366438E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB45, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10220837612214471},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S45, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":407.20839138106044},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P45, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7702148847870514}]
["RdsonBotTc",4500,"ppm/°C",{"$f":"B46/1000000","v":4.4999999999999997E-3},"Drain To Source Resitance Temp Co",null,null,40,0.2,0.16529253791360296,0.28269654921929521,0.11747353249084468,1.7700597499417037,1.7700597499417037,1,1.7700597499417037,2.2104886284858794E-6,9.9461303434435114E-2,407393.49886744621,2.4546292534858796E-6,0,6.6E-4,0.20555514871576766,5.0703502996273632E-3,9.7340212897839312E-2,0.10249371184107361,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,6.1699500635601284E-2,1.142048513604769E-5,1.142048513604769E-5,6.4826926611691496E-2,2.8871383943614155E-3,1.6356848979527966E-3,42.666666666666664,29.027857744881448,0.13785033891748591,8.5436609093686264E-2,0.22492263290912495,0.22793148130022475,0.19216282433250437,1.122567152085526E-2,4.4813284875419085E-3,7.3706807564718289E-3,2.6835152480189526E-3,1.453552449203269E-2,2.5814792373688701E-2,3.3844432885906044E-2,9.0365636567877133E-2,6.1170133854947049E-3,0.35022892362728525,0.45274532054931271,1,0.68835189888746617,2.0711465034780447E-3,7.7641054643983231E-3,4.3117135661315371E-2,0.15482592146576465,5.0736220948106887E-3,1.8472028166673156E-3,1.0005555885415974E-2,3.4901852567731282E-3,6.7004320386337912E-2,7.8613126296145093E-6,7.7540059213870945E-6,6.2203357525672874E-2,0.35741816837918527,0.68835189888746617,68.835189888746612,200,65.91703305041338,0.65917033050413376,407.39349886744623,null,5.8810452104145094E-2,null,0.35022892362728525,9.0365636567877133E-2,0.10249371184107361,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR46, IF(MODE_ILIM=4,#REF!,#REF!))","v":68.835189888746612},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ46, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.35022892362728525},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA46, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0365636567877133E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB46, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10249371184107361},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S46, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":407.39349886744623},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P46, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7700597499417037}]
["QgBot",2.2000000000000002,"nC",{"$f":"B47/1000000000","v":2.2000000000000003E-9},"Gate charge of low-side MOSFET at VDD",null,null,41,0.20499999999999999,0.16527805103975182,0.28769657020624662,0.12248077595817373,1.769904615096356,1.769904615096356,1,1.769904615096356,2.2093737410266179E-6,9.9506499077638297E-2,407578.62022200646,2.4535143660266181E-6,0,6.6E-4,0.21042319065055862,5.3133502996273599E-3,9.7384444708398202E-2,0.10278517639167004,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,6.3165088163951735E-2,1.1969485088279387E-5,1.1969485088279387E-5,6.6377260582285713E-2,3.02688127629475E-3,1.6364281601913559E-3,42.666666666666664,28.522518625504699,0.14013890140776417,8.5475431855582137E-2,0.22725076142353767,0.23040662932892303,0.19675839240921589,1.176901495497153E-2,4.4833648224420711E-3,7.6870504057755988E-3,2.7532486149255543E-3,1.4923663843143226E-2,2.6750906943941787E-2,3.3844432885906044E-2,9.0391320045438928E-2,6.1197929826334267E-3,0.35366864930093717,0.45647705977351327,1.0249999999999999,0.69187706501287372,2.1302171940939963E-3,7.9834129207553839E-3,4.2300135347182986E-2,0.1533947217908859,5.1887745105893088E-3,1.8584483618980022E-3,1.0073503160031881E-2,3.5865221567721473E-3,6.5734696373419541E-2,8.0794265488722917E-6,7.6036248712004237E-6,6.1014323137246466E-2,0.35328043800429565,0.69187706501287372,69.187706501287366,205,66.516098897051677,0.66516098897051679,407.57862022200646,null,5.7696088705315181E-2,null,0.35366864930093717,9.0391320045438928E-2,0.10278517639167004,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR47, IF(MODE_ILIM=4,#REF!,#REF!))","v":69.187706501287366},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ47, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.35366864930093717},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA47, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0391320045438928E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB47, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10278517639167004},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S47, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":407.57862022200646},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P47, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.769904615096356}]
["VSD",0.8,"V",{"$f":"B48","v":0.8},"Body diode forward voltage",null,null,42,0.21,0.16526356416590077,0.29269659119319802,0.12748801942550281,1.7697494802510088,1.7697494802510088,1,1.7697494802510088,2.2082597824503743E-6,9.9551698107006759E-2,407763.75544629968,2.4524004074503741E-6,0,6.6E-4,0.21529728090145808,5.5623502996273609E-3,9.7428679832909731E-2,0.10308277132997608,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,6.4633249760987943E-2,1.2532370923998745E-5,1.2532370923998745E-5,6.7930198107685122E-2,3.1701696168702021E-3,1.6371714781168931E-3,42.666666666666664,28.03447310470084,0.14242949076150765,8.5514257526171839E-2,0.22958091976579639,0.23288763673037094,0.20136167805748018,1.2326143718597785E-2,4.485401309909297E-3,8.0037046737190982E-3,2.8231258684060698E-3,1.5312231852034465E-2,2.7701527304235595E-2,3.3844432885906044E-2,9.0417005447268037E-2,6.12257278802619E-3,0.35712874226990077,0.46023531056661865,1.05,0.69525589333893612,2.1895375783088488E-3,8.2035530261524905E-3,4.1513494559907937E-2,0.15201665472889844,5.2996408028072282E-3,1.8693284739494493E-3,1.013897089076108E-2,3.6831017396490662E-3,6.4512251270536045E-2,8.2982902308758627E-6,7.4588348842012224E-6,5.9869481805020754E-2,0.34931177200110636,0.69525589333893612,69.525589333893606,210,67.063063929713536,0.6706306392971354,407.76375544629968,null,5.6623134771023279E-2,null,0.35712874226990077,9.0417005447268037E-2,0.10308277132997608,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR48, IF(MODE_ILIM=4,#REF!,#REF!))","v":69.525589333893606},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ48, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.35712874226990077},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA48, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0417005447268037E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB48, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10308277132997608},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S48, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":407.76375544629968},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P48, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7697494802510088}]
["BDserR",100,"mW",{"$f":"B49*0.001","v":0.1},"Series resistance of body diode",null,null,43,0.215,0.16524907729204966,0.29769661218014942,0.13249526289283192,1.7695943454056615,1.7695943454056615,1,1.7695943454056615,2.207146751596763E-6,9.9596900522921084E-2,407948.90454188472,2.4512873765967632E-6,0,6.6E-4,0.22017701779150645,5.8173502996273618E-3,9.7472918271746367E-2,0.10338649824762304,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,6.6103854926125818E-2,1.3109158908282865E-5,1.3109158908282865E-5,6.948561356490586E-2,3.3170080883416124E-3,1.6379148517356673E-3,42.666666666666664,27.56284839041253,0.14472210720651102,8.5553086105782272E-2,0.23191310816402896,0.23537451396123305,0.2059723089001286,1.2897075978229599E-2,4.487437949960732E-3,8.3206435922899835E-3,2.8931471265555165E-3,1.570122866880623E-2,2.8666683694782213E-2,3.3844432885906044E-2,9.0442692773580774E-2,6.1253528016963991E-3,0.36060924323129245,0.46402011523364162,1.075,0.69849639349047898,2.2490971774456621E-3,8.4244870470764916E-3,4.0755550930436639E-2,0.1506888089820852,5.4064553867295044E-3,1.8798631011501122E-3,1.0202094510260898E-2,3.7799053060097389E-3,6.3334401744936791E-2,8.5178606689573643E-6,7.3193298166194938E-6,5.8766413692942859E-2,0.34550291506955955,0.69849639349047898,69.849639349047905,215,67.561637846160409,0.67561637846160405,407.9489045418847,null,5.5589322880808673E-2,null,0.36060924323129245,9.0442692773580774E-2,0.10338649824762304,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR49, IF(MODE_ILIM=4,#REF!,#REF!))","v":69.849639349047905},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ49, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.36060924323129245},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA49, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0442692773580774E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB49, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10338649824762304},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S49, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":407.9489045418847},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P49, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7695943454056615}]
["QrrBot",3,"nC",{"$f":"B50*0.000000001","v":3.0000000000000004E-9},"Reverse recovery charge of body diode at 100mA",null,null,44,0.22,0.16523459041819855,0.30269663316710083,0.13750250636016098,1.7694392105603136,1.7694392105603136,1,1.7694392105603136,2.2060346473073346E-6,9.964210632576187E-2,408134.06751032063,2.4501752723073348E-6,0,6.6E-4,0.22506203403408881,6.0783502996273617E-3,9.7517160025280616E-2,0.10369635877185376,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,6.7576784240735641E-2,1.3699865304956811E-5,1.3699865304956811E-5,7.1043392071365799E-2,3.4674013636629857E-3,1.6386582810539374E-3,42.666666666666664,27.106829450898438,0.14701675097060318,8.5591917594740413E-2,0.23424732684639754,0.23786727151179346,0.21058994439716333,1.3481829903084903E-2,4.4894747426135273E-3,8.6378671934807059E-3,2.9633125074866105E-3,1.6090654443580845E-2,2.9646406607331973E-2,3.3844432885906044E-2,9.0468382024593424E-2,6.1281330236674647E-3,0.36411019316738624,0.4678315164003628,1.1000000000000001,0.70160600070441692,2.3088862722361082E-3,8.6461791474087956E-3,4.0024761274367965E-2,0.14940848196763762,5.5094358693035302E-3,1.8900707611045984E-3,1.0262999738979555E-2,3.8769154950927705E-3,6.2198749677627063E-2,8.7380979152726764E-6,7.1848254738937296E-6,5.7702872456794861E-2,0.34184527558394201,0.70160600070441692,70.160600070441689,220,68.015419380100283,0.68015419380100284,408.13406751032062,null,5.4592548178425307E-2,null,0.36411019316738624,9.0468382024593424E-2,0.10369635877185376,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR50, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.160600070441689},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ50, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.36411019316738624},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA50, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0468382024593424E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB50, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10369635877185376},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S50, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":408.13406751032062},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P50, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7694392105603136}]
["TrrBot",20,"ns",{"$f":"B51*0.000000001","v":2E-8},"Reverse recovery time of body diode (not used)",null,null,45,0.22500000000000001,0.16522010354434744,0.30769665415405223,0.1425097498274901,1.7692840757149662,1.7692840757149662,1,1.7692840757149662,2.2049234684255653E-6,9.9687315515909813E-2,408319.24435316661,2.4490640934255655E-6,0,6.6E-4,0.22995199317153428,6.3453502996273616E-3,9.7561405093885015E-2,0.10401235456554557,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,6.9051928229395279E-2,1.4304506376592669E-5,1.4304506376592669E-5,7.2603428372789089E-2,3.6213541164886258E-3,1.6394017660779641E-3,42.666666666666664,26.66565431436517,0.14931342228164707,8.5630751993373222E-2,0.23658357604109825,0.24036591990608155,0.21521427254923506,1.4080423665104515E-2,4.4915116878848334E-3,8.9553755092885122E-3,3.0336221293297658E-3,1.648050932650311E-2,3.0640726786580825E-2,3.3844432885906044E-2,9.0494073200522288E-2,6.1309134539627979E-3,0.36763163334714744,0.47166955701488739,1.125,0.70459162639969497,2.3688958359391042E-3,8.8685961336617911E-3,3.9319691098734767E-2,0.14817316144200296,5.6087845289863013E-3,1.8999686666547248E-3,1.0321803440227704E-2,3.9741161668357637E-3,6.110306585683549E-2,8.958964811313988E-6,7.0550576782254823E-6,5.6676769969679151E-2,0.33833086716204724,0.70459162639969497,70.459162639969492,225,68.427867006324419,0.68427867006324417,408.3192443531666,null,5.3630854059413119E-2,null,0.36763163334714744,9.0494073200522288E-2,0.10401235456554557,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR51, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.459162639969492},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ51, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.36763163334714744},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA51, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0494073200522288E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB51, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10401235456554557},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S51, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":408.3192443531666},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P51, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7692840757149662}]
["Idss",0,"μA",{"$f":"B52/1000000","v":0},"Leakage current of low-side device",null,null,46,0.23,0.16520561667049635,0.31269667514100363,0.14751699329481915,1.7691289408696189,1.7691289408696189,1,1.7691289408696189,2.2038132137968564E-6,9.9732528093745679E-2,408504.43507198227,2.4479538387968561E-6,0,6.6E-4,0.23484658644221626,6.6183502996273623E-3,9.7605653477932222E-2,0.10433448732723377,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,7.0529186356922943E-2,1.4923098384508696E-5,1.4923098384508696E-5,7.4165625864897597E-2,3.778871021173262E-3,1.6401453068140086E-3,42.666666666666664,26.238609820251199,0.15161212136753982,8.5669589302007784E-2,0.23892185597636162,0.24287046970199919,0.21984500699769779,1.4692875438952608E-2,4.4935487857918057E-3,9.2731685717154459E-3,3.1040761102331029E-3,1.6870793467740355E-2,3.1649675231590464E-2,3.3844432885906044E-2,9.0519766301583773E-2,6.1336940926058139E-3,0.37117360532777927,0.47553428034921535,1.1500000000000001,0.70745970349695997,2.4291174744031129E-3,9.0917072266695868E-3,3.8639005198211021E-2,0.1469805090330262,5.7046896419331618E-3,1.9095728387630501E-3,1.0378614386474817E-2,4.0714922961855556E-3,6.0045275364456467E-2,9.1804267464004209E-6,6.9297805367640574E-6,5.5686162633332655E-2,0.33495225630073883,0.70745970349695997,70.745970349695995,230,68.802277733330541,0.68802277733330541,408.50443507198224,null,5.2702419344612832E-2,null,0.37117360532777927,9.0519766301583773E-2,0.10433448732723377,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR52, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.745970349695995},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ52, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.37117360532777927},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA52, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0519766301583773E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB52, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10433448732723377},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S52, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":408.50443507198224},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P52, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7691289408696189}]
["Csw",160,"pF",{"$f":"B53/1000000000000","v":1.5999999999999999E-10},"Effective SW node capacitance (CossHS + CossLS)",null,null,47,0.23499999999999999,0.16519112979664524,0.31769669612795504,0.15252423676214821,1.7689738060242715,1.7689738060242715,1,1.7689738060242715,2.2027038822685281E-6,9.9777744059650175E-2,408689.63966832712,2.4468445072685279E-6,0,6.6E-4,0.23974553001789489,6.8973502996273603E-3,9.7649905177794843E-2,0.10466275879113547,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,7.2008466142920308E-2,1.5555657588768302E-5,1.5555657588768302E-5,7.5729895730702587E-2,3.9399567527721802E-3,1.6408889032683335E-3,42.666666666666664,25.825027772329264,0.15391284845621267,8.5708429520971172E-2,0.24126216688045216,0.24538093149144721,0.224481884467331,1.5319203402017258E-2,4.495586036351599E-3,9.5912464127683381E-3,3.1746745683624462E-3,1.7261507017482382E-2,3.2673283197221431E-2,3.3844432885906044E-2,9.0545461327994209E-2,6.1364749396199325E-3,0.37473615095628282,0.47942573000082489,1.1749999999999998,0.71021622711308663,2.4895433722449444E-3,9.3154838565834962E-3,3.7981459211031972E-2,0.14582834545273415,5.7973266728410695E-3,1.918898207875952E-3,1.0433533947440347E-2,4.1690298781946059E-3,5.9023444453892869E-2,9.4024514408153863E-6,6.8087648865332545E-6,5.4729239086452719E-2,0.33170251535561945,0.71021622711308663,71.021622711308666,235,69.1417728033842,0.69141772803384205,408.68963966832712,null,5.1805546762699613E-2,null,0.37473615095628282,9.0545461327994209E-2,0.10466275879113547,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR53, IF(MODE_ILIM=4,#REF!,#REF!))","v":71.021622711308666},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ53, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.37473615095628282},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA53, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0545461327994209E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB53, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10466275879113547},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S53, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":408.68963966832712},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P53, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7689738060242715}]
["ThetaJA",41.1,"°C/W",null,"Thermal resistance",null,null,48,0.24,0.16517664292279413,0.32269671711490638,0.15753148022947733,1.768818671178924,1.768818671178924,1,1.768818671178924,2.2015954726898172E-6,9.9822963414004193E-2,408874.85814376117,2.445736097689817E-6,0,6.5999999999999989E-4,0.24464856256181305,7.1823502996273625E-3,9.7694160193845636E-2,0.10499717072717418,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,7.3489682378274884E-2,1.6202200248179179E-5,1.6202200248179179E-5,7.7296156177946745E-2,4.1046159870413625E-3,1.6416325554472011E-3,42.666666666666664,25.424281449979873,0.15621560377563104,8.5747272650590511E-2,0.24360450898166874,0.24789731590045389,0.2291246625059315,1.5959425734410931E-2,4.4976234395813731E-3,9.9096090644588304E-3,3.2454176219013347E-3,1.7652650125941541E-2,3.3711582195579223E-2,3.3844432885906037E-2,9.0571158279970074E-2,6.139255995028574E-3,0.37831931237103178,0.48334394989427198,1.2,0.71286679117204177,2.5501662444295864E-3,9.5398994784436763E-3,3.7345892022269796E-2,0.14471463719400254,5.8868593462917881E-3,1.9279587051150029E-3,1.0486656709135572E-2,4.2667158426407592E-3,5.8035768744695133E-2,9.6250087507052929E-6,6.6917968954082575E-6,5.3804309146481148E-2,0.32857518023915111,0.71286679117204177,71.286679117204173,240,69.449289175978407,0.69449289175978413,408.87485814376117,null,5.0938652588483867E-2,null,0.37831931237103178,9.0571158279970074E-2,0.10499717072717418,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR54, IF(MODE_ILIM=4,#REF!,#REF!))","v":71.286679117204173},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ54, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.37831931237103178},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA54, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0571158279970074E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB54, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10499717072717418},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S54, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":408.87485814376117},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P54, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.768818671178924}]
["Inductor",null,"Units","Std Units","Description",null,null,49,0.245,0.16516215604894302,0.32769673810185784,0.16253872369680641,1.7686635363335763,1.7686635363335763,1,1.7686635363335763,2.2004879839118721E-6,9.9868186157188649E-2,409060.09049984469,2.4446286089118723E-6,0,6.6E-4,0.24955544306538646,7.4733502996273612E-3,9.7738418526457371E-2,0.10533772494100473,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,7.4972756430346885E-2,1.686274262029236E-5,1.686274262029236E-5,7.8864331763534842E-2,4.2728534004376076E-3,1.6423762633568765E-3,42.666666666666664,25.035782439324443,0.15852038755379463,8.5786118691193042E-2,0.24594888250834454,0.25041963358930291,0.23377311748176158,1.6613560618971016E-2,4.4996609954982923E-3,1.0228256558803354E-2,3.3163053890510174E-3,1.8044222943352665E-2,3.4764603997473602E-2,3.3844432885906044E-2,9.0596857157727806E-2,6.1420372588551686E-3,0.38192313200335948,0.48728898428280232,1.2250000000000001,0.71541662140231266,2.6109792926285523E-3,9.7649294059579082E-3,3.6731218916893557E-2,0.14363748454024014,5.973440612355216E-3,1.9367673444678861E-3,1.0538071031806902E-2,4.364537977073769E-3,5.7080562582370063E-2,9.8480704922337471E-6,6.5786768011738233E-6,5.2909793842815953E-2,0.32556421229390331,0.71541662140231266,71.541662140231267,245,69.727575757335345,0.69727575757335347,409.0600904998447,null,5.010025730389478E-2,null,0.38192313200335948,9.0596857157727806E-2,0.10533772494100473,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR55, IF(MODE_ILIM=4,#REF!,#REF!))","v":71.541662140231267},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ55, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.38192313200335948},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA55, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0596857157727806E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB55, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10533772494100473},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S55, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":409.0600904998447},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P55, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7686635363335763}]
["Ltc",4000,"ppm",{"$f":"Ltc","v":4.0000000000000001E-3},"Inductor DCR Temp Co",null,null,50,0.25,0.16514766917509191,0.33269675908880925,0.1675459671641355,1.7685084014882289,1.7685084014882289,1,1.7685084014882289,2.1993814147877497E-6,9.991341228958453E-2,409245.33673813823,2.4435220397877495E-6,0,6.6E-4,0.25446594892747704,7.7703502996273616E-3,9.7782680176002959E-2,0.10568442327403886,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,7.6457615625480785E-2,1.753730096140129E-5,1.753730096140129E-5,8.0434352793710251E-2,4.444673670118672E-3,1.6431200270036251E-3,42.666666666666664,24.658977750519423,0.16082720001873724,8.5824967643106015E-2,0.24829528768884687,0.2529478952526622,0.23842704280552546,1.7281626241260312E-2,4.5016987041195207E-3,1.0547188927823145E-2,3.3873379880304663E-3,1.8436225619973132E-2,3.5832380633891124E-2,3.3844432885906044E-2,9.0622557961483913E-2,6.1448187311231462E-3,0.38554765257916035,0.4912608777499784,1.25,0.71787060513024581,2.6719761658157361E-3,9.9905506614246936E-3,3.6136425397674338E-2,0.14259511073934478,6.0572135184315439E-3,1.94533629699848E-3,1.0587859553702283E-2,4.4624848573339843E-3,5.6156249431363624E-2,1.0071610282809908E-5,6.4692177730212603E-6,5.2044216417808986E-2,0.32266396386795426,0.71787060513024581,71.787060513024585,250,69.979193442852676,0.69979193442852672,409.24533673813823,null,4.9288977165792225E-2,null,0.38554765257916035,9.0622557961483913E-2,0.10568442327403886,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR56, IF(MODE_ILIM=4,#REF!,#REF!))","v":71.787060513024585},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ56, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.38554765257916035},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA56, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0622557961483913E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB56, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10568442327403886},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S56, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":409.24533673813823},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P56, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7685084014882289}]
["ThetaCA",20,"°C/W",{"$f":"ThetaCa","v":40},"Inductor Core-to-Ambient thermal resistance",null,null,51,0.255,0.16513318230124083,0.33769678007576059,0.17255321063146459,1.7683532666428814,1.7683532666428814,1,1.7683532666428814,2.1982757641724114E-6,9.9958641811572768E-2,409430.59686020203,2.4424163891724116E-6,0,6.5999999999999989E-4,0.25937987424540354,8.0733502996273611E-3,9.7826945142855143E-2,0.10603726760347101,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,7.7944192699094819E-2,1.8225891526540881E-5,1.8225891526540881E-5,8.2006154790347147E-2,4.6200814739433852E-3,1.6438638463937112E-3,42.666666666666664,24.293347191509969,0.16313604139852667,8.5863819506656655E-2,0.25064372475157704,0.25548211161971324,0.24308624734832948,1.7963640789567539E-2,4.5037365654622226E-3,1.0866406203544223E-2,3.4585155370763635E-3,1.882865830608281E-2,3.6914944397481102E-2,3.3844432885906037E-2,9.0648260691454874E-2,6.1476004118559335E-3,0.38919291712050513,0.49525967521132053,1.2749999999999999,0.72023331822649117,2.7331509246284057E-3,1.021674184000112E-2,3.5560561593818207E-2,0.14158585221213776,6.1383119977847728E-3,1.9536769579657919E-3,1.0636099646700242E-2,4.560545784710158E-3,5.5261353186038815E-2,1.0295603397487553E-5,6.3632448818346823E-6,5.1206194187660044E-2,0.31986914717972464,0.72023331822649117,72.023331822649112,255,70.206518151218702,0.702065181512187,409.430596860202,null,4.8503516579513607E-2,null,0.38919291712050513,9.0648260691454874E-2,0.10603726760347101,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR57, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.023331822649112},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ57, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.38919291712050513},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA57, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0648260691454874E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB57, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10603726760347101},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S57, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":409.430596860202},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P57, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7683532666428814}]
[null,null,null,null,null,null,null,52,0.26,0.16511869542738972,0.34269680106271205,0.17756045409879367,1.7681981317975339,1.7681981317975339,1,1.7681981317975339,2.1971710309227162E-6,0.10000387472353454,409615.87086759746,2.4413116559227165E-6,0,6.5999999999999989E-4,0.26429702829120377,8.3823502996273648E-3,9.7871213427387041E-2,0.10639625984230534,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,7.9432425304965221E-2,1.8928530569486639E-5,1.8928530569486639E-5,8.3579678015089143E-2,4.7990814904718057E-3,1.6446077215334037E-3,42.666666666666664,23.938400972013689,0.16544691192126526,8.5902674282172395E-2,0.25299419392497108,0.25802229345428168,0.24775055403111274,1.8659622454907886E-2,4.5057745795435726E-3,1.1185908417997437E-2,3.5298381544431275E-3,1.9221521151984139E-2,3.8012327844055137E-2,3.3844432885906037E-2,9.0673965347857308E-2,6.1503823010769761E-3,0.39285896894727107,0.4992854219159637,1.3,0.72250904951794637,2.7944980090798747E-3,1.0443482986741293E-2,3.5002737195505243E-2,0.14060814968176141,6.2168615839093251E-3,1.9618000076299124E-3,1.0682863829083971E-2,4.6587107290078766E-3,5.439449029891498E-2,1.052002663887014E-5,6.2605941673287669E-6,5.039443116884891E-2,0.31717480611128895,0.72250904951794637,72.250904951794638,260,70.411746141009829,0.70411746141009823,409.61587086759744,null,4.7742661189740083E-2,null,0.39285896894727107,9.0673965347857308E-2,0.10639625984230534,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR58, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.250904951794638},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ58, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.39285896894727107},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA58, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0673965347857308E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB58, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10639625984230534},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S58, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":409.61587086759744},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P58, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7681981317975339}]
[null,null,null,null,null,null,null,53,0.26500000000000001,0.16510420855353861,0.34769682204966346,0.18256769756612276,1.7680429969521863,1.7680429969521863,1,1.7680429969521863,2.1960672138974221E-6,0.10004911102585097,409801.15876188554,2.4402078388974219E-6,0,6.6E-4,0.26921723415034438,8.6973502996273606E-3,9.7915485029971605E-2,0.10676140193938234,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,8.0922255576476282E-2,1.964523434275364E-5,1.964523434275364E-5,8.5154867044214225E-2,4.9816783989653302E-3,1.6453516524289704E-3,42.666666666666664,23.593677514526433,0.16775981181508931,8.5941531969980597E-2,0.25534669543749888,0.26056845155496711,0.25241979856444313,1.9369589431023466E-2,4.5078127463807419E-3,1.1505695603218416E-2,3.6013059584028952E-3,1.9614814308002052E-2,3.9124563794100183E-2,3.3844432885906044E-2,9.0699671930907777E-2,6.1531643988097118E-3,0.39654585167878476,0.5033381634483276,1.3250000000000002,0.72470182293902941,2.8560122092620753E-3,1.0670755485025739E-2,3.4462116857515455E-2,0.13966054012453777,6.2929800587426116E-3,1.9697154664269933E-3,1.0728220140090295E-2,4.7569702768900084E-3,5.3554362637871437E-2,1.074485821906263E-5,6.1611117915742835E-6,4.9607711387396808E-2,0.31457629061376979,0.72470182293902941,72.470182293902937,265,70.596901007914624,0.70596901007914625,409.80115876188552,null,4.7005271611183244E-2,null,0.39654585167878476,9.0699671930907777E-2,0.10676140193938234,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR59, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.470182293902937},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ59, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.39654585167878476},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA59, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0699671930907777E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB59, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10676140193938234},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S59, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":409.80115876188552},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P59, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7680429969521863}]
[null,null,null,null,null,null,null,54,0.27,0.16508972167968752,0.3526968430366148,0.18757494103345185,1.767887862106839,1.767887862106839,1,1.767887862106839,2.1949643119571785E-6,0.10009435071890314,409986.46054462728,2.4391049369571788E-6,0,6.6E-4,0.27414032750319928,9.0183502996273625E-3,9.7959759950981815E-2,0.1071326958794066,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,8.241362973358983E-2,2.0376019097595724E-5,2.0376019097595724E-5,8.6731670388081925E-2,5.1678768793868316E-3,1.6460956390866785E-3,42.666666666666664,23.258741451778018,0.17007474130816921,8.5980392570408626E-2,0.2577012295176645,0.26312059675527438,0.25709382832046596,2.0093559914383861E-2,4.5098510659909007E-3,1.1825767791247586E-2,3.672919067245534E-3,2.0008537924484017E-2,4.0251685334305495E-2,3.3844432885906044E-2,9.0725380440822873E-2,6.1559467050775795E-3,0.40025360923548037,0.50741794572980237,1.35,0.72681541766280744,2.9176886387196764E-3,1.0898541955169759E-2,3.3937916022032645E-2,0.13874164945488912,6.3667780417622144E-3,1.9774327451124087E-3,1.0772232480300721E-2,4.8553155849282706E-3,5.2739750994756446E-2,1.0970077652388426E-5,6.0646532697199521E-6,4.8844892798306498E-2,0.31206923344689991,0.72681541766280744,72.681541766280745,270,70.763841860106652,0.70763841860106647,409.98646054462728,null,4.6290277731017543E-2,null,0.40025360923548037,9.0725380440822873E-2,0.1071326958794066,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR60, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.681541766280745},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ60, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.40025360923548037},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA60, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0725380440822873E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB60, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1071326958794066},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S60, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":409.98646054462728},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P60, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.767887862106839}]
[null,null,null,null,null,null,null,55,0.27500000000000002,0.16507523480583641,0.35769686402356626,0.19258218450078093,1.7677327272614913,1.7677327272614913,1,1.7677327272614913,2.1938623239645229E-6,0.10013959380307241,410171.77621738461,2.4380029489645227E-6,0,6.6E-4,0.27906615553227043,9.3453502996273616E-3,9.8004038190790871E-2,0.10751014368297515,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,8.3906497730121085E-2,2.1120901084004444E-5,2.1120901084004444E-5,8.8310040149846739E-2,5.3576816124008024E-3,1.6468396815127993E-3,42.666666666666664,22.933181792369243,0.1723917006287099,8.6019256083784065E-2,0.26005779639400678,0.26567873992374624,0.26177250132124724,2.0831552104186645E-2,4.5118895383912316E-3,1.2146125014130199E-2,3.7446775992786493E-3,2.040269215180008E-2,4.139372581910352E-2,3.3844432885906044E-2,9.0751090877819296E-2,6.1587292199040307E-3,0.40398228584057305,0.51152481502045,1.375,0.72885338642370046,2.9795227102159972E-3,1.1126826162144015E-2,3.3429397116694508E-2,0.13785018586738693,6.4383595261632088E-3,1.9849606903994299E-3,1.0814960921454359E-2,4.9537383368721067E-3,5.1949509177131342E-2,1.1195665657743014E-5,5.971082769820154E-6,4.81049017512317E-2,0.3096495290081212,0.72885338642370046,72.885338642370044,275,70.914272258910415,0.70914272258910416,410.1717762173846,null,4.55966735231371E-2,null,0.40398228584057305,9.0751090877819296E-2,0.10751014368297515,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR61, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.885338642370044},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ61, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.40398228584057305},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA61, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0751090877819296E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB61, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10751014368297515},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S61, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":410.1717762173846},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P61, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7677327272614913}]
[null,null,null,null,null,null,null,56,0.28000000000000003,0.1650607479319853,0.36269688501051761,0.19758942796811002,1.7675775924161439,1.7675775924161439,1,1.7675775924161439,2.1927612487838757E-6,0.10018484027874008,410357.10578171938,2.4369018737838755E-6,0,6.6E-4,0.28399457594038896,9.6783502996273616E-3,9.8048319749771976E-2,0.10789374740660584,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,8.5400812936623036E-2,2.1879896550708241E-5,2.1879896550708241E-5,8.9889931718827837E-2,5.5510972793734702E-3,1.6475837797136034E-3,42.666666666666664,22.616610238339099,0.17471069000495032,8.6058122510434445E-2,0.26241639629509839,0.26824289196409418,0.26645568532984659,2.1583584202357859E-2,4.5139281635989134E-3,1.2466767303916299E-2,3.8165816728275843E-3,2.0797277140342796E-2,4.2550718872224634E-2,3.3844432885906044E-2,9.0776803242113707E-2,6.1615119433125164E-3,0.40773192602174502,0.51565881792071933,1.4000000000000001,0.73081907221849562,3.0415101136432757E-3,1.1355592931466419E-2,3.2935866089141647E-2,0.13698493376807488,6.5078223675799881E-3,1.992307626558549E-3,1.0856461988840176E-2,5.0522307046994763E-3,5.1182558622936247E-2,1.1421604069589469E-5,5.8802724746327727E-6,4.7386727945973178E-2,0.30731331403545803,0.73081907221849562,73.081907221849562,280,71.049749591014816,0.71049749591014821,410.35710578171938,null,4.4923512321386659E-2,null,0.40773192602174502,9.0776803242113707E-2,0.10789374740660584,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR62, IF(MODE_ILIM=4,#REF!,#REF!))","v":73.081907221849562},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ62, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.40773192602174502},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA62, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0776803242113707E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB62, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10789374740660584},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S62, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":410.35710578171938},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P62, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7675775924161439}]
[null,1500,null,null,null,"Eff (%)","Iout (mA)",57,0.28499999999999998,0.16504626105813422,0.36769690599746896,0.20259667143543908,1.7674224575707964,1.7674224575707964,1,1.7674224575707964,2.1916610852815409E-6,0.10023009014628743,410542.44923919335,2.4358017102815411E-6,0,6.6E-4,0.28892545606706471,1.0017350299627361E-2,9.8092604628298233E-2,0.10828350914276655,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,8.6896531854789627E-2,2.2653021745171403E-5,2.2653021745171403E-5,9.1471303494529088E-2,5.7481285623729277E-3,1.6483279336953613E-3,42.666666666666664,22.308659640181297,0.17703170966516352,8.6096991850687296E-2,0.26477702944954618,0.27081306381533221,0.27114325703224557,2.2349674413552529E-2,4.5159669416311278E-3,1.2787694692660723E-2,3.8886314062354138E-3,2.1192293040527263E-2,4.372269838826616E-2,3.3844432885906044E-2,9.0802517533922794E-2,6.1642948753264891E-3,0.41150257461284762,0.51982000137317719,1.4249999999999998,0.73271562355068931,3.1036467958598631E-3,1.1584828072433889E-2,3.2456669243824364E-2,0.1361447482351042,6.5752587301815737E-3,1.9994813933884737E-3,1.0896788919058854E-2,5.1507853130646642E-3,5.0437883484866511E-2,1.1647875756716203E-5,5.7921019990812416E-6,4.6689419827958344E-2,0.30505694999349653,0.73271562355068931,73.271562355068937,285,71.171694607053283,0.71171694607053282,410.54244923919333,null,4.426990250506313E-2,null,0.41150257461284762,9.0802517533922794E-2,0.10828350914276655,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR63, IF(MODE_ILIM=4,#REF!,#REF!))","v":73.271562355068937},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ63, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.41150257461284762},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA63, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0802517533922794E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB63, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10828350914276655},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S63, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":410.54244923919333},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P63, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7674224575707964}]
[null,null,null,null,null,{"$f":"BR56","v":71.787060513024585},{"$f":"I56*1000","v":250},58,0.28999999999999998,0.16503177418428311,0.37269692698442036,0.20760391490276814,1.767267322725449,1.767267322725449,1,1.767267322725449,2.1905618323256967E-6,0.10027534340609601,410727.80659136921,2.4347024573256965E-6,0,6.6E-4,0.29385867209180905,1.0362350299627362E-2,9.8136892826743066E-2,0.10867943101990521,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,8.8393613859813203E-2,2.3440292913593282E-5,2.3440292913593282E-5,9.3054116637819748E-2,5.9487801441692892E-3,1.6490721434643475E-3,42.666666666666664,22.00898257638536,0.17935475983765711,8.6135864104870327E-2,0.26713969608599181,0.27338926645191025,0.27583510129978622,2.3129840945155251E-2,4.5180058725050615E-3,1.3108907212423145E-2,3.9608269178629694E-3,2.1587740002791175E-2,4.4909698534275871E-2,3.3844432885906044E-2,9.0828233753463383E-2,6.1670780159694093E-3,0.41529427675561892,0.52400841266425557,1.45,0.73454600836426098,3.1659289422599777E-3,1.1814518307957867E-2,3.1991190350751368E-2,0.1353285499555911,6.6407554944157886E-3,2.0064893809227332E-3,1.0935991895624648E-2,5.249395206802402E-3,4.9714526137348551E-2,1.1874464547978634E-5,5.7064578577977283E-6,4.6012080379574188E-2,0.30287700697365438,0.73454600836426098,73.454600836426096,290,71.281400919850697,0.71281400919850701,410.72780659136919,null,4.3635003555337191E-2,null,0.41529427675561892,9.0828233753463383E-2,0.10867943101990521,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR64, IF(MODE_ILIM=4,#REF!,#REF!))","v":73.454600836426096},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ64, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.41529427675561892},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA64, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0828233753463383E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB64, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10867943101990521},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S64, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":410.72780659136919},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P64, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.767267322725449}]
[null,null,null,null,null,{"$f":"BR81","v":75.775186608342295},{"$f":"I81*1000","v":375},59,0.29499999999999998,0.16501728731043203,0.37769694797137177,0.21261115837009725,1.7671121878801019,1.7671121878801019,1,1.7671121878801019,2.1894634887863952E-6,0.10032060005854714,410913.17783980904,2.4336041137863954E-6,0,6.6E-4,0.29879410831467434,1.0713350299627361E-2,9.8181184345479705E-2,0.10908151520247959,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,8.9892020967579367E-2,2.4241726300907187E-5,2.4241726300907187E-5,9.4638334846228883E-2,6.1530567082347882E-3,1.6498164090268334E-3,42.666666666666664,21.717250045948177,0.18167984075077251,8.6174739273311138E-2,0.26950439643311047,0.27597151088384769,0.28053111052308899,2.3924102007280543E-2,4.5200449562378996E-3,1.3430404895268012E-2,4.0331683260888167E-3,2.1983618177594727E-2,4.6111753751349391E-2,3.3844432885906044E-2,9.085395190095219E-2,6.169861365264733E-3,0.41910707790141399,0.52822409942601234,1.4749999999999999,0.73631302679647004,3.2283529599061115E-3,1.2044651210350428E-2,3.1538847999289639E-2,0.13453532059160636,6.7043946301945214E-3,2.0133385611946506E-3,1.0974118264598423E-2,5.3480538211860959E-3,4.9011583064327027E-2,1.2101355164333944E-5,5.6232329777953592E-6,4.5353863268210858E-2,0.30077024895900623,0.73631302679647004,73.631302679647007,295,71.3800443047935,0.713800443047935,410.91317783980907,null,4.3018022445917535E-2,null,0.41910707790141399,9.085395190095219E-2,0.10908151520247959,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR65, IF(MODE_ILIM=4,#REF!,#REF!))","v":73.631302679647007},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ65, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.41910707790141399},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA65, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.085395190095219E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB65, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10908151520247959},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S65, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":410.91317783980907},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P65, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7671121878801019}]
[null,null,null,null,null,{"$f":"BR106","v":77.514849349503493},{"$f":"I106*1000","v":500},60,0.3,0.16500280043658089,0.38269696895832317,0.21761840183742631,1.7669570530347538,1.7669570530347538,1,1.7669570530347538,2.1883660535355557E-6,0.10036586010402249,411098.56298607611,2.4325066785355559E-6,0,6.6E-4,0.30373165650547745,1.1070350299627361E-2,9.8225479184881656E-2,0.1094897638909885,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,9.1391717623972232E-2,2.5057338150779632E-5,2.5057338150779632E-5,9.6223924150689755E-2,6.3609629387439371E-3,1.6505607303890957E-3,42.666666666666664,21.433150263511017,0.18400695263288588,8.6213617356337563E-2,0.27187113071961255,0.27855980815686893,0.28523118400955383,2.4732475812773554E-2,4.5220841928468383E-3,1.3752187773264611E-2,4.1056557493092845E-3,2.2379927715420734E-2,4.7328898756242896E-2,3.3844432885906044E-2,9.0879671976606069E-2,6.1726449232359336E-3,0.42294102381295384,0.53246710963791088,1.5,0.73801932286482552,3.2909154620701236E-3,1.2275215142481142E-2,3.1099093173122302E-2,0.13376409853345528,6.7662535388897877E-3,2.020035517347544E-3,1.1011212732199035E-2,5.446754954671602E-3,4.8328201090732915E-2,1.2328533156555562E-5,5.5423262518691277E-6,4.471396931623485E-2,0.29873362032061307,0.73801932286482552,73.801932286482554,300,71.468691685531624,0.71468691685531627,411.0985629860761,null,4.2418210335367613E-2,null,0.42294102381295384,9.0879671976606069E-2,0.1094897638909885,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR66, IF(MODE_ILIM=4,#REF!,#REF!))","v":73.801932286482554},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ66, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.42294102381295384},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA66, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0879671976606069E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB66, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1094897638909885},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S66, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":411.0985629860761},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P66, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7669570530347538}]
[null,null,null,null,null,null,null,61,0.30499999999999999,0.16498831356272978,0.38769698994527457,0.22262564530475543,1.7668019181894064,1.7668019181894064,1,1.7668019181894064,2.1872695254469646E-6,0.1004111235429036,411283.96203173313,2.4314101504469648E-6,0,6.6E-4,0.30867121531422614,1.1433350299627363E-2,9.8269777345322315E-2,0.10990417932200271,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,9.2892670513895076E-2,2.5887144705609215E-5,2.5887144705609215E-5,9.7810852731397557E-2,6.5725035205736384E-3,1.6513051075574086E-3,42.666666666666664,21.156387547845704,0.18633609571240717,8.6252498354277327E-2,0.27423989917424191,0.28115416935253745,0.28993522743751715,2.5554980577210416E-2,4.5241235823490645E-3,1.4074255878487008E-2,4.1782893059384438E-3,2.2776668766774515E-2,4.8561168542999737E-2,3.3844432885906044E-2,9.090539398064186E-2,6.1754286899064733E-3,0.42679616056608549,0.53673749162861162,1.5249999999999999,0.73966739519072777,3.3536132540490458E-3,1.2506199203787812E-2,3.0671407025096339E-2,0.13301397500300283,6.8264053671398513E-3,2.0265864703454179E-3,1.1047317546125975E-2,5.5454927438875401E-3,4.766357392458187E-2,1.2555984848080923E-5,5.4636421288088479E-6,4.4091643261933267E-2,0.29676423342692687,0.73966739519072777,73.966739519072775,305,71.54830972155635,0.71548309721556347,411.28396203173315,null,4.1834859532066129E-2,null,0.42679616056608549,9.090539398064186E-2,0.10990417932200271,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR67, IF(MODE_ILIM=4,#REF!,#REF!))","v":73.966739519072775},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ67, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.42679616056608549},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA67, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.090539398064186E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB67, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10990417932200271},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S67, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":411.28396203173315},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P67, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7668019181894064}]
[null,null,null,null,null,null,null,62,0.31,0.16497382668887869,0.39269701093222598,0.22763288877208449,1.7666467833440589,1.7666467833440589,1,1.7666467833440589,2.1861739033962693E-6,0.10045639037557207,411469.3749783432,2.4303145283962696E-6,0,6.6E-4,0.31361268973617978,1.1802350299627364E-2,9.8314078827175161E-2,0.11032476376819707,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,9.4394848387903546E-2,2.6731162206525893E-5,2.6731162206525893E-5,9.9399090750729724E-2,6.7876831393033294E-3,1.652049540538048E-3,42.666666666666664,20.886681295359757,0.18866727021778068,8.629138226745825E-2,0.27661070202577698,0.28375460558839233,0.29464315236098693,2.6391634518898806E-2,4.5261631247617753E-3,1.4396609243014094E-2,4.2510691144081285E-3,2.3173841482183998E-2,4.9808598384592569E-2,3.3844432885906044E-2,9.0931117913276419E-2,6.1782126652998228E-3,0.43067253455156113,0.5410352940777825,1.55,0.74125960685116166,3.4164433201334626E-3,1.2737593180681057E-2,3.0255298832998503E-2,0.13228409047383952,6.8849192951396304E-3,2.0329973035117968E-3,1.1082472662138612E-2,5.6442616406590122E-3,4.7016938980236109E-2,1.2783697282505814E-5,5.3870902369320516E-6,4.3486170783827029E-2,0.29485935726068424,0.74125960685116166,74.125960685116169,310,71.619772941093288,0.71619772941093285,411.46937497834318,null,4.1267300705948001E-2,null,0.43067253455156113,9.0931117913276419E-2,0.11032476376819707,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR68, IF(MODE_ILIM=4,#REF!,#REF!))","v":74.125960685116169},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ68, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.43067253455156113},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA68, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0931117913276419E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB68, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11032476376819707},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S68, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":411.46937497834318},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P68, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7666467833440589}]
[null,null,null,null,null,null,null,63,0.315,0.16495933981502758,0.39769703191917738,0.2326401322394136,1.7664916484987117,1.7664916484987117,1,1.7664916484987117,2.1850791862609723E-6,0.10050166060240971,411654.80182747019,2.4292198112609721E-6,0,6.6E-4,0.31855599062576323,1.2177350299627361E-2,9.8358383630813839E-2,0.11075151953838278,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,9.5898221904596834E-2,2.7589406893389892E-5,2.7589406893389892E-5,0.10098861020142326,7.006506481215112E-3,1.652794029337293E-3,42.666666666666664,20.623765031129057,0.1910004763774853,8.6330269096208292E-2,0.2789835395030309,0.286361128018085,0.29935487575960379,2.7242455858878536E-2,4.5282028201021722E-3,1.4719247898929583E-2,4.3239952931679333E-3,2.3571446012199689E-2,5.1071223834580078E-2,3.3844432885906044E-2,9.0956843774726709E-2,6.1809968494394652E-3,0.43457019247683121,0.54536056601792515,1.575,0.74279819444005124,3.4794028116214891E-3,1.296938750093125E-2,2.9850304119325457E-2,0.13157363137863243,6.9418608018034364E-3,2.0392735850999497E-3,1.1116715897271794E-2,5.7430563908744264E-3,4.6387574456514549E-2,1.3011658175290105E-5,5.3125850378182952E-6,4.2896875763703379E-2,0.29301640694899123,0.74279819444005124,74.279819444005128,315,71.68387138413388,0.71683871384133879,411.65480182747018,null,4.0714900323928431E-2,null,0.43457019247683121,9.0956843774726709E-2,0.11075151953838278,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR69, IF(MODE_ILIM=4,#REF!,#REF!))","v":74.279819444005128},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ69, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.43457019247683121},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA69, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0956843774726709E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB69, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11075151953838278},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S69, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":411.65480182747018},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P69, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7664916484987117}]
[null,null,null,null,null,null,null,64,{"$f":"IF(PLOT_TYPE=1, H70/100*Iout, min_I*EXP(H70*rr/100))","v":0.32},{"$f":"IF(I70<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I70-Vout)/L*OnTime)","v":0.1649448529411765},{"$f":"IF(I70<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I70+((Vin-(Rdcr+RdsonTop)*J70-Vout)/L*OnTime)/2)","v":0.40269705290612878},{"$f":"IF(I70<Icrit, 0, I70-((Vin-(Rdcr+RdsonTop)*K70-Vout)/L*OnTime)/2)","v":0.23764737570674266},1.7663365136533642,{"$f":"IF(I70<Icrit, 1000*SQRT((J70*CoutEsr)^2+(((J70/2)-I70)*(OnTime+OffTime)/Cout)^2), 1000*J70*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":1.7663365136533642},1,{"$f":"IF(I70<Icrit, 1000*((N70/1000)*O70), 1000*J70*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":1.7663365136533642},{"$f":"IF(I70<Icrit, L*J70/(Vout+J70/2*(RdsonBot+Rdcr)), L*J70/(Vout+I70*(RdsonBot+Rdcr)))","v":2.1839853729204314E-6},0.10054693422379821,{"$f":"IF(I70<Icrit,I70/((OnTime+Q70)*J70/2),1/(OnTime+Q70))","v":411840.24258067744},2.4281259979204316E-6,0,{"$f":"S70*(T70*Iq_active+U70*Iq_sleep)","v":6.6E-4},0.32350103425423754,{"$f":"W70^2*Rdcr","v":1.2558350299627364E-2},{"$f":"Core_Loss/1000*S70/$S$106","v":9.8402691756611885E-2},{"$f":"(Y70+X70*(1+Ltc*(Ta-25)))/(1-X70*Ltc*ThetaCa)","v":0.11118444897754021},4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,9.7402763487132435E-2,2.8461895004790777E-5,2.8461895004790777E-5,0.10257938476841766,7.2289782332938821E-3,1.6535385739614198E-3,{"$f":"20*VIN_nom/24","v":42.666666666666664},{"$f":"IF(I70<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I70+Iripple/2)*1000000000)","v":20.36738553071169},{"$f":"IF(I70<Icrit, Vin*(I70+Iripple/2)*AK70/1000000000/2*S70, Vin*(I70-Iripple/2)*AJ70/1000000000/2*S70 + Vin*(I70+Iripple/2)*AK70/1000000000/2*S70)","v":0.19333571442003369},{"$f":"IF(I70<Icrit, Csw*(Vin)^2*S70/2, Csw*Vin^2*S70/2)","v":8.6369158840855303E-2},0.28135841183485044,{"$f":"(AI70+AL70+AM70+AH70*(1+RdsonTopTc*(Ta-25)))/(1-AH70*RdsonTopTc*ThetaJA)","v":0.28897374783151514},{"$f":"IF(I70<Icrit,Iripple*SQRT((OffTime)*S70/3), SQRT(OffTime*S70*(I70^2+Iripple^2/12)))","v":0.30407031962910885},2.810746282092192E-2,{"$f":"QgBot*S70*Vdd","v":4.5302426683874525E-3},{"$f":"IF(I70<Icrit, Vin*Idss*R70, QrrBot*(I70-Iripple/2)/1*S70*Vin+Vin*Idss*R70)","v":1.5042171878321967E-2},{"$f":"IF(I70<Icrit, dead1*S70*(I70+Iripple/2)*((I70+Iripple/2)*BDserR+VSD), dead1*S70*(I70+Iripple/2)*((I70+Iripple/2)*BDserR+VSD)+dead2*S70*(I70-Iripple/2)*((I70-Iripple/2)*BDserR+VSD))","v":4.3970679606852121E-3},2.3969482507394634E-2,{"$f":"(AR70+AS70+AT70+AQ70*(1+RdsonBotTc*(Ta-25)))/(1-AQ70*RdsonBotTc*ThetaJA)","v":5.2349080728778856E-2},{"$f":"Vin*V70+Vout*Ifb/0.8","v":3.3844432885906044E-2},{"$f":"(Vin-Vdd)*(S70*QgBot+S70*QgTop)+AW70","v":9.0982571565209613E-2},{"$f":"AI70+AR70","v":6.183781242348872E-3},0.43848918136785248,{"$f":"SUM(Z70,AC70,AF70,AZ70)","v":0.54971335683621525},{"$f":"Vout*I70","v":1.6},0.74428527641227404,3.542489035781202E-3,1.3201573191670146E-2,{"$f":"Vin*S70*(QgBot+QgTop)/($BB70+$BA70)","v":2.9455982919901858E-2},0.13088182707713755,6.9972919089361253E-3,2.045420589076342E-3,1.1150083070922114E-2,{"$f":"X70/($BB70+$BA70)","v":5.8418720150251978E-3},{"$f":"Y70/($BB70+$BA70)","v":4.5774796646113544E-2},1.323985586928614E-5,5.2400455074555316E-6,4.2323117766319709E-2,0.29123293412226053,{"$f":"BC70","v":0.74428527641227404},74.428527641227404,{"$f":"I70*1000","v":320},71.741317737155555,0.71741317737155552,{"$f":"S70/1000","v":411.84024258067745},null,{"$f":"AM70/($BB70+$BA70)","v":4.0177058288350991E-2},null,0.43848918136785248,9.0982571565209613E-2,0.11118444897754021,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR70, IF(MODE_ILIM=4,#REF!,#REF!))","v":74.428527641227404},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ70, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.43848918136785248},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA70, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0982571565209613E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB70, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11118444897754021},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S70, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":411.84024258067745},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P70, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7663365136533642}]
[null,null,null,null,null,null,null,65,0.32500000000000001,0.16493036606732536,0.40769707389308019,0.24265461917407177,{"$f":"IF(I71<Icrit, 1000*((((J71/2)-I71)*0.000002/Cout+Vout/306)), 1000*J71*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":1.7661813788080163},1.7661813788080163,{"$f":"ROUNDUP(M71/N71,0)","v":1},1.7661813788080163,2.1828924622558534E-6,0.10059221124011944,412025.69723952923,{"$f":"IF(1/S71-OnTime-Q71>Tsleep, OnTime+Q71+Tsleep, 1/S71)","v":2.4270330872558532E-6},{"$f":"IF(1/S71-OnTime-Q71>Tsleep, 1/S71-OnTime-Q71-Tsleep, 0)","v":0},6.6E-4,{"$f":"IF(I71<Icrit,Iripple*SQRT((OnTime+OffTime)*S71/3), SQRT(I71^2+Iripple^2/12))","v":0.32844774190662562},1.2945350299627362E-2,9.8447003204943082E-2,0.1116235544668525,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q71)*S71)","v":4.7464925614198031E-2},{"$f":"RCoutEsr*AA71^2","v":1.1264595817806762E-5},1.1264595817806762E-5,{"$f":"SQRT($R71)*SQRT($I71^2*(1-R71)+(Iripple^2)/12)","v":9.8908447192419147E-2},{"$f":"RCinEsr*AD71^2","v":2.9348642778046702E-5},2.9348642778046702E-5,{"$f":"IF(I71<Icrit,Iripple*SQRT((OnTime)*S71/3), SQRT(OnTime*S71*(I71^2+Iripple^2/12)))","v":0.10417138970295776},{"$f":"RdsonTop*AG71^2","v":7.4551030832274564E-3},{"$f":"QgTop*S71*Vdd","v":1.6542831744167097E-3},42.666666666666664,20.117302006659326,0.19567298457397328,8.6408051501727326E-2,{"$f":"AI71+AL71+AM71","v":0.2837353192501173},0.29159247625496953,0.3087894106081549,{"$f":"RdsonBot*AP71^2","v":2.8986673631534433E-2},4.5322826696348219E-3,1.5365381213284591E-2,4.470287235445093E-3,{"$f":"AR71+AS71+AT71","v":2.4367951118364508E-2},5.3642205186950745E-2,3.3844432885906044E-2,9.1008301284942195E-2,6.1865658440515316E-3,0.44242954857091399,0.55409371627636239,1.625,0.74572286077571803,{"$f":"(AO71-AN71)/($BB71+$BA71)","v":3.6056994456753104E-3},{"$f":"(AV71-AU71)/($BB71+$BA71)","v":1.3434141840677743E-2},2.9071918187778073E-2,{"$f":"AN71/($BB71+$BA71)","v":0.13020794706111333},{"$f":"AS71/(BA71+BB71)","v":7.0512714063261902E-3},{"$f":"AT71/($BB71+$BA71)","v":2.0514433142801787E-3},{"$f":"AU71/($BB71+$BA71)","v":1.1182608134910546E-2},5.9407037902657941E-3,4.5177957455253194E-2,{"$f":"(AF71)/($BB71+$BA71)","v":1.3468279293741294E-5},{"$f":"(AC71)/($BB71+$BA71)","v":5.1693948422997215E-6},{"$f":"AX71/($BB71+$BA71)","v":4.1764289716028032E-2},{"$f":"SUM(BD71:BO71)","v":0.2895066180264444},0.74572286077571803,74.572286077571803,325,71.792753953912452,{"$f":"BT71/100","v":0.71792753953912447},412.02569723952922,null,3.9653205759953035E-2,null,{"$f":"AZ71","v":0.44242954857091399},{"$f":"AX71","v":9.1008301284942195E-2},{"$f":"Z71","v":0.1116235544668525},null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR71, IF(MODE_ILIM=4,#REF!,#REF!))","v":74.572286077571803},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ71, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.44242954857091399},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA71, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1008301284942195E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB71, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1116235544668525},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S71, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":412.02569723952922},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P71, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7661813788080163}]
[null,null,null,null,null,null,null,66,0.33,0.16491587919347431,0.41269709488003159,0.24766186264140086,1.7660262439626693,1.7660262439626693,1,1.7660262439626693,2.1818004531502927E-6,{"$f":"OnTime*S72","v":0.10063749165175517},412211.16580558917,2.4259410781502925E-6,0,6.6E-4,0.33339603951391106,1.3338350299627362E-2,9.849131797618102E-2,0.11206883842373928,4.7464925614198031E-2,1.1264595817806762E-5,{"$f":"AB72","v":1.1264595817806762E-5},0.1004152485917074,3.0249666449203188E-5,{"$f":"AE72","v":3.0249666449203188E-5},0.10576460170771279,7.6848857194067024E-3,1.6550278307094408E-3,42.666666666666664,19.873285354232799,0.19801228706788518,8.6446947079152306E-2,0.28611426197774692,0.29421732455125932,0.31351207963777017,2.9880106519955062E-2,4.5343228238614811E-3,1.5688875935915565E-2,4.5436532359504657E-3,2.476685199572751E-2,5.4950633614505265E-2,3.3844432885906044E-2,9.1034032934141362E-2,6.1893506545709215E-3,{"$f":"AO72+AV72+AX72+AY72","v":0.44639134175447687},0.55850169444048314,1.6500000000000001,0.74711285219005552,3.6690316307705089E-3,1.3667085560658678E-2,2.8697714320234241E-2,0.12955129837481652,7.1038550594774569E-3,2.0573465021051685E-3,1.1214323293513302E-2,6.0395472338573815E-3,4.4596442114631686E-2,1.3696917926461831E-5,5.1005601880059275E-6,4.1219815752599878E-2,0.2878352573207793,0.74711285219005552,{"$f":"100*BQ72","v":74.711285219005546},330,71.838757366287027,0.71838757366287032,412.21116580558919,null,3.9142803148744403E-2,null,0.44639134175447687,9.1034032934141362E-2,0.11206883842373928,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR72, IF(MODE_ILIM=4,#REF!,#REF!))","v":74.711285219005546},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ72, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.44639134175447687},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA72, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1034032934141362E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB72, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11206883842373928},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S72, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":412.21116580558919},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P72, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7660262439626693}]
[null,null,null,null,null,null,null,67,0.33500000000000002,0.16490139231962317,0.41769711586698299,0.25266910610872995,1.7658711091173216,1.7658711091173216,1,1.7658711091173216,2.1807093444886416E-6,0.10068277545908745,412396.6482804222,2.4248499694886418E-6,0,6.5999999999999989E-4,0.3383458573169788,1.3737350299627365E-2,9.8535636070699609E-2,0.11252030330189151,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.10192314466144325,3.1164982253032466E-5,3.1164982253032466E-5,0.10735899883180922,7.9183308309256992E-3,1.6557725428458952E-3,42.666666666666664,19.635117451355203,0.20035362213038541,8.6485845573458411E-2,0.28849524024668971,0.29684830401985979,0.31823826165021091,3.0787779718157018E-2,4.5363631310846447E-3,1.6012656078317863E-2,4.6171660807220009E-3,2.5166185290124508E-2,5.6274402704218046E-2,3.3844432885906037E-2,9.1059766513024221E-2,6.1921356739305395E-3,0.45037460891103265,0.56293734179099497,1.675,{"$f":"BB73/(BB73+BA73)","v":0.74845705852493494},3.7324833082615343E-3,1.3900396956242749E-2,2.8332995797954057E-2,0.12891122323192941,7.1550958015219141E-3,2.0631346528348004E-3,1.1245259114352283E-2,6.1383980878720774E-3,4.4029667064692121E-2,1.3925761758857598E-5,5.0334723888166757E-6,4.0689149250331624E-2,0.28621676250014028,0.74845705852493494,74.845705852493495,335,71.879846296152991,0.71879846296152994,412.3966482804222,null,3.8645338257882057E-2,null,0.45037460891103265,9.1059766513024221E-2,0.11252030330189151,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR73, IF(MODE_ILIM=4,#REF!,#REF!))","v":74.845705852493495},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ73, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.45037460891103265},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA73, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1059766513024221E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB73, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11252030330189151},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S73, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":412.3966482804222},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P73, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7658711091173216}]
[null,null,null,null,null,null,null,68,0.34,0.16488690544577209,0.4226971368539344,0.25767634957605901,1.7657159742719741,1.7657159742719741,1,1.7657159742719741,2.1796191351576353E-6,0.10072806266249823,412582.14466559276,2.4237597601576355E-6,0,6.6E-4,0.34329712955916392,1.4142350299627364E-2,9.8579957488872647E-2,0.11297795159130618,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.10343211368337585,3.2094606423032356E-5,3.2094606423032356E-5,0.10895456037479821,8.1554431075818324E-3,1.6565173108323548E-3,42.666666666666664,19.402590508306403,0.20269698999012387,8.6524746984973727E-2,0.29087825428592995,0.2994854259970488,0.32296789528429709,3.1709711460848083E-2,4.5384035913215211E-3,1.6336721672599242E-2,4.6908258882981443E-3,2.5565951152218908E-2,5.7613549437964484E-2,3.3844432885906044E-2,9.108550202180786E-2,6.1949209021538755E-3,0.45437939835897506,0.56740070915252205,1.7000000000000002,0.74975719692502107,3.7960523150475352E-3,1.413406909347042E-2,2.7977405926527175E-2,0.12828709681168371,7.2050439107013229E-3,2.0688120407492579E-3,1.1275444630946858E-2,6.2372523050472613E-3,4.3477077999908756E-2,1.415480126361442E-5,4.96806575579536E-6,4.017177098610529E-2,0.28464914888720699,0.74975719692502107,74.975719692502111,340,71.916485184007442,0.71916485184007439,412.58214466559275,null,3.816032456711798E-2,null,0.45437939835897506,9.108550202180786E-2,0.11297795159130618,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR74, IF(MODE_ILIM=4,#REF!,#REF!))","v":74.975719692502111},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ74, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.45437939835897506},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA74, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.108550202180786E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB74, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11297795159130618},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S74, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":412.58214466559275},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P74, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7657159742719741}]
[null,null,null,null,null,null,null,69,0.34499999999999997,0.16487241857192095,0.42769715784088574,0.26268359304338806,1.7655608394266264,1.7655608394266264,1,1.7655608394266264,2.1785298240458395E-6,0.10077335326236962,412767.65496266598,2.4226704490458393E-6,0,6.6E-4,0.34824979420462165,1.4553350299627359E-2,9.8624282231074098E-2,0.11344178581832215,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.104942135153022,3.303855519142541E-5,3.303855519142541E-5,0.11055126679868789,8.3962272398759395E-3,1.657262134675104E-3,42.666666666666664,19.175506463083874,0.20504239087578499,8.6563651314026505E-2,0.29326330432448661,0.30212870185604807,0.32770092262465472,3.2645919985471179E-2,4.5404442045893258E-3,1.6661072750872294E-2,4.7646327772351213E-3,2.5966149732696741E-2,5.8968111088469485E-2,3.3844432885906044E-2,9.111123946070937E-2,6.1977063392644298E-3,0.45840575874449135,0.57189184771382273,1.7249999999999999,0.75101489942460853,3.8597366003042333E-3,1.4368095471548107E-2,2.7630605671414711E-2,0.12767832521865663,7.2537471746680826E-3,2.0743827281103932E-3,1.1304907437649607E-2,6.3361060356902834E-3,4.2938148058315549E-2,1.4384027364766802E-5,4.9042778522718911E-6,3.9667187443499174E-2,0.28313053014507383,0.75101489942460853,75.101489942460859,345,71.94908925319227,0.71949089253192267,412.76765496266597,null,3.7687299643727828E-2,null,0.45840575874449135,9.111123946070937E-2,0.11344178581832215,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR75, IF(MODE_ILIM=4,#REF!,#REF!))","v":75.101489942460859},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ75, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.45840575874449135},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA75, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.111123946070937E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB75, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11344178581832215},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S75, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":412.76765496266597},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P75, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7655608394266264}]
[null,null,null,null,null,null,null,70,0.35,0.16485793169806989,0.43269717882783715,0.26769083651071712,1.7654057045812794,1.7654057045812794,1,1.7654057045812794,2.177441410043655E-6,0.10081864725908356,412953.17917320627,2.4215820350436552E-6,0,6.6E-4,0.35320379268003527,1.497035029962736E-2,9.8668610297677761E-2,0.11391180854565593,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.10645318969568734,3.3996844789157984E-5,3.3996844789157984E-5,0.11214909964726447,8.6406879190124436E-3,1.6580070143804233E-3,42.666666666666664,18.953676418731707,0.20738982501608716,8.6602558560944801E-2,0.2956503905914124,0.30477814300716227,0.33243728896256397,3.3596423532204892E-2,4.5424849709052697E-3,1.69857093452544E-2,4.8385868661069359E-3,2.6366781182266603E-2,6.033812522107327E-2,3.3844432885906044E-2,9.1136978829945856E-2,6.2004919852856931E-3,0.46245373904346715,0.57641080902973008,1.75,0.75223171815035883,3.923534218600349E-3,1.4602469996679137E-2,2.7292272578378528E-2,0.1270843435922302,7.3012510427333272E-3,2.0798505781207889E-3,1.133367377761769E-2,6.4349556155436725E-3,4.2412376143845902E-2,1.4613431409965362E-5,4.8420492950275008E-6,3.9174929241304599E-2,0.28165911226575918,0.75223171815035883,75.223171815035883,350,71.978028730187987,0.71978028730187982,412.95317917320625,null,3.722582367000947E-2,null,0.46245373904346715,9.1136978829945856E-2,0.11391180854565593,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR76, IF(MODE_ILIM=4,#REF!,#REF!))","v":75.223171815035883},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ76, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.46245373904346715},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA76, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1136978829945856E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB76, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11391180854565593},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S76, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":412.95317917320625},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P76, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7654057045812794}]
[null,null,null,null,null,null,null,71,0.35499999999999998,0.16484344482421878,0.43769719981478855,0.27269807997804624,1.7652505697359318,1.7652505697359318,1,1.7652505697359318,2.1763538920433038E-6,0.1008639446530224,413138.71729877975,2.420494517043304E-6,0,6.6E-4,0.35815906963744665,1.5393350299627361E-2,9.8712941689057837E-2,0.11438802237243889,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.10796525898932997,3.4969491445899292E-5,3.4969491445899292E-5,0.11374804147201099,8.888829836899495E-3,1.6587519499546009E-3,42.666666666666664,18.73692011927832,0.20973929263978361,8.6641468726057075E-2,0.29803951331579526,0.30743376089792224,0.3371769425763641,3.4561240343963996E-2,4.5445258902865777E-3,1.7310631487867798E-2,4.9126882735053929E-3,2.676784565165977E-2,6.1723629695513295E-2,3.3844432885906044E-2,9.1162720129734531E-2,6.2032778402411788E-3,0.46652338856341125,0.58095764502311387,1.7749999999999999,0.75340913014698352,3.9874433235130655E-3,1.4837186957794643E-2,2.6962099772148702E-2,0.12650461435306121,7.3475987670813874E-3,2.0852192669436535E-3,1.1361768624408847E-2,6.5337975545296106E-3,4.1899285370255196E-2,1.4843005144753447E-5,4.7813235698879672E-6,3.8694549675930258E-2,0.28023318799438124,0.75340913014698352,75.340913014698359,355,72.003632642003467,0.72003632642003468,413.13871729877974,null,3.677547807749619E-2,null,0.46652338856341125,9.1162720129734531E-2,0.11438802237243889,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR77, IF(MODE_ILIM=4,#REF!,#REF!))","v":75.340913014698359},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ77, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.46652338856341125},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA77, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1162720129734531E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB77, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11438802237243889},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S77, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":413.13871729877974},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P77, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7652505697359318}]
[null,null,null,null,null,null,null,72,0.36,0.16482895795036764,0.44269722080173995,0.2777053234453753,1.7650954348905841,1.7650954348905841,1,1.7650954348905841,2.1752672689388352E-6,0.10090924544456832,413324.26934095181,2.419407893938835E-6,0,6.6E-4,0.36311557273623141,1.5822350299627364E-2,9.8757276405588346E-2,0.11487042993425388,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.10947832569362824,3.5956511390040428E-5,3.5956511390040428E-5,0.11534807576400501,9.1406576861490854E-3,1.6594969414039215E-3,42.666666666666664,18.525065461226923,0.2120907939756615,8.6680381809691592E-2,0.300430672726757,0.31009556701322583,0.3419198345295818,3.5540388666399927E-2,4.5465669627504706E-3,1.7635839210839523E-2,4.9869371180400728E-3,2.7169343291630066E-2,6.3124662667722264E-2,3.3844432885906044E-2,9.1188463360292626E-2,6.2060639041543924E-3,0.47061475694539512,0.58553240798685691,1.7999999999999998,0.75454854185737685,4.0514621617004157E-3,1.5072241004025922E-2,2.6639795026792663E-2,0.12593862557511407,7.3928315338722865E-3,2.0904922948619814E-3,1.1389215757734428E-2,6.6326285263002549E-3,4.1398421616468124E-2,1.5072740688685095E-5,4.7220468605215546E-6,3.8225623368179806E-2,0.27885113165259917,0.75454854185737685,75.454854185737688,360,72.026192211331946,0.72026192211331941,413.32426934095179,null,3.6335864278968608E-2,null,0.47061475694539512,9.1188463360292626E-2,0.11487042993425388,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR78, IF(MODE_ILIM=4,#REF!,#REF!))","v":75.454854185737688},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ78, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.47061475694539512},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA78, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1188463360292626E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB78, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11487042993425388},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S78, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":413.32426934095179},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P78, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7650954348905841}]
[null,null,null,null,null,null,null,73,0.36499999999999999,0.16481447107651656,0.44769724178869136,0.28271256691270441,1.7649403000452366,1.7649403000452366,1,1.7649403000452366,2.1741815396261178E-6,0.10095454963410348,413509.83530128788,2.418322164626118E-6,0,6.6E-4,0.36807325244244704,1.6257350299627358E-2,9.8801614447643293E-2,0.11535903390317313,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.11099237338468113,3.6957920848693412E-5,3.6957920848693412E-5,0.1169491868912427,9.3961761600771746E-3,1.6602419887346708E-3,42.666666666666664,18.31794803781634,0.21444432925254225,8.671929781217666E-2,0.3028238690534536,0.31276357287548012,0.34666591848514461,3.653388674790127E-2,4.5486081883141672E-3,1.7961332546301414E-2,5.0613335183383552E-3,2.7571274252953939E-2,6.4541262591642889E-2,3.3844432885906044E-2,9.1214208521837314E-2,6.2088501770488375E-3,0.47472789416600919,0.59013515058584887,1.825,0.75565129328572045,4.1155890673925267E-3,1.5307627123774415E-2,2.632507990186702E-2,0.12538588947289198,7.4369885850671591E-3,2.095672996648079E-3,1.1416037833852017E-2,6.7314453585273467E-3,4.0909352184152759E-2,1.5302630513132312E-5,4.6641678893515602E-6,3.7767745005786169E-2,0.27751139432836197,0.75565129328572045,75.565129328572041,365,72.045963869077937,0.72045963869077934,413.50983530128786,null,3.5906602490192244E-2,null,0.47472789416600919,9.1214208521837314E-2,0.11535903390317313,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR79, IF(MODE_ILIM=4,#REF!,#REF!))","v":75.565129328572041},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ79, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.47472789416600919},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA79, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1214208521837314E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB79, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11535903390317313},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S79, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":413.50983530128786},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P79, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7649403000452366}]
[null,null,null,null,null,null,null,74,0.37,0.16479998420266545,0.45269726277564276,0.28771981038003347,1.7647851651998891,1.7647851651998891,1,1.7647851651998891,2.1730967030028333E-6,0.10099985722201035,413695.41518135439,2.4172373280028335E-6,0,6.6E-4,0.37303206184396714,1.6698350299627358E-2,9.8845955815597006E-2,0.11585383698779687,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.11250738649482897,3.7973736047690473E-5,3.7973736047690473E-5,0.11855136004089385,9.6553899527038588E-3,1.6609870919531379E-3,42.666666666666664,18.115410713515875,0.2167998986992819,8.6758216733840779E-2,0.30521910252507584,0.31543779004474598,0.35141515053421024,3.7541752839594419E-2,4.5506495669948993E-3,1.8287111526390162E-2,5.1358775930454214E-3,2.7973638686430484E-2,6.5973468221059275E-2,3.3844432885906044E-2,9.1239955614585908E-2,6.2116366589480372E-3,0.47886285053933919,0.59476592585900157,1.85,0.75671866186942927,4.1798224572684476E-3,1.5543340625249034E-2,2.6017688938984478E-2,0.12484594099446676,7.4801073317335024E-3,2.1007645512078465E-3,1.1442256451034905E-2,6.8302450238708094E-3,4.0431664549180159E-2,1.5532667420643915E-5,4.6076377695949736E-6,3.7320528173889492E-2,0.27621249940207565,0.75671866186942927,75.671866186942921,370,72.063171902227168,0.72063171902227163,413.69541518135441,null,3.5487330634059414E-2,null,0.47886285053933919,9.1239955614585908E-2,0.11585383698779687,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR80, IF(MODE_ILIM=4,#REF!,#REF!))","v":75.671866186942921},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ80, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.47886285053933919},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA80, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1239955614585908E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB80, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11585383698779687},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S80, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":413.69541518135441},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P80, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7647851651998891}]
[null,null,null,null,null,null,null,75,0.375,0.16478549732881437,0.45769728376259416,0.29272705384736258,1.7646300303545417,1.7646300303545417,1,1.7646300303545417,2.1720127579684781E-6,0.10104516820867127,413881.00898271747,2.4161533829684783E-6,0,6.6E-4,0.37799195647997769,1.7145350299627361E-2,9.8890300509823642E-2,0.11635484193329164,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.11402335025713342,3.9003973211582787E-5,3.9003973211582787E-5,0.12015458116604207,9.9183037587534627E-3,1.6617322510656105E-3,42.666666666666664,17.917303226439724,0.21915750254477068,8.6797138575012409E-2,0.30761637337084868,0.31811823011888074,0.35616748903829187,3.8564005195343892E-2,4.5526910988098928E-3,1.8613176183247263E-2,5.2105694608242433E-3,2.83764367428814E-2,6.7421318611444833E-2,3.3844432885906044E-2,9.126570463875569E-2,6.2144233498755037E-3,0.48301967671895679,0.59942478722127779,1.875,0.75775186608342293,4.2441608256864414E-3,1.5779377118352398E-2,2.5717368913923053E-2,0.12431833651177362,7.5222234595174065E-3,2.105769990558328E-3,1.1467892210515513E-2,6.929024631571524E-3,3.9964965199396976E-2,1.5762844525730502E-5,4.5524098675299175E-6,3.6883604266365673E-2,0.2749530383820542,0.75775186608342293,75.775186608342295,375,72.078010752951272,0.72078010752951271,413.88100898271745,null,3.5077703320489123E-2,null,0.48301967671895679,9.126570463875569E-2,0.11635484193329164,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR81, IF(MODE_ILIM=4,#REF!,#REF!))","v":75.775186608342295},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ81, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.48301967671895679},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA81, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.126570463875569E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB81, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11635484193329164},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S81, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":413.88100898271745},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P81, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7646300303545417}]
[null,null,null,null,null,null,null,76,0.38,0.16477101045496323,0.46269730474954557,0.29773429731469164,1.764474895509194,1.764474895509194,1,1.764474895509194,2.1709297034243535E-6,0.10109048259446876,414066.61670694401,2.4150703284243532E-6,0,6.600000000000001E-4,0.38295289418355538,1.759835029962736E-2,9.8934648530697625E-2,0.11686205152143014,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.11554025065410438,4.0048648563639805E-5,4.0048648563639805E-5,0.12175883693651166,1.0184922273654709E-2,1.6624774660783804E-3,42.666666666666664,17.723481816566849,0.22151714101793329,8.683606333602012E-2,0.31001568182003181,0.32080490473368367,0.36092289448349701,3.9600662071753043E-2,4.5547327837763846E-3,1.8939526549019047E-2,5.2854092403556117E-3,2.8779668573151045E-2,6.8884853121827447E-2,3.3844432885906051E-2,9.1291455594564086E-2,6.2172102498547653E-3,0.48719842369992999,0.60411178846574154,1.9,0.75875206879806334,4.3086027402404322E-3,1.6015732497808601E-2,2.5423878139849178E-2,0.12380265260041648,7.563371026907394E-3,2.1106922081916956E-3,1.1492964773263666E-2,7.0277814196185676E-3,3.9508878551829531E-2,1.5993155236962259E-5,4.4984396741762596E-6,3.6456621471558967E-2,0.27373166702459567,0.75875206879806334,75.875206879806328,380,72.090646982404948,0.72090646982404949,414.06661670694399,null,3.4677390896044699E-2,null,0.48719842369992999,9.1291455594564086E-2,0.11686205152143014,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR82, IF(MODE_ILIM=4,#REF!,#REF!))","v":75.875206879806328},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ82, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.48719842369992999},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA82, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1291455594564086E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB82, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11686205152143014},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S82, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":414.06661670694399},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P82, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.764474895509194}]
[null,null,null,null,null,null,null,77,0.38500000000000001,0.16475652358111215,0.46769732573649697,0.30274154078202076,1.7643197606638465,1.7643197606638465,1,1.7643197606638465,2.1698475382735699E-6,0.10113580037978516,414252.23835559998,2.4139881632735701E-6,0,6.6E-4,0.38791483493617684,1.8057350299627357E-2,9.8978999878593085E-2,0.1173754685706305,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.11705807437030001,4.1107778325848065E-5,4.1107778325848065E-5,0.12336411469342042,1.0455250193540783E-2,1.6632227369977339E-3,42.666666666666664,17.533808877833064,0.2238788143477283,8.687499101719233E-2,0.31241702810191835,0.32349782556303963,0.36568132934581088,4.0651741728164298E-2,4.5567746219116008E-3,1.9266162655856626E-2,5.3603970503381011E-3,2.9183334328106329E-2,7.0364111416671232E-2,3.3844432885906044E-2,9.1317208482228296E-2,6.2199973589093342E-3,0.49139914282084846,0.60882698376562261,1.925,0.75972038041018086,4.3731468376162225E-3,1.6252402927434489E-2,2.513698581762484E-2,0.12329848490192601,7.6035825568580859E-3,2.1155339668740124E-3,1.1517492912928015E-2,7.1265127474456052E-3,3.9063045943056617E-2,1.6223593240275677E-5,4.4456846856473169E-6,3.6039243826552873E-2,0.27254710171624269,0.75972038041018086,75.972038041018081,385,72.101220909974245,0.7210122090997424,414.25223835559996,null,3.4286078557772673E-2,null,0.49139914282084846,9.1317208482228296E-2,0.1173754685706305,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR83, IF(MODE_ILIM=4,#REF!,#REF!))","v":75.972038041018081},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ83, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.49139914282084846},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA83, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1317208482228296E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB83, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1173754685706305},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S83, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":414.25223835559996},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P83, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7643197606638465}]
[null,null,null,null,null,null,null,78,0.39,0.16474203670726106,0.47269734672344838,0.30774878424934982,1.7641646258184995,1.7641646258184995,1,1.7641646258184995,2.168766261421034E-6,0.10118112156500321,414437.87393025315,2.4129068864210338E-6,0,6.6E-4,0.39287774073312087,1.8522350299627361E-2,9.902335455388464E-2,0.11789509593599756,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.11857680874846567,4.2181378718910617E-5,4.2181378718910617E-5,0.12497040240713565,1.0729292215249575E-2,1.6639680638299665E-3,42.666666666666664,17.348152632326055,0.22624252276314932,8.6913921618857845E-2,0.31482041244583714,0.32619700431906729,0.37044275796646758,4.171726242666008E-2,4.5588166132327851E-3,1.9593084535916003E-2,5.4355330094881232E-3,2.9587434158636912E-2,7.185913346777667E-2,3.3844432885906044E-2,9.1342963301965868E-2,6.2227846770627517E-3,0.49562188576587257,0.6135704276764069,1.9500000000000002,0.76065786176487427,4.4377918197245582E-3,1.6489384825465622E-2,2.4856471429528432E-2,0.12280544706204424,7.6428891222914304E-3,2.1202979059228859E-3,1.1541494565239873E-2,7.2252160891151419E-3,3.8627124687047647E-2,1.6454152483395345E-5,4.3941042914966336E-6,3.5631150334636277E-2,0.27139811609779096,0.76065786176487427,76.065786176487421,390,72.109847935853821,0.72109847935853821,414.43787393025315,null,3.390346552625656E-2,null,0.49562188576587257,9.1342963301965868E-2,0.11789509593599756,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR84, IF(MODE_ILIM=4,#REF!,#REF!))","v":76.065786176487421},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ84, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.49562188576587257},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA84, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1342963301965868E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB84, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11789509593599756},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S84, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":414.43787393025315},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P84, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7641646258184995}]
[null,null,null,null,null,null,null,79,0.39500000000000002,0.16472754983340995,0.47769736771039978,0.31275602771667893,1.7640094909731521,1.7640094909731521,1,1.7640094909731521,2.1676858717734517E-6,0.10122644615050544,414623.52343247028,2.4118264967734519E-6,0,6.6E-4,0.39784157545882681,1.8993350299627364E-2,9.906771255694663E-2,0.11842093650936317,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.12009644174890673,4.3269465962245638E-5,4.3269465962245638E-5,0.12657768863833901,1.1007053036323695E-2,1.6647134465813682E-3,42.666666666666664,17.166386824962167,0.22860826649322391,8.6952855141345209E-2,0.31722583508115049,0.32890245275226304,0.37520714643653713,4.2797242432062906E-2,4.5608587577571739E-3,1.9920292221357952E-2,5.5108172365398809E-3,2.9991968215655009E-2,7.3369959556196684E-2,3.3844432885906044E-2,9.1368720053994171E-2,6.2255722043385421E-3,0.49986670456679244,0.61834217513793566,1.9750000000000001,0.76156552688422341,4.50253645008935E-3,1.672667485085514E-2,2.4582124173041654E-2,0.12232316973917171,7.6813204259474251E-3,2.1249865480041288E-3,1.1564986874151993E-2,7.3238890269530805E-3,3.8200787195263722E-2,1.6684827161284337E-5,4.3436596704434557E-6,3.5232034141092237E-2,0.27028353791140214,0.76156552688422341,76.156552688422337,395,72.116619551864289,0.72116619551864292,414.62352343247028,null,3.3529264273319551E-2,null,0.49986670456679244,9.1368720053994171E-2,0.11842093650936317,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR85, IF(MODE_ILIM=4,#REF!,#REF!))","v":76.156552688422337},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ85, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.49986670456679244},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA85, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1368720053994171E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB85, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11842093650936317},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S85, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":414.62352343247028},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P85, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7640094909731521}]
[null,null,null,null,null,null,null,80,0.4,0.16471306295955884,0.48269738869735118,0.31776327118400804,1.7638543561278044,1.7638543561278044,1,1.7638543561278044,2.1666063682393223E-6,0.10127177413667457,414809.18686381902,2.4107469932393226E-6,0,6.6E-4,0.40280630477136448,1.9470350299627362E-2,9.9112073888153601E-2,0.11895299321932809,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.12161696191182365,4.4372056273985893E-5,4.4372056273985893E-5,0.1281859625019382,1.1288537355010689E-2,1.6654588852582336E-3,42.666666666666664,16.988390437158369,0.23097604576701405,8.6991791584983186E-2,0.31963329623725545,0.33161418265164988,0.37997446248995048,4.3891700011936138E-2,4.5629010555020104E-3,2.0247785744348098E-2,5.5862498502454103E-3,3.0396936650095518E-2,7.4896630274171552E-2,3.3844432885906044E-2,9.1394478738530696E-2,6.2283599407602442E-3,0.50413365160511237,0.62314228147653228,2,0.76244434551763096,4.5673795504720194E-3,1.6964269890471874E-2,2.4313742431647613E-2,0.12185129967762864,7.7189048750153514E-3,2.1296023054841627E-3,1.1587986234961484E-2,7.422529245599197E-3,3.7783720154274177E-2,1.6915611702545333E-5,4.2943136929141593E-6,3.4841601762862037E-2,0.26920224605381204,0.76244434551763096,76.244434551763092,400,72.121604042494241,0.72121604042494236,414.80918686381904,null,3.3163199800209334E-2,null,0.50413365160511237,9.1394478738530696E-2,0.11895299321932809,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR86, IF(MODE_ILIM=4,#REF!,#REF!))","v":76.244434551763092},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ86, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.50413365160511237},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA86, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1394478738530696E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB86, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11895299321932809},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S86, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":414.80918686381904},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P86, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7638543561278044}]
[null,null,null,null,null,null,null,81,0.40500000000000003,0.1646985760857077,0.48769740968430259,0.3227705146513371,1.7636992212824565,1.7636992212824565,1,1.7636992212824565,2.1655277497289341E-6,0.10131710552389335,414994.86422586715,2.4096683747289344E-6,0,6.600000000000001E-4,0.40777189599525049,1.9953350299627366E-2,9.9156438547880185E-2,0.11949126903130414,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.12313835832235966,4.5489165870977528E-5,4.5489165870977528E-5,0.12979521363358495,1.1573749870263127E-2,1.6662043798668566E-3,42.666666666666664,16.814047418134827,0.23334586081361622,8.7030730950100582E-2,0.32204279614358367,0.33433220584492473,0.38474467540425128,4.5000653436584492E-2,4.5649435064845393E-3,2.0575565137056884E-2,5.6618309693745577E-3,3.080233961291598E-2,7.6439186527081107E-2,3.3844432885906051E-2,9.1420239355792937E-2,6.2311478863513962E-3,0.50842277961415017,0.62797080240714309,2.0250000000000004,0.76329524552725547,4.6323199977136619E-3,1.72021670471296E-2,2.405113327984755E-2,0.12138949884083977,7.7556696509391947E-3,2.1341474863716399E-3,1.161050833464425E-2,7.5211345264421751E-3,3.7375623756549341E-2,1.7146500756700166E-5,4.2460308298854844E-6,3.4459572368019963E-2,0.26815316782008375,0.76329524552725547,76.329524552725545,405,72.124846875437001,0.72124846875436999,414.99486422586716,null,3.2805008962456063E-2,null,0.50842277961415017,9.1420239355792937E-2,0.11949126903130414,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR87, IF(MODE_ILIM=4,#REF!,#REF!))","v":76.329524552725545},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ87, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.50842277961415017},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA87, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1420239355792937E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB87, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11949126903130414},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S87, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":414.99486422586716},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P87, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7636992212824565}]
[null,null,null,null,null,"Eff (%)","Iout (mA)",82,0.41,0.16468408921185665,0.49269743067125393,0.32777775811866616,1.7635440864371095,1.7635440864371095,1,1.7635440864371095,2.1644500151543635E-6,0.10136244031254449,415180.55552018224,2.4085906401543633E-6,0,6.5999999999999989E-4,0.41273831802191729,2.0442350299627363E-2,9.9200806536500888E-2,0.12003576694755647,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.1246606205781377,4.6620810968779229E-5,4.6620810968779229E-5,0.13140543215858391,1.1862695281738745E-2,1.6669499304135316E-3,42.666666666666664,16.643246432594456,0.23571771186216089,8.7069673237026135E-2,0.32445433502960053,0.33705653419860598,0.38951775590843357,4.6124120979054377E-2,4.5669861107220048E-3,2.0903630431659576E-2,5.7375607127149956E-3,3.1208177255096572E-2,7.7997669535414774E-2,3.3844432885906037E-2,9.1446001905998386E-2,6.2339360411355366E-3,0.51273414168115472,0.63282779403549783,2.0499999999999998,0.76411911512084008,4.697356720779043E-3,1.7440363628385427E-2,2.3794112019842623E-2,0.12093744359997023,7.7916407747574542E-3,2.1386242998789658E-3,1.1632568189609133E-2,7.6197027424104889E-3,3.697621098046084E-2,1.7377489182282704E-5,4.1987770675592292E-6,3.4085677101341541E-2,0.26713527632368561,0.76411911512084008,76.411911512084004,410,72.126370778645395,0.72126370778645399,415.18055552018222,null,3.245443983792054E-2,null,0.51273414168115472,9.1446001905998386E-2,0.12003576694755647,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR88, IF(MODE_ILIM=4,#REF!,#REF!))","v":76.411911512084004},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ88, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.51273414168115472},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA88, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1446001905998386E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB88, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12003576694755647},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S88, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":415.18055552018222},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P88, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7635440864371095}]
[null,null,null,null,null,{"$f":"BT51","v":68.427867006324419},{"$f":"I56*1000","v":250},83,0.41499999999999998,0.16466960233800551,0.49769745165820534,0.33278500158599522,1.7633889515917618,1.7633889515917618,1,1.7633889515917618,2.1633731634294653E-6,0.10140777850301097,415366.26074833295,2.407513788429465E-6,0,6.600000000000001E-4,0.41770554121720882,2.0937350299627362E-2,9.9245177854390576E-2,0.12058649000724742,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.12618373875908287,4.7767007781661422E-5,4.7767007781661422E-5,0.13301660866299622,1.2155378289800615E-2,1.6676955369045567E-3,42.666666666666664,16.475880623626544,0.2380915991418136,8.7108618446088804E-2,0.32686791312480695,0.33978717961818472,0.39429367609728611,4.7262120915134716E-2,4.5690288682316629E-3,2.1231981660336307E-2,5.8134391990722302E-3,3.1614449727640201E-2,7.9572120836760324E-2,3.3844432885906051E-2,9.1471766389364717E-2,6.2367244051362196E-3,0.51706779124944602,0.63771331286029287,2.0749999999999997,0.76491680494320791,4.7624886979876456E-3,1.7678857136050774E-2,2.3542501747542376E-2,0.12049482397391875,7.8268431683071009E-3,2.1430348616317744E-3,1.1654180181062271E-2,7.7182318530928575E-3,3.6585206915855838E-2,1.7608572035684725E-5,4.1525198274377692E-6,3.3719658452561148E-2,0.26614758807987365,0.76491680494320791,76.491680494320789,415,72.126175499523185,0.72126175499523182,415.36626074833293,null,3.2111251134843005E-2,null,0.51706779124944602,9.1471766389364717E-2,0.12058649000724742,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR89, IF(MODE_ILIM=4,#REF!,#REF!))","v":76.491680494320789},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ89, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.51706779124944602},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA89, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1471766389364717E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB89, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12058649000724742},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S89, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":415.36626074833293},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P89, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7633889515917618}]
[null,null,null,null,null,{"$f":"BT81","v":72.078010752951272},{"$f":"I81*1000","v":375},84,0.42,0.16465511546415443,0.50269747264515674,0.33779224505332434,1.7632338167464143,1.7632338167464143,1,1.7632338167464143,2.162297193469877E-6,0.10145312009567557,415551.97991188715,2.4064378184698773E-6,0,6.6E-4,0.42267353733533086,2.1438350299627359E-2,9.9289552501923797E-2,0.12114344128647946,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.12770770339934462,4.8927772522604928E-5,4.8927772522604928E-5,0.1346287341667588,1.2451803595517197E-2,1.6684411993462271E-3,42.666666666666664,16.311847389773565,0.24046752288177362,8.7147566577617408E-2,0.32928353065873728,0.3425241540482718,0.3990724093517114,4.8414671523357093E-2,4.5710717790307586E-3,2.1560618855271968E-2,5.8894665472695833E-3,3.2021157181572307E-2,8.1162582287809912E-2,3.3844432885906044E-2,9.1497532806109394E-2,6.2395129783769862E-3,0.52142378212056806,0.64262741577538796,2.1,0.76568913003675121,4.8277149544175947E-3,1.7917645256362493E-2,2.3296132945756616E-2,0.12006134291691355,7.8613007115938896E-3,2.1473811985520935E-3,1.1675358088156271E-2,7.8167199001641895E-3,3.6202348131874458E-2,1.7839744560699726E-5,4.1072278914057549E-6,3.3361269664199528E-2,0.26518916074044274,0.76568913003675121,76.568913003675121,420,72.124237241864293,0.72124237241864297,415.55197991188714,null,3.1775211636969392E-2,null,0.52142378212056806,9.1497532806109394E-2,0.12114344128647946,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR90, IF(MODE_ILIM=4,#REF!,#REF!))","v":76.568913003675121},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ90, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.52142378212056806},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA90, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1497532806109394E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB90, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12114344128647946},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S90, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":415.55197991188714},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P90, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7632338167464143}]
[null,null,null,null,null,{"$f":"BT106","v":71.049894896969974},{"$f":"I106*1000","v":500},85,0.42499999999999999,0.16464062859030332,0.50769749363210814,0.34279948852065339,1.7630786819010669,1.7630786819010669,1,1.7630786819010669,2.161222104193009E-6,0.10149846509092139,415737.71301241399,2.4053627291930088E-6,0,6.6E-4,0.42764227943873995,2.194535029962736E-2,9.933393047947553E-2,0.12170662389834033,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.12923250546115267,5.0103121403300564E-5,5.0103121403300564E-5,0.13624180009865941,1.2751975900662552E-2,1.6691869177448422E-3,42.666666666666664,16.151048175283751,0.24284548331127509,8.7186517631941018E-2,0.33170118786096092,0.34526746947275083,0.40385393026454552,4.95817910849966E-2,4.5731148431365541E-3,2.1889542048656358E-2,5.9656428761482297E-3,3.2428299767941142E-2,8.2769096066385925E-2,3.3844432885906044E-2,9.152330115645016E-2,6.2423017608813965E-3,0.52580216845646832,0.64757016007202972,2.125,0.76643687168038832,4.8930345594707927E-3,1.8156725850766914E-2,2.3054843102605159E-2,0.11963671565026997,7.8950362966063517E-3,2.1516652534387969E-3,1.1696115119084551E-2,7.9151650030949011E-3,3.5827382083955951E-2,1.8071002178714539E-5,4.0628713314559061E-6,3.3010274176099634E-2,0.26425909096890315,0.76643687168038832,76.643687168038838,425,72.120507778355574,0.72120507778355569,415.73771301241402,null,3.1446099683073832E-2,null,0.52580216845646832,9.152330115645016E-2,0.12170662389834033,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR91, IF(MODE_ILIM=4,#REF!,#REF!))","v":76.643687168038838},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ91, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.52580216845646832},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA91, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.152330115645016E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB91, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12170662389834033},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S91, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":415.73771301241402},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P91, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7630786819010669}]
[null,null,null,null,null,null,null,86,0.43,0.16462614171645223,0.51269751461905955,0.34780673198798251,1.7629235470557194,1.7629235470557194,1,1.7629235470557194,2.1601478945180447E-6,0.10154381348913132,415923.46005148184,2.4042885195180449E-6,0,6.6E-4,0.43261174182349849,2.2458350299627356E-2,9.9378311787420487E-2,0.12227604099294724,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.13075813631045133,5.1293070634147713E-5,5.1293070634147713E-5,0.13785579827301842,1.3055899907716419E-2,1.6699326921066997E-3,42.666666666666664,15.993388272648518,0.2452254806595861,8.7225471609388538E-2,0.33412088496108133,0.3480171379149275,0.40863821457143706,5.0763497884072077E-2,4.5751580605663013E-3,2.2218751272684037E-2,6.0419683045671631E-3,3.28358776378175E-2,8.4391704673484239E-2,3.3844432885906044E-2,9.1549071440604576E-2,6.2450907526730012E-3,0.53020300478168925,0.65254160344108847,2.15,0.76716077911568981,4.9584466245866654E-3,1.8396096947272483E-2,2.281847635333982E-2,0.11922066903514741,7.9280718778279111E-3,2.1558888892669993E-3,1.1716463940267688E-2,8.0135653551233529E-3,3.5460066557227651E-2,1.8302340479501799E-5,4.019421443726501E-6,3.266644510404286E-2,0.26335651244602609,0.76716077911568981,76.716077911568988,430,72.229662267470047,0.72229662267470052,415.92346005148187,null,3.1123702678414883E-2,null,0.53020300478168925,9.1549071440604576E-2,0.12227604099294724,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR92, IF(MODE_ILIM=4,#REF!,#REF!))","v":76.716077911568988},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ92, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.53020300478168925},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA92, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1549071440604576E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB92, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12227604099294724},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S92, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":415.92346005148187},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P92, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7629235470557194}]
[null,null,null,null,null,null,null,87,0.435,0.16461165484260112,0.51769753560601095,0.35281397545531157,1.7627684122103719,1.7627684122103719,1,1.7627684122103719,2.1590745633659326E-6,0.10158916529068858,416109.22103066044,2.4032151883659324E-6,0,6.6E-4,0.43758189994966812,2.2977350299627362E-2,9.942269642613373E-2,0.12285169575749279,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.13228458769417514,5.249763642425374E-5,5.249763642425374E-5,0.13947072086794468,1.3363580319864385E-2,1.6706785224381018E-3,42.666666666666664,15.838776636593348,0.24760751515600984,8.7264428510289177E-2,0.3365426221887371,0.35077317143768277,0.41342523908639295,5.195981020734692E-2,4.5772014313372657E-3,2.254824655955447E-2,6.1184429514032357E-3,3.3243890942294969E-2,8.6030450935337482E-2,3.3844432885906044E-2,9.1574843658790442E-2,6.2478799537753673E-3,0.53462634598558612,0.65754180397532092,2.1749999999999998,0.76786157116816556,5.0239503010948905E-3,1.863575673233115E-2,2.2586883143920298E-2,0.11881294098340138,7.9604285196812324E-3,2.1600538932263339E-3,1.1736416703767247E-2,8.1119192194727286E-3,3.5100169143699587E-2,1.8533755212571306E-5,3.9768506865450327E-6,3.2329564750031244E-2,0.26248059399652524,0.76786157116816556,76.786157116816554,435,72.361493645121143,0.72361493645121144,416.10922103066042,null,3.0807816635863315E-2,null,0.53462634598558612,9.1574843658790442E-2,0.12285169575749279,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR93, IF(MODE_ILIM=4,#REF!,#REF!))","v":76.786157116816554},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ93, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.53462634598558612},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA93, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1574843658790442E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB93, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12285169575749279},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S93, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":416.10922103066042},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P93, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7627684122103719}]
[null,null,null,null,null,null,null,88,0.44,0.16459716796875001,0.52269755659296235,0.35782121892264068,1.7626132773650243,1.7626132773650243,1,1.7626132773650243,2.1580021096593892E-6,0.1016345204959762,416294.99595151847,2.4021427346593894E-6,0,6.6E-4,0.4425527303763489,2.3502350299627363E-2,9.9467084395990071E-2,0.12343359141629051,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.13381185171903723,5.3716834981432817E-5,5.3716834981432817E-5,0.14108656040504264,1.3675021840997987E-2,1.6714244087453467E-3,42.666666666666664,15.687125708754527,0.24999158702988306,8.7303388334971907E-2,0.33896639977360032,0.35353558214362402,0.41821498164162418,5.3170746344329237E-2,4.5792449554667037E-3,2.2878027941471882E-2,6.1950669355511235E-3,3.3652339832489706E-2,8.7685378005496167E-2,3.3844432885906044E-2,9.1600617811225388E-2,6.2506693642120506E-3,0.53907224732455761,0.66257082017164737,2.2000000000000002,0.76853993777107044,5.0895447781969926E-3,1.8875703543211025E-2,2.2359919914817467E-2,0.11841327990385753,7.9921264411198217E-3,2.1641619805163981E-3,1.1755985073051159E-2,8.2102249257952325E-3,3.4747466750892735E-2,1.876524227904056E-5,3.9351326221970307E-6,3.1999424142013982E-2,0.26163053782837353,0.76853993777107044,76.85399377710705,440,72.477313046906502,0.724773130469065,416.2949959515185,null,3.0498245744619498E-2,null,0.53907224732455761,9.1600617811225388E-2,0.12343359141629051,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR94, IF(MODE_ILIM=4,#REF!,#REF!))","v":76.85399377710705},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ94, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.53907224732455761},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA94, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1600617811225388E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB94, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12343359141629051},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S94, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":416.2949959515185},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P94, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7626132773650243}]
[null,null,null,null,null,null,null,89,0.44500000000000001,0.1645826810948989,0.52769757757991376,0.36282846238996974,1.7624581425196768,1.7624581425196768,1,1.7624581425196768,2.1569305323228884E-6,0.10167987910537746,416480.78481562604,2.4010711573228882E-6,0,6.6E-4,0.44752421070100928,2.4033350299627363E-2,9.9511475697364682E-2,0.12402173123082189,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.13533992083171559,5.4950682512205133E-5,5.4950682512205133E-5,0.14270330973045958,1.399022917571488E-2,1.6721703510347386E-3,42.666666666666664,15.538351252332335,0.25237769651057762,8.7342351083765993E-2,0.34139221794537833,0.35630438217523958,0.42300742103136629,5.4396324587272712E-2,4.5812886329718869E-3,2.3208095450645391E-2,6.2718403759233678E-3,3.4061224459540643E-2,8.9356529366930185E-2,3.3844432885906044E-2,9.1626393898127267E-2,6.2534589840066252E-3,0.54354076442430366,0.66762871093345555,2.2250000000000001,0.76919654139849469,5.1552292810676933E-3,1.9115935860826629E-2,2.2137448803639766E-2,0.11802144418154882,8.0231850575652013E-3,2.1682147979162651E-3,1.1775180247225382E-2,8.3084808668277953E-3,3.4401745139718325E-2,1.8996797723988736E-5,3.8942418621613076E-6,3.1675822601013766E-2,0.26080557787693581,0.76919654139849469,76.91965413984947,445,72.230234640211876,0.72230234640211877,416.48078481562607,null,3.0194801964604882E-2,null,0.54354076442430366,9.1626393898127267E-2,0.12402173123082189,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR95, IF(MODE_ILIM=4,#REF!,#REF!))","v":76.91965413984947},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ95, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54354076442430366},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA95, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1626393898127267E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB95, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12402173123082189},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S95, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":416.48078481562607},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P95, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7624581425196768}]
[null,null,null,null,null,null,null,90,0.45,0.16456819422104782,0.53269759856686516,0.36783570585729886,1.7623030076743296,1.7623030076743296,1,1.7623030076743296,2.1558598302826635E-6,0.10172524111927553,416666.58762455254,2.4000004552826637E-6,0,6.6E-4,0.45249631950277935,2.4570350299627362E-2,9.9555870330632512E-2,0.12461611849978302,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.13686878780033057,5.6199195221795762E-5,5.6199195221795762E-5,0.14432096199717076,1.4309207029318911E-2,1.6729163493125784E-3,42.666666666666664,15.392372196064581,0.25476584382749945,8.7381316757000574E-2,0.34382007693381261,0.35907958371505172,0.42780253695936771,5.5636563231176842E-2,4.5833324638700785E-3,2.3538449119288905E-2,6.3487633914503464E-3,3.447054497460933E-2,9.1043948834148888E-2,3.3844432885906044E-2,9.165217191971381E-2,6.2562488131826573E-3,0.54803195328209708,0.67271553557291974,2.25,0.76983201841398097,5.2210030690680587E-3,1.9356452302994952E-2,2.1919337365287721E-2,0.11763720168764763,8.0536230203719864E-3,2.1722139271435604E-3,1.179401298383707E-2,8.4066854952447537E-3,3.4062798489596174E-2,1.9228417729260616E-5,3.8541540155732745E-6,3.1358567333768211E-2,0.26000497824670499,0.76983201841398097,76.983201841398099,450,72.8349974854723,0.72834997485472297,416.66658762455256,null,2.9897304644761407E-2,null,0.54803195328209708,9.165217191971381E-2,0.12461611849978302,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR96, IF(MODE_ILIM=4,#REF!,#REF!))","v":76.983201841398099},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ96, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54803195328209708},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA96, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.165217191971381E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB96, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12461611849978302},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S96, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":416.66658762455256},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P96, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7623030076743296}]
[null,null,null,null,null,null,null,91,0.45500000000000002,0.16455370734719671,0.53769761955381656,0.37284294932462791,1.7621478728289819,1.7621478728289819,1,1.7621478728289819,2.1547900024667E-6,0.10177060653805377,416852.40437986824,2.3989306274667002E-6,0,6.6E-4,0.45746903628940983,2.5113350299627364E-2,9.9600268296168776E-2,0.12521675655913256,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.13839844569711759,5.7462389314134031E-5,5.7462389314134031E-5,0.14593951064841018,1.4631960107820334E-2,1.6736624035851709E-3,42.666666666666664,15.249110486913285,0.25715602921008895,8.7420285355004956E-2,0.3462499769686791,0.36186119898577168,0.43260030998977439,5.6891480573787664E-2,4.5853764481785511E-3,2.38690889796212E-2,6.4258361010802994E-3,3.4880301528880053E-2,9.2747680555341327E-2,3.3844432885906044E-2,9.167795187620284E-2,6.2590388517637218E-3,0.55254587026907953,0.67783135381334403,2.2749999999999999,0.77044698034041825,5.2868654340627857E-3,1.959725161808859E-2,2.170545830844357E-2,0.11726032931800361,8.0834582539894111E-3,2.1761608880174785E-3,1.1812493620346774E-2,8.5048373206940836E-3,3.3730428988957686E-2,1.9460098606690149E-5,3.8148456406964939E-6,3.1047473049149302E-2,0.25922803174400061,0.77044698034041825,77.044698034041829,455,73.305168165960453,0.73305168165960455,416.85240437986823,null,2.9605580163631323E-2,null,0.55254587026907953,9.167795187620284E-2,0.12521675655913256,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR97, IF(MODE_ILIM=4,#REF!,#REF!))","v":77.044698034041829},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ97, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.55254587026907953},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA97, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.167795187620284E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB97, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12521675655913256},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S97, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":416.85240437986823},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P97, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7621478728289819}]
[null,null,null,null,null,null,null,92,0.46,0.1645392204733456,0.54269764054076797,0.37785019279195703,1.7619927379836344,1.7619927379836344,1,1.7619927379836344,2.153721047804733E-6,0.10181597536209558,417038.23508314346,2.3978616728047332E-6,0,6.6E-4,0.46244234144762453,2.5662350299627362E-2,9.9644669594348687E-2,0.12582364878213997,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.13992888788220526,5.8740280991852307E-5,5.8740280991852307E-5,0.14755894940216055,1.4958493117935862E-2,1.674408513858821E-3,42.666666666666664,15.108490950902036,0.25954825288782135,8.745925687810846E-2,0.34868191827978862,0.36464924025045509,0.43740072150115494,5.8161094915598191E-2,4.5874205859145782E-3,2.4200015063865883E-2,6.5030586237793241E-3,3.5290494273559785E-2,9.4467769014536018E-2,3.3844432885906044E-2,9.1703733767812268E-2,6.2618290997733996E-3,0.55708257213257673,0.68297622579152639,2.3000000000000003,0.77104201505652292,5.3528156988343328E-3,1.9838332679059038E-2,2.1495689247293687E-2,0.11689061255835741,8.1127079909745041E-3,2.1800571414389166E-3,1.1830632094359224E-2,8.6029349070048024E-3,3.3404446449420887E-2,1.9691836791714857E-5,3.7762941991995677E-6,3.07423615967569E-2,0.25847405849449062,0.77104201505652292,77.104201505652298,460,73.638455592594738,0.73638455592594743,417.03823508314343,null,2.9319461590714264E-2,null,0.55708257213257673,9.1703733767812268E-2,0.12582364878213997,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR98, IF(MODE_ILIM=4,#REF!,#REF!))","v":77.104201505652298},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ98, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.55708257213257673},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA98, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1703733767812268E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB98, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12582364878213997},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S98, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":417.03823508314343},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P98, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7619927379836344}]
[null,null,null,null,null,null,null,93,0.46500000000000002,0.16452473359949449,0.54769766152771937,0.38285743625928614,1.7618376031382867,1.7618376031382867,1,1.7618376031382867,2.1526529652282446E-6,0.10186134759178436,417224.07973594876,2.3967935902282444E-6,0,6.6E-4,0.46741621619661566,2.6217350299627361E-2,9.9689074225547458E-2,0.12643679857943407,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.14146010798841852,6.0032886456285082E-5,6.0032886456285082E-5,0.14917927223662572,1.5288810767088865E-2,1.6751546801398345E-3,42.666666666666664,14.970441161582707,0.26194251509020583,8.749823132664046E-2,0.35111590109698615,0.36744371981265767,0.44220375364343639,5.9445424559848872E-2,4.5894648770954368E-3,2.4531227404251389E-2,6.580431078531377E-3,3.5701123359878198E-2,9.6204259033780756E-2,3.3844432885906044E-2,9.1729517594759946E-2,6.2646195572352709E-3,0.56164211599843361,0.68815021206014171,2.3250000000000002,0.77161768792481089,5.4188532155879177E-3,2.0079694477805519E-2,2.1289912467466712E-2,0.11652784507444859,8.1413888050005222E-3,2.1839040921999785E-3,1.184843796269577E-2,8.7009768695541119E-3,3.3084667942056681E-2,1.9923628837355433E-5,3.7384780130509876E-6,3.0443061626205126E-2,0.25774240463987136,0.77161768792481089,77.161768792481084,465,73.832411821820315,0.73832411821820321,417.22407973594875,null,2.9038788367214005E-2,null,0.56164211599843361,9.1729517594759946E-2,0.12643679857943407,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR99, IF(MODE_ILIM=4,#REF!,#REF!))","v":77.161768792481084},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ99, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.56164211599843361},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA99, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1729517594759946E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB99, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12643679857943407},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S99, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":417.22407973594875},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P99, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7618376031382867}]
[null,null,null,null,null,null,null,94,0.47,0.16451024672564341,0.55269768251467066,0.38786467972661515,1.7616824682929397,1.7616824682929397,1,1.7616824682929397,2.1515857536704606E-6,0.10190672322750355,417409.93833985453,2.3957263786704608E-6,0,6.6E-4,0.47239064254445318,2.677835029962736E-2,9.973348219014036E-2,0.1270562093990526,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.14299209990703229,6.1340221907468115E-5,6.1340221907468115E-5,0.15080047337661284,1.5622917763409426E-2,1.6759009024345159E-3,42.666666666666664,14.834891315648029,0.26433881604678611,8.7537208700930277E-2,0.35355192565015092,0.3702446500165914,0.44700938929753842,6.0744487812528107E-2,4.5915093217384004E-3,2.4862726033010978E-2,6.6579535843382691E-3,3.6112188939087644E-2,9.7957195775342565E-2,3.3844432885906044E-2,9.1755303357263798E-2,6.2674102241729165E-3,0.56622455937337068,0.69335337359014848,2.3499999999999996,0.77217454285559317,5.4849773645406818E-3,2.0321336119866459E-2,2.108801470524653E-2,0.11617182832537021,8.169516641993238E-3,2.1877030916341114E-3,1.1865920419385027E-2,8.7989618727837005E-3,3.2770917454284294E-2,2.0155471408536101E-5,3.7013762238587081E-6,3.0149408265732536E-2,0.25703244110846912,0.77217454285559317,77.217454285559313,470,73.8844086186851,0.73884408618685105,417.40993833985453,null,2.87634060048917E-2,null,0.56622455937337068,9.1755303357263798E-2,0.1270562093990526,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR100, IF(MODE_ILIM=4,#REF!,#REF!))","v":77.217454285559313},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ100, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.56622455937337068},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA100, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1755303357263798E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB100, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1270562093990526},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S100, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":417.40993833985453},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P100, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7616824682929397}]
[null,null,null,null,null,null,null,95,0.47499999999999998,0.16449575985179229,0.55769770350162207,0.39287192319394426,1.7615273334475918,1.7615273334475918,1,1.7615273334475918,2.1505194120663431E-6,0.10195210226963679,417595.81089643226,2.3946600370663429E-6,0,6.6E-4,0.47736560324719807,2.7345350299627359E-2,9.9777893488502856E-2,0.12768188472649225,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.14452485777440685,6.2662303544137583E-5,6.2662303544137583E-5,0.15242254728075971,1.5960818815734582E-2,1.6766471807491755E-3,42.666666666666664,14.701774115241042,0.26673715598714071,8.7576189001307481E-2,0.35598999216919736,0.37305204324728364,0.45181761203751175,6.2058302982372963E-2,4.5935539198607555E-3,2.5194510982382803E-2,6.735626260219698E-3,3.6523691162463262E-2,9.9726624743928655E-2,3.3844432885906044E-2,9.1781091055541816E-2,6.2702011006099314E-3,0.57082996014736398,0.69858577177321812,2.375,0.77271310331118925,5.5511875525903467E-3,2.0563256819412672E-2,2.0889886939190045E-2,0.11582237119864693,8.1971068495178337E-3,2.1914554401173485E-3,1.1883088312642712E-2,8.8968886278554156E-3,3.2463025566043933E-2,2.0387361276723486E-5,3.6649687544941921E-6,2.9861242818869285E-2,0.25634356245491774,0.77271310331118925,77.271310331118926,475,73.791636151568156,0.73791636151568152,417.59581089643228,null,2.8493165801838964E-2,null,0.57082996014736398,9.1781091055541816E-2,0.12768188472649225,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR101, IF(MODE_ILIM=4,#REF!,#REF!))","v":77.271310331118926},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ101, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.57082996014736398},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA101, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1781091055541816E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB101, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12768188472649225},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S101, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":417.59581089643228},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P101, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7615273334475918}]
[null,null,null,null,null,null,null,96,{"$f":"IF(PLOT_TYPE=1, H102/100*Iout, min_I*EXP(H102*rr/100))","v":0.48},{"$f":"IF(I102<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I102-Vout)/L*OnTime)","v":0.16448127297794118},{"$f":"IF(I102<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I102+((Vin-(Rdcr+RdsonTop)*J102-Vout)/L*OnTime)/2)","v":0.56269772448857347},{"$f":"IF(I102<Icrit, 0, I102-((Vin-(Rdcr+RdsonTop)*K102-Vout)/L*OnTime)/2)","v":0.39787916666127332},1.7613721986022444,{"$f":"IF(I102<Icrit, 1000*SQRT((J102*CoutEsr)^2+(((J102/2)-I102)*(OnTime+OffTime)/Cout)^2), 1000*J102*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":1.7613721986022444},1,{"$f":"IF(I102<Icrit, 1000*((N102/1000)*O102), 1000*J102*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":1.7613721986022444},2.1494539393525921E-6,0.10199748471856759,417781.69740725285,2.3935945643525923E-6,0,{"$f":"S102*(T102*Iq_active+U102*Iq_sleep)","v":6.5999999999999989E-4},0.48234108177052609,{"$f":"W102^2*Rdcr","v":2.7918350299627359E-2},{"$f":"Core_Loss/1000*S102/$S$106","v":9.9822308121010284E-2},{"$f":"(Y102+X102*(1+Ltc*(Ta-25)))/(1-X102*Ltc*ThetaCa)","v":0.12831382808475866},4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.14605837595944166,6.3999147563728809E-5,6.3999147563728809E-5,0.15404548862954567,1.6302518633608338E-2,1.6773935150901204E-3,{"$f":"20*VIN_nom/24","v":42.666666666666664},14.571024656544676,{"$f":"IF(I102<Icrit, Vin*(I102+Iripple/2)*AK102/1000000000/2*S102, Vin*(I102-Iripple/2)*AJ102/1000000000/2*S102 + Vin*(I102+Iripple/2)*AK102/1000000000/2*S102)","v":0.26913753514088223},8.7615172228101529E-2,0.3584301008840739,{"$f":"(AI102+AL102+AM102+AH102*(1+RdsonTopTc*(Ta-25)))/(1-AH102*RdsonTopTc*ThetaJA)","v":0.37586591193073354},0.45662840609499944,6.3386888380869352E-2,4.5955986714797826E-3,{"$f":"IF(I102<Icrit, Vin*Idss*R102, QrrBot*(I102-Iripple/2)/1*S102*Vin+Vin*Idss*R102)","v":2.552658228460979E-2},6.8134492252132153E-3,3.6935630181302789E-2,{"$f":"(AR102+AS102+AT102+AQ102*(1+RdsonBotTc*(Ta-25)))/(1-AQ102*RdsonBotTc*ThetaJA)","v":0.10151259178892671},{"$f":"Vin*V102+Vout*Ifb/0.8","v":3.3844432885906037E-2},{"$f":"(Vin-Vdd)*(S102*QgBot+S102*QgTop)+AW102","v":9.1806880689811937E-2},6.2729921865699034E-3,0.57545837659604215,{"$f":"SUM(Z102,AC102,AF102,AZ102)","v":0.70384746842418233},2.4,0.77323387325424076,5.6174832120573807E-3,2.0805455894522269E-2,2.0695424193344147E-2,0.1154792896656253,8.2241742045299632E-3,2.1951623894303001E-3,1.1899950160906246E-2,8.9947558904373143E-3,3.2160829143994596E-2,2.0619295314863221E-5,3.6292362728526015E-6,2.9578412477988852E-2,0.25567518576442405,0.77323387325424076,77.323387325424079,480,73.551124384272143,0.73551124384272137,417.78169740725286,null,2.8227924574071805E-2,null,0.57545837659604215,9.1806880689811937E-2,0.12831382808475866,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR102, IF(MODE_ILIM=4,#REF!,#REF!))","v":77.323387325424079},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ102, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.57545837659604215},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA102, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1806880689811937E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB102, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12831382808475866},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S102, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":417.78169740725286},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P102, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7613721986022444}]
[null,null,null,null,null,null,null,97,{"$f":"IF(PLOT_TYPE=1, H103/100*Iout, min_I*EXP(H103*rr/100))","v":0.48499999999999999},0.16446678610409007,0.56769774547552487,0.40288641012860238,1.7612170637568967,1.7612170637568967,1,1.7612170637568967,2.1483893344676402E-6,0.10204287057467966,417967.59787388786,{"$f":"IF(1/S103-OnTime-Q103>Tsleep, OnTime+Q103+Tsleep, 1/S103)","v":2.3925299594676404E-6},0,6.6E-4,0.48731706225368443,2.8497350299627359E-2,9.9866726088038135E-2,0.12895204303441821,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.14759264905179131,6.5350770162375703E-5,6.5350770162375703E-5,0.15566929231403195,{"$f":"RdsonTop*AG103^2","v":1.66480219272819E-2},1.6781399054636599E-3,42.666666666666664,14.442580324263806,0.27153995373765799,8.7654158381641978E-2,0.36087225202476364,0.37868626853407183,0.46144175632586065,{"$f":"RdsonBot*AP103^2","v":6.4730262322252874E-2},4.5976435766127673E-3,2.5858939971939762E-2,6.8914225983742541E-3,3.7348006146926779E-2,0.1033151431066677,3.3844432885906044E-2,9.1832672260292236E-2,6.2757834820764274E-3,0.58010986738310821,0.70913852578350656,2.4249999999999998,0.77373733804372014,5.6838637994964976E-3,2.1047932762719775E-2,2.0504525351315535E-2,0.11514240645586933,8.2507329395962985E-3,2.1988251449898692E-3,1.1916514167985E-2,9.0925624586115812E-3,3.1864171052577307E-2,2.0851270492595279E-5,3.59416015761164E-6,2.9300770053657693E-2,0.25502674961746907,0.77373733804372014,77.373733804372009,485,73.159788011658193,0.73159788011658189,417.96759787388788,null,2.7967544401927551E-2,null,0.58010986738310821,9.1832672260292236E-2,0.12895204303441821,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR103, IF(MODE_ILIM=4,#REF!,#REF!))","v":77.373733804372009},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ103, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.58010986738310821},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA103, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1832672260292236E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB103, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12895204303441821},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S103, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":417.96759787388788},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P103, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7612170637568967}]
[null,null,null,null,null,null,null,98,{"$f":"IF(PLOT_TYPE=1, H104/100*Iout, min_I*EXP(H104*rr/100))","v":0.49},0.16445229923023899,0.57269776646247628,0.40789365359593149,1.7610619289115497,1.7610619289115497,1,1.7610619289115497,2.1473255963516464E-6,0.10208825983835672,418153.51229790912,{"$f":"IF(1/S104-OnTime-Q104>Tsleep, OnTime+Q104+Tsleep, 1/S104)","v":2.3914662213516466E-6},0,6.600000000000001E-4,0.49229352947561816,2.9082350299627358E-2,9.9911147389962013E-2,0.12959653317364911,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.14912767185078868,6.6717187534909536E-5,6.6717187534909536E-5,0.15729395342527924,{"$f":"RdsonTop*AG104^2","v":1.6997333407713741E-2},1.6788863518761052E-3,42.666666666666664,14.316380691639452,0.27394441200714981,8.7693147462258481E-2,0.36331644582128442,0.38151312556572042,0.46625764817880183,{"$f":"RdsonBot*AP104^2","v":6.6088443123509116E-2},4.5996886352770005E-3,2.6191584076625352E-2,6.9695464987761246E-3,3.7760819210678476E-2,0.10513432524270816,3.3844432885906051E-2,9.1858465767200748E-2,6.2785749871531061E-3,0.58478449156278245,0.71445900651978422,2.4500000000000002,0.7742239652819729,5.7503287945728171E-3,2.1290686936762015E-2,2.0317092980501484E-2,0.11481155074935015,8.2767967676820649E-3,2.2024448679589968E-3,1.1932788237382525E-2,9.1903071708966787E-3,3.1572899880868581E-2,2.1083283871730069E-5,3.5597224658616647E-6,2.9028173718775724E-2,0.25439771311108861,0.7742239652819729,77.422396528197297,490,72.614496083320674,0.72614496083320679,418.15351229790912,null,2.7711892390321034E-2,null,0.58478449156278245,9.1858465767200748E-2,0.12959653317364911,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR104, IF(MODE_ILIM=4,#REF!,#REF!))","v":77.422396528197297},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ104, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.58478449156278245},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA104, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1858465767200748E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB104, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12959653317364911},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S104, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":418.15351229790912},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P104, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7610619289115497}]
[null,null,null,null,null,null,null,99,{"$f":"IF(PLOT_TYPE=1, H105/100*Iout, min_I*EXP(H105*rr/100))","v":0.495},0.16443781235638791,0.57769778744942768,0.41290089706326061,1.7609067940662022,1.7609067940662022,1,1.7609067940662022,2.1462627239464971E-6,0.10213365250998249,418339.44068088831,{"$f":"IF(1/S105-OnTime-Q105>Tsleep, OnTime+Q105+Tsleep, 1/S105)","v":2.3904033489464974E-6},0,6.6E-4,0.49727046882311576,2.9673350299627359E-2,9.9955572027157394E-2,0.13024730213829372,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.15066343935502743,6.8098415874858094E-5,6.8098415874858094E-5,0.15891946724439621,{"$f":"RdsonTop*AG105^2","v":1.735045778656975E-2},1.6796328543337664E-3,42.666666666666664,14.192367425659615,0.27635091017907376,8.7732139470280635E-2,0.36576268250368815,0.38434649557555201,0.47107606766587806,{"$f":"RdsonBot*AP105^2","v":6.7461449104374266E-2},4.6017338474897713E-3,2.6524514630924034E-2,7.0478210455100125E-3,3.8174069523923819E-2,0.10697018509413472,3.3844432885906044E-2,9.1884261210755547E-2,6.2813667018235377E-3,0.5894823085822658,0.71980897373225217,2.4750000000000001,0.77469420561588254,5.8168776989986348E-3,2.1533718020655748E-2,2.0133033165839486E-2,0.11448655788530462,8.3023789055961805E-3,2.2060226772421324E-3,1.1948779985843084E-2,9.2879889043764145E-3,3.1286869684226191E-2,2.1315332601968968E-5,3.5259059024888087E-6,2.8760486766573137E-2,0.25378755493316008,0.77469420561588254,77.469420561588251,495,71.912167665597565,0.71912167665597559,418.33944068088829,null,2.7460840441984189E-2,null,0.5894823085822658,9.1884261210755547E-2,0.13024730213829372,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR105, IF(MODE_ILIM=4,#REF!,#REF!))","v":77.469420561588251},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ105, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.5894823085822658},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA105, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1884261210755547E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB105, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13024730213829372},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S105, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":418.33944068088829},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P105, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7609067940662022}]
[null,null,null,null,null,null,null,100,{"$f":"IF(PLOT_TYPE=1, H106/100*Iout, min_I*EXP(H106*rr/100))","v":0.5},0.16442332548253677,0.58269780843637908,0.41790814053058967,1.7607516592208545,1.7607516592208545,1,1.7607516592208545,2.1452007161957983E-6,0.10217904858994088,418525.38302439783,{"$f":"IF(1/S106-OnTime-Q106>Tsleep, OnTime+Q106+Tsleep, 1/S106)","v":2.3893413411957985E-6},0,6.6E-4,0.50224786626083473,3.0270350299627363E-2,0.10000000000000002,0.13090435360191158,4.7464925614198031E-2,1.1264595817806762E-5,1.1264595817806762E-5,0.15219994675255832,6.9494471374444776E-5,6.9494471374444776E-5,0.16054582923317556,{"$f":"RdsonTop*AG106^2","v":1.7707399776223397E-2},1.6803794128429574E-3,42.666666666666664,14.070484197154395,0.27875944848318063,8.7771134406038204E-2,0.36821096230206174,0.38718639115505205,0.47589700133473567,{"$f":"RdsonBot*AP106^2","v":6.8849298587335586E-2},4.6037792132683766E-3,2.6857731667098157E-2,7.1262463576849937E-3,3.858775723805153E-2,0.10882276991188963,3.3844432885906044E-2,9.1910058591174765E-2,6.2841586261113344E-3,0.59420337828422776,0.7251884909533316,2.5,0.7751484934950349,5.883510035527062E-3,2.1777025705892118E-2,1.9952255352479867E-2,0.11416726908672011,8.3274920961780123E-3,2.2095596513736012E-3,1.196449675617111E-2,9.3856065729292521E-3,3.1005939739801404E-2,2.1547413916853878E-5,3.4926937912013529E-6,2.8497577381595803E-2,{"$f":"SUM(BD106:BO106)","v":0.25319577248637637},0.7751484934950349,77.514849349503493,500,71.049894896969974,0.71049894896969978,418.52538302439785,null,2.7214265042876298E-2,null,0.59420337828422776,9.1910058591174765E-2,0.13090435360191158,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR106, IF(MODE_ILIM=4,#REF!,#REF!))","v":77.514849349503493},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ106, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.59420337828422776},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA106, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1910058591174765E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB106, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13090435360191158},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S106, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":418.52538302439785},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P106, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7607516592208545}]
[null,null,null,null,null,null,null,null,{"$f":"Losses!$E$5/1000","v":0.5},0.16442332548253677,0.58269780843637908,0.41790814053058967,1.7607516592208545,1.7607516592208545,1,1.7607516592208545,{"$f":"IF(I107<Icrit, L*J107/(Vout+J107/2*(RdsonBot+Rdcr)), L*J107/(Vout+I107*(RdsonBot+Rdcr)))","v":2.1452007161957983E-6},{"$f":"OnTime*S107","v":0.10217904858994088},{"$f":"IF(I107<Icrit,I107/((OnTime+Q107)*J107/2),1/(OnTime+Q107))","v":418525.38302439783},{"$f":"IF(1/S107-OnTime-Q107>Tsleep, OnTime+Q107+Tsleep, 1/S107)","v":2.3893413411957985E-6},{"$f":"IF(1/S107-OnTime-Q107>Tsleep, 1/S107-OnTime-Q107-Tsleep, 0)","v":0},6.6E-4,{"$f":"IF(I107<Icrit,Iripple*SQRT((OnTime+OffTime)*S107/3), SQRT(I107^2+Iripple^2/12))","v":0.50224786626083473},3.0270350299627363E-2,0.10000000000000002,0.13090435360191158,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q107)*S107)","v":4.7464925614198031E-2},{"$f":"RCoutEsr*AA107^2","v":1.1264595817806762E-5},{"$f":"AB107","v":1.1264595817806762E-5},{"$f":"SQRT($R107)*SQRT($I107^2*(1-R107)+(Iripple^2)/12)","v":0.15219994675255832},{"$f":"RCinEsr*AD107^2","v":6.9494471374444776E-5},{"$f":"AE107","v":6.9494471374444776E-5},{"$f":"IF(I107<Icrit,Iripple*SQRT((OnTime)*S107/3), SQRT(OnTime*S107*(I107^2+Iripple^2/12)))","v":0.16054582923317556},{"$f":"RdsonTop*AG107^2","v":1.7707399776223397E-2},{"$f":"QgTop*S107*Vdd","v":1.6803794128429574E-3},42.666666666666664,{"$f":"IF(I107<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I107+Iripple/2)*1000000000)","v":14.070484197154395},0.27875944848318063,{"$f":"IF(I107<Icrit, Csw*(Vin)^2*S107/2, Csw*Vin^2*S107/2)","v":8.7771134406038204E-2},0.36821096230206174,0.38718639115505205,{"$f":"IF(I107<Icrit,Iripple*SQRT((OffTime)*S107/3), SQRT(OffTime*S107*(I107^2+Iripple^2/12)))","v":0.47589700133473567},{"$f":"RdsonBot*AP107^2","v":6.8849298587335586E-2},{"$f":"QgBot*S107*Vdd","v":4.6037792132683766E-3},2.6857731667098157E-2,{"$f":"IF(I107<Icrit, dead1*S107*(I107+Iripple/2)*((I107+Iripple/2)*BDserR+VSD), dead1*S107*(I107+Iripple/2)*((I107+Iripple/2)*BDserR+VSD)+dead2*S107*(I107-Iripple/2)*((I107-Iripple/2)*BDserR+VSD))","v":7.1262463576849937E-3},3.858775723805153E-2,0.10882276991188963,3.3844432885906044E-2,9.1910058591174765E-2,{"$f":"AI107+AR107","v":6.2841586261113344E-3},{"$f":"AO107+AV107+AX107+AY107","v":0.59420337828422776},0.7251884909533316,{"$f":"Vout*I107","v":2.5},{"$f":"BB107/(BB107+BA107)","v":0.7751484934950349},5.883510035527062E-3,2.1777025705892118E-2,{"$f":"Vin*S107*(QgBot+QgTop)/($BB107+$BA107)","v":1.9952255352479867E-2},0.11416726908672011,{"$f":"AS107/(BA107+BB107)","v":8.3274920961780123E-3},{"$f":"AT107/($BB107+$BA107)","v":2.2095596513736012E-3},1.196449675617111E-2,{"$f":"X107/($BB107+$BA107)","v":9.3856065729292521E-3},{"$f":"Y107/($BB107+$BA107)","v":3.1005939739801404E-2},{"$f":"(AF107)/($BB107+$BA107)","v":2.1547413916853878E-5},{"$f":"(AC107)/($BB107+$BA107)","v":3.4926937912013529E-6},2.8497577381595803E-2,{"$f":"SUM(BD107:BO107)","v":0.25319577248637637},{"$f":"BC107","v":0.7751484934950349},{"$f":"100*BQ107","v":77.514849349503493},{"$f":"I107*1000","v":500},72.049894896970002,{"$f":"BT107/100","v":0.72049894896970001},{"$f":"S107/1000","v":418.52538302439785},null,{"$f":"AM107/($BB107+$BA107)","v":2.7214265042876298E-2},null,0.59420337828422776,9.1910058591174765E-2,0.13090435360191158,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR107, IF(MODE_ILIM=4,#REF!,#REF!))","v":77.514849349503493},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ107, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.59420337828422776},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA107, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1910058591174765E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB107, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13090435360191158},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S107, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":418.52538302439785},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P107, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7607516592208545}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BD107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":5.883510035527062E-3},{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BE107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":2.1777025705892118E-2},null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BG107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":0.11416726908672011},null,null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BJ107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":1.196449675617111E-2},{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BK107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":9.3856065729292521E-3},{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BL107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":3.1005939739801404E-2},null,null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BO107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":2.8497577381595803E-2}]
[null,null,null,null,null,null,null,1.0000000000000001E-5,"A","min_I",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Load (A)","High-side MOSFET Rdson %","Low-side MOSFET Rdson %","Gate Drive (Qg) Loss from Vin %","High-side MOSFET Switching Loss %","Reverse Recovery & Leakage Loss %","Deadtime Loss %",null,"Inductor Cu Loss %","Inductor Core Loss %","Cin ESR %","Cout ESR %","Quiescent Current Loss %","Total Loss %","Overall Eff %"]
[null,null,null,null,null,null,null,{"$f":"Iout","v":0.5},"A","max_I",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"I107","v":0.5},{"$f":"BD107","v":5.883510035527062E-3},{"$f":"BE107","v":2.1777025705892118E-2},1.9952255352479867E-2,0.11416726908672011,8.3274920961780123E-3,2.2095596513736012E-3,null,9.3856065729292521E-3,3.1005939739801404E-2,2.1547413916853878E-5,3.4926937912013529E-6,2.8497577381595803E-2,0.25319577248637637,0.7751484934950349]
[null,null,null,null,null,null,null,{"$f":"LOG(max_I/min_I,EXP(1))","v":10.819778284410283},null,"rr",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10mA",{"$f":"BD70","v":3.542489035781202E-3},{"$f":"BE70","v":1.3201573191670146E-2},2.9455982919901858E-2,0.13088182707713755,6.9972919089361253E-3,2.045420589076342E-3,null,5.8418720150251978E-3,4.5774796646113544E-2,1.323985586928614E-5,5.2400455074555316E-6,4.2323117766319709E-2,0.29123293412226053,0.74428527641227404]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"50ma",{"$f":"BD85","v":4.50253645008935E-3},{"$f":"BE85","v":1.672667485085514E-2},2.4582124173041654E-2,0.12232316973917171,7.6813204259474251E-3,2.1249865480041288E-3,null,7.3238890269530805E-3,3.8200787195263722E-2,1.6684827161284337E-5,4.3436596704434557E-6,3.5232034141092237E-2,0.27028353791140214,0.76156552688422341]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"100mA",{"$f":"BD91","v":4.8930345594707927E-3},{"$f":"BE91","v":1.8156725850766914E-2},2.3054843102605159E-2,0.11963671565026997,7.8950362966063517E-3,2.1516652534387969E-3,null,7.9151650030949011E-3,3.5827382083955951E-2,1.8071002178714539E-5,4.0628713314559061E-6,3.3010274176099634E-2,0.26425909096890315,0.76643687168038832]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"500mA",{"$f":"BD106","v":5.883510035527062E-3},{"$f":"BE106","v":2.1777025705892118E-2},1.9952255352479867E-2,0.11416726908672011,8.3274920961780123E-3,2.2095596513736012E-3,null,9.3856065729292521E-3,3.1005939739801404E-2,2.1547413916853878E-5,3.4926937912013529E-6,2.8497577381595803E-2,0.25319577248637637,0.7751484934950349]

{"sheet":"Schematic Mgmt","index":10,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
[]
[{"$f":"'Variable Mgmt'!K27","v":"SCH_COT3_LM5163"}]

{"sheet":"Efficiency Plots","index":11,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
[]
[{"$f":"IF(PLOT_TYPE=1, \"EFF_LINEAR\", \"EFF_LOG\")","v":"EFF_LINEAR"}]