{"text_format":"1","workbook":"xlsx","n_sheets":12,"sheets":["Instructions","Design Converter","BOM & Schematic","Fsw & Ripple","Losses","EVM","Design EMI Filter","Variable Mgmt","Standard Value Calculator","Efficiency","Schematic Mgmt","Efficiency Plots"],"not_rendered":{"charts":6,"images":26,"macros":1,"external_links":0,"defined_names":205,"comments":4,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Instructions","index":0,"n_rows":74,"n_cols":3,"rows_kept":74,"cut":false,"hidden":true,"merged":[[0,0,0,16],[7,1,9,15],[16,2,17,15],[11,1,14,15],[18,2,19,15],[65,1,66,15],[69,1,70,15],[73,1,74,15],[77,1,78,15],[20,2,21,15],[50,1,52,15],[54,1,55,15],[56,1,57,15],[60,1,62,15],[24,1,26,15],[38,1,39,15],[41,1,43,15],[46,1,47,15],[28,1,28,15],[29,1,31,15],[33,1,35,15]]}
["                         LM5164 Low IQ DC/DC Converter Design Tool  "]
[]
[]
[null,"Design Regulator tab"]
[null,"Start with Step 1, and then work down towards the bottom of the worksheet."]
[]
[null,"Step 1. Operating Specifications"]
[null,"First, enter the values in the yellow shaded cells to define the power supply parameters.  If a particular specification is not known, enter an estimate. It can be changed later, if necessary, to optimize component values.  Cells  with a red mark in the upper right corner have a comment to provide additional information.  Hold the cursor over the cell to read the comment.  A red font indicates an erroneous entry and requires an adjustment to the entry.  Consult the entry's comments for the entry specific requirements."]
[]
[]
[]
[null,"Second, select a desired mode of operation. PFM mode requires the fewest external components and the lowest inductance.  As a result, it can provide the smallest solution size. At light loads, a PFM converter has a relatively longer sleep time interval and thus operates at lower input quiescent current levels.  COT mode offers nearly constant switching frequency, relatively higher conversion efficiencies at medium to heavy loads, and enables the lowest output voltage ripple.  Options COT1, COT2, and COT3 enable you to select a ripple generation method (a requirement for the stable operation in COT mode):"]
[]
[]
[]
[]
[null,"-COT1: ","Type 1 ripple generation method requires a single resistor in series with the output capacitor.  It is the simplest, the most compact, and the most economical method that works with fixed and adjustable device options, however, the output voltage ripple is the highest."]
[]
[null,"-COT2: ","Type 2 ripple generation method requires a feedforward capacitor in addition to the series resistor.  The feedforward capacitor reduces the required minimum value of the series resistor and ultimately the output voltage ripple by the VOUT / 1.223V factor.  It only works with an adjustable device option (i.e. external feedback resistor network)."]
[]
[null,"-COT3:","Type 3 ripple generation method three external components to generate and inject required voltage ripple into the FB node.  In return, it provides the lowest output voltage ripple. It also only works with an adjustable device option (i.e. external feedback resistor network)."]
[]
[]
[null,"Step 2. Filter Inductor"]
[null,"First, select an inductor current limit level.  In PFM Mode, 1.25A, 0.75A, 0.5A, and 1.25A - MOD options are available.  For the 500mA max load, select either 1.25A or 1.25A - MOD option.  The 1.25A - MOD option enables higher efficiency at the expense of slightly worse transient operation.  For the 300mA and 200mA max loads, select 0.75A and 0.5A options respectively. In COT Mode, 0.75A and 0.5A options are available.   For the 500mA and 300mA max loads, select 0.75A and 0.5A options respectively."]
[]
[]
[]
[null,"Second, select the filter inductance value based on the suggested value. Enter the inductor RDC for accurate efficiency estimates."]
[null,"In PFM mode, selected inductance defines the switching frequency.  You may select lower or higher inductance to increase or decrease the switching frequency.  Watch the minimum output capacitance.  At very low switching frequencies, the required minimum capacitance may become excessive."]
[]
[]
[]
[null,"In COT mode, the suggested inductance is  derived based on the target inductor (peak-to-peak) ripple current of 40% of the DC full load output current at nominal input voltage. It may be acceptable to use higher ripple current with the proviso that peak inductor current remains below the ILIM setting.  Pk-to-Pk Ripple Current value will turn red if this is violated.  If this happens, increase the selected inductance or decrease the Input Voltage (max) or both."]
[]
[]
[]
[null,"Step 3. Output Capacitors and Ripple Generation"]
[null,"First, select the output capacitance based on the minimum recommended value.  Make sure that the nominal capacitance is appropriately derated for applied voltage, especially with ceramics.  For PFM and COT3 modes, ensure that the capacitor ESR does not exceed the maximum allowable value.  "]
[]
[]
[null,"Second, for COT modes, select the values for the ripple generation components based on the minimum recommended values.  Ensure that the output voltage ripple meets any of your minimum ripple requirements by reviewing the VOUT Ripple vs. IOUT plot in the fSW&Ripple tab.  For accurate output voltage ripple estimates in COT3 mode, ensure that the Output Capacitor ESR is set to the levels of a typical ceramic capacitor ESR (e.g. 10 mW)."]
[]
[]
[]
[null,"Step 4. Input Capacitors"]
[null,"Select the input capacitance based on the minimum recommended value.  Make sure that the nominal capacitance is appropriately derated for applied voltage, especially with ceramics.  "]
[]
[]
[null,"Step 5. Feedback, Soft-Start, UVLO"]
[null,"First, review the feedback resistor network. With an adjustable device option, an external feedback resistor network is required. The resistor values are automatically calculated based on the selected VOUT in Step 1.  For lowering the leakage current through the resistors, adjust the upper FB resistor (R1) until the lower FB resistor (R2) reaches its upper end of the range (100kW).  Keeping the upper FB resistor below 1MW is recommended."]
[]
[]
[]
[null,"Second, select one out of three soft-start configurations.  If the external soft-start option is selected, enter a desired soft start time.  "]
[]
[null,"Third, select one out of the two UVLO options.  If the external UVLO option is selected, define desired UVLO thresholds and hysteresis.  Keeping the upper UVLO resistor at 1MW or higher is recommended for the minimum leakage current."]
[]
[]
[null,"Step 6. Efficiency and Thermals"]
[null,"Enter the LM5166's junction-to-ambient thermal impedance (dependent on your PCB design, air flow, etc.) and ambient temperature. Device power dissipation and junction temperature are derived at the maximum load.  Ensure that the junction temperature is within the recommended range."]
[]
[]
[]
[null,"BOM & Schematic tab"]
[null,"This tab summarizes the converter schematic and BOM.  It also helps you estimate the total solution size. Select a package size for each external component (i.e. inductor, capacitors, and resistors) for accurate solution size estimates."]
[]
[]
[null,"Design EMI Filter tab"]
[null,"In case an EMI filter is needed, a simple EMI filter design aid is given in this tab.  It is based on the guidelines documented in TI's literature number SNVA489C (aka AN-2162).  Suggest reviewing the note before using the design aid."]
[]
[]
[null,"fSW & Ripple tab"]
[null,"In this tab, the switching/burst frequency (COT/PFM mode) and the output voltage ripple as a function of the load current are plotted."]

{"sheet":"Design Converter","index":1,"n_rows":58,"n_cols":17,"rows_kept":58,"cut":false,"hidden":false,"merged":[[2,14,2,15],[0,0,0,16]]}
["                          LM5163/4 Low IQ DC/DC Converter Design Tool  "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"http://www.ti.com/ww/en/analog/power_management/widevin"]
["About",null,"xx",null,null,"= Input Box",null,null,null,null,null,null,null,null,"Terms Of Use",null,"                "]
[]
["Step 1: Operating Specifications"]
[null,null,null,"Input Voltage - Min, VIN(min) ",47,"V"]
[null,null,null,"Input Voltage - Nom, VIN(nom)",65,"V"]
[null,null,null,"Input Voltage - Max, VIN(max)",71,"V"]
[null,null,null,"Output Voltage, VOUT ",12,"V"]
[null,null,null,"Full Load Current, IOUT",0.5,"A"]
[null,null,null,"Mode of Operation",null,null,{"$f":"MODE","v":3}]
[null,null,null,"Switching Frequency at VIN(nom)",150,"kHz"]
[null,null,null,"Timing Resistance, RT",{"$f":"'Standard Value Calculator'!J4/1000","v":200},"kΩ"]
[]
["Step 2: Buck Inductor"]
[null,null,null,"Recommended Buck Inductance ",{"$f":"Lopt*1000000","v":326.15384615384619},"µH"]
[null,null,null,"Inductance, LF ",68,"µH"]
[null,null,null,"Inductor DCR ",120,"mΩ"]
[null,null,null,{"$f":"CHOOSE(MODE, \"Pk-to-Pk Ripple Current\",\"Pk-to-Pk Ripple Current\",\"Pk-to-Pk Ripple Current\", \"Resulting PFM Switching Frequency\")","v":"Pk-to-Pk Ripple Current"},{"$f":"Iripple_Vinnom*1000","v":967.89089686361763},"mApk-pk"]
[null,null,null,{"$f":"CHOOSE(MODE, 'Variable Mgmt'!H88,'Variable Mgmt'!H88,'Variable Mgmt'!H88, 'Variable Mgmt'!H89)","v":"% Ripple Current at Nom VIN"},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), 'Variable Mgmt'!B96*100, Ilim/2*1000)","v":193.57817937272353},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), \"%\", \"mA\")","v":"%"}]
[]
[{"$f":"IF(MODE=4, \"Step 3: Output Capacitors\", \"Step 3: Output Capacitors, Ripple Generation\")","v":"Step 3: Output Capacitors, Ripple Generation"}]
[null,null,null,"Minimum Output Capacitance ",{"$f":"'Variable Mgmt'!B116","v":13.442929123105801},"µF"]
[null,null,null,"Output Capacitance, COUT ",44,"µF"]
[null,null,null,{"$f":"IF(OR(MODE=1,MODE=2),\"Recommended Series Resistance\",IF(MODE=3,\"Maximum Allowable ESR\",\"*Higher Cout Improves Light-Load Eff\"))","v":"Maximum Allowable ESR"},{"$f":"'Variable Mgmt'!B272","v":5.8999999999999997E-2},"Ω"]
[null,null,null,{"$f":"IF(OR(MODE=1,MODE=2),\"Total ESR & Series Resistance, Rser\",IF(MODE=3,\"Output Capacitor ESR\",\"*PFM Hysteresis Sets Output Ripple\"))","v":"Output Capacitor ESR"},5.0000000000000001E-3,"Ω"]
[null,null,null,{"$f":"CHOOSE(MODE, \"Resulting Output Voltage Ripple\",\"Resulting Output Voltage Ripple\", \"Output Voltage Ripple\",\"Output Voltage Ripple\")","v":"Output Voltage Ripple"},{"$f":"CHOOSE(MODE, Vripple2*1000,Vripple2*1000,Vripple2*1000, PFM_Ripple)","v":18.959316153800394},"mVpk-pk"]
[null,null,null,{"$f":"IF(MODE=1,\"\",IF(MODE=2,\"Minimum Feedforward Capacitance\", IF(MODE=3,\"Minimum Coupling Capacitance\",\"\")))","v":"Minimum Coupling Capacitance"},{"$f":"'Variable Mgmt'!B140","v":">47"},"pF"]
[null,null,null,{"$f":"IF(MODE=1,\"\",IF(MODE=2,\"Feedforward Capacitance, Cff\", IF(MODE=3,\"Coupling Capacitance, Cb\",\"\")))","v":"Coupling Capacitance, Cb"},56,"pF",null,null,null,null,null,"** Specify Inductor Core Loss **",100,"mW"]
[null,null,null,{"$f":"IF(MODE=3,\"Minimum Ripple Generation Capacitance\",\"\")","v":"Minimum Ripple Generation Capacitance"},{"$f":"'Variable Mgmt'!B144","v":">1483"},"pF"]
[null,null,null,{"$f":"IF(MODE=3,\"Ripple Generation Capacitance, Ca\",\"\")","v":"Ripple Generation Capacitance, Ca"},3300,"pF"]
[null,null,null,{"$f":"IF(MODE=3,\"Ripple Generation Resistance, Ra\",\"\")","v":"Ripple Generation Resistance, Ra"},{"$f":"Ra","v":1000},"kΩ"]
[null,null,null,{"$f":"IF(MODE=3,\"Amplitude of Injected Ripple\",\"\")","v":"Amplitude of Injected Ripple"},20,"mVpk-pk"]
[]
["Step 4: Input Capacitors"]
[null,null,null,"Minimum Input Capacitance ",{"$f":"'Variable Mgmt'!B157","v":2.2000000000000002},"µF"]
[null,null,null,"Input Capacitance, CIN ",10,"µF"]
[null,null,null,"Maximum Allowable ESR",{"$f":"'Variable Mgmt'!B159","v":3.2513975018467276},"Ω"]
[null,null,null,"Input Capacitor ESR ",3,"mΩ"]
[null,null,null,"Resulting Input Voltage Ripple ",{"$f":"CHOOSE(MODE, Vinripple2*1000,Vinripple2*1000,Vinripple2*1000, 'Variable Mgmt'!B165*1000)","v":53.754063360654001},"mVpk-pk"]
[]
["Step 5: Feedback, PGOOD, UVLO"]
[null,null,null,"Upper Feedback Resistor, RFB1 ",453,"kΩ"]
[null,null,null,"Lower Feedback Resistor, RFB2",{"$f":"IF(Vout=Vref,\"OPEN\",Rfb2_u/1000)","v":49.9},{"$f":"IF(Vout=Vref,\"\",\"kΩ\")","v":"kΩ"}]
[null,null,null,"Acutal Output Voltage Setpoint",{"$f":"'Variable Mgmt'!B201","v":12.0937875751503},"V"]
[null,null,null,"PGOOD Pull-up Resistance",20,{"$f":"\"kΩ\"","v":"kΩ"},null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,"BST Capacitance, CBST ",2.2000000000000002,"nF"]
[null,null,null,{"$f":"\"Required Input Voltage UVLO Turn-on\"","v":"Required Input Voltage UVLO Turn-on"},20,"V"]
[null,null,null,"Upper UVLO Resistor, RUV1",1,"MΩ"]
[null,null,null,"Lower UVLO Resistor, RUV2",{"$f":"'Variable Mgmt'!F276","v":80.600000000000009},{"$f":"'Variable Mgmt'!G276","v":"kΩ"}]
[null,null,null,"Actual UVLO Turn-on Threshold",{"$f":"'Variable Mgmt'!B186","v":20.110421836228284},"V"]
[null,null,null,"Actual UVLO Turn-off Threshold",{"$f":"'Variable Mgmt'!B187","v":18.769727047146397},"V"]
[]
["Step 6: Efficiency & Thermals"]
[null,null,null,"Estimated Thermal Impedance, JJA",41,"°C/W"]
[null,null,null,"Ambient Temp, TA",25,"°C"]
[null,null,null,"IC Power Dissipation at Full Load, PD",{"$f":"'Variable Mgmt'!B26","v":0.31380731880512902},"W"]
[null,null,null,"IC Junction Temp at Full Load, TJ",{"$f":"E56+E55*'Variable Mgmt'!B26","v":37.866100071010294},"°C"]

{"sheet":"BOM & Schematic","index":2,"n_rows":53,"n_cols":13,"rows_kept":53,"cut":false,"hidden":false,"merged":[[33,3,33,5],[0,0,0,16],[29,3,29,5],[41,3,41,5],[47,7,47,9],[30,3,30,5],[43,3,43,5],[44,3,44,5],[42,3,42,5],[39,3,39,5],[40,3,40,5],[38,3,38,5],[37,3,37,5],[36,3,36,5],[31,3,31,5],[34,3,34,5],[32,3,32,5]]}
["                         LM5163/4 100V Low IQ DC/DC Converter Design Tool  "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[{"$f":"\"VIN = \"&Vin&\" V, VOUT = \"&Vout&\" V, IOUT = \"&Iout&\" A \"&'Variable Mgmt'!B35&\" Converter\"","v":"VIN = 65 V, VOUT = 12 V, IOUT = 0.5 A COT Converter"}]
["Low IQ, High Efficiency, Synchronous Buck Converter BOM"]
["Count","Ref Des","Value","Description",null,null,"Size","Part Number","MFR","Footprint (mm)","Area (mm2)"]
[{"$f":"ROUNDUP('Design Converter'!E37/10,0)","v":1},"CIN",{"$f":"Cin*1000000","v":10},{"$f":"IF(VIN_max>35, \"Capacitor, Ceramic, \"&'Variable Mgmt'!B257&\", 100V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B257&\", 50V, X7R, 10%\")","v":"Capacitor, Ceramic, 10µF, 100V, X7R, 10%"},null,null,5,"Std","Std",{"$f":"CHOOSE(G31,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)","v":"3.2 x 2.5"},{"$f":"CHOOSE(G31,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45)","v":8}]
[{"$f":"'Variable Mgmt'!D252","v":2},"COUT",{"$f":"'Variable Mgmt'!F253","v":"22µF"},{"$f":"CHOOSE(Cout_Voltage_Rating, \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 6.3V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 10V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 16V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 25V, X7R, 10%\",  \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 50V, X7R, 10%\")","v":"Capacitor, Ceramic, 22µF, 16V, X7R, 10%"},null,null,5,"Std","Std",{"$f":"CHOOSE(G32,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)","v":"3.2 x 2.5"},{"$f":"(CHOOSE(G32,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45))*A32","v":16}]
[{"$f":"CHOOSE(MODE, \"-\", \"-\", \"1\",\"-\")","v":"1"},{"$f":"CHOOSE(MODE,\"-\",\"-\",\"Ca\",\"-\")","v":"Ca"},{"$f":"CHOOSE(MODE, \"-\",\"-\",'Variable Mgmt'!B293, \"-\")","v":"3300pF"},{"$f":"CHOOSE(MODE,\"-\",\"-\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B293&\", 16V, X7R, 10%\", \"-\")","v":"Capacitor, Ceramic, 3300pF, 16V, X7R, 10%"},null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"-\", \"Std\", \"-\")","v":"Std"},{"$f":"H33","v":"Std"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G33,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G33,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[{"$f":"CHOOSE(MODE, \"-\", \"1\", \"1\",\"-\")","v":"1"},{"$f":"CHOOSE(MODE,\"-\",\"Cff\",\"Cb\",\"-\")","v":"Cb"},{"$f":"CHOOSE(MODE, \"-\",'Variable Mgmt'!B290,'Variable Mgmt'!B290, \"-\")","v":"56pF"},{"$f":"CHOOSE(MODE,\"-\",\"Capacitor, Ceramic, \"&'Variable Mgmt'!B290&\", 50V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B290&\", 50V, X7R, 10%\", \"-\")","v":"Capacitor, Ceramic, 56pF, 50V, X7R, 10%"},null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"Std\", \"Std\", \"-\")","v":"Std"},{"$f":"H34","v":"Std"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G34,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G34,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G34,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G34,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"CBST","2.2nF","Capacitor, Ceramic, 2.2nF, 25V, X7R, 10%",null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"Std\", \"Std\", \"-\")","v":"Std"},{"$f":"H35","v":"Std"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G35,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G35,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G35,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G35,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[]
[1,"LF",{"$f":"'Design Converter'!E17","v":68},{"$f":"\"Inductor, \"&Lf*1000000&\" µH, \"&Rdcr*1000&\" mΩ, >\"&ROUNDUP(Isat_min,2)&\"A\"","v":"Inductor, 68 µH, 120 mΩ, >1.8A"},null,null,4,"Various","Various",{"$f":"CHOOSE(G37,'Variable Mgmt'!T50,'Variable Mgmt'!T51,'Variable Mgmt'!T52,'Variable Mgmt'!T53,'Variable Mgmt'!T54,'Variable Mgmt'!T55,'Variable Mgmt'!T56)","v":"6.0 x 6.0"},{"$f":"CHOOSE(G37,'Variable Mgmt'!U50,'Variable Mgmt'!U51,'Variable Mgmt'!U52,'Variable Mgmt'!U53,'Variable Mgmt'!U54,'Variable Mgmt'!U55,'Variable Mgmt'!U56)","v":36}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(MODE_RSET=2,CHOOSE(G38,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":""}]
[{"$f":"CHOOSE(MODE, \"1\",\"1\",\"1\", \"-\")","v":"1"},"RT",{"$f":"CHOOSE(MODE, 'Design Converter'!E13, 'Design Converter'!E13,'Design Converter'!E13,\"-\")","v":200},{"$f":"C39","v":200},null,null,1,{"$f":"CHOOSE(MODE, \"Std\",\"Std\",\"Std\",\"-\")","v":"Std"},{"$f":"H39","v":"Std"},{"$f":"CHOOSE(MODE,CHOOSE(G39,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G39,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G39,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,CHOOSE(G39,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G39,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G39,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"RFB1",{"$f":"Rfb1_/1000","v":453},453,null,null,1,{"$f":"CHOOSE(MODE_VOUT,\"-\",\"Std\")","v":"Std"},{"$f":"H40","v":"Std"},{"$f":"(CHOOSE(MODE_VOUT,\"\",CHOOSE(G40,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)))","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE_VOUT,\"\",CHOOSE(G40,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45))","v":0.5}]
[1,"RFB2",{"$f":"Rfb2_u/1000","v":49.9},49.9,null,null,1,{"$f":"CHOOSE(MODE_VOUT,\"-\",\"Std\")","v":"Std"},{"$f":"H41","v":"Std"},{"$f":"CHOOSE(MODE_VOUT,\"\",CHOOSE(G41,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45))","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE_VOUT,\"\",CHOOSE(G41,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45))","v":0.5}]
[{"$f":"IF(MODE=3,\"1\",\"-\")","v":"1"},{"$f":"CHOOSE(MODE,\"-\",\"-\",\"Ra\",\"-\")","v":"Ra"},{"$f":"'Variable Mgmt'!F296","v":"1000k"},{"$f":"\"Resistor, Chip, \"&'Variable Mgmt'!B296&\", 1/16W, 1%\"","v":"Resistor, Chip, 1000kΩ, 1/16W, 1%"},null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"-\", \"Std\", \"-\")","v":"Std"},{"$f":"H42","v":"Std"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G42,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G42,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"RPGOOD",100,100,null,null,1,"Std","Std",{"$f":"CHOOSE(G43,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)","v":"1.0 x 0.5"},{"$f":"CHOOSE(G43,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45)","v":0.5}]
[{"$f":"CHOOSE(MODE_UVLO, \"1\", \"-\")","v":"1"},"RUV1",{"$f":"CHOOSE(MODE_UVLO, 'Variable Mgmt'!H275, \"-\")","v":"1M"},{"$f":"CHOOSE(MODE_UVLO, \"Resistor, Chip, \"&'Variable Mgmt'!C275&\", 1/16W, 1%\", \"-\")","v":"Resistor, Chip, 1MΩ, 1/16W, 1%"},null,null,2,{"$f":"CHOOSE(MODE_UVLO,\"Std\",\"-\")","v":"Std"},{"$f":"H44","v":"Std"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G44,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.6 x 0.8"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G44,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":1.3}]
[{"$f":"CHOOSE(MODE_UVLO, \"1\", \"-\")","v":"1"},"RUV2",{"$f":"CHOOSE(MODE_UVLO, 'Variable Mgmt'!H276, \"-\")","v":"80.6k"},{"$f":"CHOOSE(MODE_UVLO, \"Resistor, Chip, \"&'Variable Mgmt'!C276&\", 1/16W, 1%\", \"-\")","v":"Resistor, Chip, 80.6kΩ, 1/16W, 1%"},null,null,1,{"$f":"CHOOSE(MODE_UVLO,\"Std\",\"-\")","v":"Std"},{"$f":"H45","v":"Std"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G45,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G45,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"U1",{"$f":"CHOOSE(VARIANT, \"LM5163-Q1\", \"LM5164-Q1\")","v":"LM5164-Q1"},{"$f":"CHOOSE(VARIANT, \"IC, LM51643-Q1, Buck Converter, 6V–100V Input\", \"IC, LM5164-Q1, Buck Converter, 6V–100V Input\")","v":"IC, LM5164-Q1, Buck Converter, 6V–100V Input"},null,null,"SOIC-8",{"$f":"CHOOSE(VARIANT, \"LM5163QDDATQ1\", \"LM5164QDDATQ1\")","v":"LM5164QDDATQ1"},"TI","5.0 x 6.0",30]
[]
[null,{"$f":"\"Total Solution Size (padded by 15%) = \"&ROUND(K48,1)&\" mm^2 = \"&ROUND(M48,3)&\" in^2\"","v":"Total Solution Size (padded by 15%) = 110.2 mm^2 = 0.171 in^2"},null,null,null,null,null,null,null,null,{"$f":"SUM(K31:K46)*1.15","v":110.16999999999999},null,{"$f":"K48/25.4/25.4","v":0.17076384152768304}]
[]
["NOTES:"]
["* Inductor saturation current should be higher than the peak inductor current setting for all operating temperatures *"]
["** Effective input and output capacitances should be appropriately derated for applied voltage and temperature, particularly with ceramics **"]
["***Estimated total solution size does not include EMI filter***"]

{"sheet":"Fsw & Ripple","index":3,"n_rows":1,"n_cols":1,"rows_kept":1,"cut":false,"hidden":true,"merged":[[0,0,0,16]]}
["                         LM5164 Low IQ DC/DC Converter Design Tool  "]

{"sheet":"Losses","index":4,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":true,"merged":[[0,0,0,16]]}
["                         LM5166 Low IQ DC/DC Converter Design Tool  "]
[]
[]
[]
[null,null,null,"Load Current",500,"mA"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"Inductor Core Loss Constant",0]

{"sheet":"EVM","index":5,"n_rows":85,"n_cols":15,"rows_kept":85,"cut":false,"hidden":false,"merged":[[0,0,0,16]]}
["LM5163/4 100V, Low IQ DC/DC Converter Design Tool  "]
[]
[null,"LM5164-Q1EVM-041 PCB Layout"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Top"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer 2"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer 3"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bottom"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer"]

{"sheet":"Design EMI Filter","index":6,"n_rows":33,"n_cols":15,"rows_kept":33,"cut":false,"hidden":false,"merged":[[0,0,0,22],[32,10,32,12],[29,10,29,12],[31,10,31,12]]}
["                         LM5163/4 100V, Low IQ DC/DC Converter Design Tool  "]
[]
[]
[]
[]
[]
["Step 7: EMI Filter (Optional)"]
[null,null,null,"Desired Maximum Noise Level, Vnoise(MAX)",50,"dBmV"]
[null,null,null,"EMI Filter Inductance, LF(EMI)",22,"mH"]
[null,null,null,"Minimum EMI Filter Capacitance",{"$f":"'Variable Mgmt'!M164","v":3.1917072837200204},"mF"]
[null,null,null,"EMI Filter Capacitance, CF(EMI)",4.7,"mF"]
[null,null,null,"Minimum EMI Filter Damping Capacitance",{"$f":"'Variable Mgmt'!M168","v":40},"mF"]
[null,null,null,"EMI Filter Damping Capacitance, CD(EMI)",10,"mF"]
[null,null,null,"Minimum Damping Capacitor ESR",{"$f":"'Variable Mgmt'!M169","v":1.4832396974191324},"Ω"]
[null,null,null,"Damping Capacitor ESR, ESR CD(EMI)",3.3,"Ω"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"EMI Filter BOM"]
[null,null,null,null,null,null,null,"Count","Ref Des","Value","Description",null,null,"Part Number","MFR"]
[null,null,null,null,null,null,null,1,"LF(EMI)",{"$f":"'Variable Mgmt'!B298","v":"22µH"},{"$f":"\"Inductor, \"&Lf_emi*1000000&\" µH, \"&ROUNDUP(Isat_min,2)&\"A\"","v":"Inductor, 22 µH, 1.8A"},null,null,"Std","Std"]
[null,null,null,null,null,null,null,1,"CF(EMI)",{"$f":"'Variable Mgmt'!B299","v":"4.7µF"},{"$f":"IF(VIN_max>35, \"Capacitor, Ceramic, \"&'Variable Mgmt'!B299&\", 100V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B299&\", 50V, X7R, 10%\")","v":"Capacitor, Ceramic, 4.7µF, 100V, X7R, 10%"},null,null,"Std","Std"]
[null,null,null,null,null,null,null,1,"CD(EMI)",{"$f":"'Variable Mgmt'!B300","v":"10µF"},{"$f":"IF(VIN_max>35, \"Capacitor, Electrolytic, \"&'Variable Mgmt'!B300&\", 100V, ESR>\"&ESR_Cd&ohm, \"Capacitor, Electrolytic, \"&'Variable Mgmt'!B300&\", 50V, ESR>\"&ESR_Cd&ohm)","v":"Capacitor, Electrolytic, 10µF, 100V, ESR>3.3Ω"},null,null,"Std","Std"]

{"sheet":"Variable Mgmt","index":7,"n_rows":320,"n_cols":21,"rows_kept":320,"cut":false,"hidden":true,"merged":[[4,4,4,7],[0,0,0,8]]}
["EXCEL Variables Names/Calculations",null,null,null,null,null,null,null,null,null,null,"LM5166"]
[null,"Input from user ="]
[null,"Output ="]
[null,"Constant"]
["Variable Name","Value","STD Units",null,"Notes",null,null,null,"Iteration"]
["Step 1: Operational Specs"]
["VIN_min",{"$f":"'Design Converter'!E6","v":47},"V","Minimum input voltage",null,null,null,null,1]
["VIN_nom",{"$f":"'Design Converter'!E7","v":65},"V","Nominal input voltage"]
["VIN_max",{"$f":"'Design Converter'!E8","v":71},"V","Maximum input voltage"]
[]
["Vout",{"$f":"'Design Converter'!E9","v":12},"V","Output Voltage",null,null,null,null,1]
["Iout",{"$f":"'Design Converter'!E10","v":0.5},"A","Maximum Output Current",null,null,null,null,1]
["Rout",{"$f":"Vout/Iout","v":24},"W","Load resistance"]
["Pout",{"$f":"Vout*Iout","v":6},"W","Output power"]
[]
["Efficiency",0.9,null,"Estimate of efficiency"]
["Pin",{"$f":"Pout/Efficiency","v":6.6666666666666661},"W","Calculate input power assuming 90% efficiency"]
["Iin_Vinmin",{"$f":"Pin/VIN_min","v":0.14184397163120566},"A"]
["Iin_Vinnom",{"$f":"Pin/VIN_nom","v":0.10256410256410256},"A","Input currents at min, nom, max Vin"]
["Iin_Vinmax",{"$f":"Pin/VIN_max","v":9.3896713615023469E-2},"A"]
[]
["Fsw",{"$f":"'Design Converter'!E12*1000","v":150000},"Hz","Nominal Switching Frequency",null,null,null,null,1]
["Vref",1.2,"V","Reference Voltage"]
["Rt",{"$f":"Vout*2500000000/Fsw","v":200000},"W","Frequency Set Resistor"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"B34&\"_\"&F35&\"_\"&F39&\"_\"&I41&\"_\"&I36","v":"COT3_VOUTadj_UVLOadj_SSAdj_RsetGND"},null,null,null,null,null,"Vout<5V",100,1]
["Internal PD at Full Load",{"$f":" IF(OR(MODE=1,MODE=2,MODE=3), Efficiency!AZ106,#REF!)","v":0.31380731880512902},"W",null,null,null,null,null,null,null,null,null,null,null,null,null,"Vout<=8V",47,2]
[null,null,null,null,null,null,null,null,null,null,{"$f":"\"SCH_\"&B34&\"_\"&B41","v":"SCH_COT3_LM5164"},null,null,null,null,null,"Vout<=12V",22,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vout<=20V",22,4]
["Step 2: Circuit Configuration for COT / PFM, Fixed / Adj Vout, ILIM, UVLO, SS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vout>20V",10,5]
[null,"COT Type I",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cout Capacitance",{"$f":"CHOOSE(S30,\"100\", \"47\",\"22\",\"22\",\"10\")","v":"22"},{"$f":"IF(Vout<5, 1, IF(Vout<=8, 2, IF(Vout<=12, 3, IF(Vout<=20, 4, 5))))","v":3}]
[null,"COT Type II",2]
["COT/PFM ","COT Type III",3]
[null,null,null,null,"VOUT Fixed/Adjustable","Fixed",1,null,"ILIM shorted",1,{"$f":"B34&\", \"&F35&\", \"&I36&\", \"&F39&\", \"&I41","v":"COT3, VOUTadj, RsetGND, UVLOadj, SSAdj"},null,null,null,null,null,"Vout<=5V","6.3V",1]
["MODE",{"$f":"CHOOSE(C34, \"COT1\", \"COT2\",\"COT3\")","v":"COT3"},3,null,null,"Adjustable",2,null,"ILIM resistor needed",2,{"$f":"C34&\", \"&G35&\", \"&J36&\", \"&G39&\", \"&J41","v":"3, 2, 1, 1, 1"},null,null,null,null,null,"Vout<=8V","10V",2]
[null,{"$f":"IF(MODE=4, \"PFM\", \"COT\")","v":"COT"},null,null,"MODE_VOUT",{"$f":"CHOOSE(G35, \"VOUTfixed\", \"VOUTadj\")","v":"VOUTadj"},{"$f":"IF(AND(OR(MODE=1,MODE=4),OR(Vout=3.3,Vout=5)),1,2)","v":2},null,null,null,{"$f":"C34&G35&J36&G39&J41","v":"32111"},null,null,null,null,null,"Vout<=12V","16V",3]
[null,null,null,null,null,null,null,"MODE_RSET",{"$f":"CHOOSE(J36, \"RsetGND\",\"Rset\")","v":"RsetGND"},1,null,null,null,null,null,null,"Vout<=20V","25V",4]
[null,null,null,null,"UVLO","Adjustable",1,null,null,null,null,null,null,null,null,null,"Vout>20V","50V",5]
[null,null,null,null,null,"Internal",2,"Soft Start","Adjustable",1,null,"Iout Linear Axis",1,null,null,null,"Cout Voltage Rating",{"$f":"CHOOSE(S38,\"6.3V\", \"10V\",\"16V\",\"25V\",\"50V\")","v":"16V"},{"$f":"IF(Vout<=5, 1, IF(Vout<=8, 2, IF(Vout<=12, 3, IF(Vout<=20, 4, 5))))","v":3}]
[null,"LM5163",1,null,"MODE_UVLO",{"$f":"CHOOSE(G39, \"UVLOadj\", \"UVLOint\")","v":"UVLOadj"},1,null,"3ms Fixed",2,null,"Iout Log Axis",2]
[null,"LM5164",2,null,null,null,null,null,null,null,null,"PLOT_TYPE",1]
["VARIANT",{"$f":"CHOOSE(VARIANT, \"LM5163\", \"LM5164\")","v":"LM5164"},2,null,"ESR","NO",1,"MODE_SS",{"$f":"CHOOSE(J41, \"SSAdj\", \"SSfix\")","v":"SSAdj"},1,null,null,null,null,null,null,null,"0402",1,"1.0 x 0.5",0.5]
[null,null,null,null,null,"YES",2,null,null,null,null,null,null,null,null,null,null,"0603",2,"1.6 x 0.8",1.3]
[null,null,null,null,"MODE_ESR",null,2,null,null,null,null,null,null,null,null,null,null,"0805",3,"2.0 x 1.25",2.5]
[null,null,null,null,null,{"$f":"CHOOSE(G44, \"\", \"_ESR\")","v":"_ESR"},{"$f":"IF(MODE=2, 1, MODE_ESR)","v":2},null,null,null,null,null,null,null,null,null,null,"1206",4,"3.2 x 1.6",5.0999999999999996]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1210",5,"3.2 x 2.5",8]
["Step 3: Buck Inductor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Component Size",{"$f":"CHOOSE(S46,\"0402\", \"0603\",\"0805\",\"1206\",\"1210\")","v":"1210"},5,{"$f":"CHOOSE(S46,T41,T42,T43,T44,T45)","v":"3.2 x 2.5"}]
["Don1",{"$f":"Vout/VIN_nom","v":0.18461538461538463},{"$f":"(Vout-VIN_nom)/Vout","v":-4.416666666666667},null,"Ideal Duty Cycle at VIN(nom)",null,null,null,1]
["Doff1",{"$f":"1-47:47","v":0.81538461538461537},null,null,"Ideal 1- Duty Cycle at VIN(nom)",null,null,null,1]
[]
["Don_Vinmin",{"$f":"Vout/VIN_min","v":0.25531914893617019},{"$f":"IF(VIN_min>Vout, \"BUCK\", \"BOOST\")","v":"BUCK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3mm x 3mm",1,"3.0 x 3.0",9]
["Don_Vinnom",{"$f":"Vout/VIN_nom","v":0.18461538461538463},{"$f":"IF(VIN_nom>Vout, \"BUCK\", \"BOOST\")","v":"BUCK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4mm x 4mm",2,"4.0 x 4.0",16]
["Don_Vinmax",{"$f":"Vout/VIN_max","v":0.16901408450704225},{"$f":"IF(VIN_max>Vout, \"BUCK\", \"BOOST\")","v":"BUCK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5mm x 5mm",3,"5.0 x 5.0",25]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6mm x 6mm",4,"6.0 x 6.0",36]
["Lf_Vinmin",{"$f":"(VIN_min-Vout)*Don_Vinmin/(Fsw*Iout*0.4)","v":2.9787234042553186E-4},"H","COT",null,null,null,null,null,null,null,null,null,null,null,null,null,"7mm x 7mm",5,"7.0 x 7.0",49]
["Lf_Vinnom",{"$f":"(VIN_nom-Vout)*Don_Vinnom/(Fsw*Iout*0.4)","v":3.2615384615384619E-4},"H","COT",null,null,null,null,1,null,null,null,null,null,null,null,"Inductor Size","8mm x 8mm",6,"8.0 x 8.0",64]
["Lf_Vinmax",{"$f":"(VIN_max-Vout)*Don_Vinmax/(Fsw*Iout*0.7)","v":1.8993963782696176E-4},"H","COT",null,null,null,null,null,null,null,null,null,null,null,null,null,"10mm x 10mm",7,"10.0 x 10.0",100]
[]
["L_Vinmin_COT",{"$f":"(VIN_min-Vout)*Don_Vinmin/(Fsw*Iout*0.3)","v":3.9716312056737587E-4},"H","COT","Calculated Inductance for 30% ripple at VIN(min)"]
["L_Vinnom_COT",{"$f":"(VIN_nom-Vout)*Don_Vinnom/(Fsw*Iout*0.4)","v":3.2615384615384619E-4},"H","COT","Calculated Inductance for 40% ripple at VIN(nom)",null,null,null,null,null,"Pk-to-Pk Ripple Current at VIN(nom), DIL"]
["L_Vinmax_COT",{"$f":"(VIN_max-Vout)*Don_Vinmax/(Fsw*Iout*0.7)","v":1.8993963782696176E-4},"H","COT","Calculated Inductance for 70% ripple at VIN(max)"]
[]
[]
["Lopt",{"$f":"B59","v":3.2615384615384619E-4},"H"]
[]
["Lf",{"$f":"'Design Converter'!E17/1000000","v":6.7999999999999999E-5},"H",null,"Chosen Inductance"]
["Rdcr",{"$f":"'Design Converter'!E18/1000","v":0.12},"W",null,"Chosen Inductor DCR"]
[]
["Don2",{"$f":"(Vout+Iout*Rdcr)/Vin","v":0.18553846153846154},null,null,"**Edit to add Rdson**"]
["Doff2",{"$f":"1-_Don2","v":0.81446153846153846}]
[]
["Rdson1",0.75,"W"]
["Rdson2",0.33,"W"]
[]
["Don_Vinmin_2",{"$f":"(Vout+Iout*(Rdcr+Rdson2))/(VIN_min+Iout*Rdson2)","v":0.25919643803667974},null,null,"Duty cycles adjusted for DCR and shunt voltage drops"]
["Don_Vinnom_2",{"$f":"(Vout+Iout*(Rdcr+Rdson2))/(VIN_nom+Iout*Rdson2)","v":0.18760070590040664},null,null,"need to include RDS(on) later"]
["Don_Vinmax_2",{"$f":"(Vout+Iout*(Rdcr+Rdson2))/(VIN_max+Iout*Rdson2)","v":0.17178388252652285}]
[]
["Iripple_Vinmin",{"$f":"(VIN_min-Vout-Rdson1*Iout)*Don_Vinmin_2/(Fsw*Lf)","v":0.87987026147255265},"A","COT"]
["Iripple_Vinnom",{"$f":"(VIN_nom-Vout-Rdson1*Iout)*Don_Vinnom_2/(Fsw*Lf)","v":0.96789089686361762},"A","COT"]
["Iripple_Vinmax",{"$f":"(VIN_max-Vout)*Don_Vinmax_2/(Fsw*Lf)","v":0.99365186951616169},"A","COT"]
[]
["ILpk_Vinmin",{"$f":"Iout+Iripple_Vinmin/2","v":0.93993513073627633},"A","COT"]
["ILpk_Vinnom",{"$f":"Iout+Iripple_Vinnom/2","v":0.98394544843180887},"A","COT"]
["ILpk_Vinmax",{"$f":"Iout+Iripple_Vinmax/2","v":0.99682593475808079},"A","COT"]
[]
["ILIM_Typ",{"$f":"CHOOSE(VARIANT, 0.75, 1.5)","v":1.5},"A",null,"Isat_min",{"$f":"B86*1.2","v":1.7999999999999998}]
[]
["Ripple current",{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), Iripple_Vinnom, Iripple)","v":0.96789089686361762},"A",null,null,null,null,"% Ripple Current at Nom VIN"]
[null,null,null,null,null,null,null,"Maximum Load Current"]
["Max inductor ripple current",{"$f":"MAX(B78:B80)","v":0.99365186951616169},"A"]
[null,null,null,null,null,"Ripple I","Iin"]
["% Ripple Current",{"$f":"B78/Iout","v":1.7597405229451053},null,"COT",null,{"$f":"B78","v":0.87987026147255265},{"$f":"Iin_Vinmin","v":0.14184397163120566}]
[null,{"$f":"B79/Iout","v":1.9357817937272352},null,"COT",null,{"$f":"B79","v":0.96789089686361762},{"$f":"Iin_Vinnom","v":0.10256410256410256}]
[null,{"$f":"B80/Iout","v":1.9873037390323234},null,"COT",null,{"$f":"B80","v":0.99365186951616169},{"$f":"Iin_Vinmax","v":9.3896713615023469E-2}]
[]
[null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3), B93, Ilim/Iout)","v":1.9357817937272352}]
[]
["Iripple1",{"$f":"(Vin-Vout)*Don_Vinnom_2/(Fsw*Lf)","v":0.97478798163936786},"A","inductor ripple current with chosen inductance (pk-pk)",null,null,null,null,1]
["Temp",100]
["DCR at hot",{"$f":"Rdcr*(1+0.0039*(B99-25))","v":0.15509999999999999},"W"]
[]
[]
[]
["Step 4: Output Capacitor"]
["Icoutrms_VINmin",{"$f":"Iripple_Vinmin/SQRT(12)","v":0.25399666615656236},"A","Output Cap RMS current"]
["Icoutrms_VINnom",{"$f":"Iripple_Vinnom/SQRT(12)","v":0.279406034925199},"A"]
["Icoutrms_VINmax",{"$f":"Iripple_Vinmax/SQRT(12)","v":0.28684258717296546},"A",null,null,null,{"$f":"Vripple1","v":0.06}]
[]
["Output Ripple Spec (pk-pk)",{"$f":"Vout*0.005","v":0.06},"V","Vout capacitive ripple spec at Vin(nom) = Vripple1"]
[]
["Coutmin"]
["COT",{"$f":"Iripple_Vinnom/(Fsw*8*Vripple1)","v":1.3442929123105801E-5},"F","COT","Min recommended Cout based on ripple spec above",null,null,null,1]
[null,{"$f":"Lf*B83^2/((1.05*Vout)^2-Vout^2)","v":4.4603054128250389E-6},"F","COT","Min recommended Cout based on 5% load-off transient spec"]
["CoutMinCOT",{"$f":"MAX(B112:B113, 0.0000022)","v":1.3442929123105801E-5},"F","COT","max of 2 results and 2.2uF"]
[]
["Reported Countmin",{"$f":"CoutMinCOT*1000000","v":13.442929123105801},"µF"]
[]
["Cout",{"$f":"'Design Converter'!E24/1000000","v":4.3999999999999999E-5},"F","Chosen Output Capacitance",null,null,null,null,1]
["Resrmax",{"$f":"SQRT((Vripple1/Iripple_Vinnom)^2-(1/(Fsw*Cout*8))^2)","v":5.9026402918198155E-2},"W","Max ESR before ripple exceeds Vripple1",null,null,null,null,1]
["Type1 ESR for sufficient (20mV) COT ripple at FB pin",{"$f":"0.02*Vout/Vref/Iripple_Vinnom","v":0.20663486003235071},"W","(a)"]
["Type2 ESR for sufficient (20mV) COT ripple at FB pin",{"$f":"0.02/Iripple_Vinnom","v":2.066348600323507E-2},"W","(b)"]
[]
["Type 1 Output Cap RC Time Constant",{"$f":"Cout*B130*1000000","v":0},"µs"]
["Type 2 Output Cap RC Time Constant",{"$f":"Cout*B131*1000000","v":0},"µs"]
["Ton @ Vin(min)",{"$f":"Vout/VIN_min/(Fsw)","v":1.7021276595744679E-6},"s"]
["Ton @ Vin(nom)",{"$f":"Vout/VIN_nom/(Fsw)","v":1.2307692307692308E-6},"s"]
["ESR so that RC > Ton/2",{"$f":"B125/2/Cout","v":1.9342359767891681E-2},"W","(c)"]
[]
[]
["Type1: Need ESR of…",{"$f":"IF(MODE=1, MAX(B120,B127), 0)","v":0},"W","Max of (a) and (c)"]
["Type2: Need ESR of…",{"$f":"IF(MODE=2, MAX(B121,B127), 0)","v":0},"W","Max of (b) and (c)"]
[]
["Reported Cout ESR max",{"$f":"IF(OR(CoutEsrMax>0.5, CoutEsrMax<0, (ISERROR(CoutEsrMax))), \"N/A\", CoutEsrMax*1000)","v":59.026402918198158},"mW"]
[]
["CoutEsr",{"$f":" 'Design Converter'!E26","v":5.0000000000000001E-3},"W","Chosen ESR",null,null,null,null,1]
[]
["Actual Output Ripple",{"$f":"Iripple_Vinnom*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2)","v":1.8959316153800393E-2},"Vp-p","Vripple2"]
[]
["Minimum Feedforward / Coupling Capacitance",{"$f":"MAX(1000000000000*0.00005/(3*Rfb1_),47)","v":47},"pF",null,null,null,null,{"$f":"0.00005/3/Rfb1_","v":3.6791758646063281E-11}]
["Recommended Cff / Cb",{"$f":"IF(OR(MODE=2,MODE=3), \">\"&ROUND(B139,0),\"\")","v":">47"},"pF"]
["Selected Cff / Cb",{"$f":"'Design Converter'!$E$29","v":56},"pF"]
[]
["Minimum Ripple Generation Capacitance",{"$f":"10/(Fsw*Rfb)","v":1.4831723786056291E-9},"F",{"$f":"1000000000000*B143","v":1483.1723786056291},"pF",{"$f":"Rfb","v":44948.697554185725}]
["Recommended Ca",{"$f":"IF(MODE=3, \">\"&ROUND(D143,0),\"\")","v":">1483"},"pF"]
["Selected Ca",{"$f":"'Design Converter'!E31","v":3300},"pF",{"$f":"B145/1000000000000","v":3.3000000000000002E-9},"F"]
[]
["Maximum Ripple Generation Resistance",{"$f":"(VIN_nom-Vout)*B126/((B149/1000)*Ca)","v":988344.98834498832},"W",{"$f":"B147/1000","v":988.34498834498834},"kW"]
["Recommended Ra",{"$f":"IF(MODE=3, \"<\"&ROUND(D147,0),\"\")","v":"<988"},"kW",null,null,null,null,null,null,null,null,"Lf_emi",{"$f":"'Design EMI Filter'!$E$9","v":22},"uH",{"$f":"M148/1000000","v":2.1999999999999999E-5},"H"]
["Ripple amplitude",{"$f":"'Design Converter'!E33","v":20},"mVp-p",null,null,null,null,null,null,null,null,"Cf_emi",{"$f":"'Design EMI Filter'!$E$11","v":4.7},"uF",{"$f":"M149/1000000","v":4.6999999999999999E-6},"F"]
[null,null,null,null,null,null,null,null,null,null,null,"Cd_emi",{"$f":"'Design EMI Filter'!$E$13","v":10},"uF",{"$f":"M150/1000000","v":1.0000000000000001E-5},"F"]
[null,null,null,null,null,null,null,null,null,null,null,"ESR_Cd",{"$f":"'Design EMI Filter'!$E$15","v":3.3},"Ω",{"$f":"M151","v":3.3},"Ω",{"$f":"ESR_Cd&ohm","v":"3.3Ω"}]
["Step 5: Input Capacitor",null,null,null,null,null,null,null,null,null,null,"Min Noise",{"$f":"'Design EMI Filter'!$E$8","v":50},"dB","noise limit"]
["Vinripple1",{"$f":"0.05*VIN_nom","v":3.25},"Vp-p","Input voltage ripple spec (pk-pk) at Vin(nom)",null,null,null,null,null,null,null,"Duty Cycle",{"$f":"Vout/VIN_nom/Efficiency_COT_Full_Load","v":0.19851116625310175},null,"calculated duty cycle"]
[null,null,null,null,null,null,null,null,null,null,null,"Target Atten.",{"$f":"20*LOG(Iout/(PI()^2*Fsw*Cin)*SIN(PI()*Duty_Cycle)/0.000001) - Min_Noise","v":35.899759807081111},"dB","calculated attenuation"]
["Icinrms",{"$f":"Iout*SQRT(Don_Vinnom_2*(1-Don_Vinnom_2))","v":0.19519649141703072},"A"]
["Cinmin",{"$f":"Iout*Don_Vinnom_2*(1-Don_Vinnom_2)/(Vinripple1*Fsw-Iout*RCinEsr)*1000000","v":0.15631454514360965},"µF"]
["Reported Cinmin",{"$f":"IF(Cinmin<2.2, 2.2,Cinmin)","v":2.2000000000000002},"µF",null,null,null,null,null,null,null,null,"Filter Inductor"]
["Cin",{"$f":"'Design Converter'!E37/1000000","v":1.0000000000000001E-5},"F","Input capacitance",null,null,null,null,null,null,null,"Irms rating",{"$f":"Iout*1.5","v":0.75},"A","calculated suggested IRMS rating"]
["CinEsrMax",{"$f":"-(Iout*Don_Vinnom_2*(1-Don_Vinnom_2)/(Cin*Fsw)-Vinripple1)/(Iout+Iripple_Vinnom/2)","v":3.2513975018467276},"W"]
["RCinEsr",{"$f":"'Design Converter'!E39/1000","v":3.0000000000000001E-3},"W","Input capacitance series resistance (ESR)"]
["Reported Cin ESR max",{"$f":"IF(OR(CinEsrMax>12, CinEsrMax<0), \"N/A\",CinEsrMax*1000)","v":3251.3975018467277},"mΩ",null,null,null,null,null,null,null,null,"Filter Capacitor"]
[null,null,null,null,null,null,null,null,null,null,null,"Cfa calculation",{"$f":"Cin/(Cin*Lf_emi*0.000001*(2*PI()*Fsw/10)^2 - 1) / 0.000001","v":-10.000019541854902},"uF","calculated value"]
["COT input voltage ripple - Vinripple2",{"$f":"Iout*Don_Vinnom_2*(1-Don_Vinnom_2)/(Cin*Fsw)+(Iout +Iripple_Vinnom/2)*RCinEsr","v":5.3754063360654004E-2},"Vp-p",null,{"$f":"Iout*Don_Vinmax_2*(1-Don_Vinmax_2)/(Cin*Fsw)","v":4.7424726743545545E-2},"Vp-p",null,null,null,null,null,"Cfb calculation",{"$f":"1/(Lf_emi)*(10^(Target_Att/40)/(2*PI()*Fsw))^2/0.000001","v":3.1917072837200204},"uF","calculated value"]
[null,null,null,null,null,null,null,null,null,null,null,"Cf",{"$f":"MAX(M162,M163)","v":3.1917072837200204},"uF","calculated value"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Damping Capacitor"]
["Step 6: Soft Start",null,null,null,null,null,null,null,null,null,null,"Cd ≥",{"$f":"4*Cin*1000000","v":40},"uF","calculated value"]
["Tss",{"$f":"'Design Converter'!#REF!/1000","v":{"$error":"#REF!"}},"s","Soft-start time",null,null,null,null,null,null,null,"Cd ESR ≥",{"$f":"SQRT(Lf_emi/Cin)","v":1.4832396974191324},"Ω","calculated value"]
["Iss",1.0000000000000001E-5,"A","Soft-start current"]
["Css",{"$f":"8.16*Tss/1000000","v":{"$error":"#NAME?"}},"F","Required soft-start cap"]
["Css_u",{"$f":"'Standard Value Calculator'!B4","v":{"$error":"#NAME?"}},"F","User selected SS cap",null,null,null,null,null,null,null,"CIN and Cd Capacitors Current Sharing and Rating"]
[null,null,null,null,null,null,null,null,null,null,null,"Cd impedance",{"$f":" 1/(2*PI()*Fsw*Cd_emi) + ESR_Cd","v":3.4061032953945967},"Ω","calculated Cd impedance at the sw. frequency"]
["Step 7: Other Components - UVLO, PGOOD",null,null,null,null,null,null,null,null,null,null,"Cin impedance",{"$f":" 1/(2*PI()*Fsw*Cin) + RCinEsr","v":0.1091032953945969},"Ω","calculated CIN impedance at the sw. frequency"]
[]
["Rising UVLO/EN Threshold",1.5,"V",null,null,null,null,null,null,null,null,"IRMS Total Input Cap",{"$f":"Iout*SQRT(Duty_Cycle*(1-Duty_Cycle))","v":0.19943951659960416},"A","calculated total IRMS current for CIN and Cd combined"]
["Falling UVLO/EN Threshold",1.4,"V",null,null,null,null,null,null,null,null,"IRMS Cd Act",{"$f":"IRMSTOT*(ZCIN/(ZCIN+ZCd))","v":6.1901080152552369E-3},"A","Calculated min IRMS current rating for Cd"]
["Voltage Hysteresis",{"$f":"B176-B177","v":0.10000000000000009},"V",null,null,null,null,null,null,null,null,"IRMS CIN",{"$f":"IRMSTOT*(ZCd/(ZCIN+ZCd))","v":0.19324940858434891},"A","Calculated min IRMS current rating for CIN"]
[]
["VINUVLO_ON",{"$f":"'Design Converter'!E48","v":20},"V"]
["VINUVLO_OFF",null,"V"]
[]
["RUV1",{"$f":"'Design Converter'!E49*1000","v":1000},"kΩ",{"$f":"'Standard Value Calculator'!J16","v":1000},"kΩ",{"$f":"IF(Ruvlo1<0,\"N/A\",D183)","v":1000},{"$f":"IF(Ruvlo1<0,\"N/A\",D183&\"kΩ\")","v":"1000kΩ"}]
["RUV2",{"$f":"Vuvlo_on*Ruvlo1/(VINuvlo_on-Vuvlo_on)","v":81.081081081081081},"kΩ",{"$f":"'Standard Value Calculator'!J17","v":80.600000000000009},"kΩ",{"$f":"IF(F183=\"N/A\",\"N/A\",D184)","v":80.600000000000009},{"$f":"IF(G183=\"N/A\",\"N/A\",D184&\"kΩ\")","v":"80.6kΩ"}]
[]
["VINUVLO_ON_ACTUAL",{"$f":"(D183+D184)/D184*Vuvlo_on","v":20.110421836228284},"V"]
["VINUVLO_OFF_ACTUAL",{"$f":"(D183+D184)/D184*Vuvlo_off","v":18.769727047146397},"V"]
[]
["RPG",20,"kΩ"]
[]
[]
["Step 8: FB Divider"]
["Pi",3.1415926500000002,null,"p"]
["Toff_Vinmax",{"$f":"(1-Don_Vinmax_2)/Fsw","v":5.5214407831565143E-6},"sec"]
["Ton_Vinmin",{"$f":"IF(VIN_min>Vout, (1-Don_Vinmin_2)/Fsw, Don_Vinmin_2/Fsw)","v":4.9386904130888018E-6},"sec"]
[]
["Rfb1",{"$f":"'Design Converter'!E43*1000","v":453000},"W","Lower Feedback Resistance - chosen by user",null,null,null,null,1]
["Rfb2",{"$f":"IF(Vout=Vref,100000000,Vref*B197/((Vout-Vref)))","v":50333.333333333328},"W","Upper Feedback Resistance"]
["Rfb2_u",{"$f":"IF(Vout=Vref,\"N/A\",'Standard Value Calculator'!J10)","v":49900},"W","Std Value Upper Feedback Resistance"]
["Rfb",{"$f":"Rfb1_*Rfb2_u/(Rfb1_+Rfb2_u)","v":44948.697554185725},"W","Rfb1 || Rfb2_u"]
[null,{"$f":"1.2/Rfb2_u*(Rfb2_u+Rfb1_)","v":12.0937875751503},"V"]
["Ifb",{"$f":"CHOOSE(MODE_VOUT, IF(Vout=5, 0.000007, 0.0000038), Vout/(Rfb1_+Rfb2_u))","v":2.3861602704314974E-5}]
[]
["Other Input Variables"]
["Rfets",0,"W","Series resistance due to FETs",null,null,null,{"$f":"_Don2*RdsonTop+Doff2*RdsonBot+B209*Vin^2*Fsw/2/(((Iripple1/SQRT(3))^2))","v":5.3772364875618601}]
["Diode loss eq res",{"$f":"0.00000002*Fsw*0.6*4/Iripple1","v":7.3862215534205352E-3}]
["Fet loss eq res",{"$f":"_Don2*RdsonTop+Doff2*RdsonBot","v":0.37506123076923081}]
["cap loss eq res",{"$f":"B209*Vin^2*Fsw/2/(((Iripple1/SQRT(3))^2))","v":5.0021752567926292}]
["Sw cap",5.0000000000000001E-9]
[]
["Step 8: Efficiency"]
[]
["Design"]
["Ta",25,"°C","Ambient Temperature"]
["Components"]
["LTc",{"$f":"4000/1000000","v":4.0000000000000001E-3},"%/°C","Inductor DCR Temp Co"]
["θCA",40,"°C/W","Inductor Core to Ambient Thermal Resistance"]
["RCinEsr",{"$f":"RCinEsr","v":3.0000000000000001E-3},"W","Input Capacitor ESR"]
["Part Characteristics"]
["Vcc",{"$f":"IF(Vin>7.7,7.5,Vin-0.2)","v":7.5},"V"]
["Deadtime"]
["Deadtime",2E-8,"s","Total Deadtime",null,null,"20ns for LM5166"]
["IQ"]
["IQ ",1.0000000000000001E-5,"A","Quiescent Current Of Controller (Not Switching!)"]
[]
[]
["IC Power Disipation","Value","Units"]
["Power Dis",{"$f":"Efficiency!AZ106","v":0.31380731880512902},"W"]
["Temp rise",{"$f":"B228*ThetaJA","v":12.897480802890803},"°C"]
["Current (switching)",{"$f":"(Qg_Q1+Qg_Q2)*Fsw+Iq","v":{"$error":"#NAME?"}},"A"]
["Qrr Current",{"$f":"Qrr_Q2*Fsw","v":{"$error":"#NAME?"}},"A"]
["Diode Current",{"$f":"C232/Vin","v":{"$error":"#NAME?"}},{"$f":"Deadtime*Fsw*(Ipp/2)*(Vsd_Q1+Vsd_Q2)","v":{"$error":"#NAME?"}}]
["Total Application Switching IQ",{"$f":"SUM(B230:B232)","v":{"$error":"#NAME?"}},"A"]
[]
[]
["SCHEMATIC LABELS"]
[]
[]
[{"$f":"\"RUV1 = \"&'Design Converter'!E49&\"MΩ\"","v":"RUV1 = 1MΩ"},{"$f":"C275","v":"1MΩ"}]
[{"$f":"\"RUV2 = \"&'Design Converter'!E50&\"kΩ\"","v":"RUV2 = 80.6kΩ"},{"$f":"C276","v":"80.6kΩ"}]
[{"$f":"\"Rhys = \"&'Design Converter'!E52&\"kΩ\"","v":"Rhys = 18.7697270471464kΩ"},{"$f":"C277","v":{"$error":"#REF!"}}]
[]
[{"$f":"\"LF = \"&'Design Converter'!E17&\"µH\"","v":"LF = 68µH"},{"$f":"'Design Converter'!E17&\"µH\"","v":"68µH"}]
[{"$f":"\"Rdcr = \"&Rdcr*1000&\"mΩ\"","v":"Rdcr = 120mΩ"},{"$f":"Rdcr*1000&\"mΩ\"","v":"120mΩ"}]
[{"$f":"\"Rt = \"&'Design Converter'!I43&\"kΩ\"","v":"Rt = kΩ"},{"$f":"'Design Converter'!I43&\"kΩ\"","v":"kΩ"}]
[{"$f":"\"Css = \"&ROUND(Css_u*1000000000,1)&\"nF\"","v":{"$error":"#NAME?"}},{"$f":"ROUND(Css_u*1000000000,1)&\"nF\"","v":{"$error":"#NAME?"}}]
[]
["VIN",{"$f":"VIN_nom&\"V\"","v":"65V"}]
["VIN range",{"$f":"VIN_min&\"V...\"&VIN_max&\"V\"","v":"47V...71V"}]
[]
[{"$f":"\"VOUT = \"&'Design Converter'!E9&\"V\"","v":"VOUT = 12V"},{"$f":"'Design Converter'!E9&\"V\"","v":"12V"}]
[null,null,{"$f":"R30","v":"22"},{"$f":"ROUNDUP('Design Converter'!$E$24/C252,0)","v":2}]
[{"$f":"\"COUT = \"&'Design Converter'!$E$24&\"µF\"","v":"COUT = 44µF"},{"$f":"'Design Converter'!$E$24&\"µF\"","v":"44µF"},{"$f":"IF('Design Converter'!$E$24=OR(10, 22, 47, 100), 'Design Converter'!$E$24,C252)","v":"22"},{"$f":"IF(D252=1, \"\",B255)","v":"2 x "},{"$f":"D253&C253&\"µF\"","v":"2 x 22µF"},{"$f":"C253&\"µF\"","v":"22µF"}]
["Capacitance per component (Cout)",{"$f":"C252&\"µF\"","v":"22µF"}]
["# of output caps",{"$f":"D252&\" x \"","v":"2 x "}]
[]
["CIN",{"$f":"Cin*1000000&\"µF\"","v":"10µF"}]
["Capacitance per component (Cin)",{"$f":"\"2.2µF\"","v":"2.2µF"}]
["# of input caps",{"$f":"ROUNDUP(Cin*1000000/2.2,0)&\" x \"","v":"5 x "}]
[]
["Fixed VOUT?",{"$f":"IF(MODE_VOUT=1, \"YES\", \"NO\")","v":"NO"}]
["FB resistor ref des shown or not?",{"$f":"IF(MODE_VOUT=2, \"YES\", \"NO\")","v":"YES"},{"$f":"IF(MODE_VOUT=2, \"R1\", \"\")","v":"R1"},{"$f":"IF(MODE_VOUT=2, \"R2\", \"\")","v":"R2"}]
[{"$f":"\"RFB1 = \"&'Design Converter'!E43&\"kΩ\"","v":"RFB1 = 453kΩ"},{"$f":"'Design Converter'!E43&\"kΩ\"","v":"453kΩ"},{"$f":"IF(MODE=1,'Design Converter'!E43&\"kΩ\", \"\")","v":""}]
[{"$f":"\"RFB2 = \"&IF(Vout=Vref,\"OPEN\",'Design Converter'!E44&\"kΩ\")","v":"RFB2 = 49.9kΩ"},{"$f":"IF(Vout=Vref,\"OPEN\",Rfb2_u/1000&\"kΩ\")","v":"49.9kΩ"},{"$f":"IF(MODE=1, IF(Vout=Vref, \"OPEN\",Rfb2_u/1000&\"kΩ\" ), \"\")","v":""}]
[]
[]
["Show Rt resistor ref des?",{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), \"YES\", \"NO\")","v":"YES"},{"$f":"IF(MODE=4,\"\", \"Rt\")","v":"Rt"}]
["Rt",{"$f":"IF(MODE=4, \"\", 'Standard Value Calculator'!J4/1000&\"kΩ\")","v":"200kΩ"}]
[]
["Show ESR resistor ref des?",{"$f":"IF(OR(MODE=3, MODE=4), \"NO\", \"YES\")","v":"NO"},{"$f":"IF(OR(MODE=3, MODE=4),\"\",\"Resr\")","v":""}]
[{"$f":"\"RESR = \"&'Design Converter'!E26&\"mΩ\"","v":"RESR = 0.005mΩ"},{"$f":"IF(OR(MODE=3,MODE=4), \"\", 'Design Converter'!E26&\"Ω\")","v":""},null,null,null,{"$f":"B120","v":0.20663486003235071}]
["Resr",{"$f":"IF(MODE=1, \">\"&ROUND(B130,3), IF(MODE=2,  \">\"&ROUND(B131,3),IF(MODE=3,ROUND(B119,3),\"\")))","v":5.8999999999999997E-2}]
[]
["Adjustable UVLO?",{"$f":"IF(MODE_UVLO=1, \"YES\", \"NO\")","v":"YES"},{"$f":"IF(MODE_UVLO=1,\"Ren1\", \"\")","v":"Ren1"},{"$f":"IF(MODE_UVLO=1, \"Ren2\", \"\")","v":"Ren2"},{"$f":"IF(MODE_UVLO=1, \"Rhys\", \"\")","v":"Rhys"},"Value","Units","BOM display"]
[{"$f":"\"RUV1 = \"&C275","v":"RUV1 = 1MΩ"},{"$f":"'Design Converter'!E49&\" MΩ\"","v":"1 MΩ"},{"$f":"IF(MODE_UVLO=1,'Design Converter'!E49&\"MΩ\", \"\")","v":"1MΩ"},null,null,{"$f":"IF(MODE_UVLO=1,'Design Converter'!E49, \"\")","v":1},{"$f":"IF(MODE_UVLO=1,\"MΩ\", \"\")","v":"MΩ"},{"$f":"IF(MODE_UVLO=1,'Design Converter'!E49&\"M\", \"\")","v":"1M"}]
[{"$f":"\"RUV2 = \"&C276","v":"RUV2 = 80.6kΩ"},{"$f":"IF(D184>=1000, D184/1000&\" MΩ\", D184&\" kΩ\")","v":"80.6 kΩ"},{"$f":"IF(MODE_UVLO=1, IF(D184<1, D184*1000&\"Ω\", IF(D184<1000, D184&\"kΩ\", D184/1000&\"MΩ\")), \"\")","v":"80.6kΩ"},null,null,{"$f":"IF(MODE_UVLO=1, IF(D184<1, D184*1000, IF(D184<1000, D184, D184/1000)), \"\")","v":80.600000000000009},{"$f":"IF(MODE_UVLO=1, IF(D184<1, \"Ω\", IF(D184<1000,\"kΩ\", \"MΩ\")), \"\")","v":"kΩ"},{"$f":"IF(MODE_UVLO=1, IF(D184<1, D184*1000, IF(D184<1000, D184&\"k\", D184/1000&\"M\")), \"\")","v":"80.6k"}]
[{"$f":"\"RHYS = \"&C277","v":{"$error":"#REF!"}},{"$f":"IF(#REF!<1000,#REF!& \" kΩ\",#REF!& \" MΩ\")","v":{"$error":"#REF!"}},{"$f":"IF(MODE_UVLO=1, IF(#REF!<1,#REF!* 1000&\"Ω\", IF(#REF!<1000,#REF!& \"kΩ\",#REF!/ 1000&\"MΩ\")), \"\")","v":{"$error":"#REF!"}},null,null,{"$f":"IF(MODE_UVLO=1, IF(#REF!<1,#REF!* 1000, IF(#REF!<1000,#REF!,#REF!/ 1000)), \"\")","v":{"$error":"#REF!"}},{"$f":"IF(MODE_UVLO=1, IF(#REF!<1, \"Ω\", IF(#REF!<1000,\"kΩ\", \"MΩ\")), \"\")","v":{"$error":"#REF!"}},{"$f":"IF(MODE_UVLO=1, IF(#REF!<1,#REF!* 1000, IF(#REF!<1000,#REF!& \"k\",#REF!& \"M\")), \"\")","v":{"$error":"#REF!"}}]
[]
[{"$f":"\"Css = \"&Css*1000000000&\"nF\"","v":{"$error":"#NAME?"}},{"$f":"Css*1000000000&\"nF\"","v":{"$error":"#NAME?"}}]
["Cbst",{"$f":"\"2.2nF\"","v":"2.2nF"},null,{"$f":"B280","v":"2.2nF"}]
[]
[]
["Rset resistor ref des?",{"$f":"IF(MODE_RSET=2, \"YES\", \"NO\")","v":"NO"},{"$f":"IF(MODE_RSET=2, \"R3\", \"\")","v":""},null,null,{"$f":"MODE_RSET","v":1}]
["Rset",{"$f":"IF(MODE_RSET=2, C284&\"kΩ\", \"\")","v":""},{"$f":"IF(MODE_ILIM=3,100,IF(MODE_ILIM=2,56.2,IF(MODE_ILIM=4,24.9,0)))","v":{"$error":"#REF!"}}]
[]
[]
["Rpgood","100kΩ"]
[]
["Cff / Cb?",{"$f":"IF(MODE=2, \"Cff\", IF(MODE=3,\"Cb\",\"\"))","v":"Cb"}]
[{"$f":"\"Cff / Cb=\"&B290","v":"Cff / Cb=56pF"},{"$f":"IF(OR(MODE=2,MODE=3),B141&\"pF\",\"\")","v":"56pF"}]
[]
["Ca?",{"$f":"IF(MODE=3, \"Ca\",\"\")","v":"Ca"},null,{"$f":"Ca","v":3.3000000000000002E-9},{"$f":"Ton_Vinmin","v":4.9386904130888018E-6}]
["Ca=",{"$f":"IF(MODE=3,B145&\"pF\",\"\")","v":"3300pF"}]
[]
["Ra?",{"$f":"IF(MODE=3, \"Ra\",\"\")","v":"Ra"},"Injected Ripple"]
["Ra=",{"$f":"IF(MODE=3,Ra&\"kΩ\",\"\")","v":"1000kΩ"},{"$f":"(VIN_nom-Vout)*Ton_Vin_nom/(Ra*Ca)/1000","v":1.9766899766899767E-2},{"$f":"ROUNDUP(1000*C296,0)","v":20},null,{"$f":"IF(MODE=3,Ra&\"k\",\"\")","v":"1000k"}]
[]
["Lf(emi)",{"$f":"M148&\"µH\"","v":"22µH"}]
["Cf(emi)",{"$f":"M149&\"µF\"","v":"4.7µF"}]
["Df(emi)",{"$f":"M150&\"µF\"","v":"10µF"}]
[]
["Full-load efficiency",{"$f":"ROUND(Efficiency!CE106,1)&\"%\"","v":"93%"}]
["Full-load efficiency",{"$f":"ROUND(Efficiency!CE107,1)&\"%\"","v":"93%"}]
["10% load efficiency",{"$f":"ROUND(Efficiency!CE16,1)&\"%\"","v":"92.7%"},"linear scale only"]
["1% load efficiency",{"$f":"ROUND(Efficiency!CE56,1)&\"%\"","v":"92.7%"},"log scale only"]
[]
["Blank out",{"$f":"IF(C307=\"y\",\"\",\"|\")","v":"|"},"n"]
[]
["OUTPUT CURRENT",{"$f":"'Design Converter'!$E$10&\"A\"","v":"0.5A"}]
[]
["VIN ",2]
["RT",5]
["EN",7]
["PGOOD",6]
["SS",4]
["ILIM",3]
["GND",10]
["FB",8]
["SW",1]
["HYS",9]

{"sheet":"Standard Value Calculator","index":8,"n_rows":159,"n_cols":11,"rows_kept":159,"cut":false,"hidden":true,"merged":[]}
[]
["Capacitors","Css","Cout","Cin","Cb"]
["Inputs",{"$f":"Css","v":{"$error":"#NAME?"}},{"$f":"Cout","v":4.3999999999999999E-5},{"$f":"Cin","v":1.0000000000000001E-5},{"$f":"Cb","v":0},null,null,"Resistors","inputs","Standard Result"]
["Standard Result",{"$f":"SUM(B6:B158)/1000000000000","v":{"$error":"#NAME?"}},{"$f":"SUM(C6:C158)/1000000000000","v":4.6999999999999997E-5},{"$f":"SUM(D6:D158)/1000000000000","v":1.0000000000000001E-5},{"$f":"IF(E3=\"OPEN\",\"OPEN\",SUM(E6:E158)/1000000000000)","v":0},null,null,"Rt",{"$f":"Rt","v":200000},{"$f":"IF(I4>(INT(0.5+100*POWER(10,IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))/96))*POWER(10,INT(LOG(I4))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))+1)/96))*POWER(10,INT(LOG(I4))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))+1)/96))*POWER(10,INT(LOG(I4))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))/96))*POWER(10,INT(LOG(I4))-2))","v":200000},"Ω"]
["(pF)"]
[0.47,{"$f":"IF(IF((B$3*10^12-$A7)*(B$3*10^12-$A6)*-1<0,0,1)*IF(ABS(B$3*10^12-$A7)>(B$3*10^12-$A6),$A6,$A7)=B7,0,IF((B$3*10^12-$A7)*(B$3*10^12-$A6)*-1<0,0,1)*IF(ABS(B$3*10^12-$A7)>(B$3*10^12-$A6),$A6,$A7))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A7)*(C$3*10^12-$A6)*-1<0,0,1)*IF(ABS(C$3*10^12-$A7)>(C$3*10^12-$A6),$A6,$A7)=C7,0,IF((C$3*10^12-$A7)*(C$3*10^12-$A6)*-1<0,0,1)*IF(ABS(C$3*10^12-$A7)>(C$3*10^12-$A6),$A6,$A7))","v":0},{"$f":"IF(IF((D$3*10^12-$A7)*(D$3*10^12-$A6)*-1<0,0,1)*IF(ABS(D$3*10^12-$A7)>(D$3*10^12-$A6),$A6,$A7)=D7,0,IF((D$3*10^12-$A7)*(D$3*10^12-$A6)*-1<0,0,1)*IF(ABS(D$3*10^12-$A7)>(D$3*10^12-$A6),$A6,$A7))","v":0},{"$f":"IF(IF((E$3*10^12-$A7)*(E$3*10^12-$A6)*-1<0,0,1)*IF(ABS(E$3*10^12-$A7)>(E$3*10^12-$A6),$A6,$A7)=E7,0,IF((E$3*10^12-$A7)*(E$3*10^12-$A6)*-1<0,0,1)*IF(ABS(E$3*10^12-$A7)>(E$3*10^12-$A6),$A6,$A7))","v":0},null,null,"Rshunt",{"$f":"Rshunt","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},"Ω"]
[0.56000000000000005,{"$f":"IF(IF((B$3*10^12-$A8)*(B$3*10^12-$A7)*-1<0,0,1)*IF(ABS(B$3*10^12-$A8)>(B$3*10^12-$A7),$A7,$A8)=B8,0,IF((B$3*10^12-$A8)*(B$3*10^12-$A7)*-1<0,0,1)*IF(ABS(B$3*10^12-$A8)>(B$3*10^12-$A7),$A7,$A8))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A8)*(C$3*10^12-$A7)*-1<0,0,1)*IF(ABS(C$3*10^12-$A8)>(C$3*10^12-$A7),$A7,$A8)=C8,0,IF((C$3*10^12-$A8)*(C$3*10^12-$A7)*-1<0,0,1)*IF(ABS(C$3*10^12-$A8)>(C$3*10^12-$A7),$A7,$A8))","v":0},{"$f":"IF(IF((D$3*10^12-$A8)*(D$3*10^12-$A7)*-1<0,0,1)*IF(ABS(D$3*10^12-$A8)>(D$3*10^12-$A7),$A7,$A8)=D8,0,IF((D$3*10^12-$A8)*(D$3*10^12-$A7)*-1<0,0,1)*IF(ABS(D$3*10^12-$A8)>(D$3*10^12-$A7),$A7,$A8))","v":0},{"$f":"IF(IF((E$3*10^12-$A8)*(E$3*10^12-$A7)*-1<0,0,1)*IF(ABS(E$3*10^12-$A8)>(E$3*10^12-$A7),$A7,$A8)=E8,0,IF((E$3*10^12-$A8)*(E$3*10^12-$A7)*-1<0,0,1)*IF(ABS(E$3*10^12-$A8)>(E$3*10^12-$A7),$A7,$A8))","v":0},null,null,"Rc1ea",{"$f":"Rcea1","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},"Ω"]
[0.68,{"$error":"#NAME?"},0,0,0]
[0.82,{"$error":"#NAME?"},0,0,0,null,null,"Rfb1",{"$f":"Rfb1_","v":453000},453000,"Ω"]
[1,{"$error":"#NAME?"},0,0,0,null,null,"Rfb2",{"$f":"Rfb2_","v":50333.333333333328},{"$f":"IF(I10=\"OPEN\",\"OPEN\",IF(I10>(INT(0.5+100*POWER(10,IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))/96))*POWER(10,INT(LOG(I10))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))+1)/96))*POWER(10,INT(LOG(I10))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))+1)/96))*POWER(10,INT(LOG(I10))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))/96))*POWER(10,INT(LOG(I10))-2)))","v":49900},"Ω"]
[1.2,{"$error":"#NAME?"},0,0,0]
[1.5,{"$error":"#NAME?"},0,0,0]
[1.8,{"$error":"#NAME?"},0,0,0,null,null,"Rs",{"$f":"Rs_ideal*1000","v":{"$error":"#NAME?"}},{"$f":"IF(I13=0,0,IF(I13>(INT(0.5+100*POWER(10,IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))/96))*POWER(10,INT(LOG(I13))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))+1)/96))*POWER(10,INT(LOG(I13))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))+1)/96))*POWER(10,INT(LOG(I13))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))/96))*POWER(10,INT(LOG(I13))-2)))","v":{"$error":"#NAME?"}},"mΩ"]
[2.2000000000000002,{"$f":"IF(IF((B$3*10^12-$A15)*(B$3*10^12-$A14)*-1<0,0,1)*IF(ABS(B$3*10^12-$A15)>(B$3*10^12-$A14),$A14,$A15)=B15,0,IF((B$3*10^12-$A15)*(B$3*10^12-$A14)*-1<0,0,1)*IF(ABS(B$3*10^12-$A15)>(B$3*10^12-$A14),$A14,$A15))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A15)*(C$3*10^12-$A14)*-1<0,0,1)*IF(ABS(C$3*10^12-$A15)>(C$3*10^12-$A14),$A14,$A15)=C15,0,IF((C$3*10^12-$A15)*(C$3*10^12-$A14)*-1<0,0,1)*IF(ABS(C$3*10^12-$A15)>(C$3*10^12-$A14),$A14,$A15))","v":0},{"$f":"IF(IF((D$3*10^12-$A15)*(D$3*10^12-$A14)*-1<0,0,1)*IF(ABS(D$3*10^12-$A15)>(D$3*10^12-$A14),$A14,$A15)=D15,0,IF((D$3*10^12-$A15)*(D$3*10^12-$A14)*-1<0,0,1)*IF(ABS(D$3*10^12-$A15)>(D$3*10^12-$A14),$A14,$A15))","v":0},{"$f":"IF(IF((E$3*10^12-$A15)*(E$3*10^12-$A14)*-1<0,0,1)*IF(ABS(E$3*10^12-$A15)>(E$3*10^12-$A14),$A14,$A15)=E15,0,IF((E$3*10^12-$A15)*(E$3*10^12-$A14)*-1<0,0,1)*IF(ABS(E$3*10^12-$A15)>(E$3*10^12-$A14),$A14,$A15))","v":0},null,null,"Cslope_ideal",{"$f":"Cslope_ideal","v":{"$error":"#NAME?"}},{"$f":"#REF!*1000000000000","v":{"$error":"#REF!"}},"pF"]
[2.7,{"$error":"#NAME?"},0,0,0]
[3.3,{"$error":"#NAME?"},0,0,0,null,null,"Ruv1",{"$f":"Ruvlo1","v":1000},{"$f":"IF(I16=\"OPEN\",\"OPEN\",IF(I16>(INT(0.5+100*POWER(10,IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))/96))*POWER(10,INT(LOG(I16))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))+1)/96))*POWER(10,INT(LOG(I16))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))+1)/96))*POWER(10,INT(LOG(I16))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))/96))*POWER(10,INT(LOG(I16))-2)))","v":1000},"kΩ"]
[3.9,{"$error":"#NAME?"},0,0,0,null,null,"Ruv2",{"$f":"Ruvlo2","v":81.081081081081081},{"$f":"IF(I17=\"OPEN\",\"OPEN\",IF(I17>(INT(0.5+100*POWER(10,IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))/96))*POWER(10,INT(LOG(I17))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))+1)/96))*POWER(10,INT(LOG(I17))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))+1)/96))*POWER(10,INT(LOG(I17))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))/96))*POWER(10,INT(LOG(I17))-2)))","v":80.600000000000009},"kΩ"]
[4.7,{"$error":"#NAME?"},0,0,0,null,null,"Rhys",{"$f":"Rhys","v":{"$error":"#NAME?"}},{"$f":"IF(I18=\"OPEN\",\"OPEN\",IF(I18>(INT(0.5+100*POWER(10,IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))/96))*POWER(10,INT(LOG(I18))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))+1)/96))*POWER(10,INT(LOG(I18))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))+1)/96))*POWER(10,INT(LOG(I18))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))/96))*POWER(10,INT(LOG(I18))-2)))","v":{"$error":"#NAME?"}},"kΩ"]
[5.6,{"$error":"#NAME?"},0,0,0]
[6.8,{"$error":"#NAME?"},0,0,0,null,null,"Ra",{"$f":"'Variable Mgmt'!D147","v":988.34498834498834},{"$f":"IF(I20=\"OPEN\",\"OPEN\",IF(I20>(INT(0.5+100*POWER(10,IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))/96))*POWER(10,INT(LOG(I20))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))+1)/96))*POWER(10,INT(LOG(I20))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))+1)/96))*POWER(10,INT(LOG(I20))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))/96))*POWER(10,INT(LOG(I20))-2)))","v":1000},"kΩ"]
[8.1999999999999993,{"$error":"#NAME?"},0,0,0]
[10,{"$error":"#NAME?"},0,0,0]
[12,{"$error":"#NAME?"},0,0,0]
[15,{"$error":"#NAME?"},0,0,0]
[18,{"$error":"#NAME?"},0,0,0]
[22,{"$error":"#NAME?"},0,0,0]
[27,{"$error":"#NAME?"},0,0,0]
[33,{"$error":"#NAME?"},0,0,0]
[39,{"$error":"#NAME?"},0,0,0]
[47,{"$error":"#NAME?"},0,0,0]
[56,{"$error":"#NAME?"},0,0,0]
[68,{"$error":"#NAME?"},0,0,0]
[82,{"$error":"#NAME?"},0,0,0]
[{"$f":"A22*10","v":100},{"$error":"#NAME?"},0,0,0]
[{"$f":"A23*10","v":120},{"$error":"#NAME?"},0,0,0]
[150,{"$error":"#NAME?"},0,0,0]
[180,{"$error":"#NAME?"},0,0,0]
[220,{"$error":"#NAME?"},0,0,{"$f":"IF(IF((E$3*10^12-$A39)*(E$3*10^12-$A38)*-1<0,0,1)*IF(ABS(E$3*10^12-$A39)>(E$3*10^12-$A38),$A38,$A39)=E39,0,IF((E$3*10^12-$A39)*(E$3*10^12-$A38)*-1<0,0,1)*IF(ABS(E$3*10^12-$A39)>(E$3*10^12-$A38),$A38,$A39))","v":0}]
[270,{"$error":"#NAME?"},0,0,0]
[330,{"$error":"#NAME?"},0,0,0]
[390,{"$error":"#NAME?"},0,0,0]
[470,{"$error":"#NAME?"},0,0,0]
[560,{"$error":"#NAME?"},0,0,0]
[680,{"$error":"#NAME?"},0,0,0]
[{"$f":"A33*10","v":820},{"$error":"#NAME?"},0,0,0]
[1000,{"$error":"#NAME?"},0,0,0]
[1200,{"$error":"#NAME?"},0,0,0]
[1500,{"$error":"#NAME?"},0,0,0]
[1800,{"$error":"#NAME?"},0,0,0]
[2200,{"$error":"#NAME?"},0,0,0]
[2700,{"$error":"#NAME?"},0,0,0]
[3300,{"$error":"#NAME?"},0,0,0]
[3900,{"$error":"#NAME?"},0,0,0]
[4700,{"$error":"#NAME?"},0,0,0]
[5600,{"$error":"#NAME?"},0,0,0]
[6800,{"$error":"#NAME?"},0,0,0]
[8200,{"$error":"#NAME?"},0,0,0]
[10000,{"$error":"#NAME?"},0,0,0]
[12000,{"$error":"#NAME?"},0,0,0]
[15000,{"$error":"#NAME?"},0,0,0]
[18000,{"$error":"#NAME?"},0,0,0]
[22000,{"$error":"#NAME?"},0,0,0]
[27000,{"$error":"#NAME?"},0,0,0]
[33000,{"$error":"#NAME?"},0,0,0]
[39000,{"$error":"#NAME?"},0,0,0]
[47000,{"$error":"#NAME?"},0,0,0]
[56000,{"$error":"#NAME?"},0,0,0]
[68000,{"$error":"#NAME?"},0,0,0]
[82000,{"$error":"#NAME?"},0,0,0]
[100000,{"$error":"#NAME?"},{"$f":"IF(IF((C$3*10^12-$A71)*(C$3*10^12-$A70)*-1<0,0,1)*IF(ABS(C$3*10^12-$A71)>(C$3*10^12-$A70),$A70,$A71)=C71,0,IF((C$3*10^12-$A71)*(C$3*10^12-$A70)*-1<0,0,1)*IF(ABS(C$3*10^12-$A71)>(C$3*10^12-$A70),$A70,$A71))","v":0},{"$f":"IF(IF((D$3*10^12-$A71)*(D$3*10^12-$A70)*-1<0,0,1)*IF(ABS(D$3*10^12-$A71)>(D$3*10^12-$A70),$A70,$A71)=D71,0,IF((D$3*10^12-$A71)*(D$3*10^12-$A70)*-1<0,0,1)*IF(ABS(D$3*10^12-$A71)>(D$3*10^12-$A70),$A70,$A71))","v":0},{"$f":"IF(IF((E$3*10^12-$A71)*(E$3*10^12-$A70)*-1<0,0,1)*IF(ABS(E$3*10^12-$A71)>(E$3*10^12-$A70),$A70,$A71)=E71,0,IF((E$3*10^12-$A71)*(E$3*10^12-$A70)*-1<0,0,1)*IF(ABS(E$3*10^12-$A71)>(E$3*10^12-$A70),$A70,$A71))","v":0}]
[120000,{"$f":"IF(IF((B$3*10^12-$A72)*(B$3*10^12-$A71)*-1<0,0,1)*IF(ABS(B$3*10^12-$A72)>(B$3*10^12-$A71),$A71,$A72)=B72,0,IF((B$3*10^12-$A72)*(B$3*10^12-$A71)*-1<0,0,1)*IF(ABS(B$3*10^12-$A72)>(B$3*10^12-$A71),$A71,$A72))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A72)*(C$3*10^12-$A71)*-1<0,0,1)*IF(ABS(C$3*10^12-$A72)>(C$3*10^12-$A71),$A71,$A72)=C72,0,IF((C$3*10^12-$A72)*(C$3*10^12-$A71)*-1<0,0,1)*IF(ABS(C$3*10^12-$A72)>(C$3*10^12-$A71),$A71,$A72))","v":0},{"$f":"IF(IF((D$3*10^12-$A72)*(D$3*10^12-$A71)*-1<0,0,1)*IF(ABS(D$3*10^12-$A72)>(D$3*10^12-$A71),$A71,$A72)=D72,0,IF((D$3*10^12-$A72)*(D$3*10^12-$A71)*-1<0,0,1)*IF(ABS(D$3*10^12-$A72)>(D$3*10^12-$A71),$A71,$A72))","v":0},0]
[150000,{"$error":"#NAME?"},0,0,0]
[180000,{"$error":"#NAME?"},0,0,0]
[220000,{"$error":"#NAME?"},0,0,0]
[270000,{"$error":"#NAME?"},0,0,0]
[330000,{"$error":"#NAME?"},0,0,0]
[390000,{"$error":"#NAME?"},0,0,0]
[470000,{"$error":"#NAME?"},0,0,0]
[560000,{"$error":"#NAME?"},0,0,0]
[680000,{"$error":"#NAME?"},0,0,0]
[820000,{"$error":"#NAME?"},0,0,0]
[1000000,{"$error":"#NAME?"},0,0,0]
[1200000,{"$error":"#NAME?"},0,0,0]
[1500000,{"$error":"#NAME?"},0,0,0]
[1800000,{"$error":"#NAME?"},0,0,0]
[2200000,{"$error":"#NAME?"},0,0,0]
[2700000,{"$error":"#NAME?"},0,0,0]
[3300000,{"$error":"#NAME?"},0,0,0]
[3900000,{"$error":"#NAME?"},0,0,0]
[4700000,{"$error":"#NAME?"},0,0,0]
[5600000,{"$error":"#NAME?"},0,0,0]
[6800000,{"$error":"#NAME?"},0,0,0]
[8200000,{"$error":"#NAME?"},0,0,0]
[10000000,{"$error":"#NAME?"},0,10000000,0]
[12000000,{"$error":"#NAME?"},0,0,0]
[15000000,{"$error":"#NAME?"},0,0,0]
[18000000,{"$error":"#NAME?"},0,0,0]
[22000000,{"$error":"#NAME?"},0,0,0]
[{"$f":"A87*10","v":27000000},{"$error":"#NAME?"},0,0,0]
[33000000,{"$error":"#NAME?"},0,0,0]
[39000000,{"$error":"#NAME?"},47000000,0,0]
[47000000,{"$error":"#NAME?"},0,0,{"$f":"IF(IF((E$3*10^12-$A103)*(E$3*10^12-$A102)*-1<0,0,1)*IF(ABS(E$3*10^12-$A103)>(E$3*10^12-$A102),$A102,$A103)=E103,0,IF((E$3*10^12-$A103)*(E$3*10^12-$A102)*-1<0,0,1)*IF(ABS(E$3*10^12-$A103)>(E$3*10^12-$A102),$A102,$A103))","v":0}]
[56000000,{"$error":"#NAME?"},0,{"$f":"IF(IF((D$3*10^12-$A104)*(D$3*10^12-$A103)*-1<0,0,1)*IF(ABS(D$3*10^12-$A104)>(D$3*10^12-$A103),$A103,$A104)=D104,0,IF((D$3*10^12-$A104)*(D$3*10^12-$A103)*-1<0,0,1)*IF(ABS(D$3*10^12-$A104)>(D$3*10^12-$A103),$A103,$A104))","v":0},0]
[68000000,{"$error":"#NAME?"},0,0,0]
[82000000,{"$error":"#NAME?"},0,0,0]
[100000000,{"$error":"#NAME?"},0,0,0]
[120000000,{"$error":"#NAME?"},0,0,0]
[150000000,{"$error":"#NAME?"},0,0,0]
[180000000,{"$error":"#NAME?"},0,0,0]
[220000000,{"$error":"#NAME?"},0,0,0]
[270000000,{"$error":"#NAME?"},0,0,0]
[330000000,{"$error":"#NAME?"},0,0,0]
[390000000,{"$error":"#NAME?"},0,0,0]
[470000000,{"$error":"#NAME?"},0,0,0]
[560000000,{"$error":"#NAME?"},0,0,0]
[680000000,{"$error":"#NAME?"},0,0,0]
[820000000,{"$error":"#NAME?"},0,0,0]
[1000000000,{"$error":"#NAME?"},0,0,0]
[1200000000,{"$error":"#NAME?"},0,0,0]
[1500000000,{"$error":"#NAME?"},0,0,0]
[1800000000,{"$error":"#NAME?"},0,0,0]
[2200000000,{"$error":"#NAME?"},0,0,0]
[2700000000,{"$error":"#NAME?"},0,0,0]
[3300000000,{"$error":"#NAME?"},0,0,0]
[3900000000,{"$error":"#NAME?"},0,0,0]
[4700000000,{"$error":"#NAME?"},0,0,0]
[5600000000,{"$error":"#NAME?"},0,0,0]
[6800000000,{"$error":"#NAME?"},0,0,0]
[8200000000,{"$error":"#NAME?"},0,0,0]
[10000000000,{"$error":"#NAME?"},0,0,0]
[12000000000,{"$error":"#NAME?"},0,0,0]
[15000000000,{"$error":"#NAME?"},0,0,0]
[18000000000,{"$error":"#NAME?"},0,0,0]
[22000000000,{"$error":"#NAME?"},{"$f":"IF(IF((C$3*10^12-$A135)*(C$3*10^12-$A134)*-1<0,0,1)*IF(ABS(C$3*10^12-$A135)>(C$3*10^12-$A134),$A134,$A135)=C135,0,IF((C$3*10^12-$A135)*(C$3*10^12-$A134)*-1<0,0,1)*IF(ABS(C$3*10^12-$A135)>(C$3*10^12-$A134),$A134,$A135))","v":0},0,{"$f":"IF(IF((E$3*10^12-$A135)*(E$3*10^12-$A134)*-1<0,0,1)*IF(ABS(E$3*10^12-$A135)>(E$3*10^12-$A134),$A134,$A135)=E135,0,IF((E$3*10^12-$A135)*(E$3*10^12-$A134)*-1<0,0,1)*IF(ABS(E$3*10^12-$A135)>(E$3*10^12-$A134),$A134,$A135))","v":0}]
[27000000000,{"$f":"IF(IF((B$3*10^12-$A136)*(B$3*10^12-$A135)*-1<0,0,1)*IF(ABS(B$3*10^12-$A136)>(B$3*10^12-$A135),$A135,$A136)=B136,0,IF((B$3*10^12-$A136)*(B$3*10^12-$A135)*-1<0,0,1)*IF(ABS(B$3*10^12-$A136)>(B$3*10^12-$A135),$A135,$A136))","v":{"$error":"#NAME?"}},0,0,0]
[33000000000,{"$error":"#NAME?"},0,0,0]
[39000000000,{"$error":"#NAME?"},0,0,0]
[47000000000,{"$error":"#NAME?"},0,0,0]
[56000000000,{"$error":"#NAME?"},0,0,0]
[68000000000,{"$error":"#NAME?"},0,0,0]
[82000000000,{"$error":"#NAME?"},0,0,0]
[100000000000,{"$error":"#NAME?"},0,0,0]
[120000000000,{"$error":"#NAME?"},0,0,0]
[150000000000,{"$error":"#NAME?"},0,0,0]
[180000000000,{"$error":"#NAME?"},0,0,0]
[220000000000,{"$error":"#NAME?"},0,0,0]
[270000000000,{"$error":"#NAME?"},0,0,0]
[330000000000,{"$error":"#NAME?"},0,0,0]
[390000000000,{"$error":"#NAME?"},0,0,0]
[470000000000,{"$error":"#NAME?"},0,0,0]
[560000000000,{"$error":"#NAME?"},0,0,0]
[680000000000,{"$error":"#NAME?"},0,0,0]
[820000000000,{"$error":"#NAME?"},0,0,0]
[1000000000000,{"$error":"#NAME?"},0,0,0]
[1200000000000,{"$error":"#NAME?"},0,0,0]
[1500000000000,{"$error":"#NAME?"},0,0,0]
[1800000000000,{"$error":"#NAME?"},0,0,0]
[2200000000000,{"$error":"#NAME?"},0,0,0]
[2700000000000,{"$error":"#NAME?"},2700000000000,2700000000000,2700000000000]

{"sheet":"Efficiency","index":9,"n_rows":114,"n_cols":88,"rows_kept":114,"cut":false,"hidden":true,"merged":[[0,0,2,4],[1,6,1,7],[3,0,3,4],[3,10,3,21]]}
["LM5164 (COT) Efficiency Calculator"]
[null,null,null,null,null,null,"TERMS OF USE",null,null,{"$f":"CoutEsr","v":5.0000000000000001E-3}]
[]
[null,null,null,null,null,null,null,"Currents",null,null,"Miscellaneous",null,null,null,null,null,null,null,null,null,null,null,"Inductor",null,null,null,"Cout",null,null,"Cin",null,null,"High-side MOSFET Losses ",null,null,null,null,null,null,null,null,"Low-side MOSFET Losses ",null,null,"Diode",null,null,null,null,null,null,null,"RESULTS"]
["Input Parameters",null,null,null,null,null,null,"Step","Iout (A)","Ripple Current pk-pk (A)","Peak Current (A)","Valley Current (A)","VOUT Hysteresis +Undershoot (2us Delay) (mV)","Vout Rise per Pulse (mV)","Number of Pulses in DCM","VOUT Ripple (mV)","Off Time (sec)","Duty Cycle","Switching Frequency (Hz)","Active Mode Duration (sec)","Sleep Mode Duration (sec)","Operating Quiescent Current (A)","Irms (A)","Inductor DCR Loss @ 25°C (W)","Inductor Core Loss  (W)","Total Inductor Loss (W)","Irms (A)","Cout ESR Loss (W)","Total Cout Loss (W)","Irms (A)","Cin ESR Loss (W)","Total Cin Loss (W)","Irms (A)","Rdson HS Loss @ 25°C (W)","HS Gate Qg Loss (W)     ","SW Rise Time (ns)","SW Fall Time (ns)","HS Switching  Loss (W)","Coss Loss (W)","Total HS FET AC Loss (W)","Total HS FET Loss (W)","Irms (A)","Rdson LS Loss @ 25°C (W)","LS Gate Qg Loss (W)","Reverse Recovery & Leakage Losses","DeadTime Loss @ 25°C (W)","Total LS FET AC Loss (W)","Total LS FET Loss (W)","Quiescent Loss (W)","LDO + Quiescent Loss (W)","Total Gate Drive Loss (W)","Total Power Loss in IC (W)","Total Converter Power Loss (W)","Pout (W)","EFF (%)","High-side MOSFET Rdson %","Low-side MOSFET Rdson %","Gate Drive (Qg) Loss from Vin %","High-side MOSFET AC Loss %","Reverse Recovery & Leakage Loss %","Deadtime Loss %","Low-side MOSFET AC Loss %","Inductor Cu Loss %","Inductor Core Loss %","Cin ESR %","Cout ESR %","LDO + Quiescent Current Loss %","Total Loss %","Overall Eff %","Overall Eff","Current (mA)","Keep for \"previous\" data series","Keep for \"previous\" data series","Frequency (kHz)",null,"Coss",null,"Total Power Loss in IC (mW)","LDO + Quiescent Loss (mW)","Total Inductor Loss (mW)",null,null,"Overall Eff","Total Power Loss in IC (W)","LDO + Quiescent Loss (mW)","Total Inductor Loss (mW)","Fsw (kHz)","Ripple (mV)"]
["Design","Input Value","Units","Std Units","Description",null,null,0.04,{"$f":"IF(PLOT_TYPE=1, H6/100*Iout, min_I*EXP(H6*rr/100))","v":2.0000000000000001E-4},{"$f":"IF(I6<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I6-Vout)/L*OnTime)","v":0.95232360099097058},{"$f":"IF(I6<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I6+((Vin-(Rdcr+RdsonTop)*J6-Vout)/L*OnTime)/2)","v":0.95232360099097058},{"$f":"IF(I6<Icrit, 0, I6-((Vin-(Rdcr+RdsonTop)*K6-Vout)/L*OnTime)/2)","v":0},{"$f":"1000*((((J6/2)-I6)*0.000002/Cout+Vout/306))","v":60.85031356975913},{"$f":"IF(I6<Icrit, 1000*SQRT((J6*CoutEsr)^2+(((J6/2)-I6)*(OnTime+OffTime)/Cout)^2), 1000*J6*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":70.814995211768547},{"$f":"ROUNDUP(M6/N6,0)","v":1},{"$f":"IF(I6<Icrit, 1000*((N6/1000)*O6), 1000*J6*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":70.814995211768547},{"$f":"IF(I6<Icrit, L*J6/(Vout+J6/2*(RdsonBot+Rdcr)), L*J6/(Vout+I6*(RdsonBot+Rdcr)))","v":5.3072098708103659E-6},{"$f":"OnTime*S6","v":7.9069418750917403E-5},{"$f":"IF(I6<Icrit,I6/((OnTime+Q6)*J6/2),1/(OnTime+Q6))","v":64.243902735120386},{"$f":"IF(1/S6-OnTime-Q6>Tsleep, OnTime+Q6+Tsleep, 1/S6)","v":1.1537979101579597E-5},{"$f":"IF(1/S6-OnTime-Q6>Tsleep, 1/S6-OnTime-Q6-Tsleep, 0)","v":1.5554141523948403E-2},{"$f":"S6*(T6*Iq_active+U6*Iq_sleep)","v":1.0481809124655128E-5},{"$f":"IF(I6<Icrit,Iripple*SQRT((OnTime+OffTime)*S6/3), SQRT(I6^2+Iripple^2/12))","v":1.1258766073143675E-2},{"$f":"W6^2*Rdcr","v":1.5211177618772525E-5},{"$f":"Core_Loss/1000*S6/$S$106","v":4.19617624068034E-5},{"$f":"(Y6+X6*(1+Ltc*(Ta-25)))/(1-X6*Ltc*ThetaCa)","v":5.7173079172753893E-5},{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q6)*S6)","v":5.6321169186234806E-3},{"$f":"RCoutEsr*AA6^2","v":1.5860370492522425E-7},{"$f":"AB6","v":1.5860370492522425E-7},{"$f":"SQRT($R6)*SQRT($I6^2*(1-R6)+(Iripple^2)/12)","v":2.4436462035843983E-3},{"$f":"RCinEsr*AD6^2","v":1.7914220304877328E-8},{"$f":"AE6","v":1.7914220304877328E-8},{"$f":"IF(I6<Icrit,Iripple*SQRT((OnTime)*S6/3), SQRT(OnTime*S6*(I6^2+Iripple^2/12)))","v":4.8872911129850946E-3},{"$f":"RdsonTop*AG6^2","v":1.6409417108644341E-5},{"$f":"QgTop*S6*Vdd","v":2.5793926948150836E-7},{"$f":"20*VIN_nom/24","v":54.166666666666664},{"$f":"IF(I6<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I6+Iripple/2)*1000000000)","v":10.924681300086506},{"$f":"IF(I6<Icrit, Vin*(I6+Iripple/2)*AK6/1000000000/2*S6, Vin*(I6-Iripple/2)*AJ6/1000000000/2*S6 + Vin*(I6+Iripple/2)*AK6/1000000000/2*S6)","v":1.08617815492939E-5},{"$f":"IF(I6<Icrit, Csw*(Vin)^2*S6/2, Csw*Vin^2*S6/2)","v":2.1714439124470689E-5},{"$f":"AI6+AL6+AM6","v":3.2834159943246098E-5},{"$f":"(AI6+AL6+AM6+AH6*(1+RdsonTopTc*(Ta-25)))/(1-AH6*RdsonTopTc*ThetaJA)","v":4.9243726502744312E-5},{"$f":"IF(I6<Icrit,Iripple*SQRT((OffTime)*S6/3), SQRT(OffTime*S6*(I6^2+Iripple^2/12)))","v":1.0142691904356948E-2},{"$f":"RdsonBot*AP6^2","v":3.1273756516279217E-5},{"$f":"QgBot*S6*Vdd","v":7.0668293008632426E-7},{"$f":"IF(I6<Icrit, Vin*Idss*R6, QrrBot*(I6-Iripple/2)/1*S6*Vin+Vin*Idss*R6)","v":0},{"$f":"IF(I6<Icrit, dead1*S6*(I6+Iripple/2)*((I6+Iripple/2)*BDserR+VSD), dead1*S6*(I6+Iripple/2)*((I6+Iripple/2)*BDserR+VSD)+dead2*S6*(I6-Iripple/2)*((I6-Iripple/2)*BDserR+VSD))","v":5.1860825139070143E-7},{"$f":"AR6+AS6+AT6","v":1.2252911814770257E-6},{"$f":"(AR6+AS6+AT6+AQ6*(1+RdsonBotTc*(Ta-25)))/(1-AQ6*RdsonBotTc*ThetaJA)","v":3.2499235675976532E-5},{"$f":"Vin*V6+Vout*Ifb/0.8","v":1.0392416336673079E-3},{"$f":"(Vin-Vdd)*(S6*QgBot+S6*QgTop)+AW6","v":1.0508171000621219E-3},{"$f":"AI6+AR6","v":9.6462219956783268E-7},{"$f":"AO6+AV6+AX6+AY6","v":1.1335246844404107E-3},{"$f":"SUM(Z6,AC6,AF6,AZ6)","v":1.1908742815383948E-3},{"$f":"Vout*I6","v":2.4000000000000002E-3},{"$f":"BB6/(BB6+BA6)","v":0.66836090930251035},{"$f":"(AO6-AN6)/($BB6+$BA6)","v":4.5697970112359553E-3},{"$f":"(AV6-AU6)/($BB6+$BA6)","v":8.7092841582583017E-3},{"$f":"Vin*S6*(QgBot+QgTop)/($BB6+$BA6)","v":3.492210423197948E-3},{"$f":"AN6/($BB6+$BA6)","v":9.1437787482716755E-3},{"$f":"AS6/(BA6+BB6)","v":0},{"$f":"AT6/($BB6+$BA6)","v":1.4442395102969751E-4},{"$f":"AU6/($BB6+$BA6)","v":3.4122363675513834E-4},{"$f":"X6/($BB6+$BA6)","v":4.2360652103519986E-3},{"$f":"Y6/($BB6+$BA6)","v":1.1685667365894589E-2},{"$f":"(AF6)/($BB6+$BA6)","v":4.988818571838877E-6},{"$f":"(AC6)/($BB6+$BA6)","v":4.4168548517737458E-5},{"$f":"AX6/($BB6+$BA6)","v":0.29263544687839449},{"$f":"SUM(BD6:BO6)","v":0.33500705475047937},{"$f":"BC6","v":0.66836090930251035},{"$f":"100*BQ6","v":66.836090930251032},{"$f":"I6*1000","v":0.2},8.7924221262065743,{"$f":"BT6/100","v":8.7924221262065741E-2},{"$f":"S6/1000","v":6.4243902735120387E-2},null,{"$f":"AM6/($BB6+$BA6)","v":6.0471176159271811E-3},null,{"$f":"AZ6","v":1.1335246844404107E-3},{"$f":"AX6","v":1.0508171000621219E-3},{"$f":"Z6","v":5.7173079172753893E-5},null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR6, IF(MODE_ILIM=4,#REF!,#REF!))","v":66.836090930251032},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ6, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1335246844404107E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA6, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0508171000621219E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB6, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.7173079172753893E-5},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S6, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":6.4243902735120387E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P6, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.814995211768547}]
[null,null,null,null,null,null,null,1,5.0000000000000001E-3,0.95232360099097058,0.95232360099097058,0,{"$f":"IF(I7<Icrit, 1000*((((J7/2)-I7)*0.000002/Cout+Vout/306)), 1000*J7*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":60.632131751577319},70.104082368168022,{"$f":"ROUNDUP(M7/N7,0)","v":1},70.104082368168022,5.3072098708103659E-6,{"$f":"OnTime*S7","v":1.9767354687729348E-3},1606.0975683780096,{"$f":"IF(1/S7-OnTime-Q7>Tsleep, OnTime+Q7+Tsleep, 1/S7)","v":1.1537979101579597E-5},{"$f":"IF(1/S7-OnTime-Q7>Tsleep, 1/S7-OnTime-Q7-Tsleep, 0)","v":6.110892010204197E-4},2.2045228116378136E-5,{"$f":"IF(I7<Icrit,Iripple*SQRT((OnTime+OffTime)*S7/3), SQRT(I7^2+Iripple^2/12))","v":5.6293830365718375E-2},3.8027944046931312E-4,1.0490440601700849E-3,1.4294104727057601E-3,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q7)*S7)","v":2.8160584593117405E-2},{"$f":"RCoutEsr*AA7^2","v":3.965092623130607E-6},{"$f":"AB7","v":3.965092623130607E-6},{"$f":"SQRT($R7)*SQRT($I7^2*(1-R7)+(Iripple^2)/12)","v":1.2220245940396854E-2},{"$f":"RCinEsr*AD7^2","v":4.4800323253135733E-7},{"$f":"AE7","v":4.4800323253135733E-7},{"$f":"IF(I7<Icrit,Iripple*SQRT((OnTime)*S7/3), SQRT(OnTime*S7*(I7^2+Iripple^2/12)))","v":2.443645556492547E-2},{"$f":"RdsonTop*AG7^2","v":4.1023542771610841E-4},{"$f":"QgTop*S7*Vdd","v":6.4484817370377085E-6},54.166666666666664,10.924681300086506,2.7428173096748183E-4,5.4286097811176719E-4,{"$f":"AI7+AL7+AM7","v":8.2359119081628674E-4},1.2339202398150147E-3,5.0713459521784736E-2,{"$f":"RdsonBot*AP7^2","v":7.8184391290698043E-4},1.7667073252158109E-5,0,1.3103312782703695E-5,{"$f":"AR7+AS7+AT7","v":3.0770386034861804E-5},8.1273182161446854E-4,1.7908638681293034E-3,2.0802505279996532E-3,2.4115554989195817E-5,{"$f":"AO7+AV7+AX7+AY7","v":4.1510181444183326E-3},5.5848417129797543E-3,0.06,{"$f":"BB7/(BB7+BA7)","v":0.9148455410257631},{"$f":"(AO7-AN7)/($BB7+$BA7)","v":6.2564616804971366E-3},{"$f":"(AV7-AU7)/($BB7+$BA7)","v":1.1922898876568463E-2},4.7801017227659349E-3,{"$f":"AN7/($BB7+$BA7)","v":1.2557645475772974E-2},{"$f":"AS7/(BA7+BB7)","v":0},{"$f":"AT7/($BB7+$BA7)","v":1.9979178786537269E-4},{"$f":"AU7/($BB7+$BA7)","v":4.6916917432724558E-4},5.7982825076187215E-3,1.5995221346436078E-2,{"$f":"(AF7)/($BB7+$BA7)","v":6.83089599410734E-6},{"$f":"(AC7)/($BB7+$BA7)","v":6.0457455100419712E-5},{"$f":"AX7/($BB7+$BA7)","v":3.1718465329282873E-2},{"$f":"SUM(BD7:BO7)","v":8.9765326252229327E-2},0.9148455410257631,{"$f":"100*BQ7","v":91.484554102576311},5,9.5725635821403898,{"$f":"BT7/100","v":9.5725635821403893E-2},1.6060975683780097,null,8.27723242037391E-3,null,{"$f":"AZ7","v":4.1510181444183326E-3},{"$f":"AX7","v":2.0802505279996532E-3},{"$f":"Z7","v":1.4294104727057601E-3},null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR7, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.484554102576311},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ7, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.1510181444183326E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA7, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.0802505279996532E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB7, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.4294104727057601E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S7, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":1.6060975683780097},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P7, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.104082368168022}]
["Vin",{"$f":"Vin","v":65},"V",{"$f":"B8","v":65},"Vin",null,null,2,0.01,0.95232360099097058,0.95232360099097058,0,60.404859024304592,69.36358370395088,1,69.36358370395088,5.3072098708103659E-6,{"$f":"OnTime*S8","v":3.9534709375458697E-3},3212.1951367560191,1.1537979101579597E-5,2.9977561095942005E-4,3.4090456232756273E-5,7.9611498381129298E-2,7.6055888093862624E-4,2.0980881203401698E-3,2.8589949107139805E-3,3.982508065594146E-2,7.9301852462612139E-6,{"$f":"AB8","v":7.9301852462612139E-6},1.7290574437791181E-2,8.9689189316639355E-7,{"$f":"AE8","v":8.9689189316639355E-7},3.4558366876245097E-2,8.2047085543221715E-4,1.2896963474075417E-5,54.166666666666664,10.924681300086506,5.5426594575816001E-4,1.0857219562235344E-3,1.6528848654557698E-3,2.4737310998970267E-3,7.171966225056696E-2,1.5636878258139613E-3,3.5334146504316217E-5,0,2.6494662231231123E-5,6.182880873554734E-5,1.6259868765612197E-3,2.5738036956938822E-3,3.1525770154345817E-3,4.8231109978391634E-5,{"$f":"AO8+AV8+AX8+AY8","v":7.3005261018712206E-3},1.0168348089724628E-2,0.12,{"$f":"BB8/(BB8+BA8)","v":0.921883098011541},6.3060355799817794E-3,1.2016424044557307E-2,4.8168732178032947E-3,1.2698055170189619E-2,0,2.0354151082080596E-4,4.7499111452907841E-4,5.8428864781657625E-3,1.6118266469003387E-2,6.890245642113925E-6,6.0922531188572522E-5,2.4219228880906749E-2,8.2764115242788469E-2,0.921883098011541,{"$f":"100*BQ8","v":92.188309801154105},10,10.507357436577642,0.10507357436577643,3.2121951367560193,null,8.3409060048541886E-3,null,7.3005261018712206E-3,3.1525770154345817E-3,2.8589949107139805E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR8, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.188309801154105},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ8, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.3005261018712206E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA8, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.1525770154345817E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB8, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.8589949107139805E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S8, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":3.2121951367560193},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P8, IF(MODE_ILIM=4,#REF!,#REF!))","v":69.36358370395088}]
["Vout",{"$f":"Vout","v":12},"V",{"$f":"B9","v":12},"Vout",null,null,3,1.4999999999999999E-2,0.95232360099097058,0.95232360099097058,0,60.177586297031866,68.62312247166517,1,68.62312247166517,5.3072098708103659E-6,5.9302064063188045E-3,4818.2927051340284,1.1537979101579597E-5,1.9600441427242014E-4,4.61356843491344E-5,9.7503774346087896E-2,1.1408383214079395E-3,3.1471321805102547E-3,4.288753345785064E-3,4.8775563286120684E-2,1.189527786939182E-5,1.189527786939182E-5,2.1193906063313336E-2,1.3475449626616495E-6,1.3475449626616495E-6,4.2325182595350154E-2,1.2307062831483258E-3,1.9345445211113122E-5,54.166666666666664,10.924681300086506,8.3995264437203472E-4,1.6285829343353016E-3,2.4878810239184496E-3,3.7194339213691453E-3,8.7838288519318825E-2,2.3455317387209417E-3,5.3001219756474319E-5,0,4.0174530174852803E-5,9.3175749931327122E-5,2.4397658739589516E-3,3.3567435232584606E-3,4.2249035028695103E-3,7.2346664967587438E-5,1.0456449963165195E-2,1.4758446131782312E-2,0.18,{"$f":"BB9/(BB9+BA9)","v":0.92422179153249107},6.3234890291606234E-3,1.2048720713451453E-2,4.8290929777815529E-3,1.2774188094697766E-2,0,2.0627875695654766E-4,4.7841699182730297E-4,5.8577090958920313E-3,1.6159156344781905E-2,6.9190578864540743E-6,6.1077083462367224E-5,2.1693043802633087E-2,8.0438091948531104E-2,0.92422179153249107,92.422179153249104,15,11.516667783884284,0.11516667783884284,4.8182927051340281,null,8.3620657623922987E-3,null,1.0456449963165195E-2,4.2249035028695103E-3,4.288753345785064E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR9, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.422179153249104},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ9, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0456449963165195E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA9, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.2249035028695103E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB9, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.288753345785064E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S9, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":4.8182927051340281},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P9, IF(MODE_ILIM=4,#REF!,#REF!))","v":68.62312247166517}]
["Iout",{"$f":"Iout","v":0.5},"A",{"$f":"B10","v":0.5},"Iout(max)",null,null,4,0.02,0.95232360099097058,0.95232360099097058,0,59.950313569759132,67.882699896228061,1,67.882699896228061,5.3072098708103659E-6,7.9069418750917393E-3,6424.3902735120382,1.1537979101579597E-5,1.441188159289202E-4,5.818091246551254E-5,0.11258766073143675,1.5211177618772525E-3,4.1961762406803396E-3,5.7186858096871466E-3,5.632116918623481E-2,1.5860370492522428E-5,1.5860370492522428E-5,2.4500574063370178E-2,1.8008343883040624E-6,1.8008343883040624E-6,4.8872911129850941E-2,1.6409417108644337E-3,2.5793926948150834E-5,54.166666666666664,10.924681300086506,1.1313418268091057E-3,2.1714439124470688E-3,3.3285796662043251E-3,4.9710300457616215E-3,0.10142691904356947,3.1273756516279217E-3,7.0668293008632434E-5,0,5.4143398442839242E-5,1.2481169145147166E-4,3.2540695233367611E-3,4.1396833508230398E-3,5.2972299903044388E-3,9.6462219956783269E-5,1.3618791779359606E-2,1.9355138793927577E-2,0.24,0.92537206363469693,6.3328237381188607E-3,1.2065532406403033E-2,4.8351031919770986E-3,1.2834060977866612E-2,0,2.0876161812185743E-4,4.8123855201743913E-4,5.8649995097489359E-3,1.6179267780055212E-2,6.9435076423719051E-6,6.115309905281806E-5,2.0424619365315099E-2,7.9294503746319328E-2,0.92537206363469693,92.537206363469693,20,12.603144523181673,0.12603144523181672,6.4243902735120386,null,8.3724730597006004E-3,null,1.3618791779359606E-2,5.2972299903044388E-3,5.7186858096871466E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR10, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.537206363469693},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ10, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.3618791779359606E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA10, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.2972299903044388E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB10, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.7186858096871466E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S10, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":6.4243902735120386},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P10, IF(MODE_ILIM=4,#REF!,#REF!))","v":67.882699896228061}]
["Rt",{"$f":"Vout*2500/(Fsw/1000)","v":200},"kW",{"$f":"B11*1000","v":200000},"RT pin resistance to get Fsw",null,null,5,2.5000000000000001E-2,0.95232360099097058,0.95232360099097058,0,59.723040842486405,67.142317256523114,1,67.142317256523114,5.3072098708103659E-6,9.883677343864675E-3,8030.487841890048,1.1537979101579597E-5,1.1298745692282025E-4,7.0226140581890667E-5,0.12587683141158815,1.9013972023465661E-3,5.2452203008504254E-3,7.1487923341960954E-3,6.2968981436343774E-2,1.9825463115653036E-5,1.9825463115653036E-5,2.7432493409039364E-2,2.2576250839109643E-6,2.2576250839109643E-6,5.4641575772326381E-2,2.0511771385805424E-3,3.2242408685188543E-5,54.166666666666664,10.924681300086506,1.4284334930693733E-3,2.7143048905588362E-3,4.1749807923133981E-3,6.2285208150120071E-3,0.11339874286489464,3.9092195645349017E-3,8.8335366260790536E-5,0,6.8401748864460959E-5,1.5673711512525151E-4,4.0688985346344405E-3,4.9226231783876173E-3,6.3695564777393665E-3,1.2057777494597907E-4,1.6787553602331792E-2,2.3958429024727453E-2,0.30000000000000004,0.9260447425404118,6.3388998053878817E-3,1.2076121715019726E-2,4.8386179640909468E-3,1.2887396709763415E-2,0,2.1114359972167882E-4,4.8381860474230133E-4,5.8692629423802833E-3,1.6191028943562575E-2,6.9688727986103475E-6,6.1197552955597818E-5,1.9661647628415876E-2,7.862610433883889E-2,0.9260447425404118,92.604474254041179,25,13.76888730592373,0.1376888730592373,8.0304878418900483,null,8.378559245179126E-3,null,1.6787553602331792E-2,6.3695564777393665E-3,7.1487923341960954E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR11, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.604474254041179},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ11, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.6787553602331792E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA11, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.3695564777393665E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB11, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1487923341960954E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S11, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":8.0304878418900483},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P11, IF(MODE_ILIM=4,#REF!,#REF!))","v":67.142317256523114}]
["Tamb",{"$f":"'Design Converter'!E56","v":25},"°C",{"$f":"B12","v":25},"Ambient temperature",null,null,6,0.03,0.95232360099097058,0.95232360099097058,0,59.495768115213679,66.401975888401736,1,66.401975888401736,5.3072098708103659E-6,1.1860412812637609E-2,9636.5854102680569,1.1537979101579597E-5,9.2233217585420285E-5,8.22713686982688E-5,0.13789116006280333,2.2816766428158776E-3,6.2942643610205094E-3,8.5790729510955115E-3,6.8979063111619068E-2,2.3790555738783633E-5,2.3790555738783633E-5,3.0104124467311155E-2,2.7187749298300861E-6,2.7187749298300861E-6,5.9856847256261857E-2,2.4614125662966511E-3,3.8690890422226244E-5,54.166666666666664,10.924681300086506,1.7312276431528373E-3,3.2571658686706031E-3,5.0270844022456667E-3,7.4919075714653047E-3,0.12422209891966161,4.6910634774418834E-3,1.0600243951294864E-4,0,8.2950063268988461E-5,1.8895250278193711E-4,4.884253618202771E-3,5.7055630059521965E-3,7.441882965174295E-3,1.4469332993517488E-4,1.9962737484777546E-2,2.8568319766541672E-2,0.36,0.92647800061593799,6.3433456713623618E-3,1.2083592193624662E-2,4.8408817535290005E-3,1.2937453072000371E-2,0,2.1347613546782775E-4,4.8627871385774048E-4,5.8720089280226116E-3,1.6198604057073435E-2,6.9969032253158764E-6,6.1226184762250814E-5,1.9152057917756916E-2,7.81959215306825E-2,0.92647800061593799,92.647800061593799,30,15.015319606822954,0.15015319606822955,9.6365854102680562,null,8.3824792268900432E-3,null,1.9962737484777546E-2,7.441882965174295E-3,8.5790729510955115E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR12, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.647800061593799},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ12, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.9962737484777546E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA12, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.441882965174295E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB12, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.5790729510955115E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S12, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":9.6365854102680562},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P12, IF(MODE_ILIM=4,#REF!,#REF!))","v":66.401975888401736}]
["VDD",5,"V",{"$f":"B13","v":5},"Gate drive rail",null,null,7,3.5000000000000003E-2,0.95232360099097058,0.95232360099097058,0,59.268495387940945,65.661677187886511,1,65.661677187886511,5.3072098708103659E-6,1.3837148281410545E-2,11242.682978646068,1.1537979101579597E-5,7.7408760915848872E-5,9.4316596814646947E-5,0.14893947549494704,2.6619560832851917E-3,7.3433084211905952E-3,1.0009527692176747E-2,7.4505903607585688E-2,2.7755648361914251E-5,2.7755648361914251E-5,3.2583916139406109E-2,3.1851347729395494E-6,3.1851347729395494E-6,6.4652784348673178E-2,2.8716479940127594E-3,4.5139372159263966E-5,54.166666666666664,10.924681300086506,2.0397242770594979E-3,3.8000268467823705E-3,5.8848904960011328E-3,8.7611916578741265E-3,0.13417520201838301,5.4729073903488634E-3,1.2366951276510677E-4,0,9.7788823485692281E-5,2.2145833625079905E-4,5.7001354848038241E-3,6.4885028335167757E-3,8.5142094526092244E-3,1.6880888492437073E-4,2.3144345480211544E-2,3.3184813955523147E-2,0.42000000000000004,0.9267742145508433,6.3468613097774317E-3,1.2089277883637818E-2,4.8424294822734179E-3,1.2985630397974219E-2,0,2.1578133351857979E-4,4.8867113246326387E-4,5.8738863291796966E-3,1.6203783081555966E-2,7.0283351843562602E-6,6.1245760023720188E-5,1.8787499471341139E-2,7.7902094516929615E-2,0.9267742145508433,92.677421455084328,35,16.343061169118954,0.16343061169118955,11.242682978646068,null,8.3851592766639258E-3,null,2.3144345480211544E-2,8.5142094526092244E-3,1.0009527692176747E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR13, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.677421455084328},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ13, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.3144345480211544E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA13, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.5142094526092244E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB13, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0009527692176747E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S13, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":11.242682978646068},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P13, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.661677187886511}]
["K1",400,"pC",4,"RT constant",null,null,8,0.04,0.95232360099097058,0.95232360099097058,0,59.041222660668225,64.921422614593013,1,64.921422614593013,5.3072098708103659E-6,1.5813883750183479E-2,12848.780547024076,1.1537979101579597E-5,6.6290418413670319E-5,1.0636182493102507E-4,0.1592229967622586,3.0422355237545049E-3,8.3923524813606792E-3,1.144015658923888E-2,7.9650161311882919E-2,3.1720740985044856E-5,3.1720740985044856E-5,3.4916798376750192E-2,3.6575484266478746E-6,3.6575484266478746E-6,6.9116733752490195E-2,3.2818834217288686E-3,5.1587853896301668E-5,54.166666666666664,10.924681300086506,2.3539233947893548E-3,4.3428878248941375E-3,6.7483990735797937E-3,1.0036374417398845E-2,0.14343932450113392,6.2547513032558451E-3,1.4133658601726487E-4,0,1.129185113438429E-4,2.5425509736110778E-4,6.5165448456112598E-3,7.2714426610813532E-3,9.5865359400441521E-3,1.9292443991356654E-4,2.6332379642967828E-2,3.7807914521618399E-2,0.48,0.92698467238271642,6.3497973893594855E-3,1.209384710551523E-2,4.8435291322138649E-3,1.3032630217354567E-2,0,2.1807026925836721E-4,4.9102203776858787E-4,5.8752202089554818E-3,1.6207462740530015E-2,7.0635236041668747E-6,6.1259668103664193E-5,1.8513691411806175E-2,7.7693593704469613E-2,0.92698467238271642,92.698467238271647,40,17.75180413241851,0.17751804132418511,12.848780547024077,null,8.3870634324049575E-3,null,2.6332379642967828E-2,9.5865359400441521E-3,1.144015658923888E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR14, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.698467238271647},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ14, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.6332379642967828E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA14, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.5865359400441521E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB14, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.144015658923888E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S14, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":12.848780547024077},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P14, IF(MODE_ILIM=4,#REF!,#REF!))","v":64.921422614593013}]
["Outputs",null,null,null,null,null,null,9,4.4999999999999998E-2,0.95232360099097058,0.95232360099097058,0,58.813949933395499,64.181213695387541,1,64.181213695387541,5.3072098708103659E-6,1.7790619218956413E-2,14454.878115402085,1.1537979101579597E-5,5.764281868975366E-5,1.1840705304740321E-4,0.16888149109715511,3.4225149642238177E-3,9.4413965415307641E-3,1.2870959674088741E-2,8.4481753779352201E-2,3.568583360817545E-5,3.568583360817545E-5,3.7134228015376761E-2,4.136852670893977E-6,4.136852670893977E-6,7.3309366694776418E-2,3.6921188494449769E-3,5.803633563333937E-5,54.166666666666664,10.924681300086506,2.6738249963424079E-3,4.8857488030059045E-3,7.6176101349816512E-3,1.1317457193607754E-2,0.1521403785653542,7.0365952161628243E-3,1.5900365926942294E-4,0,1.2833960867271083E-4,2.8734326794213377E-4,7.3334824122106169E-3,8.0543824886459333E-3,1.0658862427479081E-2,2.1703999490276231E-4,2.9526842028200218E-2,4.2437624388568032E-2,0.54,0.92713790694219278,6.3523489961867284E-3,1.2097671663408397E-2,4.8443297884436781E-3,1.3078842808238005E-2,0,2.2034910400480965E-4,4.9334599261814736E-4,5.8761914081644521E-3,1.6210141903937204E-2,7.1026535678164097E-6,6.12697945906873E-5,1.8300435928514325E-2,7.7542030041674245E-2,0.92713790694219278,92.713790694219284,45,19.240199150848532,0.19240199150848533,14.454878115402085,null,8.3884498501189224E-3,null,2.9526842028200218E-2,1.0658862427479081E-2,1.2870959674088741E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR15, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.713790694219284},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ15, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.9526842028200218E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA15, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0658862427479081E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB15, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.2870959674088741E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S15, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":14.454878115402085},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P15, IF(MODE_ILIM=4,#REF!,#REF!))","v":64.181213695387541}]
["Design","Value","Units","Std Units","Description",null,null,10,0.05,0.95232360099097058,0.95232360099097058,0,58.586677206122772,63.441052028299914,1,63.441052028299914,5.3072098708103659E-6,1.976735468772935E-2,16060.975683780096,1.1537979101579597E-5,5.072473891062033E-5,1.3045228116378136E-4,0.17801672217081957,3.8027944046931314E-3,1.0490440601700851E-2,1.4301936978540906E-2,8.9051587556097017E-2,3.9650926231306071E-5,3.9650926231306071E-5,3.9259297209481347E-2,4.6238772521471694E-6,4.6238772521471694E-6,7.7274857526661092E-2,4.1023542771610848E-3,6.4484817370377085E-5,54.166666666666664,10.924681300086506,2.9994290817186584E-3,5.4286097811176723E-3,8.4925236802067088E-3,1.2604441330477214E-2,0.16037004011559325,7.8184391290698051E-3,1.7667073252158107E-4,0,1.4405259730156664E-4,3.2072332982314771E-4,8.1509488965996243E-3,8.8373223162105125E-3,1.1731188914914011E-2,2.4115554989195814E-4,3.2727734691882809E-2,4.7073946473907169E-2,0.60000000000000009,0.92725105572488786,6.3546333037785433E-3,1.2100974872262492E-2,4.8449209950100717E-3,1.3124502580400465E-2,0,2.2262153821298297E-4,4.9565174362352512E-4,5.8769085440940035E-3,1.6212120204910568E-2,7.1458251059929261E-6,6.1277272014080331E-5,1.8129595510436861E-2,7.7430352389849577E-2,0.92725105572488786,92.725105572488786,50,20.80575856495858,0.20805758564958579,16.060975683780097,null,8.3894735844330225E-3,null,3.2727734691882809E-2,1.1731188914914011E-2,1.4301936978540906E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR16, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.725105572488786},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ16, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.2727734691882809E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA16, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1731188914914011E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB16, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.4301936978540906E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S16, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":16.060975683780097},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P16, IF(MODE_ILIM=4,#REF!,#REF!))","v":63.441052028299914}]
["On-Time",{"$f":"(Rt*k_RT/10000)/Vin","v":1.2307692307692308},"µs",{"$f":"B17/1000000","v":1.2307692307692308E-6},"On Time - fixed",null,null,11,5.5E-2,0.95232360099097058,0.95232360099097058,0,58.359404478850045,62.700939286712092,1,62.700939286712092,5.3072098708103659E-6,2.1744090156502284E-2,17667.073252158105,1.1537979101579597E-5,4.5064491818602155E-5,1.424975092801595E-4,0.18670551333500315,4.1830738451624442E-3,1.1539484661870934E-2,1.573308853441769E-2,9.3398092972433511E-2,4.3616018854436672E-5,4.3616018854436672E-5,4.1309582759964852E-2,5.119444883407156E-6,5.119444883407156E-6,8.1046554315049979E-2,4.5125897048771922E-3,7.0933299107414787E-5,54.166666666666664,10.924681300086506,3.3307356509181037E-3,5.9714707592294393E-3,9.3731397092549577E-3,1.3897328172391815E-2,0.16819751705463634,8.6002830419767834E-3,1.9433780577373917E-4,0,1.6005795905968078E-4,3.5439576483341998E-4,8.9689450111884849E-3,9.6202621437750917E-3,1.280351540234894E-2,2.6527110488115398E-4,3.59350596908104E-2,5.1716883688965931E-2,0.66,0.92733503324958744,6.3567249377127532E-3,1.2103898957271033E-2,4.8453597806765994E-3,1.3169758824143899E-2,0,2.2488992846434873E-4,4.9794486115956429E-4,5.8774407928624157E-3,1.6213588473635129E-2,7.1930918048087955E-6,6.1282821658475241E-5,1.7989618759619481E-2,7.7347701229008511E-2,0.92733503324958744,92.733503324958747,55,22.444784059665849,0.22444784059665848,17.667073252158104,null,8.3902333864529863E-3,null,3.59350596908104E-2,1.280351540234894E-2,1.573308853441769E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR17, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.733503324958747},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ17, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.59350596908104E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA17, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.280351540234894E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB17, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.573308853441769E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S17, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":17.667073252158104},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P17, IF(MODE_ILIM=4,#REF!,#REF!))","v":62.700939286712092}]
["Off Time",{"$f":"L*Iripple*1000000/(Vout+(Rdcr+RdsonBot)*Iout)","v":5.3008642193050974},"µs",{"$f":"B18/1000000","v":5.3008642193050973E-6},"Off Time - depends on Vout, L, Iout, DCR, etc.",null,null,12,0.06,0.95232360099097058,0.95232360099097058,0,58.132131751577319,61.960877223845834,1,61.960877223845834,5.3072098708103659E-6,2.3720825625275218E-2,19273.170820536114,1.1537979101579597E-5,4.034761924192034E-5,1.5454273739653763E-4,0.19500754869217579,4.5633532856317579E-3,1.2588528722041019E-2,1.7164414373549174E-2,9.7551126572241367E-2,4.758111147756728E-5,4.758111147756728E-5,4.3298850039402675E-2,5.6243712442040436E-6,5.6243712442040436E-6,8.4650365190700308E-2,4.9228251325933031E-3,7.7381780844452489E-5,54.166666666666664,10.924681300086506,3.6677447039407457E-3,6.5143317373412063E-3,1.0259458222126405E-2,1.5196119064144533E-2,0.17567657703863765,9.3821269548837669E-3,2.1200487902589728E-4,0,1.7635617577632377E-4,3.8836105480222107E-4,9.7874714688001956E-3,1.0403201971339669E-2,1.3875841889783866E-2,2.8938665987034975E-4,3.9148819082598943E-2,5.6366438938869889E-2,0.72,0.9273971205969298,6.3586736809044817E-3,1.2106538797381028E-2,4.8456841893583773E-3,1.321471113067295E-2,0,2.271558466867343E-4,5.0022906107717537E-4,5.8778343018908771E-3,1.6214674013017485E-2,7.2444801347819469E-6,6.1286924693190869E-5,1.787279974228308E-2,7.7286832168100159E-2,0.9273971205969298,92.739712059692977,60,24.152326085424395,0.24152326085424394,19.273170820536112,null,8.3907951330880973E-3,null,3.9148819082598943E-2,1.3875841889783866E-2,1.7164414373549174E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR18, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.739712059692977},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ18, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.9148819082598943E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA18, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.3875841889783866E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB18, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7164414373549174E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S18, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":19.273170820536112},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P18, IF(MODE_ILIM=4,#REF!,#REF!))","v":61.960877223845834}]
["DIL",{"$f":"(Vin-Vout-(Rdcr+RdsonTop)*Iout)/L*OnTime*1000","v":951.97285067873304},"mA",{"$f":"B19/1000","v":0.95197285067873305},"Inductor pk-pk ripple current in CCM",null,null,13,6.5000000000000002E-2,0.95232360099097058,0.95232360099097058,0,57.904859024304592,61.220867677574461,1,61.220867677574461,5.3072098708103659E-6,2.5697561094048155E-2,20879.268388914126,1.1537979101579597E-5,3.6356419369343419E-5,1.6658796551291576E-4,0.20297029187586935,4.9436327261010715E-3,1.3637572782211107E-2,1.8595914527773184E-2,0.10153443169752602,5.1546204100697888E-5,5.1546204100697888E-5,4.5238129126502449E-2,6.1394649805983278E-6,6.1394649805983278E-6,8.8106893529936142E-2,5.3330605603094106E-3,8.3830262581490218E-5,54.166666666666664,10.924681300086506,4.0104562407865876E-3,7.0571927154529741E-3,1.1151479218821052E-2,1.6500815350936875E-2,0.18284997866196234,1.0163970867790745E-2,2.2967195227805543E-4,0,1.9294772928076624E-4,4.226196815588217E-4,1.0606528982670813E-2,1.1186141798904248E-2,1.4948168377218796E-2,3.1350221485954564E-4,4.2369014925686031E-2,6.1022615122540508E-2,0.78,0.92744236120969326,6.360514017017726E-3,1.2108960113549566E-2,4.8459205732300928E-3,1.325942848421054E-2,0,2.294203815823109E-4,5.0250691712641312E-4,5.87812103647268E-3,1.6215465002952456E-2,7.2999998694491492E-6,6.1289914413523107E-5,1.7773800737856241E-2,7.7242727178280984E-2,0.92744236120969326,92.744236120969319,65,25.922181532084487,0.25922181532084487,20.879268388914127,null,8.3912044558096827E-3,null,4.2369014925686031E-2,1.4948168377218796E-2,1.8595914527773184E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR19, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.744236120969319},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ19, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.2369014925686031E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA19, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.4948168377218796E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB19, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.8595914527773184E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S19, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":20.879268388914127},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P19, IF(MODE_ILIM=4,#REF!,#REF!))","v":61.220867677574461}]
["CCM Freq",{"$f":"'Design Converter'!E12","v":150},"kHz",{"$f":"B20*1000","v":150000},"Frequency in CCM",{"$f":"10000*Vout/(k_RT*Rt/1000+Vin*0.75)","v":141.38438880706923},null,14,7.0000000000000007E-2,0.95232360099097058,0.95232360099097058,0,57.677586297031858,60.480912575586267,1,60.480912575586267,5.3072098708103659E-6,2.7674296562821089E-2,22485.365957292135,1.1537979101579597E-5,3.2935390907134633E-5,1.786331936292939E-4,0.21063222621768937,5.3239121665703843E-3,1.468661684238119E-2,2.002758902893529E-2,0.10536725935871019,5.5511296723828502E-5,5.5511296723828502E-5,4.7136425070147543E-2,6.6655277051809017E-6,6.6655277051809017E-6,9.143284447107658E-2,5.7432959880255189E-3,9.0278744318527933E-5,54.166666666666664,10.924681300086506,4.3588702614556201E-3,7.6000536935647411E-3,1.2049202699338889E-2,1.7811418378379035E-2,0.18975239042854711,1.0945814780697725E-2,2.4733902553021353E-4,0,2.0983310140227848E-4,4.5717212693249202E-4,1.1426118266449785E-2,1.1969081626468828E-2,1.6020494864653727E-2,3.3761776984874147E-4,4.5595649279331282E-2,6.5685415132695574E-2,0.84000000000000008,0.92747435915916598,6.3622705883984018E-3,1.2111209870714533E-2,4.8460877636972701E-3,1.3303960180890747E-2,0,2.3168431101602203E-4,5.0478026839541172E-4,5.87832383917804E-3,1.6216024457266318E-2,7.3596500438337169E-6,6.1292028994079932E-5,1.7688807390485027E-2,7.7211800349079679E-2,0.92747435915916598,92.747435915916597,70,27.746934669307642,0.27746934669307644,22.485365957292135,null,8.3914939631121541E-3,null,4.5595649279331282E-2,1.6020494864653727E-2,2.002758902893529E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR20, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.747435915916597},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ20, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.5595649279331282E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA20, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.6020494864653727E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB20, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.002758902893529E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S20, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":22.485365957292135},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P20, IF(MODE_ILIM=4,#REF!,#REF!))","v":60.480912575586267}]
["Icrit_Skip",{"$f":"1000*Iripple/2","v":475.98642533936652},"mA",{"$f":"Iripple/2","v":0.47598642533936653},"CCM-DCM (critical conduction) boundary",null,null,15,7.4999999999999997E-2,0.95232360099097058,0.95232360099097058,0,57.450313569759132,59.741013940929861,1,59.741013940929861,5.3072098708103659E-6,2.9651032031594023E-2,24091.463525670144,1.1537979101579597E-5,2.9970499573220349E-5,1.9067842174567206E-4,0.21802506750065262,5.7041916070396954E-3,1.5735660902551275E-2,2.1459437908888837E-2,0.10906547514860887,5.9476389346959103E-5,5.9476389346959103E-5,4.900120405688365E-2,7.2033539970730517E-6,7.2033539970730517E-6,9.4641985443293913E-2,6.1535314157416272E-3,9.6727226055565635E-5,54.166666666666664,10.924681300086506,4.7129867659478526E-3,8.1429146716765089E-3,1.2952628663679928E-2,1.9127929492490078E-2,0.19641238415643622,1.1727658693604705E-2,2.6500609878237164E-4,0,2.2701277397013116E-4,4.9201887275250275E-4,1.2246240034200233E-2,1.2752021454033409E-2,1.7092821352088654E-2,3.617333248379373E-4,4.8828724203616905E-2,7.0354841855849781E-2,0.89999999999999991,0.92749575843689025,6.3639614731035863E-3,1.211332252330212E-2,4.8461995757133197E-3,1.3348342384634688E-2,0,2.3394820552032129E-4,5.0705046394316263E-4,5.878459467600696E-3,1.6216398603686129E-2,7.4234225320051948E-6,6.1293443162717349E-5,1.7615021448646379E-2,7.7191421011845118E-2,0.92749575843689025,92.74957584368903,75,29.618044224570543,0.29618044224570544,24.091463525670143,null,8.391687576992761E-3,null,4.8828724203616905E-2,1.7092821352088654E-2,2.1459437908888837E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR21, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.74957584368903},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ21, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.8828724203616905E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA21, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7092821352088654E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB21, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.1459437908888837E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S21, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":24.091463525670143},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P21, IF(MODE_ILIM=4,#REF!,#REF!))","v":59.741013940929861}]
["Tr",null,"ns",{"$f":"B22/1000000000","v":0},"Switch rise time",null,null,16,0.08,0.95232360099097058,0.95232360099097058,0,57.223040842486405,59.001173897975015,1,59.001173897975015,5.3072098708103659E-6,3.1627767500366957E-2,25697.561094048153,1.1537979101579597E-5,2.7376219656045357E-5,2.0272364986205016E-4,0.2251753214628735,6.0844710475090099E-3,1.6784704962721358E-2,2.2891461199494933E-2,0.11264233837246962,6.3441481970089711E-5,6.3441481970089711E-5,5.0838736549755945E-2,7.7537314019264726E-6,7.7537314019264726E-6,9.7745822259701881E-2,6.5637668434577346E-3,1.0317570779260334E-4,54.166666666666664,10.924681300086506,5.0728057542632817E-3,8.685775649788275E-3,1.3861757111844161E-2,2.0450350039698039E-2,0.20285383808713894,1.2509502606511687E-2,2.8267317203452974E-4,0,2.444872288135948E-4,5.2716040084812448E-4,1.3066895000399261E-2,1.3534961281597984E-2,1.8165147839523582E-2,3.8584887982713307E-4,5.206824175944802E-2,7.5030898172314966E-2,0.96,0.92750854268717342,6.3656002342424665E-3,1.2115323920951668E-2,4.8462663738929723E-3,1.3392602226968897E-2,0,2.362124930234613E-4,5.0931851578440643E-4,5.8785404940597729E-3,1.6216622124383184E-2,7.4913042843631218E-6,6.1294288008325522E-5,1.7550343542014141E-2,7.7179615517613667E-2,0.92750854268717342,92.750854268717347,80,31.525976771075946,0.31525976771075948,25.697561094048154,null,8.3918032448363124E-3,null,5.206824175944802E-2,1.8165147839523582E-2,2.2891461199494933E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR22, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.750854268717347},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ22, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.206824175944802E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA22, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.8165147839523582E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB22, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.2891461199494933E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S22, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":25.697561094048154},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P22, IF(MODE_ILIM=4,#REF!,#REF!))","v":59.001173897975015}]
["Tf",null,"ns",{"$f":"B23/1000000000","v":0},"Switch fall time",null,null,17,8.5000000000000006E-2,0.95232360099097058,0.95232360099097058,0,56.995768115213671,58.261394678825212,1,58.261394678825212,5.3072098708103659E-6,3.3604502969139895E-2,27303.658662426165,1.1537979101579597E-5,2.5087149140890944E-5,2.147688779784283E-4,0.23210540866845972,6.4647504879783236E-3,1.7833749022891449E-2,2.4323658932622425E-2,0.11610906475656439,6.7406574593220319E-5,6.7406574593220319E-5,5.2654345917259406E-2,8.3174404319232371E-6,8.3174404319232371E-6,0.10075408740990022,6.9740022711738464E-3,1.0962418952964105E-4,54.166666666666664,10.924681300086506,5.4383272264019065E-3,9.2286366279000429E-3,1.4776588043831591E-2,2.1778681366840143E-2,0.20909695024880418,1.329134651941867E-2,3.0034024528668784E-4,0,2.6225694776193988E-4,5.6259719304862772E-4,1.3888083879938248E-2,1.4317901109162564E-2,1.923747432695851E-2,4.0996443481632891E-4,5.5314204008553226E-2,7.9713586956200788E-2,1.02,0.92751422924869642,6.3671972466840393E-3,1.2117233837013915E-2,4.8462960863868447E-3,1.3436760461176433E-2,0,2.3847750075346207E-4,5.1158519792939016E-4,5.8785765354336756E-3,1.6216721548609661E-2,7.5632787760168883E-6,6.1294663804044609E-5,1.7493167816725989E-2,7.7174874173293467E-2,0.92751422924869642,92.751422924869644,85,33.460383546927204,0.33460383546927203,27.303658662426166,null,8.3918546950421547E-3,null,5.5314204008553226E-2,1.923747432695851E-2,2.4323658932622425E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR23, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.751422924869644},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ23, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.5314204008553226E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA23, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.923747432695851E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB23, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.4323658932622425E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S23, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":27.303658662426166},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P23, IF(MODE_ILIM=4,#REF!,#REF!))","v":58.261394678825212}]
[null,null,null,null,null,null,null,18,0.09,0.95232360099097058,0.95232360099097058,0,56.768495387940952,57.521678630222894,1,57.521678630222894,5.3072098708103659E-6,3.5581238437912825E-2,28909.756230804171,1.1537979101579597E-5,2.305241979408703E-5,2.2681410609480643E-4,0.23883449514338789,6.8450299284476372E-3,1.8882793083061528E-2,2.5756031140147941E-2,0.11947524196782437,7.1371667216350913E-5,7.1371667216350913E-5,5.4452592732197873E-2,8.895254565775825E-6,8.895254565775825E-6,0.10367510062873529,7.3842376988899538E-3,1.1607267126667874E-4,54.166666666666664,10.924681300086506,5.809551182363727E-3,9.771497606011809E-3,1.5697121459642215E-2,2.3112924821162895E-2,0.21515898675170081,1.4073190432325643E-2,3.1800731853884589E-4,0,2.8032241264443685E-4,5.9832973118328274E-4,1.4709807388123136E-2,1.5100840936727143E-2,2.0309800814393437E-2,4.3407998980552463E-4,5.8566613013484994E-2,8.440291107541506E-2,1.08,0.92751399857162631,6.3687605819119936E-3,1.211906765494671E-2,4.8462948810906372E-3,1.3480833232497439E-2,0,2.4074348318619171E-4,5.1385111243897486E-4,5.8785750734045563E-3,1.6216717515436154E-2,7.6393269727918994E-6,6.1294648559778785E-5,1.7442244966251231E-2,7.7176022476696471E-2,0.92751399857162631,92.751399857162625,90,35.410314704487,0.35410314704487,28.90975623080417,null,8.3918526079491546E-3,null,5.8566613013484994E-2,2.0309800814393437E-2,2.5756031140147941E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR24, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.751399857162625},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ24, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8566613013484994E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA24, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.0309800814393437E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB24, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.5756031140147941E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S24, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":28.90975623080417},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P24, IF(MODE_ILIM=4,#REF!,#REF!))","v":57.521678630222894}]
["Components","Input Value","Units","Std Units","Description",null,null,19,9.5000000000000001E-2,0.95232360099097058,0.95232360099097058,0,56.541222660668232,56.782028220991549,1,56.782028220991549,5.3072098708103659E-6,3.7557973906685763E-2,30515.853799182183,1.1537979101579597E-5,2.1231872483788786E-5,2.3885933421118456E-4,0.24537911770898771,7.2253093689169491E-3,1.9931837143231615E-2,2.7188577853955877E-2,0.12274914243242722,7.5336759839481535E-5,7.5336759839481535E-5,5.6237414143750449E-2,9.4879402487271089E-6,9.4879402487271089E-6,0.10651604034583224,7.7944731266060595E-3,1.2252115300371647E-4,54.166666666666664,10.924681300086506,6.186477622148745E-3,1.0314358584123577E-2,1.6623357359276038E-2,2.4453081750322302E-2,0.22105484513280019,1.4855034345232627E-2,3.3567439179100404E-4,0,2.9868410529035636E-4,6.3435849708136046E-4,1.5532066240674779E-2,1.588378076429172E-2,2.1382127301828369E-2,4.5819554479472051E-4,6.1825470837620168E-2,8.9098873391664252E-2,1.1400000000000001,0.92750878279971216,6.3702966136811737E-3,1.212083752260191E-2,4.8462676284898492E-3,1.3524833289777854E-2,0,2.43010641174982E-4,5.161167346373573E-4,5.8785420158908031E-3,1.6216626322527058E-2,7.7194279924327001E-6,6.1294303876133118E-5,1.7396588480164316E-2,7.7182132980813861E-2,0.92750878279971216,92.750878279971218,95,37.364462120689176,0.37364462120689174,30.515853799182182,null,8.3918054172984393E-3,null,6.1825470837620168E-2,2.1382127301828369E-2,2.7188577853955877E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR25, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.750878279971218},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ25, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1825470837620168E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA25, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.1382127301828369E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB25, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.7188577853955877E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S25, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":30.515853799182182},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P25, IF(MODE_ILIM=4,#REF!,#REF!))","v":56.782028220991549}]
["L",{"$f":"'Design Converter'!E17","v":68},"µH",{"$f":"B26/1000000","v":6.7999999999999999E-5},"Filter inductance",null,null,20,0.1,0.95232360099097058,0.95232360099097058,0,56.313949933395499,56.04244605006425,2,112.0848921001285,5.3072098708103659E-6,3.95347093754587E-2,32121.951367560192,1.1537979101579597E-5,1.9593379904520369E-5,2.509045623275627E-4,0.25175366282317629,7.6055888093862645E-3,2.0980881203401702E-2,2.8621299105938403E-2,0.12593796287268755,7.9301852462612142E-5,7.9301852462612142E-5,5.8012231160191149E-2,1.009625689255036E-5,1.009625689255036E-5,0.10928315154465276,8.2047085543221696E-3,1.2896963474075417E-4,54.166666666666664,10.924681300086506,6.5691065457569586E-3,1.0857219562235345E-2,1.7555295742733058E-2,2.5799153502383983E-2,0.22679748572978928,1.5636878258139607E-2,3.5334146504316215E-4,0,3.173425075289688E-4,6.7068397257213095E-4,1.6354861153729184E-2,1.66667205918563E-2,2.2454453789263296E-2,4.8231109978391629E-4,6.5090779545160377E-2,9.3801476760453945E-2,1.2000000000000002,0.92749932779847855,6.3718104421187534E-3,1.2122553160496166E-2,4.8462182257593793E-3,1.3568770833907002E-2,0,2.4527913534583512E-4,5.1838244477155385E-4,5.8784820901811585E-3,1.6216461010645673E-2,7.8035595676010119E-6,6.129367904353906E-5,1.7355408996353086E-2,7.7192463578189735E-2,0.92749932779847855,92.749932779847853,100,39.311419610679415,0.39311419610679416,32.121951367560193,null,8.391719871444811E-3,null,6.5090779545160377E-2,2.2454453789263296E-2,2.8621299105938403E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR26, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.749932779847853},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ26, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.5090779545160377E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA26, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.2454453789263296E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB26, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.8621299105938403E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S26, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":32.121951367560193},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P26, IF(MODE_ILIM=4,#REF!,#REF!))","v":112.0848921001285}]
["Rdcr",{"$f":"'Design Converter'!E18","v":120},"mW",{"$f":"B27/1000","v":0.12},"Inductor DCR at 25°C",null,null,21,0.105,0.95232360099097058,0.95232360099097058,0,56.086677206122772,55.302934855152913,2,110.60586971030583,5.3072098708103659E-6,4.1511444844231631E-2,33728.048935938197,1.1537979101579597E-5,1.811093423756323E-5,2.6294979044394083E-4,0.25797073880990801,7.9858682498555739E-3,2.2029925263571781E-2,3.0054194927995426E-2,0.12904801051216772,8.3266945085742737E-5,8.3266945085742737E-5,5.9780032551427609E-2,1.0720956875549234E-5,1.0720956875549234E-5,0.11198190734269585,8.6149439820382787E-3,1.3541811647779187E-4,54.166666666666664,10.924681300086506,6.9574379531883697E-3,1.1400080540347111E-2,1.8492936610013271E-2,2.7151141425823321E-2,0.23239826701165753,1.6418722171046587E-2,3.7100853829532019E-4,0,3.3629810118954471E-4,7.073066394848649E-4,1.7178192843837838E-2,1.7449660419420879E-2,2.3526780276698224E-2,5.0642665477311207E-4,6.8362541201132498E-2,9.8510724031089222E-2,1.26,0.92748623747423964,6.3733061967436557E-3,1.2124222439318807E-2,4.8461498283320099E-3,1.3612654124024466E-2,0,2.4754909566827138E-4,5.2064855063203635E-4,5.8783991238282041E-3,1.6216232138530864E-2,7.8916983766878884E-6,6.1292813971071164E-5,1.7318067395807924E-2,7.7206413405234001E-2,0.92748623747423964,92.748623747423963,105,41.239947953148963,0.41239947953148964,33.728048935938197,null,8.3916014343411414E-3,null,6.8362541201132498E-2,2.3526780276698224E-2,3.0054194927995426E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR27, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.748623747423963},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ27, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.8362541201132498E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA27, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.3526780276698224E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB27, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.0054194927995426E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S27, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":33.728048935938197},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P27, IF(MODE_ILIM=4,#REF!,#REF!))","v":110.60586971030583}]
["Kcore",0,null,{"$f":"B28","v":0},"Core loss constant - consult inductor vendor",null,null,22,0.11,0.95232360099097058,0.95232360099097058,0,55.859404478850045,54.563497522118709,2,109.12699504423742,5.3072098708103659E-6,4.3488180313004568E-2,35334.14650431621,1.1537979101579597E-5,1.6763256358511281E-5,2.7499501856031896E-4,0.26404146912819221,8.3661476903248884E-3,2.3078969323741868E-2,3.1487265352034687E-2,0.13208484978139873,8.7232037708873344E-5,8.7232037708873344E-5,6.1543441412165105E-2,1.1362785542557798E-5,1.1362785542557798E-5,0.11461713629595138,9.0251794097543862E-3,1.4186659821482957E-4,54.166666666666664,10.924681300086506,7.3514718444429757E-3,1.1942941518458879E-2,1.9436279961116684E-2,2.8509046869525666E-2,0.2378672097761467,1.720056608395357E-2,3.8867561154747835E-4,0,3.5555136810135464E-4,7.4422697964883293E-4,1.800206202796803E-2,1.8232600246985458E-2,2.4599106764133155E-2,5.3054220976230795E-4,7.1640757871389169E-2,0.10322661804667528,1.32,0.92747000601467822,6.3747872569029189E-3,1.212585180004919E-2,4.8460650183566279E-3,1.3656489918515044E-2,0,2.4982062841779576E-4,5.2291530400847637E-4,5.8782962489888711E-3,1.6215948346593519E-2,7.9838202844693774E-6,6.1291741317061658E-5,1.7284040680671429E-2,7.7223490764105396E-2,0.92747000601467822,92.747000601467818,110,43.139231734149426,0.43139231734149425,35.334146504316209,null,8.3914545772409144E-3,null,7.1640757871389169E-2,2.4599106764133155E-2,3.1487265352034687E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR28, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.747000601467818},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ28, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1640757871389169E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA28, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.4599106764133155E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB28, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.1487265352034687E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S28, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":35.334146504316209},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P28, IF(MODE_ILIM=4,#REF!,#REF!))","v":109.12699504423742}]
["Cin",{"$f":"'Design Converter'!E37","v":10},"µF",{"$f":"B29/1000000","v":1.0000000000000001E-5},"Input capacitance",null,null,23,0.115,0.95232360099097058,0.95232360099097058,0,55.632131751577319,53.824137095110636,2,107.64827419022127,5.3072098708103659E-6,4.5464915781777505E-2,36940.244072694222,1.1537979101579597E-5,1.5532767860246459E-5,2.870402466766971E-4,0.26997572623593097,8.7464271307942012E-3,2.4128013383911955E-2,3.2920510409971661E-2,0.13505341930658696,9.1197130332003979E-5,9.1197130332003979E-5,6.3304768659084187E-2,1.2022481204940504E-5,1.2022481204940504E-5,0.11719312391630012,9.4354148374704953E-3,1.483150799518673E-4,54.166666666666664,10.924681300086506,7.7512082195207808E-3,1.2485802496570646E-2,2.0385325796043297E-2,2.9872871182786434E-2,0.24321320783081884,1.7982409996860554E-2,4.0634268479963645E-4,0,3.7510279009366913E-4,7.8144547489330564E-4,1.882646942350312E-2,1.9015540074550037E-2,2.5671433251568083E-2,5.5465776475150373E-4,7.4925431622609132E-2,0.10794916164411773,1.3800000000000001,0.92745104172454473,6.3762564147418991E-3,1.2127446564552558E-2,4.845965929240627E-3,1.3700283801039556E-2,0,2.520938213233019E-4,5.2518291285559994E-4,5.8781760534948567E-3,1.6215616773661522E-2,8.0799005200259629E-6,6.1290488064279832E-5,1.7252896747629663E-2,7.7243289407123897E-2,0.92745104172454473,92.745104172454475,115,44.999115697666738,0.44999115697666736,36.94024407269422,null,8.3912829943560627E-3,null,7.4925431622609132E-2,2.5671433251568083E-2,3.2920510409971661E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR29, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.745104172454475},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ29, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.4925431622609132E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA29, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.5671433251568083E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB29, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.2920510409971661E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S29, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":36.94024407269422},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P29, IF(MODE_ILIM=4,#REF!,#REF!))","v":107.64827419022127}]
["RCinESR",{"$f":"'Design Converter'!E39","v":3},"mW",{"$f":"B30/1000","v":3.0000000000000001E-3},"Input capacitor ESR",null,null,24,0.12,0.95232360099097058,0.95232360099097058,0,55.404859024304585,53.084856787546464,2,106.16971357509293,5.3072098708103659E-6,4.7441651250550436E-2,38546.341641072228,1.1537979101579597E-5,1.4404820070170374E-5,2.9908547479307523E-4,0.27578232012560666,9.1267065712635105E-3,2.5177057444082038E-2,3.4353930133729581E-2,0.13795812622323814,9.5162222955134533E-5,9.5162222955134533E-5,6.5066056538956876E-2,1.2700775140592199E-5,1.2700775140592199E-5,0.11971369451252371,9.8456502651866045E-3,1.5476356168890498E-4,54.166666666666664,10.924681300086506,8.156647078421779E-3,1.3028663474682413E-2,2.1340074114793096E-2,3.1242615715311291E-2,0.24844419783932323,1.8764253909767534E-2,4.2400975805179455E-4,0,3.9495284899575858E-4,8.1896260704755319E-4,1.9651415748242838E-2,1.9798479902114613E-2,2.6743759739003007E-2,5.787733197406995E-4,7.8216564522297832E-2,0.11267835765412315,1.44,0.9274296849063034,6.3777159974584387E-3,1.2129011168577408E-2,4.8458543390769437E-3,1.3744040425110919E-2,0,2.5436874742846058E-4,5.2745155041955354E-4,5.8780406941800045E-3,1.6215243369606183E-2,8.1799138102119693E-6,6.1289076701572098E-5,1.7224275463856558E-2,7.726547074622625E-2,0.9274296849063034,92.742968490630346,120,46.810309970062292,0.46810309970062292,38.546341641072225,null,8.3910897646353993E-3,null,7.8216564522297832E-2,2.6743759739003007E-2,3.4353930133729581E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR30, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.742968490630346},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ30, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.8216564522297832E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA30, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.6743759739003007E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB30, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.4353930133729581E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S30, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":38.546341641072225},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P30, IF(MODE_ILIM=4,#REF!,#REF!))","v":106.16971357509293}]
["Cout",{"$f":"'Design Converter'!E24","v":44},"µF",{"$f":"B31/1000000","v":4.3999999999999999E-5},"Output capacitance",null,null,25,0.125,0.95232360099097058,0.95232360099097058,0,55.177586297031858,52.345659994018732,2,104.69131998803746,5.3072098708103659E-6,4.9418386719323373E-2,40152.43920945024,1.1537979101579597E-5,1.3367108103300375E-5,3.1113070290945342E-4,0.28146915182859189,9.5069860117328285E-3,2.6226101504252124E-2,3.5787524555239543E-2,0.14080292296558702,9.9127315578265168E-5,9.9127315578265168E-5,6.6829114398686398E-2,1.3398391593938141E-5,1.3398391593938141E-5,0.12218227782462737,1.0255885692902714E-2,1.6121204342594271E-4,54.166666666666664,10.924681300086506,8.5677884211459755E-3,1.357152445279418E-2,2.2300524917366098E-2,3.2618281817216335E-2,0.25356729760892371,1.9546097822674517E-2,4.4167683130395265E-4,0,4.1510202663689374E-4,8.5677885794084639E-4,2.0476901720403631E-2,2.0581419729679196E-2,2.7816086226437942E-2,6.0288887472989539E-4,8.1514158638787804E-2,0.11741420890119955,1.5,0.92740622145210061,6.3791679602342981E-3,1.2130549338868389E-2,4.8457317416625957E-3,1.3787763700008608E-2,0,2.566454680269539E-4,5.2972136217531093E-4,5.8778919830260786E-3,1.6214833132985142E-2,8.2838344811131723E-6,6.1287526122085905E-5,1.7197874281897754E-2,7.728975032948833E-2,0.92740622145210061,92.740622145210068,125,48.564555994658186,0.48564555994658187,40.152439209450243,null,8.3908774747404255E-3,null,8.1514158638787804E-2,2.7816086226437942E-2,3.5787524555239543E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR31, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.740622145210068},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ31, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.1514158638787804E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA31, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.7816086226437942E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB31, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.5787524555239543E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S31, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":40.152439209450243},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P31, IF(MODE_ILIM=4,#REF!,#REF!))","v":104.69131998803746}]
["RCoutESR",{"$f":"'Design Converter'!E26","v":5.0000000000000001E-3},"mW",{"$f":"B32","v":5.0000000000000001E-3},"Output capacitor ESR",null,null,26,0.13,0.95232360099097058,0.95232360099097058,0,54.950313569759132,51.606550303217816,2,103.21310060643563,5.3072098708103659E-6,5.1395122188096311E-2,41758.536777828253,1.1537979101579597E-5,1.2409220133881914E-5,3.2317593102583155E-4,0.28704333952968009,9.8872654522021448E-3,2.7275145564422214E-2,3.7221293706440353E-2,0.14359137035448596,1.0309240820139575E-4,1.0309240820139575E-4,6.8595548387957755E-2,1.4116047775933961E-5,1.4116047775933961E-5,0.12460196376859799,1.0666121120618821E-2,1.6766052516298044E-4,54.166666666666664,10.924681300086506,8.9846322476933686E-3,1.4114385430905948E-2,2.3266678203762298E-2,3.3999870839028175E-2,0.25858891970337822,2.0327941735581497E-2,4.5934390455611086E-4,0,4.3555080484634478E-4,8.9489470940245564E-4,2.1302928058618921E-2,2.1364359557243775E-2,2.8888412713872873E-2,6.2700442971909127E-4,8.4818216041239056E-2,0.12215671820365673,1.56,0.92738089330100848,6.3806139577337658E-3,1.2132064229431498E-2,4.8455994011381686E-3,1.3831456933815501E-2,0,2.5892403492075412E-4,5.3199247116409983E-4,5.8777314534406572E-3,1.6214390293877508E-2,8.3916365361059933E-6,6.1285852314335002E-5,1.7173437172204896E-2,7.7315887436577302E-2,0.92738089330100848,92.738089330100848,130,50.254747979561841,0.50254747979561842,41.758536777828255,null,8.3906483136591652E-3,null,8.4818216041239056E-2,2.8888412713872873E-2,3.7221293706440353E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR32, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.738089330100848},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ32, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.4818216041239056E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA32, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.8888412713872873E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB32, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7221293706440353E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S32, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":41.758536777828255},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P32, IF(MODE_ILIM=4,#REF!,#REF!))","v":103.21310060643563}]
["Controller",null,"Units","Std Units","Description",null,null,27,0.13500000000000001,0.95232360099097058,0.95232360099097058,0,54.723040842486405,50.867531511974619,2,101.73506302394924,5.3072098708103659E-6,5.3371857656869241E-2,43364.634346206258,1.1537979101579597E-5,1.152228682886482E-5,3.3522115914220963E-4,0.29251132303826366,1.0267544892671452E-2,2.8324189624592291E-2,3.8655237619278589E-2,0.14632668985836203,1.0705750082452636E-4,1.0705750082452636E-4,7.0366786350914395E-2,1.4854453864065699E-5,1.4854453864065699E-5,0.12697554778605044,1.1076356548334927E-2,1.7410900690001814E-4,54.166666666666664,10.924681300086506,9.4071785580639583E-3,1.4657246409017714E-2,2.423853397398169E-2,3.5387384131684171E-2,0.26351486555795645,2.1109785648488467E-2,4.7701097780826886E-4,0,4.5629966545338241E-4,9.3331064326165132E-4,2.2129495481939404E-2,2.2147299384808351E-2,2.9960739201307797E-2,6.5111998470828705E-4,8.8128738799639672E-2,0.12690588837360686,1.62,0.9273539065737777,6.3820553997228843E-3,1.2133558527535612E-2,4.8454583944921911E-3,1.3875122944687131E-2,0,2.6120449217685305E-4,5.3426498214541839E-4,5.8775604118151293E-3,1.6213918456112419E-2,8.5032937165810316E-6,6.1284068899783914E-5,1.7150746013685745E-2,7.7343676984989743E-2,0.9273539065737777,92.735390657377764,135,51.875007795911799,0.51875007795911798,43.364634346206259,null,8.3904041463068214E-3,null,8.8128738799639672E-2,2.9960739201307797E-2,3.8655237619278589E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR33, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.735390657377764},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ33, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.8128738799639672E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA33, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.9960739201307797E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB33, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.8655237619278589E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S33, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":43.364634346206259},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P33, IF(MODE_ILIM=4,#REF!,#REF!))","v":101.73506302394924}]
["Deadtime1",20,"ns",{"$f":"B34/1000000000","v":2E-8},"PMOS off to NMOS on deadtime",null,null,28,0.14000000000000001,0.95232360099097058,0.95232360099097058,0,54.495768115213679,50.128607640537489,2,100.25721528107498,5.3072098708103659E-6,5.5348593125642179E-2,44970.73191458427,1.1537979101579597E-5,1.0698705902777521E-5,3.4726638725858782E-4,0.29787895098989409,1.0647824333140767E-2,2.9373233684762381E-2,4.0089356325708723E-2,0.14901180721517138,1.11022593447657E-4,1.11022593447657E-4,7.2144098863200626E-2,1.5614313002349798E-5,1.5614313002349798E-5,0.12930556869734636,1.1486591976051038E-2,1.8055748863705587E-4,54.166666666666664,10.924681300086506,9.8354273522577446E-3,1.5200107387129482E-2,2.5216092228024282E-2,3.678082304653256E-2,0.26835040403676602,2.1891629561395454E-2,4.9467805106042707E-4,0,4.7734909028727718E-4,9.7202714134770425E-4,2.295660470983343E-2,2.2930239212372933E-2,3.1033065688742728E-2,6.7523553969748293E-4,9.1445728984806199E-2,0.13166172221696493,1.6800000000000002,0.92732543796540123,6.3834934947768806E-3,1.2135034537012118E-2,4.8453096449625234E-3,1.3918764148290812E-2,0,2.6348687750775901E-4,5.3653898485983142E-4,5.8773799780407242E-3,1.6213420709037113E-2,8.6187795496624312E-6,6.1282187555299525E-5,1.712961382810858E-2,7.7372943169701308E-2,0.92732543796540123,92.732543796540128,140,53.420714247122767,0.53420714247122769,44.97073191458427,null,8.3901465713636762E-3,null,9.1445728984806199E-2,3.1033065688742728E-2,4.0089356325708723E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR34, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.732543796540128},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ34, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1445728984806199E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA34, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.1033065688742728E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB34, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.0089356325708723E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S34, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":44.97073191458427},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P34, IF(MODE_ILIM=4,#REF!,#REF!))","v":100.25721528107498}]
["Deadtime2",20,"ns",{"$f":"B35/1000000000","v":2E-8},"NMOS off to PMOS on deadtime",null,null,29,0.14499999999999999,0.95232360099097058,0.95232360099097058,0,54.268495387940952,49.389782949211458,2,98.779565898422916,5.3072098708103659E-6,5.7325328594415109E-2,46576.829482962276,1.1537979101579597E-5,9.9319236612479679E-6,3.5931161537496595E-4,0.30315155414426626,1.102810377361008E-2,3.0422277744932461E-2,4.1523649857692885E-2,0.15164938909918996,1.1498768607078757E-4,1.1498768607078757E-4,7.3928617150449183E-2,1.6396321301333067E-5,1.6396321301333067E-5,0.13159434051934274,1.1896827403767143E-2,1.8700597037409354E-4,54.166666666666664,10.924681300086506,1.0269378630274726E-2,1.574296836524125E-2,2.6199352965890071E-2,3.8180188935332586E-2,0.27310033746475537,2.267347347430243E-2,5.1234512431258506E-4,0,4.9869956117729953E-4,1.0110446854898845E-3,2.3784256462187171E-2,2.3713179039937513E-2,3.2105392176177652E-2,6.993510946866786E-4,9.4769188668384088E-2,0.1364242225334491,1.7399999999999998,0.92729563981578944,6.3849292849495528E-3,1.2136494244329301E-2,4.8451539485308247E-3,1.3962382627163643E-2,0,2.657712233665273E-4,5.3881455661706676E-4,5.8771911176463696E-3,1.6212899716172874E-2,8.7380673860602904E-6,6.1280218348246042E-5,1.7109879413531898E-2,7.7403534418042347E-2,0.92729563981578944,92.729563981578949,145,54.888490199331855,0.54888490199331852,46.576829482962275,null,8.389876967152942E-3,null,9.4769188668384088E-2,3.2105392176177652E-2,4.1523649857692885E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR35, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.729563981578949},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ35, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.4769188668384088E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA35, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.2105392176177652E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB35, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.1523649857692885E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S35, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":46.576829482962275},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P35, IF(MODE_ILIM=4,#REF!,#REF!))","v":98.779565898422916}]
["Sleep delay",5,"µs",{"$f":"B36/1000000","v":5.0000000000000004E-6},"Delay time to enter sleep mode",null,null,30,0.15,0.95232360099097058,0.95232360099097058,0,54.041222660668218,48.651061956503348,2,97.302123913006696,5.3072098708103659E-6,5.9302064063188047E-2,48182.927051340288,1.1537979101579597E-5,9.2162602358203785E-6,3.7135684349134403E-4,0.3083340073967325,1.1408383214079394E-2,3.1471321805102551E-2,4.2958118247201117E-2,0.15424187414182841,1.1895277869391818E-4,1.1895277869391818E-4,7.5721348460639451E-2,1.7201167838092755E-5,1.7201167838092755E-5,0.13384397938382328,1.2307062831483254E-2,1.9345445211113127E-4,54.166666666666664,10.924681300086506,1.0709032392114903E-2,1.6285829343353018E-2,2.7188316187579054E-2,3.9585483150254674E-2,0.27776905749206654,2.3455317387209414E-2,5.3001219756474327E-4,0,5.2035155995271989E-4,1.0503637575174632E-3,2.4612451459305074E-2,2.4496118867502085E-2,3.3177718663612576E-2,7.234666496758746E-4,9.8099119922848199E-2,0.14119339211658133,1.7999999999999998,0.92726464416683851,6.3863636735123873E-3,1.213793937145885E-2,4.8449919951208719E-3,1.4005980186206106E-2,0,2.6805755782289897E-4,5.410917643667633E-4,5.8769946675123691E-3,1.621235778614916E-2,8.8611304303573041E-6,6.1278170004595964E-5,1.709140305049011E-2,7.7435319353074475E-2,0.92726464416683851,92.726464416683854,150,56.276153038808332,0.5627615303880833,48.182927051340286,null,8.3895965283478299E-3,null,9.8099119922848199E-2,3.3177718663612576E-2,4.2958118247201117E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR36, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.726464416683854},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ36, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.8099119922848199E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA36, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.3177718663612576E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB36, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.2958118247201117E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S36, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":48.182927051340286},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P36, IF(MODE_ILIM=4,#REF!,#REF!))","v":97.302123913006696}]
["IQ(active)",660,"µA",{"$f":"B37/1000000","v":6.6E-4},"LM5164 quiescent current - active state ",null,null,31,0.155,0.95232360099097058,0.95232360099097058,0,53.813949933395499,47.912449458933729,2,95.824898917867458,5.3072098708103659E-6,6.1278799531960977E-2,49789.024619718293,1.1537979101579597E-5,8.5467686442913491E-6,3.8340207160772217E-4,0.31343078255744528,1.1788662654548705E-2,3.2520365865272627E-2,4.4392761526211147E-2,0.15679149933401923,1.2291787131704876E-4,1.2291787131704876E-4,7.7523189339784998E-2,1.8029534656236462E-5,1.8029534656236462E-5,0.13605642644827143,1.2717298259199365E-2,1.9990293384816894E-4,54.166666666666664,10.924681300086506,1.1154388637778278E-2,1.6828690321464782E-2,2.8182981893091229E-2,4.0996707043880615E-2,0.28236059264121588,2.423716130011639E-2,5.4767927081690127E-4,0,5.4230556844280897E-4,1.0899848392597103E-3,2.5441190421910023E-2,2.5279058695066664E-2,3.4250045151047508E-2,7.4758220466507016E-4,0.10143552482150321,0.14596923375368764,1.8599999999999999,0.92723256603465376,6.3877974473275402E-3,1.2139371418515182E-2,4.8448243856960647E-3,1.4049558397440412E-2,0,2.7034590526995022E-4,5.433706663686296E-4,5.8767913566097263E-3,1.6211796929915326E-2,8.9879417654370196E-6,6.1276050125174466E-5,1.7074063038821793E-2,7.7468183537855229E-2,0.92723256603465376,92.723256603465373,155,57.582635216683897,0.57582635216683897,49.78902461971829,null,8.3893062955775997E-3,null,0.10143552482150321,3.4250045151047508E-2,4.4392761526211147E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR37, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.723256603465373},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ37, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10143552482150321},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA37, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.4250045151047508E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB37, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.4392761526211147E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S37, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":49.78902461971829},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P37, IF(MODE_ILIM=4,#REF!,#REF!))","v":95.824898917867458}]
["IQ(sleep)",10,"µA",{"$f":"B38/1000000","v":1.0000000000000001E-5},"LM5164 quiescent current - sleep state",null,null,32,{"$f":"IF(PLOT_TYPE=1, H38/100*Iout, min_I*EXP(H38*rr/100))","v":0.16},{"$f":"IF(I38<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I38-Vout)/L*OnTime)","v":0.95232360099097058},{"$f":"IF(I38<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I38+((Vin-(Rdcr+RdsonTop)*J38-Vout)/L*OnTime)/2)","v":0.95232360099097058},{"$f":"IF(I38<Icrit, 0, I38-((Vin-(Rdcr+RdsonTop)*K38-Vout)/L*OnTime)/2)","v":0},53.586677206122772,{"$f":"IF(I38<Icrit, 1000*SQRT((J38*CoutEsr)^2+(((J38/2)-I38)*(OnTime+OffTime)/Cout)^2), 1000*J38*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":47.173950552696695},2,{"$f":"IF(I38<Icrit, 1000*((N38/1000)*O38), 1000*J38*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":94.34790110539339},{"$f":"IF(I38<Icrit, L*J38/(Vout+J38/2*(RdsonBot+Rdcr)), L*J38/(Vout+I38*(RdsonBot+Rdcr)))","v":5.3072098708103659E-6},6.3255535000733915E-2,{"$f":"IF(I38<Icrit,I38/((OnTime+Q38)*J38/2),1/(OnTime+Q38))","v":51395.122188096306},1.1537979101579597E-5,7.9191202772328823E-6,{"$f":"S38*(T38*Iq_active+U38*Iq_sleep)","v":3.954472997241003E-4},0.31844599352451719,{"$f":"W38^2*Rdcr","v":1.216894209501802E-2},{"$f":"Core_Loss/1000*S38/$S$106","v":3.3569409925442717E-2},{"$f":"(Y38+X38*(1+Ltc*(Ta-25)))/(1-X38*Ltc*ThetaCa)","v":4.5827579726708603E-2},0.15930032262376584,1.2688296394017942E-4,1.2688296394017942E-4,7.9334937167056113E-2,1.8882096765902223E-5,1.8882096765902223E-5,0.13823346750498039,1.3127533686915474E-2,2.0635141558520667E-4,{"$f":"20*VIN_nom/24","v":54.166666666666664},{"$f":"IF(I38<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I38+Iripple/2)*1000000000)","v":10.924681300086506},{"$f":"IF(I38<Icrit, Vin*(I38+Iripple/2)*AK38/1000000000/2*S38, Vin*(I38-Iripple/2)*AJ38/1000000000/2*S38 + Vin*(I38+Iripple/2)*AK38/1000000000/2*S38)","v":1.1605447367264852E-2},{"$f":"IF(I38<Icrit, Csw*(Vin)^2*S38/2, Csw*Vin^2*S38/2)","v":1.737155129957655E-2},2.9183350082426611E-2,{"$f":"(AI38+AL38+AM38+AH38*(1+RdsonTopTc*(Ta-25)))/(1-AH38*RdsonTopTc*ThetaJA)","v":4.241386196920368E-2},{"$f":"IF(I38<Icrit,Iripple*SQRT((OffTime)*S38/3), SQRT(OffTime*S38*(I38^2+Iripple^2/12)))","v":0.28687864900226784},2.5019005213023381E-2,{"$f":"QgBot*S38*Vdd","v":5.6534634406905948E-4},{"$f":"IF(I38<Icrit, Vin*Idss*R38, QrrBot*(I38-Iripple/2)/1*S38*Vin+Vin*Idss*R38)","v":0},{"$f":"IF(I38<Icrit, dead1*S38*(I38+Iripple/2)*((I38+Iripple/2)*BDserR+VSD), dead1*S38*(I38+Iripple/2)*((I38+Iripple/2)*BDserR+VSD)+dead2*S38*(I38-Iripple/2)*((I38-Iripple/2)*BDserR+VSD))","v":5.6456206847683716E-4},1.1299084125458965E-3,{"$f":"(AR38+AS38+AT38+AQ38*(1+RdsonBotTc*(Ta-25)))/(1-AQ38*RdsonBotTc*ThetaJA)","v":2.627047407114378E-2},{"$f":"Vin*V38+Vout*Ifb/0.8","v":2.6061998522631243E-2},{"$f":"(Vin-Vdd)*(S38*QgBot+S38*QgTop)+AW38","v":3.5322371638482439E-2},{"$f":"AI38+AR38","v":7.7169775965426615E-4},0.10477840543848417,{"$f":"SUM(Z38,AC38,AF38,AZ38)","v":0.15075175022589887},{"$f":"Vout*I38","v":1.92},0.9271995060685313,6.3892312950278802E-3,1.2140791698403874E-2,{"$f":"Vin*S38*(QgBot+QgTop)/($BB38+$BA38)","v":4.8446516461526879E-3},1.4093118636380722E-2,0,2.7263628699830819E-4,5.4565131354960086E-4,{"$f":"X38/($BB38+$BA38)","v":5.8765818228527431E-3},{"$f":"Y38/($BB38+$BA38)","v":1.6211218907230488E-2},9.1184743723347667E-6,6.1273865361377927E-5,1.705775288352605E-2,7.7502026829856074E-2,{"$f":"BC38","v":0.9271995060685313},92.719950606853132,{"$f":"I38*1000","v":160},58.807882255999409,0.58807882255999411,{"$f":"S38/1000","v":51.395122188096309},null,{"$f":"AM38/($BB38+$BA38)","v":8.3890071794851719E-3},null,0.10477840543848417,3.5322371638482439E-2,4.5827579726708603E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR38, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.719950606853132},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ38, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10477840543848417},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA38, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.5322371638482439E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB38, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.5827579726708603E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S38, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":51.395122188096309},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P38, IF(MODE_ILIM=4,#REF!,#REF!))","v":94.34790110539339}]
["High-side N-ch MOSFET",null,"Units","Std Units","Description",null,null,33,0.16500000000000001,0.95232360099097058,0.95232360099097058,0,{"$f":"IF(I39<Icrit, 1000*((((J39/2)-I39)*0.000002/Cout+Vout/306)), 1000*J39*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":53.359404478850045},46.435570657371152,2,92.871141314742303,5.3072098708103659E-6,6.5232270469506859E-2,53001.219756474318,{"$f":"IF(1/S39-OnTime-Q39>Tsleep, OnTime+Q39+Tsleep, 1/S39)","v":1.1537979101579597E-5},{"$f":"IF(1/S39-OnTime-Q39>Tsleep, 1/S39-OnTime-Q39-Tsleep, 0)","v":7.3295112051476537E-6},4.0749252784047849E-4,{"$f":"IF(I39<Icrit,Iripple*SQRT((OnTime+OffTime)*S39/3), SQRT(I39^2+Iripple^2/12))","v":0.323383435149454},1.2549221535487334E-2,3.4618453985612807E-2,4.7262572880686839E-2,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q39)*S39)","v":0.16177024235829654},1.3084805656331E-4,1.3084805656331E-4,{"$f":"SQRT($R39)*SQRT($I39^2*(1-R39)+(Iripple^2)/12)","v":8.115730023388415E-2},1.9759522143758438E-5,1.9759522143758438E-5,{"$f":"IF(I39<Icrit,Iripple*SQRT((OnTime)*S39/3), SQRT(OnTime*S39*(I39^2+Iripple^2/12)))","v":0.14037674985205723},{"$f":"RdsonTop*AG39^2","v":1.3537769114631584E-2},{"$f":"QgTop*S39*Vdd","v":2.127998973222444E-4},54.166666666666664,10.924681300086506,1.2062208580574618E-2,1.7914412277688318E-2,3.0189420755585179E-2,4.3836949279628785E-2,0.2913266452455629,{"$f":"RdsonBot*AP39^2","v":2.5800849125930354E-2},5.8301341732121758E-4,0,5.8712154188407517E-4,1.1701349592052926E-3,2.7100303128567153E-2,2.6844938350195826E-2,3.639469812591737E-2,7.9581331464346193E-4,0.10812776384875677,0.15554094430815069,1.98,0.9271655527267163,6.39066582189319E-3,1.2142201365173281E-2,4.8444742386883396E-3,1.4136662111793704E-2,0,2.7492872166601538E-4,5.479337506143579E-4,5.8763666268889523E-3,1.6210625264704591E-2,9.2527011464816069E-6,6.1271621558958562E-5,1.7042378992039475E-2,7.7536761216167344E-2,0.9271655527267163,92.716555272671627,165,59.95273560232264,0.59952735602322638,53.00121975647432,null,8.3886999804127071E-3,null,0.10812776384875677,3.639469812591737E-2,4.7262572880686839E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR39, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.716555272671627},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ39, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10812776384875677},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA39, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.639469812591737E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB39, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.7262572880686839E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S39, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":53.00121975647432},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P39, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.871141314742303}]
["RdsonTop",687,"mW",{"$f":"B40/1000","v":0.68700000000000006},"Drain-source resistance of high-side MOSFET @ VDD, 25°C",null,null,34,0.17,0.95232360099097058,0.95232360099097058,0,53.132131751577312,45.697315541913255,2,91.394631083826511,5.3072098708103659E-6,6.7209005938279789E-2,54607.317324852331,1.1537979101579597E-5,6.7745850196556733E-6,4.1953775595685662E-4,0.32824661683908546,1.2929500975956645E-2,3.5667498045782897E-2,4.8697741020147046E-2,0.1642030140931893,1.3481314918644061E-4,1.3481314918644061E-4,8.2990906596252897E-2,2.066247173300392E-5,2.066247173300392E-5,0.14248779687960517,1.3948004542347688E-2,2.192483790592821E-4,54.166666666666664,10.924681300086506,1.2524672277707585E-2,1.8457273255800086E-2,3.1201193912566955E-2,4.5265970328972678E-2,0.29570774289271118,2.6582693038837341E-2,6.0068049057337568E-4,0,6.0998447049379306E-4,1.2106649610671687E-3,2.7930678316160435E-2,2.7627878177760405E-2,3.7467024613352301E-2,8.1992886963265781E-4,0.11148360212811807,0.16033681876918457,2.04,0.92713078406838045,6.3921015621023064E-3,1.2143601437365304E-2,4.8442925711650736E-3,1.4180189890209697E-2,0,2.7722322568551287E-4,5.5021801695996056E-4,5.8761462634566546E-3,1.6210017367129473E-2,9.3905949110836625E-6,6.1269323876447172E-5,1.7027858777689524E-2,7.757230903055104E-2,0.92713078406838045,92.713078406838051,170,61.018807215515402,0.61018807215515403,54.607317324852332,null,8.388385404614845E-3,null,0.11148360212811807,3.7467024613352301E-2,4.8697741020147046E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR40, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.713078406838051},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ40, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11148360212811807},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA40, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7467024613352301E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB40, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.8697741020147046E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S40, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":54.607317324852332},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P40, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.394631083826511}]
["RdsonTopTc",4500,"ppm/°C",{"$f":"B41/1000000","v":4.4999999999999997E-3},"Drain to Source Resistance Temp Co",null,null,35,0.17499999999999999,0.95232360099097058,0.95232360099097058,0,52.904859024304585,44.959191353189503,2,89.918382706379006,5.3072098708103659E-6,6.9185741407052706E-2,56213.414893230329,1.1537979101579597E-5,6.2513689019061005E-6,4.3158298407323465E-4,0.33303879173986572,1.3309780416425958E-2,3.6716542105952966E-2,5.0133084177098185E-2,0.16660026519160839,1.3877824180957122E-4,1.3877824180957122E-4,8.4836311886219748E-2,2.1591599443367852E-5,2.1591599443367852E-5,0.14456802073826769,1.4358239970063795E-2,2.2569686079631975E-4,54.166666666666664,10.924681300086506,1.299283845866374E-2,1.900013423391185E-2,3.2218669553371909E-2,4.6700926471464045E-2,0.30002487260787136,2.736453695174431E-2,6.1834756382553367E-4,0,6.3315133613526164E-4,1.2514988999607953E-3,2.8761600356323577E-2,2.8410818005324977E-2,3.8539351100787218E-2,8.4404442462185348E-4,0.11484592235319668,0.1651393763715478,2.0999999999999996,0.92709526923854069,6.3935389888858801E-3,1.2144992817364871E-2,4.8441070048681548E-3,1.4223702916233765E-2,0,2.7951981354431535E-4,5.5250414743375769E-4,5.8759211707963242E-3,1.6209396423441279E-2,9.5321284282094509E-6,6.126697688328369E-5,1.7014119088125227E-2,7.7608601476005082E-2,0.92709526923854069,92.709526923854071,175,62.00835196729512,0.62008351967295117,56.213414893230329,null,8.3880640776937722E-3,null,0.11484592235319668,3.8539351100787218E-2,5.0133084177098185E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR41, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.709526923854071},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ41, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11484592235319668},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA41, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.8539351100787218E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB41, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.0133084177098185E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S41, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":56.213414893230329},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P41, IF(MODE_ILIM=4,#REF!,#REF!))","v":89.918382706379006}]
["QgTop",0.80300000000000005,"nC",{"$f":"B42/1000000000","v":8.0300000000000002E-10},"Gate charge of high-side MOSFET @ VDD",null,null,36,0.18,0.95232360099097058,0.95232360099097058,0,52.677586297031866,44.221204647343946,2,88.442409294687891,5.3072098708103659E-6,7.116247687582565E-2,57819.512461608341,1.1537979101579597E-5,5.7572203462537165E-6,4.4362821218961283E-4,0.33776298219431022,1.3690059856895271E-2,3.7765586166123057E-2,5.1568602383557108E-2,0.1689635075587044,1.427433344327018E-4,1.427433344327018E-4,8.6694006234783169E-2,2.2547552151109871E-5,2.2547552151109871E-5,0.14661873338955284,1.4768475397779908E-2,2.3214534253335748E-4,54.166666666666664,10.924681300086506,1.3466707123443101E-2,1.9542995212023618E-2,3.3241847678000078E-2,4.8141819061743751E-2,0.3042807571307084,2.8146380864651297E-2,6.3601463707769177E-4,0,6.5662262063775163E-4,1.2926372577154433E-3,2.959306997187662E-2,2.919375783288956E-2,3.9611677588222149E-2,8.6815997961104925E-4,0.11821472660145357,0.16994861987159449,2.16,0.92705906970559693,6.3949785229876965E-3,1.2146376307525972E-2,4.8439178609722411E-3,1.4267202029473104E-2,0,2.8181849807226158E-4,5.547921729650337E-4,5.875691738494105E-3,1.6208763508357683E-2,9.677274408030716E-6,6.1264584641599728E-5,1.7001094895562622E-2,7.7645577393460355E-2,0.92705906970559693,92.705906970559695,180,62.924142868481049,0.62924142868481048,57.81951246160834,null,8.3877365557960878E-3,null,0.11821472660145357,3.9611677588222149E-2,5.1568602383557108E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR42, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.705906970559695},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ42, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11821472660145357},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA42, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.9611677588222149E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB42, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.1568602383557108E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S42, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":57.81951246160834},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P42, IF(MODE_ILIM=4,#REF!,#REF!))","v":88.442409294687891}]
["Coss",100,"pF",{"$f":"B43/1000000000000","v":1E-10},"Capacitance (Coss)",null,null,37,0.185,0.95232360099097058,0.95232360099097058,0,52.450313569759132,43.483362424332832,2,86.966724848665663,5.3072098708103659E-6,7.3139212344598595E-2,59425.610029986354,1.1537979101579597E-5,5.2897825233393044E-6,4.5567344030599102E-4,0.34242200203555589,1.4070339297364589E-2,3.881463022629314E-2,5.3004295671548372E-2,0.17129414879430788,1.4670842705583243E-4,1.4670842705583243E-4,8.8564420431344687E-2,2.3530969699019954E-5,2.3530969699019954E-5,0.14864115628362609,1.5178710825496017E-2,2.3859382427039521E-4,54.166666666666664,10.924681300086506,1.3946278272045651E-2,2.0085856190135386E-2,3.4270728286451432E-2,4.958864945486486E-2,0.30847793136090768,2.8928224777558277E-2,6.5368171032984988E-4,0,6.8039880583053308E-4,1.334080516160383E-3,3.0425087886059906E-2,2.9976697660454139E-2,4.0684004075657081E-2,8.9227553460024503E-4,0.1215900169511821,0.17476455201948532,2.2199999999999998,0.92702224029827573,6.396420539754504E-3,1.2147752623683743E-2,4.8437254259594562E-3,1.4310687978720584E-2,0,2.84119290665447E-4,5.5708212109426957E-4,5.8754583140539591E-3,1.6208119580507857E-2,9.8260055165659117E-6,6.1262150774745036E-5,1.6988728199333249E-2,7.7683182230064374E-2,0.92702224029827573,92.702224029827576,185,63.769353027551922,0.63769353027551923,59.425610029986352,null,8.387403334994728E-3,null,0.1215900169511821,4.0684004075657081E-2,5.3004295671548372E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR43, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.702224029827576},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ43, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1215900169511821},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA43, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.0684004075657081E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB43, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.3004295671548372E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S43, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":59.425610029986352},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P43, IF(MODE_ILIM=4,#REF!,#REF!))","v":86.966724848665663}]
["Low-side N-ch MOSFET",null,"Units","Std Units","Description",null,null,38,0.19,0.95232360099097058,0.95232360099097058,0,52.223040842486412,42.745672166004475,2,85.49134433200895,5.3072098708103659E-6,7.5115947813371525E-2,61031.707598364366,1.1537979101579597E-5,4.8469466911045944E-6,4.6771866842236915E-4,0.34701847618719456,1.4450618737833902E-2,3.986367428646323E-2,5.4440164073104418E-2,0.17359350199760534,1.5067351967896304E-4,1.5067351967896304E-4,9.0447931423588479E-2,2.4542484896418496E-5,2.4542484896418496E-5,0.15063642886735573,1.5588946253212119E-2,2.4504230600743294E-4,54.166666666666664,10.924681300086506,1.4431551904471407E-2,2.0628717168247154E-2,3.5305311378725994E-2,5.1041419006292936E-2,0.3126187600150902,2.9710068690465261E-2,6.7134878358200809E-4,0,7.0448037354287724E-4,1.3758291571248854E-3,3.1257654822534418E-2,3.0759637488018719E-2,4.1756330563092012E-2,9.1639108958944102E-4,0.1249717954815088,0.1795871755591886,2.2800000000000002,0.92698483007890975,6.397865375106831E-3,1.2149122406533885E-2,4.8435299561822957E-3,1.4354161433899698E-2,0,2.8642220147481176E-4,5.5937401641886905E-4,5.8752212084324856E-3,1.6207465497700926E-2,9.9782943822020631E-6,6.1259678524997721E-5,1.6976967101643259E-2,7.772136717030026E-2,0.92698483007890975,92.698483007890971,190,64.547447140017496,0.645474471400175,61.031707598364363,null,8.3870648591901197E-3,null,0.1249717954815088,4.1756330563092012E-2,5.4440164073104418E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR44, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.698483007890971},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ44, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1249717954815088},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA44, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.1756330563092012E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB44, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.4440164073104418E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S44, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":61.031707598364363},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P44, IF(MODE_ILIM=4,#REF!,#REF!))","v":85.49134433200895}]
["RdsonBot",304,"mW",{"$f":"B45/1000","v":0.30399999999999999},"Drain-source resistance of low-side MOSFET @ VDD, 25°C",null,null,39,0.19500000000000001,0.95232360099097058,0.95232360099097058,0,51.995768115213686,42.008141878155257,2,84.016283756310514,5.3072098708103659E-6,7.7092683282144456E-2,62637.805166742372,1.1537979101579597E-5,4.4268203887280786E-6,4.7976389653874723E-4,0.35155485795609021,1.4830898178303211E-2,4.0912718346633313E-2,5.5876207620265461E-2,0.17586279441774696,1.5463861230209368E-4,1.5463861230209368E-4,9.2344867244397624E-2,2.5582723519156262E-5,2.5582723519156262E-5,0.15260561609091094,1.5999181680928225E-2,2.5149078774447061E-4,54.166666666666664,10.924681300086506,1.4922528020720348E-2,2.1171578146358921E-2,3.6345596954823742E-2,5.2500129071906119E-2,0.31670545320540383,3.0491912603372234E-2,6.8901585683416608E-4,0,7.2886780560405353E-4,1.4178836624382197E-3,3.2090771505382074E-2,3.1542577315583298E-2,4.2828657050526936E-2,9.4050664457863669E-4,0.12836006427239377,0.18441649322848047,2.34,0.92694688308242279,6.3993133305916255E-3,1.2150486231262199E-2,4.8433316817248643E-3,1.4397622996172593E-2,0,2.8872723956572768E-4,5.6166788097034102E-4,5.8749807007226259E-3,1.62068020298465E-2,1.0134113601214225E-5,6.1257170802400408E-5,1.6965765025466657E-2,7.7760088400726762E-2,0.92694688308242279,92.694688308242277,195,65.262084299350803,0.65262084299350809,62.637805166742375,null,8.3867215267963008E-3,null,0.12836006427239377,4.2828657050526936E-2,5.5876207620265461E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR45, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.694688308242277},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ45, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12836006427239377},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA45, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.2828657050526936E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB45, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.5876207620265461E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S45, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":62.637805166742375},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P45, IF(MODE_ILIM=4,#REF!,#REF!))","v":84.016283756310514}]
["RdsonBotTc",4500,"ppm/°C",{"$f":"B46/1000000","v":4.4999999999999997E-3},"Drain To Source Resitance Temp Co",null,null,40,0.2,0.95232360099097058,0.95232360099097058,0,51.768495387940952,41.270780137052839,2,82.541560274105677,5.3072098708103659E-6,7.90694187509174E-2,64243.902735120384,1.1537979101579597E-5,4.0277004014703858E-6,4.9180912465512548E-4,0.35603344434163914,1.5211177618772526E-2,4.1961762406803403E-2,5.7312426345079583E-2,0.17810317511219403,1.5860370492522428E-4,1.5860370492522428E-4,9.4255511438526229E-2,2.6652304309614449E-5,2.6652304309614449E-5,0.15454971505332218,1.6409417108644339E-2,2.5793926948150834E-4,54.166666666666664,10.924681300086506,1.5419206620792495E-2,2.1714439124470689E-2,3.7391585014744697E-2,5.3964781007995316E-2,0.3207400802311865,3.1273756516279221E-2,7.0668293008632429E-4,0,7.5356158384333352E-4,1.4602445139296578E-3,3.2924438659106083E-2,3.232551714314788E-2,4.3900983537961874E-2,9.6462219956783258E-4,0.1317548254046311,0.18925250775894553,2.4000000000000004,0.92690843894450914,6.4007646776772179E-3,1.2151844615730184E-2,4.8431308096851255E-3,1.444107320653246E-2,0,2.9103441305365667E-4,5.6396373453492606E-4,5.8747370421350399E-3,1.6206129869937719E-2,1.0293435742457808E-5,6.125463022627299E-5,1.6955080049708679E-2,7.7799306484963748E-2,0.92690843894450914,92.690843894450907,200,65.91703305041338,0.65917033050413376,64.243902735120386,null,8.3863736964244571E-3,null,0.1317548254046311,4.3900983537961874E-2,5.7312426345079583E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR46, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.690843894450907},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ46, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1317548254046311},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA46, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.3900983537961874E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB46, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.7312426345079583E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S46, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":64.243902735120386},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P46, IF(MODE_ILIM=4,#REF!,#REF!))","v":82.541560274105677}]
["QgBot",2.2000000000000002,"nC",{"$f":"B47/1000000000","v":2.2000000000000003E-9},"Gate charge of low-side MOSFET at VDD",null,null,41,0.20499999999999999,0.95232360099097058,0.95232360099097058,0,51.541222660668225,40.533596140988195,2,81.067192281976389,5.3072098708103659E-6,8.1046154219690317E-2,65850.000303498382,1.1537979101579597E-5,3.6480496818838024E-6,5.0385435277150339E-4,0.36045638963266458,1.5591457059241835E-2,4.3010806466973472E-2,5.8748820279602598E-2,0.18031572174846808,1.6256879754835481E-4,1.6256879754835481E-4,9.6180107050444053E-2,2.7751838976704633E-5,2.7751838976704633E-5,0.15646966090472508,1.6819652536360443E-2,2.6438775121854602E-4,54.166666666666664,10.924681300086506,1.5921587704687826E-2,2.2257300102582454E-2,3.8443275558488824E-2,5.5435376171264268E-2,0.32472458182800951,3.2055600429186197E-2,7.2435000333848228E-4,0,7.7856219008998672E-4,1.5029121934284689E-3,3.375865700863117E-2,3.3108456970712449E-2,4.4973310025396784E-2,9.8873775455702835E-4,0.13515608095984924,0.19409522187597689,2.46,0.92686953343792011,6.4022196614200704E-3,1.2153198027463227E-2,4.8429275269770266E-3,1.4484512553138998E-2,0,2.9334372921996393E-4,5.6626159492731963E-4,5.874490459397092E-3,1.6205449643427797E-2,1.0456233351375005E-5,6.1252059160653389E-5,1.6944874341625386E-2,7.7838985830108912E-2,0.92686953343792011,92.686953343792013,205,66.516098897051677,0.66516098897051679,65.850000303498376,null,8.3860216917351106E-3,null,0.13515608095984924,4.4973310025396784E-2,5.8748820279602598E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR47, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.686953343792013},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ47, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13515608095984924},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA47, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.4973310025396784E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB47, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8748820279602598E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S47, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":65.850000303498376},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P47, IF(MODE_ILIM=4,#REF!,#REF!))","v":81.067192281976389}]
["VSD",0.8,"V",{"$f":"B48","v":0.8},"Body diode forward voltage",null,null,42,0.21,0.95232360099097058,0.95232360099097058,0,51.313949933395499,39.79659976749965,2,79.5931995349993,5.3072098708103659E-6,8.3022889688463261E-2,67456.097871876394,1.1537979101579597E-5,3.2864775679918165E-6,5.1589958088788163E-4,0.36482571752037934,1.5971736499711155E-2,4.4059850527143563E-2,6.0185389455898256E-2,0.18250144666357329,1.6653389017148545E-4,1.6653389017148545E-4,9.8118860225525781E-2,2.8881932195868796E-5,2.8881932195868796E-5,0.15836633210444775,1.7229887964076557E-2,2.7083623295558374E-4,54.166666666666664,10.924681300086506,1.6429671272406365E-2,2.2800161080694221E-2,3.9500668586056172E-2,5.6911915918829915E-2,0.32866078107988994,3.2837444342093174E-2,7.4201707659064039E-4,0,8.0387010617328472E-4,1.5458871827639252E-3,3.4593427279303937E-2,3.3891396798277032E-2,4.6045636512831722E-2,1.0128533095462241E-3,0.13856383302051181,0.19894463829877743,2.52,0.92683019893216523,6.4036785036078658E-3,1.2154546889640828E-2,4.8427220027324512E-3,1.4527941477606339E-2,0,2.9565519461119297E-4,5.6856147822530688E-4,5.8742411576664343E-3,1.6204761916267435E-2,1.0622478953429518E-5,6.1249459744676678E-5,1.6935113670296032E-2,7.7879094229351992E-2,0.92683019893216523,92.683019893216525,210,67.063063929713536,0.6706306392971354,67.456097871876395,null,8.3856658055973168E-3,null,0.13856383302051181,4.6045636512831722E-2,6.0185389455898256E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR48, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.683019893216525},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ48, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13856383302051181},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA48, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.6045636512831722E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB48, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.0185389455898256E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S48, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":67.456097871876395},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P48, IF(MODE_ILIM=4,#REF!,#REF!))","v":79.5931995349993}]
["BDserR",100,"mW",{"$f":"B49*0.001","v":0.1},"Series resistance of body diode",null,null,43,0.215,0.95232360099097058,0.95232360099097058,0,51.086677206122772,39.059801637008029,2,78.119603274016058,5.3072098708103659E-6,8.4999625157236192E-2,69062.195440254407,1.1537979101579597E-5,2.9417227617227114E-6,5.2794480900425977E-4,0.36914333192068344,1.6352015940180462E-2,4.5108894587313646E-2,6.1622133906038025E-2,0.18466130227777344,1.7049898279461608E-4,1.7049898279461608E-4,0.10007194346915174,3.0043181609079307E-5,3.0043181609079307E-5,0.16024055511883628,1.7640123391792661E-2,2.7728471469262147E-4,54.166666666666664,10.924681300086506,1.69434573239481E-2,2.3343022058805989E-2,4.0563764097446706E-2,5.8394401608222284E-2,0.33255039316878132,3.3619288255000157E-2,7.5968414984279849E-4,0,8.2948581392249725E-4,1.5891699637652957E-3,3.5428750196893177E-2,3.4674336625841615E-2,4.7117963000266654E-2,1.0369688645354199E-3,0.14197808366991754,0.20380075974035927,2.58,0.92679046478909377,6.4051414054641662E-3,1.2155891586251324E-2,4.8425143903681432E-3,1.4571360380413871E-2,0,2.9796881512449261E-4,5.7086339897166887E-4,5.8739893230381861E-3,1.6204067201821184E-2,1.07921450570627E-5,6.1246833918717029E-5,1.6925766987958318E-2,7.7919602468387139E-2,0.92679046478909377,92.67904647890937,215,67.561637846160409,0.67561637846160405,69.062195440254413,null,8.3853063036677788E-3,null,0.14197808366991754,4.7117963000266654E-2,6.1622133906038025E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR49, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.67904647890937},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ49, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14197808366991754},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA49, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.7117963000266654E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB49, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1622133906038025E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S49, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":69.062195440254413},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P49, IF(MODE_ILIM=4,#REF!,#REF!))","v":78.119603274016058}]
["QrrBot",3,"nC",{"$f":"B50*0.000000001","v":3.0000000000000004E-9},"Reverse recovery charge of body diode at 100mA",null,null,44,0.22,0.95232360099097058,0.95232360099097058,0,50.859404478850045,38.323213183713072,2,76.646426367426145,5.3072098708103659E-6,8.6976360626009136E-2,70668.29300863242,1.1537979101579597E-5,2.6126386284658411E-6,5.3999003712063801E-4,0.37341102667000631,1.6732295380649777E-2,4.6157938647483736E-2,6.305905366210128E-2,0.18679618594486702,1.7446407541774669E-4,1.7446407541774669E-4,0.10203949860199385,3.1236177824838917E-5,3.1236177824838917E-5,0.16209310863009996,1.8050358819508769E-2,2.8373319642965915E-4,54.166666666666664,10.924681300086506,1.7462945859313028E-2,2.3885883036917757E-2,4.1632562092660447E-2,5.9882834597384874E-2,0.33639503410927268,3.4401132167907134E-2,7.773512230949567E-4,0,8.5540979516689512E-4,1.6327610182618518E-3,3.6264626487590129E-2,3.5457276453406197E-2,4.8190289487701585E-2,1.0610844195246159E-3,0.14539883499220121,0.20866358890754508,2.64,0.92675035770455194,6.4066085499844359E-3,1.2157232466543901E-2,4.8423048293708857E-3,1.461476962557956E-2,0,3.0028459608140055E-4,5.7316737034856797E-4,5.8737351247103798E-3,1.6203365966841028E-2,1.0965204156247144E-5,6.1244183446966166E-5,1.6916806068414149E-2,7.796048398547753E-2,0.92675035770455194,92.675035770455196,220,68.015419380100283,0.68015419380100284,70.668293008632418,null,8.3849434274820521E-3,null,0.14539883499220121,4.8190289487701585E-2,6.305905366210128E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR50, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.675035770455196},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ50, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14539883499220121},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA50, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.8190289487701585E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB50, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.305905366210128E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S50, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":70.668293008632418},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P50, IF(MODE_ILIM=4,#REF!,#REF!))","v":76.646426367426145}]
["TrrBot",20,"ns",{"$f":"B51*0.000000001","v":2E-8},"Reverse recovery time of body diode (not used)",null,null,45,0.22500000000000001,0.95232360099097058,0.95232360099097058,0,50.632131751577319,37.586846734732454,2,75.173693469464908,5.3072098708103659E-6,8.8953096094782066E-2,72274.390577010432,1.1537979101579597E-5,2.2981804566870527E-6,5.5203526523701614E-4,0.37763049423476441,1.7112574821119095E-2,4.7206982707653826E-2,6.4496148756175167E-2,0.18890694430903132,1.7842916804087732E-4,1.7842916804087732E-4,0.1040216394445258,3.2461504418180781E-5,3.2461504418180781E-5,0.16392472731697913,1.8460594247224876E-2,2.9018167816669688E-4,54.166666666666664,10.924681300086506,1.7988136878501152E-2,2.4428744015029525E-2,4.2707062571697374E-2,6.1377216244674661E-2,0.34019622859468396,3.5182976080814124E-2,7.950182963471148E-4,0,8.8164253173574894E-4,1.6766608280828637E-3,3.7101056878008853E-2,3.624021628097078E-2,4.9262615975136523E-2,1.0851999745138117E-3,0.14882608907233383,0.21353312850096806,2.7,0.92670990200450121,6.4080801039606517E-3,1.2158569848887243E-2,4.8420934468447275E-3,1.4658169544710286E-2,0,3.0260254229179118E-4,5.7547340432868757E-4,5.8734787168607302E-3,1.6202658636643726E-2,1.1141628732700367E-5,6.1241509937002257E-5,1.6908205193631162E-2,7.800171457682871E-2,0.92670990200450121,92.67099020045012,225,68.427867006324419,0.68427867006324417,72.274390577010436,null,8.3845773971337242E-3,null,0.14882608907233383,4.9262615975136523E-2,6.4496148756175167E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR51, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.67099020045012},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ51, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14882608907233383},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA51, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.9262615975136523E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB51, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.4496148756175167E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S51, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":72.274390577010436},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P51, IF(MODE_ILIM=4,#REF!,#REF!))","v":75.173693469464908}]
["Idss",0,"μA",{"$f":"B52/1000000","v":0},"Leakage current of low-side device",null,null,46,0.23,0.95232360099097058,0.95232360099097058,0,50.404859024304592,36.8507155986184,2,73.701431197236801,5.3072098708103659E-6,9.0929831563555011E-2,73880.488145388445,1.1537979101579597E-5,1.99739437933343E-6,5.6408049335339428E-4,0.38180333355437945,1.7492854261588409E-2,4.8256026767823909E-2,6.59334192203547E-2,0.19099437722823565,1.823942606640079E-4,1.823942606640079E-4,0.10601845425941732,3.3719737930668489E-5,3.3719737930668489E-5,0.16573610525930235,1.8870829674940991E-2,2.9663015990373461E-4,54.166666666666664,10.924681300086506,1.8519030381512477E-2,2.4971604993141293E-2,4.3787265534557501E-2,6.287754790886238E-2,0.34395541706261024,3.59648199937211E-2,8.126853695992729E-4,0,9.0818450545832887E-4,1.7208698750576018E-3,3.7938042095186461E-2,3.7023156108535356E-2,5.0334942462571447E-2,1.1093155295030075E-3,0.1522598479961233,0.21840938121507267,2.7600000000000002,0.92666911990252654,6.4095562197419619E-3,1.2159904024125014E-2,4.8418803588564652E-3,1.470156044052414E-2,0,3.049226581094858E-4,5.7778151180666614E-4,5.8732202402787285E-3,1.6201945599613094E-2,1.1321391257810292E-5,6.1238814856807313E-5,1.6899940881208473E-2,7.8043272140378636E-2,0.92666911990252654,92.666911990252657,230,68.802277733330541,0.68802277733330541,73.880488145388441,null,8.3842084136042661E-3,null,0.1522598479961233,5.0334942462571447E-2,6.59334192203547E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR52, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.666911990252657},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ52, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1522598479961233},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA52, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.0334942462571447E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB52, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.59334192203547E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S52, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":73.880488145388441},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P52, IF(MODE_ILIM=4,#REF!,#REF!))","v":73.701431197236801}]
["Csw",160,"pF",{"$f":"B53/1000000000000","v":1.5999999999999999E-10},"Effective SW node capacitance (CossHS + CossLS)",null,null,47,0.23499999999999999,0.95232360099097058,0.95232360099097058,0,50.177586297031858,36.114834164568585,2,72.229668329137169,5.3072098708103659E-6,9.2906567032327927E-2,75486.585713766442,1.1537979101579597E-5,1.7094077095267706E-6,5.761257214697723E-4,0.38593105712093312,1.787313370205771E-2,4.9305070827993985E-2,6.7370865086742671E-2,0.19305924131578808,1.8635935328713849E-4,1.8635935328713849E-4,0.10803000797679002,3.5011447870395949E-5,3.5011447870395949E-5,0.16752789901117701,1.9281065102657098E-2,3.0307864164077228E-4,54.166666666666664,10.924681300086506,1.9055626368346987E-2,2.5514465971253057E-2,4.4873170981240815E-2,6.4383830949132526E-2,0.34767396207277568,3.6746663906628084E-2,8.303524428514309E-4,0,9.3503619816390573E-4,1.7653886410153366E-3,3.8775582866583516E-2,3.7806095936099925E-2,5.1407268950006364E-2,1.1334310844922032E-3,0.15570011385021462,0.22329234973811482,2.82,0.92662803172448094,6.4110370367706105E-3,1.2161235258503189E-2,4.8416656716094349E-3,1.4744942589923147E-2,0,3.0724494748076656E-4,5.8009170271375809E-4,5.8729598237894408E-3,1.6201227211127728E-2,1.1504464194315344E-5,6.1236099549612878E-5,1.689199164662249E-2,7.8085136452284501E-2,0.92662803172448094,92.662803172448093,235,69.1417728033842,0.69141772803384205,75.486585713766445,null,8.3838366607955558E-3,null,0.15570011385021462,5.1407268950006364E-2,6.7370865086742671E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR53, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.662803172448093},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ53, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15570011385021462},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA53, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.1407268950006364E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB53, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.7370865086742671E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S53, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":75.486585713766445},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P53, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.229668329137169}]
["ThetaJA",41.1,"°C/W",null,"Thermal resistance",null,null,48,0.24,0.95232360099097058,0.95232360099097058,0,49.950313569759132,35.379218013861824,2,70.758436027723647,5.3072098708103659E-6,9.4883302501100872E-2,77092.683282144455,1.1537979101579597E-5,1.4334204842953874E-6,5.8817094958615044E-4,0.39001509738435158,1.8253413142527031E-2,5.0354114888164075E-2,6.8808486387449838E-2,0.19510225314448273,1.9032444591026912E-4,1.9032444591026912E-4,0.11005634422420113,3.6337196711987554E-5,3.6337196711987554E-5,0.16930073038140062,1.9691300530373212E-2,3.0952712337780996E-4,54.166666666666664,10.924681300086506,1.9597924839004705E-2,2.6057326949364825E-2,4.5964778911747342E-2,6.5896066725083705E-2,0.3513531540772753,3.7528507819535067E-2,8.4801951610358911E-4,0,9.6219809168174991E-4,1.810217607785339E-3,3.9613679920084244E-2,3.8589035763664507E-2,5.2479595437441295E-2,1.157546639481399E-3,0.15914688872209062,0.22818203675216273,2.88,0.92658665610505964,6.4125226829259956E-3,1.216256379623149E-2,4.8414494824706054E-3,1.4788316246682061E-2,0,3.0956941398682718E-4,5.8240398611816586E-4,5.8726975854994003E-3,1.62005037969979E-2,1.169081999777511E-5,6.1233365246890473E-5,1.6884337795182319E-2,7.8127288971339429E-2,0.92658665610505964,92.658665610505963,240,69.449289175978407,0.69449289175978413,77.092683282144449,null,8.3834623073084057E-3,null,0.15914688872209062,5.2479595437441295E-2,6.8808486387449838E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR54, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.658665610505963},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ54, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15914688872209062},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA54, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.2479595437441295E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB54, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.8808486387449838E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S54, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":77.092683282144449},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P54, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.758436027723647}]
["Inductor",null,"Units","Std Units","Description",null,null,49,0.245,0.95232360099097058,0.95232360099097058,0,49.723040842486412,34.643884045304212,2,69.287768090608424,5.3072098708103659E-6,9.6860037969873802E-2,78698.780850522468,1.1537979101579597E-5,1.1686980437673264E-6,6.0021617770252857E-4,0.39405681256002856,1.8633692582996336E-2,5.1403158948334159E-2,7.0246283154594621E-2,0.19712409215182181,1.9428953853339967E-4,1.9428953853339967E-4,0.1120974871805757,3.7697539896598005E-5,3.7697539896598005E-5,0.17105518895447833,2.010153595808932E-2,3.1597560511484768E-4,54.166666666666664,10.924681300086506,2.014592579348562E-2,2.6600187927476593E-2,4.7062089326077056E-2,6.7414256596728617E-2,0.3549942166524932,3.8310351732442051E-2,8.6568658935574721E-4,0,9.8967066784113223E-4,1.8553572571968794E-3,4.0452333983996912E-2,3.9371975591229083E-2,5.355192192487622E-2,1.181662194470595E-3,0.16260017470007235,0.23307844493309698,2.94,0.92654501016031099,6.4140132757041493E-3,1.2163889861731369E-2,4.841231880871961E-3,1.4831681643808003E-2,0,3.1189606088102845E-4,5.8471837031309163E-4,5.872433633889949E-3,1.6199775656481754E-2,1.1880431117861267E-5,6.1230613079752013E-5,1.6876961239451909E-2,7.8169712667330818E-2,0.92654501016031099,92.654501016031105,245,69.727575757335345,0.69727575757335347,78.698780850522468,null,8.3830855080033947E-3,null,0.16260017470007235,5.355192192487622E-2,7.0246283154594621E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR55, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.654501016031105},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ55, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16260017470007235},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA55, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.355192192487622E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB55, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0246283154594621E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S55, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":78.698780850522468},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P55, IF(MODE_ILIM=4,#REF!,#REF!))","v":69.287768090608424}]
["Ltc",4000,"ppm",{"$f":"Ltc","v":4.0000000000000001E-3},"Inductor DCR Temp Co",null,null,50,0.25,0.95232360099097058,0.95232360099097058,0,49.495768115213679,33.90885061677325,2,67.817701233546501,5.3072098708103659E-6,9.8836773438646747E-2,80304.87841890048,1.1537979101579597E-5,9.1456450086038819E-7,6.122614058189067E-4,0.39805749190564649,1.9013972023465657E-2,5.2452203008504249E-2,7.1684255420303447E-2,0.19912540327970729,1.9825463115653031E-4,1.9825463115653031E-4,0.11415344327105288,3.9093025831912469E-5,3.9093025831912469E-5,0.1727918343812255,2.0511771385805431E-2,3.2242408685188541E-4,54.166666666666664,10.924681300086506,2.0699629231789723E-2,2.7143048905588361E-2,4.8165102224229969E-2,6.8938401924494325E-2,0.35859831125283476,3.9092195645349027E-2,8.8335366260790531E-4,0,1.0174544084713228E-3,1.9008080710792281E-3,4.1291545787054122E-2,4.0154915418793666E-2,5.4624248412311158E-2,1.2057777494597908E-3,0.16605997387331939,0.23798157695061128,3,0.9265031096394527,6.4155089232557447E-3,1.216521366161427E-2,4.8410129491037466E-3,1.4875038995617061E-2,0,3.1422489112168349E-4,5.8703486289422488E-4,5.8721680687794956E-3,1.6199043064939678E-2,1.2073269999494118E-5,6.1227844088982685E-5,1.6869845338574739E-2,7.8212391869989115E-2,0.9265031096394527,92.650310963945273,250,69.979193442852676,0.69979193442852672,80.304878418900486,null,8.3827064053744529E-3,null,0.16605997387331939,5.4624248412311158E-2,7.1684255420303447E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR56, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.650310963945273},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ56, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16605997387331939},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA56, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.4624248412311158E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB56, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1684255420303447E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S56, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":80.304878418900486},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P56, IF(MODE_ILIM=4,#REF!,#REF!))","v":67.817701233546501}]
["ThetaCA",20,"°C/W",{"$f":"ThetaCa","v":40},"Inductor Core-to-Ambient thermal resistance",null,null,51,0.255,0.95232360099097058,0.95232360099097058,0,49.268495387940952,33.17413770530964,2,66.34827541061928,5.3072098708103659E-6,0.10081350890741968,81910.975987278493,1.1537979101579597E-5,6.7039697924391639E-7,6.2430663393528494E-4,0.40201836052530998,1.9394251463934972E-2,5.3501247068674339E-2,7.3122403216710444E-2,0.20110679937767442,2.0221972377966094E-4,2.0221972377966094E-4,0.11622420271777369,4.0524195892146458E-5,4.0524195892146458E-5,0.17451119846418292,2.0922006813521538E-2,3.2887256858892314E-4,54.166666666666664,10.924681300086506,2.1259035153917031E-2,2.7685909883700129E-2,4.9273817606206083E-2,7.0468504069222365E-2,0.36216654153863059,3.9874039558255997E-2,9.0102073586006341E-4,0,1.045549795401592E-3,1.9465705312616554E-3,4.2131316058413082E-2,4.0937855246358248E-2,5.5696574899746089E-2,1.2298933044489866E-3,0.1695262883318305,0.24289143546821276,3.06,0.92646096905883291,6.4170097253020237E-3,1.2166535386427226E-2,4.840792763014419E-3,1.4918388499566624E-2,0,3.1655590740098806E-4,5.8935347082811774E-4,5.8719009821725102E-3,1.6198306276176494E-2,1.2269309083845746E-5,6.1225059233893531E-5,1.6862974756495629E-2,7.8255312135701777E-2,0.92646096905883291,92.646096905883297,255,70.206518151218702,0.702065181512187,81.910975987278491,null,8.3823251307608947E-3,null,0.1695262883318305,5.5696574899746089E-2,7.3122403216710444E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR57, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.646096905883297},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ57, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1695262883318305},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA57, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.5696574899746089E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB57, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.3122403216710444E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S57, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":81.910975987278491},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P57, IF(MODE_ILIM=4,#REF!,#REF!))","v":66.34827541061928}]
[null,null,null,null,null,null,null,52,0.26,0.95232360099097058,0.95232360099097058,0,49.041222660668225,32.439767088638185,2,64.879534177276369,5.3072098708103659E-6,0.10279024437619262,83517.073555656505,1.1537979101579597E-5,4.3562051615115726E-7,6.3635186205166308E-4,0.40594058375173869,1.9774530904404286E-2,5.4550291128844429E-2,7.4560726575957692E-2,0.20306886339505203,2.0618481640279155E-4,2.0618481640279155E-4,0.11830974095997045,4.1991584418045931E-5,4.1991584418045931E-5,0.17621378705987228,2.1332242241237642E-2,3.3532105032596087E-4,54.166666666666664,10.924681300086506,2.1824143559867532E-2,2.8228770861811896E-2,5.038823547200539E-2,7.2004564392168902E-2,0.36569995732392468,4.065588347116298E-2,9.1868780911222173E-4,0,1.0739573104612109E-3,1.9926451195734327E-3,4.2971645527656012E-2,4.1720795073922831E-2,5.676890138718102E-2,1.2540088594381825E-3,0.17299912016644411,0.24780802314322264,3.12,0.92641860182043878,6.4185157739450622E-3,1.2167855212197131E-2,4.8405713926298506E-3,1.4961730337876367E-2,0,3.1888911217061344E-4,5.9167420051267324E-4,5.8716324590106644E-3,1.619756552451344E-2,1.2468520809227896E-5,6.1222259400153204E-5,1.6856335336536733E-2,7.8298460129601927E-2,0.92641860182043878,92.641860182043871,260,70.411746141009829,0.70411746141009823,83.517073555656509,null,8.3819418054196532E-3,null,0.17299912016644411,5.676890138718102E-2,7.4560726575957692E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR58, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.641860182043871},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ58, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.17299912016644411},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA58, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.676890138718102E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB58, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.4560726575957692E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S58, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":83.517073555656509},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P58, IF(MODE_ILIM=4,#REF!,#REF!))","v":64.879534177276369}]
[null,null,null,null,null,null,null,53,0.26500000000000001,0.95232360099097058,0.95232360099097058,0,48.813949933395492,31.705762551520209,2,63.411525103040418,5.3072098708103659E-6,0.10476697984496557,85123.171124034518,1.1537979101579597E-5,2.0970354223170778E-7,6.4839709016804121E-4,0.4098252711509463,2.0154810344873597E-2,5.5599335189014512E-2,7.5999225530195044E-2,0.20501215038427464,2.1014990902592221E-4,2.1014990902592221E-4,0.12041001995527226,4.3495718716887189E-5,4.3495718716887189E-5,0.1779000818171779,2.1742477668953753E-2,3.417695320629986E-4,54.166666666666664,10.924681300086506,2.2394954449641229E-2,2.8771631839923664E-2,5.1508355821627896E-2,7.3546584255004918E-2,0.36919955818417238,4.1437727384069978E-2,9.3635488236437983E-4,0,1.1026774354794496E-3,2.0390323178438295E-3,4.3812534924790321E-2,4.2503734901487407E-2,5.7841227874615951E-2,1.2781244144273785E-3,0.17647847146883858,0.25273134262677643,3.18,0.92637602031699262,6.420027154386351E-3,1.2169173301800189E-2,4.8403489027024774E-3,1.50050646789658E-2,0,3.2122450766440249E-4,5.9399705783078614E-4,5.8713625778389162E-3,1.6196821026625719E-2,1.2670877611879648E-5,6.121944540673329E-5,1.6849913990168247E-2,7.8341823521001497E-2,0.92637602031699262,92.637602031699259,265,70.596901007914624,0.70596901007914625,85.123171124034513,null,8.3815565414761487E-3,null,0.17647847146883858,5.7841227874615951E-2,7.5999225530195044E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR59, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.637602031699259},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ59, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.17647847146883858},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA59, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.7841227874615951E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB59, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.5999225530195044E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S59, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":85.123171124034513},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P59, IF(MODE_ILIM=4,#REF!,#REF!))","v":63.411525103040418}]
[null,null,null,null,null,null,null,54,0.27,0.95232360099097058,0.95232360099097058,0,48.586677206122765,30.972150120966933,2,61.944300241933867,5.3072098708103659E-6,0.10674371531373848,86729.268692412516,1.1530132965222208E-5,0,6.5999999999999989E-4,0.4136734801884101,2.0535089785342908E-2,5.6648379249184581E-2,7.7437900111580249E-2,0.20693718933485722,2.1411500164905274E-4,2.1411500164905274E-4,0.12252498937288529,4.5037119062476962E-5,4.5037119062476962E-5,0.17957054176878556,2.2152713096669857E-2,3.4821801380003627E-4,54.166666666666664,10.924681300086506,2.2971467823238119E-2,2.9314492818035429E-2,5.2634178655073582E-2,7.5094565019816331E-2,0.37266629675898477,4.2219571296976934E-2,9.5402195561653772E-4,0,1.1317106522855786E-3,2.0857326079021165E-3,4.4653984980248959E-2,4.3257924040564721E-2,5.8884803673563607E-2,1.3022399694165741E-3,0.17993559364304548,0.2576326458753373,3.24,0.92634085052380888,6.4215967309287523E-3,1.2170589848120961E-2,4.8401651392348229E-3,1.5048515377149064E-2,0,3.235647556126782E-4,5.9632694999052114E-4,5.8711396720176941E-3,1.6196206115581768E-2,1.287645777082622E-5,6.1217121215274763E-5,1.6835617011696426E-2,7.8377815179318785E-2,0.92634085052380888,92.634085052380883,270,70.763841860106652,0.70763841860106647,86.729268692412518,null,8.381238336337353E-3,null,0.17993559364304548,5.8884803673563607E-2,7.7437900111580249E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR60, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.634085052380883},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ60, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.17993559364304548},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA60, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8884803673563607E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB60, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.7437900111580249E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S60, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":86.729268692412518},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P60, IF(MODE_ILIM=4,#REF!,#REF!))","v":61.944300241933867}]
[null,null,null,null,null,null,null,55,0.27500000000000002,0.95232360099097058,0.95232360099097058,0,48.359404478850045,30.23895833510284,2,60.47791667020568,5.3072098708103659E-6,0.10872045078251141,88335.366260790528,1.1320494184036351E-5,0,6.6E-4,0.41748621959106047,2.0915369225812219E-2,5.7697423309354665E-2,7.887675035227891E-2,0.20884448485520674,2.1808009427218337E-4,2.1808009427218337E-4,0.12465458768820928,4.6616298695152368E-5,4.6616298695152368E-5,0.18122560479058067,2.2562948524385961E-2,3.54666495537074E-4,54.166666666666664,10.924681300086506,2.3553683680658206E-2,2.9857353796147196E-2,5.3765703972342475E-2,7.6648508049104197E-2,0.37610108178084711,4.3001415209883924E-2,9.7168902886869582E-4,0,1.1610574427088685E-3,2.1327464715775644E-3,4.5495996424890869E-2,4.3257924040564728E-2,5.9174190333433963E-2,1.3263555244057699E-3,0.18264505033183479,0.26178649707708102,3.3000000000000003,0.92650135057451877,6.4245299642581325E-3,1.2174578680922791E-2,4.8410037579245321E-3,1.5095150710595476E-2,0,3.2597614811041321E-4,5.9878560192413717E-4,5.872156919842348E-3,1.6199012309329339E-2,1.3087898090861771E-5,6.1227727841392803E-5,1.6613626443357635E-2,7.8219136162197056E-2,0.92650135057451877,92.650135057451877,275,70.914272258910415,0.70914272258910416,88.335366260790522,null,8.3826904899126087E-3,null,0.18264505033183479,5.9174190333433963E-2,7.887675035227891E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR61, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.650135057451877},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ61, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.18264505033183479},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA61, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9174190333433963E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB61, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.887675035227891E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S61, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":88.335366260790522},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P61, IF(MODE_ILIM=4,#REF!,#REF!))","v":60.47791667020568}]
[null,null,null,null,null,null,null,56,0.28000000000000003,0.95232360099097058,0.95232360099097058,0,48.132131751577319,29.506218551391875,2,59.01243710278375,5.3072098708103659E-6,0.11069718625128436,89941.463829168541,1.1118342502178558E-5,0,6.6E-4,0.42126445243537874,2.1295648666281537E-2,5.8746467369524762E-2,8.0315776284464471E-2,0.21073451871742038,2.2204518689531401E-4,2.2204518689531401E-4,0.12679874318748974,4.8233763821780934E-5,4.8233763821780934E-5,0.18286568894215316,2.2973183952102075E-2,3.6111497727411173E-4,54.166666666666664,10.924681300086506,2.4141602021901493E-2,3.0400214774258964E-2,5.4902931773434568E-2,7.8208414705784837E-2,0.37950478085709421,4.37832591227909E-2,9.8935610212085414E-4,0,1.1907182885785902E-3,2.1800743906994443E-3,4.6338569990001063E-2,4.3257924040564728E-2,5.9463576993304318E-2,1.3504710793949659E-3,0.18536103276848517,0.26594708800366673,3.3600000000000003,0.92665444874153169,6.4274194759917297E-3,1.2178472141912557E-2,4.8418037014986912E-3,1.5141680350239861E-2,0,3.2838821408013495E-4,6.0124274783604882E-4,5.8731272545971581E-3,1.6201689088041472E-2,1.3302390424107632E-5,6.1237845314936779E-5,1.6399460761586319E-2,7.8067823971523009E-2,0.92665444874153169,92.665444874153167,280,71.049749591014816,0.71049749591014821,89.941463829168541,null,8.3840756735908059E-3,null,0.18536103276848517,5.9463576993304318E-2,8.0315776284464471E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR62, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.665444874153167},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ62, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.18536103276848517},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA62, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9463576993304318E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB62, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.0315776284464471E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S62, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":89.941463829168541},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P62, IF(MODE_ILIM=4,#REF!,#REF!))","v":59.01243710278375}]
[null,1500,null,null,null,"Eff (%)","Iout (mA)",57,0.28499999999999998,0.95232360099097058,0.95232360099097058,0,47.904859024304592,28.773965301066191,2,57.547930602132382,5.3072098708103659E-6,0.11267392172005727,91547.561397546539,1.0923283861789462E-5,0,6.6E-4,0.42500909898839073,2.1675928106750845E-2,5.9795511429694838E-2,8.1754977940318219E-2,0.2126077512784727,2.2601027951844456E-4,2.2601027951844456E-4,0.12895737489025916,4.9890013615760529E-5,4.9890013615760529E-5,0.18449119370003786,2.3383419379818183E-2,3.6756345901114941E-4,54.166666666666664,10.924681300086506,2.473522284696798E-2,3.0943075752370729E-2,5.6045862058349855E-2,7.9774286353189991E-2,0.38287822302927965,4.4565103035697877E-2,1.007023175373012E-3,0,1.2206936717240138E-3,2.2277168470970256E-3,4.7181706407291114E-2,4.3257924040564728E-2,5.9752963653174666E-2,1.3745866343841614E-3,0.18808354304803995,0.27011442128149238,3.42,0.92680052961943449,6.4302678957580397E-3,1.2182275243536376E-2,4.8425669794782107E-3,1.5188109543466787E-2,0,3.3080103551371581E-4,6.0369858296247371E-4,5.8740531138390256E-3,1.6204243175995944E-2,1.3519909661347268E-5,6.1247499051792639E-5,1.6192712970787455E-2,7.7923495950051172E-2,0.92680052961943449,92.680052961943446,285,71.171694607053283,0.71171694607053282,91.547561397546545,null,8.3853973670618333E-3,null,0.18808354304803995,5.9752963653174666E-2,8.1754977940318219E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR63, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.680052961943446},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ63, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.18808354304803995},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA63, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9752963653174666E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB63, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.1754977940318219E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S63, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":91.547561397546545},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P63, IF(MODE_ILIM=4,#REF!,#REF!))","v":57.547930602132382}]
[null,null,null,null,null,{"$f":"BR56","v":92.650310963945273},{"$f":"I56*1000","v":250},58,0.28999999999999998,0.95232360099097058,0.95232360099097058,0,47.677586297031866,28.042236697978684,2,56.084473395957367,5.3072098708103659E-6,0.11465065718883022,93153.658965924551,1.0734951381413782E-5,0,6.6E-4,0.42872103932530303,2.2056207547220163E-2,6.0844555489864921E-2,8.3194355352029334E-2,0.21446462278966905,2.2997537214157517E-4,2.2997537214157517E-4,0.13113039339657237,5.1585540217019489E-5,5.1585540217019489E-5,0.18610250109399787,2.3793654807534297E-2,3.7401194074818708E-4,54.166666666666664,10.924681300086506,2.5334546155857649E-2,3.14859367304825E-2,5.7194494827088341E-2,8.1346124355067009E-2,0.38622220113132616,4.5346946948604867E-2,1.0246902486251701E-3,0,1.2509840739744094E-3,2.2756743225995795E-3,4.8025406408899379E-2,4.3257924040564728E-2,6.0042350313045015E-2,1.3987021893733572E-3,0.19081258326638476,0.27428849953077267,3.4799999999999995,0.92693995158735021,6.4330776739713125E-3,1.2185992656669248E-2,4.8432954644072384E-3,1.523444317990926E-2,0,3.3321468878344404E-4,6.0615328920087083E-4,5.8749367689714966E-3,1.6206680839117596E-2,1.3740430503267631E-5,6.1256712735400739E-5,1.5993003819645021E-2,7.7785795523914153E-2,0.92693995158735021,92.693995158735021,290,71.281400919850697,0.71281400919850701,93.153658965924549,null,8.386658812826386E-3,null,0.19081258326638476,6.0042350313045015E-2,8.3194355352029334E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR64, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.693995158735021},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ64, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19081258326638476},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA64, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.0042350313045015E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB64, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.3194355352029334E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S64, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":93.153658965924549},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P64, IF(MODE_ILIM=4,#REF!,#REF!))","v":56.084473395957367}]
[null,null,null,null,null,{"$f":"BR81","v":92.854681246033451},{"$f":"I81*1000","v":375},59,0.29499999999999998,0.95232360099097058,0.95232360099097058,0,47.450313569759139,27.311074911801011,2,54.622149823602022,5.3072098708103659E-6,0.11662739265760315,94759.756534302564,1.0553003052915241E-5,0,6.6E-4,0.43240111574487444,2.2436486987689477E-2,6.1893599550035004E-2,8.4633908551794826E-2,0.21630555460491799,2.3394046476470581E-4,2.3394046476470581E-4,0.1333177016653784,5.3320828732016521E-5,5.3320828732016521E-5,0.18769997675550748,2.4203890235250401E-2,3.8046042248522476E-4,54.166666666666664,10.924681300086506,2.5939571948570529E-2,3.2028797708594264E-2,5.834883007965002E-2,8.2923930075578953E-2,0.38953747396546362,4.6128790861511851E-2,1.0423573218773282E-3,0,1.2815899771590484E-3,2.3239472990363766E-3,4.8869670727391339E-2,4.3257924040564728E-2,6.033173697291537E-2,1.422817744362553E-3,0.19354815552024821,0.27846932536553975,3.54,0.92707304900534138,6.4358510968466074E-3,1.2189628739232877E-2,4.8439909033294436E-3,1.5280685821422521E-2,0,3.3562924511286012E-4,6.0860703622750889E-4,5.8757803391655235E-3,1.620900792338039E-2,1.396392747685937E-5,6.1265508461904651E-5,1.5799979476629644E-2,7.7654390017286135E-2,0.92707304900534138,92.70730490053414,295,71.3800443047935,0.713800443047935,94.759756534302568,null,8.3878630360682983E-3,null,0.19354815552024821,6.033173697291537E-2,8.4633908551794826E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR65, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.70730490053414},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ65, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19354815552024821},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA65, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.033173697291537E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB65, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.4633908551794826E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S65, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":94.759756534302568},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P65, IF(MODE_ILIM=4,#REF!,#REF!))","v":54.622149823602022}]
[null,null,null,null,null,{"$f":"BR106","v":92.96157774674576},{"$f":"I106*1000","v":500},60,0.3,0.95232360099097058,0.95232360099097058,0,47.223040842486405,26.580526717591454,2,53.161053435182907,5.3072098708103659E-6,0.11860412812637609,96365.854102680576,1.0377119668699987E-5,0,6.6E-4,0.43605013500130524,2.2816766428158781E-2,6.2942643610205101E-2,8.6073637571819586E-2,0.21813095029721774,2.3790555738783641E-4,2.3790555738783641E-4,0.13551919572978174,5.5096357233740685E-5,5.5096357233740685E-5,0.18928397088658783,2.4614125662966509E-2,3.8690890422226254E-4,54.166666666666664,10.924681300086506,2.6550300225106602E-2,3.2571658686706036E-2,5.9508867816034899E-2,8.4507704879304826E-2,0.39282476831287244,4.691063477441882E-2,1.0600243951294865E-3,0,1.3125118631072009E-3,2.3725362582366874E-3,4.9714500095759888E-2,4.3257924040564728E-2,6.0621123632785712E-2,1.4469332993517492E-3,0.19629026190720217,0.28265690139364336,3.5999999999999996,0.92720013419362746,6.4385902999301407E-3,1.2193187561983714E-2,4.8446549281295024E-3,1.5326841729093999E-2,0,3.3804477100103463E-4,6.1105998250452875E-4,5.8765858039037441E-3,1.621122988941218E-2,1.4190374950195668E-5,6.1273906870947689E-5,1.561330943535761E-2,7.7528968683137592E-2,0.92720013419362746,92.720013419362743,300,71.468691685531624,0.71468691685531627,96.365854102680572,null,8.3890128625619086E-3,null,0.19629026190720217,6.0621123632785712E-2,8.6073637571819586E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR66, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.720013419362743},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ66, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19629026190720217},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA66, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.0621123632785712E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB66, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.6073637571819586E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S66, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":96.365854102680572},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P66, IF(MODE_ILIM=4,#REF!,#REF!))","v":53.161053435182907}]
[null,null,null,null,null,null,null,61,0.30499999999999999,0.95232360099097058,0.95232360099097058,0,46.995768115213679,25.850644136369652,2,51.701288272739305,5.3072098708103659E-6,0.12058086359514901,97971.951671058574,1.0207002952819661E-5,0,6.6E-4,0.43966887036939606,2.3197045868628096E-2,6.3991687670375177E-2,8.7513542444316389E-2,0.21994119669173715,2.4187065001096705E-4,2.4187065001096705E-4,0.13773476535442011,5.6912596761711505E-5,5.6912596761711505E-5,0.19085481915626651,2.5024361090682609E-2,3.9335738595930016E-4,54.166666666666664,10.924681300086506,2.7166730985465869E-2,3.3114519664817793E-2,6.0674608036242958E-2,8.6097450131239678E-2,0.39608478079412446,4.7692478687325811E-2,1.0776914683816444E-3,0,1.3437502136481375E-3,2.4214416820297819E-3,5.0559895247425699E-2,4.3257924040564728E-2,6.0910510292656067E-2,1.4710488543409445E-3,0.19903890452566236,0.28685123021675141,3.66,0.92732149921926543,6.44129728031339E-3,1.2196672931792331E-2,4.8452890648685671E-3,1.5372914887625712E-2,0,3.4046132860557349E-4,6.1351227618903744E-4,5.8773550143044456E-3,1.621335184373314E-2,1.4419747145773722E-5,6.1281927263745413E-5,1.5432684623714841E-2,7.7409240925556566E-2,0.92732149921926543,92.732149921926549,305,71.54830972155635,0.71548309721556347,97.971951671058576,null,8.3901109348373439E-3,null,0.19903890452566236,6.0910510292656067E-2,8.7513542444316389E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR67, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.732149921926549},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ67, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19903890452566236},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA67, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.0910510292656067E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB67, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.7513542444316389E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S67, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":97.971951671058576},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P67, IF(MODE_ILIM=4,#REF!,#REF!))","v":51.701288272739305}]
[null,null,null,null,null,null,null,62,0.31,0.95232360099097058,0.95232360099097058,0,46.768495387940952,25.121485184596359,2,50.242970369192719,5.3072098708103659E-6,0.12255759906392195,99578.049239436587,1.0042373872935472E-5,0,6.5999999999999989E-4,0.44325806355795161,2.3577325309097407E-2,6.5040731730545254E-2,8.8953623201505821E-2,0.2217366648229821,2.4583574263409752E-4,2.4583574263409752E-4,0.13996429463971505,5.8770011321978899E-5,5.8770011321978899E-5,0.19241284353116292,2.543459651839873E-2,3.9980586769633789E-4,54.166666666666664,10.924681300086506,2.7788864229648332E-2,3.3657380642929564E-2,6.184605074027423E-2,8.7693167196794833E-2,0.39931817959291227,4.8474322600232787E-2,1.0953585416338025E-3,0,1.3753055106111285E-3,2.4706640522449311E-3,5.1405856916237468E-2,4.3257924040564721E-2,6.1199896952526409E-2,1.4951644093301403E-3,0.20179408547488883,0.29105231443035073,3.7199999999999998,0.92743741751179676,6.4439739076779931E-3,1.2200088412694342E-2,4.8458947422260904E-3,1.5418909027382657E-2,0,3.4287897608895919E-4,6.1596405595518015E-4,5.8780897033615127E-3,1.6215378567003891E-2,1.4652018152579347E-5,6.1289587709855407E-5,1.5257815693989027E-2,7.7294934692242079E-2,0.92743741751179676,92.74374175117967,310,71.619772941093288,0.71619772941093285,99.578049239436581,null,8.391159726798424E-3,null,0.20179408547488883,6.1199896952526409E-2,8.8953623201505821E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR68, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.74374175117967},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ68, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20179408547488883},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA68, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1199896952526409E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB68, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.8953623201505821E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S68, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":99.578049239436581},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P68, IF(MODE_ILIM=4,#REF!,#REF!))","v":50.242970369192719}]
[null,null,null,null,null,null,null,63,0.315,0.95232360099097058,0.95232360099097058,0,46.541222660668218,24.393114754549256,2,48.786229509098511,5.3072098708103659E-6,0.12453433453269488,101184.1468078146,9.8829711130476081E-6,0,6.6E-4,0.44681842648484116,2.3957604749566729E-2,6.6089775790715358E-2,9.0393879875616451E-2,0.22351771082275704,2.4980083525722818E-4,2.4980083525722818E-4,0.14220766257732981,6.0669057887123071E-5,6.0669057887123071E-5,0.19395835304601955,2.5844831946114838E-2,4.0625434943337562E-4,54.166666666666664,10.924681300086506,2.8416699957653994E-2,3.4200241621041336E-2,6.3023195928128703E-2,8.9294857441797909E-2,0.40252560605514903,4.9256166513139771E-2,1.1130256148859606E-3,0,1.4071782358254445E-3,2.5202038507114053E-3,5.2252385836472265E-2,4.3257924040564728E-2,6.1489283612396764E-2,1.5192799643193363E-3,0.20455580685498626,0.29526015662374705,3.7800000000000002,0.92754814532666241,6.4466219342999278E-3,1.2203437344957813E-2,4.8464732991462057E-3,1.546482764436366E-2,0,3.4529776793225815E-4,6.1841545173875045E-4,5.8787914952195385E-3,1.62173145396119E-2,1.4887161937015058E-5,6.1296905143887065E-5,1.5088431474112103E-2,7.7185795018463066E-2,0.92754814532666241,92.754814532666245,315,71.68387138413388,0.71683871384133879,101.1841468078146,null,8.3921615569631253E-3,null,0.20455580685498626,6.1489283612396764E-2,9.0393879875616451E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR69, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.754814532666245},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ69, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20455580685498626},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA69, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1489283612396764E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB69, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0393879875616451E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S69, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":101.1841468078146},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P69, IF(MODE_ILIM=4,#REF!,#REF!))","v":48.786229509098511}]
[null,null,null,null,null,null,null,64,{"$f":"IF(PLOT_TYPE=1, H70/100*Iout, min_I*EXP(H70*rr/100))","v":0.32},{"$f":"IF(I70<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I70-Vout)/L*OnTime)","v":0.95232360099097058},{"$f":"IF(I70<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I70+((Vin-(Rdcr+RdsonTop)*J70-Vout)/L*OnTime)/2)","v":0.95232360099097058},{"$f":"IF(I70<Icrit, 0, I70-((Vin-(Rdcr+RdsonTop)*K70-Vout)/L*OnTime)/2)","v":0},46.313949933395499,{"$f":"IF(I70<Icrit, 1000*SQRT((J70*CoutEsr)^2+(((J70/2)-I70)*(OnTime+OffTime)/Cout)^2), 1000*J70*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":23.66560565274774},2,{"$f":"IF(I70<Icrit, 1000*((N70/1000)*O70), 1000*J70*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":47.331211305495479},{"$f":"IF(I70<Icrit, L*J70/(Vout+J70/2*(RdsonBot+Rdcr)), L*J70/(Vout+I70*(RdsonBot+Rdcr)))","v":5.3072098708103659E-6},0.12651107000146783,{"$f":"IF(I70<Icrit,I70/((OnTime+Q70)*J70/2),1/(OnTime+Q70))","v":102790.24437619261},9.728549689406239E-6,0,{"$f":"S70*(T70*Iq_active+U70*Iq_sleep)","v":6.6E-4},0.450350642925747,{"$f":"W70^2*Rdcr","v":2.433788419003604E-2},{"$f":"Core_Loss/1000*S70/$S$106","v":6.7138819850885434E-2},{"$f":"(Y70+X70*(1+Ltc*(Ta-25)))/(1-X70*Ltc*ThetaCa)","v":9.1834312498884588E-2},0.22528467674493924,2.5376592788035884E-4,2.5376592788035884E-4,0.14446474356079034,6.2610186396254739E-5,6.2610186396254739E-5,0.19549164451940376,2.6255067373830938E-2,4.1270283117041335E-4,{"$f":"20*VIN_nom/24","v":54.166666666666664},{"$f":"IF(I70<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I70+Iripple/2)*1000000000)","v":10.924681300086506},{"$f":"IF(I70<Icrit, Vin*(I70+Iripple/2)*AK70/1000000000/2*S70, Vin*(I70-Iripple/2)*AJ70/1000000000/2*S70 + Vin*(I70+Iripple/2)*AK70/1000000000/2*S70)","v":2.905023816948285E-2},{"$f":"IF(I70<Icrit, Csw*(Vin)^2*S70/2, Csw*Vin^2*S70/2)","v":3.47431025991531E-2},6.4206043599806362E-2,{"$f":"(AI70+AL70+AM70+AH70*(1+RdsonTopTc*(Ta-25)))/(1-AH70*RdsonTopTc*ThetaJA)","v":9.0902522232493094E-2},{"$f":"IF(I70<Icrit,Iripple*SQRT((OffTime)*S70/3), SQRT(OffTime*S70*(I70^2+Iripple^2/12)))","v":0.40570767617427789},5.0038010426046747E-2,{"$f":"QgBot*S70*Vdd","v":1.130692688138119E-3},{"$f":"IF(I70<Icrit, Vin*Idss*R70, QrrBot*(I70-Iripple/2)/1*S70*Vin+Vin*Idss*R70)","v":0},{"$f":"IF(I70<Icrit, dead1*S70*(I70+Iripple/2)*((I70+Iripple/2)*BDserR+VSD), dead1*S70*(I70+Iripple/2)*((I70+Iripple/2)*BDserR+VSD)+dead2*S70*(I70-Iripple/2)*((I70-Iripple/2)*BDserR+VSD))","v":1.4393688711203563E-3},2.5700615592584753E-3,{"$f":"(AR70+AS70+AT70+AQ70*(1+RdsonBotTc*(Ta-25)))/(1-AQ70*RdsonBotTc*ThetaJA)","v":5.3099482742835859E-2},{"$f":"Vin*V70+Vout*Ifb/0.8","v":4.3257924040564728E-2},{"$f":"(Vin-Vdd)*(S70*QgBot+S70*QgTop)+AW70","v":6.1778670272267119E-2},{"$f":"AI70+AR70","v":1.5433955193085323E-3},0.20732407076690462,{"$f":"SUM(Z70,AC70,AF70,AZ70)","v":0.29947475938006585},{"$f":"Vout*I70","v":3.84},0.92765392307285977,6.4492430041256828E-3,1.2206722862381881E-2,{"$f":"Vin*S70*(QgBot+QgTop)/($BB70+$BA70)","v":4.8470259917748016E-3},1.551067401831965E-2,0,3.4771775521972708E-4,6.2086658541272803E-4,{"$f":"X70/($BB70+$BA70)","v":5.879461913588506E-3},{"$f":"Y70/($BB70+$BA70)","v":1.6219163964884341E-2},1.5125152352814768E-5,6.1303895453239396E-5,1.4924277562576367E-2,7.7081582706089738E-2,{"$f":"BC70","v":0.92765392307285977},92.765392307285978,{"$f":"I70*1000","v":320},71.741317737155555,0.71741317737155552,{"$f":"S70/1000","v":102.79024437619262},null,{"$f":"AM70/($BB70+$BA70)","v":8.3931186004758459E-3},null,0.20732407076690462,6.1778670272267119E-2,9.1834312498884588E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR70, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.765392307285978},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ70, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20732407076690462},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA70, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1778670272267119E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB70, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1834312498884588E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S70, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":102.79024437619262},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P70, IF(MODE_ILIM=4,#REF!,#REF!))","v":47.331211305495479}]
[null,null,null,null,null,null,null,65,0.32500000000000001,0.95232360099097058,0.95232360099097058,0,{"$f":"IF(I71<Icrit, 1000*((((J71/2)-I71)*0.000002/Cout+Vout/306)), 1000*J71*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":46.086677206122772},22.939039830127278,{"$f":"ROUNDUP(M71/N71,0)","v":3},68.817119490381828,5.3072098708103659E-6,0.12848780547024077,104396.34194457062,{"$f":"IF(1/S71-OnTime-Q71>Tsleep, OnTime+Q71+Tsleep, 1/S71)","v":9.5788796941846033E-6},{"$f":"IF(1/S71-OnTime-Q71>Tsleep, 1/S71-OnTime-Q71-Tsleep, 0)","v":0},6.6E-4,{"$f":"IF(I71<Icrit,Iripple*SQRT((OnTime+OffTime)*S71/3), SQRT(I71^2+Iripple^2/12))","v":0.45385537004741711},2.4718163630505351E-2,6.8187863911055524E-2,9.3274921103554509E-2,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q71)*S71)","v":0.22703789133247754},{"$f":"RCoutEsr*AA71^2","v":2.577310205034894E-4},2.577310205034894E-4,{"$f":"SQRT($R71)*SQRT($I71^2*(1-R71)+(Iripple^2)/12)","v":0.14673540785488118},{"$f":"RCinEsr*AD71^2","v":6.4593839755014979E-5},6.4593839755014979E-5,{"$f":"IF(I71<Icrit,Iripple*SQRT((OnTime)*S71/3), SQRT(OnTime*S71*(I71^2+Iripple^2/12)))","v":0.19701300321927362},{"$f":"RdsonTop*AG71^2","v":2.6665302801547056E-2},{"$f":"QgTop*S71*Vdd","v":4.1915131290745107E-4},54.166666666666664,10.924681300086506,2.9689478865134906E-2,3.5285963577264871E-2,{"$f":"AI71+AL71+AM71","v":6.5394593755307234E-2},9.2516162935541338E-2,0.40886498197253385,{"$f":"RdsonBot*AP71^2","v":5.0819854338953724E-2},1.1483597613902771E-3,0,1.4718778983251345E-3,{"$f":"AR71+AS71+AT71","v":2.6202376597154117E-3},5.3947148370462966E-2,4.3257924040564728E-2,6.2068056932137468E-2,1.5675110742977281E-3,0.21009887931243951,0.3036961252762525,3.9000000000000004,0.92775497651931371,{"$f":"(AO71-AN71)/($BB71+$BA71)","v":6.451838661019239E-3},{"$f":"(AV71-AU71)/($BB71+$BA71)","v":1.2209947908015001E-2},4.8475539997628429E-3,{"$f":"AN71/($BB71+$BA71)","v":1.5556451229216697E-2},{"$f":"AS71/(BA71+BB71)","v":0},{"$f":"AT71/($BB71+$BA71)","v":3.5013898589741839E-4},{"$f":"AU71/($BB71+$BA71)","v":6.2331757140110077E-4},5.8801023893897547E-3,1.6220930790180377E-2,{"$f":"(AF71)/($BB71+$BA71)","v":1.536596315005288E-5},{"$f":"(AC71)/($BB71+$BA71)","v":6.1310573557823991E-5},{"$f":"AX71/($BB71+$BA71)","v":1.4765115051711441E-2},{"$f":"SUM(BD71:BO71)","v":7.6982073123301756E-2},0.92775497651931371,92.775497651931374,325,71.792753953912452,{"$f":"BT71/100","v":0.71792753953912447},104.39634194457062,null,8.3940329000222382E-3,null,{"$f":"AZ71","v":0.21009887931243951},{"$f":"AX71","v":6.2068056932137468E-2},{"$f":"Z71","v":9.3274921103554509E-2},null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR71, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.775497651931374},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ71, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21009887931243951},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA71, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.2068056932137468E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB71, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.3274921103554509E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S71, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":104.39634194457062},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P71, IF(MODE_ILIM=4,#REF!,#REF!))","v":68.817119490381828}]
[null,null,null,null,null,null,null,66,0.33,0.95232360099097058,0.95232360099097058,0,45.859404478850045,22.213509846015054,3,66.640529538045158,5.3072098708103659E-6,{"$f":"OnTime*S72","v":0.13046454093901372},106002.43951294864,9.4337451533636251E-6,0,6.6E-4,0.45733323983515811,2.5098443070974669E-2,6.9236907971225614E-2,9.4715705721878332E-2,0.22877767073148553,2.6169611312662006E-4,{"$f":"AB72","v":2.6169611312662006E-4},0.14901952202712151,6.6620453835575263E-5,{"$f":"AE72","v":6.6620453835575263E-5},0.19852270348263468,2.7075538229263164E-2,4.255997946444888E-4,54.166666666666664,10.924681300086506,3.0334422044610152E-2,3.5828824555376636E-2,6.6588846394631279E-2,9.4135780918020356E-2,0.41199809278693039,5.16016982518607E-2,1.1660268346424352E-3,0,1.5047057992690484E-3,2.6707326339114835E-3,5.4795383454917648E-2,4.3257924040564728E-2,6.2357443592007816E-2,1.5916266292869239E-3,{"$f":"AO72+AV72+AX72+AY72","v":0.21288023459423275},0.30792425688307329,3.96,0.92785151789269227,6.4544103562669602E-3,1.2213115248458875E-2,4.8480584320025064E-3,1.5602162172217668E-2,0,3.52561505008516E-4,6.2576851723745411E-4,5.8807142677139322E-3,1.6222618726085439E-2,1.5609567983343066E-5,6.1316953482614173E-5,1.4610719365846564E-2,7.6887055112303856E-2,0.92785151789269227,{"$f":"100*BQ72","v":92.785151789269221},330,71.838757366287027,0.71838757366287032,106.00243951294864,null,8.3949063757619135E-3,null,0.21288023459423275,6.2357443592007816E-2,9.4715705721878332E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR72, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.785151789269221},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ72, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21288023459423275},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA72, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.2357443592007816E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB72, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.4715705721878332E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S72, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":106.00243951294864},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P72, IF(MODE_ILIM=4,#REF!,#REF!))","v":66.640529538045158}]
[null,null,null,null,null,null,null,67,0.33500000000000002,0.95232360099097058,0.95232360099097058,0,45.632131751577312,21.489120618673361,3,64.467361856020077,5.3072098708103659E-6,0.13244127640778663,107608.53708132665,9.2929429868955106E-6,0,6.6E-4,0.46078486042335037,2.5478722511443976E-2,7.028595203139569E-2,9.6156666386116044E-2,0.23050431915682215,2.6566120574975061E-4,2.6566120574975061E-4,0.15131694934434525,6.8690457476637445E-5,6.8690457476637445E-5,0.20002100929310065,2.7485773656979268E-2,4.3204827638152648E-4,54.166666666666664,10.924681300086506,3.0985067707908601E-2,3.6371685533488407E-2,6.7788801517778538E-2,9.5761377547424961E-2,0.415107556467882,5.2383542164767698E-2,1.1836939078945933E-3,0,1.53785305578137E-3,2.7215469636759633E-3,5.5644188732193602E-2,4.3257924040564728E-2,6.2646830251878172E-2,1.6157421842761198E-3,0.21566813871577287,0.3121591567651153,4.0200000000000005,{"$f":"BB73/(BB73+BA73)","v":0.92794374687789438},6.4569594554171328E-3,1.221622748690418E-2,4.8485403318547574E-3,1.5647809571335648E-2,0,3.5498535490780691E-4,6.2821952407403727E-4,5.8812988141620582E-3,1.6224231263903797E-2,1.5855940419310353E-5,6.1323048423761876E-5,1.4460879202475433E-2,7.6796329993877921E-2,0.92794374687789438,92.794374687789443,335,71.879846296152991,0.71879846296152994,107.60853708132665,null,8.3957408343805304E-3,null,0.21566813871577287,6.2646830251878172E-2,9.6156666386116044E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR73, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.794374687789443},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ73, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21566813871577287},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA73, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.2646830251878172E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB73, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.6156666386116044E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S73, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":107.60853708132665},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P73, IF(MODE_ILIM=4,#REF!,#REF!))","v":64.467361856020077}]
[null,null,null,null,null,null,null,68,0.34,0.95232360099097058,0.95232360099097058,0,45.404859024304585,20.765991529007717,3,62.297974587023148,5.3072098708103659E-6,0.13441801187655958,109214.63464970466,9.1562820606176349E-6,0,6.6E-4,0.46421081733691943,2.5859001951913294E-2,7.1334996091565794E-2,9.759780312853561E-2,0.23221812951312878,2.6962629837288128E-4,2.6962629837288128E-4,0.15362755013715673,7.0804272483433815E-5,7.0804272483433815E-5,0.20150817481980043,2.7896009084695386E-2,4.3849675811856421E-4,54.166666666666664,10.924681300086506,3.1641415855030247E-2,3.6914546511600171E-2,6.8994459124748983E-2,9.7392954191667103E-2,0.41819390049760835,5.3165386077674681E-2,1.2013609811467514E-3,0,1.5713201496913691E-3,2.7726811308381207E-3,5.649356493871438E-2,4.3257924040564728E-2,6.2936216911748513E-2,1.6398577392653156E-3,0.21846259378139529,0.31640082748078724,4.08,0.92803185153113288,6.4594872445220015E-3,1.2219287075027516E-2,4.849000681920252E-3,1.5693395991894572E-2,0,3.5741057545741621E-4,6.3067068714635691E-4,5.8818572206326648E-3,1.6225771691623023E-2,1.6105053943410766E-5,6.1328870808938894E-5,1.4315395565925237E-2,7.6709710658901378E-2,0.92803185153113288,92.80318515311329,340,71.916485184007442,0.71916485184007439,109.21463464970466,null,8.3965379773510845E-3,null,0.21846259378139529,6.2936216911748513E-2,9.759780312853561E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR74, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.80318515311329},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ74, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21846259378139529},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA74, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.2936216911748513E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB74, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.759780312853561E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S74, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":109.21463464970466},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P74, IF(MODE_ILIM=4,#REF!,#REF!))","v":62.297974587023148}]
[null,null,null,null,null,null,null,69,0.34499999999999997,0.95232360099097058,0.95232360099097058,0,45.177586297031866,20.04425896200183,3,60.132776886005487,5.3072098708103659E-6,0.1363947473453325,110820.73221808264,9.023582320608686E-6,0,6.6E-4,0.46761167465093839,2.6239281392382605E-2,7.2384040151735857E-2,9.9039115981412712E-2,0.23391938397491208,2.7359139099601178E-4,2.7359139099601178E-4,0.15595118213480239,7.2962313627726922E-5,7.2962313627726922E-5,0.2029844449207471,2.8306244512411483E-2,4.4494523985560183E-4,54.166666666666664,10.924681300086506,3.2303466485975083E-2,3.7457407489711929E-2,7.0205819215542614E-2,9.9030512219076008E-2,0.42125763303478686,5.394722999058163E-2,1.2190280543989092E-3,0,1.6051075628283158E-3,2.8241356172272252E-3,5.7343512811333819E-2,4.3257924040564728E-2,6.3225603571618855E-2,1.663973294254511E-3,0.22126360189628319,0.32064927158231965,4.1399999999999997,0.92811600911439152,6.4619949358422557E-3,1.2222296323863862E-2,4.8494404083993994E-3,1.5738923851916879E-2,0,3.5983720420568692E-4,6.3312209619776358E-4,5.882390610610546E-3,1.6227243108503615E-2,1.6356881966163887E-5,6.1334432352481527E-5,1.4174080884236597E-2,7.6627020738095242E-2,0.92811600911439152,92.811600911439157,345,71.94908925319227,0.71949089253192267,110.82073221808264,null,8.3972994084838062E-3,null,0.22126360189628319,6.3225603571618855E-2,9.9039115981412712E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR75, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.811600911439157},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ75, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.22126360189628319},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA75, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.3225603571618855E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB75, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9039115981412712E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S75, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":110.82073221808264},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P75, IF(MODE_ILIM=4,#REF!,#REF!))","v":60.132776886005487}]
[null,null,null,null,null,null,null,70,0.35,0.95232360099097058,0.95232360099097058,0,44.950313569759132,19.324079393927242,3,57.972238181781726,5.3072098708103659E-6,0.13837148281410541,112426.82978646066,8.8946740017428485E-6,0,6.6E-4,0.47098797607486681,2.6619560832851916E-2,7.3433084211905933E-2,0.1004806049770311,0.23560835452892681,2.7755648361914233E-4,2.7755648361914233E-4,0.15828770077279114,7.5164988647809995E-5,7.5164988647809995E-5,0.204450055613493,2.8716479940127587E-2,4.513937215926395E-4,54.166666666666664,10.924681300086506,3.2971219600743111E-2,3.80002684678237E-2,7.1422881790159459E-2,0.10067405299839854,0.42429924389131174,5.4729073903488613E-2,1.2366951276510673E-3,0,1.6392157770214817E-3,2.8759109046725493E-3,5.8194033087336373E-2,4.3257924040564728E-2,6.351499023148921E-2,1.688088849243707E-3,0.22407116516646783,0.32490449161576584,4.1999999999999993,0.92819638685904104,6.4644836730673172E-3,1.2225257413756081E-2,4.8498603850822839E-3,1.5784395432544385E-2,0,3.6226527655087504E-4,6.3557383586799446E-4,5.8829000440065709E-3,1.622864843843019E-2,1.6611397828856687E-5,6.1339744105854424E-5,1.4036758201013234E-2,7.6548093842253653E-2,0.92819638685904104,92.81963868590411,350,71.978028730187987,0.71978028730187982,112.42682978646066,null,8.3980266408351222E-3,null,0.22407116516646783,6.351499023148921E-2,0.1004806049770311,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR76, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.81963868590411},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ76, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.22407116516646783},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA76, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.351499023148921E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB76, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1004806049770311},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S76, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":112.42682978646066},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P76, IF(MODE_ILIM=4,#REF!,#REF!))","v":57.972238181781726}]
[null,null,null,null,null,null,null,71,0.35499999999999998,0.95232360099097058,0.95232360099097058,0,44.723040842486405,18.605633164282768,3,55.816899492848307,5.3072098708103659E-6,0.14034821828287836,114032.92735483867,8.7693969031267506E-6,0,6.6E-4,0.47434024596732621,2.6999840273321224E-2,7.4482128272076037E-2,0.10192227014768235,0.23728530348180984,2.8152157624227299E-4,2.8152157624227299E-4,0.16063695947540255,7.7412698248506361E-5,7.7412698248506361E-5,0.20590523451563095,2.9126715367843704E-2,4.5784220332967729E-4,54.166666666666664,10.924681300086506,3.3644675199334353E-2,3.8543129445935471E-2,7.2645646848599504E-2,0.10232357789879913,0.42731920544647484,5.551091781639559E-2,1.2543622009032254E-3,0,1.6736452741001368E-3,2.928007475003362E-3,5.9045126504437315E-2,4.3257924040564728E-2,6.3804376891359565E-2,1.7122044042329027E-3,0.2268852856988289,0.32916649012100202,4.26,0.92827314266553806,6.4669545360985826E-3,1.2228172403471533E-2,4.8502614370046189E-3,1.5829812887586926E-2,0,3.6469482589114084E-4,6.3802598604919202E-4,5.8833865215923604E-3,1.6229990442145011E-2,1.6868574808769954E-5,6.1344816503889824E-5,1.3903260434919903E-2,7.6472772866071931E-2,0.92827314266553806,92.827314266553813,355,72.003632642003467,0.72003632642003468,114.03292735483868,null,8.3987211030383015E-3,null,0.2268852856988289,6.3804376891359565E-2,0.10192227014768235,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR77, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.827314266553813},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ77, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.2268852856988289},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA77, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.3804376891359565E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB77, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10192227014768235},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S77, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":114.03292735483868},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P77, IF(MODE_ILIM=4,#REF!,#REF!))","v":55.816899492848307}]
[null,null,null,null,null,null,null,72,0.36,0.95232360099097058,0.95232360099097058,0,44.495768115213679,17.889129112367566,3,53.667387337102703,5.3072098708103659E-6,0.1423249537516513,115639.02492321668,8.6475997239166565E-6,0,6.6E-4,0.47766899028677579,2.7380119713790549E-2,7.5531172332246113E-2,0.10336411152566584,0.23895048393564874,2.8548666886540365E-4,2.8548666886540365E-4,0.16299880991505214,7.9705836101169903E-5,7.9705836101169903E-5,0.20735020125747058,2.9536950795559815E-2,4.6429068506671496E-4,54.166666666666664,10.924681300086506,3.4323833281748775E-2,3.9085990424047236E-2,7.3874114390862722E-2,0.10397908828985999,0.43031797350340162,5.6292761729302573E-2,1.2720292741553835E-3,0,1.7083965358935516E-3,2.9804258100489351E-3,5.9896793800783096E-2,4.3257924040564728E-2,6.4093763551229921E-2,1.7363199592220985E-3,0.2297059656010951,0.33343526963172754,4.32,0.92834642574535797,6.4694085454378263E-3,1.2231043238566101E-2,4.8506443438018727E-3,1.5875178252282664E-2,0,3.6712588376215964E-4,6.4047862221253279E-4,5.8838509890688584E-3,1.6231271728471608E-2,1.7128386123973702E-5,6.1349659407209728E-5,1.3773429700313054E-2,7.6400909349447849E-2,0.92834642574535797,92.834642574535792,360,72.026192211331946,0.72026192211331941,115.63902492321668,null,8.3993841451114673E-3,null,0.2297059656010951,6.4093763551229921E-2,0.10336411152566584,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR78, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.834642574535792},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ78, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.2297059656010951},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA78, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.4093763551229921E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB78, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10336411152566584},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S78, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":115.63902492321668},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P78, IF(MODE_ILIM=4,#REF!,#REF!))","v":53.667387337102703}]
[null,null,null,null,null,null,null,73,0.36499999999999999,0.95232360099097058,0.95232360099097058,0,44.268495387940952,17.174810313016483,3,51.524430939049445,5.3072098708103659E-6,0.14430168922042425,117245.1224915947,8.5291394537260183E-6,0,6.6E-4,0.48097469748296756,2.7760399154259856E-2,7.6580216392416203E-2,0.10480612914328896,0.24060414023392623,2.8945176148853421E-4,2.8945176148853421E-4,0.16537310225032045,8.2044788843684834E-5,8.2044788843684834E-5,0.20878516786900866,2.9947186223275919E-2,4.7073916680375274E-4,54.166666666666664,10.924681300086506,3.5008693847986404E-2,3.9628851402159007E-2,7.5108284416949167E-2,0.10564058554158136,0.43329598809213776,5.7074605642209564E-2,1.2896963474075417E-3,0,1.7434700442309963E-3,3.0331663916385379E-3,6.0749035714951716E-2,4.3257924040564728E-2,6.4383150211100262E-2,1.7604355142112945E-3,0.2325332069818446,0.33771083267546576,4.38,0.92841637721065107,6.4718466662181976E-3,1.2233871759067072E-2,4.8510098427902411E-3,1.5920493451345011E-2,0,3.6955847996352398E-4,6.4293181570825443E-4,5.884294340803552E-3,1.6232494764624374E-2,1.7390804937732128E-5,6.1354282141193244E-5,1.3647116683196089E-2,7.6332362890795244E-2,0.92841637721065107,92.841637721065112,365,72.045963869077937,0.72045963869077934,117.2451224915947,null,8.400017043792625E-3,null,0.2325332069818446,6.4383150211100262E-2,0.10480612914328896,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR79, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.841637721065112},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ79, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.2325332069818446},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA79, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.4383150211100262E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB79, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10480612914328896},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S79, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":117.2451224915947},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P79, IF(MODE_ILIM=4,#REF!,#REF!))","v":51.524430939049445}]
[null,null,null,null,null,null,null,74,0.37,0.95232360099097058,0.95232360099097058,0,44.041222660668225,16.462961219394295,3,49.388883658182891,5.3072098708103659E-6,0.14627842468919719,118851.22005997271,8.4138808124594505E-6,0,6.6E-4,0.4842578393336307,2.8140678594729174E-2,7.7629260452586279E-2,0.10624832303286695,0.24224650838006515,2.9341685411166487E-4,2.9341685411166487E-4,0.16775968534431016,8.4429936080465854E-5,8.4429936080465854E-5,0.21021033914312279,3.0357421650992023E-2,4.7718764854079042E-4,54.166666666666664,10.924681300086506,3.5699256898047226E-2,4.0171712380270772E-2,7.6348156926858785E-2,0.1073080710243816,0.43625367422339228,5.7856449555116547E-2,1.3073634206596998E-3,0,1.7788662809417421E-3,3.0862297016014421E-3,6.1601852985952943E-2,4.3257924040564728E-2,6.4672536870970618E-2,1.7845510692004901E-3,0.23536701195050569,0.34199318177356475,4.4399999999999995,0.92848313061652565,6.4742698119114178E-3,1.2236659706538729E-2,4.8513586318000932E-3,1.5965760306362979E-2,0,3.7199264267499213E-4,6.453856340415796E-4,5.8847174232674777E-3,1.6233661885689858E-2,1.7655804362554979E-5,6.1358693531813295E-5,1.35241800673134E-2,7.6267000607494903E-2,0.92848313061652565,92.848313061652561,370,72.063171902227168,0.72063171902227163,118.8512200599727,null,8.4006210074460477E-3,null,0.23536701195050569,6.4672536870970618E-2,0.10624832303286695,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR80, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.848313061652561},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ80, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.23536701195050569},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA80, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.4672536870970618E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB80, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10624832303286695},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S80, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":118.8512200599727},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P80, IF(MODE_ILIM=4,#REF!,#REF!))","v":49.388883658182891}]
[null,null,null,null,null,null,null,75,0.375,0.95232360099097058,0.95232360099097058,0,43.813949933395499,15.753916619955382,3,47.261749859866143,5.3072098708103659E-6,0.14825516015797011,120457.31762835072,8.3016957349599903E-6,0,6.6E-4,0.48751887173043945,2.8520958035198482E-2,7.867830451275637E-2,0.10769069322672298,0.24387781643060341,2.9738194673479548E-4,2.9738194673479548E-4,0.17015840696486112,8.6861650382457885E-5,8.6861650382457885E-5,0.21162591297675076,3.0767657078708141E-2,4.836361302778282E-4,54.166666666666664,10.924681300086506,3.6395522431931247E-2,4.0714573358382543E-2,7.7593731920591616E-2,0.10898154610909737,0.43919144259659409,5.8638293468023531E-2,1.3250304939118581E-3,0,1.8145857278550588E-3,3.1396162217669169E-3,6.2455246353228723E-2,4.3257924040564728E-2,6.4961923530840959E-2,1.8086666241896863E-3,0.23820738261735674,0.34628231944119697,4.5,0.92854681246033455,6.4766788477409508E-3,1.2239408730587787E-2,4.8516913717847679E-3,1.6010980542614902E-2,0,3.7442839856351802E-4,6.4784014112676208E-4,5.8851210381996701E-3,1.623477530335633E-2,1.7923357463927837E-5,6.1362901938631854E-5,1.3404486005745416E-2,7.6204696639122646E-2,0.92854681246033455,92.854681246033451,375,72.078010752951272,0.72078010752951271,120.45731762835072,null,8.4011971805796823E-3,null,0.23820738261735674,6.4961923530840959E-2,0.10769069322672298,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR81, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.854681246033451},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ81, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.23820738261735674},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA81, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.4961923530840959E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB81, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10769069322672298},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S81, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":120.45731762835072},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P81, IF(MODE_ILIM=4,#REF!,#REF!))","v":47.261749859866143}]
[null,null,null,null,null,null,null,76,0.38,0.95232360099097058,0.95232360099097058,0,43.586677206122772,15.048072951702977,3,45.144218855108932,5.3072098708103659E-6,0.15023189562674305,122063.41519672873,8.1924628963420954E-6,0,6.6E-4,0.49075823541797542,2.8901237475667797E-2,7.972734857292646E-2,0.10913323975718808,0.24549828486485445,3.0134703935792614E-4,3.0134703935792614E-4,0.17256911396803357,8.9340297287136472E-5,8.9340297287136472E-5,0.21303208069166449,3.1177892506424238E-2,4.9008461201486588E-4,54.166666666666664,10.924681300086506,3.7097490449638462E-2,4.1257434336494307E-2,7.8845009398147634E-2,0.11066101216698372,0.44210969026560037,5.9420137380930507E-2,1.3426975671640162E-3,0,1.8506288668002178E-3,3.1933264339642341E-3,6.3309216556653433E-2,4.3257924040564728E-2,6.5251310190711315E-2,1.832782179178882E-3,0.24105432109352734,0.3505782481873605,4.5600000000000005,0.9286075426418936,6.4790745938281928E-3,1.2242120394859758E-2,4.852008689225226E-3,1.6056155795348876E-2,0,3.7686577288190842E-4,6.5029539752125621E-4,5.8855059455240515E-3,1.6235837113960289E-2,1.8193437263750883E-5,6.1366915285213542E-5,1.3287907633850959E-2,7.6145331689549484E-2,0.9286075426418936,92.860754264189353,380,72.090646982404948,0.72090646982404949,122.06341519672873,null,8.4017466480090473E-3,null,0.24105432109352734,6.5251310190711315E-2,0.10913323975718808,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR82, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.860754264189353},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ82, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.24105432109352734},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA82, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.5251310190711315E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB82, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10913323975718808},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S82, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":122.06341519672873},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P82, IF(MODE_ILIM=4,#REF!,#REF!))","v":45.144218855108932}]
[null,null,null,null,null,null,null,77,0.38500000000000001,0.95232360099097058,0.95232360099097058,0,43.359404478850038,14.345902696766274,4,57.383610787065095,5.3072098708103659E-6,0.15220863109551599,123669.51276510675,8.0860672743116777E-6,0,6.6E-4,0.49397635668907203,2.9281516916137115E-2,8.077639263309655E-2,0.11057596265660126,0.2471081269327485,3.0531213198105675E-4,3.0531213198105675E-4,0.17499165246615561,9.1866235298507354E-5,9.1866235298507354E-5,0.21442902733631108,3.1588127934140363E-2,4.9653309375190355E-4,54.166666666666664,10.924681300086506,3.7805160951168877E-2,4.1800295314606079E-2,8.0101989359526865E-2,0.11234647056971445,0.44500880126511294,6.0201981293837484E-2,1.3603646404161743E-3,0,1.8869961796064883E-3,3.2473608200226625E-3,6.4163764336534229E-2,4.3257924040564728E-2,6.554069685058167E-2,1.8568977341680778E-3,0.24390782949099843,0.35488097051487927,4.62,0.92866543488815356,6.4814578280956159E-3,1.2244796182572177E-2,4.8523111783489881E-3,1.6101287615578195E-2,0,3.7930478955985794E-4,6.5275146064179578E-4,5.8858728660409736E-3,1.623684930591144E-2,1.8466016743512073E-5,6.137074108718991E-5,1.3174324619830749E-2,7.6088792604410496E-2,0.92866543488815356,92.866543488815353,385,72.101220909974245,0.7210122090997424,123.66951276510675,null,8.4022704386995453E-3,null,0.24390782949099843,6.554069685058167E-2,0.11057596265660126,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR83, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.866543488815353},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ83, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.24390782949099843},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA83, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.554069685058167E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB83, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11057596265660126},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S83, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":123.66951276510675},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P83, IF(MODE_ILIM=4,#REF!,#REF!))","v":57.383610787065095}]
[null,null,null,null,null,null,null,78,0.39,0.95232360099097058,0.95232360099097058,0,43.132131751577319,13.647972843775717,4,54.591891375102868,5.3072098708103659E-6,0.15418536656428891,125275.61033348474,7.9823997451538375E-6,0,6.600000000000001E-4,0.4971736480396497,2.9661796356606415E-2,8.1825436693266626E-2,0.11201886195730928,0.24870754898240918,3.0927722460418735E-4,3.0927722460418735E-4,0.17742586798163221,9.4439815887106744E-5,9.4439815887106744E-5,0.2158169319700681,3.1998363361856456E-2,5.0298157548894122E-4,54.166666666666664,10.924681300086506,3.8518533936522471E-2,4.2343156292717843E-2,8.1364671804729255E-2,0.11403792268938188,0.44788914720059975,6.0983825206744474E-2,1.3780317136683322E-3,0,1.9236881481031417E-3,3.3017198617714739E-3,6.5018890433611337E-2,4.3257924040564735E-2,6.5830083510452012E-2,1.8810132891572734E-3,0.24676790992260247,0.35919048892040306,4.68,0.92872059714548405,6.4838292889484632E-3,1.2247437501625815E-2,4.8525994031798176E-3,1.6146377475434719E-2,0,3.8174547128804278E-4,6.5520838496399753E-4,5.886222483913516E-3,1.6237813766551406E-2,1.8741068847218666E-5,6.1374386478183521E-5,1.3063622749564973E-2,7.6034971980796159E-2,0.92872059714548405,92.872059714548399,390,72.109847935853821,0.72109847935853821,125.27561033348475,null,8.4027695293156998E-3,null,0.24676790992260247,6.5830083510452012E-2,0.11201886195730928,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR84, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.872059714548399},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ84, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.24676790992260247},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA84, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.5830083510452012E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB84, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11201886195730928},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S84, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":125.27561033348475},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P84, IF(MODE_ILIM=4,#REF!,#REF!))","v":54.591891375102868}]
[null,null,null,null,null,null,null,79,0.39500000000000002,0.95232360099097058,0.95232360099097058,0,42.904859024304592,12.954968747080624,4,51.819874988322496,5.3072098708103659E-6,0.15616210203306186,126881.70790186276,7.881356710405054E-6,0,6.6E-4,0.50035050878588883,3.0042075797075737E-2,8.2874480753436702E-2,0.11346193769166703,0.25029675076888946,3.1324231722731785E-4,3.1324231722731785E-4,0.17987160558761664,9.7061383490001363E-5,9.7061383490001363E-5,0.21719596793115103,3.2408598789572571E-2,5.094300572259789E-4,54.166666666666664,10.924681300086506,3.9237609405699286E-2,4.2886017270829607E-2,8.2633056733754873E-2,0.1157353698984976,0.45075108780428713,6.1765669119651437E-2,1.3956987869204905E-3,0,1.9607052541194482E-3,3.3564040410399387E-3,6.5874595589058407E-2,4.3257924040564728E-2,6.6119470170322367E-2,1.9051288441464694E-3,0.24963456450202484,0.3635068058944092,4.74,0.92877313194241873,6.4861896777546118E-3,1.2250045689331046E-2,4.8528738994330876E-3,1.6191426773119216E-2,0,3.8418783959588096E-4,6.5766622220693124E-4,5.8865554489665748E-3,1.6238732288496014E-2,1.9018566484108171E-5,6.137785823377988E-5,1.2955693542713847E-2,7.5983767806335104E-2,0.92877313194241873,92.877313194241879,395,72.116619551864289,0.72116619551864292,126.88170790186275,null,8.4032448475031794E-3,null,0.24963456450202484,6.6119470170322367E-2,0.11346193769166703,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR85, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.877313194241879},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ85, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.24963456450202484},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA85, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.6119470170322367E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB85, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11346193769166703},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S85, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":126.88170790186275},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P85, IF(MODE_ILIM=4,#REF!,#REF!))","v":51.819874988322496}]
[null,null,null,null,null,null,null,80,0.4,0.95232360099097058,0.95232360099097058,0,42.677586297031858,12.267725203364908,4,49.07090081345963,5.3072098708103659E-6,0.1581388375018348,128487.80547024077,7.7828397515249912E-6,0,6.6E-4,0.50350732564635259,3.0422355237545058E-2,8.3923524813606806E-2,0.11490518989203717,0.2518759257453751,3.1720740985044857E-4,3.1720740985044857E-4,0.18232871003656018,9.9731275510788118E-5,9.9731275510788118E-5,0.21856630308930552,3.2818834217288678E-2,5.1587853896301668E-4,54.166666666666664,10.924681300086506,3.9962387358699281E-2,4.3428878248941379E-2,8.3907144146603677E-2,0.117438813569992,0.45359497145957856,6.2547513032558427E-2,1.4133658601726486E-3,0,1.9980479794846789E-3,3.4114138396573275E-3,6.6730880544482798E-2,4.3257924040564728E-2,6.6408856830192708E-2,1.9292443991356652E-3,0.25250779534380319,0.36782992392120162,4.8000000000000007,0.92882313672542416,6.4885396611399021E-3,1.2252622016782715E-2,4.853135176270184E-3,1.6236436837483485E-2,0,3.8663191492351148E-4,6.6012502150396702E-4,5.8868723788149443E-3,1.6239606575505879E-2,1.929848253115785E-5,6.1381162793716835E-5,1.285043389736858E-2,7.5935083125118041E-2,0.92882313672542416,92.882313672542409,400,72.121604042494241,0.72121604042494236,128.48780547024077,null,8.4036972749267237E-3,null,0.25250779534380319,6.6408856830192708E-2,0.11490518989203717,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR86, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.882313672542409},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ86, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.25250779534380319},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA86, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.6408856830192708E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB86, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11490518989203717},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S86, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":128.48780547024077},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P86, IF(MODE_ILIM=4,#REF!,#REF!))","v":49.07090081345963}]
[null,null,null,null,null,null,null,81,0.40500000000000003,0.95232360099097058,0.95232360099097058,0,42.450313569759132,11.587267237220177,4,46.349068948880706,5.3072098708103659E-6,0.16011557297060772,130093.90303861878,7.6867553101481381E-6,0,6.5999999999999989E-4,0.50664447329146534,3.0802634678014362E-2,8.4972568873776883E-2,0.11634861859079024,0.25344526133805662,3.2117250247357907E-4,3.2117250247357907E-4,0.18479702587757776,1.0244982231959445E-4,1.0244982231959445E-4,0.21992810008432925,3.3229069645004793E-2,5.2232702070005447E-4,54.166666666666664,10.924681300086506,4.0692867795522482E-2,4.3971739227053143E-2,8.5186934043275681E-2,0.11914825507721487,0.45642113569606263,6.3329356945465418E-2,1.4310329334248067E-3,0,2.035716806028104E-3,3.4667497394529107E-3,6.7587746041925897E-2,4.3257924040564721E-2,6.6698243490063064E-2,1.9533599541248611E-3,0.25538760456332871,0.37215984547891212,4.8600000000000003,0.92887070417000084,6.4908798731149282E-3,1.2255167692913601E-2,4.8533837179240173E-3,1.6281408932275903E-2,0,3.890777166884835E-4,6.625848295610683E-4,5.8871738608350793E-3,1.6240438247925724E-2,1.9580789835410114E-5,6.1384306282443357E-5,1.2747745760805977E-2,7.5888825728162634E-2,0.92887070417000084,92.887070417000089,405,72.124846875437001,0.72124846875436999,130.09390303861878,null,8.4041276500848756E-3,null,0.25538760456332871,6.6698243490063064E-2,0.11634861859079024,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR87, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.887070417000089},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ87, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.25538760456332871},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA87, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.6698243490063064E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB87, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11634861859079024},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S87, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":130.09390303861878},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P87, IF(MODE_ILIM=4,#REF!,#REF!))","v":46.349068948880706}]
[null,null,null,null,null,"Eff (%)","Iout (mA)",82,0.41,0.95232360099097058,0.95232360099097058,0,42.223040842486412,10.914864008418993,4,43.659456033675973,5.3072098708103659E-6,0.16209230843938063,131700.00060699676,7.5930143917316994E-6,0,6.6E-4,0.50976231486255497,3.1182914118483677E-2,8.6021612933946945E-2,0.11779222382030481,0.25500493920577683,3.2513759509670968E-4,3.2513759509670968E-4,0.18727639756349268,1.052173472530781E-4,1.052173472530781E-4,0.22128151655138148,3.3639305072720893E-2,5.2877550243709203E-4,54.166666666666664,10.924681300086506,4.1429050716168876E-2,4.4514600205164907E-2,8.6472426423770871E-2,0.12086369579393533,0.45922990765710292,6.411120085837238E-2,1.4487000066769646E-3,0,2.0737122155789931E-3,3.5224122222559575E-3,6.8445192823863424E-2,4.3257924040564728E-2,6.6987630149933405E-2,1.9774755091140567E-3,0.25827399427684622,0.37649657303950079,4.92,0.92891592246921051,6.4932109170474433E-3,1.2257683868253735E-2,4.8536199852065899E-3,1.6326344260078871E-2,0,3.9152526334760787E-4,6.6504569080360048E-4,5.8874604539937876E-3,1.6241228847729005E-2,1.9865461216129328E-5,6.1387294528187145E-5,1.2647535824136523E-2,7.5844907866341488E-2,0.92891592246921051,92.89159224692105,410,72.126370778645395,0.72126370778645399,131.70000060699675,null,8.4045367709205017E-3,null,0.25827399427684622,6.6987630149933405E-2,0.11779222382030481,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR88, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.89159224692105},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ88, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.25827399427684622},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA88, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.6987630149933405E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB88, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11779222382030481},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S88, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":131.70000060699675},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P88, IF(MODE_ILIM=4,#REF!,#REF!))","v":43.659456033675973}]
[null,null,null,null,null,{"$f":"BT51","v":68.427867006324419},{"$f":"I56*1000","v":250},83,0.41499999999999998,0.95232360099097058,0.95232360099097058,0,41.995768115213679,10.252100494622894,5,51.260502473114478,5.3072098708103659E-6,0.16406904390815358,133306.09817537479,7.501532290626497E-6,0,6.5999999999999989E-4,0.51286120246249367,3.1563193558952991E-2,8.7070656994117049E-2,0.11923600561296742,0.25655513548547038,3.2910268771984034E-4,3.2910268771984034E-4,0.18976666954835822,1.0803416661442736E-4,1.0803416661442736E-4,0.22262670533396459,3.4049540500437001E-2,5.3522398417412981E-4,54.166666666666664,10.924681300086506,4.2170936120638457E-2,4.5057461183276679E-2,8.7763621288089261E-2,0.12258513709434216,0.46202160454184282,6.4893044771279371E-2,1.4663670799291229E-3,0,2.1120346899666182E-3,3.5784017698957411E-3,6.9303221633205833E-2,4.3257924040564721E-2,6.7277016809803761E-2,2.0015910641032527E-3,0.261166966601455,0.38084010906875665,4.9799999999999995,0.92895887560151214,6.4955333674933686E-3,1.2260171638420176E-2,4.8538444169084535E-3,1.6371243965963924E-2,0,3.9397457245437314E-4,6.6750764751261223E-4,5.8877326905457557E-3,1.6241979843200787E-2,2.0152469466804193E-5,6.1390133080654319E-5,1.2549715238847257E-2,7.580324598389418E-2,0.92895887560151214,92.895887560151209,415,72.126175499523185,0.72126175499523182,133.30609817537479,null,8.4049253972440733E-3,null,0.261166966601455,6.7277016809803761E-2,0.11923600561296742,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR89, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.895887560151209},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ89, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.261166966601455},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA89, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.7277016809803761E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB89, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11923600561296742},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S89, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":133.30609817537479},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P89, IF(MODE_ILIM=4,#REF!,#REF!))","v":51.260502473114478}]
[null,null,null,null,null,{"$f":"BT81","v":72.078010752951272},{"$f":"I81*1000","v":375},84,0.42,0.95232360099097058,0.95232360099097058,0,41.768495387940952,9.6009732170992095,5,48.004866085496047,5.3072098708103659E-6,0.16604577937692652,134912.19574375279,7.4122283347857065E-6,0,6.6E-4,0.51594147761981601,3.1943472999422295E-2,8.8119701054287125E-2,0.12067996400117226,0.25809602102433543,3.3306778034297095E-4,3.3306778034297095E-4,0.19226768637619163,1.1090058967336076E-4,1.1090058967336076E-4,0.2239638146853917,3.4459775928153115E-2,5.4167246591116749E-4,54.166666666666664,10.924681300086506,4.2918524008931244E-2,4.5600322161388443E-2,8.9060518636230851E-2,0.12431258035304379,0.46479653402331506,6.5674888684186347E-2,1.4840341531812808E-3,0,2.1506847110202491E-3,3.6347188642015301E-3,7.0161833213298511E-2,4.3257924040564728E-2,6.7566403469674102E-2,2.0257066190924483E-3,0.26406652365510891,0.38519045602629753,5.04,0.9289996435796225,6.4978477718980318E-3,1.2262632047359502E-2,4.8540574310990013E-3,1.6416109140887855E-2,0,3.9642566071229266E-4,6.6997073995145871E-4,5.8879910776108348E-3,1.6242692633288813E-2,2.0441787357008354E-5,6.1392827227475401E-5,1.2454199353429406E-2,7.5763760470821673E-2,0.9289996435796225,92.899964357962247,420,72.124237241864293,0.72124237241864297,134.91219574375279,null,8.4052942529852827E-3,null,0.26406652365510891,6.7566403469674102E-2,0.12067996400117226,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR90, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.899964357962247},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ90, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.26406652365510891},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA90, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.7566403469674102E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB90, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12067996400117226},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S90, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":134.91219574375279},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P90, IF(MODE_ILIM=4,#REF!,#REF!))","v":48.004866085496047}]
[null,null,null,null,null,{"$f":"BT106","v":71.049894896969974},{"$f":"I106*1000","v":500},85,0.42499999999999999,0.95232360099097058,0.95232360099097058,0,41.541222660668225,8.9640182291820576,5,44.82009114591029,5.3072098708103659E-6,0.16802251484569947,136518.29331213082,7.3250256484941091E-6,0,6.6E-4,0.51900347172804484,3.2323752439891607E-2,8.9168745114457229E-2,0.12212409901732175,0.25962776159960305,3.3703287296610161E-4,3.3703287296610161E-4,0.19477929276160008,1.1381691866612735E-4,1.1381691866612735E-4,0.22529298845949258,3.4870011355869229E-2,5.4812094764820527E-4,54.166666666666664,10.924681300086506,4.3671814381047225E-2,4.6143183139500214E-2,9.0363118468195641E-2,0.12604602694506861,0.46755499464421763,6.6456732597093324E-2,1.5017012264334391E-3,0,2.189662760569156E-3,3.6913639870025951E-3,7.1021028307922146E-2,4.3257924040564728E-2,6.7855790129544458E-2,2.0498221740816443E-3,0.26697266755661681,0.38954761636557078,5.0999999999999996,0.92903830268194743,6.500154652178302E-3,1.2265066090363212E-2,4.8542594263357251E-3,1.6460940824851025E-2,0,3.9887854402451692E-4,6.7243500648356031E-4,5.8882360986408549E-3,1.6243368551649911E-2,2.0733387634131024E-5,6.1395382009499504E-5,1.2360907468449889E-2,7.5726375432620632E-2,0.92903830268194743,92.903830268194739,425,72.120507778355574,0.72120507778355569,136.51829331213082,null,8.4056440282869686E-3,null,0.26697266755661681,6.7855790129544458E-2,0.12212409901732175,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR91, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.903830268194739},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ91, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.26697266755661681},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA91, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.7855790129544458E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB91, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12212409901732175},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S91, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":136.51829331213082},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P91, IF(MODE_ILIM=4,#REF!,#REF!))","v":44.82009114591029}]
[null,null,null,null,null,null,null,86,0.43,0.95232360099097058,0.95232360099097058,0,41.313949933395499,8.3444815803501395,5,41.722407901750707,5.3072098708103659E-6,0.16999925031447238,138124.39088050881,7.2398509316511548E-6,0,6.6E-4,0.52204750646182363,3.2704031880360931E-2,9.0217789174627291E-2,0.12356841069382606,0.26115051812670487,3.40997965589232E-4,3.40997965589232E-4,0.19730133366292485,1.1678344879550641E-4,1.1678344879550641E-4,0.22661436629125176,3.5280246783585323E-2,5.5456942938524295E-4,54.166666666666664,10.924681300086506,4.4430807236986412E-2,4.6686044117611979E-2,9.1671420783983631E-2,0.127785478245865,0.47029727619179562,6.7238576510000314E-2,1.519368299685597E-3,0,2.2289693204426103E-3,3.7483376201282075E-3,7.1880807661293122E-2,4.3257924040564728E-2,6.8145176789414813E-2,2.0739377290708398E-3,0.2698854004256438,0.3939115925338546,5.16,0.92907492566799377,6.5024545061951721E-3,1.2267474716874439E-2,4.8544507827897286E-3,1.6505740009837008E-2,0,4.0133323754001096E-4,6.7490048368200751E-4,5.8884682147848895E-3,1.6244008870416198E-2,2.1027243024987802E-5,6.1397802235029609E-5,1.2269762608577104E-2,7.5691018475956579E-2,0.92907492566799377,92.907492566799377,430,72.229662267470047,0.72229662267470052,138.12439088050883,null,8.4059753814540745E-3,null,0.2698854004256438,6.8145176789414813E-2,0.12356841069382606,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR92, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.907492566799377},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ92, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.2698854004256438},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA92, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.8145176789414813E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB92, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12356841069382606},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S92, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":138.12439088050883},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P92, IF(MODE_ILIM=4,#REF!,#REF!))","v":41.722407901750707}]
[null,null,null,null,null,null,null,87,0.435,0.95232360099097058,0.95232360099097058,0,41.086677206122772,7.7465435395755629,6,46.479261237453379,5.3072098708103659E-6,0.17197598578324536,139730.48844888684,7.1566342542758534E-6,0,6.6E-4,0.52507389417133665,3.3084311320830243E-2,9.1266833234797395E-2,0.12501289906310337,0.26266444685657886,3.4496305821236272E-4,3.4496305821236272E-4,0.19983365434848377,1.1980046823080786E-4,1.1980046823080786E-4,0.22792808376802148,3.5690482211301444E-2,5.6101791112228062E-4,54.166666666666664,10.924681300086506,4.5195502576748786E-2,4.722890509572375E-2,9.2985425583594822E-2,0.12953093563130158,0.47302366005316243,6.8020420422907291E-2,1.5370353729377553E-3,0,2.268604872469882E-3,3.8056402454076372E-3,7.2741172018063682E-2,4.3257924040564728E-2,6.8434563449285155E-2,2.0980532840600358E-3,0.27280472438271047,0.39828238697225704,5.22,0.92910958197904059,6.5047478091256042E-3,1.2269858833102554E-2,4.8546318632942632E-3,1.6550507642551143E-2,0,4.0378975569657221E-4,6.7736720643166734E-4,5.8886878661611169E-3,1.6244614803703719E-2,2.1323326237321692E-5,6.1400092493084252E-5,1.218069131020756E-2,7.5657620509004611E-2,0.92910958197904059,92.910958197904066,435,72.361493645121143,0.72361493645121144,139.73048844888683,null,8.4062889407692867E-3,null,0.27280472438271047,6.8434563449285155E-2,0.12501289906310337,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR93, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.910958197904066},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ93, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.27280472438271047},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA93, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.8434563449285155E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB93, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12501289906310337},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S93, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":139.73048844888683},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P93, IF(MODE_ILIM=4,#REF!,#REF!))","v":46.479261237453379}]
[null,null,null,null,null,null,null,88,0.44,0.95232360099097058,0.95232360099097058,0,40.859404478850045,7.1756055291744998,6,43.053633175046997,5.3072098708103659E-6,0.17395272125201827,141336.58601726484,7.0753088650227192E-6,0,6.6E-4,0.52808293825638442,3.3464590761299554E-2,9.2315877294967472E-2,0.12645756415757969,0.26416969956279746,3.4892815083549338E-4,3.4892815083549338E-4,0.20237610045644533,1.2286825810787176E-4,1.2286825810787176E-4,0.22923427259190277,3.6100717639017545E-2,5.674663928593183E-4,54.166666666666664,10.924681300086506,4.596590040033436E-2,4.7771766073835514E-2,9.4305132867029184E-2,0.13128240047766726,0.4757344195522934,6.8802264335814281E-2,1.5547024461899134E-3,0,2.3085698984802411E-3,3.8632723446701545E-3,7.36021221233224E-2,4.3257924040564728E-2,6.872395010915551E-2,2.1221688390492318E-3,0.27573064154919441,0.40266000211571745,5.28,0.92914233792523171,6.5070350147415166E-3,1.2272219304460884E-2,4.8548030143222747E-3,1.6595244626973694E-2,0,4.0624811226093672E-4,6.7983520802437859E-4,5.8888954730426093E-3,1.6245187510883503E-2,2.1621609961202419E-5,6.1402257165761023E-5,1.2093623423461692E-2,7.5626115555298454E-2,0.92914233792523171,92.914233792523177,440,72.477313046906502,0.724773130469065,141.33658601726484,null,8.4065853061857567E-3,null,0.27573064154919441,6.872395010915551E-2,0.12645756415757969,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR94, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.914233792523177},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ94, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.27573064154919441},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA94, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.872395010915551E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB94, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12645756415757969},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S94, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":141.33658601726484},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P94, IF(MODE_ILIM=4,#REF!,#REF!))","v":43.053633175046997}]
[null,null,null,null,null,null,null,89,0.44500000000000001,0.95232360099097058,0.95232360099097058,0,40.632131751577319,6.6386374011646412,7,46.470461808152486,5.3072098708103659E-6,0.17592945672079122,142942.68358564287,6.9958110126067328E-6,0,6.600000000000001E-4,0.53107493352138224,3.3844870201768865E-2,9.3364921355137576E-2,0.12790240600968913,0.2656664237191535,3.5289324345862404E-4,3.5289324345862404E-4,0.20492851804882981,1.2598709252906867E-4,1.2598709252906867E-4,0.2305330607338465,3.6510953066733652E-2,5.7391487459635608E-4,54.166666666666664,10.924681300086506,4.674200070774312E-2,4.8314627051947286E-2,9.5630542634286761E-2,0.13303987416167171,0.47842982026983355,6.9584108248721271E-2,1.5723695194420715E-3,0,2.348864880302959E-3,3.9212343997450305E-3,7.4463658722594375E-2,4.3257924040564735E-2,6.9013336769025865E-2,2.1462843940384278E-3,0.27866315404733039,0.40704444039300725,5.34,0.92917325686015195,6.5093165566032646E-3,1.2274556957841335E-2,4.8549645668985869E-3,1.6639951826742293E-2,0,4.0870832036620441E-4,6.8230452024778149E-4,5.8890914369637984E-3,1.624572809963392E-2,2.1922066870332596E-5,6.1404300439773818E-5,1.2008491927427386E-2,7.5596440580034674E-2,0.92917325686015195,92.917325686015189,445,72.230234640211876,0.72230234640211877,142.94268358564287,null,8.4068650509066412E-3,null,0.27866315404733039,6.9013336769025865E-2,0.12790240600968913,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR95, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.917325686015189},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ95, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.27866315404733039},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA95, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.9013336769025865E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB95, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12790240600968913},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S95, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":142.94268358564287},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P95, IF(MODE_ILIM=4,#REF!,#REF!))","v":46.470461808152486}]
[null,null,null,null,null,null,null,90,0.45,0.95232360099097058,0.95232360099097058,0,40.404859024304585,6.1445514329369075,7,43.011860030558353,5.3072098708103659E-6,0.17790619218956413,144548.78115402086,6.918079779133325E-6,0,6.5999999999999989E-4,0.53405016651245873,3.422514964223819E-2,9.4413965415307652E-2,0.1293474246518736,0.26715476266829108,3.568583360817547E-4,3.568583360817547E-4,0.20749075366009256,1.2915723856329965E-4,1.2915723856329965E-4,0.23182457257998329,3.6921188494449766E-2,5.8036335633339375E-4,54.166666666666664,10.924681300086506,4.7523803498975101E-2,4.885748803005905E-2,9.6961654885367538E-2,0.13480335806044508,0.48111012034677969,7.036595216162822E-2,1.5900365926942296E-3,0,2.3894902997673054E-3,3.979526892461535E-3,7.5325782561841637E-2,4.3257924040564721E-2,6.9302723428896207E-2,2.1703999490276234E-3,0.28160226400021054,0.4114357042267292,5.4,0.92920239934385107,6.5115928491740515E-3,1.2276872583738488E-2,4.8551168374516892E-3,1.6684630067376659E-2,0,4.1117039254678483E-4,6.8477517346826622E-4,5.889276141753717E-3,1.6246237628790971E-2,2.2224669623267445E-5,6.1406226317226083E-5,1.1925232757628459E-2,7.5568535327869571E-2,0.92920239934385107,92.920239934385108,450,72.8349974854723,0.72834997485472297,144.54878115402087,null,8.407128722860065E-3,null,0.28160226400021054,6.9302723428896207E-2,0.1293474246518736,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR96, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.920239934385108},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ96, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.28160226400021054},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA96, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.9302723428896207E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB96, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1293474246518736},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S96, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":144.54878115402087},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P96, IF(MODE_ILIM=4,#REF!,#REF!))","v":43.011860030558353}]
[null,null,null,null,null,null,null,91,0.45500000000000002,0.95232360099097058,0.95232360099097058,0,40.177586297031858,5.7045010311082072,8,45.636008248865657,5.3072098708103659E-6,0.17988292765833705,146154.87872239886,6.8420569244175747E-6,0,6.6E-4,0.53700891583774391,3.4605429082707494E-2,9.5463009475477714E-2,0.13079262011658294,0.26863485578192758,3.608234287048852E-4,3.608234287048852E-4,0.21006265434071172,1.3237895624599601E-4,1.3237895624599601E-4,0.23310892907065681,3.7331423922165867E-2,5.8681183807043143E-4,54.166666666666664,10.924681300086506,4.8311308774030254E-2,4.9400349008170814E-2,9.82984696202715E-2,0.13657285355153836,0.4837755707730193,7.1147796074535224E-2,1.6077036659463875E-3,0,2.4304466387025511E-3,4.0381503046489388E-3,7.6188494387463515E-2,4.3257924040564728E-2,6.9592110088766562E-2,2.1945155040168189E-3,0.28454797353178529,0.4158337960333191,5.46,0.9292298232951991,6.5138642888614862E-3,1.2279166938234725E-2,4.8552601286098182E-3,1.6729280138357762E-2,0,4.1363434077105896E-4,6.8724719670849594E-4,5.8894499545016164E-3,1.62467171110121E-2,2.2529390864554902E-5,6.1408038625679185E-5,1.1843784644784723E-2,7.554234217133203E-2,0.9292298232951991,92.922982329519911,455,73.305168165960453,0.73305168165960455,146.15487872239885,null,8.4073768460776049E-3,null,0.28454797353178529,6.9592110088766562E-2,0.13079262011658294,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR97, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.922982329519911},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ97, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.28454797353178529},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA97, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.9592110088766562E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB97, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13079262011658294},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S97, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":146.15487872239885},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P97, IF(MODE_ILIM=4,#REF!,#REF!))","v":45.636008248865657}]
[null,null,null,null,null,null,null,92,0.46,0.95232360099097058,0.95232360099097058,0,39.950313569759139,5.3318819988691422,8,42.655055990953137,5.3072098708103659E-6,0.18185966312711002,147760.97629077689,6.7676867404565137E-6,0,6.6E-4,0.53995145247186194,3.4985708523176805E-2,9.6512053535647818E-2,0.13223799243627513,0.27010683861317392,3.6478852132801592E-4,3.6478852132801592E-4,0.21264406769616964,1.3565249857911953E-4,1.3565249857911953E-4,0.23438624783260023,3.7741659349881981E-2,5.9326031980746921E-4,54.166666666666664,10.924681300086506,4.9104516532908614E-2,4.9943209986282586E-2,9.9640986838998663E-2,0.13834836201292369,0.48642641566163769,7.1929639987442215E-2,1.6253707391985458E-3,0,2.4717343789379675E-3,4.0971051181365129E-3,7.7051794946296756E-2,4.3257924040564728E-2,6.9881496748636918E-2,2.2186310590060149E-3,0.28750028476686335,0.42023871822304559,5.5200000000000005,0.92925558413437714,6.5161312549917002E-3,1.2281440744856764E-2,4.8553947299454676E-3,1.6773902795072369E-2,0,4.161001764719244E-4,6.8972061771990778E-4,5.889613226460093E-3,1.6247167515267516E-2,2.2836203225802079E-5,6.140974102756904E-5,1.1764088964010719E-2,7.5517805969049834E-2,0.92925558413437714,92.925558413437713,460,73.638455592594738,0.73638455592594743,147.76097629077688,null,8.4076099219834929E-3,null,0.28750028476686335,6.9881496748636918E-2,0.13223799243627513,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR98, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.925558413437713},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ98, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.28750028476686335},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA98, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.9881496748636918E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB98, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13223799243627513},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S98, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":147.76097629077688},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P98, IF(MODE_ILIM=4,#REF!,#REF!))","v":42.655055990953137}]
[null,null,null,null,null,null,null,93,0.46500000000000002,0.95232360099097058,0.95232360099097058,0,39.723040842486405,5.0416677022447267,8,40.333341617957814,5.3072098708103659E-6,0.18383639859588294,149367.07385915489,6.6949159152903149E-6,0,6.6E-4,0.54287804004556828,3.5365987963646116E-2,9.7561097595817894E-2,0.13368354164341578,0.27157084304142315,3.6875361395114647E-4,3.6875361395114647E-4,0.21523484192168821,1.3897811153116234E-4,1.3897811153116234E-4,0.23565664330466404,3.8151894777598082E-2,5.9970880154450689E-4,54.166666666666664,10.924681300086506,4.9903426775610167E-2,5.048607096439435E-2,0.10098920654154903,0.14012988482299438,0.48906289250984475,7.2711483900349164E-2,1.6430378124507039E-3,0,2.5133540023028235E-3,4.1563918147535274E-3,7.7915684985615977E-2,4.3257924040564728E-2,7.0170883408507259E-2,2.2427466139952109E-3,0.29045919983111279,0.42465047320001087,5.58,0.92927973491624316,6.5183941107210559E-3,1.2283694696313355E-2,4.855520918672228E-3,1.6818498760633047E-2,0,4.1856791057538469E-4,6.9219546305057363E-4,5.889766293890342E-3,1.6247589769171931E-2,2.3145079326673586E-5,6.141133702901937E-5,1.1686089593673159E-2,7.5494873933056775E-2,0.92927973491624316,92.927973491624314,465,73.832411821820315,0.73832411821820321,149.36707385915489,null,8.4078284306012586E-3,null,0.29045919983111279,7.0170883408507259E-2,0.13368354164341578,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR99, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.927973491624314},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ99, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.29045919983111279},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA99, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0170883408507259E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB99, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13368354164341578},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S99, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":149.36707385915489},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P99, IF(MODE_ILIM=4,#REF!,#REF!))","v":40.333341617957814}]
[null,null,null,null,null,null,null,94,0.47,0.95232360099097058,0.95232360099097058,0,39.495768115213679,4.8486776263114315,9,43.63809863680288,5.3072098708103659E-6,0.18581313406465585,150973.17142753288,6.623693405553184E-6,0,6.5999999999999989E-4,0.54578893512140925,3.574626740411542E-2,9.8610141655987971E-2,0.13512926777047871,0.27302699741024766,3.7271870657427697E-4,3.7271870657427697E-4,0.21783482583305097,1.4235603403714697E-4,1.4235603403714697E-4,0.23692022685747671,3.8562130205314189E-2,6.0615728328154456E-4,54.166666666666664,10.924681300086506,5.0708039502134906E-2,5.1028931942506114E-2,0.10234312872792256,0.1419174233605649,0.49168523244730833,7.349332781325614E-2,1.6607048857028618E-3,0,2.5553059906263907E-3,4.2160108763292523E-3,7.8780165253134138E-2,4.3257924040564721E-2,7.0460270068377601E-2,2.2668621689844065E-3,0.29342472085106108,0.42906906336215123,5.64,0.92930232645524469,6.5206532038900407E-3,1.2285929456122837E-2,4.855638960297462E-3,1.6863068727582805E-2,0,4.2103755352732779E-4,6.9467175810875698E-4,5.8899094788538546E-3,1.6247984761168593E-2,2.3455991775826715E-5,6.1412829988096685E-5,1.1609732783192935E-2,7.5473495504508534E-2,0.92930232645524469,92.93023264552447,470,73.8844086186851,0.73884408618685105,150.97317142753289,null,8.4080328316839155E-3,null,0.29342472085106108,7.0460270068377601E-2,0.13512926777047871,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR100, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.93023264552447},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ100, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.29342472085106108},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA100, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0460270068377601E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB100, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13512926777047871},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S100, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":150.97317142753289},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P100, IF(MODE_ILIM=4,#REF!,#REF!))","v":43.63809863680288}]
[null,null,null,null,null,null,null,95,0.47499999999999998,0.95232360099097058,0.95232360099097058,0,39.268495387940952,4.7647403037281144,9,42.882662733553033,5.3072098708103659E-6,0.18778986953342883,152579.26899591091,6.5539703170736767E-6,0,6.6E-4,0.54868438745621895,3.6126546844584745E-2,9.9659185716158075E-2,0.13657517084994567,0.27447542665871116,3.7668379919740763E-4,3.7668379919740763E-4,0.22044386889381951,1.4578649799862646E-4,1.4578649799862646E-4,0.23817710690739116,3.8972365633030318E-2,6.1260576501858234E-4,54.166666666666664,10.924681300086506,5.151835471248286E-2,5.1571792920617886E-2,0.10370275339811932,0.14371097900487154,0.49429366047262974,7.4275171726163131E-2,1.6783719589550201E-3,0,2.5975908257379397E-3,4.2759627846929594E-3,7.9645236497002544E-2,4.3257924040564728E-2,7.0749656728247956E-2,2.2909777239736025E-3,0.2963968499540956,0.43349449110123728,5.6999999999999993,0.92932340744249931,6.5229088678237235E-3,1.2288145660138586E-2,4.8557491092340579E-3,1.6907613359492892E-2,0,4.2350911531862414E-4,6.9714952722248755E-4,5.8900430899544859E-3,1.6248353342576294E-2,2.3768913171788186E-5,6.1414223122547556E-5,1.1534967029137288E-2,7.5453622237192763E-2,0.92932340744249931,92.932340744249927,475,73.791636151568156,0.73791636151568152,152.57926899591092,null,8.4082235657732592E-3,null,0.2963968499540956,7.0749656728247956E-2,0.13657517084994567,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR101, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.932340744249927},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ101, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.2963968499540956},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA101, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0749656728247956E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB101, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13657517084994567},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S101, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":152.57926899591092},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P101, IF(MODE_ILIM=4,#REF!,#REF!))","v":42.882662733553033}]
[null,null,null,null,null,null,null,96,{"$f":"IF(PLOT_TYPE=1, H102/100*Iout, min_I*EXP(H102*rr/100))","v":0.48},{"$f":"IF(I102<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I102-Vout)/L*OnTime)","v":0.9522649773755657},{"$f":"IF(I102<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I102+((Vin-(Rdcr+RdsonTop)*J102-Vout)/L*OnTime)/2)","v":0.95268345849102187},{"$f":"IF(I102<Icrit, 0, I102-((Vin-(Rdcr+RdsonTop)*K102-Vout)/L*OnTime)/2)","v":7.3195977466266604E-3},18.653231295757191,{"$f":"IF(I102<Icrit, 1000*SQRT((J102*CoutEsr)^2+(((J102/2)-I102)*(OnTime+OffTime)/Cout)^2), 1000*J102*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":18.653231295757191},1,{"$f":"IF(I102<Icrit, 1000*((N102/1000)*O102), 1000*J102*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":18.653231295757191},5.3061754691710642E-6,0.18827897240441271,152976.66507858533,6.5369446999402952E-6,0,{"$f":"S102*(T102*Iq_active+U102*Iq_sleep)","v":6.6E-4},0.55310127978739065,{"$f":"W102^2*Rdcr","v":3.6710523084293928E-2},{"$f":"Core_Loss/1000*S102/$S$106","v":9.9918750270810541E-2},{"$f":"(Y102+X102*(1+Ltc*(Ta-25)))/(1-X102*Ltc*ThetaCa)","v":0.1374365320724277},0.27481089080029097,3.7760512851224727E-4,3.7760512851224727E-4,0.22233095451186974,1.4829316000247728E-4,1.4829316000247728E-4,0.2399968673882247,3.9570166996682692E-2,6.1420131029052004E-4,{"$f":"20*VIN_nom/24","v":54.166666666666664},10.878815560909343,{"$f":"IF(I102<Icrit, Vin*(I102+Iripple/2)*AK102/1000000000/2*S102, Vin*(I102-Iripple/2)*AJ102/1000000000/2*S102 + Vin*(I102+Iripple/2)*AK102/1000000000/2*S102)","v":5.278697917218754E-2},5.1706112796561836E-2,0.10510729327903989,{"$f":"(AI102+AL102+AM102+AH102*(1+RdsonTopTc*(Ta-25)))/(1-AH102*RdsonTopTc*ThetaJA)","v":0.14574408873689426},0.49807024538851086,7.5414486679776904E-2,1.6827433158644388E-3,{"$f":"IF(I102<Icrit, Vin*Idss*R102, QrrBot*(I102-Iripple/2)/1*S102*Vin+Vin*Idss*R102)","v":1.1972673699238612E-4},2.6293403260067932E-3,4.431810378863618E-3,{"$f":"(AR102+AS102+AT102+AQ102*(1+RdsonBotTc*(Ta-25)))/(1-AQ102*RdsonBotTc*ThetaJA)","v":8.0975739327201909E-2},{"$f":"Vin*V102+Vout*Ifb/0.8","v":4.3257924040564728E-2},{"$f":"(Vin-Vdd)*(S102*QgBot+S102*QgTop)+AW102","v":7.082125955442424E-2},2.296944626154959E-3,0.29983803224467542,{"$f":"SUM(Z102,AC102,AF102,AZ102)","v":0.43780046260561789},5.76,0.92936196232081303,6.5566479113092083E-3,1.235017639082857E-2,4.8178834281897651E-3,1.6958805613895438E-2,1.9317617228040249E-5,4.2423765364356245E-4,7.1506180387750657E-4,5.9231534325421718E-3,1.6121646844500653E-2,2.3926739961572326E-5,6.0925667225094603E-5,1.1426837630821415E-2,7.5398620734023009E-2,0.92936196232081303,92.936196232081301,480,73.551124384272143,0.73551124384272137,152.97666507858531,null,8.3426552869086817E-3,null,0.29983803224467542,7.082125955442424E-2,0.1374365320724277,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR102, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.936196232081301},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ102, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.29983803224467542},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA102, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.082125955442424E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB102, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1374365320724277},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S102, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":152.97666507858531},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P102, IF(MODE_ILIM=4,#REF!,#REF!))","v":18.653231295757191}]
[null,null,null,null,null,null,null,97,{"$f":"IF(PLOT_TYPE=1, H103/100*Iout, min_I*EXP(H103*rr/100))","v":0.48499999999999999},0.95219194570135746,0.95768399185356567,1.2356117478966755E-2,18.65180073100548,18.65180073100548,1,18.65180073100548,5.3048469648205497E-6,0.18831724414902928,153007.7608710863,{"$f":"IF(1/S103-OnTime-Q103>Tsleep, OnTime+Q103+Tsleep, 1/S103)","v":6.5356161955897807E-6},0,6.5999999999999989E-4,0.55744598456034233,3.7289523084293931E-2,9.9939060902656127E-2,0.13805224838744323,0.27481089080029097,3.7760512851224727E-4,3.7760512851224727E-4,0.22400214415209474,1.505308817542075E-4,1.505308817542075E-4,0.24190666627968049,{"$f":"RdsonTop*AG103^2","v":4.0202439775906963E-2},6.143261598974115E-4,54.166666666666664,10.822213223591897,5.4144496321190415E-2,5.1716623174427163E-2,0.10647544565551499,0.14777667017866908,0.50203368879867583,{"$f":"RdsonBot*AP103^2","v":7.661949870539693E-2},1.6830853695819494E-3,2.689336408722381E-4,2.6573090874198995E-3,4.6093280978740866E-3,8.2396448440851255E-2,4.3257924040564721E-2,7.0826862394317056E-2,2.297411529479361E-3,0.30329739254331678,0.44187777694102648,5.82,0.92943366308294706,6.5956612368327054E-3,1.2422331306021871E-2,4.7695517138984503E-3,1.7003756612370198E-2,4.2947762708267699E-5,4.2436297578424059E-4,7.3609359078320702E-4,5.9550065351978388E-3,1.595991880753014E-2,2.4039255813731792E-5,6.030221955189776E-5,1.1310802432959094E-2,7.5304774449451647E-2,0.92943366308294706,92.943366308294699,485,73.159788011658193,0.73159788011658189,153.0077608710863,null,8.2589640067505608E-3,null,0.30329739254331678,7.0826862394317056E-2,0.13805224838744323,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR103, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.943366308294699},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ103, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.30329739254331678},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA103, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0826862394317056E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB103, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13805224838744323},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S103, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":153.0077608710863},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P103, IF(MODE_ILIM=4,#REF!,#REF!))","v":18.65180073100548}]
[null,null,null,null,null,null,null,98,{"$f":"IF(PLOT_TYPE=1, H104/100*Iout, min_I*EXP(H104*rr/100))","v":0.49},0.95211891402714932,0.96268452521610937,1.7392637211306794E-2,18.650370166253772,18.650370166253772,1,18.650370166253772,5.3035189218862553E-6,0.18835551815526461,153038.85850115248,{"$f":"IF(1/S104-OnTime-Q104>Tsleep, OnTime+Q104+Tsleep, 1/S104)","v":6.5342881526554863E-6},0,6.600000000000001E-4,0.56180158926657497,3.7874523084293933E-2,9.9959372734731974E-2,0.13867425119954663,0.27481089080029097,3.7760512851224727E-4,3.7760512851224727E-4,0.22567840340641776,1.5279222529220949E-4,1.5279222529220949E-4,0.24382157787382344,{"$f":"RdsonTop*AG104^2","v":4.0841436781937211E-2},6.1445101688212722E-4,54.166666666666664,10.766196840029416,5.5502561552136398E-2,5.172713417338954E-2,0.10784414674240807,0.14981724663410631,0.50600774270184312,{"$f":"RdsonBot*AP104^2","v":7.7837326044961255E-2},1.6834274435126775E-3,4.1820118656888414E-4,2.6853196397986466E-3,4.7869482698802077E-3,8.3831108074377561E-2,4.3257924040564735E-2,7.0832465565302385E-2,2.2978784603948045E-3,0.30677869873418107,0.44598334728753219,5.88,0.92949975951505437,6.6350316760943667E-3,1.2495157743086705E-2,4.7221780939308393E-3,1.7047807561594311E-2,6.6108486793314329E-5,4.2449046928807733E-4,7.5671212001099635E-4,5.9871360711902365E-3,1.5801396754797459E-2,2.4153118480421553E-5,5.9691135398602901E-5,1.1197067977688255E-2,7.5216931208353599E-2,0.92949975951505437,92.949975951505436,490,72.614496083320674,0.72614496083320679,153.03885850115248,null,8.176931764382403E-3,null,0.30677869873418107,7.0832465565302385E-2,0.13867425119954663,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR104, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.949975951505436},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ104, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.30677869873418107},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA104, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0832465565302385E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB104, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13867425119954663},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S104, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":153.03885850115248},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P104, IF(MODE_ILIM=4,#REF!,#REF!))","v":18.650370166253772}]
[null,null,null,null,null,null,null,99,{"$f":"IF(PLOT_TYPE=1, H105/100*Iout, min_I*EXP(H105*rr/100))","v":0.495},0.95204588235294096,0.96768505857865317,2.2429156943646833E-2,18.648939601502054,18.648939601502054,1,18.648939601502054,5.3021913401278301E-6,0.18839379442331919,153069.95796894684,{"$f":"IF(1/S105-OnTime-Q105>Tsleep, OnTime+Q105+Tsleep, 1/S105)","v":6.5329605708970603E-6},0,6.6E-4,0.56616784234222406,3.8465523084293941E-2,9.9979685767144472E-2,0.1393025440874861,0.27481089080029097,3.7760512851224727E-4,3.7760512851224727E-4,0.22735962796511819,1.5507720128531087E-4,1.5507720128531087E-4,0.24574149439888912,{"$f":"RdsonTop*AG105^2","v":4.148716198167729E-2},6.1457588124532152E-4,54.166666666666664,10.710757358286576,5.6861174913609223E-2,5.1737645793504025E-2,0.10921339658835857,0.15186583279074292,0.50999218343713837,{"$f":"RdsonBot*AP105^2","v":7.9067976258761843E-2},1.6837695376584153E-3,5.6752937945780675E-4,2.713372002794031E-3,4.964670919910253E-3,8.5279745965759796E-2,4.3257924040564728E-2,7.0838069067409568E-2,2.2983454189037366E-3,0.31028199324281602,0.45011721966009965,5.9399999999999995,0.92956041271430045,6.6747502019459202E-3,1.2568638772188539E-2,4.675734328287935E-3,1.709098484959683E-2,8.8813610134055507E-5,4.2462006713209552E-4,7.7692955375462298E-4,6.0195332514322774E-3,1.564598618935234E-2,2.426828741234886E-5,5.9092050354020381E-5,1.1085566450872957E-2,7.513491761246395E-2,0.92956041271430045,92.956041271430053,495,71.912167665597565,0.71912167665597559,153.06995796894682,null,8.0965096593730457E-3,null,0.31028199324281602,7.0838069067409568E-2,0.1393025440874861,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR105, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.956041271430053},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ105, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.31028199324281602},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA105, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0838069067409568E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB105, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1393025440874861},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S105, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":153.06995796894682},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P105, IF(MODE_ILIM=4,#REF!,#REF!))","v":18.648939601502054}]
[null,null,null,null,null,null,null,100,{"$f":"IF(PLOT_TYPE=1, H106/100*Iout, min_I*EXP(H106*rr/100))","v":0.5},0.95197285067873316,0.97268559194119697,2.7465676675986872E-2,18.647509036750353,18.647509036750353,1,18.647509036750353,5.3008642193050981E-6,0.18843207295339343,153101.05927463216,{"$f":"IF(1/S106-OnTime-Q106>Tsleep, OnTime+Q106+Tsleep, 1/S106)","v":6.5316334500743291E-6},0,6.6E-4,0.57054449931836992,3.9062523084293928E-2,0.1,0.13993713066782382,0.27481089080029097,3.7760512851224727E-4,3.7760512851224727E-4,0.22904571625256206,1.5738582040094752E-4,1.5738582040094752E-4,0.24766631111846321,{"$f":"RdsonTop*AG106^2","v":4.2139619342499837E-2},6.1470075298764818E-4,54.166666666666664,10.655885911921109,5.8220336454198295E-2,5.1748158034825666E-2,0.1105831952420116,0.15392244340996195,0.51398679364300981,{"$f":"RdsonBot*AP106^2","v":8.0311456907984261E-2},1.684111652020954E-3,7.1691822491512297E-4,2.7414661960593681E-3,5.1424960729954446E-3,8.6742390089490529E-2,4.3257924040564728E-2,7.0843672900667953E-2,2.2988124050086021E-3,0.31380731880512902,0.45427944042186608,6,0.9296157774674576,6.714808146750708E-3,1.2642758152901038E-2,4.6301932757901341E-3,1.7133313836623046E-2,1.1107641550584362E-4,4.2475170487508052E-4,7.9675758083683462E-4,6.052189627807735E-3,1.5493596291124295E-2,2.4384723632396747E-5,5.8504614186268665E-5,1.0976232677034117E-2,{"$f":"SUM(BD106:BO106)","v":7.5058567047067495E-2},0.9296157774674576,92.96157774674576,500,71.049894896969974,0.71049894896969978,153.10105927463218,null,8.017650694008888E-3,null,0.31380731880512902,7.0843672900667953E-2,0.13993713066782382,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR106, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.96157774674576},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ106, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.31380731880512902},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA106, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0843672900667953E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB106, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13993713066782382},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S106, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":153.10105927463218},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P106, IF(MODE_ILIM=4,#REF!,#REF!))","v":18.647509036750353}]
[null,null,null,null,null,null,null,null,{"$f":"Losses!$E$5/1000","v":0.5},0.95197285067873316,0.97268559194119697,2.7465676675986872E-2,18.647509036750353,18.647509036750353,1,18.647509036750353,{"$f":"IF(I107<Icrit, L*J107/(Vout+J107/2*(RdsonBot+Rdcr)), L*J107/(Vout+I107*(RdsonBot+Rdcr)))","v":5.3008642193050981E-6},{"$f":"OnTime*S107","v":0.18843207295339343},{"$f":"IF(I107<Icrit,I107/((OnTime+Q107)*J107/2),1/(OnTime+Q107))","v":153101.05927463216},{"$f":"IF(1/S107-OnTime-Q107>Tsleep, OnTime+Q107+Tsleep, 1/S107)","v":6.5316334500743291E-6},{"$f":"IF(1/S107-OnTime-Q107>Tsleep, 1/S107-OnTime-Q107-Tsleep, 0)","v":0},6.6E-4,{"$f":"IF(I107<Icrit,Iripple*SQRT((OnTime+OffTime)*S107/3), SQRT(I107^2+Iripple^2/12))","v":0.57054449931836992},3.9062523084293928E-2,0.1,0.13993713066782382,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q107)*S107)","v":0.27481089080029097},{"$f":"RCoutEsr*AA107^2","v":3.7760512851224727E-4},{"$f":"AB107","v":3.7760512851224727E-4},{"$f":"SQRT($R107)*SQRT($I107^2*(1-R107)+(Iripple^2)/12)","v":0.22904571625256206},{"$f":"RCinEsr*AD107^2","v":1.5738582040094752E-4},{"$f":"AE107","v":1.5738582040094752E-4},{"$f":"IF(I107<Icrit,Iripple*SQRT((OnTime)*S107/3), SQRT(OnTime*S107*(I107^2+Iripple^2/12)))","v":0.24766631111846321},{"$f":"RdsonTop*AG107^2","v":4.2139619342499837E-2},{"$f":"QgTop*S107*Vdd","v":6.1470075298764818E-4},54.166666666666664,{"$f":"IF(I107<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I107+Iripple/2)*1000000000)","v":10.655885911921109},5.8220336454198295E-2,{"$f":"IF(I107<Icrit, Csw*(Vin)^2*S107/2, Csw*Vin^2*S107/2)","v":5.1748158034825666E-2},0.1105831952420116,0.15392244340996195,{"$f":"IF(I107<Icrit,Iripple*SQRT((OffTime)*S107/3), SQRT(OffTime*S107*(I107^2+Iripple^2/12)))","v":0.51398679364300981},{"$f":"RdsonBot*AP107^2","v":8.0311456907984261E-2},{"$f":"QgBot*S107*Vdd","v":1.684111652020954E-3},7.1691822491512297E-4,{"$f":"IF(I107<Icrit, dead1*S107*(I107+Iripple/2)*((I107+Iripple/2)*BDserR+VSD), dead1*S107*(I107+Iripple/2)*((I107+Iripple/2)*BDserR+VSD)+dead2*S107*(I107-Iripple/2)*((I107-Iripple/2)*BDserR+VSD))","v":2.7414661960593681E-3},5.1424960729954446E-3,8.6742390089490529E-2,4.3257924040564728E-2,7.0843672900667953E-2,{"$f":"AI107+AR107","v":2.2988124050086021E-3},{"$f":"AO107+AV107+AX107+AY107","v":0.31380731880512902},0.45427944042186608,{"$f":"Vout*I107","v":6},{"$f":"BB107/(BB107+BA107)","v":0.9296157774674576},6.714808146750708E-3,1.2642758152901038E-2,{"$f":"Vin*S107*(QgBot+QgTop)/($BB107+$BA107)","v":4.6301932757901341E-3},1.7133313836623046E-2,{"$f":"AS107/(BA107+BB107)","v":1.1107641550584362E-4},{"$f":"AT107/($BB107+$BA107)","v":4.2475170487508052E-4},7.9675758083683462E-4,{"$f":"X107/($BB107+$BA107)","v":6.052189627807735E-3},{"$f":"Y107/($BB107+$BA107)","v":1.5493596291124295E-2},{"$f":"(AF107)/($BB107+$BA107)","v":2.4384723632396747E-5},{"$f":"(AC107)/($BB107+$BA107)","v":5.8504614186268665E-5},1.0976232677034117E-2,{"$f":"SUM(BD107:BO107)","v":7.5058567047067495E-2},{"$f":"BC107","v":0.9296157774674576},{"$f":"100*BQ107","v":92.96157774674576},{"$f":"I107*1000","v":500},72.049894896970002,{"$f":"BT107/100","v":0.72049894896970001},{"$f":"S107/1000","v":153.10105927463218},null,{"$f":"AM107/($BB107+$BA107)","v":8.017650694008888E-3},null,0.31380731880512902,7.0843672900667953E-2,0.13993713066782382,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR107, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.96157774674576},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ107, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.31380731880512902},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA107, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0843672900667953E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB107, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13993713066782382},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S107, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":153.10105927463218},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P107, IF(MODE_ILIM=4,#REF!,#REF!))","v":18.647509036750353}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BD107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":6.714808146750708E-3},{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BE107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":1.2642758152901038E-2},null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BG107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":1.7133313836623046E-2},null,null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BJ107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":7.9675758083683462E-4},{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BK107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":6.052189627807735E-3},{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BL107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":1.5493596291124295E-2},null,null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BO107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":1.0976232677034117E-2}]
[null,null,null,null,null,null,null,1.0000000000000001E-5,"A","min_I",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Load (A)","High-side MOSFET Rdson %","Low-side MOSFET Rdson %","Gate Drive (Qg) Loss from Vin %","High-side MOSFET Switching Loss %","Reverse Recovery & Leakage Loss %","Deadtime Loss %",null,"Inductor Cu Loss %","Inductor Core Loss %","Cin ESR %","Cout ESR %","Quiescent Current Loss %","Total Loss %","Overall Eff %"]
[null,null,null,null,null,null,null,{"$f":"Iout","v":0.5},"A","max_I",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"I107","v":0.5},{"$f":"BD107","v":6.714808146750708E-3},{"$f":"BE107","v":1.2642758152901038E-2},4.6301932757901341E-3,1.7133313836623046E-2,1.1107641550584362E-4,4.2475170487508052E-4,null,6.052189627807735E-3,1.5493596291124295E-2,2.4384723632396747E-5,5.8504614186268665E-5,1.0976232677034117E-2,7.5058567047067495E-2,0.9296157774674576]
[null,null,null,null,null,null,null,{"$f":"LOG(max_I/min_I,EXP(1))","v":10.819778284410283},null,"rr",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10mA",{"$f":"BD70","v":6.4492430041256828E-3},{"$f":"BE70","v":1.2206722862381881E-2},4.8470259917748016E-3,1.551067401831965E-2,0,3.4771775521972708E-4,null,5.879461913588506E-3,1.6219163964884341E-2,1.5125152352814768E-5,6.1303895453239396E-5,1.4924277562576367E-2,7.7081582706089738E-2,0.92765392307285977]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"50ma",{"$f":"BD85","v":6.4861896777546118E-3},{"$f":"BE85","v":1.2250045689331046E-2},4.8528738994330876E-3,1.6191426773119216E-2,0,3.8418783959588096E-4,null,5.8865554489665748E-3,1.6238732288496014E-2,1.9018566484108171E-5,6.137785823377988E-5,1.2955693542713847E-2,7.5983767806335104E-2,0.92877313194241873]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"100mA",{"$f":"BD91","v":6.500154652178302E-3},{"$f":"BE91","v":1.2265066090363212E-2},4.8542594263357251E-3,1.6460940824851025E-2,0,3.9887854402451692E-4,null,5.8882360986408549E-3,1.6243368551649911E-2,2.0733387634131024E-5,6.1395382009499504E-5,1.2360907468449889E-2,7.5726375432620632E-2,0.92903830268194743]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"500mA",{"$f":"BD106","v":6.714808146750708E-3},{"$f":"BE106","v":1.2642758152901038E-2},4.6301932757901341E-3,1.7133313836623046E-2,1.1107641550584362E-4,4.2475170487508052E-4,null,6.052189627807735E-3,1.5493596291124295E-2,2.4384723632396747E-5,5.8504614186268665E-5,1.0976232677034117E-2,7.5058567047067495E-2,0.9296157774674576]

{"sheet":"Schematic Mgmt","index":10,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
[]
[{"$f":"'Variable Mgmt'!K27","v":"SCH_COT3_LM5164"}]

{"sheet":"Efficiency Plots","index":11,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
[]
[{"$f":"IF(PLOT_TYPE=1, \"EFF_LINEAR\", \"EFF_LOG\")","v":"EFF_LINEAR"}]