{"text_format":"1","workbook":"xlsx","n_sheets":13,"sheets":["Instructions","Design Converter","Fsw & Ripple","Losses","Variable Mgmt","Standard Value Calculator","Efficiency","Design EMI Filter","EVM","BOM & Schematic","Schematic Mgmt","sch_frank","Efficiency Plots"],"not_rendered":{"charts":6,"images":28,"macros":1,"external_links":0,"defined_names":209,"comments":4,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Instructions","index":0,"n_rows":74,"n_cols":3,"rows_kept":74,"cut":false,"hidden":true,"merged":[[65,1,66,15],[69,1,70,15],[73,1,74,15],[77,1,78,15],[20,2,21,15],[50,1,52,15],[54,1,55,15],[56,1,57,15],[60,1,62,15],[24,1,26,15],[38,1,39,15],[41,1,43,15],[46,1,47,15],[28,1,28,15],[29,1,31,15],[33,1,35,15],[0,0,0,16],[7,1,9,15],[16,2,17,15],[11,1,14,15],[18,2,19,15]]}
["                         LM5164 Low IQ DC/DC Converter Design Tool  "]
[]
[]
[null,"Design Regulator tab"]
[null,"Start with Step 1, and then work down towards the bottom of the worksheet."]
[]
[null,"Step 1. Operating Specifications"]
[null,"First, enter the values in the yellow shaded cells to define the power supply parameters.  If a particular specification is not known, enter an estimate. It can be changed later, if necessary, to optimize component values.  Cells  with a red mark in the upper right corner have a comment to provide additional information.  Hold the cursor over the cell to read the comment.  A red font indicates an erroneous entry and requires an adjustment to the entry.  Consult the entry's comments for the entry specific requirements."]
[]
[]
[]
[null,"Second, select a desired mode of operation. PFM mode requires the fewest external components and the lowest inductance.  As a result, it can provide the smallest solution size. At light loads, a PFM converter has a relatively longer sleep time interval and thus operates at lower input quiescent current levels.  COT mode offers nearly constant switching frequency, relatively higher conversion efficiencies at medium to heavy loads, and enables the lowest output voltage ripple.  Options COT1, COT2, and COT3 enable you to select a ripple generation method (a requirement for the stable operation in COT mode):"]
[]
[]
[]
[]
[null,"-COT1: ","Type 1 ripple generation method requires a single resistor in series with the output capacitor.  It is the simplest, the most compact, and the most economical method that works with fixed and adjustable device options, however, the output voltage ripple is the highest."]
[]
[null,"-COT2: ","Type 2 ripple generation method requires a feedforward capacitor in addition to the series resistor.  The feedforward capacitor reduces the required minimum value of the series resistor and ultimately the output voltage ripple by the VOUT / 1.223V factor.  It only works with an adjustable device option (i.e. external feedback resistor network)."]
[]
[null,"-COT3:","Type 3 ripple generation method three external components to generate and inject required voltage ripple into the FB node.  In return, it provides the lowest output voltage ripple. It also only works with an adjustable device option (i.e. external feedback resistor network)."]
[]
[]
[null,"Step 2. Filter Inductor"]
[null,"First, select an inductor current limit level.  In PFM Mode, 1.25A, 0.75A, 0.5A, and 1.25A - MOD options are available.  For the 500mA max load, select either 1.25A or 1.25A - MOD option.  The 1.25A - MOD option enables higher efficiency at the expense of slightly worse transient operation.  For the 300mA and 200mA max loads, select 0.75A and 0.5A options respectively. In COT Mode, 0.75A and 0.5A options are available.   For the 500mA and 300mA max loads, select 0.75A and 0.5A options respectively."]
[]
[]
[]
[null,"Second, select the filter inductance value based on the suggested value. Enter the inductor RDC for accurate efficiency estimates."]
[null,"In PFM mode, selected inductance defines the switching frequency.  You may select lower or higher inductance to increase or decrease the switching frequency.  Watch the minimum output capacitance.  At very low switching frequencies, the required minimum capacitance may become excessive."]
[]
[]
[]
[null,"In COT mode, the suggested inductance is  derived based on the target inductor (peak-to-peak) ripple current of 40% of the DC full load output current at nominal input voltage. It may be acceptable to use higher ripple current with the proviso that peak inductor current remains below the ILIM setting.  Pk-to-Pk Ripple Current value will turn red if this is violated.  If this happens, increase the selected inductance or decrease the Input Voltage (max) or both."]
[]
[]
[]
[null,"Step 3. Output Capacitors and Ripple Generation"]
[null,"First, select the output capacitance based on the minimum recommended value.  Make sure that the nominal capacitance is appropriately derated for applied voltage, especially with ceramics.  For PFM and COT3 modes, ensure that the capacitor ESR does not exceed the maximum allowable value.  "]
[]
[]
[null,"Second, for COT modes, select the values for the ripple generation components based on the minimum recommended values.  Ensure that the output voltage ripple meets any of your minimum ripple requirements by reviewing the VOUT Ripple vs. IOUT plot in the fSW&Ripple tab.  For accurate output voltage ripple estimates in COT3 mode, ensure that the Output Capacitor ESR is set to the levels of a typical ceramic capacitor ESR (e.g. 10 mW)."]
[]
[]
[]
[null,"Step 4. Input Capacitors"]
[null,"Select the input capacitance based on the minimum recommended value.  Make sure that the nominal capacitance is appropriately derated for applied voltage, especially with ceramics.  "]
[]
[]
[null,"Step 5. Feedback, Soft-Start, UVLO"]
[null,"First, review the feedback resistor network. With an adjustable device option, an external feedback resistor network is required. The resistor values are automatically calculated based on the selected VOUT in Step 1.  For lowering the leakage current through the resistors, adjust the upper FB resistor (R1) until the lower FB resistor (R2) reaches its upper end of the range (100kW).  Keeping the upper FB resistor below 1MW is recommended."]
[]
[]
[]
[null,"Second, select one out of three soft-start configurations.  If the external soft-start option is selected, enter a desired soft start time.  "]
[]
[null,"Third, select one out of the two UVLO options.  If the external UVLO option is selected, define desired UVLO thresholds and hysteresis.  Keeping the upper UVLO resistor at 1MW or higher is recommended for the minimum leakage current."]
[]
[]
[null,"Step 6. Efficiency and Thermals"]
[null,"Enter the LM5166's junction-to-ambient thermal impedance (dependent on your PCB design, air flow, etc.) and ambient temperature. Device power dissipation and junction temperature are derived at the maximum load.  Ensure that the junction temperature is within the recommended range."]
[]
[]
[]
[null,"BOM & Schematic tab"]
[null,"This tab summarizes the converter schematic and BOM.  It also helps you estimate the total solution size. Select a package size for each external component (i.e. inductor, capacitors, and resistors) for accurate solution size estimates."]
[]
[]
[null,"Design EMI Filter tab"]
[null,"In case an EMI filter is needed, a simple EMI filter design aid is given in this tab.  It is based on the guidelines documented in TI's literature number SNVA489C (aka AN-2162).  Suggest reviewing the note before using the design aid."]
[]
[]
[null,"fSW & Ripple tab"]
[null,"In this tab, the switching/burst frequency (COT/PFM mode) and the output voltage ripple as a function of the load current are plotted."]

{"sheet":"Design Converter","index":1,"n_rows":58,"n_cols":17,"rows_kept":58,"cut":false,"hidden":false,"merged":[[2,14,2,15],[0,0,0,16]]}
["                          LM5168/9 Low IQ DC/DC Converter Design Tool  "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"http://www.ti.com/ww/en/analog/power_management/widevin"]
["About",null,"xx",null,null,"= Input Box",null,null,null,null,null,null,null,null,"Terms Of Use",null,"                "]
[]
["Step 1: Operating Specifications"]
[null,null,null,"Input Voltage - Min, VIN(min) ",18,"V"]
[null,null,null,"Input Voltage - Nom, VIN(nom)",24,"V"]
[null,null,null,"Input Voltage - Max, VIN(max)",80,"V"]
[null,null,null,"Output Voltage, VOUT ",12,"V"]
[null,null,null,"Full Load Current, IOUT",0.25,{"$f":"IF('Variable Mgmt'!B84>'Variable Mgmt'!B86,\"CURRENT LIMIT\",\"A\")","v":"A"}]
[null,null,null,"Mode of Operation",null,null,{"$f":"MODE","v":3}]
[null,null,null,"Switching Frequency at VIN(nom)",500,"kHz"]
[null,null,null,"Timing Resistance, RT",{"$f":"'Standard Value Calculator'!J4/1000","v":60.4},"kΩ"]
[]
["Step 2: Buck Inductor"]
[null,null,null,"Recommended Buck Inductance ",{"$f":"Lopt*1000000","v":120},"µH"]
[null,null,null,"Inductance, LF ",100,"µH"]
[null,null,null,"Inductor DCR ",170,"mΩ"]
[null,null,null,{"$f":"CHOOSE(MODE, \"Pk-to-Pk Ripple Current\",\"Pk-to-Pk Ripple Current\",\"Pk-to-Pk Ripple Current\", \"Resulting PFM Switching Frequency\")","v":"Pk-to-Pk Ripple Current"},{"$f":"Iripple_Vinnom*1000","v":116.61584798345396},"mApk-pk"]
[null,null,null,{"$f":"CHOOSE(MODE, 'Variable Mgmt'!H88,'Variable Mgmt'!H88,'Variable Mgmt'!H88, 'Variable Mgmt'!H89)","v":"% Ripple Current at Nom VIN"},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), 'Variable Mgmt'!B96*100, Ilim/2*1000)","v":46.646339193381586},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), \"%\", \"mA\")","v":"%"}]
[]
[{"$f":"IF(MODE=4, \"Step 3: Output Capacitors\", \"Step 3: Output Capacitors, Ripple Generation\")","v":"Step 3: Output Capacitors, Ripple Generation"}]
[null,null,null,"Minimum Output Capacitance ",{"$f":"'Variable Mgmt'!B116","v":2.2000000000000002},"µF"]
[null,null,null,"Output Capacitance, COUT ",33,"µF"]
[null,null,null,{"$f":"IF(OR(MODE=1,MODE=2),\"Recommended Series Resistance\",IF(MODE=3,\"Maximum Allowable ESR\",\"*Higher Cout Improves Light-Load Eff\"))","v":"Maximum Allowable ESR"},{"$f":"'Variable Mgmt'!B272","v":0.51400000000000001},"Ω"]
[null,null,null,{"$f":"IF(OR(MODE=1,MODE=2),\"Total ESR & Series Resistance, Rser\",IF(MODE=3,\"Output Capacitor ESR\",\"*PFM Hysteresis Sets Output Ripple\"))","v":"Output Capacitor ESR"},5.0000000000000001E-3,"Ω"]
[null,null,null,{"$f":"CHOOSE(MODE, \"Resulting Output Voltage Ripple\",\"Resulting Output Voltage Ripple\", \"Output Voltage Ripple\",\"Output Voltage Ripple\")","v":"Output Voltage Ripple"},{"$f":"CHOOSE(MODE, Vripple2*1000,Vripple2*1000,Vripple2*1000, PFM_Ripple)","v":1.0585231688839198},"mVpk-pk"]
[null,null,null,{"$f":"IF(MODE=1,\"\",IF(MODE=2,\"Minimum Feedforward Capacitance\", IF(MODE=3,\"Minimum Coupling Capacitance\",\"\")))","v":"Minimum Coupling Capacitance"},{"$f":"'Variable Mgmt'!B140","v":">47"},"pF"]
[null,null,null,{"$f":"IF(MODE=1,\"\",IF(MODE=2,\"Feedforward Capacitance, Cff\", IF(MODE=3,\"Coupling Capacitance, Cb\",\"\")))","v":"Coupling Capacitance, Cb"},56,"pF"]
[null,null,null,{"$f":"IF(MODE=3,\"Minimum Ripple Generation Capacitance\",\"\")","v":"Minimum Ripple Generation Capacitance"},{"$f":"'Variable Mgmt'!B144","v":">445"},"pF"]
[null,null,null,{"$f":"IF(MODE=3,\"Ripple Generation Capacitance, Ca\",\"\")","v":"Ripple Generation Capacitance, Ca"},3300,"pF"]
[null,null,null,{"$f":"IF(MODE=3,\"Ripple Generation Resistance, Ra\",\"\")","v":"Ripple Generation Resistance, Ra"},{"$f":"Ra","v":182},"kΩ"]
[null,null,null,{"$f":"IF(MODE=3,\"Amplitude of Injected Ripple\",\"\")","v":"Amplitude of Injected Ripple"},20,"mVpk-pk"]
[]
["Step 4: Input Capacitors"]
[null,null,null,"Minimum Input Capacitance ",{"$f":"'Variable Mgmt'!B157","v":2.2000000000000002},"µF"]
[null,null,null,"Input Capacitance, CIN ",2.2000000000000002,"µF"]
[null,null,null,"Maximum Allowable ESR",{"$f":"'Variable Mgmt'!B159","v":3.7079435891033978},"Ω"]
[null,null,null,"Input Capacitor ESR ",3,"mΩ"]
[null,null,null,"Resulting Input Voltage Ripple ",{"$f":"CHOOSE(MODE, Vinripple2*1000,Vinripple2*1000,Vinripple2*1000, 'Variable Mgmt'!B165*1000)","v":57.736533537073868},"mVpk-pk"]
[]
["Step 5: Feedback, PGOOD, UVLO"]
[null,null,null,"Upper Feedback Resistor, RFB1 ",453,"kΩ"]
[null,null,null,"Lower Feedback Resistor, RFB2",{"$f":"IF(Vout=Vref,\"OPEN\",Rfb2_u/1000)","v":49.9},{"$f":"IF(Vout=Vref,\"\",\"kΩ\")","v":"kΩ"}]
[null,null,null,"Acutal Output Voltage Setpoint",{"$f":"'Variable Mgmt'!B201","v":12.0937875751503},"V"]
[null,null,null,"PGOOD Pull-up Resistance",20,{"$f":"\"kΩ\"","v":"kΩ"},null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,"BST Capacitance, CBST ",2.2000000000000002,"nF"]
[null,null,null,{"$f":"\"Required Input Voltage UVLO Turn-on\"","v":"Required Input Voltage UVLO Turn-on"},6,"V"]
[null,null,null,"Upper UVLO Resistor, RUV1",1,"MΩ"]
[null,null,null,"Lower UVLO Resistor, RUV2",{"$f":"'Variable Mgmt'!F276","v":332},{"$f":"'Variable Mgmt'!G276","v":"kΩ"}]
[null,null,null,"Actual UVLO Turn-on Threshold",{"$f":"'Variable Mgmt'!B186","v":6.0180722891566267},"V"]
[null,null,null,"Actual UVLO Turn-off Threshold",{"$f":"'Variable Mgmt'!B187","v":5.6168674698795176},"V"]
[]
["Step 6: Efficiency & Thermals"]
[null,null,null,"Estimated Thermal Impedance, JJA",33,"°C/W"]
[null,null,null,"Ambient Temp, TA",25,"°C"]
[null,null,null,"IC Power Dissipation at Full Load, PD",{"$f":"'Variable Mgmt'!B26","v":0.20503948329149221},"W"]
[null,null,null,"IC Junction Temp at Full Load, TJ",{"$f":"E56+E55*'Variable Mgmt'!B26","v":31.766302948619241},"°C"]

{"sheet":"Fsw & Ripple","index":2,"n_rows":1,"n_cols":1,"rows_kept":1,"cut":false,"hidden":true,"merged":[[0,0,0,16]]}
["                         LM5164 Low IQ DC/DC Converter Design Tool  "]

{"sheet":"Losses","index":3,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":true,"merged":[[0,0,0,16]]}
["                         LM5166 Low IQ DC/DC Converter Design Tool  "]
[]
[]
[]
[null,null,null,"Load Current",500,"mA"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"Inductor Core Loss Constant",0]

{"sheet":"Variable Mgmt","index":4,"n_rows":320,"n_cols":21,"rows_kept":320,"cut":false,"hidden":true,"merged":[[4,4,4,7],[0,0,0,8]]}
["EXCEL Variables Names/Calculations",null,null,null,null,null,null,null,null,null,null,"LM5166"]
[null,"Input from user ="]
[null,"Output ="]
[null,"Constant"]
["Variable Name","Value","STD Units",null,"Notes",null,null,null,"Iteration"]
["Step 1: Operational Specs"]
["VIN_min",{"$f":"'Design Converter'!E6","v":18},"V","Minimum input voltage",null,null,null,null,1]
["VIN_nom",{"$f":"'Design Converter'!E7","v":24},"V","Nominal input voltage"]
["VIN_max",{"$f":"'Design Converter'!E8","v":80},"V","Maximum input voltage"]
[]
["Vout",{"$f":"'Design Converter'!E9","v":12},"V","Output Voltage",null,null,null,null,1]
["Iout",{"$f":"'Design Converter'!E10","v":0.25},"A","Maximum Output Current",null,null,null,null,1]
["Rout",{"$f":"Vout/Iout","v":48},"W","Load resistance"]
["Pout",{"$f":"Vout*Iout","v":3},"W","Output power"]
[]
["Efficiency",0.9,null,"Estimate of efficiency"]
["Pin",{"$f":"Pout/Efficiency","v":3.333333333333333},"W","Calculate input power assuming 90% efficiency"]
["Iin_Vinmin",{"$f":"Pin/VIN_min","v":0.18518518518518517},"A"]
["Iin_Vinnom",{"$f":"Pin/VIN_nom","v":0.13888888888888887},"A","Input currents at min, nom, max Vin"]
["Iin_Vinmax",{"$f":"Pin/VIN_max","v":4.1666666666666664E-2},"A"]
[]
["Fsw",{"$f":"'Design Converter'!E12*1000","v":500000},"Hz","Nominal Switching Frequency",null,null,null,null,1]
["Vref",1.2,"V","Reference Voltage"]
["Rt",{"$f":"Vout*2500000000/Fsw","v":60000},"W","Frequency Set Resistor"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"B34&\"_\"&F35&\"_\"&F39&\"_\"&I41&\"_\"&I36","v":"COT3_VOUTadj_UVLOadj_SSAdj_RsetGND"},null,null,null,null,null,"Vout<5V",100,1]
["Internal PD at Full Load",{"$f":" IF(OR(MODE=1,MODE=2,MODE=3), Efficiency!AZ106,#REF!)","v":0.20503948329149221},"W",null,null,null,null,null,null,null,null,null,null,null,null,null,"Vout<=8V",47,2]
[null,null,null,null,null,null,null,null,null,null,{"$f":"\"SCH_\"&B34&\"_\"&B41","v":"SCH_COT3_LM5168"},null,null,null,null,null,"Vout<=12V",22,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vout<=20V",22,4]
["Step 2: Circuit Configuration for COT / PFM, Fixed / Adj Vout, ILIM, UVLO, SS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vout>20V",10,5]
[null,"COT Type I",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cout Capacitance",{"$f":"CHOOSE(S30,\"100\", \"47\",\"22\",\"22\",\"10\")","v":"22"},{"$f":"IF(Vout<5, 1, IF(Vout<=8, 2, IF(Vout<=12, 3, IF(Vout<=20, 4, 5))))","v":3}]
[null,"COT Type II",2]
["COT/PFM ","COT Type III",3]
[null,null,null,null,"VOUT Fixed/Adjustable","Fixed",1,null,"ILIM shorted",1,{"$f":"B34&\", \"&F35&\", \"&I36&\", \"&F39&\", \"&I41","v":"COT3, VOUTadj, RsetGND, UVLOadj, SSAdj"},null,null,null,null,null,"Vout<=5V","6.3V",1]
["MODE",{"$f":"CHOOSE(C34, \"COT1\", \"COT2\",\"COT3\")","v":"COT3"},3,null,null,"Adjustable",2,null,"ILIM resistor needed",2,{"$f":"C34&\", \"&G35&\", \"&J36&\", \"&G39&\", \"&J41","v":"3, 2, 1, 1, 1"},null,null,null,null,null,"Vout<=8V","10V",2]
[null,{"$f":"IF(MODE=4, \"PFM\", \"COT\")","v":"COT"},null,null,"MODE_VOUT",{"$f":"CHOOSE(G35, \"VOUTfixed\", \"VOUTadj\")","v":"VOUTadj"},{"$f":"IF(AND(OR(MODE=1,MODE=4),OR(Vout=3.3,Vout=5)),1,2)","v":2},null,null,null,{"$f":"C34&G35&J36&G39&J41","v":"32111"},null,null,null,null,null,"Vout<=12V","16V",3]
[null,null,null,null,null,null,null,"MODE_RSET",{"$f":"CHOOSE(J36, \"RsetGND\",\"Rset\")","v":"RsetGND"},1,null,null,null,null,null,null,"Vout<=20V","25V",4]
[null,null,null,null,"UVLO","Adjustable",1,null,null,null,null,null,null,null,null,null,"Vout>20V","50V",5]
[null,null,null,null,null,"Internal",2,"Soft Start","Adjustable",1,null,"Iout Linear Axis",1,null,null,null,"Cout Voltage Rating",{"$f":"CHOOSE(S38,\"6.3V\", \"10V\",\"16V\",\"25V\",\"50V\")","v":"16V"},{"$f":"IF(Vout<=5, 1, IF(Vout<=8, 2, IF(Vout<=12, 3, IF(Vout<=20, 4, 5))))","v":3}]
[null,"LM5168",1,null,"MODE_UVLO",{"$f":"CHOOSE(G39, \"UVLOadj\", \"UVLOint\")","v":"UVLOadj"},1,null,"3ms Fixed",2,null,"Iout Log Axis",2]
[null,"LM5169",2,null,null,null,null,null,null,null,null,"PLOT_TYPE",1]
["VARIANT",{"$f":"CHOOSE(VARIANT, \"LM5168\", \"LM5169\")","v":"LM5168"},1,null,"ESR","NO",1,"MODE_SS",{"$f":"CHOOSE(J41, \"SSAdj\", \"SSfix\")","v":"SSAdj"},1,null,null,null,null,null,null,null,"0402",1,"1.0 x 0.5",0.5]
[null,null,null,null,null,"YES",2,null,null,null,null,null,null,null,null,null,null,"0603",2,"1.6 x 0.8",1.3]
[null,null,null,null,"MODE_ESR",null,2,null,null,null,null,null,null,null,null,null,null,"0805",3,"2.0 x 1.25",2.5]
[null,null,null,null,null,{"$f":"CHOOSE(G44, \"\", \"_ESR\")","v":"_ESR"},{"$f":"IF(MODE=2, 1, MODE_ESR)","v":2},null,null,null,null,null,null,null,null,null,null,"1206",4,"3.2 x 1.6",5.0999999999999996]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1210",5,"3.2 x 2.5",8]
["Step 3: Buck Inductor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Component Size",{"$f":"CHOOSE(S46,\"0402\", \"0603\",\"0805\",\"1206\",\"1210\")","v":"1210"},5,{"$f":"CHOOSE(S46,T41,T42,T43,T44,T45)","v":"3.2 x 2.5"}]
["Don1",{"$f":"Vout/VIN_nom","v":0.5},{"$f":"(Vout-VIN_nom)/Vout","v":-1},null,"Ideal Duty Cycle at VIN(nom)",null,null,null,1]
["Doff1",{"$f":"1-47:47","v":0.5},null,null,"Ideal 1- Duty Cycle at VIN(nom)",null,null,null,1]
[]
["Don_Vinmin",{"$f":"Vout/VIN_min","v":0.66666666666666663},{"$f":"IF(VIN_min>Vout, \"BUCK\", \"BOOST\")","v":"BUCK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3mm x 3mm",1,"3.0 x 3.0",9]
["Don_Vinnom",{"$f":"Vout/VIN_nom","v":0.5},{"$f":"IF(VIN_nom>Vout, \"BUCK\", \"BOOST\")","v":"BUCK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4mm x 4mm",2,"4.0 x 4.0",16]
["Don_Vinmax",{"$f":"Vout/VIN_max","v":0.15},{"$f":"IF(VIN_max>Vout, \"BUCK\", \"BOOST\")","v":"BUCK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5mm x 5mm",3,"5.0 x 5.0",25]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6mm x 6mm",4,"6.0 x 6.0",36]
["Lf_Vinmin",{"$f":"(VIN_min-Vout)*Don_Vinmin/(Fsw*Iout*0.4)","v":8.0000000000000007E-5},"H","COT",null,null,null,null,null,null,null,null,null,null,null,null,null,"7mm x 7mm",5,"7.0 x 7.0",49]
["Lf_Vinnom",{"$f":"(VIN_nom-Vout)*Don_Vinnom/(Fsw*Iout*0.4)","v":1.2E-4},"H","COT",null,null,null,null,1,null,null,null,null,null,null,null,"Inductor Size","8mm x 8mm",6,"8.0 x 8.0",64]
["Lf_Vinmax",{"$f":"(VIN_max-Vout)*Don_Vinmax/(Fsw*Iout*0.7)","v":1.1657142857142857E-4},"H","COT",null,null,null,null,null,null,null,null,null,null,null,null,null,"10mm x 10mm",7,"10.0 x 10.0",100]
[]
["L_Vinmin_COT",{"$f":"(VIN_min-Vout)*Don_Vinmin/(Fsw*Iout*0.3)","v":1.0666666666666667E-4},"H","COT","Calculated Inductance for 30% ripple at VIN(min)"]
["L_Vinnom_COT",{"$f":"(VIN_nom-Vout)*Don_Vinnom/(Fsw*Iout*0.4)","v":1.2E-4},"H","COT","Calculated Inductance for 40% ripple at VIN(nom)",null,null,null,null,null,"Pk-to-Pk Ripple Current at VIN(nom), DIL"]
["L_Vinmax_COT",{"$f":"(VIN_max-Vout)*Don_Vinmax/(Fsw*Iout*0.7)","v":1.1657142857142857E-4},"H","COT","Calculated Inductance for 70% ripple at VIN(max)"]
[]
[]
["Lopt",{"$f":"B59","v":1.2E-4},"H"]
[]
["Lf",{"$f":"'Design Converter'!E17/1000000","v":1E-4},"H",null,"Chosen Inductance"]
["Rdcr",{"$f":"'Design Converter'!E18/1000","v":0.17},"W",null,"Chosen Inductor DCR"]
[]
["Don2",{"$f":"(Vout+Iout*Rdcr)/Vin","v":0.50177083333333339},null,null,"**Edit to add Rdson**"]
["Doff2",{"$f":"1-_Don2","v":0.49822916666666661}]
[]
["Rdson1",1.85,"W"]
["Rdson2",0.7,"W"]
[]
["Don_Vinmin_2",{"$f":"(Vout+Iout*(Rdcr+Rdson2))/(VIN_min+Iout*Rdson2)","v":0.67221458046767535},null,null,"Duty cycles adjusted for DCR and shunt voltage drops"]
["Don_Vinnom_2",{"$f":"(Vout+Iout*(Rdcr+Rdson2))/(VIN_nom+Iout*Rdson2)","v":0.50537745604963802},null,null,"need to include RDS(on) later"]
["Don_Vinmax_2",{"$f":"(Vout+Iout*(Rdcr+Rdson2))/(VIN_max+Iout*Rdson2)","v":0.15238540692235733}]
[]
["Iripple_Vinmin",{"$f":"(VIN_min-Vout-Rdson1*Iout)*Don_Vinmin_2/(Fsw*Lf)","v":7.4447764786795045E-2},"A","COT"]
["Iripple_Vinnom",{"$f":"(VIN_nom-Vout-Rdson1*Iout)*Don_Vinnom_2/(Fsw*Lf)","v":0.11661584798345397},"A","COT"]
["Iripple_Vinmax",{"$f":"(VIN_max-Vout)*Don_Vinmax_2/(Fsw*Lf)","v":0.20724415341440597},"A","COT"]
[]
["ILpk_Vinmin",{"$f":"Iout+Iripple_Vinmin/2","v":0.28722388239339752},"A","COT"]
["ILpk_Vinnom",{"$f":"Iout+Iripple_Vinnom/2","v":0.30830792399172696},"A","COT"]
["ILpk_Vinmax",{"$f":"Iout+Iripple_Vinmax/2","v":0.35362207670720297},"A","COT"]
[]
["ILIM_Typ",{"$f":"CHOOSE(VARIANT, 0.42, 0.84)","v":0.42},"A",null,"Isat_min",{"$f":"B86*1.2","v":0.504}]
[]
["Ripple current",{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), Iripple_Vinnom, Iripple)","v":0.11661584798345397},"A",null,null,null,null,"% Ripple Current at Nom VIN"]
[null,null,null,null,null,null,null,"Maximum Load Current"]
["Max inductor ripple current",{"$f":"MAX(B78:B80)","v":0.20724415341440597},"A"]
[null,null,null,null,null,"Ripple I","Iin"]
["% Ripple Current",{"$f":"B78/Iout","v":0.29779105914718018},null,"COT",null,{"$f":"B78","v":7.4447764786795045E-2},{"$f":"Iin_Vinmin","v":0.18518518518518517}]
[null,{"$f":"B79/Iout","v":0.46646339193381586},null,"COT",null,{"$f":"B79","v":0.11661584798345397},{"$f":"Iin_Vinnom","v":0.13888888888888887}]
[null,{"$f":"B80/Iout","v":0.82897661365762387},null,"COT",null,{"$f":"B80","v":0.20724415341440597},{"$f":"Iin_Vinmax","v":4.1666666666666664E-2}]
[]
[null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3), B93, Ilim/Iout)","v":0.46646339193381586}]
[]
["Iripple1",{"$f":"(Vin-Vout)*Don_Vinnom_2/(Fsw*Lf)","v":0.12129058945191312},"A","inductor ripple current with chosen inductance (pk-pk)",null,null,null,null,1]
["Temp",100]
["DCR at hot",{"$f":"Rdcr*(1+0.0039*(B99-25))","v":0.219725},"W"]
["Ipk based on line 100",{"$f":"'Design Converter'!E10+0.5*Iripple1","v":0.31064529472595659}]
[]
[]
["Step 4: Output Capacitor"]
["Icoutrms_VINmin",{"$f":"Iripple_Vinmin/SQRT(12)","v":2.1491218520111034E-2},"A","Output Cap RMS current"]
["Icoutrms_VINnom",{"$f":"Iripple_Vinnom/SQRT(12)","v":3.3664095612511817E-2},"A"]
["Icoutrms_VINmax",{"$f":"Iripple_Vinmax/SQRT(12)","v":5.9826233880891699E-2},"A",null,null,null,{"$f":"Vripple1","v":0.06}]
[]
["Output Ripple Spec (pk-pk)",{"$f":"Vout*0.005","v":0.06},"V","Vout capacitive ripple spec at Vin(nom) = Vripple1"]
[]
["Coutmin"]
["COT",{"$f":"Iripple_Vinnom/(Fsw*8*Vripple1)","v":4.858993665977249E-7},"F","COT","Min recommended Cout based on ripple spec above",null,null,null,1]
[null,{"$f":"Lf*B83^2/((1.05*Vout)^2-Vout^2)","v":6.4399577233122092E-7},"F","COT","Min recommended Cout based on 5% load-off transient spec"]
["CoutMinCOT",{"$f":"MAX(B112:B113, 0.0000022)","v":2.2000000000000001E-6},"F","COT","max of 2 results and 2.2uF"]
[]
["Reported Countmin",{"$f":"CoutMinCOT*1000000","v":2.2000000000000002},"µF"]
[]
["Cout",{"$f":"'Design Converter'!E24/1000000","v":3.3000000000000003E-5},"F","Chosen Output Capacitance",null,null,null,null,1]
["Resrmax",{"$f":"SQRT((Vripple1/Iripple_Vinnom)^2-(1/(Fsw*Cout*8))^2)","v":0.51445405236393082},"W","Max ESR before ripple exceeds Vripple1",null,null,null,null,1]
["Type1 ESR for sufficient (20mV) COT ripple at FB pin",{"$f":"0.02*Vout/Vref/Iripple_Vinnom","v":1.7150327632002214},"W","(a)"]
["Type2 ESR for sufficient (20mV) COT ripple at FB pin",{"$f":"0.02/Iripple_Vinnom","v":0.17150327632002213},"W","(b)"]
[]
["Type 1 Output Cap RC Time Constant",{"$f":"Cout*B130*1000000","v":0},"µs"]
["Type 2 Output Cap RC Time Constant",{"$f":"Cout*B131*1000000","v":0},"µs"]
["Ton @ Vin(min)",{"$f":"Vout/VIN_min/(Fsw)","v":1.3333333333333332E-6},"s"]
["Ton @ Vin(nom)",{"$f":"Vout/VIN_nom/(Fsw)","v":9.9999999999999995E-7},"s"]
["ESR so that RC > Ton/2",{"$f":"B125/2/Cout","v":2.0202020202020197E-2},"W","(c)"]
[]
[]
["Type1: Need ESR of…",{"$f":"IF(MODE=1, MAX(B120,B127), 0)","v":0},"W","Max of (a) and (c)"]
["Type2: Need ESR of…",{"$f":"IF(MODE=2, MAX(B121,B127), 0)","v":0},"W","Max of (b) and (c)"]
[]
["Reported Cout ESR max",{"$f":"IF(OR(CoutEsrMax>0.5, CoutEsrMax<0, (ISERROR(CoutEsrMax))), \"N/A\", CoutEsrMax*1000)","v":"N/A"},"mW"]
[]
["CoutEsr",{"$f":" 'Design Converter'!E26","v":5.0000000000000001E-3},"W","Chosen ESR",null,null,null,null,1]
[]
["Actual Output Ripple",{"$f":"Iripple_Vinnom*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2)","v":1.0585231688839199E-3},"Vp-p","Vripple2"]
[]
["Minimum Feedforward / Coupling Capacitance",{"$f":"MAX(1000000000000*0.00005/(3*Rfb1_),47)","v":47},"pF",null,null,null,null,{"$f":"0.00005/3/Rfb1_","v":3.6791758646063281E-11}]
["Recommended Cff / Cb",{"$f":"IF(OR(MODE=2,MODE=3), \">\"&ROUND(B139,0),\"\")","v":">47"},"pF"]
["Selected Cff / Cb",{"$f":"'Design Converter'!$E$29","v":56},"pF"]
[]
["Minimum Ripple Generation Capacitance",{"$f":"10/(Fsw*Rfb)","v":4.4495171358168876E-10},"F",{"$f":"1000000000000*B143","v":444.95171358168875},"pF",{"$f":"Rfb","v":44948.697554185725}]
["Recommended Ca",{"$f":"IF(MODE=3, \">\"&ROUND(D143,0),\"\")","v":">445"},"pF"]
["Selected Ca",{"$f":"'Design Converter'!E31","v":3300},"pF",{"$f":"B145/1000000000000","v":3.3000000000000002E-9},"F"]
[]
["Maximum Ripple Generation Resistance",{"$f":"(VIN_nom-Vout)*B126/((B149/1000)*Ca)","v":181818.18181818182},"W",{"$f":"B147/1000","v":181.81818181818181},"kW"]
["Recommended Ra",{"$f":"IF(MODE=3, \"<\"&ROUND(D147,0),\"\")","v":"<182"},"kW",null,null,null,null,null,null,null,null,"Lf_emi",{"$f":"'Design EMI Filter'!$E$9","v":22},"uH",{"$f":"M148/1000000","v":2.1999999999999999E-5},"H"]
["Ripple amplitude",{"$f":"'Design Converter'!E33","v":20},"mVp-p",null,null,null,null,null,null,null,null,"Cf_emi",{"$f":"'Design EMI Filter'!$E$11","v":4.7},"uF",{"$f":"M149/1000000","v":4.6999999999999999E-6},"F"]
[null,null,null,null,null,null,null,null,null,null,null,"Cd_emi",{"$f":"'Design EMI Filter'!$E$13","v":10},"uF",{"$f":"M150/1000000","v":1.0000000000000001E-5},"F"]
[null,null,null,null,null,null,null,null,null,null,null,"ESR_Cd",{"$f":"'Design EMI Filter'!$E$15","v":3.3},"Ω",{"$f":"M151","v":3.3},"Ω",{"$f":"ESR_Cd&ohm","v":"3.3Ω"}]
["Step 5: Input Capacitor",null,null,null,null,null,null,null,null,null,null,"Min Noise",{"$f":"'Design EMI Filter'!$E$8","v":50},"dB","noise limit"]
["Vinripple1",{"$f":"0.05*VIN_nom","v":1.2000000000000002},"Vp-p","Input voltage ripple spec (pk-pk) at Vin(nom)",null,null,null,null,null,null,null,"Duty Cycle",{"$f":"Vout/VIN_nom/Efficiency_COT_Full_Load","v":0.53590568060021437},null,"calculated duty cycle"]
[null,null,null,null,null,null,null,null,null,null,null,"Target Atten.",{"$f":"20*LOG(Iout/(PI()^2*Fsw*Cin)*SIN(PI()*Duty_Cycle)/0.000001) - Min_Noise","v":37.189574038059533},"dB","calculated attenuation"]
["Icinrms",{"$f":"Iout*SQRT(Don_Vinnom_2*(1-Don_Vinnom_2))","v":0.12499277053254776},"A"]
["Cinmin",{"$f":"Iout*Don_Vinnom_2*(1-Don_Vinnom_2)/(Vinripple1*Fsw-Iout*RCinEsr)*1000000","v":0.10415461803287418},"µF"]
["Reported Cinmin",{"$f":"IF(Cinmin<2.2, 2.2,Cinmin)","v":2.2000000000000002},"µF",null,null,null,null,null,null,null,null,"Filter Inductor"]
["Cin",{"$f":"'Design Converter'!E37/1000000","v":2.2000000000000001E-6},"F","Input capacitance",null,null,null,null,null,null,null,"Irms rating",{"$f":"Iout*1.5","v":0.375},"A","calculated suggested IRMS rating"]
["CinEsrMax",{"$f":"-(Iout*Don_Vinnom_2*(1-Don_Vinnom_2)/(Cin*Fsw)-Vinripple1)/(Iout+Iripple_Vinnom/2)","v":3.7079435891033978},"W"]
["RCinEsr",{"$f":"'Design Converter'!E39/1000","v":3.0000000000000001E-3},"W","Input capacitance series resistance (ESR)"]
["Reported Cin ESR max",{"$f":"IF(OR(CinEsrMax>12, CinEsrMax<0), \"N/A\",CinEsrMax*1000)","v":3707.9435891033977},"mΩ",null,null,null,null,null,null,null,null,"Filter Capacitor"]
[null,null,null,null,null,null,null,null,null,null,null,"Cfa calculation",{"$f":"Cin/(Cin*Lf_emi*0.000001*(2*PI()*Fsw/10)^2 - 1) / 0.000001","v":-2.2000105092049682},"uF","calculated value"]
["COT input voltage ripple - Vinripple2",{"$f":"Iout*Don_Vinnom_2*(1-Don_Vinnom_2)/(Cin*Fsw)+(Iout +Iripple_Vinnom/2)*RCinEsr","v":5.7736533537073864E-2},"Vp-p",null,{"$f":"Iout*Don_Vinmax_2*(1-Don_Vinmax_2)/(Cin*Fsw)","v":2.9355476063514751E-2},"Vp-p",null,null,null,null,null,"Cfb calculation",{"$f":"1/(Lf_emi)*(10^(Target_Att/40)/(2*PI()*Fsw))^2/0.000001","v":0.33323934770334135},"uF","calculated value"]
[null,null,null,null,null,null,null,null,null,null,null,"Cf",{"$f":"MAX(M162,M163)","v":0.33323934770334135},"uF","calculated value"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Damping Capacitor"]
["Step 6: Soft Start",null,null,null,null,null,null,null,null,null,null,"Cd ≥",{"$f":"4*Cin*1000000","v":8.8000000000000007},"uF","calculated value"]
["Tss",{"$f":"'Design Converter'!#REF!/1000","v":{"$error":"#REF!"}},"s","Soft-start time",null,null,null,null,null,null,null,"Cd ESR ≥",{"$f":"SQRT(Lf_emi/Cin)","v":3.1622776601683795},"Ω","calculated value"]
["Iss",1.0000000000000001E-5,"A","Soft-start current"]
["Css",{"$f":"8.16*Tss/1000000","v":{"$error":"#NAME?"}},"F","Required soft-start cap"]
["Css_u",{"$f":"'Standard Value Calculator'!B4","v":{"$error":"#NAME?"}},"F","User selected SS cap",null,null,null,null,null,null,null,"CIN and Cd Capacitors Current Sharing and Rating"]
[null,null,null,null,null,null,null,null,null,null,null,"Cd impedance",{"$f":" 1/(2*PI()*Fsw*Cd_emi) + ESR_Cd","v":3.3318309886183788},"Ω","calculated Cd impedance at the sw. frequency"]
["Step 7: Other Components - UVLO, PGOOD",null,null,null,null,null,null,null,null,null,null,"Cin impedance",{"$f":" 1/(2*PI()*Fsw*Cin) + RCinEsr","v":0.14768631190172304},"Ω","calculated CIN impedance at the sw. frequency"]
[]
["Rising UVLO/EN Threshold",1.5,"V",null,null,null,null,null,null,null,null,"IRMS Total Input Cap",{"$f":"Iout*SQRT(Duty_Cycle*(1-Duty_Cycle))","v":0.12467727892960173},"A","calculated total IRMS current for CIN and Cd combined"]
["Falling UVLO/EN Threshold",1.4,"V",null,null,null,null,null,null,null,null,"IRMS Cd Act",{"$f":"IRMSTOT*(ZCIN/(ZCIN+ZCd))","v":5.2918626098806803E-3},"A","Calculated min IRMS current rating for Cd"]
["Voltage Hysteresis",{"$f":"B176-B177","v":0.10000000000000009},"V",null,null,null,null,null,null,null,null,"IRMS CIN",{"$f":"IRMSTOT*(ZCd/(ZCIN+ZCd))","v":0.11938541631972105},"A","Calculated min IRMS current rating for CIN"]
[]
["VINUVLO_ON",{"$f":"'Design Converter'!E48","v":6},"V"]
["VINUVLO_OFF",null,"V"]
[]
["RUV1",{"$f":"'Design Converter'!E49*1000","v":1000},"kΩ",{"$f":"'Standard Value Calculator'!J16","v":1000},"kΩ",{"$f":"IF(Ruvlo1<0,\"N/A\",D183)","v":1000},{"$f":"IF(Ruvlo1<0,\"N/A\",D183&\"kΩ\")","v":"1000kΩ"}]
["RUV2",{"$f":"Vuvlo_on*Ruvlo1/(VINuvlo_on-Vuvlo_on)","v":333.33333333333331},"kΩ",{"$f":"'Standard Value Calculator'!J17","v":332},"kΩ",{"$f":"IF(F183=\"N/A\",\"N/A\",D184)","v":332},{"$f":"IF(G183=\"N/A\",\"N/A\",D184&\"kΩ\")","v":"332kΩ"}]
[]
["VINUVLO_ON_ACTUAL",{"$f":"(D183+D184)/D184*Vuvlo_on","v":6.0180722891566267},"V"]
["VINUVLO_OFF_ACTUAL",{"$f":"(D183+D184)/D184*Vuvlo_off","v":5.6168674698795176},"V"]
[]
["RPG",20,"kΩ"]
[]
[]
["Step 8: FB Divider"]
["Pi",3.1415926500000002,null,"p"]
["Toff_Vinmax",{"$f":"(1-Don_Vinmax_2)/Fsw","v":1.6952291861552854E-6},"sec"]
["Ton_Vinmin",{"$f":"IF(VIN_min>Vout, (1-Don_Vinmin_2)/Fsw, Don_Vinmin_2/Fsw)","v":6.5557083906464927E-7},"sec"]
[]
["Rfb1",{"$f":"'Design Converter'!E43*1000","v":453000},"W","Lower Feedback Resistance - chosen by user",null,null,null,null,1]
["Rfb2",{"$f":"IF(Vout=Vref,100000000,Vref*B197/((Vout-Vref)))","v":50333.333333333328},"W","Upper Feedback Resistance"]
["Rfb2_u",{"$f":"IF(Vout=Vref,\"N/A\",'Standard Value Calculator'!J10)","v":49900},"W","Std Value Upper Feedback Resistance"]
["Rfb",{"$f":"Rfb1_*Rfb2_u/(Rfb1_+Rfb2_u)","v":44948.697554185725},"W","Rfb1 || Rfb2_u"]
[null,{"$f":"1.2/Rfb2_u*(Rfb2_u+Rfb1_)","v":12.0937875751503},"V"]
["Ifb",{"$f":"CHOOSE(MODE_VOUT, IF(Vout=5, 0.000007, 0.0000038), Vout/(Rfb1_+Rfb2_u))","v":2.3861602704314974E-5}]
[]
["Other Input Variables"]
["Rfets",0,"W","Series resistance due to FETs",null,null,null,{"$f":"_Don2*RdsonTop+Doff2*RdsonBot+B209*Vin^2*Fsw/2/(((Iripple1/SQRT(3))^2))","v":148.12678845337328}]
["Diode loss eq res",{"$f":"0.00000002*Fsw*0.6*4/Iripple1","v":0.19787190505422553}]
["Fet loss eq res",{"$f":"_Don2*RdsonTop+Doff2*RdsonBot","v":1.3019479166666668}]
["cap loss eq res",{"$f":"B209*Vin^2*Fsw/2/(((Iripple1/SQRT(3))^2))","v":146.8248405367066}]
["Sw cap",5.0000000000000001E-9]
[]
["Step 8: Efficiency"]
[]
["Design"]
["Ta",25,"°C","Ambient Temperature"]
["Components"]
["LTc",{"$f":"4000/1000000","v":4.0000000000000001E-3},"%/°C","Inductor DCR Temp Co"]
["θCA",40,"°C/W","Inductor Core to Ambient Thermal Resistance"]
["RCinEsr",{"$f":"RCinEsr","v":3.0000000000000001E-3},"W","Input Capacitor ESR"]
["Part Characteristics"]
["Vcc",{"$f":"IF(Vin>7.7,7.5,Vin-0.2)","v":7.5},"V"]
["Deadtime"]
["Deadtime",6.9999999999999998E-9,"s","Total Deadtime",null,null,"20ns for LM5166"]
["IQ"]
["IQ ",1.0000000000000001E-5,"A","Quiescent Current Of Controller (Not Switching!)"]
[]
[]
["IC Power Disipation","Value","Units"]
["Power Dis",{"$f":"Efficiency!AZ106","v":0.20503948329149221},"W"]
["Temp rise",{"$f":"B228*ThetaJA","v":8.4271227632803303},"°C"]
["Current (switching)",{"$f":"(Qg_Q1+Qg_Q2)*Fsw+Iq","v":{"$error":"#NAME?"}},"A"]
["Qrr Current",{"$f":"Qrr_Q2*Fsw","v":{"$error":"#NAME?"}},"A"]
["Diode Current",{"$f":"C232/Vin","v":{"$error":"#NAME?"}},{"$f":"Deadtime*Fsw*(Ipp/2)*(Vsd_Q1+Vsd_Q2)","v":{"$error":"#NAME?"}}]
["Total Application Switching IQ",{"$f":"SUM(B230:B232)","v":{"$error":"#NAME?"}},"A"]
[]
[]
["SCHEMATIC LABELS"]
[]
[]
[{"$f":"\"RUV1 = \"&'Design Converter'!E49&\"MΩ\"","v":"RUV1 = 1MΩ"},{"$f":"C275","v":"1MΩ"}]
[{"$f":"\"RUV2 = \"&'Design Converter'!E50&\"kΩ\"","v":"RUV2 = 332kΩ"},{"$f":"C276","v":"332kΩ"}]
[{"$f":"\"Rhys = \"&'Design Converter'!E52&\"kΩ\"","v":"Rhys = 5.61686746987952kΩ"},{"$f":"C277","v":{"$error":"#REF!"}}]
[]
[{"$f":"\"LF = \"&'Design Converter'!E17&\"µH\"","v":"LF = 100µH"},{"$f":"'Design Converter'!E17&\"µH\"","v":"100µH"}]
[{"$f":"\"Rdcr = \"&Rdcr*1000&\"mΩ\"","v":"Rdcr = 170mΩ"},{"$f":"Rdcr*1000&\"mΩ\"","v":"170mΩ"}]
[{"$f":"\"Rt = \"&'Design Converter'!I43&\"kΩ\"","v":"Rt = kΩ"},{"$f":"'Design Converter'!I43&\"kΩ\"","v":"kΩ"}]
[{"$f":"\"Css = \"&ROUND(Css_u*1000000000,1)&\"nF\"","v":{"$error":"#NAME?"}},{"$f":"ROUND(Css_u*1000000000,1)&\"nF\"","v":{"$error":"#NAME?"}}]
[]
["VIN",{"$f":"VIN_nom&\"V\"","v":"24V"}]
["VIN range",{"$f":"VIN_min&\"V...\"&VIN_max&\"V\"","v":"18V...80V"}]
[]
[{"$f":"\"VOUT = \"&'Design Converter'!E9&\"V\"","v":"VOUT = 12V"},{"$f":"'Design Converter'!E9&\"V\"","v":"12V"}]
[null,null,{"$f":"R30","v":"22"},{"$f":"ROUNDUP('Design Converter'!$E$24/C252,0)","v":2}]
[{"$f":"\"COUT = \"&'Design Converter'!$E$24&\"µF\"","v":"COUT = 33µF"},{"$f":"'Design Converter'!$E$24&\"µF\"","v":"33µF"},{"$f":"IF('Design Converter'!$E$24=OR(10, 22, 47, 100), 'Design Converter'!$E$24,C252)","v":"22"},{"$f":"IF(D252=1, \"\",B255)","v":"2 x "},{"$f":"D253&C253&\"µF\"","v":"2 x 22µF"},{"$f":"C253&\"µF\"","v":"22µF"}]
["Capacitance per component (Cout)",{"$f":"C252&\"µF\"","v":"22µF"}]
["# of output caps",{"$f":"D252&\" x \"","v":"2 x "}]
[]
["CIN",{"$f":"Cin*1000000&\"µF\"","v":"2.2µF"}]
["Capacitance per component (Cin)",{"$f":"\"2.2µF\"","v":"2.2µF"}]
["# of input caps",{"$f":"ROUNDUP(Cin*1000000/2.2,0)&\" x \"","v":"1 x "}]
[]
["Fixed VOUT?",{"$f":"IF(MODE_VOUT=1, \"YES\", \"NO\")","v":"NO"}]
["FB resistor ref des shown or not?",{"$f":"IF(MODE_VOUT=2, \"YES\", \"NO\")","v":"YES"},{"$f":"IF(MODE_VOUT=2, \"R1\", \"\")","v":"R1"},{"$f":"IF(MODE_VOUT=2, \"R2\", \"\")","v":"R2"}]
[{"$f":"\"RFB1 = \"&'Design Converter'!E43&\"kΩ\"","v":"RFB1 = 453kΩ"},{"$f":"'Design Converter'!E43&\"kΩ\"","v":"453kΩ"},{"$f":"IF(MODE=1,'Design Converter'!E43&\"kΩ\", \"\")","v":""}]
[{"$f":"\"RFB2 = \"&IF(Vout=Vref,\"OPEN\",'Design Converter'!E44&\"kΩ\")","v":"RFB2 = 49.9kΩ"},{"$f":"IF(Vout=Vref,\"OPEN\",Rfb2_u/1000&\"kΩ\")","v":"49.9kΩ"},{"$f":"IF(MODE=1, IF(Vout=Vref, \"OPEN\",Rfb2_u/1000&\"kΩ\" ), \"\")","v":""}]
[]
[]
["Show Rt resistor ref des?",{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), \"YES\", \"NO\")","v":"YES"},{"$f":"IF(MODE=4,\"\", \"Rt\")","v":"Rt"}]
["Rt",{"$f":"IF(MODE=4, \"\", 'Standard Value Calculator'!J4/1000&\"kΩ\")","v":"60.4kΩ"}]
[]
["Show ESR resistor ref des?",{"$f":"IF(OR(MODE=3, MODE=4), \"NO\", \"YES\")","v":"NO"},{"$f":"IF(OR(MODE=3, MODE=4),\"\",\"Resr\")","v":""}]
[{"$f":"\"RESR = \"&'Design Converter'!E26&\"mΩ\"","v":"RESR = 0.005mΩ"},{"$f":"IF(OR(MODE=3,MODE=4), \"\", 'Design Converter'!E26&\"Ω\")","v":""},null,null,null,{"$f":"B120","v":1.7150327632002214}]
["Resr",{"$f":"IF(MODE=1, \">\"&ROUND(B130,3), IF(MODE=2,  \">\"&ROUND(B131,3),IF(MODE=3,ROUND(B119,3),\"\")))","v":0.51400000000000001}]
[]
["Adjustable UVLO?",{"$f":"IF(MODE_UVLO=1, \"YES\", \"NO\")","v":"YES"},{"$f":"IF(MODE_UVLO=1,\"Ren1\", \"\")","v":"Ren1"},{"$f":"IF(MODE_UVLO=1, \"Ren2\", \"\")","v":"Ren2"},{"$f":"IF(MODE_UVLO=1, \"Rhys\", \"\")","v":"Rhys"},"Value","Units","BOM display"]
[{"$f":"\"RUV1 = \"&C275","v":"RUV1 = 1MΩ"},{"$f":"'Design Converter'!E49&\" MΩ\"","v":"1 MΩ"},{"$f":"IF(MODE_UVLO=1,'Design Converter'!E49&\"MΩ\", \"\")","v":"1MΩ"},null,null,{"$f":"IF(MODE_UVLO=1,'Design Converter'!E49, \"\")","v":1},{"$f":"IF(MODE_UVLO=1,\"MΩ\", \"\")","v":"MΩ"},{"$f":"IF(MODE_UVLO=1,'Design Converter'!E49&\"M\", \"\")","v":"1M"}]
[{"$f":"\"RUV2 = \"&C276","v":"RUV2 = 332kΩ"},{"$f":"IF(D184>=1000, D184/1000&\" MΩ\", D184&\" kΩ\")","v":"332 kΩ"},{"$f":"IF(MODE_UVLO=1, IF(D184<1, D184*1000&\"Ω\", IF(D184<1000, D184&\"kΩ\", D184/1000&\"MΩ\")), \"\")","v":"332kΩ"},null,null,{"$f":"IF(MODE_UVLO=1, IF(D184<1, D184*1000, IF(D184<1000, D184, D184/1000)), \"\")","v":332},{"$f":"IF(MODE_UVLO=1, IF(D184<1, \"Ω\", IF(D184<1000,\"kΩ\", \"MΩ\")), \"\")","v":"kΩ"},{"$f":"IF(MODE_UVLO=1, IF(D184<1, D184*1000, IF(D184<1000, D184&\"k\", D184/1000&\"M\")), \"\")","v":"332k"}]
[{"$f":"\"RHYS = \"&C277","v":{"$error":"#REF!"}},{"$f":"IF(#REF!<1000,#REF!& \" kΩ\",#REF!& \" MΩ\")","v":{"$error":"#REF!"}},{"$f":"IF(MODE_UVLO=1, IF(#REF!<1,#REF!* 1000&\"Ω\", IF(#REF!<1000,#REF!& \"kΩ\",#REF!/ 1000&\"MΩ\")), \"\")","v":{"$error":"#REF!"}},null,null,{"$f":"IF(MODE_UVLO=1, IF(#REF!<1,#REF!* 1000, IF(#REF!<1000,#REF!,#REF!/ 1000)), \"\")","v":{"$error":"#REF!"}},{"$f":"IF(MODE_UVLO=1, IF(#REF!<1, \"Ω\", IF(#REF!<1000,\"kΩ\", \"MΩ\")), \"\")","v":{"$error":"#REF!"}},{"$f":"IF(MODE_UVLO=1, IF(#REF!<1,#REF!* 1000, IF(#REF!<1000,#REF!& \"k\",#REF!& \"M\")), \"\")","v":{"$error":"#REF!"}}]
[]
[{"$f":"\"Css = \"&Css*1000000000&\"nF\"","v":{"$error":"#NAME?"}},{"$f":"Css*1000000000&\"nF\"","v":{"$error":"#NAME?"}}]
["Cbst",{"$f":"\"2.2nF\"","v":"2.2nF"},null,{"$f":"B280","v":"2.2nF"}]
[]
[]
["Rset resistor ref des?",{"$f":"IF(MODE_RSET=2, \"YES\", \"NO\")","v":"NO"},{"$f":"IF(MODE_RSET=2, \"R3\", \"\")","v":""},null,null,{"$f":"MODE_RSET","v":1}]
["Rset",{"$f":"IF(MODE_RSET=2, C284&\"kΩ\", \"\")","v":""},{"$f":"IF(MODE_ILIM=3,100,IF(MODE_ILIM=2,56.2,IF(MODE_ILIM=4,24.9,0)))","v":{"$error":"#REF!"}}]
[]
[]
["Rpgood","100kΩ"]
[]
["Cff / Cb?",{"$f":"IF(MODE=2, \"Cff\", IF(MODE=3,\"Cb\",\"\"))","v":"Cb"}]
[{"$f":"\"Cff / Cb=\"&B290","v":"Cff / Cb=56pF"},{"$f":"IF(OR(MODE=2,MODE=3),B141&\"pF\",\"\")","v":"56pF"}]
[]
["Ca?",{"$f":"IF(MODE=3, \"Ca\",\"\")","v":"Ca"},null,{"$f":"Ca","v":3.3000000000000002E-9},{"$f":"Ton_Vinmin","v":6.5557083906464927E-7}]
["Ca=",{"$f":"IF(MODE=3,B145&\"pF\",\"\")","v":"3300pF"}]
[]
["Ra?",{"$f":"IF(MODE=3, \"Ra\",\"\")","v":"Ra"},"Injected Ripple"]
["Ra=",{"$f":"IF(MODE=3,Ra&\"kΩ\",\"\")","v":"182kΩ"},{"$f":"(VIN_nom-Vout)*Ton_Vin_nom/(Ra*Ca)/1000","v":1.998001998001998E-2},{"$f":"ROUNDUP(1000*C296,0)","v":20},null,{"$f":"IF(MODE=3,Ra&\"k\",\"\")","v":"182k"}]
[]
["Lf(emi)",{"$f":"M148&\"µH\"","v":"22µH"}]
["Cf(emi)",{"$f":"M149&\"µF\"","v":"4.7µF"}]
["Df(emi)",{"$f":"M150&\"µF\"","v":"10µF"}]
[]
["Full-load efficiency",{"$f":"ROUND(Efficiency!CE106,1)&\"%\"","v":"93.3%"}]
["Full-load efficiency",{"$f":"ROUND(Efficiency!CE107,1)&\"%\"","v":"91.5%"}]
["10% load efficiency",{"$f":"ROUND(Efficiency!CE16,1)&\"%\"","v":"85.9%"},"linear scale only"]
["1% load efficiency",{"$f":"ROUND(Efficiency!CE56,1)&\"%\"","v":"92.1%"},"log scale only"]
[]
["Blank out",{"$f":"IF(C307=\"y\",\"\",\"|\")","v":"|"},"n"]
[]
["OUTPUT CURRENT",{"$f":"'Design Converter'!$E$10&\"A\"","v":"0.25A"}]
[]
["VIN ",2]
["RT",5]
["EN",7]
["PGOOD",6]
["SS",4]
["ILIM",3]
["GND",10]
["FB",8]
["SW",1]
["HYS",9]

{"sheet":"Standard Value Calculator","index":5,"n_rows":159,"n_cols":11,"rows_kept":159,"cut":false,"hidden":true,"merged":[]}
[]
["Capacitors","Css","Cout","Cin","Cb"]
["Inputs",{"$f":"Css","v":{"$error":"#NAME?"}},{"$f":"Cout","v":3.3000000000000003E-5},{"$f":"Cin","v":2.2000000000000001E-6},{"$f":"Cb","v":0},null,null,"Resistors","inputs","Standard Result"]
["Standard Result",{"$f":"SUM(B6:B158)/1000000000000","v":{"$error":"#NAME?"}},{"$f":"SUM(C6:C158)/1000000000000","v":3.3000000000000003E-5},{"$f":"SUM(D6:D158)/1000000000000","v":2.2000000000000001E-6},{"$f":"IF(E3=\"OPEN\",\"OPEN\",SUM(E6:E158)/1000000000000)","v":0},null,null,"Rt",{"$f":"Rt","v":60000},{"$f":"IF(I4>(INT(0.5+100*POWER(10,IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))/96))*POWER(10,INT(LOG(I4))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))+1)/96))*POWER(10,INT(LOG(I4))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))+1)/96))*POWER(10,INT(LOG(I4))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))/96))*POWER(10,INT(LOG(I4))-2))","v":60400},"Ω"]
["(pF)"]
[0.47,{"$f":"IF(IF((B$3*10^12-$A7)*(B$3*10^12-$A6)*-1<0,0,1)*IF(ABS(B$3*10^12-$A7)>(B$3*10^12-$A6),$A6,$A7)=B7,0,IF((B$3*10^12-$A7)*(B$3*10^12-$A6)*-1<0,0,1)*IF(ABS(B$3*10^12-$A7)>(B$3*10^12-$A6),$A6,$A7))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A7)*(C$3*10^12-$A6)*-1<0,0,1)*IF(ABS(C$3*10^12-$A7)>(C$3*10^12-$A6),$A6,$A7)=C7,0,IF((C$3*10^12-$A7)*(C$3*10^12-$A6)*-1<0,0,1)*IF(ABS(C$3*10^12-$A7)>(C$3*10^12-$A6),$A6,$A7))","v":0},{"$f":"IF(IF((D$3*10^12-$A7)*(D$3*10^12-$A6)*-1<0,0,1)*IF(ABS(D$3*10^12-$A7)>(D$3*10^12-$A6),$A6,$A7)=D7,0,IF((D$3*10^12-$A7)*(D$3*10^12-$A6)*-1<0,0,1)*IF(ABS(D$3*10^12-$A7)>(D$3*10^12-$A6),$A6,$A7))","v":0},{"$f":"IF(IF((E$3*10^12-$A7)*(E$3*10^12-$A6)*-1<0,0,1)*IF(ABS(E$3*10^12-$A7)>(E$3*10^12-$A6),$A6,$A7)=E7,0,IF((E$3*10^12-$A7)*(E$3*10^12-$A6)*-1<0,0,1)*IF(ABS(E$3*10^12-$A7)>(E$3*10^12-$A6),$A6,$A7))","v":0},null,null,"Rshunt",{"$f":"Rshunt","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},"Ω"]
[0.56000000000000005,{"$f":"IF(IF((B$3*10^12-$A8)*(B$3*10^12-$A7)*-1<0,0,1)*IF(ABS(B$3*10^12-$A8)>(B$3*10^12-$A7),$A7,$A8)=B8,0,IF((B$3*10^12-$A8)*(B$3*10^12-$A7)*-1<0,0,1)*IF(ABS(B$3*10^12-$A8)>(B$3*10^12-$A7),$A7,$A8))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A8)*(C$3*10^12-$A7)*-1<0,0,1)*IF(ABS(C$3*10^12-$A8)>(C$3*10^12-$A7),$A7,$A8)=C8,0,IF((C$3*10^12-$A8)*(C$3*10^12-$A7)*-1<0,0,1)*IF(ABS(C$3*10^12-$A8)>(C$3*10^12-$A7),$A7,$A8))","v":0},{"$f":"IF(IF((D$3*10^12-$A8)*(D$3*10^12-$A7)*-1<0,0,1)*IF(ABS(D$3*10^12-$A8)>(D$3*10^12-$A7),$A7,$A8)=D8,0,IF((D$3*10^12-$A8)*(D$3*10^12-$A7)*-1<0,0,1)*IF(ABS(D$3*10^12-$A8)>(D$3*10^12-$A7),$A7,$A8))","v":0},{"$f":"IF(IF((E$3*10^12-$A8)*(E$3*10^12-$A7)*-1<0,0,1)*IF(ABS(E$3*10^12-$A8)>(E$3*10^12-$A7),$A7,$A8)=E8,0,IF((E$3*10^12-$A8)*(E$3*10^12-$A7)*-1<0,0,1)*IF(ABS(E$3*10^12-$A8)>(E$3*10^12-$A7),$A7,$A8))","v":0},null,null,"Rc1ea",{"$f":"Rcea1","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},"Ω"]
[0.68,{"$error":"#NAME?"},0,0,0]
[0.82,{"$error":"#NAME?"},0,0,0,null,null,"Rfb1",{"$f":"Rfb1_","v":453000},453000,"Ω"]
[1,{"$error":"#NAME?"},0,0,0,null,null,"Rfb2",{"$f":"Rfb2_","v":50333.333333333328},{"$f":"IF(I10=\"OPEN\",\"OPEN\",IF(I10>(INT(0.5+100*POWER(10,IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))/96))*POWER(10,INT(LOG(I10))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))+1)/96))*POWER(10,INT(LOG(I10))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))+1)/96))*POWER(10,INT(LOG(I10))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))/96))*POWER(10,INT(LOG(I10))-2)))","v":49900},"Ω"]
[1.2,{"$error":"#NAME?"},0,0,0]
[1.5,{"$error":"#NAME?"},0,0,0]
[1.8,{"$error":"#NAME?"},0,0,0,null,null,"Rs",{"$f":"Rs_ideal*1000","v":{"$error":"#NAME?"}},{"$f":"IF(I13=0,0,IF(I13>(INT(0.5+100*POWER(10,IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))/96))*POWER(10,INT(LOG(I13))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))+1)/96))*POWER(10,INT(LOG(I13))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))+1)/96))*POWER(10,INT(LOG(I13))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))/96))*POWER(10,INT(LOG(I13))-2)))","v":{"$error":"#NAME?"}},"mΩ"]
[2.2000000000000002,{"$f":"IF(IF((B$3*10^12-$A15)*(B$3*10^12-$A14)*-1<0,0,1)*IF(ABS(B$3*10^12-$A15)>(B$3*10^12-$A14),$A14,$A15)=B15,0,IF((B$3*10^12-$A15)*(B$3*10^12-$A14)*-1<0,0,1)*IF(ABS(B$3*10^12-$A15)>(B$3*10^12-$A14),$A14,$A15))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A15)*(C$3*10^12-$A14)*-1<0,0,1)*IF(ABS(C$3*10^12-$A15)>(C$3*10^12-$A14),$A14,$A15)=C15,0,IF((C$3*10^12-$A15)*(C$3*10^12-$A14)*-1<0,0,1)*IF(ABS(C$3*10^12-$A15)>(C$3*10^12-$A14),$A14,$A15))","v":0},{"$f":"IF(IF((D$3*10^12-$A15)*(D$3*10^12-$A14)*-1<0,0,1)*IF(ABS(D$3*10^12-$A15)>(D$3*10^12-$A14),$A14,$A15)=D15,0,IF((D$3*10^12-$A15)*(D$3*10^12-$A14)*-1<0,0,1)*IF(ABS(D$3*10^12-$A15)>(D$3*10^12-$A14),$A14,$A15))","v":0},{"$f":"IF(IF((E$3*10^12-$A15)*(E$3*10^12-$A14)*-1<0,0,1)*IF(ABS(E$3*10^12-$A15)>(E$3*10^12-$A14),$A14,$A15)=E15,0,IF((E$3*10^12-$A15)*(E$3*10^12-$A14)*-1<0,0,1)*IF(ABS(E$3*10^12-$A15)>(E$3*10^12-$A14),$A14,$A15))","v":0},null,null,"Cslope_ideal",{"$f":"Cslope_ideal","v":{"$error":"#NAME?"}},{"$f":"#REF!*1000000000000","v":{"$error":"#REF!"}},"pF"]
[2.7,{"$error":"#NAME?"},0,0,0]
[3.3,{"$error":"#NAME?"},0,0,0,null,null,"Ruv1",{"$f":"Ruvlo1","v":1000},{"$f":"IF(I16=\"OPEN\",\"OPEN\",IF(I16>(INT(0.5+100*POWER(10,IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))/96))*POWER(10,INT(LOG(I16))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))+1)/96))*POWER(10,INT(LOG(I16))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))+1)/96))*POWER(10,INT(LOG(I16))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))/96))*POWER(10,INT(LOG(I16))-2)))","v":1000},"kΩ"]
[3.9,{"$error":"#NAME?"},0,0,0,null,null,"Ruv2",{"$f":"Ruvlo2","v":333.33333333333331},{"$f":"IF(I17=\"OPEN\",\"OPEN\",IF(I17>(INT(0.5+100*POWER(10,IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))/96))*POWER(10,INT(LOG(I17))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))+1)/96))*POWER(10,INT(LOG(I17))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))+1)/96))*POWER(10,INT(LOG(I17))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))/96))*POWER(10,INT(LOG(I17))-2)))","v":332},"kΩ"]
[4.7,{"$error":"#NAME?"},0,0,0,null,null,"Rhys",{"$f":"Rhys","v":{"$error":"#NAME?"}},{"$f":"IF(I18=\"OPEN\",\"OPEN\",IF(I18>(INT(0.5+100*POWER(10,IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))/96))*POWER(10,INT(LOG(I18))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))+1)/96))*POWER(10,INT(LOG(I18))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))+1)/96))*POWER(10,INT(LOG(I18))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))/96))*POWER(10,INT(LOG(I18))-2)))","v":{"$error":"#NAME?"}},"kΩ"]
[5.6,{"$error":"#NAME?"},0,0,0]
[6.8,{"$error":"#NAME?"},0,0,0,null,null,"Ra",{"$f":"'Variable Mgmt'!D147","v":181.81818181818181},{"$f":"IF(I20=\"OPEN\",\"OPEN\",IF(I20>(INT(0.5+100*POWER(10,IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))/96))*POWER(10,INT(LOG(I20))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))+1)/96))*POWER(10,INT(LOG(I20))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))+1)/96))*POWER(10,INT(LOG(I20))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))/96))*POWER(10,INT(LOG(I20))-2)))","v":182},"kΩ"]
[8.1999999999999993,{"$error":"#NAME?"},0,0,0]
[10,{"$error":"#NAME?"},0,0,0]
[12,{"$error":"#NAME?"},0,0,0]
[15,{"$error":"#NAME?"},0,0,0]
[18,{"$error":"#NAME?"},0,0,0]
[22,{"$error":"#NAME?"},0,0,0]
[27,{"$error":"#NAME?"},0,0,0]
[33,{"$error":"#NAME?"},0,0,0]
[39,{"$error":"#NAME?"},0,0,0]
[47,{"$error":"#NAME?"},0,0,0]
[56,{"$error":"#NAME?"},0,0,0]
[68,{"$error":"#NAME?"},0,0,0]
[82,{"$error":"#NAME?"},0,0,0]
[{"$f":"A22*10","v":100},{"$error":"#NAME?"},0,0,0]
[{"$f":"A23*10","v":120},{"$error":"#NAME?"},0,0,0]
[150,{"$error":"#NAME?"},0,0,0]
[180,{"$error":"#NAME?"},0,0,0]
[220,{"$error":"#NAME?"},0,0,{"$f":"IF(IF((E$3*10^12-$A39)*(E$3*10^12-$A38)*-1<0,0,1)*IF(ABS(E$3*10^12-$A39)>(E$3*10^12-$A38),$A38,$A39)=E39,0,IF((E$3*10^12-$A39)*(E$3*10^12-$A38)*-1<0,0,1)*IF(ABS(E$3*10^12-$A39)>(E$3*10^12-$A38),$A38,$A39))","v":0}]
[270,{"$error":"#NAME?"},0,0,0]
[330,{"$error":"#NAME?"},0,0,0]
[390,{"$error":"#NAME?"},0,0,0]
[470,{"$error":"#NAME?"},0,0,0]
[560,{"$error":"#NAME?"},0,0,0]
[680,{"$error":"#NAME?"},0,0,0]
[{"$f":"A33*10","v":820},{"$error":"#NAME?"},0,0,0]
[1000,{"$error":"#NAME?"},0,0,0]
[1200,{"$error":"#NAME?"},0,0,0]
[1500,{"$error":"#NAME?"},0,0,0]
[1800,{"$error":"#NAME?"},0,0,0]
[2200,{"$error":"#NAME?"},0,0,0]
[2700,{"$error":"#NAME?"},0,0,0]
[3300,{"$error":"#NAME?"},0,0,0]
[3900,{"$error":"#NAME?"},0,0,0]
[4700,{"$error":"#NAME?"},0,0,0]
[5600,{"$error":"#NAME?"},0,0,0]
[6800,{"$error":"#NAME?"},0,0,0]
[8200,{"$error":"#NAME?"},0,0,0]
[10000,{"$error":"#NAME?"},0,0,0]
[12000,{"$error":"#NAME?"},0,0,0]
[15000,{"$error":"#NAME?"},0,0,0]
[18000,{"$error":"#NAME?"},0,0,0]
[22000,{"$error":"#NAME?"},0,0,0]
[27000,{"$error":"#NAME?"},0,0,0]
[33000,{"$error":"#NAME?"},0,0,0]
[39000,{"$error":"#NAME?"},0,0,0]
[47000,{"$error":"#NAME?"},0,0,0]
[56000,{"$error":"#NAME?"},0,0,0]
[68000,{"$error":"#NAME?"},0,0,0]
[82000,{"$error":"#NAME?"},0,0,0]
[100000,{"$error":"#NAME?"},{"$f":"IF(IF((C$3*10^12-$A71)*(C$3*10^12-$A70)*-1<0,0,1)*IF(ABS(C$3*10^12-$A71)>(C$3*10^12-$A70),$A70,$A71)=C71,0,IF((C$3*10^12-$A71)*(C$3*10^12-$A70)*-1<0,0,1)*IF(ABS(C$3*10^12-$A71)>(C$3*10^12-$A70),$A70,$A71))","v":0},{"$f":"IF(IF((D$3*10^12-$A71)*(D$3*10^12-$A70)*-1<0,0,1)*IF(ABS(D$3*10^12-$A71)>(D$3*10^12-$A70),$A70,$A71)=D71,0,IF((D$3*10^12-$A71)*(D$3*10^12-$A70)*-1<0,0,1)*IF(ABS(D$3*10^12-$A71)>(D$3*10^12-$A70),$A70,$A71))","v":0},{"$f":"IF(IF((E$3*10^12-$A71)*(E$3*10^12-$A70)*-1<0,0,1)*IF(ABS(E$3*10^12-$A71)>(E$3*10^12-$A70),$A70,$A71)=E71,0,IF((E$3*10^12-$A71)*(E$3*10^12-$A70)*-1<0,0,1)*IF(ABS(E$3*10^12-$A71)>(E$3*10^12-$A70),$A70,$A71))","v":0}]
[120000,{"$f":"IF(IF((B$3*10^12-$A72)*(B$3*10^12-$A71)*-1<0,0,1)*IF(ABS(B$3*10^12-$A72)>(B$3*10^12-$A71),$A71,$A72)=B72,0,IF((B$3*10^12-$A72)*(B$3*10^12-$A71)*-1<0,0,1)*IF(ABS(B$3*10^12-$A72)>(B$3*10^12-$A71),$A71,$A72))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A72)*(C$3*10^12-$A71)*-1<0,0,1)*IF(ABS(C$3*10^12-$A72)>(C$3*10^12-$A71),$A71,$A72)=C72,0,IF((C$3*10^12-$A72)*(C$3*10^12-$A71)*-1<0,0,1)*IF(ABS(C$3*10^12-$A72)>(C$3*10^12-$A71),$A71,$A72))","v":0},{"$f":"IF(IF((D$3*10^12-$A72)*(D$3*10^12-$A71)*-1<0,0,1)*IF(ABS(D$3*10^12-$A72)>(D$3*10^12-$A71),$A71,$A72)=D72,0,IF((D$3*10^12-$A72)*(D$3*10^12-$A71)*-1<0,0,1)*IF(ABS(D$3*10^12-$A72)>(D$3*10^12-$A71),$A71,$A72))","v":0},0]
[150000,{"$error":"#NAME?"},0,0,0]
[180000,{"$error":"#NAME?"},0,0,0]
[220000,{"$error":"#NAME?"},0,0,0]
[270000,{"$error":"#NAME?"},0,0,0]
[330000,{"$error":"#NAME?"},0,0,0]
[390000,{"$error":"#NAME?"},0,0,0]
[470000,{"$error":"#NAME?"},0,0,0]
[560000,{"$error":"#NAME?"},0,0,0]
[680000,{"$error":"#NAME?"},0,0,0]
[820000,{"$error":"#NAME?"},0,0,0]
[1000000,{"$error":"#NAME?"},0,0,0]
[1200000,{"$error":"#NAME?"},0,0,0]
[1500000,{"$error":"#NAME?"},0,0,0]
[1800000,{"$error":"#NAME?"},0,0,0]
[2200000,{"$error":"#NAME?"},0,2200000,0]
[2700000,{"$error":"#NAME?"},0,0,0]
[3300000,{"$error":"#NAME?"},0,0,0]
[3900000,{"$error":"#NAME?"},0,0,0]
[4700000,{"$error":"#NAME?"},0,0,0]
[5600000,{"$error":"#NAME?"},0,0,0]
[6800000,{"$error":"#NAME?"},0,0,0]
[8200000,{"$error":"#NAME?"},0,0,0]
[10000000,{"$error":"#NAME?"},0,0,0]
[12000000,{"$error":"#NAME?"},0,0,0]
[15000000,{"$error":"#NAME?"},0,0,0]
[18000000,{"$error":"#NAME?"},0,0,0]
[22000000,{"$error":"#NAME?"},0,0,0]
[{"$f":"A87*10","v":27000000},{"$error":"#NAME?"},0,0,0]
[33000000,{"$error":"#NAME?"},33000000,0,0]
[39000000,{"$error":"#NAME?"},0,0,0]
[47000000,{"$error":"#NAME?"},0,0,{"$f":"IF(IF((E$3*10^12-$A103)*(E$3*10^12-$A102)*-1<0,0,1)*IF(ABS(E$3*10^12-$A103)>(E$3*10^12-$A102),$A102,$A103)=E103,0,IF((E$3*10^12-$A103)*(E$3*10^12-$A102)*-1<0,0,1)*IF(ABS(E$3*10^12-$A103)>(E$3*10^12-$A102),$A102,$A103))","v":0}]
[56000000,{"$error":"#NAME?"},0,{"$f":"IF(IF((D$3*10^12-$A104)*(D$3*10^12-$A103)*-1<0,0,1)*IF(ABS(D$3*10^12-$A104)>(D$3*10^12-$A103),$A103,$A104)=D104,0,IF((D$3*10^12-$A104)*(D$3*10^12-$A103)*-1<0,0,1)*IF(ABS(D$3*10^12-$A104)>(D$3*10^12-$A103),$A103,$A104))","v":0},0]
[68000000,{"$error":"#NAME?"},0,0,0]
[82000000,{"$error":"#NAME?"},0,0,0]
[100000000,{"$error":"#NAME?"},0,0,0]
[120000000,{"$error":"#NAME?"},0,0,0]
[150000000,{"$error":"#NAME?"},0,0,0]
[180000000,{"$error":"#NAME?"},0,0,0]
[220000000,{"$error":"#NAME?"},0,0,0]
[270000000,{"$error":"#NAME?"},0,0,0]
[330000000,{"$error":"#NAME?"},0,0,0]
[390000000,{"$error":"#NAME?"},0,0,0]
[470000000,{"$error":"#NAME?"},0,0,0]
[560000000,{"$error":"#NAME?"},0,0,0]
[680000000,{"$error":"#NAME?"},0,0,0]
[820000000,{"$error":"#NAME?"},0,0,0]
[1000000000,{"$error":"#NAME?"},0,0,0]
[1200000000,{"$error":"#NAME?"},0,0,0]
[1500000000,{"$error":"#NAME?"},0,0,0]
[1800000000,{"$error":"#NAME?"},0,0,0]
[2200000000,{"$error":"#NAME?"},0,0,0]
[2700000000,{"$error":"#NAME?"},0,0,0]
[3300000000,{"$error":"#NAME?"},0,0,0]
[3900000000,{"$error":"#NAME?"},0,0,0]
[4700000000,{"$error":"#NAME?"},0,0,0]
[5600000000,{"$error":"#NAME?"},0,0,0]
[6800000000,{"$error":"#NAME?"},0,0,0]
[8200000000,{"$error":"#NAME?"},0,0,0]
[10000000000,{"$error":"#NAME?"},0,0,0]
[12000000000,{"$error":"#NAME?"},0,0,0]
[15000000000,{"$error":"#NAME?"},0,0,0]
[18000000000,{"$error":"#NAME?"},0,0,0]
[22000000000,{"$error":"#NAME?"},{"$f":"IF(IF((C$3*10^12-$A135)*(C$3*10^12-$A134)*-1<0,0,1)*IF(ABS(C$3*10^12-$A135)>(C$3*10^12-$A134),$A134,$A135)=C135,0,IF((C$3*10^12-$A135)*(C$3*10^12-$A134)*-1<0,0,1)*IF(ABS(C$3*10^12-$A135)>(C$3*10^12-$A134),$A134,$A135))","v":0},0,{"$f":"IF(IF((E$3*10^12-$A135)*(E$3*10^12-$A134)*-1<0,0,1)*IF(ABS(E$3*10^12-$A135)>(E$3*10^12-$A134),$A134,$A135)=E135,0,IF((E$3*10^12-$A135)*(E$3*10^12-$A134)*-1<0,0,1)*IF(ABS(E$3*10^12-$A135)>(E$3*10^12-$A134),$A134,$A135))","v":0}]
[27000000000,{"$f":"IF(IF((B$3*10^12-$A136)*(B$3*10^12-$A135)*-1<0,0,1)*IF(ABS(B$3*10^12-$A136)>(B$3*10^12-$A135),$A135,$A136)=B136,0,IF((B$3*10^12-$A136)*(B$3*10^12-$A135)*-1<0,0,1)*IF(ABS(B$3*10^12-$A136)>(B$3*10^12-$A135),$A135,$A136))","v":{"$error":"#NAME?"}},0,0,0]
[33000000000,{"$error":"#NAME?"},0,0,0]
[39000000000,{"$error":"#NAME?"},0,0,0]
[47000000000,{"$error":"#NAME?"},0,0,0]
[56000000000,{"$error":"#NAME?"},0,0,0]
[68000000000,{"$error":"#NAME?"},0,0,0]
[82000000000,{"$error":"#NAME?"},0,0,0]
[100000000000,{"$error":"#NAME?"},0,0,0]
[120000000000,{"$error":"#NAME?"},0,0,0]
[150000000000,{"$error":"#NAME?"},0,0,0]
[180000000000,{"$error":"#NAME?"},0,0,0]
[220000000000,{"$error":"#NAME?"},0,0,0]
[270000000000,{"$error":"#NAME?"},0,0,0]
[330000000000,{"$error":"#NAME?"},0,0,0]
[390000000000,{"$error":"#NAME?"},0,0,0]
[470000000000,{"$error":"#NAME?"},0,0,0]
[560000000000,{"$error":"#NAME?"},0,0,0]
[680000000000,{"$error":"#NAME?"},0,0,0]
[820000000000,{"$error":"#NAME?"},0,0,0]
[1000000000000,{"$error":"#NAME?"},0,0,0]
[1200000000000,{"$error":"#NAME?"},0,0,0]
[1500000000000,{"$error":"#NAME?"},0,0,0]
[1800000000000,{"$error":"#NAME?"},0,0,0]
[2200000000000,{"$error":"#NAME?"},0,0,0]
[2700000000000,{"$error":"#NAME?"},2700000000000,2700000000000,2700000000000]

{"sheet":"Efficiency","index":6,"n_rows":114,"n_cols":88,"rows_kept":114,"cut":false,"hidden":true,"merged":[[0,0,2,4],[1,6,1,7],[3,0,3,4],[3,10,3,21]]}
["LM5169 (COT) Efficiency Calculator"]
[null,null,null,null,null,null,"TERMS OF USE",null,null,{"$f":"CoutEsr","v":5.0000000000000001E-3},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"didn't include FB"]
[]
[null,null,null,null,null,null,null,"Currents",null,null,"Miscellaneous",null,null,null,null,null,null,null,null,null,null,null,"Inductor",null,null,null,"Cout",null,null,"Cin",null,null,"High-side MOSFET Losses ",null,null,null,null,null,null,null,null,"Low-side MOSFET Losses ",null,null,"Diode",null,null,null,null,null,null,null,"RESULTS"]
["Input Parameters",null,null,null,null,null,null,"Step","Iout (A)","Ripple Current pk-pk (A)","Peak Current (A)","Valley Current (A)","VOUT Hysteresis +Undershoot (2us Delay) (mV)","Vout Rise per Pulse (mV)","Number of Pulses in DCM","VOUT Ripple (mV)","Off Time (sec)","Duty Cycle","Switching Frequency (Hz)","Active Mode Duration (sec)","Sleep Mode Duration (sec)","Operating Quiescent Current (A)","Irms (A)","Inductor DCR Loss @ 25°C (W)","Inductor Core Loss  (W)","Total Inductor Loss (W)","Irms (A)","Cout ESR Loss (W)","Total Cout Loss (W)","Irms (A)","Cin ESR Loss (W)","Total Cin Loss (W)","Irms (A)","Rdson HS Loss @ 25°C (W)","HS Gate Qg Loss (W)     ","SW Rise Time (ns)","SW Fall Time (ns)","HS Switching  Loss (W)","Coss Loss (W)","Total HS FET AC Loss (W)","Total HS FET Loss (W)","Irms (A)","Rdson LS Loss @ 25°C (W)","LS Gate Qg Loss (W)","Reverse Recovery & Leakage Losses","DeadTime Loss @ 25°C (W)","Total LS FET AC Loss (W)","Total LS FET Loss (W)","Quiescent Loss (W)","LDO + Quiescent Loss (W)","Total Gate Drive Loss (W)","Total Power Loss in IC (W)","Total Converter Power Loss (W)","Pout (W)","EFF (%)","High-side MOSFET Rdson %","Low-side MOSFET Rdson %","Gate Drive (Qg) Loss from Vin %","High-side MOSFET AC Loss %","Reverse Recovery & Leakage Loss %","Deadtime Loss %","Low-side MOSFET AC Loss %","Inductor Cu Loss %","Inductor Core Loss %","Cin ESR %","Cout ESR %","LDO + Quiescent Current Loss %","Total Loss %","Overall Eff %","Overall Eff","Current (mA)","Keep for \"previous\" data series","Keep for \"previous\" data series","Frequency (kHz)",null,"Coss",null,"Total Power Loss in IC (mW)","LDO + Quiescent Loss (mW)","Total Inductor Loss (mW)",null,null,"Overall Eff","Total Power Loss in IC (W)","LDO + Quiescent Loss (mW)","Total Inductor Loss (mW)","Fsw (kHz)","Ripple (mV)"]
["Design","Input Value","Units","Std Units","Description",null,null,0.04,{"$f":"IF(PLOT_TYPE=1, H6/100*Iout, min_I*EXP(H6*rr/100))","v":1E-4},{"$f":"IF(I6<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I6-Vout)/L*OnTime)","v":0.11883900499999998},{"$f":"IF(I6<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I6+((Vin-(Rdcr+RdsonTop)*J6-Vout)/L*OnTime)/2)","v":0.11883900499999998},{"$f":"IF(I6<Icrit, 0, I6-((Vin-(Rdcr+RdsonTop)*K6-Vout)/L*OnTime)/2)","v":0},{"$f":"1000*((((J6/2)-I6)*0.000002/Cout+Vout/306))","v":42.810807638146166},{"$f":"IF(I6<Icrit, 1000*SQRT((J6*CoutEsr)^2+(((J6/2)-I6)*(OnTime+OffTime)/Cout)^2), 1000*J6*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":3.5373540664433958},{"$f":"ROUNDUP(M6/N6,0)","v":13},{"$f":"IF(I6<Icrit, 1000*((N6/1000)*O6), 1000*J6*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":45.985602863764143},{"$f":"IF(I6<Icrit, L*J6/(Vout+J6/2*(RdsonBot+Rdcr)), L*J6/(Vout+I6*(RdsonBot+Rdcr)))","v":9.8583407925882194E-7},{"$f":"OnTime*S6","v":8.4747721219417132E-4},{"$f":"IF(I6<Icrit,I6/((OnTime+Q6)*J6/2),1/(OnTime+Q6))","v":847.47721219417133},{"$f":"IF(1/S6-OnTime-Q6>Tsleep, OnTime+Q6+Tsleep, 1/S6)","v":6.9858340792588225E-6},{"$f":"IF(1/S6-OnTime-Q6>Tsleep, 1/S6-OnTime-Q6-Tsleep, 0)","v":1.1729868962917888E-3},{"$f":"S6*(T6*Iq_active+U6*Iq_sleep)","v":1.3848217873721848E-5},{"$f":"IF(I6<Icrit,Iripple*SQRT((OnTime+OffTime)*S6/3), SQRT(I6^2+Iripple^2/12))","v":2.6909290361979824E-3},{"$f":"W6^2*Rdcr","v":1.2309868432350785E-6},{"$f":"Core_Loss/1000*S6/$S$106","v":0},{"$f":"(Y6+X6*(1+Ltc*(Ta-25)))/(1-X6*Ltc*ThetaCa)","v":1.2309870856877035E-6},{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q6)*S6)","v":1.3613000076002472E-3},{"$f":"RCoutEsr*AA6^2","v":9.265688553462167E-9},{"$f":"AB6","v":9.265688553462167E-9},{"$f":"SQRT($R6)*SQRT($I6^2*(1-R6)+(Iripple^2)/12)","v":9.660160399418867E-4},{"$f":"RCinEsr*AD6^2","v":2.7995609682750147E-9},{"$f":"AE6","v":2.7995609682750147E-9},{"$f":"IF(I6<Icrit,Iripple*SQRT((OnTime)*S6/3), SQRT(OnTime*S6*(I6^2+Iripple^2/12)))","v":1.9320233143883736E-3},{"$f":"RdsonTop*AG6^2","v":6.9055210615794369E-6},{"$f":"QgTop*S6*Vdd","v":2.5424316365825139E-6},{"$f":"5*VIN_nom/24","v":5},{"$f":"IF(I6<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I6+Iripple/2)*1000000000)","v":33.405828621139626},{"$f":"IF(I6<Icrit, Vin*(I6+Iripple/2)*AK6/1000000000/2*S6, Vin*(I6-Iripple/2)*AJ6/1000000000/2*S6 + Vin*(I6+Iripple/2)*AK6/1000000000/2*S6)","v":1.9559847783166758E-5},{"$f":"IF(I6<Icrit, Csw*(Vin)^2*S6/2, Csw*Vin^2*S6/2)","v":3.9051749937907417E-5},{"$f":"AI6+AL6+AM6","v":6.1154029357656691E-5},{"$f":"(AI6+AL6+AM6+AH6*(1+RdsonTopTc*(Ta-25)))/(1-AH6*RdsonTopTc*ThetaJA)","v":6.8059643138330508E-5},{"$f":"IF(I6<Icrit,Iripple*SQRT((OffTime)*S6/3), SQRT(OffTime*S6*(I6^2+Iripple^2/12)))","v":1.8730683357830716E-3},{"$f":"RdsonBot*AP6^2","v":2.6312887428848739E-6},{"$f":"QgBot*S6*Vdd","v":6.864565418772788E-6},{"$f":"IF(I6<Icrit, Vin*Idss*R6, QrrBot*(I6-Iripple/2)/1*S6*Vin+Vin*Idss*R6)","v":0},{"$f":"IF(I6<Icrit, dead1*S6*(I6+Iripple/2)*((I6+Iripple/2)*BDserR+VSD), dead1*S6*(I6+Iripple/2)*((I6+Iripple/2)*BDserR+VSD)+dead2*S6*(I6-Iripple/2)*((I6-Iripple/2)*BDserR+VSD))","v":2.7521010280922668E-7},{"$f":"AR6+AS6+AT6","v":7.1397755215820144E-6},{"$f":"(AR6+AS6+AT6+AQ6*(1+RdsonBotTc*(Ta-25)))/(1-AQ6*RdsonBotTc*ThetaJA)","v":9.7710693366352663E-6},{"$f":"Vin*V6+Vout*Ifb/0.8","v":6.90281269534049E-4},{"$f":"(Vin-Vdd)*(S6*QgBot+S6*QgTop)+AW6","v":7.260278583443991E-4},{"$f":"AI6+AR6","v":9.4069970553553023E-6},{"$f":"AO6+AV6+AX6+AY6","v":8.1326556787472009E-4},{"$f":"SUM(Z6,AC6,AF6,AZ6)","v":8.1450862020992956E-4},{"$f":"Vout*I6","v":1.2000000000000001E-3},{"$f":"BB6/(BB6+BA6)","v":0.59567876154084132},{"$f":"(AO6-AN6)/($BB6+$BA6)","v":3.4279395537926221E-3},{"$f":"(AV6-AU6)/($BB6+$BA6)","v":1.3061715341674972E-3},{"$f":"Vin*S6*(QgBot+QgTop)/($BB6+$BA6)","v":2.241419342300955E-2},{"$f":"AN6/($BB6+$BA6)","v":3.0356797059167658E-2},{"$f":"AS6/(BA6+BB6)","v":0},{"$f":"AT6/($BB6+$BA6)","v":1.3661401100410647E-4},{"$f":"AU6/($BB6+$BA6)","v":3.5441772003129905E-3},{"$f":"X6/($BB6+$BA6)","v":6.1106059854278442E-4},{"$f":"Y6/($BB6+$BA6)","v":0},{"$f":"(AF6)/($BB6+$BA6)","v":1.3896991753667827E-6},{"$f":"(AC6)/($BB6+$BA6)","v":4.5994782352912443E-6},{"$f":"AX6/($BB6+$BA6)","v":0.36039947958561752},{"$f":"SUM(BD6:BO6)","v":0.42220242214302539},{"$f":"BC6","v":0.59567876154084132},{"$f":"100*BQ6","v":59.567876154084132},{"$f":"I6*1000","v":0.1},8.7924221262065743,{"$f":"BT6/100","v":8.7924221262065741E-2},{"$f":"S6/1000","v":0.84747721219417138},null,{"$f":"AM6/($BB6+$BA6)","v":1.9385248365846097E-2},null,{"$f":"AZ6","v":8.1326556787472009E-4},{"$f":"AX6","v":7.260278583443991E-4},{"$f":"Z6","v":1.2309870856877035E-6},null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR6, IF(MODE_ILIM=4,#REF!,#REF!))","v":59.567876154084132},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ6, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.1326556787472009E-4},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA6, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.260278583443991E-4},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB6, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.2309870856877035E-6},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S6, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":0.84747721219417138},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P6, IF(MODE_ILIM=4,#REF!,#REF!))","v":45.985602863764143}]
[null,null,null,null,null,null,null,1,2.5000000000000001E-3,0.11883900499999998,0.11883900499999998,0,{"$f":"IF(I7<Icrit, 1000*((((J7/2)-I7)*0.000002/Cout+Vout/306)), 1000*J7*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":42.665353092691625},3.39835760527968,{"$f":"ROUNDUP(M7/N7,0)","v":13},44.17864886863584,9.8583407925882194E-7,{"$f":"OnTime*S7","v":2.118693030485428E-2},21186.930304854282,{"$f":"IF(1/S7-OnTime-Q7>Tsleep, OnTime+Q7+Tsleep, 1/S7)","v":6.9858340792588225E-6},{"$f":"IF(1/S7-OnTime-Q7>Tsleep, 1/S7-OnTime-Q7-Tsleep, 0)","v":4.0213075135583081E-5},1.0620544684304616E-4,{"$f":"IF(I7<Icrit,Iripple*SQRT((OnTime+OffTime)*S7/3), SQRT(I7^2+Iripple^2/12))","v":1.3454645180989912E-2},3.0774671080876958E-5,0,3.0774822614483923E-5,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q7)*S7)","v":6.8065000380012359E-3},{"$f":"RCoutEsr*AA7^2","v":2.3164221383655413E-7},{"$f":"AB7","v":2.3164221383655413E-7},{"$f":"SQRT($R7)*SQRT($I7^2*(1-R7)+(Iripple^2)/12)","v":4.8434570115448968E-3},{"$f":"RCinEsr*AD7^2","v":7.0377227468050262E-8},{"$f":"AE7","v":7.0377227468050262E-8},{"$f":"IF(I7<Icrit,Iripple*SQRT((OnTime)*S7/3), SQRT(OnTime*S7*(I7^2+Iripple^2/12)))","v":9.660116571941867E-3},{"$f":"RdsonTop*AG7^2","v":1.7263802653948591E-4},{"$f":"QgTop*S7*Vdd","v":6.3560790914562841E-5},5,33.405828621139626,{"$f":"IF(I7<Icrit, Vin*(I7+Iripple/2)*AK7/1000000000/2*S7, Vin*(I7-Iripple/2)*AJ7/1000000000/2*S7 + Vin*(I7+Iripple/2)*AK7/1000000000/2*S7)","v":5.0937988310700236E-4},{"$f":"IF(I7<Icrit, Csw*(Vin)^2*S7/2, Csw*Vin^2*S7/2)","v":9.7629374844768538E-4},{"$f":"AI7+AL7+AM7","v":1.5492344224692506E-3},1.7219310945894E-3,9.3653416789153572E-3,{"$f":"RdsonBot*AP7^2","v":6.5782218572121842E-5},1.7161413546931968E-4,0,7.1691889932722331E-6,{"$f":"AR7+AS7+AT7","v":1.7878332446259193E-4},2.4456871692917035E-4,2.9068547647978327E-3,3.8005194850565865E-3,2.3517492638388252E-4,{"$f":"AO7+AV7+AX7+AY7","v":6.002194222959039E-3},6.0332710650148275E-3,0.03,{"$f":"BB7/(BB7+BA7)","v":0.83256388091636213},{"$f":"(AO7-AN7)/($BB7+$BA7)","v":4.792700385389737E-3},{"$f":"(AV7-AU7)/($BB7+$BA7)","v":1.8256847219860182E-3},3.1327703904701604E-2,{"$f":"AN7/($BB7+$BA7)","v":4.2994554107340606E-2},{"$f":"AS7/(BA7+BB7)","v":0},{"$f":"AT7/($BB7+$BA7)","v":1.9896026037538659E-4},{"$f":"AU7/($BB7+$BA7)","v":4.9616179485901567E-3},8.5406265296731525E-4,0,{"$f":"(AF7)/($BB7+$BA7)","v":1.953117920964451E-6},{"$f":"(AC7)/($BB7+$BA7)","v":6.428564684527311E-6},{"$f":"AX7/($BB7+$BA7)","v":0.1054725083992322},{"$f":"SUM(BD7:BO7)","v":0.1924361740631885},0.83256388091636213,{"$f":"100*BQ7","v":83.256388091636211},2.5,9.5725635821403898,{"$f":"BT7/100","v":9.5725635821403893E-2},21.186930304854283,null,2.709423040406625E-2,null,{"$f":"AZ7","v":6.002194222959039E-3},{"$f":"AX7","v":3.8005194850565865E-3},{"$f":"Z7","v":3.0774822614483923E-5},null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR7, IF(MODE_ILIM=4,#REF!,#REF!))","v":83.256388091636211},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ7, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.002194222959039E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA7, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.8005194850565865E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB7, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.0774822614483923E-5},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S7, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":21.186930304854283},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P7, IF(MODE_ILIM=4,#REF!,#REF!))","v":44.17864886863584}]
["Vin",{"$f":"Vin","v":24},"V",{"$f":"B8","v":24},"Vin",null,null,2,5.0000000000000001E-3,0.11883900499999998,0.11883900499999998,0,42.513837941176469,3.2537606896542566,14,45.552649655159591,9.8583407925882194E-7,{"$f":"OnTime*S8","v":4.2373860609708561E-2},42373.860609708565,6.9858340792588225E-6,1.661362052816213E-5,2.0241089368609231E-4,1.902774169187374E-2,6.154934216175393E-5,0,6.1549948299166395E-5,9.6258446660343333E-3,4.6328442767310815E-7,{"$f":"AB8","v":4.6328442767310815E-7},6.9045915161884408E-3,1.4302015201626419E-7,{"$f":"AE8","v":1.4302015201626419E-7},1.3661467870145281E-2,3.4527605307897193E-4,1.2712158182912568E-4,5,33.405828621139626,1.0612257839803241E-3,1.9525874968953708E-3,3.1409348627048205E-3,3.4864483989112531E-3,1.3244593218580113E-2,1.3156443714424374E-4,3.4322827093863936E-4,0,1.4940692223735785E-5,3.5816896316237512E-4,4.897461116826977E-4,5.2157854890309396E-3,7.0031149295484464E-3,4.7034985276776505E-4,{"$f":"AO8+AV8+AX8+AY8","v":1.1449659292910162E-2},1.1511815545789018E-2,0.06,{"$f":"BB8/(BB8+BA8)","v":0.83902218874001311},4.8315587231203801E-3,1.8399357856615139E-3,3.1570717035420262E-2,4.3921900719940184E-2,0,2.0892620484749488E-4,5.0085284568539522E-3,8.6068772960104587E-4,0,1.9999513496435895E-6,6.4784319085909256E-6,9.792948026979334E-2,0.18618021330849641,0.83902218874001311,{"$f":"100*BQ8","v":83.902218874001306},5,10.507357436577642,0.10507357436577643,42.373860609708565,null,2.7304403922525627E-2,null,1.1449659292910162E-2,7.0031149295484464E-3,6.1549948299166395E-5,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR8, IF(MODE_ILIM=4,#REF!,#REF!))","v":83.902218874001306},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ8, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1449659292910162E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA8, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0031149295484464E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB8, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1549948299166395E-5},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S8, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":42.373860609708565},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P8, IF(MODE_ILIM=4,#REF!,#REF!))","v":45.552649655159591}]
["Vout",{"$f":"Vout","v":12},"V",{"$f":"B9","v":12},"Vout",null,null,3,7.4999999999999997E-3,0.11883900499999998,0.11883900499999998,0,42.362322789661313,3.1093855746128307,14,43.531398044579632,9.8583407925882194E-7,6.3560790914562834E-2,63560.790914562844,6.9858340792588225E-6,8.7471356590218132E-6,2.986163405291385E-4,2.3304129051286277E-2,9.2324013242630861E-5,{"$f":"Core_Loss/1000*S9/$S$106","v":0},9.2325377058524331E-5,1.1789203887537633E-2,6.9492664150966235E-7,6.9492664150966235E-7,8.5636694869141126E-3,2.2000930524331147E-7,2.2000930524331147E-7,1.6731812709641407E-2,5.1791407961845784E-4,1.9068237274368852E-4,{"$f":"15*VIN_nom/24","v":15},33.405828621139626,1.6555377026199656E-3,2.9288812453430557E-3,4.7751013207067098E-3,5.2935562646173953E-3,1.6221247618123814E-2,1.9734665571636561E-4,5.148424064079591E-4,0,2.3315065848311168E-5,5.3815747225627027E-4,7.3553276413745752E-4,7.5247162132640478E-3,1.0205710374040309E-2,7.0552477915164762E-4,1.6940324181946811E-2,1.7033564494952087E-2,0.09,{"$f":"BB9/(BB9+BA9)","v":0.84085772929896752},4.8438538542284731E-3,1.8440504416770674E-3,3.1639784733952528E-2,4.4613120596688281E-2,0,2.178294814185204E-4,5.0279318902964392E-3,8.6257066816629335E-4,0,2.0555169425726035E-6,6.4926048645463593E-6,9.535056056664945E-2,0.18440825035488417,0.84085772929896752,84.085772929896748,7.5,11.516667783884284,0.11516667783884284,63.560790914562844,null,2.7364138148283267E-2,null,1.6940324181946811E-2,1.0205710374040309E-2,9.2325377058524331E-5,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR9, IF(MODE_ILIM=4,#REF!,#REF!))","v":84.085772929896748},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ9, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.6940324181946811E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA9, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0205710374040309E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB9, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.2325377058524331E-5},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S9, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":63.560790914562844},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P9, IF(MODE_ILIM=4,#REF!,#REF!))","v":43.531398044579632}]
["Iout",{"$f":"Iout","v":0.25},"A",{"$f":"B10","v":0.25},"Iout(max)",null,null,4,0.01,0.11883900499999998,0.11883900499999998,0,42.210807638146164,2.9652646579311104,15,44.478969868966658,9.8583407925882194E-7,8.4747721219417121E-2,84747.72121941713,6.9858340792588225E-6,4.8138932244516521E-6,3.9482178737218466E-4,2.6909290361979823E-2,1.2309868432350783E-4,0,1.2310110889703486E-4,1.3613000076002472E-2,9.2656885534621651E-7,9.2656885534621651E-7,1.0053576810282955E-2,3.0322322004077761E-7,3.0322322004077761E-7,1.9320233143883734E-2,6.9055210615794364E-4,2.5424316365825136E-4,15,33.405828621139626,2.292315639025926E-3,3.9051749937907415E-3,6.4517337964749184E-3,7.1432590439525784E-3,1.8730683357830714E-2,2.6312887428848737E-4,6.8645654187727873E-4,0,3.229286602391888E-5,7.187494079011976E-4,9.8192925420042794E-4,9.833646937497156E-3,1.3408305818532171E-2,9.4069970553553009E-4,2.2474193822220705E-2,2.2598524723193125E-2,0.12,0.84152343253858675,4.8494558328708009E-3,1.8456000636058833E-3,3.166483380761189E-2,4.5244043085289842E-2,0,2.2646002885797433E-4,5.0403705739341048E-3,8.6325356144085195E-4,0,2.1264120412843198E-6,6.4977450302858115E-6,9.4028362807819149E-2,0.18377100391850204,0.84152343253858675,84.152343253858675,10,12.603144523181673,0.12603144523181672,84.74772121941713,null,2.7385802211988657E-2,null,2.2474193822220705E-2,1.3408305818532171E-2,1.2310110889703486E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR10, IF(MODE_ILIM=4,#REF!,#REF!))","v":84.152343253858675},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ10, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.2474193822220705E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA10, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.3408305818532171E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB10, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.2310110889703486E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S10, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":84.74772121941713},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P10, IF(MODE_ILIM=4,#REF!,#REF!))","v":44.478969868966658}]
["Rt",{"$f":"Vout*2500/(Fsw/1000)","v":60},"kW",{"$f":"B11*1000","v":60000},"RT pin resistance to get Fsw",null,null,5,1.2500000000000001E-2,0.11883900499999998,0.11883900499999998,0,42.059292486631009,2.8214368937536363,15,42.321553406304545,9.8583407925882194E-7,0.10593465152427142,105934.65152427142,6.9858340792588225E-6,2.453947763709557E-6,4.9102723421523087E-4,3.008550123783341E-2,1.5387335540438486E-4,0,1.5387714381917517E-4,1.5219796773825666E-2,1.1582110691827709E-6,1.1582110691827709E-6,1.1464996447058094E-2,3.9433843059316414E-7,3.9433843059316414E-7,2.1600677325434255E-2,8.6319013269742977E-4,3.1780395457281426E-4,15,33.405828621139626,2.9715595931982071E-3,4.8814687422384269E-3,8.1708322900094481E-3,9.0355610897545711E-3,2.0941540626566751E-2,3.2891109286060932E-4,8.5807067734659868E-4,0,4.1874648907479419E-5,8.9994532625407809E-4,1.2289361618086927E-3,1.2142577661730266E-2,1.6610901263024034E-2,1.175874631919413E-3,2.8051273146506711E-2,2.8206702839825661E-2,0.15000000000000002,0.84171918120735234,4.8523921152525424E-3,1.8461193115183524E-3,3.1672199436214556E-2,4.5850308432862315E-2,0,2.3497796794499283E-4,5.0500082876397739E-3,8.6345436480404487E-4,0,2.2128148061164695E-6,6.4992564854520922E-6,9.3211428068191757E-2,0.18358960005571989,0.84171918120735234,84.171918120735228,12.5,13.76888730592373,0.1376888730592373,105.93465152427142,null,2.7392172485374747E-2,null,2.8051273146506711E-2,1.6610901263024034E-2,1.5387714381917517E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR11, IF(MODE_ILIM=4,#REF!,#REF!))","v":84.171918120735228},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ11, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.8051273146506711E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA11, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.6610901263024034E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB11, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.5387714381917517E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S11, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":105.93465152427142},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P11, IF(MODE_ILIM=4,#REF!,#REF!))","v":42.321553406304545}]
["Tamb",{"$f":"'Design Converter'!E56","v":25},"°C",{"$f":"B12","v":25},"Ambient temperature",null,null,6,1.4999999999999999E-2,0.11883900499999998,0.11883900499999998,0,41.907777335115867,2.6779495165493619,16,42.84719226478979,9.8583407925882194E-7,0.12712158182912567,127121.58182912569,6.9858340792588225E-6,8.8065078988149702E-7,5.8723268105827697E-4,3.2957015363621903E-2,1.8464802648526172E-4,0,1.8465348182942229E-4,1.6672452027337342E-2,1.3898532830193251E-6,1.3898532830193251E-6,1.2843019795176516E-2,4.9482947237788743E-7,4.9482947237788743E-7,2.3662356457061398E-2,1.0358281592369152E-3,3.8136474548737705E-4,15,33.405828621139626,3.6932695651368062E-3,5.8577624906861114E-3,9.9323968013102955E-3,1.0970466755454256E-2,2.294030838016296E-2,3.9469331143273122E-4,1.0296848128159182E-3,0,5.2060970655913278E-5,1.0817457834718315E-3,1.4765540669294413E-3,1.4451508385963371E-2,1.9813496707515893E-2,1.4110495583032952E-3,3.3671567088202889E-2,3.3858105252787707E-2,0.18,0.84167957902382862,4.8540126777843005E-3,1.8461226100873413E-3,3.1670709285719384E-2,4.6443864213469292E-2,0,2.4343697702911658E-4,5.0582407535742935E-3,8.6341373999831029E-4,0,2.3138214555533533E-6,6.4989507008699548E-6,9.2647864265399962E-2,0.18363647729521843,0.84167957902382862,84.167957902382867,15,15.015319606822954,0.15015319606822955,127.12158182912569,null,2.7390883706568114E-2,null,3.3671567088202889E-2,1.9813496707515893E-2,1.8465348182942229E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR12, IF(MODE_ILIM=4,#REF!,#REF!))","v":84.167957902382867},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ12, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.3671567088202889E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA12, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.9813496707515893E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB12, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.8465348182942229E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S12, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":127.12158182912569},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P12, IF(MODE_ILIM=4,#REF!,#REF!))","v":42.84719226478979}]
["VDD",5,"V",{"$f":"B13","v":5},"Gate drive rail",null,null,7,1.7500000000000002E-2,0.11883900499999998,0.11883900499999998,0,41.756262183600711,2.5348603304390691,17,43.092625617464179,9.8583407925882194E-7,0.14830851213398,148308.51213398,6.7427013164059854E-6,0,6.6E-4,3.5597645127512935E-2,2.1542269756613875E-4,0,2.154301229322538E-4,1.8008306399302954E-2,1.6214954968558785E-6,1.6214954968558785E-6,1.4212305491665562E-2,6.0596888216528131E-7,6.0596888216528131E-7,2.5558266085251979E-2,1.2084661857764019E-3,4.4492553640194E-4,15,33.405828621139626,4.4574455548417264E-3,6.8340562391337985E-3,1.1736427330377466E-2,1.2947980395075746E-2,2.4778365025558163E-2,4.6047553000485306E-4,1.201298948285238E-3,0,6.2852387426141001E-5,1.2641513357113791E-3,1.7247835495599734E-3,1.6197924040564724E-2,2.2453577082376001E-2,1.6462244846871779E-3,3.87725655116989E-2,3.8990223099010173E-2,0.21000000000000002,0.8434066100518901,4.8658660152150228E-3,1.850001209346382E-3,3.173569398890131E-2,4.7136097089685774E-2,0,2.5242913815595058E-4,5.0771123459281099E-3,8.6518536705947914E-4,0,2.4337055271616816E-6,6.5122858105601034E-6,9.0178549193264526E-2,0.18196988033889427,0.8434066100518901,84.340661005189006,17.5,16.343061169118954,0.16343061169118955,148.30851213398,null,2.7447086693103837E-2,null,3.87725655116989E-2,2.2453577082376001E-2,2.154301229322538E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR13, IF(MODE_ILIM=4,#REF!,#REF!))","v":84.340661005189006},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ13, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.87725655116989E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA13, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.2453577082376001E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB13, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.154301229322538E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S13, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":148.30851213398},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P13, IF(MODE_ILIM=4,#REF!,#REF!))","v":43.092625617464179}]
["K1",400,"pC",4,"RT constant",null,null,8,0.02,0.11883900499999998,0.11883900499999998,0,41.604747032085562,2.392240788544143,18,43.060334193794574,9.8583407925882194E-7,0.16949544243883424,169495.44243883426,5.8998636518552377E-6,0,6.6E-4,3.8055483383747479E-2,2.4619736864701572E-4,0,2.4620706713214692E-4,1.9251689332068667E-2,1.8531377106924326E-6,1.8531377106924326E-6,1.5586609616575731E-2,7.2882719801859322E-7,7.2882719801859322E-7,2.7322935740290561E-2,1.3811042123158877E-3,5.0848632731650273E-4,15,33.405828621139626,5.2640875623129642E-3,7.810349987581483E-3,1.358292387721095E-2,1.4968106363236455E-2,2.6489186437160226E-2,5.2625774857697496E-4,1.3729130837545575E-3,0,7.4249455375083033E-5,1.4471625391296406E-3,1.9736251897276989E-3,1.6197924040564724E-2,2.3347241802634755E-2,1.8813994110710602E-3,4.2170372766669968E-2,4.2419161798710824E-2,0.24,0.8498006950783874,4.9047043309786787E-3,1.8641180267126678E-3,3.1976290544965119E-2,4.8094908966877875E-2,0,2.6290516161223864E-4,5.1241655485157189E-3,8.7174456251126644E-4,0,2.5806577477843083E-6,6.5616571442600033E-6,8.2668759633509156E-2,0.17577673909057479,0.8498006950783874,84.980069507838735,20,17.75180413241851,0.17751804132418511,169.49544243883426,null,2.7655170201050912E-2,null,4.2170372766669968E-2,2.3347241802634755E-2,2.4620706713214692E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR14, IF(MODE_ILIM=4,#REF!,#REF!))","v":84.980069507838735},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ14, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.2170372766669968E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA14, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.3347241802634755E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB14, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.4620706713214692E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S14, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":169.49544243883426},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P14, IF(MODE_ILIM=4,#REF!,#REF!))","v":43.060334193794574}]
["Outputs",null,null,null,null,null,null,9,2.2499999999999999E-2,0.11883900499999998,0.11883900499999998,0,41.453231880570407,2.2501801927420964,19,42.753423662099827,9.8583407925882194E-7,0.19068237274368852,190682.37274368852,5.2443232460935452E-6,0,6.6E-4,4.0363935542969735E-2,2.7697203972789264E-4,0,2.7698431443357925E-4,2.0419500114003706E-2,2.0847799245289868E-6,2.0847799245289868E-6,1.6973243250225614E-2,8.6427295929398818E-7,8.6427295929398818E-7,2.8980349715825603E-2,1.5537422388553733E-3,5.7204711823106557E-4,15,33.405828621139626,6.1131955875505222E-3,8.7866437360291667E-3,1.5471886441810755E-2,1.7030849015147228E-2,2.8096025036746075E-2,5.9203996714909674E-4,1.5445272192238773E-3,0,8.6252730659659919E-5,1.6307799498835372E-3,2.2230795674901402E-3,1.6197924040564724E-2,2.4240906522893506E-2,2.1165743374549429E-3,4.5611409442985813E-2,4.5891342810303215E-2,0.27,0.85472427828494957,4.9351228161787566E-3,1.8750106043972415E-3,3.216155507586882E-2,4.8978507306234792E-2,0,2.7304556653031097E-4,5.1624711692806391E-3,8.767952843019755E-4,0,2.7359817828657468E-6,6.5996741347258878E-6,7.6738116047233615E-2,0.17100995952594372,0.85472427828494957,85.472427828494958,22.5,19.240199150848532,0.19240199150848533,190.68237274368852,null,2.7815398984535191E-2,null,4.5611409442985813E-2,2.4240906522893506E-2,2.7698431443357925E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR15, IF(MODE_ILIM=4,#REF!,#REF!))","v":85.472427828494958},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ15, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.5611409442985813E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA15, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.4240906522893506E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB15, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.7698431443357925E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S15, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":190.68237274368852},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P15, IF(MODE_ILIM=4,#REF!,#REF!))","v":42.753423662099827}]
["Design","Value","Units","Std Units","Description",null,null,10,2.5000000000000001E-2,0.11883900499999998,0.11883900499999998,0,41.301716729055258,2.1087915077449777,20,42.17583015489955,9.8583407925882194E-7,0.21186930304854285,211869.30304854285,4.7198909214841902E-6,0,6.6E-4,4.2547323881336543E-2,3.0774671080876966E-4,0,3.0776186484102842E-4,2.1524043014106535E-2,2.3164221383655417E-6,2.3164221383655417E-6,1.8375461052179947E-2,1.0129727066405464E-6,1.0129727066405464E-6,3.0547970830074121E-2,1.72638026539486E-3,6.3560790914562852E-4,15,33.405828621139626,7.0047696305544013E-3,9.7629374844768538E-3,1.7403315024176885E-2,1.9136212706612442E-2,2.9615810771077861E-2,6.5782218572121853E-4,1.7161413546931974E-3,0,9.886276943679217E-5,1.8150041241299895E-3,2.4731472629349353E-3,1.6197924040564724E-2,2.5134571243152264E-2,2.351749263838826E-3,4.9095680476538464E-2,4.94067717362245E-2,0.30000000000000004,0.85859812764727172,4.9595423518115503E-3,1.8836015556727493E-3,3.2307320234045846E-2,4.9808178982046349E-2,0,2.8294462910817889E-4,5.1945304755002834E-3,8.8076916563338667E-4,0,2.89912156426454E-6,6.6295857028044772E-6,7.193498602862497E-2,0.16726140212971036,0.85859812764727172,85.859812764727167,25,20.80575856495858,0.20805758564958579,211.86930304854283,null,2.7941466148363969E-2,null,4.9095680476538464E-2,2.5134571243152264E-2,3.0776186484102842E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR16, IF(MODE_ILIM=4,#REF!,#REF!))","v":85.859812764727167},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ16, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.9095680476538464E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA16, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.5134571243152264E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB16, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.0776186484102842E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S16, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":211.86930304854283},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P16, IF(MODE_ILIM=4,#REF!,#REF!))","v":42.17583015489955}]
["On-Time",{"$f":"(Rt*k_RT/10000)/Vin","v":1},"µs",{"$f":"B17/1000000","v":9.9999999999999995E-7},"On Time - fixed",null,null,11,2.75E-2,0.11883900499999998,0.11883900499999998,0,41.150201577540102,1.9682195406914689,21,41.332610354520845,9.8583407925882194E-7,0.23305623335339709,233056.23335339711,4.2908099286219916E-6,0,6.6E-4,4.4624009752706958E-2,3.3852138188964658E-4,0,3.3853971835897192E-4,2.2574606761589872E-2,2.5480643522020958E-6,2.5480643522020958E-6,1.9793862533626114E-2,1.1753909820002629E-6,1.1753909820002629E-6,3.2038982100225426E-2,1.8990182919343458E-3,6.9916870006019125E-4,15,33.405828621139626,7.9388096913245981E-3,1.0739231232924539E-2,1.9377209624309329E-2,2.1284201794030077E-2,3.1061324382439342E-2,7.2360440429334054E-4,1.8877554901625168E-3,0,1.1208012786340024E-4,1.9998356180259171E-3,2.7238288561798377E-3,1.6197924040564724E-2,2.6028235963411014E-2,2.5869241902227082E-3,5.2623190803843638E-2,5.2965453977536811E-2,0.33,0.86169652268258234,4.9795409740341851E-3,1.8904922901907156E-3,3.2423906605939821E-2,5.059780046229944E-2,0,2.9266380739912485E-4,5.2219739333021382E-3,8.839475685697302E-4,0,3.0691827938851278E-6,6.6535096723151287E-6,6.7964970973433347E-2,0.16426501930763471,0.86169652268258234,86.169652268258233,27.5,22.444784059665849,0.22444784059665848,233.05623335339712,null,2.8042297605137139E-2,null,5.2623190803843638E-2,2.6028235963411014E-2,3.3853971835897192E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR17, IF(MODE_ILIM=4,#REF!,#REF!))","v":86.169652268258233},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ17, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.2623190803843638E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA17, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.6028235963411014E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB17, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.3853971835897192E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S17, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":233.05623335339712},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P17, IF(MODE_ILIM=4,#REF!,#REF!))","v":41.332610354520845}]
["Off Time",{"$f":"L*Iripple*1000000/(Vout+(Rdcr+RdsonBot)*Iout)","v":0.93990188062142266},"µs",{"$f":"B18/1000000","v":9.3990188062142269E-7},"Off Time - depends on Vout, L, Iout, DCR, etc.",null,null,12,0.03,0.11883900499999998,0.11883900499999998,0,40.998686426024953,1.8286526492136392,23,42.059010931913704,9.8583407925882194E-7,0.25424316365825134,254243.16365825137,3.9332424345701593E-6,0,6.600000000000001E-4,4.6608258102572554E-2,3.6929605297052344E-4,0,3.6931787499188757E-4,2.3578407775075267E-2,2.7797065660386494E-6,2.7797065660386494E-6,2.1227264925154234E-2,1.3517903286080496E-6,1.3517903286080496E-6,3.3463625419282814E-2,2.0716563184738314E-3,7.6272949097475409E-4,15,33.405828621139626,8.9153157698611159E-3,1.1715524981372223E-2,2.1393570242208095E-2,2.3474820634391842E-2,3.2442495236247627E-2,7.8938662286546243E-4,2.0593696256318364E-3,0,1.2590536209640464E-4,2.1852749877282408E-3,2.9751249273727198E-3,1.6197924040564728E-2,2.6921900683669772E-2,2.8220991166065905E-3,5.619394536204092E-2,5.6567394733927454E-2,0.36,0.86420589933578806,4.9961912970003242E-3,1.8960916039743748E-3,3.251832940108975E-2,5.1356804475474443E-2,0,3.0224487967144838E-4,5.2459098224046877E-3,8.8652174327374456E-4,0,3.2450699351337219E-6,6.6728855910917396E-6,6.4627959422665568E-2,0.16183997060108057,0.86420589933578806,86.42058993357881,30,24.152326085424395,0.24152326085424394,254.24316365825138,null,2.812396056310465E-2,null,5.619394536204092E-2,2.6921900683669772E-2,3.6931787499188757E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR18, IF(MODE_ILIM=4,#REF!,#REF!))","v":86.42058993357881},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ18, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.619394536204092E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA18, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.6921900683669772E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB18, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.6931787499188757E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S18, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":254.24316365825138},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P18, IF(MODE_ILIM=4,#REF!,#REF!))","v":42.059010931913704}]
["DIL",{"$f":"(Vin-Vout-(Rdcr+RdsonTop)*Iout)/L*OnTime*1000","v":114.94999999999999},"mA",{"$f":"B19/1000","v":0.11494999999999998},"Inductor pk-pk ripple current in CCM",null,null,13,3.2500000000000001E-2,0.11883900499999998,0.11883900499999998,0,40.847171274509805,1.6903398109511314,25,42.258495273778287,9.8583407925882194E-7,0.27543009396310569,275430.0939631057,3.6306853242186077E-6,0,6.5999999999999989E-4,4.8511413093233598E-2,4.0007072405140058E-4,0,4.000963347442536E-4,2.4541184893461049E-2,3.0113487798752043E-6,3.0113487798752043E-6,2.2673268335139621E-2,1.542231290991735E-6,1.542231290991735E-6,3.4830045627095824E-2,2.2442943450133174E-3,8.2629028188931715E-4,15,33.405828621139626,9.934287866163953E-3,1.269181872981991E-2,2.3452396877873181E-2,2.5708073585283289E-2,3.3767219635569327E-2,8.5516884143758401E-4,2.2309837611011567E-3,0,1.4033902829272592E-4,2.3713227893938827E-3,3.2270360566915767E-3,1.6197924040564721E-2,2.781556540392852E-2,3.0572740429904736E-3,5.9807949088893857E-2,6.0212599003708976E-2,0.39,0.8662574100836905,5.0102478526850933E-3,1.9006870735988543E-3,3.2595523623347951E-2,5.2091827127387816E-2,0,3.1171723892953467E-4,5.2671177897763519E-3,8.8862622888993099E-4,0,3.4255622663705811E-6,6.6887261408035272E-6,6.1783178581591332E-2,0.15985903980461405,0.8662574100836905,86.625741008369047,32.5,25.922181532084487,0.25922181532084487,275.43009396310572,null,2.8190723133706332E-2,null,5.9807949088893857E-2,2.781556540392852E-2,4.000963347442536E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR19, IF(MODE_ILIM=4,#REF!,#REF!))","v":86.625741008369047},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ19, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9807949088893857E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA19, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.781556540392852E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB19, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.000963347442536E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S19, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":275.43009396310572},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P19, IF(MODE_ILIM=4,#REF!,#REF!))","v":42.258495273778287}]
["CCM Freq",{"$f":"'Design Converter'!E12","v":500},"kHz",{"$f":"B20*1000","v":500000},"Frequency in CCM",{"$f":"10000*Vout/(k_RT*Rt/1000+Vin*0.75)","v":465.11627906976742},null,14,3.5000000000000003E-2,0.11883900499999998,0.11883900499999998,0,40.695656122994656,1.5536159935423151,27,41.947631825642503,9.8583407925882194E-7,0.29661702426795999,296617.02426795999,3.3713506582029927E-6,0,6.6E-4,5.0342672527873319E-2,4.308453951322775E-4,0,4.3087509762054739E-4,2.5467591145264441E-2,3.2429909937117584E-6,3.2429909937117584E-6,2.4128630400225518E-2,1.746572414972061E-6,1.746572414972061E-6,3.6144846528503659E-2,2.4169323715528038E-3,8.8985107280387999E-4,15,33.405828621139626,1.0995725980233113E-2,1.3668112478267597E-2,2.5553689531304588E-2,2.7983965004883871E-2,3.504189987257552E-2,9.2095106000970623E-4,2.4025978965704761E-3,0,1.5538168260928456E-4,2.5579795791797607E-3,3.4795628243445226E-3,1.6197924040564724E-2,2.8709230124187277E-2,3.2924489693743559E-3,6.3465206922790035E-2,6.3901071583819261E-2,0.42000000000000004,0.8679460010810276,5.0222568543296158E-3,1.9044868864381698E-3,3.2659061905506548E-2,5.2807672956099845E-2,0,3.2110216681421422E-4,5.2861622538000067E-3,8.9035842330770351E-4,0,3.6093584361272223E-6,6.7017644393664487E-6,5.9328717810484093E-2,0.15823013037965569,0.8679460010810276,86.794600108102756,35,27.746934669307642,0.27746934669307644,296.61702426796001,null,2.8245675161519174E-2,null,6.3465206922790035E-2,2.8709230124187277E-2,4.3087509762054739E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR20, IF(MODE_ILIM=4,#REF!,#REF!))","v":86.794600108102756},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ20, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.3465206922790035E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA20, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.8709230124187277E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB20, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.3087509762054739E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S20, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":296.61702426796001},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P20, IF(MODE_ILIM=4,#REF!,#REF!))","v":41.947631825642503}]
["Icrit_Skip",{"$f":"1000*Iripple/2","v":57.474999999999994},"mA",{"$f":"Iripple/2","v":5.7474999999999991E-2},"CCM-DCM (critical conduction) boundary",null,null,15,3.7499999999999999E-2,0.11883900499999998,0.11883900499999998,0,40.5441409714795,1.4189406077030025,29,41.149277623387079,9.8583407925882194E-7,0.31780395457281418,317803.95457281423,3.1465939476561272E-6,0,6.6E-4,5.21096167151038E-2,4.6162006621315431E-4,0,4.6165416362524712E-4,2.6361461293138936E-2,3.474633207548312E-6,3.474633207548312E-6,2.5589517695485425E-2,1.9644702476626853E-6,1.9644702476626853E-6,3.741347060555314E-2,2.5895703980922894E-3,9.5341186371844262E-4,15,33.405828621139626,1.2099630112068582E-2,1.4644406226715279E-2,2.7697448202502306E-2,3.0302499251967079E-2,3.6271812353981386E-2,9.8673327858182737E-4,2.5742120320397955E-3,0,1.7103388120300099E-4,2.7452459132427964E-3,3.7327058105697973E-3,1.6197924040564724E-2,2.9602894844446028E-2,3.5276238957582381E-3,6.7165723802741148E-2,6.7632817069821605E-2,0.44999999999999996,0.86934209957422603,5.0326234418661044E-3,1.9076454675280106E-3,3.2711594283164565E-2,5.3507906162692735E-2,0,3.3041545196299034E-4,5.303461880146792E-3,8.917905723718597E-4,0,3.795103754787064E-6,6.7125442842230609E-6,5.7188983905657208E-2,0.15688492881342928,0.86934209957422603,86.93420995742261,37.5,29.618044224570543,0.29618044224570544,317.80395457281423,null,2.8291108569223403E-2,null,6.7165723802741148E-2,2.9602894844446028E-2,4.6165416362524712E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR21, IF(MODE_ILIM=4,#REF!,#REF!))","v":86.93420995742261},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ21, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.7165723802741148E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA21, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.9602894844446028E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB21, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.6165416362524712E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S21, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":317.80395457281423},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P21, IF(MODE_ILIM=4,#REF!,#REF!))","v":41.149277623387079}]
["Tr",null,"ns",{"$f":"B22/1000000000","v":0},"Switch rise time",null,null,16,0.04,0.11883900499999998,0.11883900499999998,0,40.392625819964351,1.286956897056222,32,41.182620705799103,9.8583407925882194E-7,0.33899088487766849,338990.88487766852,2.9499318259276189E-6,0,6.6E-4,5.3818580723959647E-2,4.9239473729403133E-4,0,4.9243353276283127E-4,2.7226000152004944E-2,3.706275421384866E-6,3.706275421384866E-6,2.7051674855543821E-2,2.1953793374701851E-6,2.1953793374701851E-6,3.8640466287767468E-2,2.7622084246317746E-3,1.0169726546330055E-3,15,33.405828621139626,1.3246000261670377E-2,1.5620699975162966E-2,2.9883672891466349E-2,3.2663680685900538E-2,3.7461366715661429E-2,1.0525154971539495E-3,2.7458261675091149E-3,0,1.8729618023079583E-4,2.9331223477399109E-3,3.9864655956357697E-3,1.6197924040564724E-2,3.0496559564704782E-2,3.7627988221421204E-3,7.0909504668383208E-2,7.1407839855904889E-2,0.48,0.87049904862693761,5.0416544588134026E-3,1.9102797816061533E-3,3.2755127948492779E-2,5.4195226711458461E-2,0,3.3966905562993167E-4,5.3193337775291711E-3,8.929773965903441E-4,0,3.9814075513396514E-6,6.7214775588852672E-6,5.5306721015563019E-2,0.1557716930307935,0.87049904862693761,87.049904862693765,40,31.525976771075946,0.31525976771075948,338.99088487766852,null,2.8328759306804563E-2,null,7.0909504668383208E-2,3.0496559564704782E-2,4.9243353276283127E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR22, IF(MODE_ILIM=4,#REF!,#REF!))","v":87.049904862693765},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ22, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0909504668383208E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA22, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.0496559564704782E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB22, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.9243353276283127E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S22, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":338.99088487766852},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P22, IF(MODE_ILIM=4,#REF!,#REF!))","v":41.182620705799103}]
["Tf",null,"ns",{"$f":"B23/1000000000","v":0},"Switch fall time",null,null,17,4.2500000000000003E-2,0.11883900499999998,0.11883900499999998,0,40.241110668449195,1.1585851179203517,35,40.550479127212306,9.8583407925882194E-7,0.36017781518252279,360177.81518252281,2.776406424402465E-6,0,6.6E-4,5.5474923236429052E-2,5.231694083749083E-4,0,5.2321320503777768E-4,2.8063918597449718E-2,3.9379176352214209E-6,3.9379176352214209E-6,2.8510537432640877E-2,2.4385522340940499E-6,2.4385522340940499E-6,3.9829680981895904E-2,2.9348464511712606E-3,1.0805334455475683E-3,15,33.405828621139626,1.4434836429038495E-2,1.6596993723610651E-2,3.2112363598196719E-2,3.5067513666646108E-2,3.8614292962167458E-2,1.1182977157260714E-3,2.9174403029784352E-3,0,2.0416913584958953E-4,3.1216094388280247E-3,4.2408427598409357E-3,1.6197924040564724E-2,3.139022428496354E-2,3.9979737485260035E-3,7.4696554459976583E-2,7.5226144134883682E-2,0.51,0.87145799125893886,5.0495865539600393E-3,1.9124800425097696E-3,3.279121103055474E-2,5.4871717403649378E-2,0,3.4887220589128765E-4,5.3340225314823797E-3,8.9396110139318636E-4,0,4.1668545715756829E-6,6.7288819453592361E-6,5.3637768236356645E-2,0.15485051484231438,0.87145799125893886,87.145799125893888,42.5,33.460383546927204,0.33460383546927203,360.17781518252281,null,2.8359966296695988E-2,null,7.4696554459976583E-2,3.139022428496354E-2,5.2321320503777768E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR23, IF(MODE_ILIM=4,#REF!,#REF!))","v":87.145799125893888},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ23, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.4696554459976583E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA23, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.139022428496354E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB23, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.2321320503777768E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S23, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":360.17781518252281},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P23, IF(MODE_ILIM=4,#REF!,#REF!))","v":40.550479127212306}]
[null,null,null,null,null,null,null,18,4.4999999999999998E-2,0.11883900499999998,0.11883900499999998,0,40.08959551693404,1.0351698942426668,39,40.371625875463998,9.8583407925882194E-7,0.38136474548737703,381364.74548737705,2.6221616230467726E-6,0,6.6E-4,5.7083225075621219E-2,5.5394407945578527E-4,0,5.5399318045456472E-4,2.8877533998103007E-2,4.1695598490579754E-6,4.1695598490579754E-6,2.9961305537457728E-2,2.6930394885266855E-6,2.6930394885266855E-6,4.0984403610435836E-2,3.1074844777107462E-3,1.1440942364621311E-3,15,33.405828621139626,1.5666138614172924E-2,1.7573287472058333E-2,3.4383520322693387E-2,3.7514002554759951E-2,3.9733779655740334E-2,1.1840799342981933E-3,3.0890544384477546E-3,0,2.2165330421630253E-4,3.310707742664057E-3,4.4958378835139173E-3,1.6197924040564724E-2,3.2283889005222291E-2,4.2331486749098857E-3,7.8526878118406043E-2,7.908773389819819E-2,0.54,0.87225116963599336,5.0566051637865846E-3,1.9143169472725188E-3,3.2821056737184023E-2,5.553901077346713E-2,0,3.5803213677102321E-4,5.3477198164104869E-3,8.9477476151526348E-4,0,4.3500126735987383E-6,6.7350063985335084E-6,5.2147518417043938E-2,0.1540901197725231,0.87225116963599336,87.225116963599334,45,35.410314704487,0.35410314704487,381.36474548737704,null,2.8385778799726719E-2,null,7.8526878118406043E-2,3.2283889005222291E-2,5.5399318045456472E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR24, IF(MODE_ILIM=4,#REF!,#REF!))","v":87.225116963599334},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ24, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.8526878118406043E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA24, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.2283889005222291E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB24, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.5399318045456472E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S24, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":381.36474548737704},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P24, IF(MODE_ILIM=4,#REF!,#REF!))","v":40.371625875463998}]
["Components","Input Value","Units","Std Units","Description",null,null,19,4.7500000000000001E-2,0.11883900499999998,0.11883900499999998,0,39.938080365418891,0.91871092206425564,44,40.423280570827252,9.8583407925882194E-7,0.40255167579223139,402551.6757922314,2.4841531165706262E-6,0,6.6E-4,5.8647438665131543E-2,5.8471875053666225E-4,0,5.847734590176709E-4,2.9668845824853143E-2,4.401202062894529E-6,4.401202062894529E-6,3.1398989649633703E-2,2.9576896530534136E-6,2.9576896530534136E-6,4.2107471919917164E-2,3.2801225042502335E-3,1.2076550273766942E-3,15,33.405828621139626,1.6939906817073677E-2,1.8549581220506022E-2,3.6697143064956389E-2,4.0003151711392695E-2,4.0822577950121598E-2,1.2498621528703156E-3,3.2606685739170744E-3,0,2.3974924148785549E-4,3.5004178154049298E-3,4.7514515470134765E-3,1.6197924040564724E-2,3.3177553725481049E-2,4.4683236012937689E-3,8.2400480585180999E-2,8.2992612935914617E-2,0.57000000000000006,0.87290420857477657,5.0628576509804428E-3,1.9158466831405399E-3,3.2845629278680691E-2,5.6198404603633519E-2,0,3.6715459981992893E-4,5.3605779698896287E-3,8.954446634667322E-4,0,4.5294381505410447E-6,6.740048778050215E-6,5.0808467152961688E-2,0.15346565208950178,0.87290420857477657,87.290420857477656,47.5,37.364462120689176,0.37364462120689174,402.55167579223138,null,2.8407030727507623E-2,null,8.2400480585180999E-2,3.3177553725481049E-2,5.847734590176709E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR25, IF(MODE_ILIM=4,#REF!,#REF!))","v":87.290420857477656},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ25, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.2400480585180999E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA25, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.3177553725481049E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB25, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.847734590176709E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S25, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":402.55167579223138},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P25, IF(MODE_ILIM=4,#REF!,#REF!))","v":40.423280570827252}]
["L",{"$f":"'Design Converter'!E17","v":100},"µH",{"$f":"B26/1000000","v":1E-4},"Filter inductance",null,null,20,0.05,0.11883900499999998,0.11883900499999998,0,39.786565213903742,0.81220602102413542,49,39.798095030182637,9.8583407925882194E-7,0.42373860609708569,423738.60609708569,2.3599454607420951E-6,0,6.6E-4,6.017100247566682E-2,6.1549342161753944E-4,0,6.1555404073157472E-4,3.0439593547651331E-2,4.6328442767310835E-6,4.6328442767310835E-6,3.281843628842622E-2,3.2311492812524728E-6,3.2311492812524728E-6,4.3201354650868509E-2,3.4527605307897191E-3,1.271215818291257E-3,15,33.405828621139626,1.8256141037740755E-2,1.9525874968953708E-2,3.9053231824985719E-2,4.2534965498289501E-2,4.1883081253133503E-2,1.3156443714424373E-3,3.4322827093863947E-3,0,2.5845750382116878E-4,3.6907402132075637E-3,5.0076843307285037E-3,1.6197924040564724E-2,3.40712184457398E-2,4.703498527677652E-3,8.6317366802435458E-2,8.6940784836725016E-2,0.60000000000000009,0.87343773036071892,5.0684625955515726E-3,1.9171144683656494E-3,3.2865704630158005E-2,5.6850943614110867E-2,0,3.7624422588709746E-4,5.3727195919584161E-3,8.9599196204929435E-4,0,4.7036794911230457E-6,6.744168316971072E-6,4.9598479516452049E-2,0.15295710845234106,0.87343773036071892,87.343773036071894,50,39.311419610679415,0.39311419610679416,423.73860609708566,null,2.8424393193650161E-2,null,8.6317366802435458E-2,3.40712184457398E-2,6.1555404073157472E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR26, IF(MODE_ILIM=4,#REF!,#REF!))","v":87.343773036071894},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ26, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.6317366802435458E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA26, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.40712184457398E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB26, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1555404073157472E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S26, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":423.73860609708566},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P26, IF(MODE_ILIM=4,#REF!,#REF!))","v":39.798095030182637}]
["Rdcr",{"$f":"'Design Converter'!E18","v":170},"mW",{"$f":"B27/1000","v":0.17},"Inductor DCR at 25°C",null,null,21,5.2499999999999998E-2,0.11883900499999998,0.11883900499999998,0,39.635050062388594,0.7200856176521544,56,40.324794588520646,9.8583407925882194E-7,0.44492553640193988,444925.53640193993,2.2475671054686624E-6,0,6.6E-4,6.1656929990659082E-2,6.4626809269841608E-4,0,6.4633492560075406E-4,3.1191301641860465E-2,4.8644864905676371E-6,4.8644864905676371E-6,3.4214338748517974E-2,3.5118629279950152E-6,3.5118629279950152E-6,4.4268215413020937E-2,3.6253985573292055E-3,1.3347766092058197E-3,15,33.405828621139626,1.9614841276174143E-2,2.0502168717401393E-2,4.1451786602781357E-2,4.5109448277790121E-2,4.2917387152754442E-2,1.381426590014559E-3,3.6038968448557137E-3,0,2.777786473731629E-4,3.8816754922288768E-3,5.2645368150780253E-3,1.6197924040564724E-2,3.496488316599855E-2,4.9386734540615334E-3,9.0277541712928219E-2,9.0932252987947534E-2,0.63,0.87386851869773718,5.0735164918053847E-3,1.9181571043850455E-3,3.2881914328629254E-2,5.7497478342773418E-2,0,3.8530478588229673E-4,5.3842444642212038E-3,8.9643387436186793E-4,0,4.871280086915083E-6,6.7474946091071349E-6,4.8499540728112064E-2,0.15254820889486653,0.87386851869773718,87.386851869773722,52.5,41.239947953148963,0.41239947953148964,444.92553640193995,null,2.8438412392328003E-2,null,9.0277541712928219E-2,3.496488316599855E-2,6.4633492560075406E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR27, IF(MODE_ILIM=4,#REF!,#REF!))","v":87.386851869773722},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ27, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0277541712928219E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA27, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.496488316599855E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB27, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.4633492560075406E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S27, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":444.92553640193995},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P27, IF(MODE_ILIM=4,#REF!,#REF!))","v":40.324794588520646}]
["Kcore",0,null,{"$f":"B28","v":0},"Core loss constant - consult inductor vendor",null,null,22,5.5E-2,0.11883900499999998,0.11883900499999998,0,39.483534910873438,0.64850889493131336,61,39.559042590810115,9.8583407925882194E-7,0.46611246670679418,466112.46670679422,2.1454049643109958E-6,0,6.6E-4,6.3107879799747441E-2,6.7704276377929316E-4,0,6.7711611362968863E-4,3.1925315047479766E-2,5.0961287044041899E-6,5.0961287044041899E-6,3.558123639150796E-2,3.7980731494451112E-6,3.7980731494451112E-6,4.5309963010767618E-2,3.7980365838686902E-3,1.3983374001203825E-3,15,33.405828621139626,2.101600753237386E-2,2.1478462465849078E-2,4.3892807398343323E-2,4.7726604412829096E-2,4.3927346206915817E-2,1.4472088085866811E-3,3.7755109803250335E-3,0,2.9771322830075847E-4,4.0732242086257923E-3,5.5220095805112125E-3,1.6197924040564724E-2,3.5858547886257308E-2,5.1738483804454165E-3,9.4281010260043027E-2,9.496702057552657E-2,0.66,0.87421037212575026,5.0780986586184823E-3,1.9190048471004494E-3,3.2894777585391978E-2,5.8138708317196364E-2,0,3.9433938196903714E-4,5.3952346229914671E-3,8.9678455525536705E-4,0,5.0307802141473191E-6,6.7501341986028847E-6,4.7496840138687935E-2,0.15222556902162382,0.87421037212575026,87.42103721257503,55,43.139231734149426,0.43139231734149425,466.11246670679424,null,2.844953737114982E-2,null,9.4281010260043027E-2,3.5858547886257308E-2,6.7711611362968863E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR28, IF(MODE_ILIM=4,#REF!,#REF!))","v":87.42103721257503},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ28, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.4281010260043027E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA28, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.5858547886257308E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB28, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.7711611362968863E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S28, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":466.11246670679424},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P28, IF(MODE_ILIM=4,#REF!,#REF!))","v":39.559042590810115}]
["Cin",{"$f":"'Design Converter'!E37","v":2.2000000000000002},"µF",{"$f":"B29/1000000","v":2.2000000000000001E-6},"Input capacitance",null,null,23,5.7500000000000002E-2,0.11883849999999999,0.11629973115,-1.3253727153849856E-3,1.0786982025226954,1.0786982025226954,1,1.0786982025226954,9.859743298293358E-7,0.50353118113361262,503531.18113361258,1.9859743298293355E-6,0,6.6E-4,6.638806525523494E-2,7.4925378541666667E-4,0,7.4934361718334704E-4,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,3.7161433641648874E-2,4.1429164509080184E-6,4.1429164509080184E-6,4.7108925315178705E-2,4.1056140620495075E-3,1.5105935434008377E-3,15,33.398564905414226,2.3204982716951972E-2,2.3202716826636868E-2,4.791829308698968E-2,5.2066078357763654E-2,4.5671413840347279E-2,1.5644085316321985E-3,4.0786025671822618E-3,4.2296619215242272E-7,3.2893349428697675E-4,4.4079590276613909E-3,5.9742113593260118E-3,1.6197924040564724E-2,3.7436869260780506E-2,5.5891961105830994E-3,0.10106635508845328,0.10182534724812921,0.69000000000000006,0.8714042842881855,5.2382577612461916E-3,1.9780275247665373E-3,3.3881387384271142E-2,6.0516240422869197E-2,5.3416601731982765E-7,4.1541167560515203E-4,5.5668324372042319E-3,9.4623617192931035E-4,0,5.2321089054626831E-6,6.9530813339086016E-6,4.7279200382870736E-2,0.15583431311701917,0.8714042842881855,87.140428428818552,57.5,44.999115697666738,0.44999115697666736,503.53118113361256,null,2.9302821521531793E-2,null,0.10106635508845328,3.7436869260780506E-2,7.4934361718334704E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR29, IF(MODE_ILIM=4,#REF!,#REF!))","v":87.140428428818552},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ29, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10106635508845328},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA29, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7436869260780506E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB29, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.4934361718334704E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S29, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":503.53118113361256},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P29, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0786982025226954}]
["RCinESR",{"$f":"'Design Converter'!E39","v":3},"mW",{"$f":"B30/1000","v":3.0000000000000001E-3},"Input capacitor ESR",null,null,24,0.06,0.11878799999999996,0.11880024119999999,1.1998824361199936E-3,1.0782398135390965,1.0782398135390965,1,1.0782398135390965,9.853673103722872E-7,0.50368513411882687,503685.13411882689,1.9853673103722869E-6,0,6.5999999999999989E-4,6.8564751938101062E-2,7.9919128541666674E-4,0,7.9929349155953783E-4,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,3.8138845151269203E-2,4.3637145284174716E-6,4.3637145284174716E-6,4.8660937938646155E-2,4.3805907299772299E-3,1.5110554023564805E-3,15,32.687805916152371,2.3438735873652552E-2,2.3209810980195544E-2,4.8159602256204581E-2,5.2585637648798124E-2,4.7176067371235329E-2,1.6691859994615009E-3,4.0798495863624985E-3,4.2732646778641383E-5,3.4334438887642269E-4,4.4659266220175627E-3,6.137133561235136E-3,1.6197924040564721E-2,3.7443362997696843E-2,5.5909049887189789E-3,0.10175703919644907,0.10256620202857869,0.72,0.87530948660954688,5.380764954453803E-3,2.0316990110900643E-3,3.2625147835722429E-2,5.8547995453053343E-2,5.1950404323999576E-5,4.1740638994123636E-4,5.4292610260473625E-3,9.7158293575123108E-4,0,5.3050010049718304E-6,6.6932315333269442E-6,4.5520181725623513E-2,0.15098798796854529,0.87530948660954688,87.530948660954692,60,46.810309970062292,0.46810309970062292,503.68513411882691,null,2.8216344074138311E-2,null,0.10175703919644907,3.7443362997696843E-2,7.9929349155953783E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR30, IF(MODE_ILIM=4,#REF!,#REF!))","v":87.530948660954692},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ30, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10175703919644907},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA30, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7443362997696843E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB30, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.9929349155953783E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S30, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":503.68513411882691},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P30, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0782398135390965}]
["Cout",{"$f":"'Design Converter'!E24","v":33},"µF",{"$f":"B31/1000000","v":3.3000000000000003E-5},"Output capacitance",null,null,25,6.25E-2,0.1187375,0.12130075124999999,3.7251375876250076E-3,1.0777814245554982,1.0777814245554982,1,1.0777814245554982,9.847605224963715E-7,0.50383912248628893,503839.12248628895,1.9847605224963712E-6,0,6.6E-4,7.0762809500000301E-2,8.5125378541666666E-4,0,8.5136974249124019E-4,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,3.9131763122003616E-2,4.5938846551098061E-6,4.5938846551098061E-6,5.022859276275083E-2,4.6673863322135908E-3,1.5115173674588669E-3,15,32.006668055844962,2.3672629250457041E-2,2.3216906764168193E-2,4.84010533820841E-2,5.3117349212044807E-2,4.8695885786779448E-2,1.7784669694193014E-3,4.081096892138941E-3,8.5068197440585168E-5,3.577728737680988E-4,4.5239379633476252E-3,6.304616945221172E-3,1.6197924040564724E-2,3.7449858227036392E-2,5.5926142595978078E-3,0.10246443864390017,0.10332590789708819,0.75,0.87891389803021269,5.5269572695658686E-3,2.0867513401319326E-3,3.1458728954127754E-2,5.6720477995754595E-2,9.9690161347877959E-5,4.1926873479065458E-4,5.3015359330836299E-3,9.9757171033804885E-4,0,5.383505425764985E-6,6.451961660503864E-6,4.3886934500004512E-2,0.14650975206623118,0.87891389803021269,87.891389803021269,62.5,48.564555994658186,0.48564555994658187,503.83912248628894,null,2.7207549365732105E-2,null,0.10246443864390017,3.7449858227036392E-2,8.5136974249124019E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR31, IF(MODE_ILIM=4,#REF!,#REF!))","v":87.891389803021269},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ31, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10246443864390017},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA31, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7449858227036392E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB31, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.5136974249124019E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S31, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":503.83912248628894},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P31, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0777814245554982}]
["RCoutESR",{"$f":"'Design Converter'!E26","v":5.0000000000000001E-3},"mW",{"$f":"B32","v":5.0000000000000001E-3},"Output capacitor ESR",null,null,26,6.5000000000000002E-2,0.118687,0.12380126130000001,6.2503927391300076E-3,1.0773230355718995,1.0773230355718995,1,1.0773230355718995,9.8415396606908922E-7,0.50399314624819769,503993.14624819771,1.9841539660690892E-6,0,6.6E-4,7.2980306989853999E-2,9.0544128541666664E-4,0,9.0557247624977605E-4,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,4.0139035733553256E-2,4.8334265688583959E-6,4.8334265688583959E-6,5.1810525967796874E-2,4.9660116119605449E-3,1.5119794387445931E-3,15,31.353337415799146,2.3906662895710137E-2,2.322400417911695E-2,4.8642646513571683E-2,5.3661229751715091E-2,5.0229546883738631E-2,1.8922555351092731E-3,4.0823444846104021E-3,1.274296270973945E-4,3.7221896007302277E-4,4.5819930717808195E-3,6.4766663734677418E-3,1.6197924040564724E-2,3.7456354949313708E-2,5.5943239233549949E-3,0.10318857499785153,0.10410448652671182,0.78,0.88224866165344762,5.6764594169851886E-3,2.1430422880561618E-3,3.0372829502989591E-2,5.5019115110103024E-2,1.4413412559189E-4,4.2101240944418257E-4,5.1826375067743555E-3,1.0241337977751684E-3,0,5.4670309250968402E-6,6.2273477010574142E-6,4.2366434646728859E-2,0.14236149318307456,0.88224866165344762,88.224866165344764,65,50.254747979561841,0.50254747979561842,503.99314624819772,null,2.6268393083666672E-2,null,0.10318857499785153,3.7456354949313708E-2,9.0557247624977605E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR32, IF(MODE_ILIM=4,#REF!,#REF!))","v":88.224866165344764},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ32, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10318857499785153},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA32, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7456354949313708E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB32, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0557247624977605E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S32, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":503.99314624819772},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P32, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0773230355718995}]
["Controller",null,"Units","Std Units","Description",null,null,27,6.7500000000000004E-2,0.11863649999999998,0.12630177135000001,8.7756478906350147E-3,1.0768646465883005,1.0768646465883005,1,1.0768646465883005,9.8354764095804191E-7,0.50414720541675806,504147.20541675814,1.9835476409580419E-6,0,6.5999999999999989E-4,7.5215525048578452E-2,9.6175378541666658E-4,0,9.6190180344877315E-4,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,4.1159608018376377E-2,5.0823399966791792E-6,5.0823399966791792E-6,5.3405523134553226E-2,5.2764773173593054E-3,1.5124416162502743E-3,15,30.726145229045805,2.4140836857778757E-2,2.3231103225604215E-2,4.8884381699633245E-2,5.4217296156040956E-2,5.1775873300436558E-2,2.0105557920171444E-3,4.0835923638757416E-3,1.6981694467258103E-4,3.8668265890732118E-4,4.6400919674556441E-3,6.6532867354017764E-3,1.6197924040564721E-2,3.746285316504358E-2,5.5960339801260162E-3,0.10392947003661233,0.10490195980609945,0.81,0.88534076391274552,5.8289463687868229E-3,2.2004486342698409E-3,2.9359389622793768E-2,5.3431278811550034E-2,1.856121771873473E-4,4.2264928472693743E-4,5.0716821815957698E-3,1.0512096679960077E-3,0,5.5550651544743757E-6,6.0177224266013204E-6,4.0947396345050242E-2,0.13851018588153785,0.88534076391274552,88.534076391274553,67.5,51.875007795911799,0.51875007795911798,504.14720541675814,null,2.5391904538632444E-2,null,0.10392947003661233,3.746285316504358E-2,9.6190180344877315E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR33, IF(MODE_ILIM=4,#REF!,#REF!))","v":88.534076391274553},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ33, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10392947003661233},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA33, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.746285316504358E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB33, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.6190180344877315E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S33, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":504.14720541675814},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P33, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0768646465883005}]
["Deadtime1",7,"ns",{"$f":"B34/1000000000","v":6.9999999999999998E-9},"PMOS off to NMOS on deadtime",null,null,28,7.0000000000000007E-2,0.11858599999999998,0.1288022814,1.1300903042140022E-2,1.0764062576047018,1.0764062576047018,1,1.0764062576047018,9.8294154703093384E-7,0.50430130000418005,504301.30000418011,1.9829415470309338E-6,0,6.6E-4,7.7466929772215282E-2,1.020191285416667E-3,0,1.020357839044731E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,4.2192513770092165E-2,5.3406246547182509E-6,5.3406246547182509E-6,5.5012500798003683E-2,5.5987942014931588E-3,1.5129039000125403E-3,15,30.123553637968229,2.4375151185052044E-2,2.3238203904192619E-2,4.9126258989257203E-2,5.4785565497987992E-2,5.3333814633392262E-2,2.133371837511785E-3,4.0848405300338599E-3,2.122301590937594E-4,4.0116398139223143E-4,4.6982346705198514E-3,6.8344829477784159E-3,1.6197924040564724E-2,3.7469352874741041E-2,5.5977444300464004E-3,0.10468714575055385,0.10571834984029496,0.84000000000000008,0.88821370563641089,5.9841352445857542E-3,2.2588630934562244E-3,2.8411390419526238E-2,5.1945972072502594E-2,2.2441159054342031E-4,4.2418969819077386E-4,4.9679005079189273E-3,1.0787474786641798E-3,0,5.6471619225958035E-6,5.8216339384727049E-6,3.9619991386514335E-2,0.13492707028776352,0.88821370563641089,88.821370563641082,70,53.420714247122767,0.53420714247122769,504.30130000418012,null,2.4572013335806473E-2,null,0.10468714575055385,3.7469352874741041E-2,1.020357839044731E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR34, IF(MODE_ILIM=4,#REF!,#REF!))","v":88.821370563641082},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ34, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10468714575055385},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA34, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7469352874741041E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB34, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.020357839044731E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S34, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":504.30130000418012},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P34, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0764062576047018}]
["Deadtime2",7,"ns",{"$f":"B35/1000000000","v":6.9999999999999998E-9},"NMOS off to PMOS on deadtime",null,null,29,7.2499999999999995E-2,0.11853549999999997,0.13130279144999998,1.3826158193644994E-2,1.075947868621103,1.075947868621103,1,1.075947868621103,9.8233568415556836E-7,0.50445543002267956,504455.43002267956,1.9823356841555685E-6,0,6.6E-4,7.9733149996305375E-2,1.0807537854166664E-3,0,1.0809407023376044E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,4.3236867941759419E-2,5.6082802482394296E-6,5.6082802482394296E-6,5.6630490414045623E-2,5.9329730223903294E-3,1.5133662900680387E-3,15,29.544143104443169,2.4609605925941417E-2,2.3245306215445075E-2,4.9368278431454526E-2,5.5366055035976171E-2,5.4902431893269057E-2,2.2607077708462855E-3,4.0860889831837053E-3,2.5466927929264962E-4,4.1566293865410531E-4,4.7564212011304606E-3,7.0202599547664127E-3,1.6197924040564724E-2,3.7475854078921352E-2,5.5994552732517439E-3,0.10546162434291569,0.10655367895154319,0.86999999999999988,0.89088804717223291,6.1417787202041312E-3,2.318191823378799E-3,2.752269116477522E-2,5.0553573751785735E-2,2.607836975905616E-4,4.2564269390738799E-4,4.8706193050617507E-3,1.1067018728320144E-3,0,5.7429308486765877E-6,5.6378119916333397E-6,3.83756212143469E-2,0.1315869849867228,0.89088804717223291,89.088804717223297,72.5,54.888490199331855,0.54888490199331852,504.45543002267954,null,2.3803408574940729E-2,null,0.10546162434291569,3.7475854078921352E-2,1.0809407023376044E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR35, IF(MODE_ILIM=4,#REF!,#REF!))","v":89.088804717223297},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ35, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10546162434291569},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA35, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7475854078921352E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB35, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0809407023376044E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S35, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":504.45543002267954},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P35, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.075947868621103}]
["Sleep delay",5,"µs",{"$f":"B36/1000000","v":5.0000000000000004E-6},"Delay time to enter sleep mode",null,null,30,7.4999999999999997E-2,0.11848500000000001,0.1338033015,1.6351413345150001E-2,1.0754894796375047,1.0754894796375047,1,1.0754894796375047,9.8173005219985088E-7,0.50460959548447781,504609.59548447788,1.9817300521998508E-6,0,6.6E-4,8.2012957563627309E-2,1.1434412854166667E-3,0,1.1436505169714177E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,4.429185956663606E-2,5.885306471611831E-6,5.885306471611831E-6,5.8258624430680063E-2,6.2790245430268095E-3,1.5138287864534337E-3,15,28.986601245518028,2.4844201128880528E-2,2.3252410159924741E-2,4.9610440075258701E-2,5.595878221460817E-2,5.6480884001097117E-2,2.3925676931590414E-3,4.0873377234242718E-3,2.9713431420508004E-4,4.3017954182441204E-4,4.8146515794537633E-3,7.2106227280340114E-3,1.6197924040564724E-2,3.7482356778100002E-2,5.6011665098777055E-3,0.10625292823061989,0.10740796968010459,0.89999999999999991,0.89338185431051198,6.3016596358328805E-3,2.3783523862145662E-3,2.6687896122114575E-2,4.9245629941772402E-2,2.9494933844868528E-4,4.2701621862393304E-4,4.7792470621238212E-3,1.1350329954008191E-3,0,5.8420288986602611E-6,5.4651404469382329E-6,3.7206730447052416E-2,0.12846782131692969,0.89338185431051198,89.338185431051201,75,56.276153038808332,0.5627615303880833,504.60959548447789,null,2.3081423673180175E-2,null,0.10625292823061989,3.7482356778100002E-2,1.1436505169714177E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR36, IF(MODE_ILIM=4,#REF!,#REF!))","v":89.338185431051201},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ36, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10625292823061989},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA36, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7482356778100002E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB36, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1436505169714177E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S36, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":504.60959548447789},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P36, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0754894796375047}]
["IQ(active)",660,"µA",{"$f":"B37/1000000","v":6.6E-4},"LM5164 quiescent current - active state ",null,null,31,7.7499999999999999E-2,0.1184345,0.13630381154999999,1.8876668496655001E-2,1.0750310906539058,1.0750310906539058,1,1.0750310906539058,9.8112465103178615E-7,0.50476379640180224,504763.79640180228,1.9811246510317859E-6,0,6.6E-4,8.4305250182496544E-2,1.2082537854166667E-3,0,1.2084874109348893E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,4.5356745210598348E-2,6.171703008297409E-6,6.171703008297409E-6,5.9896124186881936E-2,6.6369595313292094E-3,1.5142913892054067E-3,15,28.449712909798112,2.5078936842325344E-2,2.3259515738195048E-2,4.9852743969725798E-2,5.6563764665405483E-2,5.806841605640526E-2,2.5289557074748381E-3,4.0885867508545989E-3,3.3962527277098877E-4,4.4471380203974067E-4,4.8729258256653279E-3,7.4055762668353182E-3,1.6197924040564724E-2,3.7488860972792748E-2,5.6028781400600056E-3,0.10706108004509356,0.1082812447850784,0.92999999999999994,0.89571106544692292,6.4635865565200014E-3,2.4392720699623564E-3,2.5902244894980241E-2,4.8014682168361029E-2,3.2710334938323028E-4,4.2831728327308397E-4,4.6932619173661481E-3,1.1637056832966024E-3,0,5.9441534163269371E-6,5.3026345889608305E-6,3.6106653337991138E-2,0.12555007404913909,0.89571106544692292,89.571106544692299,77.5,57.582635216683897,0.57582635216683897,504.76379640180227,null,2.240194153079372E-2,null,0.10706108004509356,3.7488860972792748E-2,1.2084874109348893E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR37, IF(MODE_ILIM=4,#REF!,#REF!))","v":89.571106544692299},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ37, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10706108004509356},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA37, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7488860972792748E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB37, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.2084874109348893E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S37, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":504.76379640180227},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P37, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0750310906539058}]
["IQ(sleep)",10,"µA",{"$f":"B38/1000000","v":1.0000000000000001E-5},"LM5164 quiescent current - sleep state","QRR",2.0000000000000001E-10,32,{"$f":"IF(PLOT_TYPE=1, H38/100*Iout, min_I*EXP(H38*rr/100))","v":0.08},{"$f":"IF(I38<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I38-Vout)/L*OnTime)","v":0.11838399999999999},{"$f":"IF(I38<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I38+((Vin-(Rdcr+RdsonTop)*J38-Vout)/L*OnTime)/2)","v":0.1388043216},{"$f":"IF(I38<Icrit, 0, I38-((Vin-(Rdcr+RdsonTop)*K38-Vout)/L*OnTime)/2)","v":2.1401923648160015E-2},1.0745727016703071,{"$f":"IF(I38<Icrit, 1000*SQRT((J38*CoutEsr)^2+(((J38/2)-I38)*(OnTime+OffTime)/Cout)^2), 1000*J38*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":1.0745727016703071},1,{"$f":"IF(I38<Icrit, 1000*((N38/1000)*O38), 1000*J38*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":1.0745727016703071},{"$f":"IF(I38<Icrit, L*J38/(Vout+J38/2*(RdsonBot+Rdcr)), L*J38/(Vout+I38*(RdsonBot+Rdcr)))","v":9.8051948051948056E-7},0.5049180327868853,{"$f":"IF(I38<Icrit,I38/((OnTime+Q38)*J38/2),1/(OnTime+Q38))","v":504918.03278688528},1.9805194805194805E-6,0,{"$f":"S38*(T38*Iq_active+U38*Iq_sleep)","v":6.600000000000001E-4},8.6609036528143724E-2,{"$f":"W38^2*Rdcr","v":1.2751912854166668E-3},{"$f":"Core_Loss/1000*S38/$S$106","v":0},{"$f":"(Y38+X38*(1+Ltc*(Ta-25)))/(1-X38*Ltc*ThetaCa)","v":1.2754515165620895E-3},3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,4.6430842948908015E-2,6.4674695308384836E-6,6.4674695308384836E-6,6.1542289394202601E-2,7.006788760177597E-3,1.5147540983606559E-3,15,{"$f":"IF(I38<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I38+Iripple/2)*1000000000)","v":27.932351336606658},{"$f":"IF(I38<Icrit, Vin*(I38+Iripple/2)*AK38/1000000000/2*S38, Vin*(I38-Iripple/2)*AJ38/1000000000/2*S38 + Vin*(I38+Iripple/2)*AK38/1000000000/2*S38)","v":2.53138131147541E-2},{"$f":"IF(I38<Icrit, Csw*(Vin)^2*S38/2, Csw*Vin^2*S38/2)","v":2.3266622950819674E-2},5.0095190163934433E-2,{"$f":"(AI38+AL38+AM38+AH38*(1+RdsonTopTc*(Ta-25)))/(1-AH38*RdsonTopTc*ThetaJA)","v":5.7181020207552433E-2},{"$f":"IF(I38<Icrit,Iripple*SQRT((OffTime)*S38/3), SQRT(OffTime*S38*(I38^2+Iripple^2/12)))","v":5.9664349139788471E-2},2.6698759187059329E-3,{"$f":"QgBot*S38*Vdd","v":4.0898360655737707E-3},{"$f":"IF(I38<Icrit, Vin*Idss*R38, QrrBot*(I38-Iripple/2)/1*S38*Vin+Vin*Idss*R38)","v":3.8214216393442639E-4},{"$f":"IF(I38<Icrit, dead1*S38*(I38+Iripple/2)*((I38+Iripple/2)*BDserR+VSD), dead1*S38*(I38+Iripple/2)*((I38+Iripple/2)*BDserR+VSD)+dead2*S38*(I38-Iripple/2)*((I38-Iripple/2)*BDserR+VSD))","v":4.5926573044180333E-4},4.9312439599499998E-3,{"$f":"(AR38+AS38+AT38+AQ38*(1+RdsonBotTc*(Ta-25)))/(1-AQ38*RdsonBotTc*ThetaJA)","v":7.6051255980971464E-3},{"$f":"Vin*V38+Vout*Ifb/0.8","v":1.6197924040564728E-2},{"$f":"(Vin-Vdd)*(S38*QgBot+S38*QgTop)+AW38","v":3.749536666351555E-2},{"$f":"AI38+AR38","v":5.6045901639344264E-3},0.10788610263309956,{"$f":"SUM(Z38,AC38,AF38,AZ38)","v":0.10917352724523414},{"$f":"Vout*I38","v":0.96},0.89788979575043926,6.6273900943609292E-3,2.5008864978508247E-3,{"$f":"Vin*S38*(QgBot+QgTop)/($BB38+$BA38)","v":2.516152158780002E-2},4.685412506705678E-2,3.5741828075282607E-4,4.2955209677246573E-4,4.6122016999948882E-3,{"$f":"X38/($BB38+$BA38)","v":1.1926887945890741E-3},{"$f":"Y38/($BB38+$BA38)","v":0},6.0490363500695371E-6,5.1494223354483138E-6,3.5069486578220635E-2,0.12281646915608396,{"$f":"BC38","v":0.89788979575043926},89.788979575043925,{"$f":"I38*1000","v":80},58.807882255999409,0.58807882255999411,{"$f":"S38/1000","v":504.91803278688525},null,{"$f":"AM38/($BB38+$BA38)","v":2.1761315967827044E-2},null,0.10788610263309956,3.749536666351555E-2,1.2754515165620895E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR38, IF(MODE_ILIM=4,#REF!,#REF!))","v":89.788979575043925},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ38, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10788610263309956},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA38, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.749536666351555E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB38, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.2754515165620895E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S38, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":504.91803278688525},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P38, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0745727016703071}]
["High-side N-ch MOSFET",null,"Units","Std Units","Description","QG_high",1.81E-9,33,8.2500000000000004E-2,0.11833349999999998,0.14130483164999999,2.3927178799665015E-2,{"$f":"IF(I39<Icrit, 1000*((((J39/2)-I39)*0.000002/Cout+Vout/306)), 1000*J39*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":1.0741143126867083},1.0741143126867083,1,1.0741143126867083,9.7991454053114042E-7,0.50507230465196518,505072.30465196521,{"$f":"IF(1/S39-OnTime-Q39>Tsleep, OnTime+Q39+Tsleep, 1/S39)","v":1.9799145405311406E-6},{"$f":"IF(1/S39-OnTime-Q39>Tsleep, 1/S39-OnTime-Q39-Tsleep, 0)","v":0},6.6E-4,{"$f":"IF(I39<Icrit,Iripple*SQRT((OnTime+OffTime)*S39/3), SQRT(I39^2+Iripple^2/12))","v":8.8923423282807404E-2},1.3442537854166669E-3,0,1.3445429705331139E-3,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q39)*S39)","v":3.3183206721673734E-2},5.5056260416666642E-6,5.5056260416666642E-6,{"$f":"SQRT($R39)*SQRT($I39^2*(1-R39)+(Iripple^2)/12)","v":4.7513526848836397E-2},6.7726057008452915E-6,6.7726057008452915E-6,{"$f":"IF(I39<Icrit,Iripple*SQRT((OnTime)*S39/3), SQRT(OnTime*S39*(I39^2+Iripple^2/12)))","v":6.3196488986499322E-2},{"$f":"RdsonTop*AG39^2","v":7.3885230074083501E-3},{"$f":"QgTop*S39*Vdd","v":1.5152169139558958E-3},15,27.433470262546884,2.5548829994667333E-2,2.3273731798362556E-2,5.0337778706985789E-2,5.7810566848647854E-2,6.126807144185456E-2,{"$f":"RdsonBot*AP39^2","v":2.8153324336531458E-3},4.0910856676809187E-3,4.2468499664355869E-4,4.7383533817743813E-4,4.9896060025019151E-3,7.8092757765063844E-3,1.6197924040564724E-2,3.7501873850784614E-2,5.6063025816368147E-3,0.10872801905757568,0.1100848402598513,0.99,0.89993059059531433,6.7929198441612154E-3,2.5631384697006048E-3,2.4461979119265231E-2,4.5758087799024204E-2,3.8604749479435033E-4,4.3072617750601247E-4,4.5356556329994684E-3,1.2219546495151597E-3,0,6.156439442657471E-6,5.0047285810848726E-6,3.4089983316128863E-2,0.12025165367111885,0.89993059059531433,89.993059059531433,82.5,59.95273560232264,0.59952735602322638,505.07230465196523,null,2.1156306265310464E-2,null,0.10872801905757568,3.7501873850784614E-2,1.3445429705331139E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR39, IF(MODE_ILIM=4,#REF!,#REF!))","v":89.993059059531433},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ39, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10872801905757568},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA39, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7501873850784614E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB39, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.3445429705331139E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S39, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":505.07230465196523},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P39, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0741143126867083}]
["RdsonTop",1850,"mW",{"$f":"B40/1000","v":1.85},"Drain-source resistance of high-side MOSFET @ VDD, 25°C","QG_low",1.92E-9,34,8.5000000000000006E-2,0.11828299999999999,0.14380534170000001,2.6452433951170001E-2,1.0736559237031096,1.0736559237031096,1,1.0736559237031096,9.7930983093507309E-7,0.5052266120092862,505226.61200928624,1.9793098309350728E-6,0,6.6E-4,9.1247603849818074E-2,1.4154412854166668E-3,0,1.4157619138747818E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,4.8604221932473657E-2,7.0871111689834596E-6,7.0871111689834596E-6,6.4858153151098621E-2,7.7821730558170245E-3,1.5156798360278587E-3,15,26.952096859098088,2.5783987530587915E-2,2.3280842281387909E-2,5.0580509648003681E-2,5.8452422785464919E-2,6.2879030537553504E-2,2.9653293610069397E-3,4.0923355572752189E-3,4.6725377985066852E-4,4.8842263639861238E-4,5.0480119735244995E-3,8.0180318845978239E-3,1.6197924040564724E-2,3.7508382535116416E-2,5.6080153933030777E-3,0.10958685259848223,0.11101520724956766,1.02,0.90184463786341362,6.9600418164176255E-3,2.6259769913225981E-3,2.3800275818851122E-2,4.4721334712206642E-2,4.1312776066640915E-4,4.3184444671294151E-4,4.463257382542528E-3,1.2514785622191357E-3,0,6.2661502016565119E-6,4.8678620821159333E-6,3.3163464376690641E-2,0.11784193587991341,0.90184463786341362,90.184463786341368,85,61.018807215515402,0.61018807215515403,505.22661200928621,null,2.0584022329817184E-2,null,0.10958685259848223,3.7508382535116416E-2,1.4157619138747818E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR40, IF(MODE_ILIM=4,#REF!,#REF!))","v":90.184463786341368},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ40, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10958685259848223},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA40, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7508382535116416E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB40, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.4157619138747818E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S40, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":505.22661200928621},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P40, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0736559237031096}]
["RdsonTopTc",4800,"ppm/°C",{"$f":"B41/1000000","v":4.7999999999999996E-3},"Drain to Source Resistance Temp Co","Qoss_hs",1.4499999999999999E-10,35,8.7499999999999994E-2,0.1182325,0.14630585174999999,2.8977689102675001E-2,1.0731975347195111,1.0731975347195111,1,1.0731975347195111,9.7870535159968543E-7,0.50538095487109758,505380.95487109758,1.9787053515996856E-6,0,6.6E-4,9.3580848512574047E-2,1.4887537854166666E-3,0,1.4891084919613552E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,4.970239958983047E-2,7.4109855749615402E-6,7.4109855749615402E-6,6.6526766379796168E-2,8.1877496931611598E-3,1.5161428646132927E-3,{"$f":"15*VIN_nom/24","v":15},26.487325400931194,2.6019285771061024E-2,2.3287954400460175E-2,5.0823383036134491E-2,5.910660640471866E-2,6.4496726649223637E-2,3.119870811348506E-3,4.0935857344558913E-3,5.0984852251215814E-4,5.0302763626242487E-4,5.1064618932304745E-3,8.2313990328425121E-3,1.6197924040564724E-2,3.7514892717027619E-2,5.6097285990691845E-3,0.11046262675365798,0.11196465185723596,1.0499999999999998,0.90364194669925946,7.1286362759354262E-3,2.6893564572874644E-3,2.317342204213663E-2,4.3739181699633048E-2,4.3878143943297895E-4,4.3291130711971878E-4,4.3946792056613077E-3,1.2812384464855318E-3,0,6.3779785065889313E-6,4.7382044134188608E-6,3.2285743509551157E-2,0.11557506656616326,0.90364194669925946,90.364194669925951,87.5,62.00835196729512,0.62008351967295117,505.38095487109757,null,2.0041878522928974E-2,null,0.11046262675365798,3.7514892717027619E-2,1.4891084919613552E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR41, IF(MODE_ILIM=4,#REF!,#REF!))","v":90.364194669925951},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ41, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11046262675365798},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA41, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7514892717027619E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB41, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.4891084919613552E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S41, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":505.38095487109757},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P41, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0731975347195111}]
["QgTop",0.6,"nC",{"$f":"B42/1000000000","v":6E-10},"Gate charge of high-side MOSFET @ VDD",null,null,36,0.09,0.118182,0.14880636179999998,3.1502944254180001E-2,1.0727391457359123,1.0727391457359123,1,1.0727391457359123,9.781011023934849E-7,0.50553533324965494,505535.33324965491,1.9781011023934846E-6,0,6.6E-4,9.5922495840826266E-2,1.5641912854166666E-3,0,1.5645828545152818E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,5.0807573410265226E-2,7.7442285475184695E-6,7.7442285475184695E-6,6.8201861400306305E-2,8.6052637121631931E-3,1.5166059997489647E-3,15,26.0383115782336,2.6254724764654205E-2,2.32950681561441E-2,5.1066398920547269E-2,5.9773136283841864E-2,6.6120706763220724E-2,3.2789608971508667E-3,4.0948361993222047E-3,5.52469233588553E-4,5.1765034893110962E-4,5.164955781841867E-3,8.4493823597365965E-3,1.6197924040564724E-2,3.752140439703517E-2,5.6114421990711696E-3,0.11135536523968481,0.11293319794878928,1.08,0.90533149874362262,7.2985959132209179E-3,2.7532359595174283E-3,2.2578735005325829E-2,4.280742543535071E-2,4.6311833264302331E-4,4.339307094657043E-4,4.3296269989994782E-3,1.3112144821740594E-3,0,6.4917537384611509E-6,4.6152006257629619E-6,3.1453064146049446E-2,0.11344005393711082,0.90533149874362262,90.533149874362266,90,62.924142868481049,0.62924142868481048,505.53533324965491,null,1.9527554599200716E-2,null,0.11135536523968481,3.752140439703517E-2,1.5645828545152818E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR42, IF(MODE_ILIM=4,#REF!,#REF!))","v":90.533149874362266},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ42, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11135536523968481},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA42, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.752140439703517E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB42, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.5645828545152818E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S42, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":505.53533324965491},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P42, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0727391457359123}]
["Coss",145,"pF",{"$f":"B43/1000000000000","v":1.4499999999999999E-10},"Capacitance (Coss)",null,null,37,9.2499999999999999E-2,0.1181315,0.15130687184999997,3.4028199405685008E-2,1.0722807567523136,1.0722807567523136,1,1.0722807567523136,9.774970831850791E-7,0.50568974715721859,505689.74715721863,1.9774970831850791E-6,0,6.6E-4,9.8271945174262895E-2,1.6417537854166667E-3,0,1.6421851556079586E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,5.191929539972287E-2,8.0868397044110526E-6,8.0868397044110526E-6,6.9883013868210303E-2,9.0347259105132763E-3,1.5170692414716561E-3,15,25.604267377896317,2.6490304559957323E-2,2.3302183549004634E-2,5.1309557350433611E-2,6.0452031191768639E-2,6.7750559483839373E-2,3.4426037327799429E-3,4.0960869519734711E-3,5.9511592204450131E-4,5.3229078557203823E-4,5.2234936595900111E-3,8.6719870318906749E-3,1.6197924040564724E-2,3.7527917575656211E-2,5.6131561934451273E-3,0.11226509199276065,0.11392086961411468,1.1099999999999999,0.9069213766654437,7.4698242903706051E-3,2.8175786996653845E-3,2.2013800399556398E-2,4.1922283232747562E-2,4.8623725341993162E-4,4.3490620904263378E-4,4.2678360907735047E-3,1.3413888317259342E-3,0,6.6073223401776961E-6,4.4983513055076123E-6,3.0662045649640934E-2,0.11142700633058858,0.9069213766654437,90.692137666544369,92.5,63.769353027551922,0.63769353027551923,505.68974715721862,null,1.9038962507724452E-2,null,0.11226509199276065,3.7527917575656211E-2,1.6421851556079586E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR43, IF(MODE_ILIM=4,#REF!,#REF!))","v":90.692137666544369},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ43, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11226509199276065},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA43, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7527917575656211E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB43, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.6421851556079586E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S43, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":505.68974715721862},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P43, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0722807567523136}]
["Low-side N-ch MOSFET",null,"Units","Std Units","Description",null,null,38,9.5000000000000001E-2,0.11808099999999998,0.15380738189999998,3.6553454557190015E-2,1.0718223677687146,1.0718223677687146,1,1.0718223677687146,9.7689329384317539E-7,0.50584419660605562,505844.1966060556,1.9768932938431753E-6,0,6.6E-4,0.10062865003731955,1.7214412854166664E-3,0,1.7219155536605181E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,5.3037152551777024E-2,8.4388186524014054E-6,8.4388186524014054E-6,7.1569837716329229E-2,9.4761470908721491E-3,1.5175325898181668E-3,15,25.184456468273488,2.6726025205582645E-2,2.3309300579607041E-2,5.1552858375007851E-2,6.1143310089726517E-2,6.9385910524598179E-2,3.6108034344956583E-3,4.097337992509051E-3,6.3778859684877919E-4,5.4694895735772338E-4,5.2820755467155537E-3,8.8992182441196346E-3,1.6197924040564724E-2,3.7534432253408148E-2,5.6148705823272178E-3,0.11319183116958152,0.11492769116793611,1.1400000000000001,0.9084188738707526,7.6422345145583841E-3,2.8823514875487995E-3,2.1476439626642981E-2,4.1080341710388615E-2,5.0822736747103102E-4,4.3584101395410991E-4,4.2090676489891076E-3,1.3717453981866919E-3,0,6.7245457342227949E-6,4.3872057971265966E-6,2.9909637437736034E-2,0.10952699795700709,0.9084188738707526,90.841887387075261,95,64.547447140017496,0.645474471400175,505.84419660605562,null,1.8574218055475007E-2,null,0.11319183116958152,3.7534432253408148E-2,1.7219155536605181E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR44, IF(MODE_ILIM=4,#REF!,#REF!))","v":90.841887387075261},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ44, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11319183116958152},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA44, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7534432253408148E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB44, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7219155536605181E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S44, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":505.84419660605562},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P44, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0718223677687146}]
["RdsonBot",750,"mW",{"$f":"B45/1000","v":0.75},"Drain-source resistance of low-side MOSFET @ VDD, 25°C",null,null,39,9.7500000000000003E-2,0.11803049999999998,0.15630789195,3.9078709708695002E-2,1.0713639787851159,1.0713639787851159,1,1.0713639787851159,9.7628973423658149E-7,0.50599868160843764,505998.68160843768,1.9762897342365817E-6,0,6.6E-4,0.10299211235979838,1.8032537854166671E-3,0,1.8037742114446391E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,5.4160763741674445E-2,8.800164987244431E-6,8.800164987244431E-6,7.326198107301421E-2,9.9295380608739811E-3,1.5179960448253129E-3,15,24.778190030650105,2.6961886750164803E-2,2.3316419248516809E-2,5.1796302043506923E-2,6.1846992132036503E-2,7.102641875108183E-2,3.7835641204530214E-3,4.098589321028346E-3,6.8048726697429143E-4,5.6162487546582076E-4,5.3407014634684578E-3,9.1310812195330229E-3,1.6197924040564724E-2,3.7540948430808629E-2,5.6165853658536585E-3,0.11413560714823182,0.11595368715070536,1.17,0.90983058852793941,7.8157481011613648E-3,2.9475243112859922E-3,2.0964681718695578E-2,4.0278512796422923E-2,5.2916934239058855E-4,4.3673802647606704E-4,4.1531056031278071E-3,1.4022696178212658E-3,0,6.8432985380235617E-6,4.2813563946190864E-6,2.9193079662136447E-2,0.10773195383445064,0.90983058852793941,90.983058852793945,97.5,65.262084299350803,0.65262084299350809,505.99868160843766,null,1.8131616621574552E-2,null,0.11413560714823182,3.7540948430808629E-2,1.8037742114446391E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR45, IF(MODE_ILIM=4,#REF!,#REF!))","v":90.983058852793945},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ45, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11413560714823182},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA45, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7540948430808629E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB45, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.8037742114446391E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S45, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":505.99868160843766},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P45, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0713639787851159}]
["RdsonBotTc",4800,"ppm/°C",{"$f":"B46/1000000","v":4.7999999999999996E-3},"Drain To Source Resitance Temp Co",null,null,40,0.1,0.11797999999999996,0.15880840199999999,4.1603964860200009E-2,1.070905589801517,1.070905589801517,1,1.070905589801517,9.7568640423420403E-7,0.50615320217664306,506153.20217664307,1.975686404234204E-6,0,6.600000000000001E-4,0.10536187739563743,1.8871912854166672E-3,0,1.8877612960833735E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,5.5289776914227769E-2,9.1708782936752221E-6,9.1708782936752221E-6,7.495912267337293E-2,1.0394909633129277E-2,1.5184596065299294E-3,15,24.384822987775834,2.7197889242360825E-2,2.3323539556299712E-2,5.2039888405190471E-2,6.2563096666921503E-2,7.2671772701677628E-2,3.9608899107032233E-3,4.0998409376308094E-3,7.2321194139807492E-4,5.7631855107913375E-4,5.3993714301080178E-3,9.3675812096259328E-3,1.6197924040564728E-2,3.7547466108375532E-2,5.6183005441607387E-3,0.1150964445290837,0.11699888232950241,1.2000000000000002,0.9111625044642746,7.9902939956316595E-3,3.0130699674543082E-3,2.0476739178601978E-2,3.9513995876095588E-2,5.491363364856167E-4,4.3759987864207115E-4,4.0997539956583937E-3,1.4329482816861699E-3,0,6.9634670285018066E-6,4.1804333439739398E-6,2.850986937966243E-2,0.10603455079029069,0.9111625044642746,91.116250446427458,100,65.91703305041338,0.65917033050413376,506.15320217664305,null,1.7709612262574684E-2,null,0.1150964445290837,3.7547466108375532E-2,1.8877612960833735E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR46, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.116250446427458},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ46, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1150964445290837},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA46, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7547466108375532E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB46, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.8877612960833735E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S46, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":506.15320217664305},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P46, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.070905589801517}]
["QgBot",1.62,"nC",{"$f":"B47/1000000000","v":1.6200000000000002E-9},"Gate charge of low-side MOSFET at VDD",null,null,41,0.10249999999999999,0.11792949999999999,0.16130891204999998,4.4129220011704995E-2,1.0704472008179187,1.0704472008179187,1,1.0704472008179187,9.7508330370505105E-7,0.50630775832295483,506307.75832295482,1.9750833037050508E-6,0,6.6E-4,0.10773752924739517,1.9732537854166661E-3,0,1.9738769790520038E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,5.6423866538302413E-2,9.5509581453964875E-6,9.5509581453964875E-6,7.6660968698188836E-2,1.0872272625227674E-2,1.5189232749688644E-3,15,24.003750586029071,2.7434032730850145E-2,2.3330661503521758E-2,5.2283617509340768E-2,6.3291643237322934E-2,7.4321687522954052E-2,4.1427849271947186E-3,4.1010928424159345E-3,7.6596262910129907E-4,5.9102999538561429E-4,5.4580854669028477E-3,9.6087234943703533E-3,1.6197924040564724E-2,3.7553985286626956E-2,5.6200161173847992E-3,0.11607436813570504,0.11806330169894411,1.23,0.91242006102372886,8.1658077288424922E-3,3.0789637417148871E-3,2.0010987117184693E-2,3.8784245104401628E-2,5.6819485267195372E-4,4.3842896297284262E-4,4.0488346949465234E-3,1.4637693815489257E-3,0,7.0849478161445067E-6,4.0841005275701856E-6,2.7857731338949906E-2,0.10442813197157756,0.91242006102372886,91.242006102372883,102.5,66.516098897051677,0.66516098897051679,506.30775832295484,null,1.7306799668916493E-2,null,0.11607436813570504,3.7553985286626956E-2,1.9738769790520038E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR47, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.242006102372883},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ47, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11607436813570504},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA47, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7553985286626956E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB47, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.9738769790520038E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S47, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":506.30775832295484},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P47, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0704472008179187}]
["VSD",0.8,"V",{"$f":"B48","v":0.8},"Body diode forward voltage",null,null,42,0.105,0.117879,0.16380942209999999,4.6654475163210009E-2,1.0699888118343199,1.0699888118343199,1,1.0699888118343199,9.7448043251822821E-7,0.50646235005966211,506462.35005966219,1.974480432518228E-6,0,6.6E-4,0.11011868691704116,2.0614412854166667E-3,0,2.0621214361789199E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,5.7562731302657946E-2,9.9404041050659903E-6,9.9404041050659903E-6,7.8367249984481455E-2,1.1361637859740885E-2,1.5193870501789865E-3,15,23.634405293122018,2.767031726433461E-2,2.3337785090749234E-2,5.2527489405262834E-2,6.4032651581725983E-2,7.5975902265339637E-2,4.3292532937743312E-3,4.1023450354832642E-3,8.0873933906927108E-4,6.0575921957836784E-4,5.5168435941309029E-3,9.8545133823071222E-3,1.6197924040564724E-2,3.7560505966081278E-2,5.6217320856622507E-3,0.11706940301577663,0.11914697048210228,1.26,0.91360821360434663,8.342230685132377E-3,3.1451831320485875E-3,1.9565945173882389E-2,3.8086941079891606E-2,5.8640547844336253E-4,4.3922745910583797E-4,4.0001854133083475E-3,1.4947219763648959E-3,0,7.207646695979884E-6,3.9920517243655964E-6,2.7234592664878508E-2,0.10290663276147627,0.91360821360434663,91.36082136043467,105,67.063063929713536,0.6706306392971354,506.46235005966219,null,1.6921898528763146E-2,null,0.11706940301577663,3.7560505966081278E-2,2.0621214361789199E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR48, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.36082136043467},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ48, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11706940301577663},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA48, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7560505966081278E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB48, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.0621214361789199E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S48, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":506.46235005966219},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P48, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0699888118343199}]
["BDserR",100,"mW",{"$f":"B49*0.001","v":0.1},"Series resistance of body diode",null,null,43,0.1075,0.11782849999999997,0.16630993215000001,4.9179730314715009E-2,1.069530422850721,1.069530422850721,1,1.069530422850721,9.7387779054294178E-7,0.50661697739905998,506616.97739905998,1.9738777905429417E-6,0,6.5999999999999989E-4,0.11250500081477859,2.1517537854166663E-3,0,2.1524948476465086E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,5.870609202994153E-2,1.0339215724283894E-5,1.0339215724283894E-5,8.0077719559510624E-2,1.1863016164225517E-2,1.5198509321971798E-3,15,23.276253977875438,2.7906742891538518E-2,2.3344910318548684E-2,5.2771504142284383E-2,6.4786141634993064E-2,7.7634177492376263E-2,4.520299136188336E-3,4.1035975169323863E-3,8.515420802914361E-4,6.2050623485565494E-4,5.5756458320794771E-3,1.0104956210638307E-2,1.6197924040564721E-2,3.756702814725707E-2,5.6234484491295665E-3,0.11808157444201801,0.12024991413143048,1.29,0.91473148629440482,8.5195094658867387E-3,3.2117076081145672E-3,1.9140261797106057E-2,3.7419966215552811E-2,6.038235292614067E-4,4.3999735694919239E-4,3.9536579837436145E-3,1.5257960761812393E-3,0,7.3314776485214625E-6,3.9040073581976187E-6,2.6638560847135038E-2,0.10146451636493736,0.91473148629440482,91.473148629440487,107.5,67.561637846160409,0.67561637846160405,506.61697739905998,null,1.6553739932632264E-2,null,0.11808157444201801,3.756702814725707E-2,2.1524948476465086E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR49, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.473148629440487},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ49, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11808157444201801},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA49, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.756702814725707E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB49, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.1524948476465086E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S49, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":506.61697739905998},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P49, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.069530422850721}]
["QrrBot",1.4,"nC",{"$f":"B50*0.000000001","v":1.3999999999999999E-9},"Reverse recovery charge of body diode at 100mA",null,null,44,0.11,0.11777799999999998,0.16881044219999999,5.1704985466219995E-2,1.0690720338671222,1.0690720338671222,1,1.0690720338671222,9.7327537764849753E-7,0.50677164035344868,506771.64035344869,1.9732753776484975E-6,0,6.6E-4,0.11489614966713781,2.2441912854166664E-3,0,2.2449973979920836E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,5.9853689787626216E-2,1.0747392543580171E-5,1.0747392543580171E-5,8.1792150456742152E-2,1.2376418371225941E-2,1.5203149210603461E-3,15,22.928795342588447,2.8143309661208593E-2,2.3352037187486914E-2,5.3015661769755855E-2,6.5552133529205844E-2,7.9296293163329826E-2,4.7159265820835607E-3,4.1048502868629346E-3,8.9437086176138059E-4,6.3527105242089496E-4,5.6344922010452096E-3,1.0360057345320183E-2,1.6197924040564724E-2,3.7573551830673194E-2,5.6251652079232807E-3,0.1191109079131225,0.12137215832969983,1.32,0.91579401778486613,8.6975953344191025E-3,3.2785184013482561E-3,1.8732700532609829E-2,3.6781383255794123E-2,6.2049960975921799E-4,4.407404768779937E-4,3.9091168567974895E-3,1.5569825408708424E-3,0,7.4563619683306033E-6,3.8197116614537148E-6,2.6067904540500085E-2,0.10009671762260672,0.91579401778486613,91.579401778486613,110,68.015419380100283,0.68015419380100284,506.77164035344867,null,1.6201254514689581E-2,null,0.1191109079131225,3.7573551830673194E-2,2.2449973979920836E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR50, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.579401778486613},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ50, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1191109079131225},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA50, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7573551830673194E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB50, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.2449973979920836E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S50, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":506.77164035344867},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P50, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0690720338671222}]
["TrrBot",20,"ns",{"$f":"B51*0.000000001","v":2E-8},"Reverse recovery time of body diode (not used)",null,null,45,0.1125,0.11772749999999998,0.17131095224999998,5.4230240617725009E-2,1.0686136448835237,1.0686136448835237,1,1.0686136448835237,9.7267319370430014E-7,0.50692633893513428,506926.33893513435,1.9726731937043001E-6,0,6.6E-4,0.11729183777370586,2.3387537854166664E-3,0,2.3396292761088218E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,6.1005284176596737E-2,1.1164934092401974E-5,1.1164934092401974E-5,8.3510333778026524E-2,1.2901855318277186E-2,1.5207790168054029E-3,15,22.591557581997353,2.8380017622114031E-2,2.3359165698130992E-2,5.3259962337050423E-2,6.6330647594515887E-2,8.0962046754500736E-2,4.9161397610084723E-3,4.106103345374589E-3,9.3722569247683388E-4,6.5005368348266851E-4,5.6933827213340909E-3,1.0619822181156672E-2,1.6197924040564724E-2,3.7580077016848693E-2,5.6268823621799923E-3,0.12015742915470125,0.12251372899094413,1.35,0.91679960153926854,8.8764437302885392E-3,3.3455983213130898E-3,1.8342128026862057E-2,3.6169416480447608E-2,6.3648010475194532E-4,4.4145848740447723E-4,3.8664377854293708E-3,1.5882729915321892E-3,0,7.5822275015750546E-6,3.7389301934994204E-6,2.5521036766564371E-2,9.879859385228873E-2,0.91679960153926854,91.679960153926856,112.5,68.427867006324419,0.68427867006324417,506.92633893513437,null,1.5863462077286103E-2,null,0.12015742915470125,3.7580077016848693E-2,2.3396292761088218E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR51, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.679960153926856},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ51, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12015742915470125},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA51, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7580077016848693E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB51, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.3396292761088218E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S51, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":506.92633893513437},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P51, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0686136448835237}]
["Idss",0,"μA",{"$f":"B52/1000000","v":0},"Leakage current of low-side device",null,null,46,0.115,0.117677,0.1738114623,5.6755495769230016E-2,1.0681552558999252,1.0681552558999252,1,1.0681552558999252,9.7207123857985423E-7,0.50708107315642859,507081.07315642864,1.9720712385798544E-6,0,6.6E-4,0.11969179256880287,2.4354412854166669E-3,0,2.436390675246731E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,6.2160651779886604E-2,1.1591839889100959E-5,1.1591839889100959E-5,8.5232076971144086E-2,1.3439337847907806E-2,1.5212432194692859E-3,15,22.264096245832732,2.8616866823046476E-2,2.3366295851048231E-2,5.3504405893563992E-2,6.7121704360003934E-2,8.2631251589329283E-2,5.1209428044142746E-3,4.1073566925670726E-3,9.801065814396717E-4,6.648541392547207E-4,5.7523174132614657E-3,1.0884256141893362E-2,1.6197924040564724E-2,3.7586603706302887E-2,5.6285999120363585E-3,0.12122116412023655,0.12367465226141405,1.3800000000000001,0.9177517210419045,9.0560138431279302E-3,3.4129315945532791E-3,1.7967503500270189E-2,3.5582435211697801E-2,6.5180761008750451E-4,4.4215292068322748E-4,3.8255066710145115E-3,1.6196597327446769E-3,0,7.7090079770033354E-6,3.6614476631541367E-6,2.499650017360833E-2,9.7565881713427602E-2,0.9177517210419045,91.775172104190446,115,68.802277733330541,0.68802277733330541,507.08107315642866,null,1.5539462486720163E-2,null,0.12122116412023655,3.7586603706302887E-2,2.436390675246731E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR52, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.775172104190446},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ52, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12122116412023655},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA52, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7586603706302887E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB52, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.436390675246731E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S52, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":507.08107315642866},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P52, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0681552558999252}]
["Csw",160,"pF",{"$f":"B53/1000000000000","v":1.5999999999999999E-10},"Effective SW node capacitance (CossHS + CossLS)",null,null,47,0.11749999999999999,0.11762649999999999,0.17631197234999998,5.9280750920735002E-2,1.0676968669163263,1.0676968669163263,1,1.0676968669163263,9.7146951214476246E-7,0.5072358430296493,507235.84302964935,1.9714695121447622E-6,0,6.6E-4,0.12209576245035424,2.5342537854166668E-3,0,2.5352817930136338E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,6.3319584755746991E-2,1.202810944092068E-5,1.202810944092068E-5,8.6957202296062006E-2,1.3988876807642766E-2,1.521707529088948E-3,15,21.945992284612089,2.8853857312820089E-2,2.3373427646806243E-2,5.3748992488715279E-2,6.7925324554547889E-2,8.4303735351454162E-2,5.3303398456560173E-3,4.1086103285401599E-3,1.023013537655918E-3,6.7967243095596458E-4,5.8112962971520422E-3,1.1153364680312042E-2,1.6197924040564724E-2,3.7593131899555335E-2,5.6303178576291076E-3,0.12230213899204437,0.12485495452054059,1.41,0.91865358081373694,9.2362682376466165E-3,3.4805037227955914E-3,1.7607869484359176E-2,3.5018939301339674E-2,6.6652131176492041E-4,4.4282518615466258E-4,3.7862185479066199E-3,1.6511356841587155E-3,0,7.8366424172491485E-6,3.5870660126230083E-6,2.4492954066333072E-2,9.6394659250888928E-2,0.91865358081373694,91.865358081373699,117.5,69.1417728033842,0.69141772803384205,507.23584302964935,null,1.5228427662148478E-2,null,0.12230213899204437,3.7593131899555335E-2,2.5352817930136338E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR53, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.865358081373699},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ53, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12230213899204437},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA53, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7593131899555335E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB53, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.5352817930136338E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S53, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":507.23584302964935},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P53, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0676968669163263}]
["ThetaJA",41.1,"°C/W",null,"Thermal resistance",null,null,48,0.12,0.117576,0.17881248239999997,6.1806006072239995E-2,1.0672384779327275,1.0672384779327275,1,1.0672384779327275,9.7086801426872767E-7,0.50739064856711913,507390.64856711921,1.9708680142687274E-6,0,6.6E-4,0.12450351484329,2.6351912854166671E-3,0,2.6363028313761811E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,6.4481889560774816E-2,1.2473742243983882E-5,1.2473742243983882E-5,8.8685545456835116E-2,1.4550483050006282E-2,1.5221719457013576E-3,15,21.636850260600085,2.909098914027149E-2,2.3380561085972851E-2,5.3993722171945702E-2,6.8741529107699414E-2,8.5979338758360363E-2,5.5443350199936665E-3,4.1098642533936658E-3,1.0659465701357465E-3,6.945085698104828E-4,5.8703193933398951E-3,1.1427153278325742E-2,1.6197924040564724E-2,3.7599661597125814E-2,5.6320361990950234E-3,0.123400380182246,0.12605466238190782,1.44,0.91950813377728224,9.4171725227795537E-3,3.548301357842848E-3,1.7262343649319879E-2,3.4477546326399211E-2,6.8065732042487163E-4,4.4347658258247667E-4,3.7484766875323298E-3,1.6826943201386369E-3,0,7.9650746194336594E-6,3.515602726978139E-6,2.4009162962382296E-2,9.5281312406748503E-2,0.91950813377728224,91.950813377728224,120,69.449289175978407,0.69449289175978413,507.39064856711923,null,1.4929594507519893E-2,null,0.123400380182246,3.7599661597125814E-2,2.6363028313761811E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR54, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.950813377728224},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ54, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.123400380182246},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA54, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7599661597125814E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB54, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.6363028313761811E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S54, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":507.39064856711923},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P54, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0672384779327275}]
["Inductor",null,"Units","Std Units","Description",null,null,49,0.1225,0.11752549999999998,0.18131299244999999,6.4331261223744995E-2,1.0667800889491288,1.0667800889491288,1,1.0667800889491288,9.7026674482155072E-7,0.5075454897811672,507545.48978116718,1.9702667448215509E-6,0,6.6E-4,0.12691483446915625,2.7382537854166661E-3,0,2.739453996660879E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,6.5647385790245025E-2,1.2928737783279793E-5,1.2928737783279793E-5,9.0416954379157075E-2,1.512416743252476E-2,1.5226364693435015E-3,15,21.336296707876095,2.9328262354259851E-2,2.3387696169116182E-2,5.4238594992719533E-2,6.9570339150569635E-2,8.7657914376232854E-2,5.7629324645932277E-3,4.1111184672274551E-3,1.1089056878934853E-3,7.0936256704753203E-4,5.9293867221684726E-3,1.1705627447074356E-2,1.6197924040564724E-2,3.7606192799534359E-2,5.6337549365709566E-3,0.12451591433374931,0.12727380269423513,1.47,0.92031810546222359,9.5986950590368179E-3,3.6163121909109689E-3,1.6930111575064272E-2,3.3956980263015302E-2,6.9424896722341243E-4,4.4410830870136343E-4,3.7121918059176552E-3,1.714329616373761E-3,0,8.0942526957319243E-6,3.4468893388096234E-6,2.3543986470009916E-2,9.4222505398287998E-2,0.92031810546222359,92.03181054622236,122.5,69.727575757335345,0.69727575757335347,507.54548978116719,null,1.4642258659515042E-2,null,0.12451591433374931,3.7606192799534359E-2,2.739453996660879E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR55, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.03181054622236},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ55, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12451591433374931},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA55, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7606192799534359E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB55, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.739453996660879E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S55, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":507.54548978116719},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P55, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0667800889491288}]
["Ltc",4000,"ppm",{"$f":"Ltc","v":4.0000000000000001E-3},"Inductor DCR Temp Co",null,null,50,0.125,0.11747499999999998,0.1838135025,6.6856516375250002E-2,1.0663216999655301,1.0663216999655301,1,1.0663216999655301,9.6966570367313243E-7,0.50770036668412777,507700.36668412777,1.9696657036731326E-6,0,6.6E-4,0.12932952179735815,2.8434412854166677E-3,0,2.8447354995551517E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,6.6815905124083294E-2,1.3393095532651501E-5,1.3393095532651501E-5,9.2151288116203059E-2,1.5709940817729612E-2,1.5231011000523833E-3,15,21.043978627209206,2.9565677003666843E-2,2.3394832896804607E-2,5.4483611000523832E-2,7.0411776016723507E-2,8.9339325559187208E-2,5.9861363185278304E-3,4.1123729701414355E-3,1.1518908999476165E-3,7.2423443390154526E-4,5.9884983039905975E-3,1.1988792727020773E-2,1.6197924040564724E-2,3.7612725507301242E-2,5.6354740701938192E-3,0.12564876832123933,0.12851240254236881,1.5,0.92108601546924651,9.7808066990053358E-3,3.6845248545008041E-3,1.661042034110426E-2,3.3456061443232599E-2,7.07327066192023E-4,4.4472147265866646E-4,3.6772813609780267E-3,1.746036002536794E-3,0,8.2241286659792902E-6,3.3807701022549782E-6,2.3096370312305728E-2,9.3215154451282478E-2,0.92108601546924651,92.108601546924646,125,69.979193442852676,0.69979193442852672,507.7003666841278,null,1.4365768943657736E-2,null,0.12564876832123933,3.7612725507301242E-2,2.8447354995551517E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR56, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.108601546924646},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ56, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12564876832123933},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA56, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7612725507301242E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB56, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.8447354995551517E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S56, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":507.7003666841278},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P56, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0663216999655301}]
["ThetaCA",20,"°C/W",{"$f":"ThetaCa","v":40},"Inductor Core-to-Ambient thermal resistance",null,null,51,0.1275,0.11742450000000001,0.18631401254999999,6.9381771526755009E-2,1.0658633109819315,1.0658633109819315,1,1.0658633109819315,9.6906489069347146E-7,0.50785527928834118,507855.27928834117,1.9690648906934716E-6,0,6.6E-4,0.13174739165665988,2.950753785416667E-3,0,2.9521475551084024E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,6.7987290368085623E-2,1.3866814954783166E-5,1.3866814954783166E-5,9.3888415867670563E-2,1.6307814073160211E-2,1.5235658378650236E-3,15,20.759562102986891,2.9803233137396658E-2,2.3401971269606761E-2,5.4728770244868441E-2,7.1265861243083248E-2,9.1023445498243899E-2,6.2139507227788335E-3,4.1136277622355636E-3,1.1949022153207806E-3,7.3912418161213491E-4,6.0476541591684791E-3,1.2276654688047553E-2,1.6197924040564724E-2,3.7619259720946957E-2,5.6371936001005877E-3,0.12679896925217835,0.12977048924828319,1.53,0.92181419654770658,9.9634805567030676E-3,3.752928835179021E-3,1.6302572829052852E-2,3.2973697628312044E-2,7.1992014743071898E-4,4.4531710040638647E-4,3.6436689279295996E-3,1.7778083202052083E-3,0,8.3546580955680829E-6,3.3171008144386184E-6,2.2665338349270731E-2,9.2256404453399637E-2,0.92181419654770658,92.181419654770664,127.5,70.206518151218702,0.702065181512187,507.85527928834119,null,1.4099522446748411E-2,null,0.12679896925217835,3.7619259720946957E-2,2.9521475551084024E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR57, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.181419654770664},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ57, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12679896925217835},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA57, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7619259720946957E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB57, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.9521475551084024E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S57, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":507.85527928834119},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P57, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0658633109819315}]
[null,null,null,null,null,null,null,52,0.13,0.11737399999999999,0.18881452260000001,7.1907026678260016E-2,1.0654049219983328,1.0654049219983328,1,1.0654049219983328,9.6846430575266514E-7,0.50801022760615322,508010.22760615329,1.9684643057526653E-6,0,6.6E-4,0.13416827198832568,3.0601912854166676E-3,0,3.0616903827331288E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,6.9161394581050639E-2,1.4349895501187341E-5,1.4349895501187341E-5,9.5628216098870525E-2,1.6917798071366719E-2,1.5240306828184598E-3,15,20.482731030804107,3.0040930804376073E-2,2.3409111288091543E-2,5.497407277528607E-2,7.2132616570840857E-2,9.2710156367300026E-2,6.4463798202369161E-3,4.114882843609842E-3,1.2379396430397787E-3,7.5403182142409558E-4,6.1068543080737168E-3,1.2569218929554159E-2,1.6197924040564724E-2,3.7625795440992274E-2,5.6389135264283017E-3,0.12796654446781561,0.13104809037209159,1.56,0.92250481159098419,1.0146691802111486E-2,3.8215143958788829E-3,1.6005922647001822E-2,3.2508876056380982E-2,7.3205466484834694E-4,4.4589614317720635E-4,3.611283642873804E-3,1.8096417853754325E-3,0,8.4857997728673962E-6,3.2557477655500784E-6,2.2249985470675315E-2,9.1343608155861691E-2,0.92250481159098419,92.250481159098413,130,70.411746141009829,0.70411746141009823,508.01022760615331,null,1.3842960127136712E-2,null,0.12796654446781561,3.7625795440992274E-2,3.0616903827331288E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR58, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.250481159098413},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ58, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12796654446781561},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA58, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7625795440992274E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB58, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.0616903827331288E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S58, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":508.01022760615331},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P58, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0654049219983328}]
[null,null,null,null,null,null,null,53,0.13250000000000001,0.1173235,0.19131503264999999,7.4432281829764996E-2,1.0649465330147341,1.0649465330147341,1,1.0649465330147341,9.6786394872091013E-7,0.50816521164991557,508165.21164991561,1.9678639487209101E-6,0,6.6E-4,0.13659200272465932,3.1717537854166681E-3,0,3.1733642062060346E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,7.0338080279443271E-2,1.4842336612192219E-5,1.4842336612192219E-5,9.7370575748398441E-2,1.7539903689913008E-2,1.5244956349497467E-3,15,20.213185945519147,3.0278770053554397E-2,2.341625295282811E-2,5.521951864133226E-2,7.3012063946379616E-2,9.4399348554978141E-2,6.6834277557031897E-3,4.1161382143643172E-3,1.2810031921355733E-3,7.6895736458740737E-4,6.1660987710872982E-3,1.2866491080554735E-2,1.6197924040564724E-2,3.7632332667958165E-2,5.6406338493140643E-3,0.12915152154420659,0.13234523371306647,1.59,0.92315986880995171,1.0330417477737509E-2,3.8902725065302944E-3,1.5719869598000733E-2,3.2060656342566649E-2,7.4375518163333654E-4,4.4645948415909255E-4,3.5800597060290278E-3,1.8415319549954208E-3,0,8.6175154212229636E-6,3.1965868014727366E-6,2.1849471250795421E-2,9.0474307604670193E-2,0.92315986880995171,92.315986880995169,132.5,70.596901007914624,0.70596901007914625,508.16521164991559,null,1.3595562895568201E-2,null,0.12915152154420659,3.7632332667958165E-2,3.1733642062060346E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR59, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.315986880995169},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ59, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12915152154420659},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA59, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7632332667958165E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB59, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.1733642062060346E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S59, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":508.16521164991559},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P59, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0649465330147341}]
[null,null,null,null,null,null,null,54,0.13500000000000001,0.11727299999999997,0.19381554270000001,7.6957536981270003E-2,1.0644881440311351,1.0644881440311351,1,1.0644881440311351,9.6726381946850089E-7,0.50832023143198546,508320.23143198551,1.9672638194685006E-6,0,6.6E-4,0.13901843477874917,3.2854412854166674E-3,0,3.2871692536691724E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,7.151721871206701E-2,1.5344137716928885E-5,1.5344137716928885E-5,9.9115389514361135E-2,1.8174141811379531E-2,1.5249606942959566E-3,15,19.950642940641643,3.051675093390354E-2,2.3423396264385891E-2,5.5465107892585394E-2,7.3904225522204797E-2,9.6090919972633498E-2,6.9250986758902918E-3,4.1173938745990828E-3,1.3240928716432932E-3,7.8390082235723876E-4,6.2253875685996142E-3,1.3168476799776433E-2,1.6197924040564724E-2,3.7638871402365874E-2,5.6423545688950392E-3,0.13035392829324213,0.13366194731066991,1.62,0.92378123530840861,1.0514636334498065E-2,3.9591947819956974E-3,1.5443855625783416E-2,3.1628164126868329E-2,7.5504453619117248E-4,4.4700794446694278E-4,3.5499359372805936E-3,1.8734746970218855E-3,0,8.7497694412882149E-6,3.1395024851339347E-6,2.146301427141474E-2,8.9646217527447267E-2,0.92378123530840861,92.378123530840867,135,70.763841860106652,0.70763841860106647,508.32023143198552,null,1.3356848108785653E-2,null,0.13035392829324213,3.7638871402365874E-2,3.2871692536691724E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR60, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.378123530840867},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ60, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13035392829324213},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA60, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7638871402365874E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB60, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.2871692536691724E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S60, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":508.32023143198552},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P60, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0644881440311351}]
[null,null,null,null,null,null,null,55,0.13750000000000001,0.11722249999999998,0.19631605275,7.948279213277501E-2,1.0640297550475364,1.0640297550475364,1,1.0640297550475364,9.666639178658308E-7,0.50847528696472566,508475.2869647257,1.9666639178658308E-6,0,6.6E-4,0.14144742913299393,3.4012537854166683E-3,0,3.4031057576311189E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,7.2698689197991648E-2,1.5855298233318564E-5,1.5855298233318564E-5,0.10086255921038406,1.8820523323366228E-2,1.5254258608941771E-3,15,19.694832670855238,3.0754873494417957E-2,2.3430541223334562E-2,5.5710840578646698E-2,7.4809123657883725E-2,9.778477543001253E-2,7.171396729423486E-3,4.1186498244142784E-3,1.3672086906022334E-3,7.9886220599394912E-4,6.2847207210104611E-3,1.3475181775758278E-2,1.6197924040564724E-2,3.7645411644736851E-2,5.644075685308456E-3,0.1315737927636873,0.1349982594455934,1.6500000000000001,0.92437064925344925,1.0699328684594238E-2,4.0282734264296249E-3,1.5177361180113988E-2,3.1210585379478212E-2,7.6594399090723912E-4,4.4754228849616326E-4,3.5208553777315425E-3,1.9054661635765802E-3,0,8.8825286800240896E-6,3.0843873446558253E-6,2.1089887032399248E-2,8.8857210439751505E-2,0.92437064925344925,92.437064925344927,137.5,70.914272258910415,0.70914272258910416,508.47528696472568,null,1.312636642604453E-2,null,0.1315737927636873,3.7645411644736851E-2,3.4031057576311189E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR61, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.437064925344927},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ61, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1315737927636873},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA61, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7645411644736851E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB61, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.4031057576311189E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S61, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":508.47528696472568},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P61, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0640297550475364}]
[null,null,null,null,null,null,null,56,0.14000000000000001,0.11717199999999997,0.19881656280000001,8.2008047284280017E-2,1.0635713660639377,1.0635713660639377,1,1.0635713660639377,9.6606424378339128E-7,0.50863037826050495,508630.37826050498,1.9660642437833912E-6,0,6.6E-4,0.14387885601551514,3.5191912854166678E-3,0,3.5211739549681491E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,7.3882378521674175E-2,1.6375817568059824E-5,1.6375817568059824E-5,0.1026119931837047,1.9479059118495425E-2,1.5258911347815151E-3,15,19.445499430307635,3.0993137784114742E-2,2.343768783024407E-2,5.5956716749140323E-2,7.5726780920995065E-2,9.9480826071102951E-2,7.4223260668417768E-3,4.1199060639100903E-3,1.4103506580558588E-3,8.1384152676309261E-4,6.344098248729042E-3,1.3786611726950636E-2,1.6197924040564724E-2,3.7651953395592824E-2,5.6457971986916058E-3,0.13281114324223012,0.136354198640808,1.6800000000000002,0.92492973080754681,1.0884476269358054E-2,4.0975011832994268E-3,1.4919901951942368E-2,3.080716128550982E-2,7.7647336577372139E-4,4.4806322873154169E-4,3.4927649317937986E-3,1.9375027668337517E-3,0,9.0157622232018251E-6,3.0311411980034324E-6,2.0729411380097599E-2,8.810530326676129E-2,0.92492973080754681,92.49297308075468,140,71.049749591014816,0.71049749591014821,508.63037826050498,null,1.2903698985463667E-2,null,0.13281114324223012,3.7651953395592824E-2,3.5211739549681491E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR62, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.49297308075468},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ62, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13281114324223012},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA62, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7651953395592824E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB62, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.5211739549681491E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S62, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":508.63037826050498},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P62, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0635713660639377}]
[null,1500,null,null,null,"Eff (%)","Iout (mA)",57,0.14249999999999999,0.11712149999999999,0.20131707284999997,8.4533302435784996E-2,1.0631129770803391,1.0631129770803391,1,1.0631129770803391,9.6546479709177242E-7,0.50878550533169764,508785.50533169764,1.9654647970917724E-6,0,6.5999999999999989E-4,0.14631259415488926,3.6392537854166673E-3,0,3.6413740869254614E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,7.5068180379829375E-2,1.6905695116615799E-5,1.6905695116615799E-5,0.10436360578859438,2.0149760094414694E-2,1.526356515995093E-3,15,19.202400300037507,3.123154385203359E-2,2.3444836085684626E-2,5.6202736453713306E-2,7.6657220088087508E-2,0.10117898886362392,7.6778908405989998E-3,4.1211625931867508E-3,1.4535187830518066E-3,8.2883879593542026E-4,6.4035201721739776E-3,1.4102772401815188E-2,1.6197924040564721E-2,3.7658496655455731E-2,5.6475191091818443E-3,0.13406600825454026,0.137729793662624,1.71,0.92545999196689255,1.1070062140324494E-2,4.1668712904063361E-3,1.4671025935203653E-2,3.0417183641503448E-2,7.8665115864728203E-4,4.4857143007499584E-4,3.4656150450876979E-3,1.9695811573199953E-3,0,9.1494412086654922E-6,2.9796705452009037E-6,2.0380954393124741E-2,8.7388645303446533E-2,0.92545999196689255,92.545999196689252,142.5,71.171694607053283,0.71171694607053282,508.78550533169766,null,1.2688454862878834E-2,null,0.13406600825454026,3.7658496655455731E-2,3.6413740869254614E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR63, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.545999196689252},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ63, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13406600825454026},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA63, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7658496655455731E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB63, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.6413740869254614E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S63, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":508.78550533169766},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P63, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0631129770803391}]
[null,null,null,null,null,{"$f":"BR56","v":92.108601546924646},{"$f":"I56*1000","v":125},58,0.14499999999999999,0.11707099999999999,0.20381758289999999,8.7058557587289989E-2,1.0626545880967404,1.0626545880967404,1,1.0626545880967404,9.648655776616613E-7,0.50894066819068395,508940.66819068394,1.964865577661661E-6,0,6.6E-4,0.14874853010478231,3.7614412854166663E-3,0,3.7637063991183993E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,7.6255994875160243E-2,1.7444930263201395E-5,1.7444930263201395E-5,0.1061173169091638,2.0832637153799818E-2,1.5268220045720519E-3,15,18.965304358562786,3.1470091747236847E-2,2.3451985990226715E-2,5.6448899742035617E-2,7.7600464145647946E-2,0.10287918613639291,7.9380952050649347E-3,4.12241941234454E-3,1.4967130746418908E-3,8.4385402478688468E-4,6.462986511773316E-3,1.4423669578925514E-2,1.6197924040564724E-2,3.7665041424847778E-2,5.6492414169165917E-3,0.13533841656633783,0.13912507352176109,1.7399999999999998,0.92596284543156038,1.1256070552010219E-2,4.236377439332811E-3,1.4430310777759747E-2,3.0039990704951829E-2,7.9649465367242806E-4,4.490675137474358E-4,3.4393594140387446E-3,2.0016982043495187E-3,0,9.2835386579707507E-6,2.9298880203584849E-6,2.0043924673017039E-2,8.6705507359558107E-2,0.92596284543156038,92.596284543156031,145,71.281400919850697,0.71281400919850701,508.94066819068394,null,1.2480268780765184E-2,null,0.13533841656633783,3.7665041424847778E-2,3.7637063991183993E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR64, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.596284543156031},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ64, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13533841656633783},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA64, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7665041424847778E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB64, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7637063991183993E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S64, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":508.94066819068394},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P64, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0626545880967404}]
[null,null,null,null,null,{"$f":"BR81","v":93.133536343118365},{"$f":"I81*1000","v":187.5},59,0.14749999999999999,0.1170205,0.20631809294999998,8.9583812738794996E-2,1.0621961991131417,1.0621961991131417,1,1.0621961991131417,9.6426658536384389E-7,0.50909586684984942,509095.86684984947,1.9642665853638441E-6,0,6.6E-4,0.15118655763107158,3.8857537854166662E-3,0,3.8881711415337163E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,7.7445728052554008E-2,1.7993522380770454E-5,1.7993522380770454E-5,0.10787305152631363,2.1527701204357624E-2,1.5272876005495485E-3,15,18.733991950237836,3.1708781518809452E-2,2.3459137544441063E-2,5.6695206663800068E-2,7.8556536291079102E-2,0.10458134515949076,8.2029433165264065E-3,4.1236765214837812E-3,1.5399335418820985E-3,8.5888722459864016E-4,6.5224972879645198E-3,1.4749309067068185E-2,1.6197924040564724E-2,3.7671587704291375E-2,5.6509641220333293E-3,0.13662839718447201,0.14054006747442815,1.77,0.92643961261686059,1.1442486865076771E-2,4.3060137388161723E-3,1.4197361388822606E-2,2.9674963445674458E-2,8.0602001920732286E-4,4.4955206081284449E-4,3.4139547235911716E-3,2.0338509783536249E-3,0,9.4180293243241768E-6,2.881711896754217E-6,1.9717768994025872E-2,8.6054271955601919E-2,0.92643961261686059,92.643961261686059,147.5,71.3800443047935,0.713800443047935,509.09586684984947,null,1.2278799038981712E-2,null,0.13662839718447201,3.7671587704291375E-2,3.8881711415337163E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR65, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.643961261686059},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ65, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13662839718447201},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA65, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7671587704291375E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB65, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.8881711415337163E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S65, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":509.09586684984947},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P65, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0621961991131417}]
[null,null,null,null,null,{"$f":"BR106","v":93.285773549830381},{"$f":"I106*1000","v":250},60,0.15,0.11696999999999998,0.20881860299999999,9.2109067890299989E-2,1.0617378101295427,1.0617378101295427,1,1.0617378101295427,9.63667820069204E-7,0.50925110132158591,509251.10132158594,1.963667820069204E-6,0,6.6E-4,0.15362657715490941,4.0121912854166669E-3,0,4.0147685685308467E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,7.8637291473793197E-2,1.8551470831002925E-5,1.8551470831002925E-5,0.10963073932420776,2.2234963158828929E-2,1.5277533039647578E-3,15,18.50825400650681,3.1947613215859039E-2,2.346629074889868E-2,5.6941657268722475E-2,7.9525459933686954E-2,0.10628539776274311,8.4724393331883883E-3,4.1249339207048465E-3,1.5831801938325993E-3,8.7393840665704841E-4,6.5820525211944944E-3,1.507969670534451E-2,1.6197924040564724E-2,3.767813549430922E-2,5.6526872246696041E-3,0.13793597935801027,0.14197480502341378,1.7999999999999998,0.92689153090134868,1.1629297458723825E-2,4.3757746816120843E-3,1.3971807774348016E-2,2.9321522154370047E-2,8.1524239641899549E-4,4.5002561536657617E-4,3.3893604099128039E-3,2.0660367348938357E-3,0,9.5528895550111198E-6,2.8350656390726375E-6,1.9401969272127065E-2,8.5433424452967324E-2,0.92689153090134868,92.689153090134866,150,71.468691685531624,0.71468691685531627,509.25110132158596,null,1.2083725642679363E-2,null,0.13793597935801027,3.767813549430922E-2,4.0147685685308467E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR66, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.689153090134866},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ66, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13793597935801027},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA66, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.767813549430922E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB66, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.0147685685308467E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S66, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":509.25110132158596},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P66, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0617378101295427}]
[null,null,null,null,null,null,null,61,0.1525,0.11691949999999998,0.21131911304999998,9.463432304180501E-2,1.0612794211459442,1.0612794211459442,1,1.0612794211459442,9.6306928164872368E-7,0.50940637161829039,509406.37161829037,1.9630692816487236E-6,0,6.6E-4,0.15606849524594429,4.140753785416668E-3,0,4.1434989388432096E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,7.9830601827227579E-2,1.9118774964292054E-5,1.9118774964292054E-5,0.11139031433218233,2.295443393499141E-2,1.5282191148548712E-3,15,18.287891415644722,3.2186586887515869E-2,2.347344560417082E-2,5.7188251606541562E-2,8.0507258695677639E-2,0.10799127998855661,8.7465874151751201E-3,4.1261916101081528E-3,1.6264530395577424E-3,8.8900758225367998E-4,6.6416522319195752E-3,1.5414838363272768E-2,1.6197924040564724E-2,3.7684684795424216E-2,5.654410724963024E-3,0.13926119257933767,0.14342931591918684,1.83,0.92731976019501861,1.1816489651302517E-2,4.445655114465959E-3,1.3753303075454039E-2,2.8979123369262574E-2,8.2417597956893163E-4,4.5048868742460972E-4,3.3655384453564864E-3,2.0982529001744264E-3,0,9.6880971667266854E-6,2.7898774976403173E-6,1.9096039818315654E-2,8.4841545015989561E-2,0.92731976019501861,92.731976019501857,152.5,71.54830972155635,0.71548309721556347,509.40637161829039,null,1.1894748605798087E-2,null,0.13926119257933767,3.7684684795424216E-2,4.1434989388432096E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR67, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.731976019501857},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ67, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13926119257933767},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA67, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7684684795424216E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB67, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.1434989388432096E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S67, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":509.40637161829039},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P67, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0612794211459442}]
[null,null,null,null,null,null,null,62,0.155,0.11686900000000001,0.21381962309999999,9.7159578193310003E-2,1.0608210321623457,1.0608210321623457,1,1.0608210321623457,9.6247096997348198E-7,0.50956167775236572,509561.67775236577,1.9624709699734817E-6,0,6.5999999999999989E-4,0.15851222416057803,4.2714412854166677E-3,0,4.274362515579529E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,8.1025580569207639E-2,1.9695434119731476E-5,1.9695434119731476E-5,0.11315171459847324,2.3686124455662535E-2,1.5286850332570973E-3,15,18.072714436992587,3.2425702582932925E-2,2.3480602110829016E-2,5.7434989727019041E-2,8.1501956413164295E-2,0.10969893177560237,9.0253917245311979E-3,4.1274495897941632E-3,1.669752088126062E-3,9.0409476268531771E-4,6.7012964406055432E-3,1.5754739940891074E-2,1.6197924040564721E-2,3.7691235608159512E-2,5.6561346230512601E-3,0.14060406658526614,0.14490363016100707,1.8599999999999999,0.92772538890092671,1.2004051628263308E-2,4.5156502108575055E-3,1.3541521787990262E-2,2.8647257086569608E-2,8.32834088884347E-4,4.509417555459825E-4,3.3424531432802006E-3,2.1304970578928236E-3,0,9.8236313324196049E-6,2.7460801401334816E-6,1.8799524845557119E-2,8.427730131631371E-2,0.92772538890092671,92.772538890092676,155,71.619772941093288,0.71619772941093285,509.56167775236577,null,1.1711586411234822E-2,null,0.14060406658526614,3.7691235608159512E-2,4.274362515579529E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR68, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.772538890092676},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ68, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14060406658526614},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA68, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7691235608159512E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB68, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.274362515579529E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S68, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":509.56167775236577},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P68, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0608210321623457}]
[null,null,null,null,null,null,null,63,0.1575,0.11681849999999999,0.21632013314999998,9.9684833344814996E-2,1.0603626431787467,1.0603626431787467,1,1.0603626431787467,9.6187288491465556E-7,0.50971701973622086,509717.01973622083,1.9618728849146555E-6,0,6.6E-4,0.16095768142071795,4.4042537854166669E-3,0,4.4073595662251852E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,8.222215359439812E-2,2.0281447625102387E-5,2.0281447625102387E-5,0.11491488189255437,2.4430045648702485E-2,1.5291510592086626E-3,15,17.862542156064659,3.2664960351285841E-2,2.3487760269445056E-2,5.7681871679939559E-2,8.2509577137183654E-2,0.11140829667023729,9.3088564252227033E-3,4.1287078598633894E-3,1.7130773486102803E-3,9.1919995925395989E-4,6.7609851677276293E-3,1.6099407368860813E-2,1.6197924040564724E-2,3.7697787933038518E-2,5.657858919072052E-3,0.14196463135815504,0.14639777799804699,1.8900000000000001,0.92810943933460355,1.2191972376660049E-2,4.5857554462240911E-3,1.3336158144036183E-2,2.8325444224676848E-2,8.4122923680184992E-4,4.5138526921671061E-4,3.3200709806186562E-3,2.162766937285909E-3,0,9.9594724784274615E-6,2.7036103167816085E-6,1.8511996202479977E-2,8.3739441900795478E-2,0.92810943933460355,92.810943933460351,157.5,71.68387138413388,0.71683871384133879,509.71701973622083,null,1.1533974611058321E-2,null,0.14196463135815504,3.7697787933038518E-2,4.4073595662251852E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR69, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.810943933460351},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ69, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14196463135815504},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA69, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7697787933038518E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB69, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.4073595662251852E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S69, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":509.71701973622083},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P69, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0603626431787467}]
[null,null,null,null,null,null,null,64,{"$f":"IF(PLOT_TYPE=1, H70/100*Iout, min_I*EXP(H70*rr/100))","v":0.16},{"$f":"IF(I70<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I70-Vout)/L*OnTime)","v":0.116768},{"$f":"IF(I70<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I70+((Vin-(Rdcr+RdsonTop)*J70-Vout)/L*OnTime)/2)","v":0.2188206432},{"$f":"IF(I70<Icrit, 0, I70-((Vin-(Rdcr+RdsonTop)*K70-Vout)/L*OnTime)/2)","v":0.10221008849632},1.0599042541951482,{"$f":"IF(I70<Icrit, 1000*SQRT((J70*CoutEsr)^2+(((J70/2)-I70)*(OnTime+OffTime)/Cout)^2), 1000*J70*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":1.0599042541951482},1,{"$f":"IF(I70<Icrit, 1000*((N70/1000)*O70), 1000*J70*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":1.0599042541951482},{"$f":"IF(I70<Icrit, L*J70/(Vout+J70/2*(RdsonBot+Rdcr)), L*J70/(Vout+I70*(RdsonBot+Rdcr)))","v":9.6127502634351956E-7},0.50987239758226999,{"$f":"IF(I70<Icrit,I70/((OnTime+Q70)*J70/2),1/(OnTime+Q70))","v":509872.39758227003},1.9612750263435193E-6,0,{"$f":"S70*(T70*Iq_active+U70*Iq_sleep)","v":6.6E-4},0.16340478942899236,{"$f":"W70^2*Rdcr","v":4.5391912854166674E-3},{"$f":"Core_Loss/1000*S70/$S$106","v":0},{"$f":"(Y70+X70*(1+Ltc*(Ta-25)))/(1-X70*Ltc*ThetaCa)","v":4.5424903626435798E-3},3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,8.3420250932373846E-2,2.087681479686066E-5,2.087681479686066E-5,0.11667976143323788,2.5186208447017019E-2,1.5296171927468101E-3,15,{"$f":"IF(I70<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I70+Iripple/2)*1000000000)","v":17.657201977238763},{"$f":"IF(I70<Icrit, Vin*(I70+Iripple/2)*AK70/1000000000/2*S70, Vin*(I70-Iripple/2)*AJ70/1000000000/2*S70 + Vin*(I70+Iripple/2)*AK70/1000000000/2*S70)","v":3.2904360241773012E-2},{"$f":"IF(I70<Icrit, Csw*(Vin)^2*S70/2, Csw*Vin^2*S70/2)","v":2.3494920080591002E-2},5.7928897515110822E-2,{"$f":"(AI70+AL70+AM70+AH70*(1+RdsonTopTc*(Ta-25)))/(1-AH70*RdsonTopTc*ThetaJA)","v":8.3530145134722622E-2},{"$f":"IF(I70<Icrit,Iripple*SQRT((OffTime)*S70/3), SQRT(OffTime*S70*(I70^2+Iripple^2/12)))","v":0.11311932156290126},9.596985683138293E-3,{"$f":"QgBot*S70*Vdd","v":4.129966420416388E-3},{"$f":"IF(I70<Icrit, Vin*Idss*R70, QrrBot*(I70-Iripple/2)/1*S70*Vin+Vin*Idss*R70)","v":1.7564288300873072E-3},{"$f":"IF(I70<Icrit, dead1*S70*(I70+Iripple/2)*((I70+Iripple/2)*BDserR+VSD), dead1*S70*(I70+Iripple/2)*((I70+Iripple/2)*BDserR+VSD)+dead2*S70*(I70-Iripple/2)*((I70-Iripple/2)*BDserR+VSD))","v":9.3432318326682352E-4},6.8207184337705186E-3,{"$f":"(AR70+AS70+AT70+AQ70*(1+RdsonBotTc*(Ta-25)))/(1-AQ70*RdsonBotTc*ThetaJA)","v":1.6448846608570624E-2},{"$f":"Vin*V70+Vout*Ifb/0.8","v":1.6197924040564724E-2},{"$f":"(Vin-Vdd)*(S70*QgBot+S70*QgTop)+AW70","v":3.7704341770584876E-2},{"$f":"AI70+AR70","v":5.6595836131631983E-3},0.14334291712704134,{"$f":"SUM(Z70,AC70,AF70,AZ70)","v":0.14791178993052345},{"$f":"Vout*I70","v":1.92},0.92847287265793244,1.2380241625525012E-2,4.6559665754038696E-3,{"$f":"Vin*S70*(QgBot+QgTop)/($BB70+$BA70)","v":1.3136924638403489E-2},2.8013234315500995E-2,8.4937318827623634E-4,4.5181965102013104E-4,3.2983604363509516E-3,{"$f":"X70/($BB70+$BA70)","v":2.1950604022472221E-3},{"$f":"Y70/($BB70+$BA70)","v":0},1.0095602190827525E-5,2.6624085555659217E-6,1.8233051310110111E-2,8.3226790153584418E-2,{"$f":"BC70","v":0.92847287265793244},92.847287265793241,{"$f":"I70*1000","v":160},71.741317737155555,0.71741317737155552,{"$f":"S70/1000","v":509.87239758227003},null,{"$f":"AM70/($BB70+$BA70)","v":1.1361664552132745E-2},null,0.14334291712704134,3.7704341770584876E-2,4.5424903626435798E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR70, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.847287265793241},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ70, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14334291712704134},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA70, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7704341770584876E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB70, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.5424903626435798E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S70, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":509.87239758227003},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P70, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0599042541951482}]
[null,null,null,null,null,null,null,65,0.16250000000000001,0.11671749999999997,0.22132115325000001,0.10473534364782501,{"$f":"IF(I71<Icrit, 1000*((((J71/2)-I71)*0.000002/Cout+Vout/306)), 1000*J71*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":1.0594458652115493},1.0594458652115493,{"$f":"ROUNDUP(M71/N71,0)","v":1},1.0594458652115493,9.6067739413144545E-7,0.51002781130293329,510027.81130293332,{"$f":"IF(1/S71-OnTime-Q71>Tsleep, OnTime+Q71+Tsleep, 1/S71)","v":1.9606773941314456E-6},{"$f":"IF(1/S71-OnTime-Q71>Tsleep, 1/S71-OnTime-Q71-Tsleep, 0)","v":0},6.6E-4,{"$f":"IF(I71<Icrit,Iripple*SQRT((OnTime+OffTime)*S71/3), SQRT(I71^2+Iripple^2/12))","v":0.16585347511684323},4.6762537854166675E-3,0,4.6797551810775218E-3,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q71)*S71)","v":3.3183206721673734E-2},{"$f":"RCoutEsr*AA71^2","v":5.5056260416666642E-6},5.5056260416666642E-6,{"$f":"SQRT($R71)*SQRT($I71^2*(1-R71)+(Iripple^2)/12)","v":8.4619806468154798E-2},{"$f":"RCinEsr*AD71^2","v":2.1481534940123919E-5},2.1481534940123919E-5,{"$f":"IF(I71<Icrit,Iripple*SQRT((OnTime)*S71/3), SQRT(OnTime*S71*(I71^2+Iripple^2/12)))","v":0.11844630164000403},{"$f":"RdsonTop*AG71^2","v":2.5954623788560418E-2},{"$f":"QgTop*S71*Vdd","v":1.5300834339088E-3},15,17.456529151039891,3.3143902303615469E-2,2.3502081544839168E-2,{"$f":"AI71+AL71+AM71","v":5.8176067282363436E-2},8.4563684889754673E-2,0.11483195644703506,{"$f":"RdsonBot*AP71^2","v":9.8897836660903175E-3},4.13122527155376E-3,1.7998065416382431E-3,9.4946444603634644E-4,{"$f":"AR71+AS71+AT71","v":6.8804962592283496E-3},1.6803063652241011E-2,1.6197924040564724E-2,3.7710897121322452E-2,5.6613087054625602E-3,0.14473895436878068,0.14944569671083999,1.9500000000000002,0.928816593377493,{"$f":"(AO71-AN71)/($BB71+$BA71)","v":1.2568849791510297E-2},{"$f":"(AV71-AU71)/($BB71+$BA71)","v":4.7262796120700569E-3},1.2943550685208811E-2,{"$f":"AN71/($BB71+$BA71)","v":2.7710203399643401E-2},{"$f":"AS71/(BA71+BB71)","v":8.572770157656204E-4},{"$f":"AT71/($BB71+$BA71)","v":4.5224529861565525E-4},{"$f":"AU71/($BB71+$BA71)","v":3.2772918442272097E-3},2.2273754414047771E-3,0,{"$f":"(AF71)/($BB71+$BA71)","v":1.0232003130054096E-5},{"$f":"(AC71)/($BB71+$BA71)","v":2.6224188843237139E-6},{"$f":"AX71/($BB71+$BA71)","v":1.7962311280736321E-2},{"$f":"SUM(BD71:BO71)","v":8.2738238791196517E-2},0.928816593377493,92.881659337749298,162.5,71.792753953912452,{"$f":"BT71/100","v":0.71792753953912447},510.02781130293334,null,1.1194422214234648E-2,null,{"$f":"AZ71","v":0.14473895436878068},{"$f":"AX71","v":3.7710897121322452E-2},{"$f":"Z71","v":4.6797551810775218E-3},null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR71, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.881659337749298},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ71, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14473895436878068},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA71, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7710897121322452E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB71, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.6797551810775218E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S71, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":510.02781130293334},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P71, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0594458652115493}]
[null,null,null,null,null,null,null,66,0.16500000000000001,0.11666699999999998,0.2238216633,0.10726059879933002,1.0589874762279505,1.0589874762279505,1,1.0589874762279505,9.6007998814990362E-7,{"$f":"OnTime*S72","v":0.5101832609106367},510183.26091063675,1.9600799881499036E-6,0,6.600000000000001E-4,0.16830366962230306,4.8154412854166679E-3,0,4.8191543021506474E-3,3.3183206721673734E-2,5.5056260416666642E-6,{"$f":"AB72","v":5.5056260416666642E-6},8.5820757684565332E-2,2.2095607348658641E-5,{"$f":"AE72","v":2.2095607348658641E-5},0.12021445390530412,2.6735302616338406E-2,1.5305497827319101E-3,15,17.260366333295874,3.3383586586057064E-2,2.3509244662762142E-2,5.8423381031551119E-2,8.5610221104286774E-2,0.11654615419833145,1.0187254543815938E-2,4.1324844133761585E-3,1.8432104923483848E-3,9.6462375888019096E-4,6.9403186646047341E-3,1.7162064523029534E-2,1.6197924040564728E-2,3.771745398577539E-2,5.6630341961080681E-3,{"$f":"AO72+AV72+AX72+AY72","v":0.14615277380919975},0.15099952934474073,1.98,0.92914145345157761,1.2757787929261211E-2,4.7966908099542739E-3,1.2755781391315968E-2,2.7415952104651885E-2,8.6495114943322033E-4,4.5266258654538621E-4,3.2568372583070479E-3,2.2597101590620082E-3,0,1.0368658952943458E-5,2.5835885770277879E-6,1.7699419200422395E-2,8.2272744836483364E-2,0.92914145345157761,{"$f":"100*BQ72","v":92.914145345157763},165,71.838757366287027,0.71838757366287032,510.18326091063676,null,1.1032027149246242E-2,null,0.14615277380919975,3.771745398577539E-2,4.8191543021506474E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR72, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.914145345157763},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ72, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14615277380919975},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA72, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.771745398577539E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB72, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.8191543021506474E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S72, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":510.18326091063676},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P72, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0589874762279505}]
[null,null,null,null,null,null,null,67,0.16750000000000001,0.11661650000000001,0.22632217334999999,0.10978585395083501,1.0585290872443522,1.0585290872443522,1,1.0585290872443522,9.5948280827046035E-7,0.51033874641781174,510338.74641781178,1.9594828082704601E-6,0,6.6E-4,0.1707553079946077,4.9567537854166678E-3,0,4.9606880108688505E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,8.7023045424506701E-2,2.2719031304867272E-5,2.2719031304867272E-5,0.12198417238582479,2.7528255878411047E-2,1.5310162392534355E-3,{"$f":"15*VIN_nom/24","v":15},17.068563173685963,3.3623413138364318E-2,2.3516409434932765E-2,5.8670838812550516E-2,8.6669778699415834E-2,0.11826187037236881,1.0489402487978222E-2,4.1337438459842762E-3,1.8866406913072232E-3,9.7980113312124729E-4,7.0001856704127469E-3,1.7525855275136559E-2,1.6197924040564724E-2,3.7724012364468026E-2,5.6647600852377114E-3,0.14758440642425816,0.15257331909247354,2.0100000000000002,{"$f":"BB73/(BB73+BA73)","v":0.92944825604502457},1.2947047686047982E-2,4.8671966456799347E-3,1.2573376434955593E-2,2.7130103888071546E-2,8.7240542304431738E-4,4.5307186788581203E-4,3.2369703300281086E-3,2.2920627669154705E-3,0,1.0505554241463285E-5,2.545867921822464E-6,1.7444038558793902E-2,8.1829325023585947E-2,0.92944825604502457,92.944825604502455,167.5,71.879846296152991,0.71879846296152994,510.33874641781176,null,1.0874271511312945E-2,null,0.14758440642425816,3.7724012364468026E-2,4.9606880108688505E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR73, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.944825604502455},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ73, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14758440642425816},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA73, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7724012364468026E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB73, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.9606880108688505E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S73, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":510.33874641781176},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P73, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0585290872443522}]
[null,null,null,null,null,null,null,68,0.17,0.11656599999999999,0.2288226834,0.11231110910234002,1.0580706982607533,1.0580706982607533,1,1.0580706982607533,9.5888585436477895E-7,0.51049426783689589,510494.26783689589,1.9588858543647787E-6,0,6.6E-4,0.17320832892310156,5.1001912854166682E-3,0,5.1043565966217485E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,8.8226613671414808E-2,2.3351806079775235E-5,2.3351806079775235E-5,0.12375541381091645,2.8333494527895669E-2,1.5314828035106875E-3,15,16.880975931421037,3.3863382009826581E-2,2.3523575861924162E-2,5.8918440675261433E-2,8.7742382816396056E-2,0.11997906301888546,1.0796231672167266E-2,4.1350035694788572E-3,1.9300971476084495E-3,9.9499658008763521E-4,7.0600972971749422E-3,1.7894441993911658E-2,1.6197924040564724E-2,3.7730572257924991E-2,5.6664863729895447E-3,0.14903388344122226,0.15416709746996546,2.04,0.92973775896661126,1.3136621260236162E-2,4.9377938030469529E-3,1.2396109039148567E-2,2.6852303429031766E-2,8.7964911598300427E-4,4.534734757598629E-4,3.2176661956674806E-3,2.3244315764727125E-3,0,1.0642674437467214E-5,2.5092100086702838E-6,1.7195851811574007E-2,8.1407051591366658E-2,0.92973775896661126,92.973775896661124,170,71.916485184007442,0.71916485184007439,510.49426783689592,null,1.0720959168993354E-2,null,0.14903388344122226,3.7730572257924991E-2,5.1043565966217485E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR74, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.973775896661124},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ74, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14903388344122226},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA74, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7730572257924991E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB74, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.1043565966217485E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S74, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":510.49426783689592},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P74, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0580706982607533}]
[null,null,null,null,null,null,null,69,0.17249999999999999,0.11651549999999999,0.23132319344999999,0.114836364253845,1.0576123092771545,1.0576123092771545,1,1.0576123092771545,9.5828912630462136E-7,0.51064982518033208,510649.82518033206,1.9582891263046211E-6,0,6.6E-4,0.1756626744881602,5.2457537854166663E-3,0,5.250160353184148E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,8.9431409346340196E-2,2.3993930933017992E-5,2.3993930933017992E-5,0.12552813730657891,2.915102952296976E-2,1.531949475540996E-3,15,16.697467115990868,3.4103493249755881E-2,2.35307439443097E-2,5.9166186669606574E-2,8.8828058817716035E-2,0.12169769251113627,1.1107746271901305E-2,4.13626358396069E-3,1.973579870349954E-3,1.0102101111127083E-3,7.1200535654233526E-3,1.8267830795960546E-2,1.6197924040564724E-2,3.7737133666671134E-2,5.6682130595016858E-3,0.15050123633984941,0.15578089625000824,2.0699999999999998,0.93001067781987556,1.3326501363222111E-2,5.0084791586265083E-3,1.2223765030712194E-2,2.6582215153921788E-2,8.8669099176609805E-4,4.5386772472290901E-4,3.1989013731851179E-3,2.3568149921021895E-3,0,1.0780005782888571E-5,2.4735705347020158E-6,1.6954559062956554E-2,8.1005048427533061E-2,0.93001067781987556,93.001067781987558,172.5,71.94908925319227,0.71949089253192267,510.64982518033207,null,1.0571904891426762E-2,null,0.15050123633984941,3.7737133666671134E-2,5.250160353184148E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR75, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.001067781987558},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ75, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15050123633984941},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA75, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7737133666671134E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB75, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.250160353184148E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S75, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":510.64982518033207},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P75, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0576123092771545}]
[null,null,null,null,null,null,null,70,0.17499999999999999,0.11646499999999999,0.23382370349999998,0.11736161940535,1.0571539202935558,1.0571539202935558,1,1.0571539202935558,9.5769262396184528E-7,0.51080541846056915,510805.41846056917,1.9576926239618452E-6,0,6.600000000000001E-4,0.17811828993209353,5.3934412854166666E-3,0,5.3980995787175695E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,9.0637382120234353E-2,2.4645405112828133E-5,2.4645405112828133E-5,0.12730230423356492,2.9980871826873975E-2,1.5324162553817075E-3,15,16.517905151091515,3.4343746907487135E-2,2.3537913682663027E-2,5.9414076845531877E-2,8.9926832288186889E-2,0.12341772138893636,1.142395046462784E-2,4.1375238895306112E-3,2.0170888686338335E-3,1.0254417375350573E-3,7.1800544956995022E-3,1.86460278292527E-2,1.6197924040564728E-2,3.7743696591231536E-2,5.6699401449123183E-3,0.15198649685358345,0.15741474746345552,2.0999999999999996,0.93026768889485867,1.3516681184501287E-2,5.0792497685402923E-3,1.205614197663946E-2,2.6319521883292611E-2,8.9353933339025794E-4,4.5425491203479341E-4,3.1806536675492939E-3,2.3892115046546089E-3,0,1.0917535264851506E-5,2.438907625571713E-6,1.6719876856320821E-2,8.0622487529813824E-2,0.93026768889485867,93.026768889485865,175,71.978028730187987,0.71978028730187982,510.80541846056917,null,1.042693360141791E-2,null,0.15198649685358345,3.7743696591231536E-2,5.3980995787175695E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR76, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.026768889485865},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ76, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15198649685358345},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA76, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7743696591231536E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB76, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.3980995787175695E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S76, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":510.80541846056917},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P76, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0571539202935558}]
[null,null,null,null,null,null,null,71,0.17749999999999999,0.11641449999999998,0.23632421355,0.11988687455685501,1.0566955313099569,1.0566955313099569,1,1.0566955313099569,9.5709634720840557E-7,0.51096104769006179,510961.04769006185,1.9570963472084055E-6,0,6.6E-4,0.18057512344820184,5.5432537854166681E-3,0,5.5481745757717561E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,9.1844484240158855E-2,2.5306227856022368E-5,2.5306227856022368E-5,0.12907787803831045,3.0823032407914952E-2,1.5328831430701855E-3,15,16.342164060006386,3.4584143032377994E-2,2.3545085077558051E-2,5.9662111253006231E-2,9.1038729036040197E-2,0.12513911421414023,1.1744848429724723E-2,4.1387844862895012E-3,2.0606241515663888E-3,1.0406914706985113E-3,7.2401001085544009E-3,1.9029039273229482E-2,1.6197924040564724E-2,3.7750261032131534E-2,5.6716676293596868E-3,0.1534896969707609,0.15906868340043034,2.13,0.93050943182529033,1.3707154359572883E-2,5.150102856312077E-3,1.1893048390529293E-2,2.606392358851272E-2,9.0020197581197722E-4,4.5463531882868432E-4,3.1629020837413984E-3,2.4216196856016218E-3,0,1.1055250565234136E-5,2.4051816713022395E-6,1.6491537063035265E-2,8.025858575418246E-2,0.93050943182529033,93.050943182529039,177.5,72.003632642003467,0.72003632642003468,510.96104769006183,null,1.0285879689106416E-2,null,0.1534896969707609,3.7750261032131534E-2,5.5481745757717561E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR77, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.050943182529039},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ77, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1534896969707609},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA77, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7750261032131534E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB77, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.5481745757717561E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S77, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":510.96104769006183},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P77, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0566955313099569}]
[null,null,null,null,null,null,null,72,0.18,0.11636399999999997,0.23882472359999998,0.12241212970835999,1.0562371423263581,1.0562371423263581,1,1.0562371423263581,9.565002959163541E-7,0.51111671288127059,511116.71288127062,1.9565002959163538E-6,0,6.6E-4,0.18303312598634525,5.6951912854166665E-3,0,5.7003856512862217E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,9.3052670368253362E-2,2.5976398387988455E-5,2.5976398387988455E-5,0.13085482411553348,3.1677522239468327E-2,1.5333501386438119E-3,15,16.170123170860091,3.4824681673808928E-2,2.3552258129568949E-2,5.9910289942021688E-2,9.216377509403717E-2,0.12686183743743326,1.2070444348501307E-2,4.1400453743382923E-3,2.1041857282581302E-3,1.0559593219521429E-3,7.3001904245485645E-3,1.9416871338912966E-2,1.6197924040564724E-2,3.775682698989672E-2,5.6733955129821042E-3,0.15501086893582897,0.16074273661154484,2.16,0.93073651203310837,1.3897914940415989E-2,5.2210358016915072E-3,1.1734303002527225E-2,2.5815136247930311E-2,9.0668633582815638E-4,4.5500921118638124E-4,3.1456267467230678E-3,2.4540381816435474E-3,0,1.1193140014267978E-5,2.3723551752682774E-6,1.6269285860191666E-2,7.9912601823327378E-2,0.93073651203310837,93.073651203310831,180,72.026192211331946,0.72026192211331941,511.11671288127064,null,1.0148586380564085E-2,null,0.15501086893582897,3.775682698989672E-2,5.7003856512862217E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR78, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.073651203310831},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ78, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15501086893582897},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA78, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.775682698989672E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB78, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.7003856512862217E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S78, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":511.11671288127064},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P78, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0562371423263581}]
[null,null,null,null,null,null,null,73,0.1825,0.1163135,0.24132523365,0.124937384859865,1.0557787533427598,1.0557787533427598,1,1.0557787533427598,9.5590446995783993E-7,0.51127241404666113,511272.41404666111,1.9559044699578399E-6,0,6.6E-4,0.18549225107355111,5.8492537854166644E-3,0,5.8547331165918369E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,9.4261897432406094E-2,2.665591592267234E-5,2.665591592267234E-5,0.13263310968145858,3.2544352299981573E-2,1.5338172421399832E-3,15,16.001666840295865,3.5065362881183226E-2,2.3559432839270145E-2,6.0158612962593352E-2,9.3301996720587976E-2,0.12858585927542479,1.240074240419951E-2,4.1413065537779558E-3,2.1477736078237756E-3,1.0712453026502687E-3,7.3603254642519997E-3,1.9809530269015281E-2,1.6197924040564724E-2,3.7763394465052891E-2,5.675123795917939E-3,0.15655004525057409,0.16243693990913027,2.19,0.9309495029799163,1.4088957368300332E-2,5.2920461303605313E-3,1.1579734086924498E-2,2.5572890793373257E-2,9.1299943959676974E-4,4.5537684112869302E-4,3.1288088277241191E-3,2.48646570974294E-3,0,1.1331192547801942E-5,2.3403926151063311E-6,1.6052882789075577E-2,7.9583833571389623E-2,0.9309495029799163,93.09495029799163,182.5,72.045963869077937,0.72045963869077934,511.27241404666114,null,1.0014905156259024E-2,null,0.15655004525057409,3.7763394465052891E-2,5.8547331165918369E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR79, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.09495029799163},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ79, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15655004525057409},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA79, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7763394465052891E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB79, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8547331165918369E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S79, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":511.27241404666114},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P79, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0557787533427598}]
[null,null,null,null,null,null,null,74,0.185,0.11626299999999999,0.24382574369999999,0.12746264001137,1.0553203643591609,1.0553203643591609,1,1.0553203643591609,9.5530886920510762E-7,0.51142815119870566,511428.15119870566,1.9553088692051078E-6,0,6.6E-4,0.18795245464833207,6.0054412854166654E-3,0,6.0112172874124152E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,9.5472124487665788E-2,2.734477966256506E-5,2.734477966256506E-5,0.13441270365672997,3.3423533572977039E-2,1.5342844535961172E-3,15,15.83668419424683,3.5306186703927045E-2,2.3566609207236355E-2,6.0407080364759516E-2,9.4453420400882282E-2,0.13031114959713419,1.2735746781995015E-2,4.1425680247095158E-3,2.1913877993822621E-3,1.086549424152456E-3,7.4205052482442342E-3,2.0207022338048723E-2,1.6197924040564724E-2,3.7769963458126131E-2,5.6768524783056325E-3,0.15810725867536277,0.1641513263684794,2.2199999999999998,0.93114894824293171,1.4280276448719339E-2,5.3631315044422164E-3,1.1429178842172046E-2,2.5336932138771206E-2,9.19147948012246E-4,4.557384475286138E-4,3.1124304762764747E-3,2.5189010525452291E-3,0,1.1469397667897372E-5,2.3092603144670314E-6,1.584209988703068E-2,7.9271615403480433E-2,0.93114894824293171,93.114894824293174,185,72.063171902227168,0.72063171902227163,511.42815119870568,null,9.8846952148514966E-3,null,0.15810725867536277,3.7769963458126131E-2,6.0112172874124152E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR80, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.114894824293174},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ80, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15810725867536277},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA80, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7769963458126131E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB80, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.0112172874124152E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S80, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":511.42815119870568},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P80, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0553203643591609}]
[null,null,null,null,null,null,null,75,0.1875,0.1162125,0.24632625375,0.12998789516287501,1.0548619753755621,1.0548619753755621,1,1.0548619753755621,9.5471349353049914E-7,0.51158392434988176,511583.92434988177,1.9547134935304991E-6,0,6.6E-4,0.19041369490751797,6.1637537854166676E-3,0,6.1698384838663224E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,9.6683312587522399E-2,2.80429887986897E-5,2.80429887986897E-5,0.13619357655816694,3.4315077047054769E-2,1.5347517730496451E-3,15,15.67506888458006,3.5547153191489364E-2,2.3573787234042552E-2,6.0655692198581565E-2,9.5618072848030256E-2,0.1320376798190491,1.3075461668998294E-2,4.1438297872340426E-3,2.2350283120567372E-3,1.1018716978235224E-3,7.4807297971143018E-3,2.0609353852436275E-2,1.6197924040564724E-2,3.7776533969642742E-2,5.6785815602836878E-3,0.15968254223039297,0.16588592932909965,2.25,0.93133536343118362,1.4471867328254969E-2,5.4342897137398529E-3,1.1282482818603577E-2,2.5107018283527099E-2,9.2513818012815397E-4,4.560942569542247E-4,3.0964747574781927E-3,2.5513430541517185E-3,0,1.1607745406455238E-5,2.2789263246363607E-6,1.5636720886127858E-2,7.8975315950696748E-2,0.93133536343118362,93.133536343118365,187.5,72.078010752951272,0.72078010752951271,511.58392434988178,null,9.7578229782517411E-3,null,0.15968254223039297,3.7776533969642742E-2,6.1698384838663224E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR81, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.133536343118365},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ81, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15968254223039297},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA81, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7776533969642742E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB81, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1698384838663224E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S81, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":511.58392434988178},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P81, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0548619753755621}]
[null,null,null,null,null,null,null,76,0.19,0.11616199999999997,0.24882676379999999,0.13251315031438002,1.0544035863919634,1.0544035863919634,1,1.0544035863919634,9.541183428064526E-7,0.51173973351267277,511739.73351267283,1.9541183428064528E-6,0,6.6E-4,0.19287593216452209,6.3241912854166658E-3,0,6.3305970304681171E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,9.7895424664261738E-2,2.8750542510588435E-5,2.8750542510588435E-5,0.13797570039859944,3.5218993715895534E-2,1.5352192005380185E-3,15,15.516718860490959,3.578826239334202E-2,2.3580966920263964E-2,6.0904448514144005E-2,9.6795981004214771E-2,0.13376542280801762,1.3419891254255792E-2,4.1450918414526507E-3,2.2786951549745699E-3,1.1172121350335401E-3,7.5409991314607612E-3,2.1016531150622936E-2,1.6197924040564724E-2,3.7783106000129268E-2,5.6803110419906691E-3,0.16127592919695766,0.16764078239597802,2.2800000000000002,0.93150923795612062,1.4663725473203139E-2,5.505518667641692E-3,1.1139499389638872E-2,2.4882919484012306E-2,9.3097613480029183E-4,4.5644448444755409E-4,3.0809255940240261E-3,2.5837906162136915E-3,0,1.1746226291606702E-5,2.2493603151510028E-6,1.543654047271743E-2,7.8694335903305754E-2,0.93150923795612062,93.150923795612059,190,72.090646982404948,0.72090646982404949,511.73973351267284,null,9.6341616342822678E-3,null,0.16127592919695766,3.7783106000129268E-2,6.3305970304681171E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR82, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.150923795612059},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ82, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16127592919695766},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA82, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7783106000129268E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB82, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.3305970304681171E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S82, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":511.73973351267284},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P82, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0544035863919634}]
[null,null,null,null,null,null,null,77,0.1925,0.11611149999999998,0.25132727384999998,0.135038405465885,1.0539451974083647,1.0539451974083647,1,1.0539451974083647,9.5352341690550287E-7,0.51189557869956803,511895.57869956805,1.953523416905503E-6,0,6.6E-4,0.19533912871806644,6.4867537854166662E-3,0,6.4934932561302311E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,9.9108425417669607E-2,2.946743996630934E-5,2.946743996630934E-5,0.13975904859409405,3.6135294578263734E-2,1.5356867360987042E-3,15,15.361536153615361,3.6029514358979747E-2,2.3588148266476094E-2,6.1153349361554546E-2,9.7987172041854559E-2,0.13549435279130526,1.3769039728751018E-2,4.1463541874665012E-3,2.3223883372673485E-3,1.1325707471578389E-3,7.6013132718916882E-3,2.1428560603187565E-2,1.6197924040564724E-2,3.7789679550112504E-2,5.6820409235652054E-3,0.16288745311871983,0.16941591944085804,2.31,0.93167103666936868,1.4855846649805549E-2,5.5768163876329831E-3,1.1000089262661345E-2,2.4664417487222336E-2,9.3666751070594018E-4,4.5678933424499792E-4,3.0657677125852639E-3,2.6162426943195224E-3,0,1.1884831316625025E-5,2.2205334726205427E-6,1.5241363602535305E-2,7.842810600650249E-2,0.93167103666936868,93.167103666936868,192.5,72.101220909974245,0.7210122090997424,511.89557869956803,null,9.5135907136530539E-3,null,0.16288745311871983,3.7789679550112504E-2,6.4934932561302311E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR83, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.167103666936868},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ83, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16288745311871983},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA83, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7789679550112504E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB83, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.4934932561302311E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S83, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":511.89557869956803},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P83, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0539451974083647}]
[null,null,null,null,null,null,null,78,0.19500000000000001,0.11606100000000001,0.25382778389999999,0.13756366061739,1.0534868084247662,1.0534868084247662,1,1.0534868084247662,9.5292871570028099E-7,0.51205145992306245,512051.45992306242,1.9529287157002807E-6,0,6.6E-4,0.19780324873048302,6.651441285416667E-3,0,6.6585274941646294E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.10032228121142622,3.0193680322393453E-5,3.0193680322393453E-5,0.14154359587794715,3.7063990638010295E-2,1.5361543797691871E-3,15,15.209426675908507,3.6270909137920165E-2,2.3595331273254715E-2,6.1402394790944066E-2,9.9191673364778452E-2,0.13722444527321256,1.4122911285405684E-2,4.1476168253768058E-3,2.3661078680708835E-3,1.1479475455770103E-3,7.6616722390246998E-3,2.1845448612955433E-2,1.6197924040564724E-2,3.7796254620119499E-2,5.6837712051459929E-3,0.16451714780299939,0.17121137460352809,2.34,0.93182120137913149,1.5048226905949159E-2,5.6481810003628534E-3,1.0864120026140008E-2,2.4451304821219329E-2,9.4221772487966939E-4,4.5712900044435692E-4,3.0509865941628789E-3,2.6486982946494503E-3,0,1.2023551911141073E-5,2.1924184070470357E-6,1.5051004866560386E-2,7.8176085204686274E-2,0.93182120137913149,93.182120137913145,195,72.109847935853821,0.72109847935853821,512.05145992306245,null,9.3959956982832497E-3,null,0.16451714780299939,3.7796254620119499E-2,6.6585274941646294E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR84, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.182120137913145},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ84, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16451714780299939},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA84, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7796254620119499E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB84, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.6585274941646294E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S84, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":512.05145992306245},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P84, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0534868084247662}]
[null,null,null,null,null,null,null,79,0.19750000000000001,0.11601049999999999,0.25632829395000001,0.14008891576889501,1.0530284194411674,1.0530284194411674,1,1.0530284194411674,9.5233423906351337E-7,0.51220737719565645,512207.37719565653,1.9523342390635132E-6,0,6.6E-4,0.20026825811479296,6.8182537854166681E-3,0,6.825700082284533E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.10153695997658781,3.0929262723861582E-5,3.0929262723861582E-5,0.1433293182208808,3.8005092904075645E-2,1.5366221315869697E-3,15,15.060300029414648,3.6512446779703785E-2,2.3602515941175854E-2,6.1651584852466607E-2,0.1004095126094109,0.13895567695770611,1.4481510119080783E-2,4.1488797552848185E-3,2.4098537565252127E-3,1.1633425416769083E-3,7.7220760534869393E-3,2.2267201615111296E-2,1.6197924040564724E-2,3.7802831210677526E-2,5.6855018868717886E-3,0.16616504732207149,0.17302718229312156,2.37,0.93196015225558926,1.5240862554207989E-2,5.7196107312186073E-3,1.0731465729900701E-2,2.424338413751188E-2,9.4763192989238011E-4,4.574636676230446E-4,3.0365684280746529E-3,2.6811564708751753E-3,0,1.2162379914465469E-5,2.1649890650016886E-6,1.4865287903289184E-2,7.7937758921573091E-2,0.93196015225558926,93.196015225558924,197.5,72.116619551864289,0.72116619551864292,512.20737719565648,null,9.2812676582924979E-3,null,0.16616504732207149,3.7802831210677526E-2,6.825700082284533E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR85, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.196015225558924},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ85, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16616504732207149},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA85, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7802831210677526E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB85, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.825700082284533E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S85, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":512.20737719565648},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P85, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0530284194411674}]
[null,null,null,null,null,null,null,80,0.2,0.11595999999999999,0.25882880399999997,0.14261417092040002,1.0525700304575687,1.0525700304575687,1,1.0525700304575687,9.5173998686802372E-7,0.51236333052985694,512363.33052985702,1.9517399868680236E-6,0,6.5999999999999989E-4,0.20273412442983874,6.9871912854166671E-3,0,6.9950113626061376E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.10275243112160623,3.1674186304201303E-5,3.1674186304201303E-5,0.14511619275692952,3.8958612390492704E-2,1.537089991589571E-3,15,14.914069327119137,3.6754127333894028E-2,2.3609702270815811E-2,6.1900919596299411E-2,0.10164071764596883,0.14068802567656694,1.4844840426577768E-2,4.1501429772918428E-3,2.4536260117746004E-3,1.1787557468486544E-3,7.782524735915097E-3,2.269382607731325E-2,1.6197924040564721E-2,3.7809409322314094E-2,5.6872329688814139E-3,0.16783118601447758,0.1748633771894296,2.4000000000000004,0.93208828913466457,1.5433750156113932E-2,5.7911038983646801E-3,1.0602006495749871E-2,2.4040467600990476E-2,9.5291502978804056E-4,4.5779351141158996E-4,3.0225000692697119E-3,2.7136163212836076E-3,0,1.2301307550839838E-5,2.1382206490801399E-6,1.4684044853511657E-2,7.7712637464683487E-2,0.93208828913466457,93.208828913466462,200,72.121604042494241,0.72121604042494236,512.36333052985697,null,9.1693029152431303E-3,null,0.16783118601447758,3.7809409322314094E-2,6.9950113626061376E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR86, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.208828913466462},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ86, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16783118601447758},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA86, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7809409322314094E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB86, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.9950113626061376E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S86, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":512.36333052985697},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P86, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0525700304575687}]
[null,null,null,null,null,null,null,81,0.20250000000000001,0.11590949999999998,0.26132931405000004,0.14513942607190503,1.0521116414739697,1.0521116414739697,1,1.0521116414739697,9.5114595898673107E-7,0.51251931993817612,512519.3199381762,1.951145958986731E-6,0,6.6E-4,0.20520081678281238,7.1582537854166673E-3,0,7.1664616816503818E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.10396866544838364,3.2428450185353766E-5,3.2428450185353766E-5,0.14690419771455349,3.9924560116389757E-2,1.5375579598145286E-3,15,14.770651024136935,3.6995950850077279E-2,2.3616890262751159E-2,6.215039907264297E-2,0.10288531657966977,0.14242147032260569,1.5212906406639639E-2,4.1514064914992274E-3,2.4974246429675427E-3,1.1941871724886399E-3,7.8430183069554092E-3,2.3125328499807116E-2,1.6197924040564724E-2,3.7815988955556996E-2,5.6889644513137558E-3,0.16951559848634765,0.17671999424422505,2.4300000000000002,0.93220599272862747,1.5626886507554186E-2,5.8626589072074686E-3,1.0475628155920614E-2,2.384237632345412E-2,9.5807169488168562E-4,4.5811869902615855E-4,3.0087689986930725E-3,2.7460769861060905E-3,0,1.2440327406456194E-5,2.112089543112945E-6,1.4507115854045195E-2,7.7500254543838146E-2,0.93220599272862747,93.220599272862742,202.5,72.124846875437001,0.72124846875436999,512.51931993817618,null,9.0600027294448562E-3,null,0.16951559848634765,3.7815988955556996E-2,7.1664616816503818E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR87, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.220599272862742},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ87, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16951559848634765},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA87, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7815988955556996E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB87, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1664616816503818E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S87, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":512.51931993817618},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P87, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0521116414739697}]
[null,null,null,null,null,"Eff (%)","Iout (mA)",82,0.20499999999999999,0.11585899999999998,0.2638298241,0.14766468122340998,1.051653252490371,1.051653252490371,1,1.051653252490371,9.5055215529265045E-7,0.51267534543313209,512675.34543313214,1.9505521552926505E-6,0,6.6E-4,0.20766830573858236,7.3314412854166644E-3,0,7.3400513903447047E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.10518563507390259,3.3192053477700617E-5,3.3192053477700617E-5,0.14869331235255603,4.0902947105993369E-2,1.5380260362993963E-3,15,14.629964758548436,3.7237917377862834E-2,2.362407991755873E-2,6.2400023331720962E-2,0.10414333775195167,0.14415599078753571,1.5585712259952061E-2,4.1526702980083704E-3,2.5412496592567661E-3,1.2096368299985287E-3,7.9035567872636648E-3,2.3561715415541484E-2,1.6197924040564724E-2,3.7822570110934241E-2,5.6906963343077667E-3,0.17121831961273515,0.17859706868259922,2.46,0.93231362575121435,1.5820268625202537E-2,5.9342742452509565E-3,1.0352221917049013E-2,2.3648939837137051E-2,9.6310637551248529E-4,4.58439389763469E-4,2.9953632864489457E-3,2.7785376450361601E-3,0,1.2579432408098889E-5,2.086573242657136E-6,1.4334348567217322E-2,7.7300165894268705E-2,0.93231362575121435,93.231362575121437,205,72.126370778645395,0.72126370778645399,512.67534543313218,null,8.9532730093396865E-3,null,0.17121831961273515,3.7822570110934241E-2,7.3400513903447047E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR88, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.231362575121437},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ88, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.17121831961273515},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA88, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7822570110934241E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB88, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.3400513903447047E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S88, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":512.67534543313218},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P88, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.051653252490371}]
[null,null,null,null,null,{"$f":"BT51","v":68.427867006324419},{"$f":"I56*1000","v":125},83,0.20749999999999999,0.11580850000000001,0.26633033414999996,0.15018993637491498,1.0511948635067727,1.0511948635067727,1,1.0511948635067727,9.4995857565889325E-7,0.51283140702724872,512831.40702724876,1.9499585756588931E-6,0,6.6E-4,0.21013656323527644,7.5067537854166672E-3,0,7.515780844024867E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.1064033133570111,3.3964995280050889E-5,3.3964995280050889E-5,0.15048351690042244,4.1893784388631498E-2,1.5384942210817463E-3,15,14.491933201245404,3.7480026966882962E-2,2.3631271235815623E-2,6.2649792423780326E-2,0.10541480974170428,0.14589156790413224,1.5963262189144522E-2,4.1539343969207157E-3,2.5851010697992365E-3,1.2251047307852614E-3,7.9641401975052133E-3,2.4002993390283483E-2,1.6197924040564724E-2,3.7829152788974078E-2,5.6924286180024619E-3,0.17293938453896429,0.18049463600431087,2.4899999999999998,0.93241153396421972,1.6013893733900358E-2,6.0059484773113698E-3,1.0231684047601925E-2,2.34599956049787E-2,9.6802331483696849E-4,4.5875573546116786E-4,2.9822715575349157E-3,2.8109975149205094E-3,0,1.2718615803277E-5,2.0616502903388631E-6,1.416559774318641E-2,7.7111947995825936E-2,0.93241153396421972,93.241153396421979,207.5,72.126175499523185,0.72126175499523182,512.83140702724882,null,8.8490240411692317E-3,null,0.17293938453896429,3.7829152788974078E-2,7.515780844024867E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR89, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.241153396421979},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ89, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.17293938453896429},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA89, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7829152788974078E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB89, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.515780844024867E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S89, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":512.83140702724882},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P89, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0511948635067727}]
[null,null,null,null,null,{"$f":"BT81","v":72.078010752951272},{"$f":"I81*1000","v":187.5},84,0.21,0.115758,0.26883084419999997,0.15271519152641999,1.0507364745231738,1.0507364745231738,1,1.0507364745231738,9.4936521995866554E-7,0.51298750473305565,512987.50473305566,1.9493652199586656E-6,0,6.600000000000001E-4,0.21260556250562526,7.6841912854166668E-3,0,7.6936504024367382E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.10762167482997675,3.4747274679627755E-5,3.4747274679627755E-5,0.15227479250272954,4.2897082998736277E-2,1.538962514199167E-3,15,14.356481914197591,3.7722279666792882E-2,2.3638464218099203E-2,6.289970639909126E-2,0.10669976136651201,0.14762818339233832,1.6345560398791408E-2,4.1551987883377516E-3,2.628978883756153E-3,1.2405908862610565E-3,8.0247685583549611E-3,2.4449169022735067E-2,1.6197924040564728E-2,3.7835736990205017E-2,5.6941613025369188E-3,0.174678828681989,0.18241273198514704,2.52,0.9325000471518835,1.6207759254910688E-2,6.0776802410618521E-3,1.0113915586868775E-2,2.3275388564679457E-2,9.7282656073965034E-4,4.5906788092644135E-4,2.9694829599400609E-3,2.8434558476091803E-3,0,1.2857871141727115E-5,2.0373002156566678E-6,1.4000724812457319E-2,7.693519688055081E-2,0.9325000471518835,93.250004715188354,210,72.124237241864293,0.72124237241864297,512.98750473305563,null,8.7471702372919121E-3,null,0.174678828681989,3.7835736990205017E-2,7.6936504024367382E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR90, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.250004715188354},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ90, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.174678828681989},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA90, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7835736990205017E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB90, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.6936504024367382E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S90, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":512.98750473305563},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P90, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0507364745231738}]
[null,null,null,null,null,{"$f":"BT106","v":71.049894896969974},{"$f":"I106*1000","v":250},85,0.21249999999999999,0.11570749999999999,0.27133135424999999,0.155240446677925,1.050278085539575,1.050278085539575,1,1.050278085539575,9.4877208806527003E-7,0.51314363856308831,513143.63856308837,1.9487720880652701E-6,0,6.6E-4,0.21507527800361745,7.8637537854166668E-3,0,7.8736604297381767E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.10884069513445702,3.5538890752055447E-5,3.5538890752055447E-5,0.15406712116730861,4.3912853975846988E-2,1.5394309156892651E-3,15,14.22353921659413,3.7964675527270814E-2,2.3645658864987113E-2,6.3149765307947192E-2,0.10799822168390891,0.14936581980900976,1.6732611095413179E-2,4.1564634723610158E-3,2.6728831102929571E-3,1.2560953078434149E-3,8.0854418904973881E-3,2.4900248944650115E-2,1.6197924040564724E-2,3.7842322715155793E-2,5.6958943880502811E-3,0.17643668773176513,0.18435139267829703,2.5499999999999998,0.93257948002881785,1.6401862794976275E-2,6.1494682428810381E-3,9.9988220738014E-3,2.3094970703853832E-2,9.7751997693130022E-4,4.5937596433539207E-4,2.9569871349189318E-3,2.8759119279523622E-3,0,1.2997192258177582E-5,2.0135034788904379E-6,1.3839597506189299E-2,7.6769527021576911E-2,0.93257948002881785,93.25794800288179,212.5,72.120507778355574,0.72120507778355569,513.14363856308842,null,8.6476299016660738E-3,null,0.17643668773176513,3.7842322715155793E-2,7.8736604297381767E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR91, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.25794800288179},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ91, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.17643668773176513},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA91, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7842322715155793E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB91, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.8736604297381767E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S91, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":513.14363856308842},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P91, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.050278085539575}]
[null,null,null,null,null,null,null,86,0.215,0.11565699999999998,0.27383186430000001,0.15776570182943001,1.0498196965559763,1.0498196965559763,1,1.0498196965559763,9.4817917985210429E-7,0.51329980852988821,513299.80852988828,1.9481791798521044E-6,0,6.6E-4,0.21754568533605378,8.0454412854166664E-3,0,8.0558112945008746E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.11006035096156118,3.6339842561346063E-5,3.6339842561346063E-5,0.15586048571687119,4.4941108364613173E-2,1.5398994255896646E-3,15,14.093036058353979,3.8207214598017965E-2,2.3652855177057251E-2,6.3399969200664874E-2,0.10931021999264552,0.15110446050101661,1.7124418487477467E-2,4.1577284490920954E-3,2.7168137585793332E-3,1.2716180069551231E-3,8.1461602146265522E-3,2.5356239820952045E-2,1.6197924040564724E-2,3.7848909964355415E-2,5.6976278746817596E-3,0.17821299765263474,0.18631065441573863,2.58,0.93265013308670186,1.6596202136118066E-2,6.2213112539814741E-3,9.8863132941403638E-3,2.2918600663834453E-2,9.8210725329875878E-4,4.5968011760548141E-4,2.944774189270174E-3,2.9083650719322089E-3,0,1.3136573256274883E-5,1.9902414187930335E-6,1.3682089502109564E-2,7.6614570296965612E-2,0.93265013308670186,93.265013308670191,215,72.229662267470047,0.72229662267470052,513.29980852988831,null,8.5503250111484217E-3,null,0.17821299765263474,3.7848909964355415E-2,8.0558112945008746E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR92, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.265013308670191},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ92, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.17821299765263474},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA92, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7848909964355415E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB92, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.0558112945008746E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S92, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":513.29980852988831},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P92, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0498196965559763}]
[null,null,null,null,null,null,null,87,0.2175,0.11560649999999999,0.27633237435000002,0.16029095698093498,1.0493613075723776,1.0493613075723776,1,1.0493613075723776,9.4758649519266227E-7,0.51345601464600232,513456.01464600232,1.9475864951926623E-6,0,6.6E-4,0.22001676119862626,8.2292537854166663E-3,0,8.240103369712256E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.1112806199957062,3.71501291598863E-5,3.71501291598863E-5,0.15765486974383167,4.5981857214797382E-2,1.540368043938007E-3,15,13.964905900536415,3.8449896928758567E-2,2.3660053154887787E-2,6.3650318127584357E-2,0.1106357858339674,0.15284408956144466,1.7520986785400185E-2,4.1589937186326193E-3,2.7607708377892113E-3,1.2871589950242555E-3,8.2069235514460864E-3,2.5817148349852166E-2,1.6197924040564724E-2,3.7855498738333104E-2,5.6993617625706264E-3,0.1800077946847233,0.18829055380963711,2.61,0.932712293384511,1.679077522611663E-2,6.2932081067962149E-3,9.7763030444050353E-3,2.2746143369897671E-2,9.8659191556454149E-4,4.599804667431325E-4,2.9328346694638451E-3,2.9408146249192135E-3,0,1.3276008493581743E-5,1.967496203770269E-6,1.352808009404028E-2,7.6469975022643938E-2,0.932712293384511,93.271229338451107,217.5,72.361493645121143,0.72361493645121144,513.45601464600236,null,8.455181011377327E-3,null,0.1800077946847233,3.7855498738333104E-2,8.240103369712256E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR93, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.271229338451107},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ93, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1800077946847233},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA93, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7855498738333104E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB93, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.240103369712256E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S93, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":513.45601464600236},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P93, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0493613075723776}]
[null,null,null,null,null,null,null,88,0.22,0.11555599999999996,0.27883288439999998,0.16281621213244002,1.0489029185887786,1.0489029185887786,1,1.0489029185887786,9.4699403396053203E-7,0.5136122569239836,513612.25692398357,1.946994033960532E-6,0,6.5999999999999989E-4,0.22248848331617826,8.4151912854166684E-3,0,8.4265370327773828E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.11250148086199334,3.796974958842436E-5,3.796974958842436E-5,0.15945025756808542,4.7035111581278252E-2,1.5408367707719507E-3,15,13.839084602216417,3.8692722569239842E-2,2.3667252799057164E-2,6.3900812139068952E-2,0.11197494899290615,0.15458469178866194,1.7922320201546705E-2,4.1602592810842673E-3,2.8047543571007661E-3,1.302718283484178E-3,8.2677319216692118E-3,2.6282981262968706E-2,1.6197924040564721E-2,3.7862089037618354E-2,5.7010960518562182E-3,0.18182111534534942,0.19029112775375689,2.64,0.93276623528662228,1.6985580169624086E-2,6.3651576916036847E-3,9.668708911449728E-3,2.2577469685877663E-2,9.9097733430933031E-4,4.602771321684043E-4,2.9211595374751594E-3,2.9732599600435215E-3,0,1.3415492567564532E-5,1.945250786280834E-6,1.3377453883222031E-2,7.6335405049127447E-2,0.93276623528662228,93.276623528662228,220,72.477313046906502,0.724773130469065,513.61225692398352,null,8.3621266261186822E-3,null,0.18182111534534942,3.7862089037618354E-2,8.4265370327773828E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR94, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.276623528662228},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ94, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.18182111534534942},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA94, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7862089037618354E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB94, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.4265370327773828E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S94, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":513.61225692398352},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P94, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0489029185887786}]
[null,null,null,null,null,null,null,89,0.2225,0.1155055,0.28133339445,0.165341467283945,1.0484445296051803,1.0484445296051803,1,1.0484445296051803,9.4640179602939851E-7,0.51376853537639045,513768.53537639044,1.9464017960293987E-6,0,6.6E-4,0.22496083038683276,8.6032537854166691E-3,0,8.6151126655208982E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.11372291307685344,3.8798702876056684E-5,3.8798702876056684E-5,0.16124663419752014,4.8100882524053409E-2,1.5413056061291714E-3,15,13.715510313420843,3.8935691569232066E-2,2.3674454110144072E-2,6.4151451285505312E-2,0.11332773949958239,0.15632625264803496,1.8328422950232941E-2,4.1615251365487629E-3,2.8487643256964248E-3,1.3182958837735493E-3,8.3285853460187374E-3,2.6753745325446467E-2,1.6197924040564724E-2,3.7868680862740881E-2,5.7028307426779338E-3,0.18365299643044766,0.19231241342488628,2.67,0.93281222115276519,1.7180615219858347E-2,6.4371589533726665E-3,9.5634520664012179E-3,2.2412456091312968E-2,9.9526673340585826E-4,4.6057022901848396E-4,2.9097401481947976E-3,3.0057004766724563E-3,0,1.3555020302494613E-5,1.9234888602110816E-6,1.3230100489774733E-2,7.6210538917174234E-2,0.93281222115276519,93.28122211527652,222.5,72.230234640211876,0.72230234640211877,513.76853537639045,null,8.2710936790497021E-3,null,0.18365299643044766,3.7868680862740881E-2,8.6151126655208982E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR95, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.28122211527652},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ95, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.18365299643044766},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA95, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7868680862740881E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB95, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.6151126655208982E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S95, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":513.76853537639045},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P95, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0484445296051803}]
[null,null,null,null,null,null,null,90,0.22500000000000001,0.11545499999999999,0.28383390450000001,0.16786672243545001,1.0479861406215814,1.0479861406215814,1,1.0479861406215814,9.4580978127304003E-7,0.5139248500157878,513924.85001578782,1.9458097812730401E-6,0,6.6E-4,0.22743378202970055,8.7934412854166685E-3,0,8.8058306541889779E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.11494489700172961,3.9636988040214686E-5,3.9636988040214686E-5,0.16304398529105749,4.9179181108242556E-2,1.5417745500473632E-3,15,13.594123373749889,3.9178803978528576E-2,2.3681657088727503E-2,6.4402235617303447E-2,0.11469418763052136,0.15806875823609803,1.8739299247726507E-2,4.1627912851278821E-3,2.8928007527628673E-3,1.3338918073363276E-3,8.3894838452270772E-3,2.7229447336077191E-2,1.6197924040564724E-2,3.7875274214230654E-2,5.7045658351752449E-3,0.18550347501600445,0.19435444828427531,2.7,0.93285050198344388,1.7375878770836149E-2,6.5092108888108458E-3,9.4604570718948115E-3,2.2250984379428723E-2,9.9946319790849072E-4,4.6085986743159128E-4,2.8985682282970638E-3,3.0381355989862516E-3,0,1.3694586737194827E-5,1.9021948210006922E-6,1.3085914282779871E-2,7.6095069067931995E-2,0.93285050198344388,93.285050198344393,225,72.8349974854723,0.72834997485472297,513.9248500157878,null,8.1820169270441605E-3,null,0.18550347501600445,3.7875274214230654E-2,8.8058306541889779E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR96, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.285050198344393},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ96, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.18550347501600445},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA96, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7875274214230654E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB96, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.8058306541889779E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S96, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":513.9248500157878},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P96, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0479861406215814}]
[null,null,null,null,null,null,null,91,0.22750000000000001,0.11540449999999999,0.28633441454999997,0.17039197758695501,1.0475277516379828,1.0475277516379828,1,1.0475277516379828,9.4521798956533139E-7,0.51408120085474585,514081.20085474587,1.9452179895653313E-6,0,6.6E-4,0.2299073187359057,8.9857537854166683E-3,0,8.9986913894513181E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.11616741379958427,4.0484604086651524E-5,4.0484604086651524E-5,0.16484229712403875,5.0270018404090275E-2,1.5422436025642377E-3,15,13.474866216334767,3.9422059846945759E-2,2.3688861735386691E-2,6.4653165184896694E-2,0.11607432390998057,0.15981219524699536,1.9154953312247827E-2,4.1640577269234421E-3,2.9368636474910266E-3,1.3495060656217701E-3,8.4504274400362383E-3,2.7710094127420547E-2,1.6197924040564724E-2,3.7881869092617912E-2,5.7063013294876798E-3,0.18737258845950672,0.19641727007908635,2.73,0.93288131802414553,1.7571369350104411E-2,6.5813125436017597E-3,9.3596517016182861E-3,2.2092941374402646E-2,1.0035696814390579E-3,4.6114615281275307E-4,2.8876358564572939E-3,3.0705647746446726E-3,0,1.3834187113568199E-5,1.8813537283143066E-6,1.2944794127596901E-2,7.5988701103519657E-2,0.93288131802414553,93.288131802414554,227.5,73.305168165960453,0.73305168165960455,514.08120085474582,null,8.0948339041023009E-3,null,0.18737258845950672,3.7881869092617912E-2,8.9986913894513181E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR97, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.288131802414554},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ97, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.18737258845950672},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA97, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7881869092617912E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB97, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.9986913894513181E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S97, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":514.08120085474582},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P97, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0475277516379828}]
[null,null,null,null,null,null,null,92,0.23,0.11535399999999998,0.28883492459999999,0.17291723273846002,1.0470693626543839,1.0470693626543839,1,1.0470693626543839,9.4462642078024169E-7,0.51423758790584073,514237.58790584077,1.9446264207802415E-6,0,6.6E-4,0.23238142182268645,9.1801912854166667E-3,0,9.1936952664031322E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.11739044539403382,4.1341550009428907E-5,4.1341550009428907E-5,0.16664155655578419,5.1373405486969052E-2,1.5427127637175223E-3,15,13.357683276806679,3.9665459224323074E-2,2.3696068050701142E-2,6.4904240038741734E-2,0.11746817911129018,0.16155655094103022,1.9575389363971268E-2,4.165324462037311E-3,2.9809530190760937E-3,1.3651386700844381E-3,8.5114161511978433E-3,2.8195692565925884E-2,1.6197924040564724E-2,3.788846549843309E-2,5.7080372257548332E-3,0.18926037440140397,0.19850091684385821,2.7600000000000002,0.93290489933137488,1.776708561193345E-2,6.6534630098162391E-3,9.2609667712566131E-3,2.1938218666493387E-2,1.0075890131060656E-3,4.6142918608278613E-4,2.8769354448190802E-3,3.1029874735378259E-3,0,1.3973816865851186E-5,1.8609512710714621E-6,1.2806643149143475E-2,7.5891153094325842E-2,0.93290489933137488,93.290489933137493,230,73.638455592594738,0.73638455592594743,514.23758790584077,null,8.0094847751408533E-3,null,0.18926037440140397,3.788846549843309E-2,9.1936952664031322E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR98, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.290489933137493},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ98, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.18926037440140397},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA98, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.788846549843309E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB98, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1936952664031322E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S98, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":514.23758790584077},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P98, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0470693626543839}]
[null,null,null,null,null,null,null,93,0.23250000000000001,0.11530349999999998,0.29133543465,0.17544248788996503,1.0466109736707851,1.0466109736707851,1,1.0466109736707851,9.4403507479183536E-7,0.51439401118165451,514394.01118165452,1.9440350747918355E-6,0,6.600000000000001E-4,0.23485607339034972,9.376753785416669E-3,0,9.3908426845671911E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.11861397443092959,4.2207824790903657E-5,4.2207824790903657E-5,0.16844175099916925,5.2489353437382355E-2,1.5431820335449634E-3,15,13.24252090697474,3.990900216052308E-2,2.3703276035250642E-2,6.5155460229318687E-2,0.11887578425820625,0.16330181311516945,2.0000611625026296E-2,4.1665914905714019E-3,3.0250688767175212E-3,1.3807896321841988E-3,8.5724499994731217E-3,2.8686249552054611E-2,1.6197924040564728E-2,3.7895063432206916E-2,5.7097735241163653E-3,0.19116687076658415,0.20060542690198391,2.79,0.9329214663032982,1.7963026330938381E-2,6.7256614234856441E-3,9.1643359800058343E-3,2.1786712363728394E-2,1.0115239039913194E-3,4.617090639117113E-4,2.8664597216201335E-3,3.1354031866150257E-3,0,1.4113471610538545E-5,1.8409737346628273E-6,1.2671368509975259E-2,7.5802154929616908E-2,0.9329214663032982,93.292146630329825,232.5,73.832411821820315,0.73832411821820321,514.39401118165449,null,7.9259121989239626E-3,null,0.19116687076658415,3.7895063432206916E-2,9.3908426845671911E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR99, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.292146630329825},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ99, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19116687076658415},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA99, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7895063432206916E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB99, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.3908426845671911E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S99, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":514.39401118165449},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P99, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0466109736707851}]
[null,null,null,null,null,null,null,94,0.23499999999999999,0.11525300000000001,0.29383594469999996,0.17796774304147001,1.0461525846871869,1.0461525846871869,1,1.0461525846871869,9.4344395147427187E-7,0.514550470694775,514550.47069477499,1.9434439514742717E-6,0,6.6E-4,0.23733125628187562,9.5754412854166665E-3,0,9.5901340478958506E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.11983798424221846,4.30834274017146E-5,4.30834274017146E-5,0.17024286839207317,5.361787334096739E-2,1.543651412084325E-3,15,13.12932729293102,4.015268870543142E-2,2.3710485689615233E-2,6.5406825807130975E-2,0.12029717062627611,0.16504797007536354,2.0430624319498575E-2,4.1678588126276778E-3,3.0692112296190214E-3,1.3964589633862299E-3,8.633529005632929E-3,2.9181772020403264E-2,1.6197924040564724E-2,3.7901662894470334E-2,5.7115102247120028E-3,0.19309211576586172,0.20273083886720095,2.82,0.93293123017755153,1.8159190396097542E-2,6.7979069623251669E-3,9.0696957618931623E-3,2.1638322858955859E-2,1.0153769532351877E-3,4.6198587893772478E-4,2.8562017148931569E-3,3.1678114247860592E-3,0,1.4253147136931501E-5,1.8214079701949096E-6,1.2538881202096832E-2,7.572144770832781E-2,0.93293123017755153,93.29312301775515,235,73.8844086186851,0.73884408618685105,514.55047069477496,null,7.8440611994751667E-3,null,0.19309211576586172,3.7901662894470334E-2,9.5901340478958506E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR100, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.29312301775515},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ100, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19309211576586172},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA100, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7901662894470334E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB100, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.5901340478958506E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S100, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":514.55047069477496},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P100, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0461525846871869}]
[null,null,null,null,null,null,null,95,0.23749999999999999,0.1152025,0.29633645474999998,0.18049299819297498,1.0456941957035879,1.0456941957035879,1,1.0456941957035879,9.4285305070180465E-7,0.51470696645779579,514706.96645779576,1.9428530507018047E-6,0,6.6E-4,0.23980695404498453,9.7762537854166661E-3,0,9.791569764773151E-3,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.12106245881192788,4.3968356800769211E-5,4.3968356800769211E-5,0.17204489717056853,5.4758976288498282E-2,1.5441208993733874E-3,15,13.018052377320112,4.0396518908956874E-2,2.371769701437523E-2,6.5658336822705485E-2,0.12173236974421747,0.16679501061055399,2.0865431673431113E-2,4.1691264283081463E-3,3.1133800869885724E-3,1.4121466751610208E-3,8.69465319045774E-3,2.9682266939827284E-2,1.6197924040564724E-2,3.7908263885754551E-2,5.7132473276815341E-3,0.19503614789748083,0.20487719164509641,2.8499999999999996,0.93293439349855922,1.8355576805140012E-2,6.8701988435965269E-3,8.9769851462026713E-3,2.1492954611163111E-2,1.0191506537491845E-3,4.6225971997275581E-4,2.8461547371649142E-3,3.2002117178897165E-3,0,1.439283939826452E-5,1.802241365618303E-6,1.2409095851522724E-2,7.5648783167165501E-2,0.93293439349855922,93.293439349855916,237.5,73.791636151568156,0.73791636151568152,514.70696645779572,null,7.7638790453644722E-3,null,0.19503614789748083,3.7908263885754551E-2,9.791569764773151E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR101, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.293439349855916},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ101, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19503614789748083},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA101, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7908263885754551E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB101, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.791569764773151E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S101, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":514.70696645779572},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P101, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0456941957035879}]
[null,null,null,null,null,null,null,96,{"$f":"IF(PLOT_TYPE=1, H102/100*Iout, min_I*EXP(H102*rr/100))","v":0.24},{"$f":"IF(I102<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I102-Vout)/L*OnTime)","v":0.11515199999999999},{"$f":"IF(I102<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I102+((Vin-(Rdcr+RdsonTop)*J102-Vout)/L*OnTime)/2)","v":0.29883696479999999},{"$f":"IF(I102<Icrit, 0, I102-((Vin-(Rdcr+RdsonTop)*K102-Vout)/L*OnTime)/2)","v":0.18301825334448002},1.0452358067199892,{"$f":"IF(I102<Icrit, 1000*SQRT((J102*CoutEsr)^2+(((J102/2)-I102)*(OnTime+OffTime)/Cout)^2), 1000*J102*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":1.0452358067199892},1,{"$f":"IF(I102<Icrit, 1000*((N102/1000)*O102), 1000*J102*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":1.0452358067199892},9.4226237234878228E-7,0.51486349848331647,514863.49848331651,1.9422623723487822E-6,0,{"$f":"S102*(T102*Iq_active+U102*Iq_sleep)","v":6.6E-4},0.2422831508964941,{"$f":"W102^2*Rdcr","v":9.9791912854166661E-3},{"$f":"Core_Loss/1000*S102/$S$106","v":0},{"$f":"(Y102+X102*(1+Ltc*(Ta-25)))/(1-X102*Ltc*ThetaCa)","v":9.9951502480168965E-3},3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.12228738274413289,4.4862611935230154E-5,4.4862611935230154E-5,0.17384782624372874,5.5912673375888948E-2,1.5445904954499495E-3,15,12.908647785528196,{"$f":"IF(I102<Icrit, Vin*(I102+Iripple/2)*AK102/1000000000/2*S102, Vin*(I102-Iripple/2)*AJ102/1000000000/2*S102 + Vin*(I102+Iripple/2)*AK102/1000000000/2*S102)","v":4.064049282103134E-2},2.3724910010111226E-2,6.5909993326592517E-2,{"$f":"(AI102+AL102+AM102+AH102*(1+RdsonTopTc*(Ta-25)))/(1-AH102*RdsonTopTc*ThetaJA)","v":0.12318141339530973},0.16854292396824977,2.1305037914825416E-2,4.1703943377148639E-3,{"$f":"IF(I102<Icrit, Vin*Idss*R102, QrrBot*(I102-Iripple/2)/1*S102*Vin+Vin*Idss*R102)","v":3.1575754580384224E-3},1.4278527789843784E-3,8.7558225747376654E-3,{"$f":"(AR102+AS102+AT102+AQ102*(1+RdsonBotTc*(Ta-25)))/(1-AQ102*RdsonBotTc*ThetaJA)","v":3.0187741313565535E-2},{"$f":"Vin*V102+Vout*Ifb/0.8","v":1.6197924040564724E-2},{"$f":"(Vin-Vdd)*(S102*QgBot+S102*QgTop)+AW102","v":3.7914866406591016E-2},5.7149848331648134E-3,0.1969990059486311,{"$f":"SUM(Z102,AC102,AF102,AZ102)","v":0.2070445244346249},2.88,0.93293115055652009,1.8552184659275741E-2,6.9425363221001834E-3,8.8861456263625207E-3,2.1350515940052266E-2,1.0228473975822279E-3,4.6253067219556278E-4,2.8363123710829037E-3,3.2326036137247812E-3,0,1.4532544503369772E-5,1.7834618186062572E-6,1.2281930534686705E-2,7.5583923143384871E-2,0.93293115055652009,93.293115055652009,240,73.551124384272143,0.73551124384272137,514.86349848331656,null,7.6853151363135306E-3,null,0.1969990059486311,3.7914866406591016E-2,9.9951502480168965E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR102, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.293115055652009},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ102, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1969990059486311},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA102, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7914866406591016E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB102, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9951502480168965E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S102, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":514.86349848331656},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P102, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0452358067199892}]
[null,null,null,null,null,null,null,97,{"$f":"IF(PLOT_TYPE=1, H103/100*Iout, min_I*EXP(H103*rr/100))","v":0.24249999999999999},0.11510149999999998,0.30133747485000001,0.185543508495985,1.0447774177363904,1.0447774177363904,1,1.0447774177363904,9.4167191628964811E-7,0.51502006678394241,515020.0667839424,{"$f":"IF(1/S103-OnTime-Q103>Tsleep, OnTime+Q103+Tsleep, 1/S103)","v":1.9416719162896482E-6},0,6.6E-4,0.24475983168880741,1.0184253785416668E-2,0,1.0200875914880779E-2,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.1235127412327735,4.5766191740502201E-5,4.5766191740502201E-5,0.17565164496994193,{"$f":"RdsonTop*AG103^2","v":5.7078975704196074E-2},1.5450602003518272E-3,15,12.801066755562964,4.088461049160988E-2,2.3732124677404067E-2,6.616179536936577E-2,0.12464433361879888,0.17029169983156386,{"$f":"RdsonBot*AP103^2","v":2.1749447273642586E-2},4.1716625409499337E-3,3.2017973519850845E-3,1.4435772863374257E-3,8.8170371792724439E-3,3.0698202179365405E-2,1.6197924040564724E-2,3.7921470457511416E-2,5.7167227413017609E-3,0.19898072899697744,0.20923287672964039,2.91,0.93292168780004314,1.8749013158244576E-2,7.0149186882879572E-3,8.7971210367012425E-3,2.1210918832944944E-2,1.0264694809648226E-3,4.6279881733323614E-4,2.8266684559046665E-3,3.2649866771391396E-3,0,1.4672258708841823E-5,1.7650577110610085E-6,1.2157306605869767E-2,7.5526639069810247E-2,0.93292168780004314,93.292168780004317,242.5,73.159788011658193,0.73159788011658189,515.02006678394241,null,7.6083208966064792E-3,null,0.19898072899697744,3.7921470457511416E-2,1.0200875914880779E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR103, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.292168780004317},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ103, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19898072899697744},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA103, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7921470457511416E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB103, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0200875914880779E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S103, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":515.02006678394241},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P103, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0447774177363904}]
[null,null,null,null,null,null,null,98,{"$f":"IF(PLOT_TYPE=1, H104/100*Iout, min_I*EXP(H104*rr/100))","v":0.245},0.11505099999999999,0.30383798489999997,0.18806876364749001,1.0443190287527917,1.0443190287527917,1,1.0443190287527917,9.4108168239893983E-7,0.51517667137228451,515176.67137228459,{"$f":"IF(1/S104-OnTime-Q104>Tsleep, OnTime+Q104+Tsleep, 1/S104)","v":1.94108168239894E-6},0,6.6E-4,0.24723698187838591,1.0391441285416666E-2,0,1.0408747187056512E-2,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.12473852003319941,4.6679095140218672E-5,4.6679095140218672E-5,0.17745634313462749,{"$f":"RdsonTop*AG104^2","v":5.8257894379622109E-2},1.5455300141168538E-3,15,12.695264071410859,4.1128871970670652E-2,2.3739341016834874E-2,6.641374300162238E-2,0.12612116271131521,0.17204132829760985,{"$f":"RdsonBot*AP104^2","v":2.2198663981804478E-2},4.1729310381155059E-3,3.2460457780493449E-3,1.4593202087066106E-3,8.8782970248714611E-3,3.1213656609608727E-2,1.6197924040564724E-2,3.7928076039047687E-2,5.7184610522323601E-3,0.20098135641220399,0.2114422883204424,2.94,0.93290618422426186,1.8946061595661912E-2,7.0873452664877669E-3,8.7098574365275881E-3,2.1074078763161329E-2,1.0300191090534998E-3,4.6306423383191754E-4,2.8172170747899493E-3,3.2973604891729661E-3,0,1.481197841166758E-5,1.7470178851350255E-6,1.2035148534882868E-2,7.5476711499866594E-2,0.93290618422426186,93.290618422426192,245,72.614496083320674,0.72614496083320679,515.17667137228455,null,7.5328496748346702E-3,null,0.20098135641220399,3.7928076039047687E-2,1.0408747187056512E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR104, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.290618422426192},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ104, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20098135641220399},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA104, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7928076039047687E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB104, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0408747187056512E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S104, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":515.17667137228455},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P104, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0443190287527917}]
[null,null,null,null,null,null,null,99,{"$f":"IF(PLOT_TYPE=1, H105/100*Iout, min_I*EXP(H105*rr/100))","v":0.2475},0.11500050000000001,0.30633849494999998,0.19059401879899501,1.0438606397691932,1.0438606397691932,1,1.0438606397691932,9.4049167055128938E-7,0.51533331226096024,515333.31226096029,{"$f":"IF(1/S105-OnTime-Q105>Tsleep, OnTime+Q105+Tsleep, 1/S105)","v":1.9404916705512892E-6},0,6.6E-4,0.24971458749607187,1.0600753785416667E-2,0,1.0618764490676023E-2,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.12596470543532984,4.7601321046228245E-5,4.7601321046228245E-5,0.17926191092925986,{"$f":"RdsonTop*AG105^2","v":5.9449440513518303E-2},1.545999936782881E-3,15,12.591195999672104,4.1373277308215065E-2,2.3746559028985051E-2,6.6665836273982995E-2,0.12761193322830502,0.17379179985716564,{"$f":"RdsonBot*AP105^2","v":2.2652692273194837E-2},4.1741998293137791E-3,3.2903207454562694E-3,1.4750815575837043E-3,8.9396021323537526E-3,3.173411171143839E-2,1.6197924040564724E-2,3.7934683151732027E-2,5.7201997660966605E-3,0.20300092785757212,0.21367279929533603,2.9699999999999998,0.93288481173610882,1.9143329354640855E-2,7.1598154132327622E-3,8.6243030010311368E-3,2.093991451908582E-2,1.0334984003960892E-3,4.6332699701746811E-4,2.8079525428405883E-3,3.3297246462522796E-3,0,1.4951700142289802E-5,1.7293316206631733E-6,1.1915383754300495E-2,7.5433929660560464E-2,0.93288481173610882,93.288481173610876,247.5,71.912167665597565,0.71912167665597559,515.33331226096027,null,7.458856649540443E-3,null,0.20300092785757212,3.7934683151732027E-2,1.0618764490676023E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR105, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.288481173610876},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ105, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20300092785757212},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA105, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7934683151732027E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB105, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0618764490676023E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S105, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":515.33331226096027},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P105, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0438606397691932}]
[null,null,null,null,null,null,null,100,{"$f":"IF(PLOT_TYPE=1, H106/100*Iout, min_I*EXP(H106*rr/100))","v":0.25},0.11495,0.308839005,0.19311927395049999,1.0434022507855945,1.0434022507855945,1,1.0434022507855945,9.3990188062142279E-7,0.51548998946259217,515489.98946259223,{"$f":"IF(1/S106-OnTime-Q106>Tsleep, OnTime+Q106+Tsleep, 1/S106)","v":1.9399018806214226E-6},0,6.6E-4,0.25219263511913531,1.0812191285416665E-2,0,1.0830928256313608E-2,3.3183206721673734E-2,5.5056260416666642E-6,5.5056260416666642E-6,0.12719128423832268,4.8532868358581379E-5,4.8532868358581379E-5,0.18106833893161101,{"$f":"RdsonTop*AG106^2","v":6.0653625222387611E-2},1.5464699683877766E-3,15,12.488820229286935,4.1617826554267656E-2,2.3753778714436249E-2,6.6918075237091673E-2,0.12911667798547499,0.17554310537551901,{"$f":"RdsonBot*AP106^2","v":2.3111536383660428E-2},4.1754689146469978E-3,3.3346222634351953E-3,1.4908613444658061E-3,9.0009525225479992E-3,3.2259574626885591E-2,1.6197924040564724E-2,3.7941291796096871E-2,5.7219388830347748E-3,0.20503948329149221,0.21592445004220606,3,0.93285773549830375,1.9340815903671812E-2,7.2323285156877196E-3,8.5404079185400199E-3,2.0808348043192818E-2,1.0369093911367947E-3,4.6358717924677617E-4,2.7988693958372903E-3,3.3620787594294279E-3,0,1.50914205580745E-5,1.7119886139098847E-6,1.1797942515595764E-2,{"$f":"SUM(BD106:BO106)","v":7.539809103151042E-2},0.93285773549830375,93.285773549830381,250,71.049894896969974,0.71049894896969978,515.48998946259223,null,7.386298740358936E-3,null,0.20503948329149221,3.7941291796096871E-2,1.0830928256313608E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR106, IF(MODE_ILIM=4,#REF!,#REF!))","v":93.285773549830381},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ106, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20503948329149221},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA106, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7941291796096871E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB106, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0830928256313608E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S106, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":515.48998946259223},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P106, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0434022507855945}]
[null,null,null,null,null,null,null,null,{"$f":"Losses!$E$5/1000","v":0.5},0.10989999999999998,0.55889001000000005,0.44564478910100003,0.99756335242572247,0.99756335242572247,1,0.99756335242572247,{"$f":"IF(I107<Icrit, L*J107/(Vout+J107/2*(RdsonBot+Rdcr)), L*J107/(Vout+I107*(RdsonBot+Rdcr)))","v":8.820224719101121E-7},{"$f":"OnTime*S107","v":0.5313432835820896},{"$f":"IF(I107<Icrit,I107/((OnTime+Q107)*J107/2),1/(OnTime+Q107))","v":531343.28358208959},{"$f":"IF(1/S107-OnTime-Q107>Tsleep, OnTime+Q107+Tsleep, 1/S107)","v":1.8820224719101122E-6},{"$f":"IF(1/S107-OnTime-Q107>Tsleep, 1/S107-OnTime-Q107-Tsleep, 0)","v":0},6.5999999999999989E-4,{"$f":"IF(I107<Icrit,Iripple*SQRT((OnTime+OffTime)*S107/3), SQRT(I107^2+Iripple^2/12))","v":0.50109991539445842},4.2687191285416676E-2,0,4.2980747668990509E-2,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q107)*S107)","v":3.3183206721673734E-2},{"$f":"RCoutEsr*AA107^2","v":5.5056260416666642E-6},{"$f":"AB107","v":5.5056260416666642E-6},{"$f":"SQRT($R107)*SQRT($I107^2*(1-R107)+(Iripple^2)/12)","v":0.25067803080326767},{"$f":"RCinEsr*AD107^2","v":1.8851842538221203E-4},{"$f":"AE107","v":1.8851842538221203E-4},{"$f":"IF(I107<Icrit,Iripple*SQRT((OnTime)*S107/3), SQRT(OnTime*S107*(I107^2+Iripple^2/12)))","v":0.36526825262997226},{"$f":"RdsonTop*AG107^2","v":0.24682865830180348},{"$f":"QgTop*S107*Vdd","v":1.5940298507462689E-3},15,{"$f":"IF(I107<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I107+Iripple/2)*1000000000)","v":6.8882012646307018},6.6808182089552234E-2,{"$f":"IF(I107<Icrit, Csw*(Vin)^2*S107/2, Csw*Vin^2*S107/2)","v":2.4484298507462688E-2},9.2886510447761181E-2,0.35710412473925579,{"$f":"IF(I107<Icrit,Iripple*SQRT((OffTime)*S107/3), SQRT(OffTime*S107*(I107^2+Iripple^2/12)))","v":0.3541222266691969},{"$f":"RdsonBot*AP107^2","v":9.4051913565862538E-2},{"$f":"QgBot*S107*Vdd","v":4.3038805970149266E-3},7.9004582686567175E-3,{"$f":"IF(I107<Icrit, dead1*S107*(I107+Iripple/2)*((I107+Iripple/2)*BDserR+VSD), dead1*S107*(I107+Iripple/2)*((I107+Iripple/2)*BDserR+VSD)+dead2*S107*(I107-Iripple/2)*((I107-Iripple/2)*BDserR+VSD))","v":3.1639498543455224E-3},1.5368288720017166E-2,0.11148882861388132,1.6197924040564721E-2,3.8609983742057263E-2,{"$f":"AI107+AR107","v":5.8979104477611954E-3},{"$f":"AO107+AV107+AX107+AY107","v":0.5131008475429556},0.55627561926336999,{"$f":"Vout*I107","v":6},{"$f":"BB107/(BB107+BA107)","v":0.91515371659651645},4.0299955284854354E-2,1.4660844887522251E-2,{"$f":"Vin*S107*(QgBot+QgTop)/($BB107+$BA107)","v":4.3179957331376658E-3},1.4167572542991632E-2,{"$f":"AS107/(BA107+BB107)","v":1.2050222912294792E-3},{"$f":"AT107/($BB107+$BA107)","v":4.825834113882186E-4},2.3440577566420048E-3,{"$f":"X107/($BB107+$BA107)","v":6.5108902926525828E-3},{"$f":"Y107/($BB107+$BA107)","v":0},{"$f":"(AF107)/($BB107+$BA107)","v":2.8753889605909063E-5},{"$f":"(AC107)/($BB107+$BA107)","v":8.3974902237030251E-7},5.8890116865457963E-3,{"$f":"SUM(BD107:BO107)","v":8.9907527525592279E-2},{"$f":"BC107","v":0.91515371659651645},{"$f":"100*BQ107","v":91.515371659651649},{"$f":"I107*1000","v":500},72.049894896970002,{"$f":"BT107/100","v":0.72049894896970001},{"$f":"S107/1000","v":531.34328358208961},null,{"$f":"AM107/($BB107+$BA107)","v":3.7344827962271696E-3},null,0.5131008475429556,3.8609983742057263E-2,4.2980747668990509E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR107, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.515371659651649},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ107, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.5131008475429556},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA107, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.8609983742057263E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB107, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.2980747668990509E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S107, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":531.34328358208961},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P107, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.99756335242572247}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BD107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":4.0299955284854354E-2},{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BE107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":1.4660844887522251E-2},null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BG107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":1.4167572542991632E-2},null,null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BJ107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":2.3440577566420048E-3},{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BK107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":6.5108902926525828E-3},{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BL107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":0},null,null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BO107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":5.8890116865457963E-3}]
[null,null,null,null,null,null,null,1.0000000000000001E-5,"A","min_I",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Load (A)","High-side MOSFET Rdson %","Low-side MOSFET Rdson %","Gate Drive (Qg) Loss from Vin %","High-side MOSFET Switching Loss %","Reverse Recovery & Leakage Loss %","Deadtime Loss %",null,"Inductor Cu Loss %","Inductor Core Loss %","Cin ESR %","Cout ESR %","Quiescent Current Loss %","Total Loss %","Overall Eff %"]
[null,null,null,null,null,null,null,{"$f":"Iout","v":0.25},"A","max_I",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"I107","v":0.5},{"$f":"BD107","v":4.0299955284854354E-2},{"$f":"BE107","v":1.4660844887522251E-2},4.3179957331376658E-3,1.4167572542991632E-2,1.2050222912294792E-3,4.825834113882186E-4,null,6.5108902926525828E-3,0,2.8753889605909063E-5,8.3974902237030251E-7,5.8890116865457963E-3,8.9907527525592279E-2,0.91515371659651645]
[null,null,null,null,null,null,null,{"$f":"LOG(max_I/min_I,EXP(1))","v":10.126631103850338},null,"rr",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10mA",{"$f":"BD70","v":1.2380241625525012E-2},{"$f":"BE70","v":4.6559665754038696E-3},1.3136924638403489E-2,2.8013234315500995E-2,8.4937318827623634E-4,4.5181965102013104E-4,null,2.1950604022472221E-3,0,1.0095602190827525E-5,2.6624085555659217E-6,1.8233051310110111E-2,8.3226790153584418E-2,0.92847287265793244]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"50ma",{"$f":"BD85","v":1.5240862554207989E-2},{"$f":"BE85","v":5.7196107312186073E-3},1.0731465729900701E-2,2.424338413751188E-2,9.4763192989238011E-4,4.574636676230446E-4,null,2.6811564708751753E-3,0,1.2162379914465469E-5,2.1649890650016886E-6,1.4865287903289184E-2,7.7937758921573091E-2,0.93196015225558926]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"100mA",{"$f":"BD91","v":1.6401862794976275E-2},{"$f":"BE91","v":6.1494682428810381E-3},9.9988220738014E-3,2.3094970703853832E-2,9.7751997693130022E-4,4.5937596433539207E-4,null,2.8759119279523622E-3,0,1.2997192258177582E-5,2.0135034788904379E-6,1.3839597506189299E-2,7.6769527021576911E-2,0.93257948002881785]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"500mA",{"$f":"BD106","v":1.9340815903671812E-2},{"$f":"BE106","v":7.2323285156877196E-3},8.5404079185400199E-3,2.0808348043192818E-2,1.0369093911367947E-3,4.6358717924677617E-4,null,3.3620787594294279E-3,0,1.50914205580745E-5,1.7119886139098847E-6,1.1797942515595764E-2,7.539809103151042E-2,0.93285773549830375]

{"sheet":"Design EMI Filter","index":7,"n_rows":33,"n_cols":15,"rows_kept":33,"cut":false,"hidden":false,"merged":[[0,0,0,22],[32,10,32,12],[29,10,29,12],[31,10,31,12]]}
["                         LM5168/9 100V, Low IQ DC/DC Converter Design Tool  "]
[]
[]
[]
[]
[]
["Step 7: EMI Filter (Optional)"]
[null,null,null,"Desired Maximum Noise Level, Vnoise(MAX)",50,"dBmV"]
[null,null,null,"EMI Filter Inductance, LF(EMI)",22,"mH"]
[null,null,null,"Minimum EMI Filter Capacitance",{"$f":"'Variable Mgmt'!M164","v":0.33323934770334135},"mF"]
[null,null,null,"EMI Filter Capacitance, CF(EMI)",4.7,"mF"]
[null,null,null,"Minimum EMI Filter Damping Capacitance",{"$f":"'Variable Mgmt'!M168","v":8.8000000000000007},"mF"]
[null,null,null,"EMI Filter Damping Capacitance, CD(EMI)",10,"mF"]
[null,null,null,"Minimum Damping Capacitor ESR",{"$f":"'Variable Mgmt'!M169","v":3.1622776601683795},"Ω"]
[null,null,null,"Damping Capacitor ESR, ESR CD(EMI)",3.3,"Ω"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"EMI Filter BOM"]
[null,null,null,null,null,null,null,"Count","Ref Des","Value","Description",null,null,"Part Number","MFR"]
[null,null,null,null,null,null,null,1,"LF(EMI)",{"$f":"'Variable Mgmt'!B298","v":"22µH"},{"$f":"\"Inductor, \"&Lf_emi*1000000&\" µH, \"&ROUNDUP(Isat_min,2)&\"A\"","v":"Inductor, 22 µH, 0.51A"},null,null,"Std","Std"]
[null,null,null,null,null,null,null,1,"CF(EMI)",{"$f":"'Variable Mgmt'!B299","v":"4.7µF"},{"$f":"IF(VIN_max>35, \"Capacitor, Ceramic, \"&'Variable Mgmt'!B299&\", 120V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B299&\", 50V, X7R, 10%\")","v":"Capacitor, Ceramic, 4.7µF, 120V, X7R, 10%"},null,null,"Std","Std"]
[null,null,null,null,null,null,null,1,"CD(EMI)",{"$f":"'Variable Mgmt'!B300","v":"10µF"},{"$f":"IF(VIN_max>35, \"Capacitor, Electrolytic, \"&'Variable Mgmt'!B300&\", 120V, ESR>\"&ESR_Cd&ohm, \"Capacitor, Electrolytic, \"&'Variable Mgmt'!B300&\", 50V, ESR>\"&ESR_Cd&ohm)","v":"Capacitor, Electrolytic, 10µF, 120V, ESR>3.3Ω"},null,null,"Std","Std"]

{"sheet":"EVM","index":8,"n_rows":85,"n_cols":15,"rows_kept":85,"cut":false,"hidden":true,"merged":[[0,0,0,16]]}
["LM5163/4 100V, Low IQ DC/DC Converter Design Tool  "]
[]
[null,"LM5164-Q1EVM-041 PCB Layout"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Top"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer 2"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer 3"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bottom"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer"]

{"sheet":"BOM & Schematic","index":9,"n_rows":53,"n_cols":13,"rows_kept":53,"cut":false,"hidden":true,"merged":[[0,0,0,16],[29,3,29,5],[41,3,41,5],[47,7,47,9],[30,3,30,5],[43,3,43,5],[44,3,44,5],[42,3,42,5],[39,3,39,5],[40,3,40,5],[38,3,38,5],[37,3,37,5],[36,3,36,5],[31,3,31,5],[34,3,34,5],[32,3,32,5],[33,3,33,5]]}
["                         LM5163/4 100V Low IQ DC/DC Converter Design Tool  "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[{"$f":"\"VIN = \"&Vin&\" V, VOUT = \"&Vout&\" V, IOUT = \"&Iout&\" A \"&'Variable Mgmt'!B35&\" Converter\"","v":"VIN = 24 V, VOUT = 12 V, IOUT = 0.25 A COT Converter"}]
["Low IQ, High Efficiency, Synchronous Buck Converter BOM"]
["Count","Ref Des","Value","Description",null,null,"Size","Part Number","MFR","Footprint (mm)","Area (mm2)"]
[{"$f":"ROUNDUP('Design Converter'!E37/10,0)","v":1},"CIN",{"$f":"Cin*1000000","v":2.2000000000000002},{"$f":"IF(VIN_max>35, \"Capacitor, Ceramic, \"&'Variable Mgmt'!B257&\", 100V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B257&\", 50V, X7R, 10%\")","v":"Capacitor, Ceramic, 2.2µF, 100V, X7R, 10%"},null,null,5,"Std","Std",{"$f":"CHOOSE(G31,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)","v":"3.2 x 2.5"},{"$f":"CHOOSE(G31,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45)","v":8}]
[{"$f":"'Variable Mgmt'!D252","v":2},"COUT",{"$f":"'Variable Mgmt'!F253","v":"22µF"},{"$f":"CHOOSE(Cout_Voltage_Rating, \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 6.3V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 10V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 16V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 25V, X7R, 10%\",  \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 50V, X7R, 10%\")","v":"Capacitor, Ceramic, 22µF, 16V, X7R, 10%"},null,null,5,"Std","Std",{"$f":"CHOOSE(G32,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)","v":"3.2 x 2.5"},{"$f":"(CHOOSE(G32,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45))*A32","v":16}]
[{"$f":"CHOOSE(MODE, \"-\", \"-\", \"1\",\"-\")","v":"1"},{"$f":"CHOOSE(MODE,\"-\",\"-\",\"Ca\",\"-\")","v":"Ca"},{"$f":"CHOOSE(MODE, \"-\",\"-\",'Variable Mgmt'!B293, \"-\")","v":"3300pF"},{"$f":"CHOOSE(MODE,\"-\",\"-\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B293&\", 16V, X7R, 10%\", \"-\")","v":"Capacitor, Ceramic, 3300pF, 16V, X7R, 10%"},null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"-\", \"Std\", \"-\")","v":"Std"},{"$f":"H33","v":"Std"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G33,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G33,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[{"$f":"CHOOSE(MODE, \"-\", \"1\", \"1\",\"-\")","v":"1"},{"$f":"CHOOSE(MODE,\"-\",\"Cff\",\"Cb\",\"-\")","v":"Cb"},{"$f":"CHOOSE(MODE, \"-\",'Variable Mgmt'!B290,'Variable Mgmt'!B290, \"-\")","v":"56pF"},{"$f":"CHOOSE(MODE,\"-\",\"Capacitor, Ceramic, \"&'Variable Mgmt'!B290&\", 50V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B290&\", 50V, X7R, 10%\", \"-\")","v":"Capacitor, Ceramic, 56pF, 50V, X7R, 10%"},null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"Std\", \"Std\", \"-\")","v":"Std"},{"$f":"H34","v":"Std"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G34,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G34,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G34,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G34,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"CBST","2.2nF","Capacitor, Ceramic, 2.2nF, 25V, X7R, 10%",null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"Std\", \"Std\", \"-\")","v":"Std"},{"$f":"H35","v":"Std"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G35,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G35,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G35,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G35,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[]
[1,"LF",{"$f":"'Design Converter'!E17","v":100},{"$f":"\"Inductor, \"&Lf*1000000&\" µH, \"&Rdcr*1000&\" mΩ, >\"&ROUNDUP(Isat_min,2)&\"A\"","v":"Inductor, 100 µH, 170 mΩ, >0.51A"},null,null,4,"Various","Various",{"$f":"CHOOSE(G37,'Variable Mgmt'!T50,'Variable Mgmt'!T51,'Variable Mgmt'!T52,'Variable Mgmt'!T53,'Variable Mgmt'!T54,'Variable Mgmt'!T55,'Variable Mgmt'!T56)","v":"6.0 x 6.0"},{"$f":"CHOOSE(G37,'Variable Mgmt'!U50,'Variable Mgmt'!U51,'Variable Mgmt'!U52,'Variable Mgmt'!U53,'Variable Mgmt'!U54,'Variable Mgmt'!U55,'Variable Mgmt'!U56)","v":36}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(MODE_RSET=2,CHOOSE(G38,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":""}]
[{"$f":"CHOOSE(MODE, \"1\",\"1\",\"1\", \"-\")","v":"1"},"RT",{"$f":"CHOOSE(MODE, 'Design Converter'!E13, 'Design Converter'!E13,'Design Converter'!E13,\"-\")","v":60.4},{"$f":"C39","v":60.4},null,null,1,{"$f":"CHOOSE(MODE, \"Std\",\"Std\",\"Std\",\"-\")","v":"Std"},{"$f":"H39","v":"Std"},{"$f":"CHOOSE(MODE,CHOOSE(G39,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G39,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G39,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,CHOOSE(G39,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G39,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G39,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"RFB1",{"$f":"Rfb1_/1000","v":453},453,null,null,1,{"$f":"CHOOSE(MODE_VOUT,\"-\",\"Std\")","v":"Std"},{"$f":"H40","v":"Std"},{"$f":"(CHOOSE(MODE_VOUT,\"\",CHOOSE(G40,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)))","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE_VOUT,\"\",CHOOSE(G40,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45))","v":0.5}]
[1,"RFB2",{"$f":"Rfb2_u/1000","v":49.9},49.9,null,null,1,{"$f":"CHOOSE(MODE_VOUT,\"-\",\"Std\")","v":"Std"},{"$f":"H41","v":"Std"},{"$f":"CHOOSE(MODE_VOUT,\"\",CHOOSE(G41,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45))","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE_VOUT,\"\",CHOOSE(G41,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45))","v":0.5}]
[{"$f":"IF(MODE=3,\"1\",\"-\")","v":"1"},{"$f":"CHOOSE(MODE,\"-\",\"-\",\"Ra\",\"-\")","v":"Ra"},{"$f":"'Variable Mgmt'!F296","v":"182k"},{"$f":"\"Resistor, Chip, \"&'Variable Mgmt'!B296&\", 1/16W, 1%\"","v":"Resistor, Chip, 182kΩ, 1/16W, 1%"},null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"-\", \"Std\", \"-\")","v":"Std"},{"$f":"H42","v":"Std"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G42,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G42,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"RPGOOD",100,100,null,null,1,"Std","Std",{"$f":"CHOOSE(G43,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)","v":"1.0 x 0.5"},{"$f":"CHOOSE(G43,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45)","v":0.5}]
[{"$f":"CHOOSE(MODE_UVLO, \"1\", \"-\")","v":"1"},"RUV1",{"$f":"CHOOSE(MODE_UVLO, 'Variable Mgmt'!H275, \"-\")","v":"1M"},{"$f":"CHOOSE(MODE_UVLO, \"Resistor, Chip, \"&'Variable Mgmt'!C275&\", 1/16W, 1%\", \"-\")","v":"Resistor, Chip, 1MΩ, 1/16W, 1%"},null,null,2,{"$f":"CHOOSE(MODE_UVLO,\"Std\",\"-\")","v":"Std"},{"$f":"H44","v":"Std"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G44,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.6 x 0.8"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G44,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":1.3}]
[{"$f":"CHOOSE(MODE_UVLO, \"1\", \"-\")","v":"1"},"RUV2",{"$f":"CHOOSE(MODE_UVLO, 'Variable Mgmt'!H276, \"-\")","v":"332k"},{"$f":"CHOOSE(MODE_UVLO, \"Resistor, Chip, \"&'Variable Mgmt'!C276&\", 1/16W, 1%\", \"-\")","v":"Resistor, Chip, 332kΩ, 1/16W, 1%"},null,null,1,{"$f":"CHOOSE(MODE_UVLO,\"Std\",\"-\")","v":"Std"},{"$f":"H45","v":"Std"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G45,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G45,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"U1",{"$f":"CHOOSE(VARIANT, \"LM5163-Q1\", \"LM5164-Q1\")","v":"LM5163-Q1"},{"$f":"CHOOSE(VARIANT, \"IC, LM51643-Q1, Buck Converter, 6V–100V Input\", \"IC, LM5164-Q1, Buck Converter, 6V–100V Input\")","v":"IC, LM51643-Q1, Buck Converter, 6V–100V Input"},null,null,"SOIC-8",{"$f":"CHOOSE(VARIANT, \"LM5163QDDATQ1\", \"LM5164QDDATQ1\")","v":"LM5163QDDATQ1"},"TI","5.0 x 6.0",30]
[]
[null,{"$f":"\"Total Solution Size (padded by 15%) = \"&ROUND(K48,1)&\" mm^2 = \"&ROUND(M48,3)&\" in^2\"","v":"Total Solution Size (padded by 15%) = 110.2 mm^2 = 0.171 in^2"},null,null,null,null,null,null,null,null,{"$f":"SUM(K31:K46)*1.15","v":110.16999999999999},null,{"$f":"K48/25.4/25.4","v":0.17076384152768304}]
[]
["NOTES:"]
["* Inductor saturation current should be higher than the peak inductor current setting for all operating temperatures *"]
["** Effective input and output capacitances should be appropriately derated for applied voltage and temperature, particularly with ceramics **"]
["***Estimated total solution size does not include EMI filter***"]

{"sheet":"Schematic Mgmt","index":10,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
[]
[{"$f":"'Variable Mgmt'!K27","v":"SCH_COT3_LM5168"}]

{"sheet":"sch_frank","index":11,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
[]
[{"$f":"CHOOSE(MODE,\"cot1_sch\",\"cot2_sch\",\"cot3_sch\")","v":"cot3_sch"}]

{"sheet":"Efficiency Plots","index":12,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
[]
[{"$f":"IF(PLOT_TYPE=1, \"EFF_LINEAR\", \"EFF_LOG\")","v":"EFF_LINEAR"}]