{"text_format":"1","workbook":"xlsx","n_sheets":13,"sheets":["Instructions","Design Converter","Fsw & Ripple","Losses","Variable Mgmt","Standard Value Calculator","Efficiency","Design EMI Filter","EVM","BOM & Schematic","Schematic Mgmt","sch_frank","Efficiency Plots"],"not_rendered":{"charts":6,"images":28,"macros":1,"external_links":0,"defined_names":209,"comments":4,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Instructions","index":0,"n_rows":74,"n_cols":3,"rows_kept":74,"cut":false,"hidden":true,"merged":[[0,0,0,16],[7,1,9,15],[16,2,17,15],[11,1,14,15],[18,2,19,15],[65,1,66,15],[69,1,70,15],[73,1,74,15],[77,1,78,15],[20,2,21,15],[50,1,52,15],[54,1,55,15],[56,1,57,15],[60,1,62,15],[24,1,26,15],[38,1,39,15],[41,1,43,15],[46,1,47,15],[28,1,28,15],[29,1,31,15],[33,1,35,15]]}
["                         LM5164 Low IQ DC/DC Converter Design Tool  "]
[]
[]
[null,"Design Regulator tab"]
[null,"Start with Step 1, and then work down towards the bottom of the worksheet."]
[]
[null,"Step 1. Operating Specifications"]
[null,"First, enter the values in the yellow shaded cells to define the power supply parameters.  If a particular specification is not known, enter an estimate. It can be changed later, if necessary, to optimize component values.  Cells  with a red mark in the upper right corner have a comment to provide additional information.  Hold the cursor over the cell to read the comment.  A red font indicates an erroneous entry and requires an adjustment to the entry.  Consult the entry's comments for the entry specific requirements."]
[]
[]
[]
[null,"Second, select a desired mode of operation. PFM mode requires the fewest external components and the lowest inductance.  As a result, it can provide the smallest solution size. At light loads, a PFM converter has a relatively longer sleep time interval and thus operates at lower input quiescent current levels.  COT mode offers nearly constant switching frequency, relatively higher conversion efficiencies at medium to heavy loads, and enables the lowest output voltage ripple.  Options COT1, COT2, and COT3 enable you to select a ripple generation method (a requirement for the stable operation in COT mode):"]
[]
[]
[]
[]
[null,"-COT1: ","Type 1 ripple generation method requires a single resistor in series with the output capacitor.  It is the simplest, the most compact, and the most economical method that works with fixed and adjustable device options, however, the output voltage ripple is the highest."]
[]
[null,"-COT2: ","Type 2 ripple generation method requires a feedforward capacitor in addition to the series resistor.  The feedforward capacitor reduces the required minimum value of the series resistor and ultimately the output voltage ripple by the VOUT / 1.223V factor.  It only works with an adjustable device option (i.e. external feedback resistor network)."]
[]
[null,"-COT3:","Type 3 ripple generation method three external components to generate and inject required voltage ripple into the FB node.  In return, it provides the lowest output voltage ripple. It also only works with an adjustable device option (i.e. external feedback resistor network)."]
[]
[]
[null,"Step 2. Filter Inductor"]
[null,"First, select an inductor current limit level.  In PFM Mode, 1.25A, 0.75A, 0.5A, and 1.25A - MOD options are available.  For the 500mA max load, select either 1.25A or 1.25A - MOD option.  The 1.25A - MOD option enables higher efficiency at the expense of slightly worse transient operation.  For the 300mA and 200mA max loads, select 0.75A and 0.5A options respectively. In COT Mode, 0.75A and 0.5A options are available.   For the 500mA and 300mA max loads, select 0.75A and 0.5A options respectively."]
[]
[]
[]
[null,"Second, select the filter inductance value based on the suggested value. Enter the inductor RDC for accurate efficiency estimates."]
[null,"In PFM mode, selected inductance defines the switching frequency.  You may select lower or higher inductance to increase or decrease the switching frequency.  Watch the minimum output capacitance.  At very low switching frequencies, the required minimum capacitance may become excessive."]
[]
[]
[]
[null,"In COT mode, the suggested inductance is  derived based on the target inductor (peak-to-peak) ripple current of 40% of the DC full load output current at nominal input voltage. It may be acceptable to use higher ripple current with the proviso that peak inductor current remains below the ILIM setting.  Pk-to-Pk Ripple Current value will turn red if this is violated.  If this happens, increase the selected inductance or decrease the Input Voltage (max) or both."]
[]
[]
[]
[null,"Step 3. Output Capacitors and Ripple Generation"]
[null,"First, select the output capacitance based on the minimum recommended value.  Make sure that the nominal capacitance is appropriately derated for applied voltage, especially with ceramics.  For PFM and COT3 modes, ensure that the capacitor ESR does not exceed the maximum allowable value.  "]
[]
[]
[null,"Second, for COT modes, select the values for the ripple generation components based on the minimum recommended values.  Ensure that the output voltage ripple meets any of your minimum ripple requirements by reviewing the VOUT Ripple vs. IOUT plot in the fSW&Ripple tab.  For accurate output voltage ripple estimates in COT3 mode, ensure that the Output Capacitor ESR is set to the levels of a typical ceramic capacitor ESR (e.g. 10 mW)."]
[]
[]
[]
[null,"Step 4. Input Capacitors"]
[null,"Select the input capacitance based on the minimum recommended value.  Make sure that the nominal capacitance is appropriately derated for applied voltage, especially with ceramics.  "]
[]
[]
[null,"Step 5. Feedback, Soft-Start, UVLO"]
[null,"First, review the feedback resistor network. With an adjustable device option, an external feedback resistor network is required. The resistor values are automatically calculated based on the selected VOUT in Step 1.  For lowering the leakage current through the resistors, adjust the upper FB resistor (R1) until the lower FB resistor (R2) reaches its upper end of the range (100kW).  Keeping the upper FB resistor below 1MW is recommended."]
[]
[]
[]
[null,"Second, select one out of three soft-start configurations.  If the external soft-start option is selected, enter a desired soft start time.  "]
[]
[null,"Third, select one out of the two UVLO options.  If the external UVLO option is selected, define desired UVLO thresholds and hysteresis.  Keeping the upper UVLO resistor at 1MW or higher is recommended for the minimum leakage current."]
[]
[]
[null,"Step 6. Efficiency and Thermals"]
[null,"Enter the LM5166's junction-to-ambient thermal impedance (dependent on your PCB design, air flow, etc.) and ambient temperature. Device power dissipation and junction temperature are derived at the maximum load.  Ensure that the junction temperature is within the recommended range."]
[]
[]
[]
[null,"BOM & Schematic tab"]
[null,"This tab summarizes the converter schematic and BOM.  It also helps you estimate the total solution size. Select a package size for each external component (i.e. inductor, capacitors, and resistors) for accurate solution size estimates."]
[]
[]
[null,"Design EMI Filter tab"]
[null,"In case an EMI filter is needed, a simple EMI filter design aid is given in this tab.  It is based on the guidelines documented in TI's literature number SNVA489C (aka AN-2162).  Suggest reviewing the note before using the design aid."]
[]
[]
[null,"fSW & Ripple tab"]
[null,"In this tab, the switching/burst frequency (COT/PFM mode) and the output voltage ripple as a function of the load current are plotted."]

{"sheet":"Design Converter","index":1,"n_rows":58,"n_cols":17,"rows_kept":58,"cut":false,"hidden":false,"merged":[[2,14,2,15],[0,0,0,16]]}
["                          LM5168/9 Low IQ DC/DC Converter Design Tool  "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"http://www.ti.com/ww/en/analog/power_management/widevin"]
["About",null,"xx",null,null,"= Input Box",null,null,null,null,null,null,null,null,"Terms Of Use",null,"                "]
[]
["Step 1: Operating Specifications"]
[null,null,null,"Input Voltage - Min, VIN(min) ",48,"V"]
[null,null,null,"Input Voltage - Nom, VIN(nom)",68,"V"]
[null,null,null,"Input Voltage - Max, VIN(max)",75,"V"]
[null,null,null,"Output Voltage, VOUT ",3.3,"V"]
[null,null,null,"Full Load Current, IOUT",0.3,{"$f":"IF('Variable Mgmt'!B84>'Variable Mgmt'!B86,\"CURRENT LIMIT\",\"A\")","v":"A"}]
[null,null,null,"Mode of Operation",null,null,{"$f":"MODE","v":3}]
[null,null,null,"Switching Frequency at VIN(nom)",750,"kHz"]
[null,null,null,"Timing Resistance, RT",{"$f":"'Standard Value Calculator'!J4/1000","v":11},"kΩ"]
[]
["Step 2: Buck Inductor"]
[null,null,null,"Recommended Buck Inductance ",{"$f":"Lopt*1000000","v":34.887254901960787},"µH"]
[null,null,null,"Inductance, LF ",33,"µH"]
[null,null,null,"Inductor DCR ",170,"mΩ"]
[null,null,null,{"$f":"CHOOSE(MODE, \"Pk-to-Pk Ripple Current\",\"Pk-to-Pk Ripple Current\",\"Pk-to-Pk Ripple Current\", \"Resulting PFM Switching Frequency\")","v":"Pk-to-Pk Ripple Current"},{"$f":"Iripple_Vinnom*1000","v":135.30427867592505},"mApk-pk"]
[null,null,null,{"$f":"CHOOSE(MODE, 'Variable Mgmt'!H88,'Variable Mgmt'!H88,'Variable Mgmt'!H88, 'Variable Mgmt'!H89)","v":"% Ripple Current at Nom VIN"},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), 'Variable Mgmt'!B96*100, Ilim/2*1000)","v":45.101426225308352},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), \"%\", \"mA\")","v":"%"}]
[]
[{"$f":"IF(MODE=4, \"Step 3: Output Capacitors\", \"Step 3: Output Capacitors, Ripple Generation\")","v":"Step 3: Output Capacitors, Ripple Generation"}]
[null,null,null,"Minimum Output Capacitance ",{"$f":"'Variable Mgmt'!B116","v":3.996100386098465},"µF"]
[null,null,null,"Output Capacitance, COUT ",33,"µF"]
[null,null,null,{"$f":"IF(OR(MODE=1,MODE=2),\"Recommended Series Resistance\",IF(MODE=3,\"Maximum Allowable ESR\",\"*Higher Cout Improves Light-Load Eff\"))","v":"Maximum Allowable ESR"},{"$f":"'Variable Mgmt'!B272","v":0.122},"Ω"]
[null,null,null,{"$f":"IF(OR(MODE=1,MODE=2),\"Total ESR & Series Resistance, Rser\",IF(MODE=3,\"Output Capacitor ESR\",\"*PFM Hysteresis Sets Output Ripple\"))","v":"Output Capacitor ESR"},2.5000000000000001E-3,"Ω"]
[null,null,null,{"$f":"CHOOSE(MODE, \"Resulting Output Voltage Ripple\",\"Resulting Output Voltage Ripple\", \"Output Voltage Ripple\",\"Output Voltage Ripple\")","v":"Output Voltage Ripple"},{"$f":"CHOOSE(MODE, Vripple2*1000,Vripple2*1000,Vripple2*1000, PFM_Ripple)","v":0.7624921486709193},"mVpk-pk"]
[null,null,null,{"$f":"IF(MODE=1,\"\",IF(MODE=2,\"Minimum Feedforward Capacitance\", IF(MODE=3,\"Minimum Coupling Capacitance\",\"\")))","v":"Minimum Coupling Capacitance"},{"$f":"'Variable Mgmt'!B140","v":">47"},"pF"]
[null,null,null,{"$f":"IF(MODE=1,\"\",IF(MODE=2,\"Feedforward Capacitance, Cff\", IF(MODE=3,\"Coupling Capacitance, Cb\",\"\")))","v":"Coupling Capacitance, Cb"},56,"pF"]
[null,null,null,{"$f":"IF(MODE=3,\"Minimum Ripple Generation Capacitance\",\"\")","v":"Minimum Ripple Generation Capacitance"},{"$f":"'Variable Mgmt'!B144","v":">81"},"pF"]
[null,null,null,{"$f":"IF(MODE=3,\"Ripple Generation Capacitance, Ca\",\"\")","v":"Ripple Generation Capacitance, Ca"},3300,"pF"]
[null,null,null,{"$f":"IF(MODE=3,\"Ripple Generation Resistance, Ra\",\"\")","v":"Ripple Generation Resistance, Ra"},{"$f":"Ra","v":31.6},"kΩ"]
[null,null,null,{"$f":"IF(MODE=3,\"Amplitude of Injected Ripple\",\"\")","v":"Amplitude of Injected Ripple"},40,"mVpk-pk"]
[]
["Step 4: Input Capacitors"]
[null,null,null,"Minimum Input Capacitance ",{"$f":"'Variable Mgmt'!B157","v":2.2000000000000002},"µF"]
[null,null,null,"Input Capacitance, CIN ",40,"µF"]
[null,null,null,"Maximum Allowable ESR",{"$f":"'Variable Mgmt'!B159","v":9.246526341482431},"Ω"]
[null,null,null,"Input Capacitor ESR ",3,"mΩ"]
[null,null,null,"Resulting Input Voltage Ripple ",{"$f":"CHOOSE(MODE, Vinripple2*1000,Vinripple2*1000,Vinripple2*1000, 'Variable Mgmt'!B165*1000)","v":1.5977655271749269},"mVpk-pk"]
[]
["Step 5: Feedback, PGOOD, UVLO"]
[null,null,null,"Upper Feedback Resistor, RFB1 ",453,"kΩ"]
[null,null,null,"Lower Feedback Resistor, RFB2",{"$f":"IF(Vout=Vref,\"OPEN\",Rfb2_u/1000)","v":261},{"$f":"IF(Vout=Vref,\"\",\"kΩ\")","v":"kΩ"}]
[null,null,null,"Acutal Output Voltage Setpoint",{"$f":"'Variable Mgmt'!B201","v":3.2827586206896551},"V"]
[null,null,null,"PGOOD Pull-up Resistance",20,{"$f":"\"kΩ\"","v":"kΩ"},null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,"BST Capacitance, CBST ",2.2000000000000002,"nF"]
[null,null,null,{"$f":"\"Required Input Voltage UVLO Turn-on\"","v":"Required Input Voltage UVLO Turn-on"},6,"V"]
[null,null,null,"Upper UVLO Resistor, RUV1",1,"MΩ"]
[null,null,null,"Lower UVLO Resistor, RUV2",{"$f":"'Variable Mgmt'!F276","v":332},{"$f":"'Variable Mgmt'!G276","v":"kΩ"}]
[null,null,null,"Actual UVLO Turn-on Threshold",{"$f":"'Variable Mgmt'!B186","v":6.0180722891566267},"V"]
[null,null,null,"Actual UVLO Turn-off Threshold",{"$f":"'Variable Mgmt'!B187","v":5.6168674698795176},"V"]
[]
["Step 6: Efficiency & Thermals"]
[null,null,null,"Estimated Thermal Impedance, JJA",33,"°C/W"]
[null,null,null,"Ambient Temp, TA",25,"°C"]
[null,null,null,"IC Power Dissipation at Full Load, PD",{"$f":"'Variable Mgmt'!B26","v":1.1592207770612202},"W"]
[null,null,null,"IC Junction Temp at Full Load, TJ",{"$f":"E56+E55*'Variable Mgmt'!B26","v":63.254285643020268},"°C"]

{"sheet":"Fsw & Ripple","index":2,"n_rows":1,"n_cols":1,"rows_kept":1,"cut":false,"hidden":true,"merged":[[0,0,0,16]]}
["                         LM5164 Low IQ DC/DC Converter Design Tool  "]

{"sheet":"Losses","index":3,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":true,"merged":[[0,0,0,16]]}
["                         LM5166 Low IQ DC/DC Converter Design Tool  "]
[]
[]
[]
[null,null,null,"Load Current",500,"mA"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"Inductor Core Loss Constant",0]

{"sheet":"Variable Mgmt","index":4,"n_rows":320,"n_cols":21,"rows_kept":320,"cut":false,"hidden":true,"merged":[[4,4,4,7],[0,0,0,8]]}
["EXCEL Variables Names/Calculations",null,null,null,null,null,null,null,null,null,null,"LM5166"]
[null,"Input from user ="]
[null,"Output ="]
[null,"Constant"]
["Variable Name","Value","STD Units",null,"Notes",null,null,null,"Iteration"]
["Step 1: Operational Specs"]
["VIN_min",{"$f":"'Design Converter'!E6","v":48},"V","Minimum input voltage",null,null,null,null,1]
["VIN_nom",{"$f":"'Design Converter'!E7","v":68},"V","Nominal input voltage"]
["VIN_max",{"$f":"'Design Converter'!E8","v":75},"V","Maximum input voltage"]
[]
["Vout",{"$f":"'Design Converter'!E9","v":3.3},"V","Output Voltage",null,null,null,null,1]
["Iout",{"$f":"'Design Converter'!E10","v":0.3},"A","Maximum Output Current",null,null,null,null,1]
["Rout",{"$f":"Vout/Iout","v":11},"W","Load resistance"]
["Pout",{"$f":"Vout*Iout","v":0.98999999999999988},"W","Output power"]
[]
["Efficiency",0.9,null,"Estimate of efficiency"]
["Pin",{"$f":"Pout/Efficiency","v":1.0999999999999999},"W","Calculate input power assuming 90% efficiency"]
["Iin_Vinmin",{"$f":"Pin/VIN_min","v":2.2916666666666665E-2},"A"]
["Iin_Vinnom",{"$f":"Pin/VIN_nom","v":1.6176470588235292E-2},"A","Input currents at min, nom, max Vin"]
["Iin_Vinmax",{"$f":"Pin/VIN_max","v":1.4666666666666665E-2},"A"]
[]
["Fsw",{"$f":"'Design Converter'!E12*1000","v":750000},"Hz","Nominal Switching Frequency",null,null,null,null,1]
["Vref",1.2,"V","Reference Voltage"]
["Rt",{"$f":"Vout*2500000000/Fsw","v":11000},"W","Frequency Set Resistor"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"B34&\"_\"&F35&\"_\"&F39&\"_\"&I41&\"_\"&I36","v":"COT3_VOUTadj_UVLOadj_SSAdj_RsetGND"},null,null,null,null,null,"Vout<5V",100,1]
["Internal PD at Full Load",{"$f":" IF(OR(MODE=1,MODE=2,MODE=3), Efficiency!AZ106,#REF!)","v":1.1592207770612202},"W",null,null,null,null,null,null,null,null,null,null,null,null,null,"Vout<=8V",47,2]
[null,null,null,null,null,null,null,null,null,null,{"$f":"\"SCH_\"&B34&\"_\"&B41","v":"SCH_COT3_LM5168"},null,null,null,null,null,"Vout<=12V",22,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vout<=20V",22,4]
["Step 2: Circuit Configuration for COT / PFM, Fixed / Adj Vout, ILIM, UVLO, SS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vout>20V",10,5]
[null,"COT Type I",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cout Capacitance",{"$f":"CHOOSE(S30,\"100\", \"47\",\"22\",\"22\",\"10\")","v":"100"},{"$f":"IF(Vout<5, 1, IF(Vout<=8, 2, IF(Vout<=12, 3, IF(Vout<=20, 4, 5))))","v":1}]
[null,"COT Type II",2]
["COT/PFM ","COT Type III",3]
[null,null,null,null,"VOUT Fixed/Adjustable","Fixed",1,null,"ILIM shorted",1,{"$f":"B34&\", \"&F35&\", \"&I36&\", \"&F39&\", \"&I41","v":"COT3, VOUTadj, RsetGND, UVLOadj, SSAdj"},null,null,null,null,null,"Vout<=5V","6.3V",1]
["MODE",{"$f":"CHOOSE(C34, \"COT1\", \"COT2\",\"COT3\")","v":"COT3"},3,null,null,"Adjustable",2,null,"ILIM resistor needed",2,{"$f":"C34&\", \"&G35&\", \"&J36&\", \"&G39&\", \"&J41","v":"3, 2, 1, 1, 1"},null,null,null,null,null,"Vout<=8V","10V",2]
[null,{"$f":"IF(MODE=4, \"PFM\", \"COT\")","v":"COT"},null,null,"MODE_VOUT",{"$f":"CHOOSE(G35, \"VOUTfixed\", \"VOUTadj\")","v":"VOUTadj"},{"$f":"IF(AND(OR(MODE=1,MODE=4),OR(Vout=3.3,Vout=5)),1,2)","v":2},null,null,null,{"$f":"C34&G35&J36&G39&J41","v":"32111"},null,null,null,null,null,"Vout<=12V","16V",3]
[null,null,null,null,null,null,null,"MODE_RSET",{"$f":"CHOOSE(J36, \"RsetGND\",\"Rset\")","v":"RsetGND"},1,null,null,null,null,null,null,"Vout<=20V","25V",4]
[null,null,null,null,"UVLO","Adjustable",1,null,null,null,null,null,null,null,null,null,"Vout>20V","50V",5]
[null,null,null,null,null,"Internal",2,"Soft Start","Adjustable",1,null,"Iout Linear Axis",1,null,null,null,"Cout Voltage Rating",{"$f":"CHOOSE(S38,\"6.3V\", \"10V\",\"16V\",\"25V\",\"50V\")","v":"6.3V"},{"$f":"IF(Vout<=5, 1, IF(Vout<=8, 2, IF(Vout<=12, 3, IF(Vout<=20, 4, 5))))","v":1}]
[null,"LM5168",1,null,"MODE_UVLO",{"$f":"CHOOSE(G39, \"UVLOadj\", \"UVLOint\")","v":"UVLOadj"},1,null,"3ms Fixed",2,null,"Iout Log Axis",2]
[null,"LM5169",2,null,null,null,null,null,null,null,null,"PLOT_TYPE",1]
["VARIANT",{"$f":"CHOOSE(VARIANT, \"LM5168\", \"LM5169\")","v":"LM5168"},1,null,"ESR","NO",1,"MODE_SS",{"$f":"CHOOSE(J41, \"SSAdj\", \"SSfix\")","v":"SSAdj"},1,null,null,null,null,null,null,null,"0402",1,"1.0 x 0.5",0.5]
[null,null,null,null,null,"YES",2,null,null,null,null,null,null,null,null,null,null,"0603",2,"1.6 x 0.8",1.3]
[null,null,null,null,"MODE_ESR",null,2,null,null,null,null,null,null,null,null,null,null,"0805",3,"2.0 x 1.25",2.5]
[null,null,null,null,null,{"$f":"CHOOSE(G44, \"\", \"_ESR\")","v":"_ESR"},{"$f":"IF(MODE=2, 1, MODE_ESR)","v":2},null,null,null,null,null,null,null,null,null,null,"1206",4,"3.2 x 1.6",5.0999999999999996]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1210",5,"3.2 x 2.5",8]
["Step 3: Buck Inductor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Component Size",{"$f":"CHOOSE(S46,\"0402\", \"0603\",\"0805\",\"1206\",\"1210\")","v":"1210"},5,{"$f":"CHOOSE(S46,T41,T42,T43,T44,T45)","v":"3.2 x 2.5"}]
["Don1",{"$f":"Vout/VIN_nom","v":4.8529411764705876E-2},{"$f":"(Vout-VIN_nom)/Vout","v":-19.606060606060609},null,"Ideal Duty Cycle at VIN(nom)",null,null,null,1]
["Doff1",{"$f":"1-47:47","v":0.95147058823529407},null,null,"Ideal 1- Duty Cycle at VIN(nom)",null,null,null,1]
[]
["Don_Vinmin",{"$f":"Vout/VIN_min","v":6.8749999999999992E-2},{"$f":"IF(VIN_min>Vout, \"BUCK\", \"BOOST\")","v":"BUCK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3mm x 3mm",1,"3.0 x 3.0",9]
["Don_Vinnom",{"$f":"Vout/VIN_nom","v":4.8529411764705876E-2},{"$f":"IF(VIN_nom>Vout, \"BUCK\", \"BOOST\")","v":"BUCK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4mm x 4mm",2,"4.0 x 4.0",16]
["Don_Vinmax",{"$f":"Vout/VIN_max","v":4.3999999999999997E-2},{"$f":"IF(VIN_max>Vout, \"BUCK\", \"BOOST\")","v":"BUCK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5mm x 5mm",3,"5.0 x 5.0",25]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6mm x 6mm",4,"6.0 x 6.0",36]
["Lf_Vinmin",{"$f":"(VIN_min-Vout)*Don_Vinmin/(Fsw*Iout*0.4)","v":3.4145833333333328E-5},"H","COT",null,null,null,null,null,null,null,null,null,null,null,null,null,"7mm x 7mm",5,"7.0 x 7.0",49]
["Lf_Vinnom",{"$f":"(VIN_nom-Vout)*Don_Vinnom/(Fsw*Iout*0.4)","v":3.4887254901960786E-5},"H","COT",null,null,null,null,1,null,null,null,null,null,null,null,"Inductor Size","8mm x 8mm",6,"8.0 x 8.0",64]
["Lf_Vinmax",{"$f":"(VIN_max-Vout)*Don_Vinmax/(Fsw*Iout*0.7)","v":2.003047619047619E-5},"H","COT",null,null,null,null,null,null,null,null,null,null,null,null,null,"10mm x 10mm",7,"10.0 x 10.0",100]
[]
["L_Vinmin_COT",{"$f":"(VIN_min-Vout)*Don_Vinmin/(Fsw*Iout*0.3)","v":4.552777777777777E-5},"H","COT","Calculated Inductance for 30% ripple at VIN(min)"]
["L_Vinnom_COT",{"$f":"(VIN_nom-Vout)*Don_Vinnom/(Fsw*Iout*0.4)","v":3.4887254901960786E-5},"H","COT","Calculated Inductance for 40% ripple at VIN(nom)",null,null,null,null,null,"Pk-to-Pk Ripple Current at VIN(nom), DIL"]
["L_Vinmax_COT",{"$f":"(VIN_max-Vout)*Don_Vinmax/(Fsw*Iout*0.7)","v":2.003047619047619E-5},"H","COT","Calculated Inductance for 70% ripple at VIN(max)"]
[]
[]
["Lopt",{"$f":"B59","v":3.4887254901960786E-5},"H"]
[]
["Lf",{"$f":"'Design Converter'!E17/1000000","v":3.3000000000000003E-5},"H",null,"Chosen Inductance"]
["Rdcr",{"$f":"'Design Converter'!E18/1000","v":0.17},"W",null,"Chosen Inductor DCR"]
[]
["Don2",{"$f":"(Vout+Iout*Rdcr)/Vin","v":4.9279411764705884E-2},null,null,"**Edit to add Rdson**"]
["Doff2",{"$f":"1-_Don2","v":0.95072058823529415}]
[]
["Rdson1",1.85,"W"]
["Rdson2",0.7,"W"]
[]
["Don_Vinmin_2",{"$f":"(Vout+Iout*(Rdcr+Rdson2))/(VIN_min+Iout*Rdson2)","v":7.3864343497199753E-2},null,null,"Duty cycles adjusted for DCR and shunt voltage drops"]
["Don_Vinnom_2",{"$f":"(Vout+Iout*(Rdcr+Rdson2))/(VIN_nom+Iout*Rdson2)","v":5.2206421345843725E-2},null,null,"need to include RDS(on) later"]
["Don_Vinmax_2",{"$f":"(Vout+Iout*(Rdcr+Rdson2))/(VIN_max+Iout*Rdson2)","v":4.7347427203829284E-2}]
[]
["Iripple_Vinmin",{"$f":"(VIN_min-Vout-Rdson1*Iout)*Don_Vinmin_2/(Fsw*Lf)","v":0.13174712903773264},"A","COT"]
["Iripple_Vinnom",{"$f":"(VIN_nom-Vout-Rdson1*Iout)*Don_Vinnom_2/(Fsw*Lf)","v":0.13530427867592504},"A","COT"]
["Iripple_Vinmax",{"$f":"(VIN_max-Vout)*Don_Vinmax_2/(Fsw*Lf)","v":0.13716406183897209},"A","COT"]
[]
["ILpk_Vinmin",{"$f":"Iout+Iripple_Vinmin/2","v":0.36587356451886632},"A","COT"]
["ILpk_Vinnom",{"$f":"Iout+Iripple_Vinnom/2","v":0.36765213933796248},"A","COT"]
["ILpk_Vinmax",{"$f":"Iout+Iripple_Vinmax/2","v":0.36858203091948605},"A","COT"]
[]
["ILIM_Typ",{"$f":"CHOOSE(VARIANT, 0.42, 0.84)","v":0.42},"A",null,"Isat_min",{"$f":"B86*1.2","v":0.504}]
[]
["Ripple current",{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), Iripple_Vinnom, Iripple)","v":0.13530427867592504},"A",null,null,null,null,"% Ripple Current at Nom VIN"]
[null,null,null,null,null,null,null,"Maximum Load Current"]
["Max inductor ripple current",{"$f":"MAX(B78:B80)","v":0.13716406183897209},"A"]
[null,null,null,null,null,"Ripple I","Iin"]
["% Ripple Current",{"$f":"B78/Iout","v":0.43915709679244214},null,"COT",null,{"$f":"B78","v":0.13174712903773264},{"$f":"Iin_Vinmin","v":2.2916666666666665E-2}]
[null,{"$f":"B79/Iout","v":0.4510142622530835},null,"COT",null,{"$f":"B79","v":0.13530427867592504},{"$f":"Iin_Vinnom","v":1.6176470588235292E-2}]
[null,{"$f":"B80/Iout","v":0.45721353946324034},null,"COT",null,{"$f":"B80","v":0.13716406183897209},{"$f":"Iin_Vinmax","v":1.4666666666666665E-2}]
[]
[null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3), B93, Ilim/Iout)","v":0.4510142622530835}]
[]
["Iripple1",{"$f":"(Vin-Vout)*Don_Vinnom_2/(Fsw*Lf)","v":0.13647496812428639},"A","inductor ripple current with chosen inductance (pk-pk)",null,null,null,null,1]
["Temp",100]
["DCR at hot",{"$f":"Rdcr*(1+0.0039*(B99-25))","v":0.219725},"W"]
["Ipk based on line 100",{"$f":"'Design Converter'!E10+0.5*Iripple1","v":0.36823748406214318}]
[]
[]
["Step 4: Output Capacitor"]
["Icoutrms_VINmin",{"$f":"Iripple_Vinmin/SQRT(12)","v":3.8032120207447652E-2},"A","Output Cap RMS current"]
["Icoutrms_VINnom",{"$f":"Iripple_Vinnom/SQRT(12)","v":3.9058980858026733E-2},"A"]
["Icoutrms_VINmax",{"$f":"Iripple_Vinmax/SQRT(12)","v":3.9595854012936506E-2},"A",null,null,null,{"$f":"Vripple1","v":1.6500000000000001E-2}]
[]
["Output Ripple Spec (pk-pk)",{"$f":"Vout*0.005","v":1.6500000000000001E-2},"V","Vout capacitive ripple spec at Vin(nom) = Vripple1"]
[]
["Coutmin"]
["COT",{"$f":"Iripple_Vinnom/(Fsw*8*Vripple1)","v":1.3667098856154045E-6},"F","COT","Min recommended Cout based on ripple spec above",null,null,null,1]
[null,{"$f":"Lf*B83^2/((1.05*Vout)^2-Vout^2)","v":3.9961003860984651E-6},"F","COT","Min recommended Cout based on 5% load-off transient spec"]
["CoutMinCOT",{"$f":"MAX(B112:B113, 0.0000022)","v":3.9961003860984651E-6},"F","COT","max of 2 results and 2.2uF"]
[]
["Reported Countmin",{"$f":"CoutMinCOT*1000000","v":3.996100386098465},"µF"]
[]
["Cout",{"$f":"'Design Converter'!E24/1000000","v":3.3000000000000003E-5},"F","Chosen Output Capacitance",null,null,null,null,1]
["Resrmax",{"$f":"SQRT((Vripple1/Iripple_Vinnom)^2-(1/(Fsw*Cout*8))^2)","v":0.12184273373721724},"W","Max ESR before ripple exceeds Vripple1",null,null,null,null,1]
["Type1 ESR for sufficient (20mV) COT ripple at FB pin",{"$f":"0.02*Vout/Vref/Iripple_Vinnom","v":0.40649121031666435},"W","(a)"]
["Type2 ESR for sufficient (20mV) COT ripple at FB pin",{"$f":"0.02/Iripple_Vinnom","v":0.14781498556969611},"W","(b)"]
[]
["Type 1 Output Cap RC Time Constant",{"$f":"Cout*B130*1000000","v":0},"µs"]
["Type 2 Output Cap RC Time Constant",{"$f":"Cout*B131*1000000","v":0},"µs"]
["Ton @ Vin(min)",{"$f":"Vout/VIN_min/(Fsw)","v":9.1666666666666654E-8},"s"]
["Ton @ Vin(nom)",{"$f":"Vout/VIN_nom/(Fsw)","v":6.4705882352941165E-8},"s"]
["ESR so that RC > Ton/2",{"$f":"B125/2/Cout","v":1.3888888888888885E-3},"W","(c)"]
[]
[]
["Type1: Need ESR of…",{"$f":"IF(MODE=1, MAX(B120,B127), 0)","v":0},"W","Max of (a) and (c)"]
["Type2: Need ESR of…",{"$f":"IF(MODE=2, MAX(B121,B127), 0)","v":0},"W","Max of (b) and (c)"]
[]
["Reported Cout ESR max",{"$f":"IF(OR(CoutEsrMax>0.5, CoutEsrMax<0, (ISERROR(CoutEsrMax))), \"N/A\", CoutEsrMax*1000)","v":121.84273373721724},"mW"]
[]
["CoutEsr",{"$f":" 'Design Converter'!E26","v":2.5000000000000001E-3},"W","Chosen ESR",null,null,null,null,1]
[]
["Actual Output Ripple",{"$f":"Iripple_Vinnom*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2)","v":7.6249214867091925E-4},"Vp-p","Vripple2"]
[]
["Minimum Feedforward / Coupling Capacitance",{"$f":"MAX(1000000000000*0.00005/(3*Rfb1_),47)","v":47},"pF",null,null,null,null,{"$f":"0.00005/3/Rfb1_","v":3.6791758646063281E-11}]
["Recommended Cff / Cb",{"$f":"IF(OR(MODE=2,MODE=3), \">\"&ROUND(B139,0),\"\")","v":">47"},"pF"]
["Selected Cff / Cb",{"$f":"'Design Converter'!$E$29","v":56},"pF"]
[]
["Minimum Ripple Generation Capacitance",{"$f":"10/(Fsw*Rfb)","v":8.0518975243798257E-11},"F",{"$f":"1000000000000*B143","v":80.518975243798252},"pF",{"$f":"Rfb","v":165592.43697478992}]
["Recommended Ca",{"$f":"IF(MODE=3, \">\"&ROUND(D143,0),\"\")","v":">81"},"pF"]
["Selected Ca",{"$f":"'Design Converter'!E31","v":3300},"pF",{"$f":"B145/1000000000000","v":3.3000000000000002E-9},"F"]
[]
["Maximum Ripple Generation Resistance",{"$f":"(VIN_nom-Vout)*B126/((B149/1000)*Ca)","v":31715.686274509793},"W",{"$f":"B147/1000","v":31.715686274509792},"kW"]
["Recommended Ra",{"$f":"IF(MODE=3, \"<\"&ROUND(D147,0),\"\")","v":"<32"},"kW",null,null,null,null,null,null,null,null,"Lf_emi",{"$f":"'Design EMI Filter'!$E$9","v":22},"uH",{"$f":"M148/1000000","v":2.1999999999999999E-5},"H"]
["Ripple amplitude",{"$f":"'Design Converter'!E33","v":40},"mVp-p",null,null,null,null,null,null,null,null,"Cf_emi",{"$f":"'Design EMI Filter'!$E$11","v":4.7},"uF",{"$f":"M149/1000000","v":4.6999999999999999E-6},"F"]
[null,null,null,null,null,null,null,null,null,null,null,"Cd_emi",{"$f":"'Design EMI Filter'!$E$13","v":10},"uF",{"$f":"M150/1000000","v":1.0000000000000001E-5},"F"]
[null,null,null,null,null,null,null,null,null,null,null,"ESR_Cd",{"$f":"'Design EMI Filter'!$E$15","v":3.3},"Ω",{"$f":"M151","v":3.3},"Ω",{"$f":"ESR_Cd&ohm","v":"3.3Ω"}]
["Step 5: Input Capacitor",null,null,null,null,null,null,null,null,null,null,"Min Noise",{"$f":"'Design EMI Filter'!$E$8","v":50},"dB","noise limit"]
["Vinripple1",{"$f":"0.05*VIN_nom","v":3.4000000000000004},"Vp-p","Input voltage ripple spec (pk-pk) at Vin(nom)",null,null,null,null,null,null,null,"Duty Cycle",{"$f":"Vout/VIN_nom/Efficiency_COT_Full_Load","v":0.10619127300810914},null,"calculated duty cycle"]
[null,null,null,null,null,null,null,null,null,null,null,"Target Atten.",{"$f":"20*LOG(Iout/(PI()^2*Fsw*Cin)*SIN(PI()*Duty_Cycle)/0.000001) - Min_Noise","v":0.41706044830564792},"dB","calculated attenuation"]
["Icinrms",{"$f":"Iout*SQRT(Don_Vinnom_2*(1-Don_Vinnom_2))","v":6.6732915285107663E-2},"A"]
["Cinmin",{"$f":"Iout*Don_Vinnom_2*(1-Don_Vinnom_2)/(Vinripple1*Fsw-Iout*RCinEsr)*1000000","v":5.8212836392432703E-3},"µF"]
["Reported Cinmin",{"$f":"IF(Cinmin<2.2, 2.2,Cinmin)","v":2.2000000000000002},"µF",null,null,null,null,null,null,null,null,"Filter Inductor"]
["Cin",{"$f":"'Design Converter'!E37/1000000","v":4.0000000000000003E-5},"F","Input capacitance",null,null,null,null,null,null,null,"Irms rating",{"$f":"Iout*1.5","v":0.44999999999999996},"A","calculated suggested IRMS rating"]
["CinEsrMax",{"$f":"-(Iout*Don_Vinnom_2*(1-Don_Vinnom_2)/(Cin*Fsw)-Vinripple1)/(Iout+Iripple_Vinnom/2)","v":9.246526341482431},"W"]
["RCinEsr",{"$f":"'Design Converter'!E39/1000","v":3.0000000000000001E-3},"W","Input capacitance series resistance (ESR)"]
["Reported Cin ESR max",{"$f":"IF(OR(CinEsrMax>12, CinEsrMax<0), \"N/A\",CinEsrMax*1000)","v":9246.5263414824312},"mΩ",null,null,null,null,null,null,null,null,"Filter Capacitor"]
[null,null,null,null,null,null,null,null,null,null,null,"Cfa calculation",{"$f":"Cin/(Cin*Lf_emi*0.000001*(2*PI()*Fsw/10)^2 - 1) / 0.000001","v":-40.007818254514632},"uF","calculated value"]
["COT input voltage ripple - Vinripple2",{"$f":"Iout*Don_Vinnom_2*(1-Don_Vinnom_2)/(Cin*Fsw)+(Iout +Iripple_Vinnom/2)*RCinEsr","v":1.5977655271749269E-3},"Vp-p",null,{"$f":"Iout*Don_Vinmax_2*(1-Don_Vinmax_2)/(Cin*Fsw)","v":4.5105648341007361E-4},"Vp-p",null,null,null,null,null,"Cfb calculation",{"$f":"1/(Lf_emi)*(10^(Target_Att/40)/(2*PI()*Fsw))^2/0.000001","v":2.1475737064492679E-3},"uF","calculated value"]
[null,null,null,null,null,null,null,null,null,null,null,"Cf",{"$f":"MAX(M162,M163)","v":2.1475737064492679E-3},"uF","calculated value"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Damping Capacitor"]
["Step 6: Soft Start",null,null,null,null,null,null,null,null,null,null,"Cd ≥",{"$f":"4*Cin*1000000","v":160},"uF","calculated value"]
["Tss",{"$f":"'Design Converter'!#REF!/1000","v":{"$error":"#REF!"}},"s","Soft-start time",null,null,null,null,null,null,null,"Cd ESR ≥",{"$f":"SQRT(Lf_emi/Cin)","v":0.74161984870956621},"Ω","calculated value"]
["Iss",1.0000000000000001E-5,"A","Soft-start current"]
["Css",{"$f":"8.16*Tss/1000000","v":{"$error":"#NAME?"}},"F","Required soft-start cap"]
["Css_u",{"$f":"'Standard Value Calculator'!B4","v":{"$error":"#NAME?"}},"F","User selected SS cap",null,null,null,null,null,null,null,"CIN and Cd Capacitors Current Sharing and Rating"]
[null,null,null,null,null,null,null,null,null,null,null,"Cd impedance",{"$f":" 1/(2*PI()*Fsw*Cd_emi) + ESR_Cd","v":3.3212206590789193},"Ω","calculated Cd impedance at the sw. frequency"]
["Step 7: Other Components - UVLO, PGOOD",null,null,null,null,null,null,null,null,null,null,"Cin impedance",{"$f":" 1/(2*PI()*Fsw*Cin) + RCinEsr","v":8.3051647697298444E-3},"Ω","calculated CIN impedance at the sw. frequency"]
[]
["Rising UVLO/EN Threshold",1.5,"V",null,null,null,null,null,null,null,null,"IRMS Total Input Cap",{"$f":"Iout*SQRT(Duty_Cycle*(1-Duty_Cycle))","v":9.2424681709229448E-2},"A","calculated total IRMS current for CIN and Cd combined"]
["Falling UVLO/EN Threshold",1.4,"V",null,null,null,null,null,null,null,null,"IRMS Cd Act",{"$f":"IRMSTOT*(ZCIN/(ZCIN+ZCd))","v":2.3054400265852385E-4},"A","Calculated min IRMS current rating for Cd"]
["Voltage Hysteresis",{"$f":"B176-B177","v":0.10000000000000009},"V",null,null,null,null,null,null,null,null,"IRMS CIN",{"$f":"IRMSTOT*(ZCd/(ZCIN+ZCd))","v":9.2194137706570922E-2},"A","Calculated min IRMS current rating for CIN"]
[]
["VINUVLO_ON",{"$f":"'Design Converter'!E48","v":6},"V"]
["VINUVLO_OFF",null,"V"]
[]
["RUV1",{"$f":"'Design Converter'!E49*1000","v":1000},"kΩ",{"$f":"'Standard Value Calculator'!J16","v":1000},"kΩ",{"$f":"IF(Ruvlo1<0,\"N/A\",D183)","v":1000},{"$f":"IF(Ruvlo1<0,\"N/A\",D183&\"kΩ\")","v":"1000kΩ"}]
["RUV2",{"$f":"Vuvlo_on*Ruvlo1/(VINuvlo_on-Vuvlo_on)","v":333.33333333333331},"kΩ",{"$f":"'Standard Value Calculator'!J17","v":332},"kΩ",{"$f":"IF(F183=\"N/A\",\"N/A\",D184)","v":332},{"$f":"IF(G183=\"N/A\",\"N/A\",D184&\"kΩ\")","v":"332kΩ"}]
[]
["VINUVLO_ON_ACTUAL",{"$f":"(D183+D184)/D184*Vuvlo_on","v":6.0180722891566267},"V"]
["VINUVLO_OFF_ACTUAL",{"$f":"(D183+D184)/D184*Vuvlo_off","v":5.6168674698795176},"V"]
[]
["RPG",20,"kΩ"]
[]
[]
["Step 8: FB Divider"]
["Pi",3.1415926500000002,null,"p"]
["Toff_Vinmax",{"$f":"(1-Don_Vinmax_2)/Fsw","v":1.2702034303948943E-6},"sec"]
["Ton_Vinmin",{"$f":"IF(VIN_min>Vout, (1-Don_Vinmin_2)/Fsw, Don_Vinmin_2/Fsw)","v":1.2348475420037336E-6},"sec"]
[]
["Rfb1",{"$f":"'Design Converter'!E43*1000","v":453000},"W","Lower Feedback Resistance - chosen by user",null,null,null,null,1]
["Rfb2",{"$f":"IF(Vout=Vref,100000000,Vref*B197/((Vout-Vref)))","v":258857.1428571429},"W","Upper Feedback Resistance"]
["Rfb2_u",{"$f":"IF(Vout=Vref,\"N/A\",'Standard Value Calculator'!J10)","v":261000},"W","Std Value Upper Feedback Resistance"]
["Rfb",{"$f":"Rfb1_*Rfb2_u/(Rfb1_+Rfb2_u)","v":165592.43697478992},"W","Rfb1 || Rfb2_u"]
[null,{"$f":"1.2/Rfb2_u*(Rfb2_u+Rfb1_)","v":3.2827586206896551},"V"]
["Ifb",{"$f":"CHOOSE(MODE_VOUT, IF(Vout=5, 0.000007, 0.0000038), Vout/(Rfb1_+Rfb2_u))","v":4.6218487394957983E-6}]
[]
["Other Input Variables"]
["Rfets",0,"W","Series resistance due to FETs",null,null,null,{"$f":"_Don2*RdsonTop+Doff2*RdsonBot+B209*Vin^2*Fsw/2/(((Iripple1/SQRT(3))^2))","v":1397.2830139965322}]
["Diode loss eq res",{"$f":"0.00000002*Fsw*0.6*4/Iripple1","v":0.26378463754038151}]
["Fet loss eq res",{"$f":"_Don2*RdsonTop+Doff2*RdsonBot","v":0.80420735294117651}]
["cap loss eq res",{"$f":"B209*Vin^2*Fsw/2/(((Iripple1/SQRT(3))^2))","v":1396.478806643591}]
["Sw cap",5.0000000000000001E-9]
[]
["Step 8: Efficiency"]
[]
["Design"]
["Ta",25,"°C","Ambient Temperature"]
["Components"]
["LTc",{"$f":"4000/1000000","v":4.0000000000000001E-3},"%/°C","Inductor DCR Temp Co"]
["θCA",40,"°C/W","Inductor Core to Ambient Thermal Resistance"]
["RCinEsr",{"$f":"RCinEsr","v":3.0000000000000001E-3},"W","Input Capacitor ESR"]
["Part Characteristics"]
["Vcc",{"$f":"IF(Vin>7.7,7.5,Vin-0.2)","v":7.5},"V"]
["Deadtime"]
["Deadtime",6.9999999999999998E-9,"s","Total Deadtime",null,null,"20ns for LM5166"]
["IQ"]
["IQ ",1.0000000000000001E-5,"A","Quiescent Current Of Controller (Not Switching!)"]
[]
[]
["IC Power Disipation","Value","Units"]
["Power Dis",{"$f":"Efficiency!AZ106","v":1.1592207770612202},"W"]
["Temp rise",{"$f":"B228*ThetaJA","v":47.643973937216153},"°C"]
["Current (switching)",{"$f":"(Qg_Q1+Qg_Q2)*Fsw+Iq","v":{"$error":"#NAME?"}},"A"]
["Qrr Current",{"$f":"Qrr_Q2*Fsw","v":{"$error":"#NAME?"}},"A"]
["Diode Current",{"$f":"C232/Vin","v":{"$error":"#NAME?"}},{"$f":"Deadtime*Fsw*(Ipp/2)*(Vsd_Q1+Vsd_Q2)","v":{"$error":"#NAME?"}}]
["Total Application Switching IQ",{"$f":"SUM(B230:B232)","v":{"$error":"#NAME?"}},"A"]
[]
[]
["SCHEMATIC LABELS"]
[]
[]
[{"$f":"\"RUV1 = \"&'Design Converter'!E49&\"MΩ\"","v":"RUV1 = 1MΩ"},{"$f":"C275","v":"1MΩ"}]
[{"$f":"\"RUV2 = \"&'Design Converter'!E50&\"kΩ\"","v":"RUV2 = 332kΩ"},{"$f":"C276","v":"332kΩ"}]
[{"$f":"\"Rhys = \"&'Design Converter'!E52&\"kΩ\"","v":"Rhys = 5.61686746987952kΩ"},{"$f":"C277","v":{"$error":"#REF!"}}]
[]
[{"$f":"\"LF = \"&'Design Converter'!E17&\"µH\"","v":"LF = 33µH"},{"$f":"'Design Converter'!E17&\"µH\"","v":"33µH"}]
[{"$f":"\"Rdcr = \"&Rdcr*1000&\"mΩ\"","v":"Rdcr = 170mΩ"},{"$f":"Rdcr*1000&\"mΩ\"","v":"170mΩ"}]
[{"$f":"\"Rt = \"&'Design Converter'!I43&\"kΩ\"","v":"Rt = kΩ"},{"$f":"'Design Converter'!I43&\"kΩ\"","v":"kΩ"}]
[{"$f":"\"Css = \"&ROUND(Css_u*1000000000,1)&\"nF\"","v":{"$error":"#NAME?"}},{"$f":"ROUND(Css_u*1000000000,1)&\"nF\"","v":{"$error":"#NAME?"}}]
[]
["VIN",{"$f":"VIN_nom&\"V\"","v":"68V"}]
["VIN range",{"$f":"VIN_min&\"V...\"&VIN_max&\"V\"","v":"48V...75V"}]
[]
[{"$f":"\"VOUT = \"&'Design Converter'!E9&\"V\"","v":"VOUT = 3.3V"},{"$f":"'Design Converter'!E9&\"V\"","v":"3.3V"}]
[null,null,{"$f":"R30","v":"100"},{"$f":"ROUNDUP('Design Converter'!$E$24/C252,0)","v":1}]
[{"$f":"\"COUT = \"&'Design Converter'!$E$24&\"µF\"","v":"COUT = 33µF"},{"$f":"'Design Converter'!$E$24&\"µF\"","v":"33µF"},{"$f":"IF('Design Converter'!$E$24=OR(10, 22, 47, 100), 'Design Converter'!$E$24,C252)","v":"100"},{"$f":"IF(D252=1, \"\",B255)","v":""},{"$f":"D253&C253&\"µF\"","v":"100µF"},{"$f":"C253&\"µF\"","v":"100µF"}]
["Capacitance per component (Cout)",{"$f":"C252&\"µF\"","v":"100µF"}]
["# of output caps",{"$f":"D252&\" x \"","v":"1 x "}]
[]
["CIN",{"$f":"Cin*1000000&\"µF\"","v":"40µF"}]
["Capacitance per component (Cin)",{"$f":"\"2.2µF\"","v":"2.2µF"}]
["# of input caps",{"$f":"ROUNDUP(Cin*1000000/2.2,0)&\" x \"","v":"19 x "}]
[]
["Fixed VOUT?",{"$f":"IF(MODE_VOUT=1, \"YES\", \"NO\")","v":"NO"}]
["FB resistor ref des shown or not?",{"$f":"IF(MODE_VOUT=2, \"YES\", \"NO\")","v":"YES"},{"$f":"IF(MODE_VOUT=2, \"R1\", \"\")","v":"R1"},{"$f":"IF(MODE_VOUT=2, \"R2\", \"\")","v":"R2"}]
[{"$f":"\"RFB1 = \"&'Design Converter'!E43&\"kΩ\"","v":"RFB1 = 453kΩ"},{"$f":"'Design Converter'!E43&\"kΩ\"","v":"453kΩ"},{"$f":"IF(MODE=1,'Design Converter'!E43&\"kΩ\", \"\")","v":""}]
[{"$f":"\"RFB2 = \"&IF(Vout=Vref,\"OPEN\",'Design Converter'!E44&\"kΩ\")","v":"RFB2 = 261kΩ"},{"$f":"IF(Vout=Vref,\"OPEN\",Rfb2_u/1000&\"kΩ\")","v":"261kΩ"},{"$f":"IF(MODE=1, IF(Vout=Vref, \"OPEN\",Rfb2_u/1000&\"kΩ\" ), \"\")","v":""}]
[]
[]
["Show Rt resistor ref des?",{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), \"YES\", \"NO\")","v":"YES"},{"$f":"IF(MODE=4,\"\", \"Rt\")","v":"Rt"}]
["Rt",{"$f":"IF(MODE=4, \"\", 'Standard Value Calculator'!J4/1000&\"kΩ\")","v":"11kΩ"}]
[]
["Show ESR resistor ref des?",{"$f":"IF(OR(MODE=3, MODE=4), \"NO\", \"YES\")","v":"NO"},{"$f":"IF(OR(MODE=3, MODE=4),\"\",\"Resr\")","v":""}]
[{"$f":"\"RESR = \"&'Design Converter'!E26&\"mΩ\"","v":"RESR = 0.0025mΩ"},{"$f":"IF(OR(MODE=3,MODE=4), \"\", 'Design Converter'!E26&\"Ω\")","v":""},null,null,null,{"$f":"B120","v":0.40649121031666435}]
["Resr",{"$f":"IF(MODE=1, \">\"&ROUND(B130,3), IF(MODE=2,  \">\"&ROUND(B131,3),IF(MODE=3,ROUND(B119,3),\"\")))","v":0.122}]
[]
["Adjustable UVLO?",{"$f":"IF(MODE_UVLO=1, \"YES\", \"NO\")","v":"YES"},{"$f":"IF(MODE_UVLO=1,\"Ren1\", \"\")","v":"Ren1"},{"$f":"IF(MODE_UVLO=1, \"Ren2\", \"\")","v":"Ren2"},{"$f":"IF(MODE_UVLO=1, \"Rhys\", \"\")","v":"Rhys"},"Value","Units","BOM display"]
[{"$f":"\"RUV1 = \"&C275","v":"RUV1 = 1MΩ"},{"$f":"'Design Converter'!E49&\" MΩ\"","v":"1 MΩ"},{"$f":"IF(MODE_UVLO=1,'Design Converter'!E49&\"MΩ\", \"\")","v":"1MΩ"},null,null,{"$f":"IF(MODE_UVLO=1,'Design Converter'!E49, \"\")","v":1},{"$f":"IF(MODE_UVLO=1,\"MΩ\", \"\")","v":"MΩ"},{"$f":"IF(MODE_UVLO=1,'Design Converter'!E49&\"M\", \"\")","v":"1M"}]
[{"$f":"\"RUV2 = \"&C276","v":"RUV2 = 332kΩ"},{"$f":"IF(D184>=1000, D184/1000&\" MΩ\", D184&\" kΩ\")","v":"332 kΩ"},{"$f":"IF(MODE_UVLO=1, IF(D184<1, D184*1000&\"Ω\", IF(D184<1000, D184&\"kΩ\", D184/1000&\"MΩ\")), \"\")","v":"332kΩ"},null,null,{"$f":"IF(MODE_UVLO=1, IF(D184<1, D184*1000, IF(D184<1000, D184, D184/1000)), \"\")","v":332},{"$f":"IF(MODE_UVLO=1, IF(D184<1, \"Ω\", IF(D184<1000,\"kΩ\", \"MΩ\")), \"\")","v":"kΩ"},{"$f":"IF(MODE_UVLO=1, IF(D184<1, D184*1000, IF(D184<1000, D184&\"k\", D184/1000&\"M\")), \"\")","v":"332k"}]
[{"$f":"\"RHYS = \"&C277","v":{"$error":"#REF!"}},{"$f":"IF(#REF!<1000,#REF!& \" kΩ\",#REF!& \" MΩ\")","v":{"$error":"#REF!"}},{"$f":"IF(MODE_UVLO=1, IF(#REF!<1,#REF!* 1000&\"Ω\", IF(#REF!<1000,#REF!& \"kΩ\",#REF!/ 1000&\"MΩ\")), \"\")","v":{"$error":"#REF!"}},null,null,{"$f":"IF(MODE_UVLO=1, IF(#REF!<1,#REF!* 1000, IF(#REF!<1000,#REF!,#REF!/ 1000)), \"\")","v":{"$error":"#REF!"}},{"$f":"IF(MODE_UVLO=1, IF(#REF!<1, \"Ω\", IF(#REF!<1000,\"kΩ\", \"MΩ\")), \"\")","v":{"$error":"#REF!"}},{"$f":"IF(MODE_UVLO=1, IF(#REF!<1,#REF!* 1000, IF(#REF!<1000,#REF!& \"k\",#REF!& \"M\")), \"\")","v":{"$error":"#REF!"}}]
[]
[{"$f":"\"Css = \"&Css*1000000000&\"nF\"","v":{"$error":"#NAME?"}},{"$f":"Css*1000000000&\"nF\"","v":{"$error":"#NAME?"}}]
["Cbst",{"$f":"\"2.2nF\"","v":"2.2nF"},null,{"$f":"B280","v":"2.2nF"}]
[]
[]
["Rset resistor ref des?",{"$f":"IF(MODE_RSET=2, \"YES\", \"NO\")","v":"NO"},{"$f":"IF(MODE_RSET=2, \"R3\", \"\")","v":""},null,null,{"$f":"MODE_RSET","v":1}]
["Rset",{"$f":"IF(MODE_RSET=2, C284&\"kΩ\", \"\")","v":""},{"$f":"IF(MODE_ILIM=3,100,IF(MODE_ILIM=2,56.2,IF(MODE_ILIM=4,24.9,0)))","v":{"$error":"#REF!"}}]
[]
[]
["Rpgood","100kΩ"]
[]
["Cff / Cb?",{"$f":"IF(MODE=2, \"Cff\", IF(MODE=3,\"Cb\",\"\"))","v":"Cb"}]
[{"$f":"\"Cff / Cb=\"&B290","v":"Cff / Cb=56pF"},{"$f":"IF(OR(MODE=2,MODE=3),B141&\"pF\",\"\")","v":"56pF"}]
[]
["Ca?",{"$f":"IF(MODE=3, \"Ca\",\"\")","v":"Ca"},null,{"$f":"Ca","v":3.3000000000000002E-9},{"$f":"Ton_Vinmin","v":1.2348475420037336E-6}]
["Ca=",{"$f":"IF(MODE=3,B145&\"pF\",\"\")","v":"3300pF"}]
[]
["Ra?",{"$f":"IF(MODE=3, \"Ra\",\"\")","v":"Ra"},"Injected Ripple"]
["Ra=",{"$f":"IF(MODE=3,Ra&\"kΩ\",\"\")","v":"31.6kΩ"},{"$f":"(VIN_nom-Vout)*Ton_Vin_nom/(Ra*Ca)/1000","v":4.0146438322164302E-2},{"$f":"ROUNDUP(1000*C296,0)","v":41},null,{"$f":"IF(MODE=3,Ra&\"k\",\"\")","v":"31.6k"}]
[]
["Lf(emi)",{"$f":"M148&\"µH\"","v":"22µH"}]
["Cf(emi)",{"$f":"M149&\"µF\"","v":"4.7µF"}]
["Df(emi)",{"$f":"M150&\"µF\"","v":"10µF"}]
[]
["Full-load efficiency",{"$f":"ROUND(Efficiency!CE106,1)&\"%\"","v":"45.7%"}]
["Full-load efficiency",{"$f":"ROUND(Efficiency!CE107,1)&\"%\"","v":"49.6%"}]
["10% load efficiency",{"$f":"ROUND(Efficiency!CE16,1)&\"%\"","v":"22.6%"},"linear scale only"]
["1% load efficiency",{"$f":"ROUND(Efficiency!CE56,1)&\"%\"","v":"36%"},"log scale only"]
[]
["Blank out",{"$f":"IF(C307=\"y\",\"\",\"|\")","v":"|"},"n"]
[]
["OUTPUT CURRENT",{"$f":"'Design Converter'!$E$10&\"A\"","v":"0.3A"}]
[]
["VIN ",2]
["RT",5]
["EN",7]
["PGOOD",6]
["SS",4]
["ILIM",3]
["GND",10]
["FB",8]
["SW",1]
["HYS",9]

{"sheet":"Standard Value Calculator","index":5,"n_rows":159,"n_cols":11,"rows_kept":159,"cut":false,"hidden":true,"merged":[]}
[]
["Capacitors","Css","Cout","Cin","Cb"]
["Inputs",{"$f":"Css","v":{"$error":"#NAME?"}},{"$f":"Cout","v":3.3000000000000003E-5},{"$f":"Cin","v":4.0000000000000003E-5},{"$f":"Cb","v":0},null,null,"Resistors","inputs","Standard Result"]
["Standard Result",{"$f":"SUM(B6:B158)/1000000000000","v":{"$error":"#NAME?"}},{"$f":"SUM(C6:C158)/1000000000000","v":3.3000000000000003E-5},{"$f":"SUM(D6:D158)/1000000000000","v":3.8999999999999999E-5},{"$f":"IF(E3=\"OPEN\",\"OPEN\",SUM(E6:E158)/1000000000000)","v":0},null,null,"Rt",{"$f":"Rt","v":11000},{"$f":"IF(I4>(INT(0.5+100*POWER(10,IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))/96))*POWER(10,INT(LOG(I4))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))+1)/96))*POWER(10,INT(LOG(I4))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))+1)/96))*POWER(10,INT(LOG(I4))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))/96))*POWER(10,INT(LOG(I4))-2))","v":11000},"Ω"]
["(pF)"]
[0.47,{"$f":"IF(IF((B$3*10^12-$A7)*(B$3*10^12-$A6)*-1<0,0,1)*IF(ABS(B$3*10^12-$A7)>(B$3*10^12-$A6),$A6,$A7)=B7,0,IF((B$3*10^12-$A7)*(B$3*10^12-$A6)*-1<0,0,1)*IF(ABS(B$3*10^12-$A7)>(B$3*10^12-$A6),$A6,$A7))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A7)*(C$3*10^12-$A6)*-1<0,0,1)*IF(ABS(C$3*10^12-$A7)>(C$3*10^12-$A6),$A6,$A7)=C7,0,IF((C$3*10^12-$A7)*(C$3*10^12-$A6)*-1<0,0,1)*IF(ABS(C$3*10^12-$A7)>(C$3*10^12-$A6),$A6,$A7))","v":0},{"$f":"IF(IF((D$3*10^12-$A7)*(D$3*10^12-$A6)*-1<0,0,1)*IF(ABS(D$3*10^12-$A7)>(D$3*10^12-$A6),$A6,$A7)=D7,0,IF((D$3*10^12-$A7)*(D$3*10^12-$A6)*-1<0,0,1)*IF(ABS(D$3*10^12-$A7)>(D$3*10^12-$A6),$A6,$A7))","v":0},{"$f":"IF(IF((E$3*10^12-$A7)*(E$3*10^12-$A6)*-1<0,0,1)*IF(ABS(E$3*10^12-$A7)>(E$3*10^12-$A6),$A6,$A7)=E7,0,IF((E$3*10^12-$A7)*(E$3*10^12-$A6)*-1<0,0,1)*IF(ABS(E$3*10^12-$A7)>(E$3*10^12-$A6),$A6,$A7))","v":0},null,null,"Rshunt",{"$f":"Rshunt","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},"Ω"]
[0.56000000000000005,{"$f":"IF(IF((B$3*10^12-$A8)*(B$3*10^12-$A7)*-1<0,0,1)*IF(ABS(B$3*10^12-$A8)>(B$3*10^12-$A7),$A7,$A8)=B8,0,IF((B$3*10^12-$A8)*(B$3*10^12-$A7)*-1<0,0,1)*IF(ABS(B$3*10^12-$A8)>(B$3*10^12-$A7),$A7,$A8))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A8)*(C$3*10^12-$A7)*-1<0,0,1)*IF(ABS(C$3*10^12-$A8)>(C$3*10^12-$A7),$A7,$A8)=C8,0,IF((C$3*10^12-$A8)*(C$3*10^12-$A7)*-1<0,0,1)*IF(ABS(C$3*10^12-$A8)>(C$3*10^12-$A7),$A7,$A8))","v":0},{"$f":"IF(IF((D$3*10^12-$A8)*(D$3*10^12-$A7)*-1<0,0,1)*IF(ABS(D$3*10^12-$A8)>(D$3*10^12-$A7),$A7,$A8)=D8,0,IF((D$3*10^12-$A8)*(D$3*10^12-$A7)*-1<0,0,1)*IF(ABS(D$3*10^12-$A8)>(D$3*10^12-$A7),$A7,$A8))","v":0},{"$f":"IF(IF((E$3*10^12-$A8)*(E$3*10^12-$A7)*-1<0,0,1)*IF(ABS(E$3*10^12-$A8)>(E$3*10^12-$A7),$A7,$A8)=E8,0,IF((E$3*10^12-$A8)*(E$3*10^12-$A7)*-1<0,0,1)*IF(ABS(E$3*10^12-$A8)>(E$3*10^12-$A7),$A7,$A8))","v":0},null,null,"Rc1ea",{"$f":"Rcea1","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},"Ω"]
[0.68,{"$error":"#NAME?"},0,0,0]
[0.82,{"$error":"#NAME?"},0,0,0,null,null,"Rfb1",{"$f":"Rfb1_","v":453000},453000,"Ω"]
[1,{"$error":"#NAME?"},0,0,0,null,null,"Rfb2",{"$f":"Rfb2_","v":258857.1428571429},{"$f":"IF(I10=\"OPEN\",\"OPEN\",IF(I10>(INT(0.5+100*POWER(10,IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))/96))*POWER(10,INT(LOG(I10))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))+1)/96))*POWER(10,INT(LOG(I10))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))+1)/96))*POWER(10,INT(LOG(I10))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))/96))*POWER(10,INT(LOG(I10))-2)))","v":261000},"Ω"]
[1.2,{"$error":"#NAME?"},0,0,0]
[1.5,{"$error":"#NAME?"},0,0,0]
[1.8,{"$error":"#NAME?"},0,0,0,null,null,"Rs",{"$f":"Rs_ideal*1000","v":{"$error":"#NAME?"}},{"$f":"IF(I13=0,0,IF(I13>(INT(0.5+100*POWER(10,IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))/96))*POWER(10,INT(LOG(I13))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))+1)/96))*POWER(10,INT(LOG(I13))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))+1)/96))*POWER(10,INT(LOG(I13))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))/96))*POWER(10,INT(LOG(I13))-2)))","v":{"$error":"#NAME?"}},"mΩ"]
[2.2000000000000002,{"$f":"IF(IF((B$3*10^12-$A15)*(B$3*10^12-$A14)*-1<0,0,1)*IF(ABS(B$3*10^12-$A15)>(B$3*10^12-$A14),$A14,$A15)=B15,0,IF((B$3*10^12-$A15)*(B$3*10^12-$A14)*-1<0,0,1)*IF(ABS(B$3*10^12-$A15)>(B$3*10^12-$A14),$A14,$A15))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A15)*(C$3*10^12-$A14)*-1<0,0,1)*IF(ABS(C$3*10^12-$A15)>(C$3*10^12-$A14),$A14,$A15)=C15,0,IF((C$3*10^12-$A15)*(C$3*10^12-$A14)*-1<0,0,1)*IF(ABS(C$3*10^12-$A15)>(C$3*10^12-$A14),$A14,$A15))","v":0},{"$f":"IF(IF((D$3*10^12-$A15)*(D$3*10^12-$A14)*-1<0,0,1)*IF(ABS(D$3*10^12-$A15)>(D$3*10^12-$A14),$A14,$A15)=D15,0,IF((D$3*10^12-$A15)*(D$3*10^12-$A14)*-1<0,0,1)*IF(ABS(D$3*10^12-$A15)>(D$3*10^12-$A14),$A14,$A15))","v":0},{"$f":"IF(IF((E$3*10^12-$A15)*(E$3*10^12-$A14)*-1<0,0,1)*IF(ABS(E$3*10^12-$A15)>(E$3*10^12-$A14),$A14,$A15)=E15,0,IF((E$3*10^12-$A15)*(E$3*10^12-$A14)*-1<0,0,1)*IF(ABS(E$3*10^12-$A15)>(E$3*10^12-$A14),$A14,$A15))","v":0},null,null,"Cslope_ideal",{"$f":"Cslope_ideal","v":{"$error":"#NAME?"}},{"$f":"#REF!*1000000000000","v":{"$error":"#REF!"}},"pF"]
[2.7,{"$error":"#NAME?"},0,0,0]
[3.3,{"$error":"#NAME?"},0,0,0,null,null,"Ruv1",{"$f":"Ruvlo1","v":1000},{"$f":"IF(I16=\"OPEN\",\"OPEN\",IF(I16>(INT(0.5+100*POWER(10,IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))/96))*POWER(10,INT(LOG(I16))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))+1)/96))*POWER(10,INT(LOG(I16))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))+1)/96))*POWER(10,INT(LOG(I16))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))/96))*POWER(10,INT(LOG(I16))-2)))","v":1000},"kΩ"]
[3.9,{"$error":"#NAME?"},0,0,0,null,null,"Ruv2",{"$f":"Ruvlo2","v":333.33333333333331},{"$f":"IF(I17=\"OPEN\",\"OPEN\",IF(I17>(INT(0.5+100*POWER(10,IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))/96))*POWER(10,INT(LOG(I17))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))+1)/96))*POWER(10,INT(LOG(I17))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))+1)/96))*POWER(10,INT(LOG(I17))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))/96))*POWER(10,INT(LOG(I17))-2)))","v":332},"kΩ"]
[4.7,{"$error":"#NAME?"},0,0,0,null,null,"Rhys",{"$f":"Rhys","v":{"$error":"#NAME?"}},{"$f":"IF(I18=\"OPEN\",\"OPEN\",IF(I18>(INT(0.5+100*POWER(10,IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))/96))*POWER(10,INT(LOG(I18))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))+1)/96))*POWER(10,INT(LOG(I18))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))+1)/96))*POWER(10,INT(LOG(I18))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))/96))*POWER(10,INT(LOG(I18))-2)))","v":{"$error":"#NAME?"}},"kΩ"]
[5.6,{"$error":"#NAME?"},0,0,0]
[6.8,{"$error":"#NAME?"},0,0,0,null,null,"Ra",{"$f":"'Variable Mgmt'!D147","v":31.715686274509792},{"$f":"IF(I20=\"OPEN\",\"OPEN\",IF(I20>(INT(0.5+100*POWER(10,IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))/96))*POWER(10,INT(LOG(I20))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))+1)/96))*POWER(10,INT(LOG(I20))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))+1)/96))*POWER(10,INT(LOG(I20))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))/96))*POWER(10,INT(LOG(I20))-2)))","v":31.6},"kΩ"]
[8.1999999999999993,{"$error":"#NAME?"},0,0,0]
[10,{"$error":"#NAME?"},0,0,0]
[12,{"$error":"#NAME?"},0,0,0]
[15,{"$error":"#NAME?"},0,0,0]
[18,{"$error":"#NAME?"},0,0,0]
[22,{"$error":"#NAME?"},0,0,0]
[27,{"$error":"#NAME?"},0,0,0]
[33,{"$error":"#NAME?"},0,0,0]
[39,{"$error":"#NAME?"},0,0,0]
[47,{"$error":"#NAME?"},0,0,0]
[56,{"$error":"#NAME?"},0,0,0]
[68,{"$error":"#NAME?"},0,0,0]
[82,{"$error":"#NAME?"},0,0,0]
[{"$f":"A22*10","v":100},{"$error":"#NAME?"},0,0,0]
[{"$f":"A23*10","v":120},{"$error":"#NAME?"},0,0,0]
[150,{"$error":"#NAME?"},0,0,0]
[180,{"$error":"#NAME?"},0,0,0]
[220,{"$error":"#NAME?"},0,0,{"$f":"IF(IF((E$3*10^12-$A39)*(E$3*10^12-$A38)*-1<0,0,1)*IF(ABS(E$3*10^12-$A39)>(E$3*10^12-$A38),$A38,$A39)=E39,0,IF((E$3*10^12-$A39)*(E$3*10^12-$A38)*-1<0,0,1)*IF(ABS(E$3*10^12-$A39)>(E$3*10^12-$A38),$A38,$A39))","v":0}]
[270,{"$error":"#NAME?"},0,0,0]
[330,{"$error":"#NAME?"},0,0,0]
[390,{"$error":"#NAME?"},0,0,0]
[470,{"$error":"#NAME?"},0,0,0]
[560,{"$error":"#NAME?"},0,0,0]
[680,{"$error":"#NAME?"},0,0,0]
[{"$f":"A33*10","v":820},{"$error":"#NAME?"},0,0,0]
[1000,{"$error":"#NAME?"},0,0,0]
[1200,{"$error":"#NAME?"},0,0,0]
[1500,{"$error":"#NAME?"},0,0,0]
[1800,{"$error":"#NAME?"},0,0,0]
[2200,{"$error":"#NAME?"},0,0,0]
[2700,{"$error":"#NAME?"},0,0,0]
[3300,{"$error":"#NAME?"},0,0,0]
[3900,{"$error":"#NAME?"},0,0,0]
[4700,{"$error":"#NAME?"},0,0,0]
[5600,{"$error":"#NAME?"},0,0,0]
[6800,{"$error":"#NAME?"},0,0,0]
[8200,{"$error":"#NAME?"},0,0,0]
[10000,{"$error":"#NAME?"},0,0,0]
[12000,{"$error":"#NAME?"},0,0,0]
[15000,{"$error":"#NAME?"},0,0,0]
[18000,{"$error":"#NAME?"},0,0,0]
[22000,{"$error":"#NAME?"},0,0,0]
[27000,{"$error":"#NAME?"},0,0,0]
[33000,{"$error":"#NAME?"},0,0,0]
[39000,{"$error":"#NAME?"},0,0,0]
[47000,{"$error":"#NAME?"},0,0,0]
[56000,{"$error":"#NAME?"},0,0,0]
[68000,{"$error":"#NAME?"},0,0,0]
[82000,{"$error":"#NAME?"},0,0,0]
[100000,{"$error":"#NAME?"},{"$f":"IF(IF((C$3*10^12-$A71)*(C$3*10^12-$A70)*-1<0,0,1)*IF(ABS(C$3*10^12-$A71)>(C$3*10^12-$A70),$A70,$A71)=C71,0,IF((C$3*10^12-$A71)*(C$3*10^12-$A70)*-1<0,0,1)*IF(ABS(C$3*10^12-$A71)>(C$3*10^12-$A70),$A70,$A71))","v":0},{"$f":"IF(IF((D$3*10^12-$A71)*(D$3*10^12-$A70)*-1<0,0,1)*IF(ABS(D$3*10^12-$A71)>(D$3*10^12-$A70),$A70,$A71)=D71,0,IF((D$3*10^12-$A71)*(D$3*10^12-$A70)*-1<0,0,1)*IF(ABS(D$3*10^12-$A71)>(D$3*10^12-$A70),$A70,$A71))","v":0},{"$f":"IF(IF((E$3*10^12-$A71)*(E$3*10^12-$A70)*-1<0,0,1)*IF(ABS(E$3*10^12-$A71)>(E$3*10^12-$A70),$A70,$A71)=E71,0,IF((E$3*10^12-$A71)*(E$3*10^12-$A70)*-1<0,0,1)*IF(ABS(E$3*10^12-$A71)>(E$3*10^12-$A70),$A70,$A71))","v":0}]
[120000,{"$f":"IF(IF((B$3*10^12-$A72)*(B$3*10^12-$A71)*-1<0,0,1)*IF(ABS(B$3*10^12-$A72)>(B$3*10^12-$A71),$A71,$A72)=B72,0,IF((B$3*10^12-$A72)*(B$3*10^12-$A71)*-1<0,0,1)*IF(ABS(B$3*10^12-$A72)>(B$3*10^12-$A71),$A71,$A72))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A72)*(C$3*10^12-$A71)*-1<0,0,1)*IF(ABS(C$3*10^12-$A72)>(C$3*10^12-$A71),$A71,$A72)=C72,0,IF((C$3*10^12-$A72)*(C$3*10^12-$A71)*-1<0,0,1)*IF(ABS(C$3*10^12-$A72)>(C$3*10^12-$A71),$A71,$A72))","v":0},{"$f":"IF(IF((D$3*10^12-$A72)*(D$3*10^12-$A71)*-1<0,0,1)*IF(ABS(D$3*10^12-$A72)>(D$3*10^12-$A71),$A71,$A72)=D72,0,IF((D$3*10^12-$A72)*(D$3*10^12-$A71)*-1<0,0,1)*IF(ABS(D$3*10^12-$A72)>(D$3*10^12-$A71),$A71,$A72))","v":0},0]
[150000,{"$error":"#NAME?"},0,0,0]
[180000,{"$error":"#NAME?"},0,0,0]
[220000,{"$error":"#NAME?"},0,0,0]
[270000,{"$error":"#NAME?"},0,0,0]
[330000,{"$error":"#NAME?"},0,0,0]
[390000,{"$error":"#NAME?"},0,0,0]
[470000,{"$error":"#NAME?"},0,0,0]
[560000,{"$error":"#NAME?"},0,0,0]
[680000,{"$error":"#NAME?"},0,0,0]
[820000,{"$error":"#NAME?"},0,0,0]
[1000000,{"$error":"#NAME?"},0,0,0]
[1200000,{"$error":"#NAME?"},0,0,0]
[1500000,{"$error":"#NAME?"},0,0,0]
[1800000,{"$error":"#NAME?"},0,0,0]
[2200000,{"$error":"#NAME?"},0,0,0]
[2700000,{"$error":"#NAME?"},0,0,0]
[3300000,{"$error":"#NAME?"},0,0,0]
[3900000,{"$error":"#NAME?"},0,0,0]
[4700000,{"$error":"#NAME?"},0,0,0]
[5600000,{"$error":"#NAME?"},0,0,0]
[6800000,{"$error":"#NAME?"},0,0,0]
[8200000,{"$error":"#NAME?"},0,0,0]
[10000000,{"$error":"#NAME?"},0,0,0]
[12000000,{"$error":"#NAME?"},0,0,0]
[15000000,{"$error":"#NAME?"},0,0,0]
[18000000,{"$error":"#NAME?"},0,0,0]
[22000000,{"$error":"#NAME?"},0,0,0]
[{"$f":"A87*10","v":27000000},{"$error":"#NAME?"},0,0,0]
[33000000,{"$error":"#NAME?"},33000000,0,0]
[39000000,{"$error":"#NAME?"},0,39000000,0]
[47000000,{"$error":"#NAME?"},0,0,{"$f":"IF(IF((E$3*10^12-$A103)*(E$3*10^12-$A102)*-1<0,0,1)*IF(ABS(E$3*10^12-$A103)>(E$3*10^12-$A102),$A102,$A103)=E103,0,IF((E$3*10^12-$A103)*(E$3*10^12-$A102)*-1<0,0,1)*IF(ABS(E$3*10^12-$A103)>(E$3*10^12-$A102),$A102,$A103))","v":0}]
[56000000,{"$error":"#NAME?"},0,{"$f":"IF(IF((D$3*10^12-$A104)*(D$3*10^12-$A103)*-1<0,0,1)*IF(ABS(D$3*10^12-$A104)>(D$3*10^12-$A103),$A103,$A104)=D104,0,IF((D$3*10^12-$A104)*(D$3*10^12-$A103)*-1<0,0,1)*IF(ABS(D$3*10^12-$A104)>(D$3*10^12-$A103),$A103,$A104))","v":0},0]
[68000000,{"$error":"#NAME?"},0,0,0]
[82000000,{"$error":"#NAME?"},0,0,0]
[100000000,{"$error":"#NAME?"},0,0,0]
[120000000,{"$error":"#NAME?"},0,0,0]
[150000000,{"$error":"#NAME?"},0,0,0]
[180000000,{"$error":"#NAME?"},0,0,0]
[220000000,{"$error":"#NAME?"},0,0,0]
[270000000,{"$error":"#NAME?"},0,0,0]
[330000000,{"$error":"#NAME?"},0,0,0]
[390000000,{"$error":"#NAME?"},0,0,0]
[470000000,{"$error":"#NAME?"},0,0,0]
[560000000,{"$error":"#NAME?"},0,0,0]
[680000000,{"$error":"#NAME?"},0,0,0]
[820000000,{"$error":"#NAME?"},0,0,0]
[1000000000,{"$error":"#NAME?"},0,0,0]
[1200000000,{"$error":"#NAME?"},0,0,0]
[1500000000,{"$error":"#NAME?"},0,0,0]
[1800000000,{"$error":"#NAME?"},0,0,0]
[2200000000,{"$error":"#NAME?"},0,0,0]
[2700000000,{"$error":"#NAME?"},0,0,0]
[3300000000,{"$error":"#NAME?"},0,0,0]
[3900000000,{"$error":"#NAME?"},0,0,0]
[4700000000,{"$error":"#NAME?"},0,0,0]
[5600000000,{"$error":"#NAME?"},0,0,0]
[6800000000,{"$error":"#NAME?"},0,0,0]
[8200000000,{"$error":"#NAME?"},0,0,0]
[10000000000,{"$error":"#NAME?"},0,0,0]
[12000000000,{"$error":"#NAME?"},0,0,0]
[15000000000,{"$error":"#NAME?"},0,0,0]
[18000000000,{"$error":"#NAME?"},0,0,0]
[22000000000,{"$error":"#NAME?"},{"$f":"IF(IF((C$3*10^12-$A135)*(C$3*10^12-$A134)*-1<0,0,1)*IF(ABS(C$3*10^12-$A135)>(C$3*10^12-$A134),$A134,$A135)=C135,0,IF((C$3*10^12-$A135)*(C$3*10^12-$A134)*-1<0,0,1)*IF(ABS(C$3*10^12-$A135)>(C$3*10^12-$A134),$A134,$A135))","v":0},0,{"$f":"IF(IF((E$3*10^12-$A135)*(E$3*10^12-$A134)*-1<0,0,1)*IF(ABS(E$3*10^12-$A135)>(E$3*10^12-$A134),$A134,$A135)=E135,0,IF((E$3*10^12-$A135)*(E$3*10^12-$A134)*-1<0,0,1)*IF(ABS(E$3*10^12-$A135)>(E$3*10^12-$A134),$A134,$A135))","v":0}]
[27000000000,{"$f":"IF(IF((B$3*10^12-$A136)*(B$3*10^12-$A135)*-1<0,0,1)*IF(ABS(B$3*10^12-$A136)>(B$3*10^12-$A135),$A135,$A136)=B136,0,IF((B$3*10^12-$A136)*(B$3*10^12-$A135)*-1<0,0,1)*IF(ABS(B$3*10^12-$A136)>(B$3*10^12-$A135),$A135,$A136))","v":{"$error":"#NAME?"}},0,0,0]
[33000000000,{"$error":"#NAME?"},0,0,0]
[39000000000,{"$error":"#NAME?"},0,0,0]
[47000000000,{"$error":"#NAME?"},0,0,0]
[56000000000,{"$error":"#NAME?"},0,0,0]
[68000000000,{"$error":"#NAME?"},0,0,0]
[82000000000,{"$error":"#NAME?"},0,0,0]
[100000000000,{"$error":"#NAME?"},0,0,0]
[120000000000,{"$error":"#NAME?"},0,0,0]
[150000000000,{"$error":"#NAME?"},0,0,0]
[180000000000,{"$error":"#NAME?"},0,0,0]
[220000000000,{"$error":"#NAME?"},0,0,0]
[270000000000,{"$error":"#NAME?"},0,0,0]
[330000000000,{"$error":"#NAME?"},0,0,0]
[390000000000,{"$error":"#NAME?"},0,0,0]
[470000000000,{"$error":"#NAME?"},0,0,0]
[560000000000,{"$error":"#NAME?"},0,0,0]
[680000000000,{"$error":"#NAME?"},0,0,0]
[820000000000,{"$error":"#NAME?"},0,0,0]
[1000000000000,{"$error":"#NAME?"},0,0,0]
[1200000000000,{"$error":"#NAME?"},0,0,0]
[1500000000000,{"$error":"#NAME?"},0,0,0]
[1800000000000,{"$error":"#NAME?"},0,0,0]
[2200000000000,{"$error":"#NAME?"},0,0,0]
[2700000000000,{"$error":"#NAME?"},2700000000000,2700000000000,2700000000000]

{"sheet":"Efficiency","index":6,"n_rows":114,"n_cols":88,"rows_kept":114,"cut":false,"hidden":true,"merged":[[0,0,2,4],[1,6,1,7],[3,0,3,4],[3,10,3,21]]}
["LM5169 (COT) Efficiency Calculator"]
[null,null,null,null,null,null,"TERMS OF USE",null,null,{"$f":"CoutEsr","v":2.5000000000000001E-3},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"didn't include FB"]
[]
[null,null,null,null,null,null,null,"Currents",null,null,"Miscellaneous",null,null,null,null,null,null,null,null,null,null,null,"Inductor",null,null,null,"Cout",null,null,"Cin",null,null,"High-side MOSFET Losses ",null,null,null,null,null,null,null,null,"Low-side MOSFET Losses ",null,null,"Diode",null,null,null,null,null,null,null,"RESULTS"]
["Input Parameters",null,null,null,null,null,null,"Step","Iout (A)","Ripple Current pk-pk (A)","Peak Current (A)","Valley Current (A)","VOUT Hysteresis +Undershoot (2us Delay) (mV)","Vout Rise per Pulse (mV)","Number of Pulses in DCM","VOUT Ripple (mV)","Off Time (sec)","Duty Cycle","Switching Frequency (Hz)","Active Mode Duration (sec)","Sleep Mode Duration (sec)","Operating Quiescent Current (A)","Irms (A)","Inductor DCR Loss @ 25°C (W)","Inductor Core Loss  (W)","Total Inductor Loss (W)","Irms (A)","Cout ESR Loss (W)","Total Cout Loss (W)","Irms (A)","Cin ESR Loss (W)","Total Cin Loss (W)","Irms (A)","Rdson HS Loss @ 25°C (W)","HS Gate Qg Loss (W)     ","SW Rise Time (ns)","SW Fall Time (ns)","HS Switching  Loss (W)","Coss Loss (W)","Total HS FET AC Loss (W)","Total HS FET Loss (W)","Irms (A)","Rdson LS Loss @ 25°C (W)","LS Gate Qg Loss (W)","Reverse Recovery & Leakage Losses","DeadTime Loss @ 25°C (W)","Total LS FET AC Loss (W)","Total LS FET Loss (W)","Quiescent Loss (W)","LDO + Quiescent Loss (W)","Total Gate Drive Loss (W)","Total Power Loss in IC (W)","Total Converter Power Loss (W)","Pout (W)","EFF (%)","High-side MOSFET Rdson %","Low-side MOSFET Rdson %","Gate Drive (Qg) Loss from Vin %","High-side MOSFET AC Loss %","Reverse Recovery & Leakage Loss %","Deadtime Loss %","Low-side MOSFET AC Loss %","Inductor Cu Loss %","Inductor Core Loss %","Cin ESR %","Cout ESR %","LDO + Quiescent Current Loss %","Total Loss %","Overall Eff %","Overall Eff","Current (mA)","Keep for \"previous\" data series","Keep for \"previous\" data series","Frequency (kHz)",null,"Coss",null,"Total Power Loss in IC (mW)","LDO + Quiescent Loss (mW)","Total Inductor Loss (mW)",null,null,"Overall Eff","Total Power Loss in IC (W)","LDO + Quiescent Loss (mW)","Total Inductor Loss (mW)","Fsw (kHz)","Ripple (mV)"]
["Design","Input Value","Units","Std Units","Description",null,null,0.04,{"$f":"IF(PLOT_TYPE=1, H6/100*Iout, min_I*EXP(H6*rr/100))","v":1.2E-4},{"$f":"IF(I6<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I6-Vout)/L*OnTime)","v":0.12661386028450594},{"$f":"IF(I6<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I6+((Vin-(Rdcr+RdsonTop)*J6-Vout)/L*OnTime)/2)","v":0.12661386028450594},{"$f":"IF(I6<Icrit, 0, I6-((Vin-(Rdcr+RdsonTop)*K6-Vout)/L*OnTime)/2)","v":0},{"$f":"1000*((((J6/2)-I6)*0.000002/Cout+Vout/306))","v":14.613824643202497},{"$f":"IF(I6<Icrit, 1000*SQRT((J6*CoutEsr)^2+(((J6/2)-I6)*(OnTime+OffTime)/Cout)^2), 1000*J6*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":2.3658008997793498},{"$f":"ROUNDUP(M6/N6,0)","v":7},{"$f":"IF(I6<Icrit, 1000*((N6/1000)*O6), 1000*J6*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":16.560606298455451},{"$f":"IF(I6<Icrit, L*J6/(Vout+J6/2*(RdsonBot+Rdcr)), L*J6/(Vout+I6*(RdsonBot+Rdcr)))","v":1.2441798184621381E-6},{"$f":"OnTime*S6","v":9.3706999559216823E-5},{"$f":"IF(I6<Icrit,I6/((OnTime+Q6)*J6/2),1/(OnTime+Q6))","v":1448.1990840969872},{"$f":"IF(1/S6-OnTime-Q6>Tsleep, OnTime+Q6+Tsleep, 1/S6)","v":6.3088857008150795E-6},{"$f":"IF(1/S6-OnTime-Q6>Tsleep, 1/S6-OnTime-Q6-Tsleep, 0)","v":6.8420391117996859E-4},{"$f":"S6*(T6*Iq_active+U6*Iq_sleep)","v":1.5938739620835435E-5},{"$f":"IF(I6<Icrit,Iripple*SQRT((OnTime+OffTime)*S6/3), SQRT(I6^2+Iripple^2/12))","v":3.0554270691185432E-3},{"$f":"W6^2*Rdcr","v":1.5870578776993964E-6},{"$f":"Core_Loss/1000*S6/$S$106","v":0},{"$f":"(Y6+X6*(1+Ltc*(Ta-25)))/(1-X6*Ltc*ThetaCa)","v":1.5870582806999318E-6},{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q6)*S6)","v":1.5795070647594705E-3},{"$f":"RCoutEsr*AA6^2","v":6.2371064190626955E-9},{"$f":"AB6","v":6.2371064190626955E-9},{"$f":"SQRT($R6)*SQRT($I6^2*(1-R6)+(Iripple^2)/12)","v":3.5119228646875536E-4},{"$f":"RCinEsr*AD6^2","v":3.7000806622545697E-10},{"$f":"AE6","v":3.7000806622545697E-10},{"$f":"IF(I6<Icrit,Iripple*SQRT((OnTime)*S6/3), SQRT(OnTime*S6*(I6^2+Iripple^2/12)))","v":7.0238073100222528E-4},{"$f":"RdsonTop*AG6^2","v":9.1267657887395771E-7},{"$f":"QgTop*S6*Vdd","v":4.3445972522909614E-6},{"$f":"5*VIN_nom/24","v":14.166666666666666},{"$f":"IF(I6<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I6+Iripple/2)*1000000000)","v":86.572846132243242},{"$f":"IF(I6<Icrit, Vin*(I6+Iripple/2)*AK6/1000000000/2*S6, Vin*(I6-Iripple/2)*AJ6/1000000000/2*S6 + Vin*(I6+Iripple/2)*AK6/1000000000/2*S6)","v":2.6837043143780235E-4},{"$f":"IF(I6<Icrit, Csw*(Vin)^2*S6/2, Csw*Vin^2*S6/2)","v":5.3571780518915744E-4},{"$f":"AI6+AL6+AM6","v":8.0843283387925079E-4},{"$f":"(AI6+AL6+AM6+AH6*(1+RdsonTopTc*(Ta-25)))/(1-AH6*RdsonTopTc*ThetaJA)","v":8.0934565618310508E-4},{"$f":"IF(I6<Icrit,Iripple*SQRT((OffTime)*S6/3), SQRT(OffTime*S6*(I6^2+Iripple^2/12)))","v":2.9735998189768425E-3},{"$f":"RdsonBot*AP6^2","v":6.6317219125643326E-6},{"$f":"QgBot*S6*Vdd","v":1.1730412581185599E-5},{"$f":"IF(I6<Icrit, Vin*Idss*R6, QrrBot*(I6-Iripple/2)/1*S6*Vin+Vin*Idss*R6)","v":0},{"$f":"IF(I6<Icrit, dead1*S6*(I6+Iripple/2)*((I6+Iripple/2)*BDserR+VSD), dead1*S6*(I6+Iripple/2)*((I6+Iripple/2)*BDserR+VSD)+dead2*S6*(I6-Iripple/2)*((I6-Iripple/2)*BDserR+VSD))","v":5.1459605124983945E-7},{"$f":"AR6+AS6+AT6","v":1.2245008632435438E-5},{"$f":"(AR6+AS6+AT6+AQ6*(1+RdsonBotTc*(Ta-25)))/(1-AQ6*RdsonBotTc*ThetaJA)","v":1.8876755241573782E-5},{"$f":"Vin*V6+Vout*Ifb/0.8","v":1.1028994202672297E-3},{"$f":"(Vin-Vdd)*(S6*QgBot+S6*QgTop)+AW6","v":1.3054445441690343E-3},{"$f":"AI6+AR6","v":1.607500983347656E-5},{"$f":"AO6+AV6+AX6+AY6","v":2.1497419654271893E-3},{"$f":"SUM(Z6,AC6,AF6,AZ6)","v":2.1513356308223747E-3},{"$f":"Vout*I6","v":3.9599999999999998E-4},{"$f":"BB6/(BB6+BA6)","v":0.15545654652196594},{"$f":"(AO6-AN6)/($BB6+$BA6)","v":3.5834394683184942E-4},{"$f":"(AV6-AU6)/($BB6+$BA6)","v":2.6034051143065781E-3},{"$f":"Vin*S6*(QgBot+QgTop)/($BB6+$BA6)","v":8.582305805721506E-2},{"$f":"AN6/($BB6+$BA6)","v":0.3173640819440266},{"$f":"AS6/(BA6+BB6)","v":0},{"$f":"AT6/($BB6+$BA6)","v":2.0201344692207234E-4},{"$f":"AU6/($BB6+$BA6)","v":4.806986752853723E-3},{"$f":"X6/($BB6+$BA6)","v":6.2302660807482015E-4},{"$f":"Y6/($BB6+$BA6)","v":0},{"$f":"(AF6)/($BB6+$BA6)","v":1.4525297010272832E-7},{"$f":"(AC6)/($BB6+$BA6)","v":2.4484823843370518E-6},{"$f":"AX6/($BB6+$BA6)","v":0.51247449624358621},{"$f":"SUM(BD6:BO6)","v":0.92425800584917139},{"$f":"BC6","v":0.15545654652196594},{"$f":"100*BQ6","v":15.545654652196594},{"$f":"I6*1000","v":0.12000000000000001},8.7924221262065743,{"$f":"BT6/100","v":8.7924221262065741E-2},{"$f":"S6/1000","v":1.4481990840969872},null,{"$f":"AM6/($BB6+$BA6)","v":0.21030515127533775},null,{"$f":"AZ6","v":2.1497419654271893E-3},{"$f":"AX6","v":1.3054445441690343E-3},{"$f":"Z6","v":1.5870582806999318E-6},null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR6, IF(MODE_ILIM=4,#REF!,#REF!))","v":15.545654652196594},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ6, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.1497419654271893E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA6, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.3054445441690343E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB6, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.5870582806999318E-6},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S6, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":1.4481990840969872},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P6, IF(MODE_ILIM=4,#REF!,#REF!))","v":16.560606298455451}]
[null,null,null,null,null,null,null,1,3.0000000000000001E-3,0.12661386028450594,0.12661386028450594,0,{"$f":"IF(I7<Icrit, 1000*((((J7/2)-I7)*0.000002/Cout+Vout/306)), 1000*J7*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":14.439279188657041},2.2599455003647693,{"$f":"ROUNDUP(M7/N7,0)","v":7},15.819618502553386,1.2441798184621381E-6,{"$f":"OnTime*S7","v":2.3426749889804204E-3},36204.97710242468,{"$f":"IF(1/S7-OnTime-Q7>Tsleep, OnTime+Q7+Tsleep, 1/S7)","v":6.3088857008150795E-6},{"$f":"IF(1/S7-OnTime-Q7>Tsleep, 1/S7-OnTime-Q7-Tsleep, 0)","v":2.131162617441627E-5},1.5846849052088591E-4,{"$f":"IF(I7<Icrit,Iripple*SQRT((OnTime+OffTime)*S7/3), SQRT(I7^2+Iripple^2/12))","v":1.5277135345592715E-2},3.9676446942484905E-5,0,3.9676698819354594E-5,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q7)*S7)","v":7.8975353237973524E-3},{"$f":"RCoutEsr*AA7^2","v":1.5592766047656739E-7},{"$f":"AB7","v":1.5592766047656739E-7},{"$f":"SQRT($R7)*SQRT($I7^2*(1-R7)+(Iripple^2)/12)","v":1.7619311854570299E-3},{"$f":"RCinEsr*AD7^2","v":9.3132045068580447E-9},{"$f":"AE7","v":9.3132045068580447E-9},{"$f":"IF(I7<Icrit,Iripple*SQRT((OnTime)*S7/3), SQRT(OnTime*S7*(I7^2+Iripple^2/12)))","v":3.5119036550111263E-3},{"$f":"RdsonTop*AG7^2","v":2.2816914471848939E-5},{"$f":"QgTop*S7*Vdd","v":1.0861493130727404E-4},14.166666666666666,86.572846132243242,{"$f":"IF(I7<Icrit, Vin*(I7+Iripple/2)*AK7/1000000000/2*S7, Vin*(I7-Iripple/2)*AJ7/1000000000/2*S7 + Vin*(I7+Iripple/2)*AK7/1000000000/2*S7)","v":7.0161780918792478E-3},{"$f":"IF(I7<Icrit, Csw*(Vin)^2*S7/2, Csw*Vin^2*S7/2)","v":1.3392945129728936E-2},{"$f":"AI7+AL7+AM7","v":2.0517738152915459E-2},2.0540647527433054E-2,1.4867999094884211E-2,{"$f":"RdsonBot*AP7^2","v":1.6579304781410829E-4},2.9326031452963996E-4,0,1.3458215764547082E-5,{"$f":"AR7+AS7+AT7","v":3.0671853029418702E-4},4.7252703335828633E-4,1.0794922481470662E-2,1.5858550579015779E-2,4.0187524583691397E-4,{"$f":"AO7+AV7+AX7+AY7","v":3.7273600385644035E-2},3.7313442325328371E-2,9.8999999999999991E-3,{"$f":"BB7/(BB7+BA7)","v":0.20968604516872927},{"$f":"(AO7-AN7)/($BB7+$BA7)","v":4.8522991311958309E-4},{"$f":"(AV7-AU7)/($BB7+$BA7)","v":3.5118918447331433E-3},0.11576159403335812,{"$f":"AN7/($BB7+$BA7)","v":0.43457407768610012},{"$f":"AS7/(BA7+BB7)","v":0},{"$f":"AT7/($BB7+$BA7)","v":2.8505050895912362E-4},{"$f":"AU7/($BB7+$BA7)","v":6.4964237977124407E-3},8.4036335815319005E-4,0,{"$f":"(AF7)/($BB7+$BA7)","v":1.9725747685764133E-7},{"$f":"(AC7)/($BB7+$BA7)","v":3.3026115613882624E-6},{"$f":"AX7/($BB7+$BA7)","v":0.33589058111334147},{"$f":"SUM(BD7:BO7)","v":0.89784871212451545},0.20968604516872927,{"$f":"100*BQ7","v":20.968604516872926},3,9.5725635821403898,{"$f":"BT7/100","v":9.5725635821403893E-2},36.204977102424678,null,0.28366805024390451,null,{"$f":"AZ7","v":3.7273600385644035E-2},{"$f":"AX7","v":1.5858550579015779E-2},{"$f":"Z7","v":3.9676698819354594E-5},null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR7, IF(MODE_ILIM=4,#REF!,#REF!))","v":20.968604516872926},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ7, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7273600385644035E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA7, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.5858550579015779E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB7, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.9676698819354594E-5},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S7, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":36.204977102424678},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P7, IF(MODE_ILIM=4,#REF!,#REF!))","v":15.819618502553386}]
["Vin",{"$f":"Vin","v":68},"V",{"$f":"B8","v":68},"Vin",null,null,2,6.0000000000000001E-3,0.12661386028450594,0.12661386028450594,0,14.257461006838859,2.1497853144283807,7,15.048497200998666,1.2441798184621381E-6,{"$f":"OnTime*S8","v":4.6853499779608409E-3},72409.95420484936,6.3088857008150795E-6,7.501370236800596E-6,3.0693698104177175E-4,2.1605131999946597E-2,7.9352893884969809E-5,0,7.9353901398844534E-5,1.1168801564234809E-2,3.1185532095313479E-7,{"$f":"AB8","v":3.1185532095313479E-7},2.5168662956319048E-3,1.9003847850263601E-8,{"$f":"AE8","v":1.9003847850263601E-8},4.9665817786643781E-3,4.5633828943697885E-5,2.1722986261454809E-4,14.166666666666666,86.572846132243242,1.4671767237788054E-2,2.6785890259457872E-2,4.1674887359860475E-2,4.172089678709244E-2,2.1026525965336152E-2,3.3158609562821653E-4,5.8652062905927992E-4,0,2.8153397487419308E-5,6.1467402654669925E-4,9.4632202611883104E-4,2.0890779836890899E-2,3.1018036031981132E-2,8.0375049167382795E-4,{"$f":"AO8+AV8+AX8+AY8","v":7.4489005336866226E-2},7.4568690097433873E-2,1.9799999999999998E-2,{"$f":"BB8/(BB8+BA8)","v":0.20981535273571009},4.8754970726478097E-4,3.5143859603191645E-3,0.11583298099695995,0.44161773695101575,0,2.9833409214805739E-4,6.5135377624936834E-3,8.4088158692294506E-4,0,2.0137873939590018E-7,3.3046481903176799E-6,0.32868990763732758,0.89779882072138162,0.20981535273571009,{"$f":"100*BQ8","v":20.981535273571009},6,10.507357436577642,0.10507357436577643,72.409954204849356,null,0.28384298046101891,null,7.4489005336866226E-2,3.1018036031981132E-2,7.9353901398844534E-5,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR8, IF(MODE_ILIM=4,#REF!,#REF!))","v":20.981535273571009},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ8, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.4489005336866226E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA8, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.1018036031981132E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB8, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.9353901398844534E-5},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S8, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":72.409954204849356},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P8, IF(MODE_ILIM=4,#REF!,#REF!))","v":15.048497200998666}]
["Vout",{"$f":"Vout","v":3.3},"V",{"$f":"B9","v":3.3},"Vout",null,null,3,8.9999999999999993E-3,0.12661386028450594,0.12661386028450594,0,14.075642825020678,2.0397504111527498,7,14.278252878069248,1.2441798184621381E-6,7.0280249669412613E-3,108614.93130727403,6.3088857008150795E-6,2.8979515909287055E-6,4.5540547156265766E-4,2.6460774612672901E-2,1.1902934082745471E-4,{"$f":"Core_Loss/1000*S9/$S$106","v":0},1.1903160774806397E-4,1.3678932435386938E-2,4.6778298142970202E-7,4.6778298142970202E-7,3.1329490324537375E-3,2.944610891985843E-8,2.944610891985843E-8,6.082795561766113E-3,6.8450743415546825E-5,3.258447939218221E-4,{"$f":"15*VIN_nom/24","v":42.5},86.572846132243242,2.2966767437726413E-2,4.0178835389186804E-2,6.3471447620835036E-2,6.3540756416252675E-2,2.5752129839227533E-2,4.973791434423248E-4,8.7978094358891971E-4,0,4.4086913716751137E-5,9.2386785730567088E-4,1.421386471392203E-3,3.098663719231114E-2,4.6177521484946485E-2,1.2056257375107418E-3,0.11234529011010211,0.11246481894694052,2.9699999999999997E-2,{"$f":"BB9/(BB9+BA9)","v":0.2089124455684411},4.8752424074416292E-4,3.4995902486410408E-3,0.11533451209378094,0.44646381637164517,0,3.1011127818624017E-4,6.4985688030910205E-3,8.3726298608293131E-4,0,2.0712655309502737E-7,3.2904271597904285E-6,0.32481679945149505,0.89825168302737923,0.2089124455684411,20.891244556844111,9,11.516667783884284,0.11516667783884284,108.61493130727403,null,0.28262150711268835,null,0.11234529011010211,4.6177521484946485E-2,1.1903160774806397E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR9, IF(MODE_ILIM=4,#REF!,#REF!))","v":20.891244556844111},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ9, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11234529011010211},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA9, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.6177521484946485E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB9, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1903160774806397E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S9, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":108.61493130727403},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P9, IF(MODE_ILIM=4,#REF!,#REF!))","v":14.278252878069248}]
["Iout",{"$f":"Iout","v":0.3},"A",{"$f":"B10","v":0.3},"Iout(max)",null,null,4,1.2E-2,0.12661386028450594,0.12661386028450594,0,13.893824643202498,1.9298622203713416,8,15.438897762970733,1.2441798184621381E-6,9.3706999559216818E-3,144819.90840969872,6.3088857008150795E-6,5.9624226799275778E-7,6.0387396208354358E-4,3.055427069118543E-2,1.5870578776993962E-4,0,1.587098178766073E-4,1.5795070647594705E-2,6.2371064190626957E-7,6.2371064190626957E-7,3.6973238204395385E-3,4.1010610299568876E-8,4.1010610299568876E-8,7.0238073100222526E-3,9.1267657887395757E-5,4.3445972522909617E-4,42.5,86.572846132243242,3.1901178691694336E-2,5.3571780518915743E-2,8.5907418935839169E-2,8.6000235052343874E-2,2.9735998189768423E-2,6.6317219125643318E-4,1.1730412581185598E-3,0,6.1260133000677061E-5,1.234301391119237E-3,1.8977218624843424E-3,4.1082494547731385E-2,6.1337006937911852E-2,1.6075009833476559E-3,0.15084246483608774,0.15100183937521655,3.9599999999999996E-2,0.20776294777535645,4.8696338298177442E-4,3.4806614329628985E-3,0.11469990764617344,0.45071663115864707,0,3.2140368215482476E-4,6.4758104914685831E-3,8.3265611858820141E-4,0,2.1516376984608143E-7,3.2723222606390494E-6,0.3218070042711631,0.89882452567017035,0.20776294777535645,20.776294777535647,12,12.603144523181673,0.12603144523181672,144.81990840969871,null,0.28106644035819067,null,0.15084246483608774,6.1337006937911852E-2,1.587098178766073E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR10, IF(MODE_ILIM=4,#REF!,#REF!))","v":20.776294777535647},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ10, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15084246483608774},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA10, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1337006937911852E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB10, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.587098178766073E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S10, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":144.81990840969871},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P10, IF(MODE_ILIM=4,#REF!,#REF!))","v":15.438897762970733}]
["Rt",{"$f":"Vout*2500/(Fsw/1000)","v":11},"kW",{"$f":"B11*1000","v":11000},"RT pin resistance to get Fsw",null,null,5,1.4999999999999999E-2,0.12661386028450594,0.12661386028450594,0,13.712006461384314,1.8201473148040275,8,14.56117851843222,1.2441798184621381E-6,1.1713374944902101E-2,181024.88551212338,5.5241023750462709E-6,0,6.6E-4,3.4160713134210048E-2,1.9838223471242445E-4,0,1.9838853179406904E-4,1.7659425838716693E-2,7.7963830238283692E-7,7.7963830238283692E-7,4.2451705214123781E-3,5.4064418267605926E-8,5.4064418267605926E-8,7.8528553030348478E-3,1.140845723592447E-4,5.4307465653637014E-4,42.5,86.572846132243242,4.1475000999691813E-2,6.6964725648644668E-2,0.10898280130487285,0.1090993413329516,3.3245856665566446E-2,8.2896523907054177E-4,1.4663015726481994E-3,0,7.9674423887331536E-5,1.545975996535531E-3,2.3753296928965902E-3,4.4899065126050422E-2,7.0217205613776007E-2,2.0093762291845695E-3,0.18370125286880878,0.1839004751033235,4.9499999999999995E-2,0.2120818305022171,4.9931358548929749E-4,3.5533505062228972E-3,0.11708423774549986,0.46693478775751218,0,3.413635891360575E-4,6.6237054395503975E-3,8.4996499953396887E-4,0,2.3163799578245193E-7,3.3403458242220834E-6,0.30084431311757925,0.89673460872434396,0.2120818305022171,21.208183050221709,15,13.76888730592373,0.1376888730592373,181.02488551212338,null,0.28690912312410771,null,0.18370125286880878,7.0217205613776007E-2,1.9838853179406904E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR11, IF(MODE_ILIM=4,#REF!,#REF!))","v":21.208183050221709},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ11, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.18370125286880878},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA11, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0217205613776007E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB11, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.9838853179406904E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S11, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":181.02488551212338},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P11, IF(MODE_ILIM=4,#REF!,#REF!))","v":14.56117851843222}]
["Tamb",{"$f":"'Design Converter'!E56","v":25},"°C",{"$f":"B12","v":25},"Ambient temperature",null,null,6,1.7999999999999999E-2,0.12661386028450594,0.12661386028450594,0,13.530188279566133,1.7106390366506117,8,13.685112293204893,1.2441798184621381E-6,1.4056049933882523E-2,217229.86261454807,4.6034186458718921E-6,0,6.6E-4,3.7421186328139698E-2,2.3805868165490941E-4,0,2.3806774951004429E-4,1.9344931768909439E-2,9.3556596285940426E-7,9.3556596285940426E-7,4.7948250853208094E-3,6.8971042796465116E-8,6.8971042796465116E-8,8.6023719805925058E-3,1.3690148683109362E-4,6.5168958784364421E-4,42.5,86.572846132243242,5.1688234361718863E-2,8.0357670778373608E-2,0.13269759472793613,0.132838083895817,3.6419011278628448E-2,9.947582868846496E-4,1.7595618871778394E-3,0,9.9331154924849033E-5,1.8588930421026884E-3,2.8542114563257213E-3,4.4899065126050422E-2,7.5280833711321118E-2,2.4112514750214836E-3,0.2133843805384853,0.213623452825001,5.9399999999999994E-2,0.21756372716476274,5.1456813115215573E-4,3.6455418167354254E-3,0.12011063416340068,0.48603002179813065,0,3.6381912944496021E-4,6.8085471151600203E-3,8.719349169153506E-4,0,2.5261948042490425E-7,3.4266871698347138E-6,0.27573028226103946,0.89407902863862898,0.21756372716476274,21.756372716476275,18,15.015319606822954,0.15015319606822955,217.22986261454807,null,0.29432515758959438,null,0.2133843805384853,7.5280833711321118E-2,2.3806774951004429E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR12, IF(MODE_ILIM=4,#REF!,#REF!))","v":21.756372716476275},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ12, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.2133843805384853},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA12, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.5280833711321118E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB12, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.3806774951004429E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S12, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":217.22986261454807},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P12, IF(MODE_ILIM=4,#REF!,#REF!))","v":13.685112293204893}]
["VDD",5,"V",{"$f":"B13","v":5},"Gate drive rail",null,null,7,2.1000000000000001E-2,0.12661386028450594,0.12661386028450594,0,13.348370097747951,1.601379776314934,9,14.412417986834406,1.2441798184621381E-6,1.6398724922862946E-2,253434.83971697278,3.9457874107473357E-6,0,6.600000000000001E-4,4.0419500869913125E-2,2.7773512859739433E-4,0,2.77747471034128E-4,2.0894914437115761E-2,1.0914936233359717E-6,1.0914936233359717E-6,5.356940593066367E-3,8.6090437552926719E-8,8.6090437552926719E-8,9.2916236995782154E-3,1.5971840130294261E-4,7.6030451915091828E-4,42.5,86.572846132243242,6.2540878777775463E-2,9.3750615908102561E-2,0.15705179920502893,0.15721647137883668,3.9337028098197051E-2,1.1605513346987582E-3,2.0528222017074799E-3,0,1.2023169466136406E-4,2.173053896368844E-3,3.3343686466639805E-3,4.4899065126050429E-2,8.0344461808866244E-2,2.8131267208583981E-3,0.24370842855522531,0.24398735361032034,6.93E-2,0.22120267288605011,5.2562662332223146E-4,3.7068676309852818E-3,0.12211959072967157,0.50130270946198618,0,3.8377449097710205E-4,6.9362962511144884E-3,8.865187994241627E-4,0,2.7479704035551186E-7,3.484001542857093E-6,0.25645612848069821,0.89232127126676242,0.22120267288605011,22.12026728860501,21,16.343061169118954,0.16343061169118955,253.43483971697279,null,0.29924800611234831,null,0.24370842855522531,8.0344461808866244E-2,2.77747471034128E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR13, IF(MODE_ILIM=4,#REF!,#REF!))","v":22.12026728860501},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ13, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.24370842855522531},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA13, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.0344461808866244E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB13, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.77747471034128E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S13, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":253.43483971697279},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P13, IF(MODE_ILIM=4,#REF!,#REF!))","v":14.412417986834406}]
["K1",400,"pC",4,"RT constant",null,null,8,2.4E-2,0.12661386028450594,0.12661386028450594,0,13.166551915929769,1.4924242260231899,9,13.43181803420871,1.2441798184621381E-6,1.8741399911843364E-2,289639.81681939744,3.4525639844039187E-6,0,6.5999999999999989E-4,4.3210263999893195E-2,3.1741157553987924E-4,0,3.1742769637591549E-4,2.2337603128469618E-2,1.2474212838125391E-6,1.2474212838125391E-6,5.9379850650439622E-3,1.0577899989805544E-7,1.0577899989805544E-7,9.9331635573287561E-3,1.8253531577479154E-4,8.6891945045819235E-4,42.5,86.572846132243242,7.4032934247861615E-2,0.10714356103783149,0.1820454147361513,0.18223451242006278,4.2053051930672304E-2,1.3263443825128661E-3,2.3460825162371197E-3,0,1.4237741164501097E-4,2.4884599278821307E-3,3.8158027579991028E-3,4.4899065126050408E-2,8.5408089906411341E-2,3.2150019666953118E-3,0.27467340705116855,0.27499218794782815,7.9199999999999993E-2,0.22360741624167613,5.3388440046378419E-4,3.7475214736031595E-3,0.12344717990645437,0.51397354580549426,0,4.0197784279189951E-4,7.0257335213973612E-3,8.9615634206656578E-4,0,2.9864859671505937E-7,3.5218768969469254E-6,0.24113487765289673,0.89116469747066185,0.22360741624167613,22.360741624167613,24,17.75180413241851,0.17751804132418511,289.63981681939742,null,0.30250119760860883,null,0.27467340705116855,8.5408089906411341E-2,3.1742769637591549E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR14, IF(MODE_ILIM=4,#REF!,#REF!))","v":22.360741624167613},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ14, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.27467340705116855},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA14, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.5408089906411341E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB14, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.1742769637591549E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S14, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":289.63981681939742},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P14, IF(MODE_ILIM=4,#REF!,#REF!))","v":13.43181803420871}]
["Outputs",null,null,null,null,null,null,9,2.7E-2,0.12661386028450594,0.12661386028450594,0,12.98473373411159,1.3838441245329194,10,13.838441245329193,1.2441798184621381E-6,2.1084074900823785E-2,325844.7939218221,3.0689457639145945E-6,0,6.6E-4,4.5831406036778141E-2,3.570880224823641E-4,0,3.5710842554500247E-4,2.3692605971392056E-2,1.4033489442891062E-6,1.4033489442891062E-6,6.541905198722075E-3,1.2838957088720073E-7,1.2838957088720073E-7,1.0535710965033378E-2,2.0535223024664042E-4,9.775343817654662E-4,42.5,86.572846132243242,8.6164400771977331E-2,0.12053650616756043,0.20767844132130323,0.20789221565770313,4.4603997284652627E-2,1.4921374303269741E-3,2.6393428307667595E-3,0,1.6576967442392444E-4,2.8051125051906838E-3,4.29851528461436E-3,4.4899065126050422E-2,9.0471718003956467E-2,3.6168772125322254E-3,0.30627932615880621,0.30663796632286638,8.9099999999999999E-2,0.2251489813522389,5.4019162827935018E-4,3.7737162125234909E-3,0.12429823336764848,0.52478776108094438,0,4.18887467291121E-4,7.088307779148254E-3,9.0233450634107364E-4,0,3.2443076432664774E-7,3.5461569617107984E-6,0.22861520931288229,0.8904285119427845,0.2251489813522389,22.514898135223891,27,19.240199150848532,0.19240199150848533,325.84479392182209,null,0.30458666194594941,null,0.30627932615880621,9.0471718003956467E-2,3.5710842554500247E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR15, IF(MODE_ILIM=4,#REF!,#REF!))","v":22.514898135223891},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ15, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.30627932615880621},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA15, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0471718003956467E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB15, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.5710842554500247E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S15, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":325.84479392182209},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P15, IF(MODE_ILIM=4,#REF!,#REF!))","v":13.838441245329193}]
["Design","Value","Units","Std Units","Description",null,null,10,0.03,0.12661386028450594,0.12661386028450594,0,12.802915552293406,1.2757353407899932,11,14.033088748689924,1.2441798184621381E-6,2.3426749889804203E-2,362049.77102424676,2.7620511875231354E-6,0,6.6E-4,4.8310543814736567E-2,3.967644694248489E-4,0,3.9678965855098462E-4,2.4974199524835015E-2,1.5592766047656736E-6,1.5592766047656736E-6,7.1710397960592538E-3,1.5427143526999666E-7,1.5427143526999666E-7,1.1105614472905364E-2,2.2816914471848941E-4,1.0861493130727403E-3,42.5,86.572846132243242,9.8935278350122585E-2,0.13392945129728934,0.23395087896048467,0.23418958973012088,4.7016741389156028E-2,1.6579304781410833E-3,2.9326031452963988E-3,0,1.9040985154623871E-4,3.1230129968426376E-3,4.7825077209885849E-3,4.4899065126050422E-2,9.5535346101501578E-2,4.0187524583691391E-3,0.33852619601098022,0.33892469921757123,9.8999999999999991E-2,0.22606626248046924,5.4509546975248788E-4,3.7894522211488041E-3,0.12480463771847315,0.53422627081431739,0,4.3480043917696145E-4,7.1313926855974203E-3,9.0601071401941419E-4,0,3.5227845231298775E-7,3.5606043859859764E-6,0.21815473361560131,0.88999630656092521,0.22606626248046924,22.606626248046922,30,20.80575856495858,0.20805758564958579,362.04977102424675,null,0.30582758071553773,null,0.33852619601098022,9.5535346101501578E-2,3.9678965855098462E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR16, IF(MODE_ILIM=4,#REF!,#REF!))","v":22.606626248046922},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ16, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.33852619601098022},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA16, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.5535346101501578E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB16, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.9678965855098462E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S16, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":362.04977102424675},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P16, IF(MODE_ILIM=4,#REF!,#REF!))","v":14.033088748689924}]
["On-Time",{"$f":"(Rt*k_RT/10000)/Vin","v":6.4705882352941183E-2},"µs",{"$f":"B17/1000000","v":6.4705882352941178E-8},"On Time - fixed",null,null,11,3.3000000000000002E-2,0.12661386028450594,0.12661386028450594,0,12.621097370475225,1.1682287304418391,11,12.850516034860231,1.2441798184621381E-6,2.5769424878784624E-2,398254.74812667147,2.5109556250210319E-6,0,6.6E-4,5.0668525812807508E-2,4.3644091636733397E-4,0,4.3647139540345847E-4,2.6193161437613757E-2,1.7152042652422411E-6,1.7152042652422411E-6,7.8266706734166722E-3,1.8377032149036176E-7,1.8377032149036176E-7,1.1647666723549638E-2,2.5098605919033831E-4,1.1947642443800146E-3,42.5,86.572846132243242,0.11234556698229746,0.1473223964270183,0.26086272765369578,0.26112664327583496,4.9311574381074627E-2,1.8237235259551917E-3,3.225863459826039E-3,0,2.1629931156008848E-4,3.4421627713861276E-3,5.2677815617962016E-3,4.4899065126050422E-2,0.1005989741990467,4.4206277042060536E-3,0.37141402674088386,0.37185239711087403,0.1089,0.22651993137100224,5.489637154701719E-4,3.7974200469541052E-3,0.12505509517685665,0.54261347259290738,0,4.4991832148931379E-4,7.1599492630138152E-3,9.078288927734235E-4,0,3.8225565300297302E-7,3.5677497929285835E-6,0.20925319312728452,0.88978979114219525,0.22651993137100224,22.651993137100224,33,22.444784059665849,0.22444784059665848,398.25474812667147,null,0.30644131430725224,null,0.37141402674088386,0.1005989741990467,4.3647139540345847E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR17, IF(MODE_ILIM=4,#REF!,#REF!))","v":22.651993137100224},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ17, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.37141402674088386},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA17, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1005989741990467},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB17, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.3647139540345847E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S17, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":398.25474812667147},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P17, IF(MODE_ILIM=4,#REF!,#REF!))","v":12.850516034860231}]
["Off Time",{"$f":"L*Iripple*1000000/(Vout+(Rdcr+RdsonBot)*Iout)","v":1.1597479931569947},"µs",{"$f":"B18/1000000","v":1.1597479931569948E-6},"Off Time - depends on Vout, L, Iout, DCR, etc.",null,null,12,3.5999999999999997E-2,0.12661386028450594,0.12661386028450594,0,12.439279188657043,1.0615072687795677,12,12.738087225354814,1.2441798184621381E-6,2.8112099867765045E-2,434459.72522909613,2.3017093229359461E-6,0,6.6E-4,5.2921549225345803E-2,4.7611736330981883E-4,0,4.7615363611201982E-4,2.7357864870773876E-2,1.8711319257188081E-6,1.8711319257188081E-6,8.5093752549075634E-3,2.1722840168649947E-7,2.1722840168649947E-7,1.2165591123532226E-2,2.738029736621873E-4,1.3033791756872884E-3,42.5,86.572846132243242,0.12639526666850182,0.16071534155674722,0.28841398740093632,0.28870338493351955,5.1504259678455067E-2,1.9895165737692992E-3,3.5191237743556788E-3,0,2.4343942301360803E-4,3.7625631973692867E-3,5.7543383019072591E-3,4.4899065126050422E-2,0.10566260229659181,4.8225029500429673E-3,0.40494282848206153,0.40542107047850096,0.11879999999999999,0.22662194766715724,5.5205246198720449E-4,3.7994945581258503E-3,0.12511141542006013,0.55017625891625543,0,4.6438313284775115E-4,7.1774360270083701E-3,9.0823774571904597E-4,0,4.1438319426614561E-7,3.5693565770083746E-6,0.2015611509093761,0.8897544129111512,0.22662194766715724,22.662194766715725,36,24.152326085424395,0.24152326085424394,434.45972522909614,null,0.30657932427257972,null,0.40494282848206153,0.10566260229659181,4.7615363611201982E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR18, IF(MODE_ILIM=4,#REF!,#REF!))","v":22.662194766715725},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ18, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.40494282848206153},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA18, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10566260229659181},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB18, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.7615363611201982E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S18, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":434.45972522909614},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P18, IF(MODE_ILIM=4,#REF!,#REF!))","v":12.738087225354814}]
["DIL",{"$f":"(Vin-Vout-(Rdcr+RdsonTop)*Iout)/L*OnTime*1000","v":125.67450980392158},"mA",{"$f":"B19/1000","v":0.12567450980392159},"Inductor pk-pk ripple current in CCM",null,null,13,3.9E-2,0.12661386028450594,0.12661386028450594,0,12.257461006838859,0.95583398394641583,13,12.425841791303405,1.2441798184621381E-6,3.0454774856745467E-2,470664.70233152085,2.1246547596331809E-6,0,6.600000000000001E-4,5.5082494830737808E-2,5.157938102523038E-4,0,5.1583638068626559E-4,2.8474968559739453E-2,2.027059586195376E-6,2.027059586195376E-6,9.2192604853624707E-3,2.5498429169089759E-7,2.5498429169089759E-7,1.2662348702632012E-2,2.9661988813403623E-4,1.4119941069945625E-3,42.5,86.572846132243242,0.14108437740873581,0.17410828668647618,0.31660465820220651,0.31691982334200464,5.3607333100157202E-2,2.1553096215834074E-3,3.8123840888853191E-3,0,2.7183155445493199E-4,4.0842156433402513E-3,6.2421794363874726E-3,4.4899065126050429E-2,0.11072623039413693,5.2243781958798818E-3,0.43911261136840896,0.43963072979297313,0.12869999999999998,0.22645265028495248,5.5454530835052581E-4,3.7970211356216947E-3,0.12501795123738682,0.55707819691104266,0,4.7829818133176177E-4,7.1863361054363816E-3,9.0755924889050592E-4,0,4.486547679443291E-7,3.566690097742518E-6,0.19482710434199355,0.88985102781491954,0.22645265028495248,22.645265028495249,39,25.922181532084487,0.25922181532084487,470.66470233152086,null,0.30635029492404697,null,0.43911261136840896,0.11072623039413693,5.1583638068626559E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR19, IF(MODE_ILIM=4,#REF!,#REF!))","v":22.645265028495249},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ19, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.43911261136840896},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA19, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11072623039413693},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB19, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.1583638068626559E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S19, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":470.66470233152086},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P19, IF(MODE_ILIM=4,#REF!,#REF!))","v":12.425841791303405}]
["CCM Freq",{"$f":"'Design Converter'!E12","v":750},"kHz",{"$f":"B20*1000","v":750000},"Frequency in CCM",{"$f":"10000*Vout/(k_RT*Rt/1000+Vin*0.75)","v":347.36842105263156},null,14,4.2000000000000003E-2,0.12661386028450594,0.12661386028450594,0,12.075642825020678,0.85159916405243785,15,12.773987460786568,1.2441798184621381E-6,3.2797449845725891E-2,506869.67943394557,1.9728937053736679E-6,0,6.600000000000001E-4,5.7161806314582259E-2,5.5547025719478876E-4,0,5.5551962913579238E-4,2.9549871381594494E-2,2.1829872466719434E-6,2.1829872466719434E-6,9.9561212499367866E-3,2.9737305103032852E-7,2.9737305103032852E-7,1.3140340252410785E-2,3.1943680260588522E-4,1.5206090383018366E-3,42.5,86.572846132243242,0.15641289920299931,0.18750123181620512,0.3454347400575063,0.34577596714027575,5.5630958639921783E-2,2.321102669397516E-3,4.1056444034149597E-3,0,3.014770744321947E-4,4.4071214778471542E-3,6.7313064604982379E-3,4.4899065126050429E-2,0.11578985849168205,5.6262534417167963E-3,0.47392338553417285,0.47448138552360636,0.1386,0.22607112737834589,5.5657713776129428E-4,3.7909893164772856E-3,0.1248073234877267,0.56344026782428791,0,4.9174070776054652E-4,7.1884770634215583E-3,9.0603021117724133E-4,0,4.8504661542831716E-7,3.5606810094349028E-6,0.18886539573011327,0.89005084720635075,0.22607112737834589,22.607112737834591,42,27.746934669307642,0.27746934669307644,506.86967943394558,null,0.30583416206001496,null,0.47392338553417285,0.11578985849168205,5.5551962913579238E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR20, IF(MODE_ILIM=4,#REF!,#REF!))","v":22.607112737834591},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ20, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.47392338553417285},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA20, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11578985849168205},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB20, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.5551962913579238E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S20, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":506.86967943394558},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P20, IF(MODE_ILIM=4,#REF!,#REF!))","v":12.773987460786568}]
["Icrit_Skip",{"$f":"1000*Iripple/2","v":62.83725490196079},"mA",{"$f":"Iripple/2","v":6.2837254901960793E-2},"CCM-DCM (critical conduction) boundary",null,null,15,4.4999999999999998E-2,0.12661386028450594,0.12661386028450594,0,11.893824643202498,0.74940327976040977,16,11.990452476166556,1.2441798184621381E-6,3.5140124834706306E-2,543074.65653637017,1.8413674583487569E-6,0,6.6E-4,5.9168090771237268E-2,5.951467041372734E-4,0,5.9520338147019711E-4,3.0587022785151945E-2,2.3389149071485109E-6,2.3389149071485109E-6,1.0719548854403797E-2,3.4472618292584927E-7,3.4472618292584927E-7,1.3601544369343049E-2,3.422537170777341E-4,1.6292239696091104E-3,42.5,86.572846132243242,0.17238083205129237,0.20089417694593403,0.3749042329668355,0.37527182496747374,5.7583512885913492E-2,2.4868957172116241E-3,4.3989047179445991E-3,0,3.3237735149353059E-4,4.7312820694381296E-3,7.2217208696966741E-3,4.4899065126050422E-2,0.12085348658922716,6.0281286875537091E-3,0.50937516111395131,0.50997304813651156,0.14849999999999999,0.22552175889393983,5.5824912147661959E-4,3.7821423478250527E-3,0.12450403305456813,0.56935395310076853,0,5.0476986481703913E-4,7.1852326876972834E-3,9.0382849506376512E-4,0,5.2352360343590286E-7,3.5520283081709641E-6,0.18353596541459719,0.89033224963872526,0.22552175889393983,22.552175889393983,45,29.618044224570543,0.29618044224570544,543.07465653637018,null,0.30509096388146412,null,0.50937516111395131,0.12085348658922716,5.9520338147019711E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR21, IF(MODE_ILIM=4,#REF!,#REF!))","v":22.552175889393983},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ21, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.50937516111395131},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA21, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12085348658922716},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB21, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9520338147019711E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S21, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":543.07465653637018},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P21, IF(MODE_ILIM=4,#REF!,#REF!))","v":11.990452476166556}]
["Tr",null,"ns",{"$f":"B22/1000000000","v":0},"Switch rise time",null,null,16,4.8000000000000001E-2,0.12661386028450594,0.12661386028450594,0,11.712006461384314,0.65020844609203676,19,12.353960475748698,1.2441798184621381E-6,3.7482799823686727E-2,579279.63363879488,1.7262819922019593E-6,0,6.5999999999999989E-4,6.110854138237086E-2,6.3482315107975848E-4,0,6.3488763769907778E-4,3.159014129518941E-2,2.4948425676250783E-6,2.4948425676250783E-6,1.1509005666474139E-2,3.9737163429280157E-7,3.9737163429280157E-7,1.4047614620044505E-2,3.6507063154958303E-4,1.7378389009163847E-3,42.5,86.572846132243242,0.188988175953615,0.21428712207566297,0.40501313693019436,0.40540740546289522,5.9471996379536846E-2,2.6526887650257327E-3,4.6921650324742393E-3,0,3.6453375418707428E-4,5.0566987866613134E-3,7.7134241596356614E-3,4.4899065126050408E-2,0.12591711468677227,6.4300039333906236E-3,0.54546794824269385,0.54610572809459479,0.15839999999999999,0.22483848417869987,5.5963850537765953E-4,3.7710486473399212E-3,0.12412681686864969,0.57488977133740604,0,5.1743192375879152E-4,7.1776546094772771E-3,9.0109012001463821E-4,0,5.6404315599751383E-7,3.5412665477860997E-6,0.17873114392884715,0.8906787012505748,0.22483848417869987,22.483848417869986,48,31.525976771075946,0.31525976771075948,579.27963363879485,null,0.30416661430876313,null,0.54546794824269385,0.12591711468677227,6.3488763769907778E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR22, IF(MODE_ILIM=4,#REF!,#REF!))","v":22.483848417869986},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ22, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54546794824269385},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA22, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12591711468677227},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB22, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.3488763769907778E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S22, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":579.27963363879485},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P22, IF(MODE_ILIM=4,#REF!,#REF!))","v":12.353960475748698}]
["Tf",null,"ns",{"$f":"B23/1000000000","v":0},"Switch fall time",null,null,17,5.1000000000000004E-2,0.12661386028450594,0.12661386028450594,0,11.530188279566133,0.55562431478121732,21,11.668110610405565,1.2441798184621381E-6,3.9825474812667148E-2,615484.6107412196,1.6247359926606675E-6,0,6.6E-4,6.2989242686735725E-2,6.7449959802224333E-4,0,6.7457239783203133E-4,3.2562372322063056E-2,2.6507702281016453E-6,2.6507702281016453E-6,1.2323876497011967E-2,4.5563379574081185E-7,4.5563379574081185E-7,1.4479949716603598E-2,3.8788754602143202E-4,1.846453832223659E-3,42.5,86.572846132243242,0.2062349309099672,0.22768006720539194,0.43576145194758276,0.43618271726599245,6.1302330709795377E-2,2.8184818128398409E-3,4.9854253470038795E-3,0,3.979476510609603E-4,5.38337299806484E-3,8.2064178261638584E-3,4.4899065126050422E-2,0.13098074278431743,6.8318791792275381E-3,0.58220175705570132,0.58287943585755719,0.16830000000000001,0.22404766686386499,5.6080517956241577E-4,3.7581497753279014E-3,0.12369022952741389,0.58010301020835486,0,5.2976377156365784E-4,7.1665606659201261E-3,8.9792074413249203E-4,0,6.0655786619165602E-7,3.5288109625571526E-6,0.17436678446180831,0.89107735970291235,0.22404766686386499,22.404766686386498,51.000000000000007,33.460383546927204,0.33460383546927203,615.48461074121963,null,0.30309677866177087,null,0.58220175705570132,0.13098074278431743,6.7457239783203133E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR23, IF(MODE_ILIM=4,#REF!,#REF!))","v":22.404766686386498},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ23, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.58220175705570132},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA23, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13098074278431743},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB23, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.7457239783203133E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S23, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":615.48461074121963},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P23, IF(MODE_ILIM=4,#REF!,#REF!))","v":11.668110610405565}]
[null,null,null,null,null,null,null,18,5.3999999999999999E-2,0.12661386028450594,0.12661386028450594,0,11.348370097747953,0.46845207133247657,25,11.711301783311914,1.2441798184621381E-6,4.216814980164757E-2,651689.5878436442,1.5344728819572972E-6,0,6.6E-4,6.4815395999839792E-2,7.1417604496472819E-4,0,7.1425766187865566E-4,3.3506404692704418E-2,2.8066978885782119E-6,2.8066978885782119E-6,1.3163503859456657E-2,5.1983350157379088E-7,5.1983350157379088E-7,1.4899745335993133E-2,4.1070446049328089E-4,1.9550687635309324E-3,42.5,86.572846132243242,0.2241210969203489,0.24107301233512085,0.46714917801900069,0.46759776901637301,6.307957789600846E-2,2.9842748606539495E-3,5.2786856615335189E-3,0,4.3262041066332283E-4,5.7113060721968416E-3,8.7007033653257425E-3,4.4899065126050422E-2,0.1360443708818625,7.2337544250644509E-3,0.61957659768862572,0.62029418188189456,0.1782,0.22317006691271996,5.6179620033684036E-4,3.7437934564325519E-3,0.12320573200548103,0.58503767293334741,0,5.4179531984030384E-4,7.1525957255398039E-3,8.9440356757710488E-4,0,6.510172689657488E-7,3.5149885274847889E-6,0.17037615798431058,0.89151811319866214,0.22317006691271996,22.317006691271995,54,35.410314704487,0.35410314704487,651.68958784364418,null,0.30190954149090843,null,0.61957659768862572,0.1360443708818625,7.1425766187865566E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR24, IF(MODE_ILIM=4,#REF!,#REF!))","v":22.317006691271995},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ24, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.61957659768862572},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA24, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1360443708818625},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB24, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1425766187865566E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S24, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":651.68958784364418},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P24, IF(MODE_ILIM=4,#REF!,#REF!))","v":11.711301783311914}]
["Components","Input Value","Units","Std Units","Description",null,null,19,5.6999999999999995E-2,0.12661386028450594,0.12661386028450594,0,11.166551915929769,0.3936469423838983,29,11.415761329133051,1.2441798184621381E-6,4.4510824790627984E-2,687894.5649460688,1.4537111513279661E-6,0,6.6E-4,6.6591489118231956E-2,7.5385249190721283E-4,0,7.5394342984854866E-4,3.4424558379475424E-2,2.9626255490547789E-6,2.9626255490547789E-6,1.4027212003696414E-2,5.9028802978993422E-7,5.9028802978993422E-7,1.5308033131644628E-2,4.3352137496512983E-4,2.0636836948382063E-3,42.5,86.572846132243242,0.2426466739847602,0.25446595746484973,0.49917631514444816,0.49965256935380015,6.4808105547254483E-2,3.1500679084680576E-3,5.5719459760631574E-3,0,4.6855340154229651E-4,6.0404993776054542E-3,9.1962822733616459E-3,4.4899065126050422E-2,0.14110799897940762,7.6356296709013637E-3,0.65759248027747075,0.65834997662089811,0.18809999999999996,0.22222222836004027,5.6264897218526449E-4,3.7282568172006471E-3,0.12268245778541466,0.58972925622516226,0,5.5355120146946242E-4,7.1362744928172286E-3,8.9060489423918186E-4,0,6.9736906621040426E-7,3.5000598155626846E-6,0.16670565642015023,0.89199290423752065,0.22222222836004027,22.222222836004025,56.999999999999993,37.364462120689176,0.37364462120689174,687.89456494606884,null,0.30062728394263766,null,0.65759248027747075,0.14110799897940762,7.5394342984854866E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR25, IF(MODE_ILIM=4,#REF!,#REF!))","v":22.222222836004025},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ25, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.65759248027747075},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA25, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14110799897940762},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB25, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.5394342984854866E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S25, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":687.89456494606884},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P25, IF(MODE_ILIM=4,#REF!,#REF!))","v":11.415761329133051}]
["L",{"$f":"'Design Converter'!E17","v":33},"µH",{"$f":"B26/1000000","v":3.3000000000000003E-5},"Filter inductance",null,null,20,0.06,0.12661386028450594,0.12661386028450594,0,10.984733734111588,0.3394850446096418,33,11.203006472118179,1.2441798184621381E-6,4.6853499779608405E-2,724099.54204849352,1.3810255937615677E-6,0,6.6E-4,6.8321426268420096E-2,7.935289388496978E-4,0,7.9362970175130909E-4,3.5318851677433385E-2,3.1185532095313477E-6,3.1185532095313477E-6,1.4914323116629895E-2,6.6731110208172268E-7,6.6731110208172268E-7,1.5705710606069696E-2,4.5633828943697881E-4,2.1722986261454805E-3,42.5,86.572846132243242,0.26181166210320111,0.26785890259457867,0.53184286332392527,0.53234712691819297,6.6491713331132893E-2,3.3158609562821671E-3,5.8652062905927976E-3,0,5.05747992246016E-4,6.3709542828388139E-3,9.6931560467077814E-3,4.4899065126050422E-2,0.14617162707695275,8.0375049167382782E-3,0.69624941495859172,0.69704683052465466,0.19799999999999998,0.22121747516153675,5.6339353100899581E-4,3.7117630615166514E-3,0.12212776263736469,0.59420674448081334,0,5.6505198945798051E-4,7.1180122263595031E-3,8.8657812282799827E-4,0,7.4555998560495571E-7,3.4842346826738976E-6,0.16331170849604651,0.892495244340064,0.22121747516153675,22.121747516153675,60,39.311419610679415,0.39311419610679416,724.0995420484935,null,0.29926803096723592,null,0.69624941495859172,0.14617162707695275,7.9362970175130909E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR26, IF(MODE_ILIM=4,#REF!,#REF!))","v":22.121747516153675},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ26, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.69624941495859172},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA26, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14617162707695275},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB26, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.9362970175130909E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S26, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":724.0995420484935},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P26, IF(MODE_ILIM=4,#REF!,#REF!))","v":11.203006472118179}]
["Rdcr",{"$f":"'Design Converter'!E18","v":170},"mW",{"$f":"B27/1000","v":0.17},"Inductor DCR at 25°C",null,null,21,6.3E-2,0.12661321568627451,0.12618062872971936,-1.8148542153526015E-4,0.71351463400499127,0.71351463400499127,1,0.71351463400499127,1.2442781086275772E-6,4.943214187399806E-2,763951.28350724268,1.3089839909805184E-6,0,6.6E-4,7.2699198995160863E-2,8.9847950087145975E-4,0,8.9860868190825974E-4,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,1.5860613198206922E-2,7.5467715306940691E-7,7.5467715306940691E-7,1.6163460272725704E-2,4.8332627877776689E-4,2.2918538505217281E-3,42.5,86.460881624257894,0.28278051467183724,0.28260085879499919,0.56767322731735814,0.56821073283514145,6.8429642812715866E-2,3.5119620116069073E-3,6.1880053964086671E-3,1.1836151885804955E-5,5.4751206568096685E-4,6.7473536139754384E-3,1.026642861660578E-2,4.4899065126050422E-2,0.15174529163737338,8.4798592469303956E-3,0.73870231233605099,0.73960496612894866,0.2079,0.21941837502908276,5.6728517210764601E-4,3.7140438609072372E-3,0.12171554754949783,0.59912427650548261,1.2491915408276751E-5,5.7784611717428657E-4,7.1211802103179397E-3,9.482583553542907E-4,0,7.964888629055489E-7,3.4727351876456475E-6,0.16015250269065284,0.89393770160095343,0.21941837502908276,21.941837502908275,63,41.239947953148963,0.41239947953148964,763.95128350724269,null,0.29825791831949011,null,0.73870231233605099,0.15174529163737338,8.9860868190825974E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR27, IF(MODE_ILIM=4,#REF!,#REF!))","v":21.941837502908275},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ27, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.73870231233605099},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA27, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15174529163737338},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB27, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.9860868190825974E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S27, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":763.95128350724269},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P27, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71351463400499127}]
["Kcore",0,null,{"$f":"B28","v":0},"Core loss constant - consult inductor vendor",null,null,22,6.6000000000000003E-2,0.12660133333333334,0.12918065226143791,2.8244558015373677E-3,0.71344767233227813,0.71344767233227813,1,0.71344767233227813,1.2431395653312389E-6,4.9475174966213918E-2,764616.34038694238,1.3078454476841801E-6,0,6.600000000000001E-4,7.53138336199798E-2,9.6426950087146E-4,0,9.6441829433502953E-4,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,1.6430739241505232E-2,8.0990757606701981E-7,8.0990757606701981E-7,1.6752067874146032E-2,5.1916878941099173E-4,2.2938490211608271E-3,42.5,84.447623540870822,0.28634130074756275,0.28284687663593772,0.57148202640466128,0.57205978648343991,7.0921572587802947E-2,3.7724020937452518E-3,6.1933923571342343E-3,2.3022088264823871E-4,5.740940798276725E-4,6.9977073196101462E-3,1.0778130708240932E-2,4.4899065126050429E-2,0.15183830649256819,8.4872413782950615E-3,0.74316346506254405,0.74413198369829148,0.21779999999999999,0.22641933493326138,6.006246684483324E-4,3.9300319073458621E-3,0.1199944327675211,0.59409816503606949,2.3933176830561354E-4,5.9681358927320604E-4,7.2746383717343646E-3,1.0024300233413403E-3,0,8.4195929628330784E-7,3.4206512436507538E-6,0.15784723771092743,0.88558796845350674,0.22641933493326138,22.641933493326139,66,43.139231734149426,0.43139231734149425,764.6163403869424,null,0.29404041182671831,null,0.74316346506254405,0.15183830649256819,9.6441829433502953E-4,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR28, IF(MODE_ILIM=4,#REF!,#REF!))","v":22.641933493326139},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ28, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.74316346506254405},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA28, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15183830649256819},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB28, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.6441829433502953E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S28, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":764.6163403869424},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P28, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71344767233227813}]
["Cin",{"$f":"'Design Converter'!E37","v":40},"µF",{"$f":"B29/1000000","v":4.0000000000000003E-5},"Input capacitance",null,null,23,6.9000000000000006E-2,0.12658945098039215,0.13218067579315648,5.8303970246099818E-3,0.71338071065956488,0.71338071065956488,1,0.71338071065956488,1.2420028905636249E-6,4.9518212239838287E-2,765281.46188840992,1.3067087729165661E-6,0,6.6E-4,7.79562283242205E-2,1.0331195008714599E-3,0,1.0332903028493694E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,1.7007543706647123E-2,8.6776962880053647E-7,8.6776962880053647E-7,1.7347356251071252E-2,5.5672192246792457E-4,2.2958443856652298E-3,42.5,82.525990154230541,0.28990787734678719,0.28309291838176059,0.575296640114213,0.57591661501659774,7.3441786101260287E-2,4.0452719593074516E-3,6.1987798412961211E-3,4.4898553181351727E-4,6.0074084227119658E-4,7.2485062153808347E-3,1.1302798387093704E-2,4.4899065126050422E-2,0.15193133038576345,8.4946242269613517E-3,0.74764536801641623,0.74868281652273072,0.22770000000000001,0.23320770925785647,6.349711321146671E-4,4.1523592008222143E-3,0.11832130546716237,0.58921217208949084,4.5984579430896264E-4,6.1527182996794477E-4,7.4238363198519943E-3,1.0581090566001458E-3,0,8.8875962800225528E-7,3.3700243190099138E-6,0.15560631323567176,0.87748844290993788,0.23320770925785647,23.320770925785649,69,44.999115697666738,0.44999115697666736,765.28146188840992,null,0.28994049627989332,null,0.74764536801641623,0.15193133038576345,1.0332903028493694E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR29, IF(MODE_ILIM=4,#REF!,#REF!))","v":23.320770925785649},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ29, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.74764536801641623},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA29, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15193133038576345},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB29, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0332903028493694E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S29, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":765.28146188840992},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P29, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71338071065956488}]
["RCinESR",{"$f":"'Design Converter'!E39","v":3},"mW",{"$f":"B30/1000","v":3.0000000000000001E-3},"Input capacitor ESR",null,null,24,7.1999999999999995E-2,0.12657756862745101,0.13518069932487503,8.8363382476825958E-3,0.71331374898685207,0.71331374898685207,1,0.71331374898685207,1.2408680797286836E-6,4.9561253695480603E-2,765946.64802106388,1.3055739620816248E-6,0,6.6E-4,8.0623653691320629E-2,1.1050295008714598E-3,0,1.1052249098523373E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,1.7590429152890497E-2,9.2826959334857967E-7,9.2826959334857967E-7,1.7948725570632769E-2,5.9598998677829027E-4,2.2978399440631916E-3,42.5,80.689865778643806,0.29348024531352546,0.28333898403595192,0.57911706929354057,0.57978122816246658,7.5987743900009591E-2,4.3306029172600832E-3,6.2041678489706178E-3,6.6813015475778619E-4,6.2745240992623599E-4,7.4997504136546395E-3,1.1840469133221872E-2,4.4899065126050422E-2,0.1520243633182764,8.5020077930338094E-3,0.75214806840699866,0.75325751202028068,0.23759999999999998,0.23979229820395895,6.7028695939524616E-4,4.3807698553113327E-3,0.11669418113357673,0.58446049231918962,6.742948876630316E-4,6.3324181561374027E-4,7.5689494429559672E-3,1.1152254360149033E-3,0,9.3683459234810745E-7,3.3207941570085702E-6,0.1534270684473196,0.86962876792578947,0.23979229820395895,23.979229820395894,72,46.810309970062292,0.46810309970062292,765.94664802106388,null,0.28595330872371949,null,0.75214806840699866,0.1520243633182764,1.1052249098523373E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR30, IF(MODE_ILIM=4,#REF!,#REF!))","v":23.979229820395894},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ30, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.75214806840699866},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA30, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1520243633182764},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB30, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1052249098523373E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S30, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":765.94664802106388},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P30, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71331374898685207}]
["Cout",{"$f":"'Design Converter'!E24","v":33},"µF",{"$f":"B31/1000000","v":3.3000000000000003E-5},"Output capacitance",null,null,25,7.4999999999999997E-2,0.12656568627450981,0.13818072285659361,1.184227947075521E-2,0.71324678731413871,0.71324678731413871,1,0.71324678731413871,1.2397351282454214E-6,4.960429933375049E-2,766611.89879432577,1.3044410105983626E-6,0,6.6E-4,8.331370556239831E-2,1.1799995008714599E-3,0,1.1802223267524975E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,1.8178868243169676E-2,9.9141375180756879E-7,9.9141375180756879E-7,1.8555647381181012E-2,6.3697729200925006E-4,2.2998356963829774E-3,42.5,78.933667155070609,0.29705840549195706,0.28358507360199697,0.58294331479033701,0.58365363567922601,7.8557208730578296E-2,4.6284262826547344E-3,6.2095563802340393E-3,8.8765480686795698E-4,6.542288397185502E-4,7.7514400268205467E-3,1.2391180646178463E-2,4.4899065126050422E-2,0.15211740529142481,8.5093920766170159E-3,0.75667161369344638,0.75785611786778706,0.24749999999999997,0.24618142328005244,7.0653659560503893E-4,4.6150220174699151E-3,0.11511118317699502,0.57983763606738115,8.8292575246922723E-4,6.5074338146573743E-4,7.7101435889804053E-3,1.1737129559365152E-3,0,9.8613191304809687E-7,3.2729037779404231E-6,0.15130698723358199,0.8619991498055759,0.24618142328005244,24.618142328005245,75,48.564555994658186,0.48564555994658187,766.61189879432573,null,0.28207425066795172,null,0.75667161369344638,0.15211740529142481,1.1802223267524975E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR31, IF(MODE_ILIM=4,#REF!,#REF!))","v":24.618142328005245},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ31, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.75667161369344638},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA31, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15211740529142481},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB31, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1802223267524975E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S31, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":766.61189879432573},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P31, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71324678731413871}]
["RCoutESR",{"$f":"'Design Converter'!E26","v":2.5000000000000001E-3},"mW",{"$f":"B32","v":2.5000000000000001E-3},"Output capacitor ESR",null,null,26,7.8E-2,0.12655380392156862,0.14118074638831218,1.4848220693827838E-2,0.71317982564142546,0.71317982564142546,1,0.71317982564142546,1.2386040315478459E-6,4.9647349155257668E-2,767277.21421761846,1.3033099139007871E-6,0,6.600000000000001E-4,8.6024261313527112E-2,1.2580295008714597E-3,0,1.258282773967474E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,1.8772394504443932E-2,1.0572083862914301E-6,1.0572083862914301E-6,1.9167655028164119E-2,6.796881486656048E-4,2.3018316426528553E-3,42.5,77.252286744538949,0.30064235872642514,0.2838311870833814,0.58677537745245933,0.58753384735548553,8.1148204963753204E-2,4.9387733766294746E-3,6.2149454351627109E-3,1.1075595435417035E-3,6.8107018858496208E-4,8.0035751672893774E-3,1.2954970846812394E-2,4.4899065126050429E-2,0.15221045630652655,8.5167770778155662E-3,0.76121605158664007,0.7624786820028302,0.25739999999999996,0.25238295940701477,7.436863976181125E-4,4.8548869261582205E-3,0.11357053569433298,0.57533840819199622,1.085971854384373E-3,6.6779529820888261E-4,7.8475757053495972E-3,1.2335089683421473E-3,0,1.0366021027278384E-6,3.2262992593229503E-6,0.1492436884822583,0.85459032042001093,0.25238295940701477,25.238295940701477,78,50.254747979561841,0.50254747979561842,767.27721421761851,null,0.27829897035007717,null,0.76121605158664007,0.15221045630652655,1.258282773967474E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR32, IF(MODE_ILIM=4,#REF!,#REF!))","v":25.238295940701477},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ32, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.76121605158664007},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA32, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15221045630652655},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB32, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.258282773967474E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S32, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":767.27721421761851},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P32, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71317982564142546}]
["Controller",null,"Units","Std Units","Description",null,null,27,8.1000000000000003E-2,0.12654192156862745,0.14418076992003076,1.7854161916900452E-2,0.71311286396871243,0.71311286396871243,1,0.71311286396871243,1.2374747850849029E-6,4.9690403160611914E-2,767942.59430036589,1.3021806674378441E-6,0,6.6E-4,8.8753442381340891E-2,1.3391195008714595E-3,0,1.3394064809255715E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,1.9370594371635488E-2,1.1256597789313094E-6,1.1256597789313094E-6,1.9784335437342735E-2,7.2412686808999676E-4,2.3038277829010977E-3,42.5,75.641043117902839,0.30423210586143679,0.2840773244835913,0.5906132581279292,0.59142187301038907,8.3758983807989879E-2,5.2616755264103332E-3,6.2203350138329647E-3,1.3278444201874668E-3,7.079765134733614E-4,8.2561559474937929E-3,1.353187787908287E-2,4.4899065126050422E-2,0.15230351636489961,8.5241627967340625E-3,0.76578143005110555,0.76712525262564635,0.26729999999999998,0.25840436447343246,7.8170450731687832E-4,5.1001480466547891E-3,0.11207055680565184,0.57095788857512486,1.2836542967382559E-3,6.8441534241002792E-4,7.981394428004801E-3,1.2945541473126435E-3,0,1.0881982782942369E-6,3.1809295335675546E-6,0.14723491714680476,0.8473935024238306,0.25840436447343246,25.840436447343247,81,51.875007795911799,0.51875007795911798,767.94259430036584,null,0.27462334640664227,null,0.76578143005110555,0.15230351636489961,1.3394064809255715E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR33, IF(MODE_ILIM=4,#REF!,#REF!))","v":25.840436447343247},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ33, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.76578143005110555},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA33, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15230351636489961},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB33, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.3394064809255715E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S33, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":767.94259430036584},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P33, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71311286396871243}]
["Deadtime1",7,"ns",{"$f":"B34/1000000000","v":6.9999999999999998E-9},"PMOS off to NMOS on deadtime",null,null,28,8.4000000000000005E-2,0.12653003921568629,0.14718079345174934,2.086010313997308E-2,0.7130459022959994,0.7130459022959994,1,0.7130459022959994,1.236347384320414E-6,4.9733461350423218E-2,768608.03905199515,1.3010532666733552E-6,0,6.600000000000001E-4,9.149958215499128E-2,1.42326950087146E-3,0,1.4235936860674621E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,1.9973100342504702E-2,1.1967742118752843E-6,1.1967742118752843E-6,2.0405322072904943E-2,7.7029776246311616E-4,2.3058241171559856E-3,42.5,74.095637427056744,0.30782764774166382,0.284323485806114,0.59445695766493378,0.59531772249372106,8.6387993496880353E-2,5.5971640653127812E-3,6.2257251163211616E-3,1.5485094922244604E-3,7.3494787134270861E-4,8.509182479888331E-3,1.4121940111887688E-2,4.4899065126050429E-2,0.1523965854678625,8.5315492334771467E-3,0.77036779730694838,0.7717958782010641,0.2772,0.26425270657438016,8.2056073496057115E-4,5.3506002727339063E-3,0.11060965251290489,0.56669141415920088,1.4761826279813591E-3,7.0062036144801615E-4,8.1117406242633035E-3,1.3567922719698788E-3,0,1.1408759907881117E-6,3.1367462015082487E-6,0.1452785360121808,0.84040037719983585,0.26425270657438016,26.425270657438016,84,53.420714247122767,0.53420714247122769,768.60803905199509,null,0.27104347282441554,null,0.77036779730694838,0.1523965854678625,1.4235936860674621E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR34, IF(MODE_ILIM=4,#REF!,#REF!))","v":26.425270657438016},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ34, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.77036779730694838},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA34, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1523965854678625},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB34, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.4235936860674621E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S34, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":768.60803905199509},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P34, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.7130459022959994}]
["Deadtime2",7,"ns",{"$f":"B35/1000000000","v":6.9999999999999998E-9},"NMOS off to PMOS on deadtime",null,null,29,8.6999999999999994E-2,0.12651815686274509,0.15018081698346791,2.3866044363045694E-2,0.71297894062328615,0.71297894062328615,1,0.71297894062328615,1.2352218247330175E-6,4.9776523725301634E-2,769273.54848193435,1.2999277070859587E-6,0,6.6E-4,9.426119845693666E-2,1.5104795008714599E-3,0,1.5108446368479334E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,2.0579585088853429E-2,1.2705579672880753E-6,1.2705579672880753E-6,2.1030288900663083E-2,8.1820514480390283E-4,2.3078206454458031E-3,42.5,72.61211510527761,0.3114289852119419,0.28456967105443715,0.59830647691182492,0.59922140568601001,8.9033853731736723E-2,5.9452703327432174E-3,6.2311157427036691E-3,1.7695548150826691E-3,7.6198431916303514E-4,8.7626548769493724E-3,1.4725196140905472E-2,4.4899065126050422E-2,0.15248966361673377,8.5389363881494713E-3,0.7749752018317988,0.7764906074604504,0.28709999999999997,0.26993468914276375,8.6022645157583159E-4,5.6060491904802922E-3,0.10918631103382613,0.56253456237302557,1.6637555866611674E-3,7.1642633342018256E-4,8.2387478936769495E-3,1.4201700262077832E-3,0,1.1945930684004475E-6,3.0937033603574314E-6,0.14337251809776264,0.83360305528306533,0.26993468914276375,26.993468914276374,87,54.888490199331855,0.54888490199331852,769.27354848193431,null,0.26755564505586221,null,0.7749752018317988,0.15248966361673377,1.5108446368479334E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR35, IF(MODE_ILIM=4,#REF!,#REF!))","v":26.993468914276374},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ35, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.7749752018317988},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA35, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15248966361673377},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB35, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.5108446368479334E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S35, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":769.27354848193431},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P35, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71297894062328615}]
["Sleep delay",5,"µs",{"$f":"B36/1000000","v":5.0000000000000004E-6},"Delay time to enter sleep mode",null,null,30,0.09,0.12650627450980392,0.15318084051518649,2.6871985586118308E-2,0.71291197895057312,0.71291197895057312,1,0.71291197895057312,1.2340981018161077E-6,4.9819590285857356E-2,769939.12259961362,1.2988039841690489E-6,0,6.6E-4,9.7036969936916309E-2,1.6007495008714598E-3,0,1.601159589737714E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,2.1189756388018854E-2,1.3470173273507574E-6,1.3470173273507574E-6,2.1658945208648007E-2,8.6785332896975056E-4,2.3098173677988409E-3,42.5,71.186832078206976,0.31503611911727097,0.28481588023204907,0.60216181671711888,0.60313293249863342,9.1695333754053407E-2,6.306025674200434E-3,6.2365068930568708E-3,1.9909804442028558E-3,7.8908591391544844E-4,9.0165732511751744E-3,1.5341684790452193E-2,4.4899065126050422E-2,0.1525827508128324,8.5463242608557113E-3,0.7796036923627736,0.78120948940367496,0.29699999999999999,0.27545667416103126,9.0067448956662115E-4,5.8663103983394235E-3,0.10779909756861905,0.55848313582377795,1.8465617894941797E-3,7.3184842247295376E-4,8.3625430306331003E-3,1.4846368137204822E-3,0,1.2493094714791947E-6,3.0517574448030842E-6,0.14151493964055289,0.82699404904409279,0.27545667416103126,27.545667416103125,90,56.276153038808332,0.5627615303880833,769.9391225996136,null,0.26415634719517461,null,0.7796036923627736,0.1525827508128324,1.601159589737714E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR36, IF(MODE_ILIM=4,#REF!,#REF!))","v":27.545667416103125},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ36, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.7796036923627736},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA36, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1525827508128324},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB36, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.601159589737714E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S36, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":769.9391225996136},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P36, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71291197895057312}]
["IQ(active)",660,"µA",{"$f":"B37/1000000","v":6.6E-4},"LM5164 quiescent current - active state ",null,null,31,9.2999999999999999E-2,0.12649439215686276,0.15618086404690504,2.9877926809190936E-2,0.71284501727785998,0.71284501727785998,1,0.71284501727785998,1.2329762110777749E-6,4.9862661032700657E-2,770604.76141446468,1.2976820934307161E-6,0,6.6E-4,9.9825715797774273E-2,1.69407950087146E-3,0,1.6945388102253534E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,2.180335275640324E-2,1.4261585742604703E-6,1.4261585742604703E-6,2.2291031157950229E-2,9.1924662965670978E-4,2.3118142842433942E-3,42.5,69.816424877637544,0.3186490503028151,0.28506211334243875,0.60602297792949722,0.60705231287392492,9.4371333509543479E-2,6.6794614412771132E-3,6.2418985674571655E-3,2.2127864350365584E-3,8.1625271259213293E-4,9.2709377150858568E-3,1.5971445115351941E-2,4.4899065126050422E-2,0.15267584705747747,8.5537128517005588E-3,0.78425331789845498,0.78595257330109092,0.30690000000000001,0.28082470362216572,9.4187905082061265E-4,6.1312088784550378E-3,0.10644664946136104,0.5545331481436081,2.0247803675408609E-3,7.4690102995918716E-4,8.4832464520643337E-3,1.5501445869814735E-3,0,1.3049871584715119E-6,3.0108670800910055E-6,0.13970397360762207,0.82056624743265127,0.28082470362216572,28.082470362216572,93,57.582635216683897,0.57582635216683897,770.60476141446463,null,0.26084224012153329,null,0.78425331789845498,0.15267584705747747,1.6945388102253534E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR37, IF(MODE_ILIM=4,#REF!,#REF!))","v":28.082470362216572},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ37, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.78425331789845498},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA37, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15267584705747747},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB37, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.6945388102253534E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S37, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":770.60476141446463},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P37, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71284501727785998}]
["IQ(sleep)",10,"µA",{"$f":"B38/1000000","v":1.0000000000000001E-5},"LM5164 quiescent current - sleep state","QRR",2.0000000000000001E-10,32,{"$f":"IF(PLOT_TYPE=1, H38/100*Iout, min_I*EXP(H38*rr/100))","v":9.6000000000000002E-2},{"$f":"IF(I38<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I38-Vout)/L*OnTime)","v":0.12648250980392156},{"$f":"IF(I38<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I38+((Vin-(Rdcr+RdsonTop)*J38-Vout)/L*OnTime)/2)","v":0.15918088757862359},{"$f":"IF(I38<Icrit, 0, I38-((Vin-(Rdcr+RdsonTop)*K38-Vout)/L*OnTime)/2)","v":3.288386803226355E-2},0.71277805560514673,{"$f":"IF(I38<Icrit, 1000*SQRT((J38*CoutEsr)^2+(((J38/2)-I38)*(OnTime+OffTime)/Cout)^2), 1000*J38*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":0.71277805560514673},1,{"$f":"IF(I38<Icrit, 1000*((N38/1000)*O38), 1000*J38*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":0.71277805560514673},{"$f":"IF(I38<Icrit, L*J38/(Vout+J38/2*(RdsonBot+Rdcr)), L*J38/(Vout+I38*(RdsonBot+Rdcr)))","v":1.2318561480407435E-6},4.9905735966442002E-2,{"$f":"IF(I38<Icrit,I38/((OnTime+Q38)*J38/2),1/(OnTime+Q38))","v":771270.46493592183},1.2965620303936847E-6,0,{"$f":"S38*(T38*Iq_active+U38*Iq_sleep)","v":6.6E-4},0.10262637835633683,{"$f":"W38^2*Rdcr","v":1.79046950087146E-3},{"$f":"Core_Loss/1000*S38/$S$106","v":0},{"$f":"(Y38+X38*(1+Ltc*(Ta-25)))/(1-X38*Ltc*ThetaCa)","v":1.790982572819176E-3},3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,2.2420139683107319E-2,1.5079879902301307E-6,1.5079879902301307E-6,2.2926313955091027E-2,9.7238936239969298E-4,2.3138113948077653E-3,42.5,{"$f":"IF(I38<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I38+Iripple/2)*1000000000)","v":68.497784142111158},{"$f":"IF(I38<Icrit, Vin*(I38+Iripple/2)*AK38/1000000000/2*S38, Vin*(I38-Iripple/2)*AJ38/1000000000/2*S38 + Vin*(I38+Iripple/2)*AK38/1000000000/2*S38)","v":0.32226777961390302},{"$f":"IF(I38<Icrit, Csw*(Vin)^2*S38/2, Csw*Vin^2*S38/2)","v":0.28530837038909618},0.60988996139780693,{"$f":"(AI38+AL38+AM38+AH38*(1+RdsonTopTc*(Ta-25)))/(1-AH38*RdsonTopTc*ThetaJA)","v":0.61097955678528004},{"$f":"IF(I38<Icrit,Iripple*SQRT((OffTime)*S38/3), SQRT(OffTime*S38*(I38^2+Iripple^2/12)))","v":9.7060867443484786E-2},7.0656089916612931E-3,{"$f":"QgBot*S38*Vdd","v":6.2472907659809679E-3},{"$f":"IF(I38<Icrit, Vin*Idss*R38, QrrBot*(I38-Iripple/2)/1*S38*Vin+Vin*Idss*R38)","v":2.4349728430460987E-3},{"$f":"IF(I38<Icrit, dead1*S38*(I38+Iripple/2)*((I38+Iripple/2)*BDserR+VSD), dead1*S38*(I38+Iripple/2)*((I38+Iripple/2)*BDserR+VSD)+dead2*S38*(I38-Iripple/2)*((I38-Iripple/2)*BDserR+VSD))","v":8.4348477219635431E-4},9.5257483812234214E-3,{"$f":"(AR38+AS38+AT38+AQ38*(1+RdsonBotTc*(Ta-25)))/(1-AQ38*RdsonBotTc*ThetaJA)","v":1.6614516402822244E-2},{"$f":"Vin*V38+Vout*Ifb/0.8","v":4.4899065126050422E-2},{"$f":"(Vin-Vdd)*(S38*QgBot+S38*QgTop)+AW38","v":0.15276895235198845},{"$f":"AI38+AR38","v":8.561102160788734E-3},0.78892412770087939,{"$f":"SUM(Z38,AC38,AF38,AZ38)","v":0.79071990869552511},{"$f":"Vout*I38","v":0.31679999999999997},0.28604451939210546,9.8381562165909126E-4,6.4005784148370003E-3,{"$f":"Vin*S38*(QgBot+QgTop)/($BB38+$BA38)","v":0.1051276717218232},0.55068081089048437,2.1985815549935292E-3,7.6159784178492977E-4,8.6009725932991807E-3,{"$f":"X38/($BB38+$BA38)","v":1.6166476889614893E-3},{"$f":"Y38/($BB38+$BA38)","v":0},1.3615899618511516E-6,2.9709929460505891E-6,0.13793788369179294,0.8143128926025438,{"$f":"BC38","v":0.28604451939210546},28.604451939210545,{"$f":"I38*1000","v":96},58.807882255999409,0.58807882255999411,{"$f":"S38/1000","v":771.27046493592184},null,{"$f":"AM38/($BB38+$BA38)","v":0.25761015052554875},null,0.78892412770087939,0.15276895235198845,1.790982572819176E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR38, IF(MODE_ILIM=4,#REF!,#REF!))","v":28.604451939210545},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ38, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.78892412770087939},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA38, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15276895235198845},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB38, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.790982572819176E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S38, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":771.27046493592184},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P38, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71277805560514673}]
["High-side N-ch MOSFET",null,"Units","Std Units","Description","QG_high",1.81E-9,33,9.9000000000000005E-2,0.12647062745098039,0.16218091111034216,3.5889809255336177E-2,{"$f":"IF(I39<Icrit, 1000*((((J39/2)-I39)*0.000002/Cout+Vout/306)), 1000*J39*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":0.71271109393243359},0.71271109393243359,1,0.71271109393243359,1.2307379082423162E-6,4.9948815087691896E-2,771936.23317342019,{"$f":"IF(1/S39-OnTime-Q39>Tsleep, OnTime+Q39+Tsleep, 1/S39)","v":1.2954437905952574E-6},{"$f":"IF(1/S39-OnTime-Q39>Tsleep, 1/S39-OnTime-Q39-Tsleep, 0)","v":0},6.6E-4,{"$f":"IF(I39<Icrit,Iripple*SQRT((OnTime+OffTime)*S39/3), SQRT(I39^2+Iripple^2/12))","v":0.10543800801673939},1.8899195008714601E-3,0,1.8904911610492989E-3,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q39)*S39)","v":3.6279106032784197E-2},3.2904338363449972E-6,3.2904338363449972E-6,{"$f":"SQRT($R39)*SQRT($I39^2*(1-R39)+(Iripple^2)/12)","v":2.3039906376315433E-2},1.5925118574881416E-6,1.5925118574881416E-6,{"$f":"IF(I39<Icrit,Iripple*SQRT((OnTime)*S39/3), SQRT(OnTime*S39*(I39^2+Iripple^2/12)))","v":2.3564584553401758E-2},{"$f":"RdsonTop*AG39^2","v":1.0272858435726785E-3},{"$f":"QgTop*S39*Vdd","v":2.3158086995202607E-3},42.5,67.228031064855742,0.32589230789602741,0.28555465137551156,0.61376276797105922,0.61491467423726132,9.9763050535675871E-2,{"$f":"RdsonBot*AP39^2","v":7.4644996891378634E-3},6.2526834887047036E-3,2.6575397237045789E-3,8.7078214974246014E-4,9.7810053621517432E-3,1.7270938174373991E-2,4.4899065126050422E-2,0.15286206669768498,8.5684921882249639E-3,0.79361617129754525,0.79551154540428837,0.32669999999999999,0.29112158161080304,1.026460894043921E-3,6.6742610543397331E-3,0.10384093287676686,0.54692252141279185,2.3681272346446698E-3,7.7595187227266652E-4,8.7158302747883717E-3,1.6841027064915793E-3,0,1.419083473173877E-6,2.9320976511247564E-6,0.13621501874908515,0.80822755825634907,0.29112158161080304,29.112158161080302,99,59.95273560232264,0.59952735602322638,771.93623317342019,null,0.25445706074306829,null,0.79361617129754525,0.15286206669768498,1.8904911610492989E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR39, IF(MODE_ILIM=4,#REF!,#REF!))","v":29.112158161080302},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ39, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.79361617129754525},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA39, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15286206669768498},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB39, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.8904911610492989E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S39, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":771.93623317342019},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P39, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71271109393243359}]
["RdsonTop",1850,"mW",{"$f":"B40/1000","v":1.85},"Drain-source resistance of high-side MOSFET @ VDD, 25°C","QG_low",1.92E-9,34,0.10200000000000001,0.1264587450980392,0.16518093464206074,3.8895750478408792E-2,0.71264413225972045,0.71264413225972045,1,0.71264413225972045,1.2296214872343109E-6,4.9991898397061044E-2,772602.06613639789,1.2943273695872521E-6,0,6.6E-4,0.1082597502977815,1.9924295008714602E-3,0,1.993064867469716E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,2.3662462947871013E-2,1.6797364582781056E-6,1.6797364582781056E-6,2.4205654804911755E-2,1.0839403903889131E-3,2.317806198409194E-3,42.5,66.00449641357487,0.32952263599484605,0.28580095630517627,0.61764139849843147,0.61885767526570701,0.10247708624266558,7.8761649035900393E-3,6.2580767357048239E-3,2.8804871324958907E-3,8.9814490225588548E-4,1.00367087704566E-2,1.7940750187726204E-2,4.4899065126050422E-2,0.15295519009588704,8.5758829341140187E-3,0.79832949848343437,0.80032753352119868,0.33660000000000001,0.29606108575584417,1.0697926925110032E-3,6.9521066068211537E-3,0.10258526112278021,0.54325485159597031,2.5335714437090657E-3,7.8997550483646457E-4,8.8279230421764235E-3,1.7524683342839545E-3,0,1.4774349364869047E-6,2.894145615555756E-6,0.13453380764046302,0.8023041295641038,0.29606108575584417,29.606108575584418,102.00000000000001,61.018807215515402,0.61018807215515403,772.60206613639787,null,0.25138009932789379,null,0.79832949848343437,0.15295519009588704,1.993064867469716E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR40, IF(MODE_ILIM=4,#REF!,#REF!))","v":29.606108575584418},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ40, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.79832949848343437},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA40, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15295519009588704},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB40, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.993064867469716E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S40, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":772.60206613639787},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P40, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71264413225972045}]
["RdsonTopTc",4800,"ppm/°C",{"$f":"B41/1000000","v":4.7999999999999996E-3},"Drain to Source Resistance Temp Co","Qoss_hs",1.4499999999999999E-10,35,0.105,0.12644686274509803,0.16818095817377932,4.1901691701481406E-2,0.71257717058700731,0.71257717058700731,1,0.71257717058700731,1.2285068805830053E-6,5.0034985895160158E-2,773267.9638342933,1.2932127629359465E-6,0,6.6E-4,0.11109083461086247,2.0979995008714599E-3,0,2.0987039936604481E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,2.4287637972560786E-2,1.7696680748585297E-6,1.7696680748585297E-6,2.4849354996263638E-2,1.1423573209011152E-3,2.3198038915028798E-3,{"$f":"15*VIN_nom/24","v":42.5},64.824701800296737,0.33315876475618,0.28604728518158173,0.62152585382926462,0.6228085699378354,0.10520225606580136,8.3006360110008288E-3,6.2634705070577761E-3,3.1038151249147099E-3,9.2557308677315123E-4,1.0292858718745638E-2,1.862399243873571E-2,4.4899065126050422E-2,0.15304832254791467,8.5832743985606551E-3,0.80306415932304642,0.80516792341861809,0.34649999999999997,0.30086797848067809,1.1137899063500512E-3,7.2339721811994937E-3,0.10135954075539012,0.53967453741728222,2.6950608433213338E-3,8.0368052973610175E-4,8.93734948195158E-3,1.8217052487176559E-3,0,1.5366131493924363E-6,2.8571029629597164E-6,0.13289275444401119,0.79653678452407206,0.30086797848067809,30.08679784806781,105,62.00835196729512,0.62008351967295117,773.26796383429325,null,0.24837653230149648,null,0.80306415932304642,0.15304832254791467,2.0987039936604481E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR41, IF(MODE_ILIM=4,#REF!,#REF!))","v":30.08679784806781},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ41, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.80306415932304642},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA41, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15304832254791467},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB41, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.0987039936604481E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S41, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":773.26796383429325},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P41, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71257717058700731}]
["QgTop",0.6,"nC",{"$f":"B42/1000000000","v":6E-10},"Gate charge of high-side MOSFET @ VDD",null,null,36,0.108,0.12643498039215686,0.17118098170549789,4.490763292455402E-2,0.71251020891429417,0.71251020891429417,1,0.71251020891429417,1.2273940838690746E-6,5.0078077582600175E-2,773933.92627654818,1.2920999662220158E-6,0,6.6E-4,0.11393056453181472,2.2066295008714596E-3,0,2.2074088502297639E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,2.4915276368141059E-2,1.862312989502545E-6,1.862312989502545E-6,2.5495531712404183E-2,1.2025409540016836E-3,2.3218017788296445E-3,42.5,63.686342924696127,0.33680069502601589,0.28629363800822066,0.62541613481306624,0.62676736835235591,0.10793791050694874,8.7379443934545581E-3,6.2688648028400408E-3,3.3275237564665094E-3,9.530667603418725E-4,1.0549455319648422E-2,1.9320705163342083E-2,4.4899065126050422E-2,0.15314146405508844,8.5906665816696849E-3,0.80782020415245614,0.81003276574951177,0.35639999999999999,0.30554697232890998,1.1584324265971875E-3,7.5197217544360926E-3,0.10016270885157671,0.53617846924181201,2.8527351547162267E-3,8.1707817915202584E-4,9.0442035146960954E-3,1.891775990580607E-3,0,1.5965883711316043E-6,2.8209374195954378E-6,0.13129043400687113,0.79091997664622882,0.30554697232890998,30.554697232890998,108,62.924142868481049,0.62924142868481048,773.93392627654816,null,0.24544375502368343,null,0.80782020415245614,0.15314146405508844,2.2074088502297639E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR42, IF(MODE_ILIM=4,#REF!,#REF!))","v":30.554697232890998},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ42, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.80782020415245614},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA42, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15314146405508844},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB42, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.2074088502297639E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S42, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":773.93392627654816},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P42, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71251020891429417}]
["Coss",145,"pF",{"$f":"B43/1000000000000","v":1.4499999999999999E-10},"Capacitance (Coss)",null,null,37,0.111,0.12642309803921567,0.17418100523721647,4.7913574147626647E-2,0.71244324724158103,0.71244324724158103,1,0.71244324724158103,1.2262830926875353E-6,5.0121173459992133E-2,774599.95347260567,1.2909889750404765E-6,0,6.5999999999999989E-4,0.11677830934954488,2.3183195008714603E-3,0,2.3191797568164608E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,2.5545237550259784E-2,1.9576774844976077E-6,1.9576774844976077E-6,2.6144045980463566E-2,1.2644956094228974E-3,2.3237998604178169E-3,42.5,62.5872745524888,0.34044842765050448,0.28654001478858626,0.62931224229950855,0.63073408063957404,0.11068346121041638,9.1881214391383095E-3,6.2742596231281063E-3,3.5516130826675537E-3,9.8062598002075676E-4,1.0806498685816417E-2,2.0030928839527718E-2,4.4899065126050408E-2,0.15323461461872903,8.5980594835459237E-3,0.81259768358137674,0.8149221114495141,0.36629999999999996,0.31010255941662146,1.2037010874446827E-3,7.8092257707500232E-3,9.8993752184956749E-2,0.53276368279904629,3.0067275648178139E-3,8.3017915980035319E-4,9.1485746677696621E-3,1.9626448560352287E-3,0,1.6573322371143911E-6,2.7856182206978875E-6,0.12972548780913873,0.78544841885021721,0.31010255941662146,31.010255941662145,111,63.769353027551922,0.63769353027551923,774.59995347260565,null,0.2425792846334075,null,0.81259768358137674,0.15323461461872903,2.3191797568164608E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR43, IF(MODE_ILIM=4,#REF!,#REF!))","v":31.010255941662145},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ43, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.81259768358137674},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA43, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15323461461872903},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB43, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.3191797568164608E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S43, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":774.59995347260565},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P43, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71244324724158103}]
["Low-side N-ch MOSFET",null,"Units","Std Units","Description",null,null,38,0.11399999999999999,0.12641121568627453,0.17718102876893502,5.0919515370699261E-2,0.71237628556886812,0.71237628556886812,1,0.71237628556886812,1.2251739026476881E-6,5.0164273527947112E-2,775266.04543190985,1.2898797850006293E-6,0,6.6E-4,0.11963349670781172,2.4330695008714597E-3,0,2.4340170420922144E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,2.6177393823330411E-2,2.0557678421452114E-6,2.0557678421452114E-6,2.6794771653552298E-2,1.3282256077371179E-3,2.3257981362957295E-3,42.5,61.525497022852505,0.34410196347596067,0.28678641552617207,0.63321417713842854,0.63470871696150011,0.11343837412059714,9.6511985423434216E-3,6.2796549679984713E-3,3.7760831590448987E-3,1.008250802879607E-3,1.1063988929922977E-2,2.0754704189293469E-2,4.4899065126050422E-2,0.15332777424015737,8.6054531042942008E-3,0.81739664849524518,0.81983601173901588,0.37619999999999992,0.31453902416618007,1.2495776117129927E-3,8.1023607686196309E-3,9.7851704354817423E-2,0.52942735078498682,3.1571651037116673E-3,8.4299368328686665E-4,9.2505483290892948E-3,2.0342777951424876E-3,0,1.7188176793741855E-6,2.7511160233049861E-6,0.12819662011449087,0.78011706847956086,0.31453902416618007,31.453902416618007,113.99999999999999,64.547447140017496,0.645474471400175,775.2660454319099,null,0.23978075301360663,null,0.81739664849524518,0.15332777424015737,2.4340170420922144E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR44, IF(MODE_ILIM=4,#REF!,#REF!))","v":31.453902416618007},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ44, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.81739664849524518},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA44, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15332777424015737},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB44, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.4340170420922144E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S44, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":775.2660454319099},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P44, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71237628556886812}]
["RdsonBot",750,"mW",{"$f":"B45/1000","v":0.75},"Drain-source resistance of low-side MOSFET @ VDD, 25°C",null,null,39,0.11699999999999999,0.12639933333333334,0.18018105230065359,5.3925456593771876E-2,0.71230932389615487,0.71230932389615487,1,0.71230932389615487,1.2240665093730562E-6,5.0207377787076415E-2,775932.20216390816,1.2887723917259974E-6,0,6.600000000000001E-4,0.12249560618462198,2.5508795008714596E-3,0,2.5519210437640002E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,2.6811628974262907E-2,2.1565903447606029E-6,2.1565903447606029E-6,2.7447594000370779E-2,1.3937352703570014E-3,2.3277966064917245E-3,42.5,60.499144106327066,0.34776130334886485,0.2870328402244729,0.63712194017982948,0.63869128751195958,0.11620216351093753,1.0127207103466995E-2,6.285050837527657E-3,4.0009340411364114E-3,1.0359412859993282E-3,1.1321926164663397E-2,2.149207218064994E-2,4.4899065126050429E-2,0.15342094292069464,8.6128474440193819E-3,0.82221715005732354,0.8247745181252687,0.38609999999999994,0.31886045516737577,1.2960445600588204E-3,8.3990090333492425E-3,9.6735643111903052E-2,0.52616677503978759,3.3041689962481336E-3,8.5553149438078846E-4,9.350205983517202E-3,2.1066423173400723E-3,0,1.7810188524732809E-6,2.7174028250585346E-6,0.12670259438461712,0.7749211133428795,0.31886045516737577,31.886045516737578,117,65.262084299350803,0.65262084299350809,775.93220216390819,null,0.23704590023817684,null,0.82221715005732354,0.15342094292069464,2.5519210437640002E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR45, IF(MODE_ILIM=4,#REF!,#REF!))","v":31.886045516737578},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ45, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.82221715005732354},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA45, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15342094292069464},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB45, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.5519210437640002E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S45, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":775.93220216390819},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P45, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71230932389615487}]
["RdsonBotTc",4800,"ppm/°C",{"$f":"B46/1000000","v":4.7999999999999996E-3},"Drain To Source Resitance Temp Co",null,null,40,0.12,0.12638745098039214,0.18318107583237214,5.6931397816844503E-2,0.71224236222344162,0.71224236222344162,1,0.71224236222344162,1.2229609085013317E-6,5.0250486237991387E-2,776598.42367804865,1.287666790854273E-6,0,6.6E-4,0.12536416367741618,2.6717495008714591E-3,0,2.6728921085765749E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,2.7447837040906531E-2,2.2601512746724819E-6,2.2601512746724819E-6,2.8102408471716196E-2,1.4610289195356946E-3,2.329795271034146E-3,42.5,59.506472058082288,0.35142644811586116,0.28727928888698373,0.64103553227387899,0.64268180251669915,0.11897438676181993,1.0616178529013335E-2,6.2904472317921942E-3,4.2261657844907471E-3,1.0636974864719245E-3,1.1580310502754865E-2,2.2243074029624495E-2,4.4899065126050422E-2,0.15351412066166231,8.6202425028263398E-3,0.8270592397108123,0.82973768240449985,0.39599999999999996,0.32307075623487103,1.3430852836234174E-3,8.6990582731802327E-3,9.564468786540084E-2,0.52297937925541715,3.4478549898216233E-3,8.6780189737276818E-4,9.4476254332313998E-3,2.1797074033249536E-3,0,1.8439110644284004E-6,2.6844518885070359E-6,0.12524222993660225,0.7698559587009276,0.32307075623487103,32.307075623487101,120,65.91703305041338,0.65917033050413376,776.59842367804868,null,0.2343725684629642,null,0.8270592397108123,0.15351412066166231,2.6728921085765749E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR46, IF(MODE_ILIM=4,#REF!,#REF!))","v":32.307075623487101},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ46, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.8270592397108123},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA46, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15351412066166231},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB46, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.6728921085765749E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S46, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":776.59842367804868},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P46, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71224236222344162}]
["QgBot",1.62,"nC",{"$f":"B47/1000000000","v":1.6200000000000002E-9},"Gate charge of low-side MOSFET at VDD",null,null,41,0.12299999999999998,0.12637556862745097,0.18618109936409072,5.9937339039917104E-2,0.71217540055072848,0.71217540055072848,1,0.71217540055072848,1.2218570956843167E-6,5.0293598881303539E-2,777264.70998378191,1.2865629780372579E-6,0,6.6E-4,0.12823873648214876,2.7956795008714586E-3,0,2.796930592315026E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,2.8085921231242764E-2,2.3664569142227192E-6,2.3664569142227192E-6,2.8759119619339579E-2,1.5301108783670433E-3,2.3317941299513456E-3,42.5,58.545849731474931,0.355097398623759,0.28752576151720061,0.64495495427091099,0.64668027223349933,0.12175463978343476,1.1118144231595465E-2,6.2958441508686337E-3,4.451778444667375E-3,1.0915194614005068E-3,1.1839142056936515E-2,2.3007751202284342E-2,4.4899065126050422E-2,0.15360730746438217,8.6276382808199784E-3,0.83192296918098585,0.83472555666405146,0.40589999999999993,0.32717365672478521,1.3906838798546084E-3,9.0024013171060048E-3,9.4577997356961638E-2,0.51986270217191577,3.5883336601882291E-3,8.798137806668439E-4,9.5428810033311544E-3,2.2534434228397085E-3,0,1.9074707122638546E-6,2.6522376704803065E-6,0.12381439882426785,0.76491721512551447,0.32717365672478521,32.717365672478522,122.99999999999999,66.516098897051677,0.66516098897051679,777.26470998378193,null,0.23175869622606818,null,0.83192296918098585,0.15360730746438217,2.796930592315026E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR47, IF(MODE_ILIM=4,#REF!,#REF!))","v":32.717365672478522},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ47, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.83192296918098585},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA47, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15360730746438217},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB47, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.796930592315026E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S47, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":777.26470998378193},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P47, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71217540055072848}]
["VSD",0.8,"V",{"$f":"B48","v":0.8},"Body diode forward voltage",null,null,42,0.126,0.12636368627450981,0.18918112289580929,6.2943280262989745E-2,0.71210843887801545,0.71210843887801545,1,0.71210843887801545,1.2207550665878664E-6,5.0336715717624443E-2,777931.06109055958,1.2854609489408076E-6,0,6.6E-4,0.13111892897113672,2.9226695008714595E-3,0,2.9240368598073929E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,2.8725792972901901E-2,2.475513545766061E-6,2.475513545766061E-6,2.9417640146281378E-2,1.6009854707857961E-3,2.3337931832716789E-3,42.5,57.615749633982986,0.35877415571953197,0.28777225811861978,0.64888020702142346,0.65068670695228037,0.12454255299528007,1.1633135629936607E-2,6.3012415948335331E-3,4.6777720772365689E-3,1.1194072678992911E-3,1.2098420939969393E-2,2.3786145416775716E-2,4.4899065126050422E-2,0.1537005033301761,8.635034778105212E-3,0.83680839047733735,0.83973819328452681,0.4158,0.33117272116768848,1.4388251512533032E-3,9.3089358327131996E-3,9.3534767488843512E-2,0.51681439122447781,3.7257106970193968E-3,8.9157563974289541E-4,9.6360437338186798E-3,2.3278220579062317E-3,0,1.9716752218345827E-6,2.6207357561438417E-6,0.12241802292616109,0.76010068716291423,0.33117272116768848,33.117272116768845,126,67.063063929713536,0.6706306392971354,777.93106109055964,null,0.22920231312581471,null,0.83680839047733735,0.1537005033301761,2.9240368598073929E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR48, IF(MODE_ILIM=4,#REF!,#REF!))","v":33.117272116768845},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ48, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.83680839047733735},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA48, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1537005033301761},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB48, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.9240368598073929E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S48, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":777.93106109055964},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P48, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71210843887801545}]
["BDserR",100,"mW",{"$f":"B49*0.001","v":0.1},"Series resistance of body diode",null,null,43,0.129,0.12635180392156861,0.19218114642752787,6.5949221486062359E-2,0.7120414772053022,0.7120414772053022,1,0.7120414772053022,1.2196548168918312E-6,5.0379836747565868E-2,778597.4770078361,1.2843606992447724E-6,0,6.6E-4,0.13400437878867241,3.0527195008714599E-3,0,3.0542112849273446E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,2.9367371075565252E-2,2.5873274516698399E-6,2.5873274516698399E-6,3.0077890070909805E-2,1.6736570215678092E-3,2.3357924310235083E-3,42.5,56.714739822357579,0.362456720250319,0.28801877869473869,0.65281129137608118,0.65470111699521605,0.12733778778703342,1.2161184148871669E-2,6.3066395637634727E-3,4.9041467377794103E-3,1.1473609630936062E-3,1.235814726463649E-2,2.4578298645379412E-2,4.4899065126050422E-2,0.15379370826036637,8.642431994786981E-3,0.84171555589574887,0.84477564494196422,0.42569999999999997,0.33507135827026902,1.4874945668251628E-3,9.6185640625178169E-3,9.2514229294393194E-2,0.51383219660688728,3.8600871707410293E-3,9.0309559861418537E-4,9.7271815589987289E-3,2.4028162310902935E-3,0,2.0365029915925938E-6,2.5899227973750772E-6,0.12105207122438914,0.75540236274024586,0.33507135827026902,33.5071358270269,129,67.561637846160409,0.67561637846160405,778.59747700783612,null,0.22670153484752203,null,0.84171555589574887,0.15379370826036637,3.0542112849273446E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR49, IF(MODE_ILIM=4,#REF!,#REF!))","v":33.5071358270269},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ49, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.84171555589574887},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA49, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15379370826036637},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB49, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.0542112849273446E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S49, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":778.59747700783612},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P49, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.7120414772053022}]
["QrrBot",1.4,"nC",{"$f":"B50*0.000000001","v":1.3999999999999999E-9},"Reverse recovery charge of body diode at 100mA",null,null,44,0.13200000000000001,0.12633992156862747,0.19518116995924645,6.8955162709134987E-2,0.71197451553258928,0.71197451553258928,1,0.71197451553258928,1.2185563422900028E-6,5.0422961971739642E-2,779263.95774506719,1.283262224642944E-6,0,6.6E-4,0.13689475349529653,3.1858295008714609E-3,0,3.1874542505969375E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,3.0010580991341941E-2,2.7019049143136827E-6,2.7019049143136827E-6,3.0739795989495625E-2,1.748129856330251E-3,2.3377918732352017E-3,42.5,55.841476546539589,0.36614509306342358,0.28826532324905524,0.656748208185714,0.65872351271684182,0.13014003339658767,1.2702321219348715E-2,6.3120380577350458E-3,5.1309024818877941E-3,1.1753806041198919E-3,1.2618321143742731E-2,2.5384253116582822E-2,4.4899065126050422E-2,0.15388692225627554,8.6498299309702466E-3,0.84664451802067053,0.84983796461001815,0.43559999999999999,0.33887282933342822,1.5366782260294422E-3,9.9311925773976004E-3,9.1515647040100304E-2,0.51091396571981695,3.991559782073521E-3,9.1438142989380602E-4,9.8163594752477493E-3,2.4784000384164727E-3,0,2.1019333399985575E-6,2.559776455134701E-6,0.11971555725986548,0.75081840325863647,0.33887282933342822,33.887282933342824,132,68.015419380100283,0.68015419380100284,779.26395774506716,null,0.2242545585126782,null,0.84664451802067053,0.15388692225627554,3.1874542505969375E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR50, IF(MODE_ILIM=4,#REF!,#REF!))","v":33.887282933342824},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ50, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.84664451802067053},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA50, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15388692225627554},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB50, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.1874542505969375E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S50, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":779.26395774506716},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P50, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71197451553258928}]
["TrrBot",20,"ns",{"$f":"B51*0.000000001","v":2E-8},"Reverse recovery time of body diode (not used)",null,null,45,0.13500000000000001,0.12632803921568628,0.19818119349096502,7.1961103932207601E-2,0.71190755385987603,0.71190755385987603,1,0.71190755385987603,1.2174596384900553E-6,5.0466091390757757E-2,779930.50331171078,1.2821655208429965E-6,0,6.6E-4,0.13978974760166785,3.3219995008714606E-3,0,3.3237661487894275E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,3.0655354160348685E-2,2.8192522160892224E-6,2.8192522160892224E-6,3.1403290424359222E-2,1.8244083015318056E-3,2.3397915099351322E-3,42.5,54.994697562861127,0.36983927500631392,0.28851189178506803,0.66069095830131708,0.66275390450416627,0.13294900415036576,1.3256578278430478E-2,6.3174370768248576E-3,5.3580393651644328E-3,1.2034662481257038E-3,1.2878942690114994E-2,2.6204051317168686E-2,4.4899065126050422E-2,0.1539801453192263,8.6572285867599907E-3,0.85159532972732133,0.85492520556216323,0.44550000000000001,0.34258025613046617,1.5863628250402889E-3,1.0246732045841388E-2,9.0538316449379E-2,0.50805763797519266,4.1202210955671196E-3,9.2544057357412963E-4,9.9036396980228727E-3,2.5545486865854675E-3,0,2.1679464563057916E-6,2.5302753455340551E-6,0.11840753675076755,0.74634513432177241,0.34258025613046617,34.25802561304662,135,68.427867006324419,0.68427867006324417,779.93050331171082,null,0.22185965832640617,null,0.85159532972732133,0.1539801453192263,3.3237661487894275E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR51, IF(MODE_ILIM=4,#REF!,#REF!))","v":34.25802561304662},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ51, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.85159532972732133},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA51, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1539801453192263},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB51, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.3237661487894275E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S51, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":779.93050331171082},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P51, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71190755385987603}]
["Idss",0,"μA",{"$f":"B52/1000000","v":0},"Leakage current of low-side device",null,null,46,0.13800000000000001,0.12631615686274508,0.2011812170226836,7.4967045155280229E-2,0.71184059218716289,0.71184059218716289,1,0.71184059218716289,1.216364701213492E-6,5.0509225005232271E-2,780597.11371722596,1.2810705835664332E-6,0,6.6E-4,0.14268907994145172,3.4612295008714603E-3,0,3.4631473805321585E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,3.1301627430533593E-2,2.9393756393997991E-6,2.9393756393997991E-6,3.2068311246486854E-2,1.9024966844728773E-3,2.3417913411516778E-3,42.5,54.173216046550209,0.37353926692662304,0.28875848430627621,0.664639542574051,0.6667923027767817,0.13576443701890822,1.3823986769295821E-2,6.3228366211095302E-3,5.5855574432228531E-3,1.2316179522697153E-3,1.3140012016602098E-2,2.7037735994320692E-2,4.4899065126050422E-2,0.15407337745054167,8.6646279622612076E-3,0.85656804418390531,0.86003742137391326,0.45540000000000003,0.34619662828533182,1.6365356251475944E-3,1.0565097017844503E-2,8.9581563039065087E-2,0.50526123993026284,4.2461597583175019E-3,9.3628015461453694E-4,9.9890818089073113E-3,2.6312384341752775E-3,0,2.2345233544669559E-6,2.5013989893250048E-6,0.11712710536212295,0.74197903705280144,0.34619662828533182,34.61966282853318,138,68.802277733330541,0.68802277733330541,780.59711371722597,null,0.21951518150113244,null,0.85656804418390531,0.15407337745054167,3.4631473805321585E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR52, IF(MODE_ILIM=4,#REF!,#REF!))","v":34.61966282853318},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ52, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.85656804418390531},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA52, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15407337745054167},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB52, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.4631473805321585E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S52, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":780.59711371722597},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P52, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71184059218716289}]
["Csw",160,"pF",{"$f":"B53/1000000000000","v":1.5999999999999999E-10},"Effective SW node capacitance (CossHS + CossLS)",null,null,47,0.14099999999999999,0.12630427450980394,0.20418124055440212,7.7972986378352829E-2,0.71177363051444986,0.71177363051444986,1,0.71177363051444986,1.2152715261955876E-6,5.0552362815775381E-2,781263.78897107404,1.2799774085485288E-6,0,6.6E-4,0.14559249133982835,3.6035195008714592E-3,0,3.6055983559095122E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,3.1949342542323546E-2,3.062281466660176E-6,3.062281466660176E-6,3.2734801163088141E-2,1.9823993332957961E-3,2.343791366913222E-3,42.5,53.375915041796127,0.37724506967214916,0.28900510081617969,0.66859396185524211,0.67083871798697692,0.13858608944739606,1.4404578141241246E-2,6.328236690665701E-3,5.813456771687397E-3,1.2598357737217212E-3,1.340152923607482E-2,2.7885350157746156E-2,4.4899065126050422E-2,0.15416661865154485,8.6720280575789226E-3,0.86156271485384694,0.86517466592505943,0.46529999999999994,0.34972481018756096,1.6871844231427424E-3,1.0886205722377248E-2,8.8644740560371138E-2,0.50252288072721674,4.3694607049472728E-3,9.469069994247325E-4,1.0072742893422127E-2,2.708446536534377E-3,0,2.3016458299347003E-6,2.4731277645615354E-6,0.1158733966154516,0.73771673995648235,0.34972481018756096,34.972481018756099,141,69.1417728033842,0.69141772803384205,781.26378897107406,null,0.21721954443622477,null,0.86156271485384694,0.15416661865154485,3.6055983559095122E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR53, IF(MODE_ILIM=4,#REF!,#REF!))","v":34.972481018756099},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ53, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.86156271485384694},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA53, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15416661865154485},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB53, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.6055983559095122E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S53, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":781.26378897107406},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P53, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71177363051444986}]
["ThetaJA",41.1,"°C/W",null,"Thermal resistance",null,null,48,0.14399999999999999,0.12629239215686275,0.2071812640861207,8.0978927601425443E-2,0.71170666884173661,0.71170666884173661,1,0.71170666884173661,1.2141801091853328E-6,5.0595504822999453E-2,781930.52908271877,1.278885991538274E-6,0,6.6E-4,0.14849974254030879,3.7488695008714595E-3,0,3.7511194940659277E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,3.259844566998172E-2,3.1879759802962497E-6,3.1879759802962497E-6,3.3402707261902261E-2,2.0641205769850253E-3,2.3457915872481562E-3,42.5,52.601742394797455,0.38095668409085531,0.2892517413182793,0.67255421699638274,0.67489316061984861,0.14141373742642485,1.4998383849682374E-2,6.3336372855700221E-3,6.0417374061932476E-3,1.2881197696626408E-3,1.366349446142591E-2,2.8746937081815985E-2,4.4899065126050422E-2,0.15425986892355947,8.6794288728181783E-3,0.86657939549804219,0.87033699340192472,0.47519999999999996,0.35316754747749485,1.7382975235428607E-3,1.1209979877442513E-2,8.7727229536726292E-2,0.49984074781620247,4.4902053498491381E-3,9.573276513237173E-4,1.0154677670273829E-2,2.786151194099229E-3,0,2.3692964191464416E-6,2.4454428622031301E-6,0.11464557992831088,0.73355501128705225,0.35316754747749485,35.316754747749485,144,69.449289175978407,0.69449289175978413,781.93052908271875,null,0.21497122913504099,null,0.86657939549804219,0.15425986892355947,3.7511194940659277E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR54, IF(MODE_ILIM=4,#REF!,#REF!))","v":35.316754747749485},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ54, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.86657939549804219},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA54, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15425986892355947},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB54, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7511194940659277E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S54, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":781.93052908271875},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P54, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71170666884173661}]
["Inductor",null,"Units","Std Units","Description",null,null,49,0.14699999999999999,0.12628050980392155,0.21018128761783927,8.3984868824498071E-2,0.71163970716902336,0.71163970716902336,1,0.71163970716902336,1.2130904459453814E-6,5.0638651027516905E-2,782597.33406162483,1.2777963282983226E-6,0,6.6E-4,0.15141061235771419,3.8972795008714593E-3,0,3.8997112232089844E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,3.3248887012674325E-2,3.3164654627447501E-6,3.3164654627447501E-6,3.4071980605194285E-2,2.1476647453673608E-3,2.3477920021848743E-3,42.5,51.849706121457338,0.38467411103086968,0.28949840581607622,0.67652030884913072,0.67895564119341356,0.1442471737731473,1.5605435356155415E-2,6.3390384058991615E-3,6.2703994023863945E-3,1.3164699972845178E-3,1.3925907805570074E-2,2.9622540307721972E-2,4.4899065126050422E-2,0.15435312826790928,8.6868304080840349E-3,0.8716181401771288,0.87552445829963688,0.48509999999999992,0.35652747313261307,1.789863712523774E-3,1.1536344511819136E-2,8.6828435891548483E-2,0.49721310294140503,4.6084717676047587E-3,9.6754838504792241E-4,1.0234938612652301E-2,2.8643315038903998E-3,0,2.4374583615006558E-6,2.4183262444488395E-6,0.11344285877442138,0.72949075188551915,0.35652747313261307,35.652747313261308,147,69.727575757335345,0.69727575757335347,782.59733406162479,null,0.21276877984235301,null,0.8716181401771288,0.15435312826790928,3.8997112232089844E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR55, IF(MODE_ILIM=4,#REF!,#REF!))","v":35.652747313261308},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ55, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.8716181401771288},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA55, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15435312826790928},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB55, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.8997112232089844E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S55, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":782.59733406162479},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P55, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71163970716902336}]
["Ltc",4000,"ppm",{"$f":"Ltc","v":4.0000000000000001E-3},"Inductor DCR Temp Co",null,null,50,0.15,0.12626862745098039,0.21318131114955785,8.6990810047570685E-2,0.71157274549631033,0.71157274549631033,1,0.71157274549631033,1.2120025322519934E-6,5.068180142994029E-2,783264.203917259,1.2767084146049346E-6,0,6.6E-4,0.15432489602957131,4.0487495008714588E-3,0,4.0513739806125543E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,3.390062042919445E-2,3.4477561964529481E-6,3.4477561964529481E-6,3.4742575867348323E-2,2.2330361691121404E-3,2.3497926117517767E-3,42.5,51.118870166840168,0.3883973513404852,0.28974509431307244,0.68049223826530936,0.68302617025872114,0.14708620659698718,1.6225764128318696E-2,6.3444400517297982E-3,6.4994428159236622E-3,1.3448865137905257E-3,1.4188769381443986E-2,3.0512203645651857E-2,4.4899065126050422E-2,0.15444639668591825,8.6942326634815749E-3,0.87667900325377279,0.88073711542441813,0.49499999999999994,0.35980711318331432,1.8418722334390628E-3,1.1865227797661075E-2,8.5947789659561263E-2,0.49463827837150121,4.7243348624192412E-3,9.7757522037604191E-4,1.0313576062143762E-2,2.9429674139615043E-3,0,2.5061155636477158E-6,2.391760605608064E-6,0.11226446895580861,0.72552098845304092,0.35980711318331432,35.98071131833143,150,69.979193442852676,0.69979193442852672,783.26420391725901,null,0.21061079988649242,null,0.87667900325377279,0.15444639668591825,4.0513739806125543E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR56, IF(MODE_ILIM=4,#REF!,#REF!))","v":35.98071131833143},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ56, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.87667900325377279},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA56, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15444639668591825},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB56, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.0513739806125543E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S56, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":783.26420391725901},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P56, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71157274549631033}]
["ThetaCA",20,"°C/W",{"$f":"ThetaCa","v":40},"Inductor Core-to-Ambient thermal resistance",null,null,51,0.153,0.12625674509803922,0.21618133468127643,8.9996751270643313E-2,0.71150578382359719,0.71150578382359719,1,0.71150578382359719,1.210916363894981E-6,5.0724956030882305E-2,783931.13865909015,1.2756222462479222E-6,0,6.6E-4,0.15724240374192325,4.2032795008714596E-3,0,4.2061082126200284E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,3.4553603111100548E-2,3.5818544638783728E-6,3.5818544638783728E-6,3.5414451010786184E-2,2.3202391797314428E-3,2.3517934159772705E-3,42.5,50.408350518273565,0.39212640586815994,0.28999180681277059,0.68447000609690778,0.68710475839996676,0.14993065792760824,1.6859401639954107E-2,6.3498422231386305E-3,6.7288677024727071E-3,1.3733693763949696E-3,1.4452079302006308E-2,3.1415971176982138E-2,4.4899065126050422E-2,0.15453967417891079,8.7016356391159018E-3,0.88176203939497555,0.88597501989589578,0.50490000000000002,0.3630088920842009,1.8943127638140992E-3,1.2196560893189053E-2,8.508474377578075E-2,0.4921146733573078,4.8378665273435921E-3,9.8741393493267525E-4,1.0390638335778017E-2,3.022039680593348E-3,0,2.5752525659325358E-6,2.3657293353296973E-6,0.11110967697908455,0.72164286722972515,0.3630088920842009,36.300889208420088,153,70.206518151218702,0.702065181512187,783.93113865909015,null,0.20849594871182306,null,0.88176203939497555,0.15453967417891079,4.2061082126200284E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR57, IF(MODE_ILIM=4,#REF!,#REF!))","v":36.300889208420088},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ57, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.88176203939497555},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA57, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15453967417891079},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB57, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.2061082126200284E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S57, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":783.93113865909015},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P57, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71150578382359719}]
[null,null,null,null,null,null,null,52,0.156,0.12624486274509805,0.219181358212995,9.3002692493715927E-2,0.71143882215088416,0.71143882215088416,1,0.71143882215088416,1.2098319366776542E-6,5.0768114830955759E-2,784598.13829658902,1.2745378190305954E-6,0,6.6E-4,0.16016295930875526,4.3608695008714596E-3,0,4.3639143746475898E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,3.5207795289720123E-2,3.718766547488515E-6,3.718766547488515E-6,3.6087566995643104E-2,2.4092781095803048E-3,2.3537944148897668E-3,42.5,49.71731163815889,0.39586127546251737,0.29023854331867416,0.68845361319608123,0.691191416234606,0.15278036248579693,1.750637937096863E-2,6.3552449202023721E-3,6.9586741177120213E-3,1.4019186423232903E-3,1.4715837680237685E-2,3.2333887256488926E-2,4.4899065126050422E-2,0.15463296074821137,8.7090393350921398E-3,0.88686730357439836,0.8912382271494298,0.51479999999999992,0.36613513776484863,1.9471753937126859E-3,1.253027779477211E-2,8.4238772936765488E-2,0.48964075080080621,4.9491357939960715E-3,9.9707007622794786E-4,1.0466171826687987E-2,3.10152982804215E-3,0,2.644854510839196E-6,2.3402164840254374E-6,0.10997777852861851,0.7178536480506239,0.36613513776484863,36.613513776484865,156,70.411746141009829,0.70411746141009823,784.59813829658901,null,0.20642293908829012,null,0.88686730357439836,0.15463296074821137,4.3639143746475898E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR58, IF(MODE_ILIM=4,#REF!,#REF!))","v":36.613513776484865},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ58, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.88686730357439836},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA58, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15463296074821137},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB58, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.3639143746475898E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S58, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":784.59813829658901},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P58, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71143882215088416}]
[null,null,null,null,null,null,null,53,0.159,0.12623298039215686,0.22218138174471358,9.6008633716788555E-2,0.71137186047817091,0.71137186047817091,1,0.71137186047817091,1.2087492464167672E-6,5.0811277830773563E-2,785265.20283922774,1.2734551287697084E-6,0,6.6E-4,0.16308639898697255,4.5215195008714605E-3,0,4.5247929311875833E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,3.5863159973063011E-2,3.8584987297605267E-6,3.8584987297605267E-6,3.6761887519232581E-2,2.5001572918569104E-3,2.3557956085176832E-3,42.5,49.044963186225537,0.39960196097234574,0.29048530383428711,0.69244306041515058,0.69528615441346731,0.15563516658046062,1.8166728807395793E-2,6.3606481429977456E-3,7.1888621173309252E-3,1.4305343688120632E-3,1.4980044629140734E-2,3.3265996514576991E-2,4.4899065126050422E-2,0.15472625639514481,8.7164437515154288E-3,0.89199485107470455,0.89652679293845827,0.52469999999999994,0.36918808638215728,2.0004506053805E-3,1.2866315197751884E-2,8.3409372529147763E-2,0.487215034120972,5.0582089734373704E-3,1.0065489729857689E-3,1.0540221098821767E-2,3.1814201106657933E-3,0,2.7149071132995497E-6,2.3152067303360209E-6,0.10886809702991909,0.71415069875292558,0.36918808638215728,36.918808638215729,159,70.596901007914624,0.70596901007914625,785.26520283922775,null,0.20439053448583955,null,0.89199485107470455,0.15472625639514481,4.5247929311875833E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR59, IF(MODE_ILIM=4,#REF!,#REF!))","v":36.918808638215729},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ59, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.89199485107470455},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA59, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15472625639514481},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB59, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.5247929311875833E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S59, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":785.26520283922775},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P59, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71137186047817091}]
[null,null,null,null,null,null,null,54,0.16200000000000001,0.12622109803921569,0.22518140527643216,9.9014574939861183E-2,0.71130489880545789,0.71130489880545789,1,0.71130489880545789,1.2076682889424648E-6,5.0854445030948735E-2,785932.33229648042,1.272374171295406E-6,0,6.6E-4,0.16601257041121312,4.6852295008714597E-3,0,4.6887443558119224E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,3.6519662709198798E-2,4.0010572931809361E-6,4.0010572931809361E-6,3.7437378781848107E-2,2.5928810606028062E-3,2.3577969968894413E-3,42.5,48.390557004194747,0.40334846324659879,0.29073208836311404,0.69643834860660225,0.6993889836208671,0.15849492711712548,1.8840481441397189E-2,6.3660518916014916E-3,7.4194317570295812E-3,1.4592166131090049E-3,1.5244700261740079E-2,3.4212343859527317E-2,4.4899065126050422E-2,0.15481956112103618,8.7238488884909329E-3,0.89714473748992163,0.90184077333686308,0.53459999999999996,0.37216988679465007,2.054129254080207E-3,1.3204612365412916E-2,8.2596057620854743E-2,0.48483610430297835,5.1651497888034626E-3,1.0158557458092986E-3,1.0612828976113315E-2,3.2616934772657803E-3,0,2.7853966327386048E-6,2.2906853505009424E-6,0.10777998229706967,0.71053148991037096,0.37216988679465007,37.216988679465004,162,70.763841860106652,0.70763841860106647,785.93233229648047,null,0.20239754660245485,null,0.89714473748992163,0.15481956112103618,4.6887443558119224E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR60, IF(MODE_ILIM=4,#REF!,#REF!))","v":37.216988679465004},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ60, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.89714473748992163},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA60, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15481956112103618},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB60, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.6887443558119224E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S60, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":785.93233229648047},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P60, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71130489880545789}]
[null,null,null,null,null,null,null,55,0.16500000000000001,0.12620921568627452,0.22818142880815073,0.1020205161629338,0.71123793713274475,0.71123793713274475,1,0.71123793713274475,1.206589060098227E-6,5.0897616432094478E-2,786599.52667782374,1.2712949424511682E-6,0,6.600000000000001E-4,0.16894133163479563,4.8519995008714607E-3,0,4.8557691311755906E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,3.7177271373091028E-2,4.1464485202453605E-6,4.1464485202453605E-6,3.8114009275891737E-2,2.6874537507031089E-3,2.3597985800334711E-3,42.5,47.753384338666223,0.40710078313439535,0.29097889690866052,0.70043947862308942,0.70349991457472461,0.16135951070519086,1.9527668771263954E-2,6.3714561660903734E-3,7.6503830925190013E-3,1.4879654324729762E-3,1.5509804691082351E-2,3.5172974479763162E-2,4.4899065126050429E-2,0.15491287492721087,8.7312547461238441E-3,0.90231701872782244,0.90718022474135462,0.54449999999999998,0.37508260477751798,2.1082025500350566E-3,1.3545111005548203E-2,8.1798362010780348E-2,0.48250259711837473,5.2700195002532797E-3,1.0249953172284114E-3,1.0684036626486201E-2,3.3423335374951051E-3,0,2.8563098467392378E-6,2.2666381895029622E-6,0.10671280925853464,0.70699358987277228,0.37508260477751798,37.508260477751797,165,70.914272258910415,0.70914272258910416,786.59952667782375,null,0.20044283303542568,null,0.90231701872782244,0.15491287492721087,4.8557691311755906E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR61, IF(MODE_ILIM=4,#REF!,#REF!))","v":37.508260477751797},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ61, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.90231701872782244},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA61, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15491287492721087},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB61, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.8557691311755906E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S61, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":786.59952667782375},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P61, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71123793713274475}]
[null,null,null,null,null,null,null,56,0.16800000000000001,0.12619733333333333,0.23118145233986931,0.10502645738600642,0.71117097546003161,0.71117097546003161,1,0.71117097546003161,1.205511555740818E-6,5.0940792034824052E-2,787266.7859927353,1.2702174380937592E-6,0,6.600000000000001E-4,0.17187255026483433,5.0218295008714608E-3,0,5.0258677490201825E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,3.7835955974259011E-2,4.2946786934581985E-6,4.2946786934581985E-6,3.8791749595700288E-2,2.7838796978867002E-3,2.3618003579782059E-3,42.5,47.132773280555853,0.41085892148501968,0.29122572947443259,0.70444645131743044,0.70761895802667629,0.16422879285280953,2.0228322301418269E-2,6.376860966541156E-3,7.8817161795210287E-3,1.5167808841739802E-3,1.5775358030236164E-2,3.61479338461351E-2,4.4899065126050429E-2,0.15500619781499439,8.738661324519361E-3,0.90751175101232517,0.91254520387387517,0.5544,0.37792822699576867,2.1626620414095668E-3,1.388775515411176E-2,8.1015837332995194E-2,0.48021320050479355,5.3728770227457539E-3,1.0339724211705387E-3,1.0753883641036462E-2,3.4233245301937176E-3,0,2.9276340262178231E-6,2.2430516338685967E-6,0.10566597675608987,0.70353466009020649,0.37792822699576867,37.792822699576867,168,71.049749591014816,0.71049749591014821,787.26678599273532,null,0.19852529508625844,null,0.90751175101232517,0.15500619781499439,5.0258677490201825E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR62, IF(MODE_ILIM=4,#REF!,#REF!))","v":37.792822699576867},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ62, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.90751175101232517},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA62, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15500619781499439},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB62, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.0258677490201825E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S62, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":787.26678599273532},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P62, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71117097546003161}]
[null,1500,null,null,null,"Eff (%)","Iout (mA)",57,0.17099999999999999,0.12618545098039213,0.23418147587158783,0.10803239860907901,0.71110401378731836,0.71110401378731836,1,0.71110401378731836,1.2044357717402326E-6,5.0983971839750841E-2,787934.11025069479,1.2691416540931738E-6,0,6.5999999999999989E-4,0.17480610268105057,5.1947195008714593E-3,0,5.1990407101775368E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,3.849568848296453E-2,4.4457540953323434E-6,4.4457540953323434E-6,3.9470572265768646E-2,2.8821632387264402E-3,2.3638023307520845E-3,42.5,46.528086401636799,0.41462287914792101,0.291472586063937,0.70845926754261002,0.71174612476219179,0.16710265723965334,2.0942473542414804E-2,6.3822662930306286E-3,8.1134310737683603E-3,1.5456630254931686E-3,1.6041360392292158E-2,3.713726771422491E-2,4.4899065126050408E-2,0.15509952978571259,8.7460686237827122E-3,0.91272899088591197,0.91793576778402119,0.56429999999999991,0.38070866475152082,2.2174995982560224E-3,1.423249106548795E-2,8.0248052211877807E-2,0.47796665209460848,5.473779037121834E-3,1.0427916118931422E-3,1.0822408108714302E-2,3.5046512935237644E-3,0,2.999356912010601E-6,2.2199125860147585E-6,0.10463890641202797,0.70015245070300935,0.38070866475152082,38.07086647515208,170.99999999999997,71.171694607053283,0.71171694607053282,787.93411025069474,null,0.1966438756903672,null,0.91272899088591197,0.15509952978571259,5.1990407101775368E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR63, IF(MODE_ILIM=4,#REF!,#REF!))","v":38.07086647515208},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ63, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.91272899088591197},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA63, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15509952978571259},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB63, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.1990407101775368E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S63, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":787.93411025069474},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P63, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71110401378731836}]
[null,null,null,null,null,{"$f":"BR56","v":35.98071131833143},{"$f":"I56*1000","v":150},58,0.17399999999999999,0.12617356862745099,0.23718149940330641,0.11103833983215164,0.71103705211460533,0.71103705211460533,1,0.71103705211460533,1.2033617039796432E-6,5.1027155847488348E-2,788601.49946118356,1.2680675863325844E-6,0,6.6E-4,0.17774187332910046,5.3706695008714587E-3,0,5.3752885245734287E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,3.915644267290249E-2,4.5996810083888973E-6,4.5996810083888973E-6,4.0150451585352902E-2,2.9823087106393698E-3,2.3658044983835506E-3,42.5,45.93871857070711,0.41839265697271411,0.29171946668068099,0.71247792815177857,0.71588142560068979,0.16998099505902534,2.1670154010942296E-2,6.3876721456355883E-3,8.3455278310045344E-3,1.5746119137228448E-3,1.6307811890362966E-2,3.814102212666895E-2,4.4899065126050422E-2,0.15519287084069155,8.7534766440191397E-3,0.91796879521206942,0.9233519738514876,0.57419999999999993,0.38342575752028185,2.272707397365258E-3,1.4579267108943217E-2,7.9494591464820977E-2,0.47576173688275286,5.5727800949312237E-3,1.0514572724131706E-3,1.088964668680021E-2,3.5862992367863347E-3,0,3.0714666927780688E-6,2.1972084400399647E-6,0.10363104156015226,0.69684479638009833,0.38342575752028185,38.342575752028182,174,71.281400919850697,0.71281400919850701,788.60149946118361,null,0.19479755746334509,null,0.91796879521206942,0.15519287084069155,5.3752885245734287E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR64, IF(MODE_ILIM=4,#REF!,#REF!))","v":38.342575752028182},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ64, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.91796879521206942},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA64, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15519287084069155},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB64, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.3752885245734287E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S64, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":788.60149946118361},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P64, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71103705211460533}]
[null,null,null,null,null,{"$f":"BR81","v":42.141814955058685},{"$f":"I81*1000","v":224.99999999999997},59,0.17699999999999999,0.1261616862745098,0.24018152293502498,0.11404428105522425,0.71097009044189219,0.71097009044189219,1,0.71097009044189219,1.2022893483553454E-6,5.1070344058650276E-2,789268.95363368606,1.2669952307082866E-6,0,6.6E-4,0.18067975408035622,5.5496795008714598E-3,0,5.5546117112313187E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,3.9818193978619333E-2,4.7564657151568709E-6,4.7564657151568709E-6,4.0831363487681863E-2,3.0843204518869191E-3,2.367806860901058E-3,42.5,45.364094933655991,0.42216825580917972,0.2919663713281731,0.71650243399825386,0.72002487139565552,0.17286370442181703,2.2411395229824993E-2,6.3930785244328573E-3,8.5780065069839626E-3,1.6036276061664665E-3,1.6574712637583287E-2,3.9159243415500866E-2,4.4899065126050422E-2,0.15528622098125777,8.7608853853339153E-3,0.92323122117774814,0.92879387978853101,0.58409999999999995,0.38608127628994321,2.3282779079614067E-3,1.4928033670857599E-2,7.8755055349417846E-2,0.4735972850246476,5.6699327174110706E-3,1.0599736224662485E-3,1.0955634667449421E-2,3.6682543138102865E-3,0,3.1439519841416237E-6,2.1749270588661029E-6,0.10264184623640843,0.69360961238947305,0.38608127628994321,38.608127628994318,177,71.3800443047935,0.713800443047935,789.26895363368601,null,0.19298536085623105,null,0.92323122117774814,0.15528622098125777,5.5546117112313187E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR65, IF(MODE_ILIM=4,#REF!,#REF!))","v":38.608127628994318},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ65, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.92323122117774814},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA65, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15528622098125777},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB65, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.5546117112313187E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S65, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":789.26895363368601},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P65, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71097009044189219}]
[null,null,null,null,null,{"$f":"BR106","v":45.731703226723738},{"$f":"I106*1000","v":300},60,0.18,0.12614980392156863,0.24318154646674356,0.11705022227829688,0.71090312876917905,0.71090312876917905,1,0.71090312876917905,1.2012187007767096E-6,5.1113536473850328E-2,789936.4727776869,1.2659245831296508E-6,0,6.6E-4,0.18361964365104841,5.7317495008714602E-3,0,5.7370107982761829E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,4.0480919366095103E-2,4.9161144981728804E-6,4.9161144981728804E-6,4.1513285412218041E-2,3.1882028015751095E-3,2.3698094183330605E-3,42.5,44.803669043254978,0.42594967650726312,0.29221330000992191,0.72053278593551806,0.7241764730347543,0.1757506898157126,2.3166228728024117E-2,6.3984854294992649E-3,8.810867157471888E-3,1.6327101601386453E-3,1.6842062747109799E-2,4.0191978204513909E-2,4.4899065126050422E-2,0.15537958020873771,8.7682948478323246E-3,0.92851632629583836,0.93426154364244907,0.59399999999999997,0.38867692671521664,2.3842038781869078E-3,1.5278743062363572E-2,7.8029058852258207E-2,0.47147216975584216,5.7652874889936199E-3,1.0683447260259223E-3,1.102040604055804E-2,3.7505029978117778E-3,0,3.2168018089729876E-6,2.1530567526436595E-6,0.10167080422530754,0.69044489088590921,0.38867692671521664,38.867692671521667,180,71.468691685531624,0.71468691685531627,789.93647277768684,null,0.19120634241274079,null,0.92851632629583836,0.15537958020873771,5.7370107982761829E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR66, IF(MODE_ILIM=4,#REF!,#REF!))","v":38.867692671521667},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ66, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.92851632629583836},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA66, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15537958020873771},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB66, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.7370107982761829E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S66, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":789.93647277768684},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P66, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71090312876917905}]
[null,null,null,null,null,null,null,61,0.183,0.12613792156862746,0.24618156999846214,0.12005616350136949,0.71083616709646591,0.71083616709646591,1,0.71083616709646591,1.2001497571661268E-6,5.1156733093702368E-2,790604.05690267298,1.264855639519068E-6,0,6.6E-4,0.18656144707451752,5.9168795008714614E-3,0,5.9224863229384037E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,4.1144597215109824E-2,5.0786336399808689E-6,5.0786336399808689E-6,4.2196196188594465E-2,3.2939600996547552E-3,2.371812170708019E-3,42.5,44.256921125884325,0.42973691991707519,0.29246025272943676,0.72456898481721999,0.72833624143995168,0.17864186161382364,2.3934686040639388E-2,6.4038928609116523E-3,9.0441098382444129E-3,1.6618596329651509E-3,1.7109862332121216E-2,4.1239273411643261E-2,4.4899065126050422E-2,0.15547294852445828,8.7757050316196704E-3,0.93382416840767279,0.93975502379808751,0.60389999999999999,0.39121435209930105,2.4404783223278383E-3,1.5631349432046554E-2,7.7316231016677353E-2,0.46938530542559537,5.8588931456925036E-3,1.0765744984110677E-3,1.1083993553186022E-2,3.8330322576305095E-3,0,3.2900055787627599E-6,2.1315862583396682E-6,0.10071741815857582,0.68734869740198024,0.39121435209930105,39.121435209930105,183,71.54830972155635,0.71548309721556347,790.60405690267294,null,0.1894595931219481,null,0.93382416840767279,0.15547294852445828,5.9224863229384037E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR67, IF(MODE_ILIM=4,#REF!,#REF!))","v":39.121435209930105},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ67, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.93382416840767279},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA67, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15547294852445828},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB67, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9224863229384037E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S67, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":790.60405690267294},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P67, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71083616709646591}]
[null,null,null,null,null,null,null,62,0.186,0.12612603921568627,0.24918159353018071,0.12306210472444212,0.71076920542375277,0.71076920542375277,1,0.71076920542375277,1.1990825134589549E-6,5.1199933918820446E-2,791271.70601813414,1.2637883958118961E-6,0,6.6E-4,0.18950507522105575,6.1050695008714601E-3,0,6.1110388315577299E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,4.1809207212175195E-2,5.2440294231318074E-6,5.2440294231318074E-6,4.2880075931014373E-2,3.401596686921683E-3,2.3738151180544022E-3,42.5,43.723356473638169,0.4335299868888931,0.29270722949022815,0.72861103149717565,0.73250418756763069,0.18153713562761964,2.4716798708910578E-2,6.4093008187468877E-3,9.2777346050885168E-3,1.6910760819829188E-3,1.7378111505818326E-2,4.2301176251368679E-2,4.4899065126050422E-2,0.15556632592974667,8.7831159368012904E-3,0.93915480568554721,0.94527437898036437,0.61380000000000001,0.39369513621372293,2.4970945087309858E-3,1.5985808683386903E-2,7.6616214306990393E-2,0.46733564563718105,5.9507966586919104E-3,1.0846667130075499E-3,1.1146428765754989E-2,3.9158295352555144E-3,0,3.3635530759997521E-6,2.1105047204335069E-6,9.9781208662724066E-2,0.68431916752951982,0.39369513621372293,39.369513621372292,186,71.619772941093288,0.71619772941093285,791.27170601813418,null,0.18774423686037281,null,0.93915480568554721,0.15556632592974667,6.1110388315577299E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR68, IF(MODE_ILIM=4,#REF!,#REF!))","v":39.369513621372292},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ68, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.93915480568554721},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA68, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15556632592974667},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB68, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1110388315577299E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S68, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":791.27170601813418},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P68, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71076920542375277}]
[null,null,null,null,null,null,null,63,0.189,0.12611415686274507,0.25218161706189929,0.12606804594751475,0.71070224375103952,0.71070224375103952,1,0.71070224375103952,1.1980169656034716E-6,5.1243138949818641E-2,791939.42013356078,1.2627228479564128E-6,0,6.6E-4,0.19245044436045869,6.2963195008714614E-3,0,6.3026688795873144E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,4.247473025295314E-2,5.4123081301833982E-6,5.4123081301833982E-6,4.3564905942040967E-2,3.5111169050169215E-3,2.3758182604006824E-3,42.5,43.202503951353577,0.43732887827315892,0.29295423029580675,0.7326589268293664,0.73668032240870851,0.18443643269961199,2.5512598280218873E-2,6.4147093030818437E-3,9.5117415138020224E-3,1.720359564540045E-3,1.7646810381423912E-2,4.3377734237136936E-2,4.4899065126050422E-2,0.15565971242593024,8.7905275634825256E-3,0.94450829663525826,0.95081966825681208,0.62369999999999992,0.39612080596650334,2.5540459483712231E-3,1.6342078396645459E-2,7.5928664006922358E-2,0.4653221814882188,6.0410433134396443E-3,1.0926250076283236E-3,1.1207742105223184E-2,3.998882724559589E-3,0,3.4374344374976858E-6,2.0898016726510088E-6,9.8861713552466951E-2,0.68135450377958584,0.39612080596650334,39.612080596650337,189,71.68387138413388,0.71683871384133879,791.93942013356082,null,0.18605942891786376,null,0.94450829663525826,0.15565971242593024,6.3026688795873144E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR69, IF(MODE_ILIM=4,#REF!,#REF!))","v":39.612080596650337},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ69, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.94450829663525826},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA69, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15565971242593024},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB69, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.3026688795873144E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S69, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":791.93942013356082},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P69, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71070224375103952}]
[null,null,null,null,null,null,null,64,{"$f":"IF(PLOT_TYPE=1, H70/100*Iout, min_I*EXP(H70*rr/100))","v":0.192},{"$f":"IF(I70<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I70-Vout)/L*OnTime)","v":0.12610227450980391},{"$f":"IF(I70<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I70+((Vin-(Rdcr+RdsonTop)*J70-Vout)/L*OnTime)/2)","v":0.25518164059361781},{"$f":"IF(I70<Icrit, 0, I70-((Vin-(Rdcr+RdsonTop)*K70-Vout)/L*OnTime)/2)","v":0.12907398717058738},0.71063528207832638,{"$f":"IF(I70<Icrit, 1000*SQRT((J70*CoutEsr)^2+(((J70/2)-I70)*(OnTime+OffTime)/Cout)^2), 1000*J70*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":0.71063528207832638},1,{"$f":"IF(I70<Icrit, 1000*((N70/1000)*O70), 1000*J70*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":0.71063528207832638},{"$f":"IF(I70<Icrit, L*J70/(Vout+J70/2*(RdsonBot+Rdcr)), L*J70/(Vout+I70*(RdsonBot+Rdcr)))","v":1.1969531095608201E-6},5.1286348187311176E-2,{"$f":"IF(I70<Icrit,I70/((OnTime+Q70)*J70/2),1/(OnTime+Q70))","v":792607.19925844541},1.2616589919137613E-6,0,{"$f":"S70*(T70*Iq_active+U70*Iq_sleep)","v":6.6E-4},0.19539747576296373,{"$f":"W70^2*Rdcr","v":6.490629500871461E-3},{"$f":"Core_Loss/1000*S70/$S$106","v":0},{"$f":"(Y70+X70*(1+Ltc*(Ta-25)))/(1-X70*Ltc*ThetaCa)","v":6.4973770315977925E-3},3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,4.3141148353205178E-2,5.5834760436997733E-6,5.5834760436997733E-6,4.4250668624827343E-2,3.6225250964269161E-3,2.3778215977753362E-3,42.5,{"$f":"IF(I70<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I70+Iripple/2)*1000000000)","v":42.693914609093071},{"$f":"IF(I70<Icrit, Vin*(I70+Iripple/2)*AK70/1000000000/2*S70, Vin*(I70-Iripple/2)*AJ70/1000000000/2*S70 + Vin*(I70+Iripple/2)*AK70/1000000000/2*S70)","v":0.44113359492048021},{"$f":"IF(I70<Icrit, Csw*(Vin)^2*S70/2, Csw*Vin^2*S70/2)","v":0.29320125514968409},0.73671267166793963,{"$f":"(AI70+AL70+AM70+AH70*(1+RdsonTopTc*(Ta-25)))/(1-AH70*RdsonTopTc*ThetaJA)","v":0.7408646569887547},{"$f":"IF(I70<Icrit,Iripple*SQRT((OffTime)*S70/3), SQRT(OffTime*S70*(I70^2+Iripple^2/12)))","v":0.18733967833177068},2.6322116308088478E-2,{"$f":"QgBot*S70*Vdd","v":6.4201183139934084E-3},{"$f":"IF(I70<Icrit, Vin*Idss*R70, QrrBot*(I70-Iripple/2)/1*S70*Vin+Vin*Idss*R70)","v":9.7461306201936278E-3},{"$f":"IF(I70<Icrit, dead1*S70*(I70+Iripple/2)*((I70+Iripple/2)*BDserR+VSD), dead1*S70*(I70+Iripple/2)*((I70+Iripple/2)*BDserR+VSD)+dead2*S70*(I70-Iripple/2)*((I70-Iripple/2)*BDserR+VSD))","v":1.7497101379957926E-3},1.7915959072182828E-2,{"$f":"(AR70+AS70+AT70+AQ70*(1+RdsonBotTc*(Ta-25)))/(1-AQ70*RdsonBotTc*ThetaJA)","v":4.4468995183805433E-2},{"$f":"Vin*V70+Vout*Ifb/0.8","v":4.4899065126050422E-2},{"$f":"(Vin-Vdd)*(S70*QgBot+S70*QgTop)+AW70","v":0.15575310801433662},{"$f":"AI70+AR70","v":8.797939911768745E-3},0.94988470009866544,{"$f":"SUM(Z70,AC70,AF70,AZ70)","v":0.95639095104014327},{"$f":"Vout*I70","v":0.63359999999999994},0.39849283392808638,2.6113263840268474E-3,1.6700117754916838E-2,{"$f":"Vin*S70*(QgBot+QgTop)/($BB70+$BA70)","v":7.5253247650108171E-2},0.46334393990481237,6.1296767845237642E-3,1.10045289053448E-3,1.1267962915425733E-2,{"$f":"X70/($BB70+$BA70)","v":4.0821801511671555E-3},{"$f":"Y70/($BB70+$BA70)","v":0},3.5116401386103263E-6,2.0694670206723219E-6,9.7958487067140693E-2,0.6784529726098153,{"$f":"BC70","v":0.39849283392808638},39.849283392808637,{"$f":"I70*1000","v":192},71.741317737155555,0.71741317737155552,{"$f":"S70/1000","v":792.60719925844546},null,{"$f":"AM70/($BB70+$BA70)","v":0.18440435460206683},null,0.94988470009866544,0.15575310801433662,6.4973770315977925E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR70, IF(MODE_ILIM=4,#REF!,#REF!))","v":39.849283392808637},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ70, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.94988470009866544},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA70, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15575310801433662},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB70, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.4973770315977925E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S70, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":792.60719925844546},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P70, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71063528207832638}]
[null,null,null,null,null,null,null,65,0.19500000000000001,0.12609039215686274,0.25818166412533639,0.13207992839366001,{"$f":"IF(I71<Icrit, 1000*((((J71/2)-I71)*0.000002/Cout+Vout/306)), 1000*J71*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":0.71056832040561335},0.71056832040561335,{"$f":"ROUNDUP(M71/N71,0)","v":1},0.71056832040561335,1.195890941304958E-6,5.1329561631912421E-2,793275.04340228287,{"$f":"IF(1/S71-OnTime-Q71>Tsleep, OnTime+Q71+Tsleep, 1/S71)","v":1.2605968236578992E-6},{"$f":"IF(1/S71-OnTime-Q71>Tsleep, 1/S71-OnTime-Q71-Tsleep, 0)","v":0},6.6E-4,{"$f":"IF(I71<Icrit,Iripple*SQRT((OnTime+OffTime)*S71/3), SQRT(I71^2+Iripple^2/12))","v":0.1983460953347406},6.6879995008714615E-3,0,6.6951638612814616E-3,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q71)*S71)","v":3.6279106032784197E-2},{"$f":"RCoutEsr*AA71^2","v":3.2904338363449972E-6},3.2904338363449972E-6,{"$f":"SQRT($R71)*SQRT($I71^2*(1-R71)+(Iripple^2)/12)","v":4.3808444567424144E-2},{"$f":"RCinEsr*AD71^2","v":5.757539446251222E-6},5.757539446251222E-6,{"$f":"IF(I71<Icrit,Iripple*SQRT((OnTime)*S71/3), SQRT(OnTime*S71*(I71^2+Iripple^2/12)))","v":4.4937347402943473E-2},{"$f":"RdsonTop*AG71^2","v":3.7358256044837368E-3},{"$f":"QgTop*S71*Vdd","v":2.3798251302068487E-3},42.5,42.197160391491813,0.44494413768163066,0.29344830405537248,{"$f":"AI71+AL71+AM71","v":0.74077226686720998},0.74505720236811235,0.19024680234610369,{"$f":"RdsonBot*AP71^2","v":2.7145384352188082E-2},6.4255278515584924E-3,9.9809019800828919E-3,1.7791278597205956E-3,{"$f":"AR71+AS71+AT71","v":1.818555769136198E-2},4.5575007210106287E-2,4.4899065126050422E-2,0.15584651269629371,8.8053529817653416E-3,0.95528407525627768,0.96198828709084172,0.64349999999999996,0.40081264072379341,{"$f":"(AO71-AN71)/($BB71+$BA71)","v":2.6689297800276727E-3},{"$f":"(AV71-AU71)/($BB71+$BA71)","v":1.7059887474093146E-2},7.4589644480684267E-2,{"$f":"AN71/($BB71+$BA71)","v":0.46139998206370952},{"$f":"AS71/(BA71+BB71)","v":6.2167392065926377E-3},{"$f":"AT71/($BB71+$BA71)","v":1.1081537461381237E-3},{"$f":"AU71/($BB71+$BA71)","v":1.1327119504754759E-2},4.1657105533857075E-3,0,{"$f":"(AF71)/($BB71+$BA71)","v":3.5861609782802792E-6},{"$f":"(AC71)/($BB71+$BA71)","v":2.0494910257534743E-6},{"$f":"AX71/($BB71+$BA71)","v":9.7071099147468032E-2},{"$f":"SUM(BD71:BO71)","v":0.6756129016088579},0.40081264072379341,40.081264072379341,195,71.792753953912452,{"$f":"BT71/100","v":0.71792753953912447},793.2750434022829,null,0.1827782279166317,null,{"$f":"AZ71","v":0.95528407525627768},{"$f":"AX71","v":0.15584651269629371},{"$f":"Z71","v":6.6951638612814616E-3},null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR71, IF(MODE_ILIM=4,#REF!,#REF!))","v":40.081264072379341},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ71, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.95528407525627768},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA71, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15584651269629371},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB71, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.6951638612814616E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S71, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":793.2750434022829},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P71, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71056832040561335}]
[null,null,null,null,null,null,null,66,0.19800000000000001,0.12607850980392157,0.26118168765705496,0.13508586961673261,0.71050135873290032,0.71050135873290032,1,0.71050135873290032,1.194830456822608E-6,{"$f":"OnTime*S72","v":5.137277928423685E-2},793942.9525745695,1.2595363391755492E-6,0,6.6E-4,0.20129623328452523,6.8884295008714612E-3,0,6.8960299514565027E-3,3.6279106032784197E-2,3.2904338363449972E-6,{"$f":"AB72","v":3.2904338363449972E-6},4.447660291439335E-2,5.9345046204138695E-6,{"$f":"AE72","v":5.9345046204138695E-6},4.5624926647051131E-2,3.8510227733652732E-3,2.3818288577237084E-3,42.5,41.711832936170843,0.44876050740754925,0.29369537701638471,0.74483771328165771,0.74925796964201485,0.19315773857422797,2.7982433978332343E-2,6.4309379158540136E-3,1.0216055649300254E-2,1.8086127870960609E-3,1.8455606352250329E-2,4.6695818741131483E-2,4.4899065126050422E-2,0.15593992647312971,8.8127667735777224E-3,{"$f":"AO72+AV72+AX72+AY72","v":0.96070648162985373},0.96761173651976695,0.65339999999999998,0.40308159730096582,2.7268503125382785E-3,1.7421349736499447E-2,7.3937544942134045E-2,0.45948940189710652,6.3022712415603029E-3,1.1157308404065379E-3,1.1385239191342078E-2,4.2494630641358487E-3,0,3.6609880648704997E-6,2.0298642892058254E-6,9.6199134750205528E-2,0.67283267682828263,0.40308159730096582,{"$f":"100*BQ72","v":40.308159730096584},198,71.838757366287027,0.71838757366287032,793.94295257456952,null,0.18118029030865276,null,0.96070648162985373,0.15593992647312971,6.8960299514565027E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR72, IF(MODE_ILIM=4,#REF!,#REF!))","v":40.308159730096584},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ72, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.96070648162985373},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA72, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15593992647312971},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB72, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.8960299514565027E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S72, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":793.94295257456952},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P72, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71050135873290032}]
[null,null,null,null,null,null,null,67,0.20100000000000001,0.12606662745098041,0.26418171118877354,0.13809181083980523,0.71043439706018718,0.71043439706018718,1,0.71043439706018718,1.1937716521132059E-6,5.1416001144899068E-2,794610.92678480374,1.2584775344661471E-6,0,6.6E-4,0.20424782381836534,7.0919195008714618E-3,0,7.0999758940712828E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,4.5145608309001689E-2,6.114377848769407E-6,6.114377848769407E-6,4.6313391607760268E-2,3.9681209480954549E-3,2.3838327803544111E-3,{"$f":"15*VIN_nom/24","v":42.5},41.237542454127237,0.45258270494934116,0.29394247403623458,0.74890901176593017,0.75346696994070694,0.1960724245731098,2.8833296758483375E-2,6.4363485069569111E-3,1.0451591683687025E-2,1.8381649775149693E-3,1.8726105168158903E-2,4.7831478510839388E-2,4.4899065126050422E-2,0.15603334934617308,8.8201812873113222E-3,0.9661519790850307,0.9732613597907871,0.6633,{"$f":"BB73/(BB73+BA73)","v":0.40530102707838234},2.785082360345751E-3,1.7784468127978546E-2,7.3296650192675075E-2,0.45761132467509091,6.3863121423220724E-3,1.1231873259857209E-3,1.1442348345895683E-2,4.3334271938194058E-3,0,3.7361128027311179E-6,2.0105777376814248E-6,9.5342193198377778E-2,0.6701107402530313,0.40530102707838234,40.530102707838232,201,71.879846296152991,0.71879846296152994,794.61092678480372,null,0.17960980948114971,null,0.9661519790850307,0.15603334934617308,7.0999758940712828E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR73, IF(MODE_ILIM=4,#REF!,#REF!))","v":40.530102707838232},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ73, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.9661519790850307},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA73, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15603334934617308},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB73, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0999758940712828E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S73, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":794.61092678480372},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P73, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71043439706018718}]
[null,null,null,null,null,null,null,68,0.20400000000000001,0.12605474509803921,0.26718173472049211,0.14109775206287783,0.71036743538747393,0.71036743538747393,1,0.71036743538747393,1.1927145231888518E-6,5.1459227214513771E-2,795278.96604248555,1.257420405541793E-6,0,6.6E-4,0.20720080485977366,7.2984695008714608E-3,0,7.3070022902087224E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,4.5815446499715091E-2,6.2971654139047678E-6,6.2971654139047678E-6,4.7002728354072446E-2,4.0871244745444429E-3,2.3858368981274566E-3,42.5,40.77391668564961,0.45641073115827674,0.29418959511843623,0.75298616317484046,0.75768421442956391,0.19899080136445932,2.9698004270752275E-2,6.4417596249441338E-3,1.0687510139095377E-2,1.8677844883812802E-3,1.8997054252420792E-2,4.8982035564582714E-2,4.4899065126050422E-2,0.15612678131675245,8.8275965230715896E-3,0.97162062783397063,0.97893721772342956,0.67320000000000002,0.40747220798502387,2.8436204961214706E-3,1.8149207578217908E-2,7.2666671645593942E-2,0.45576490566105721,6.4688998131900216E-3,1.1305262470601581E-3,1.1498472432330938E-2,4.4175928140692943E-3,0,3.8115268794573716E-6,1.9916226092158772E-6,9.4499887564961513E-2,0.66744558740209092,0.40747220798502387,40.74722079850239,204.00000000000003,71.916485184007442,0.71916485184007439,795.27896604248554,null,0.17806607826668064,null,0.97162062783397063,0.15612678131675245,7.3070022902087224E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR74, IF(MODE_ILIM=4,#REF!,#REF!))","v":40.74722079850239},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ74, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.97162062783397063},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA74, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15612678131675245},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB74, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.3070022902087224E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S74, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":795.27896604248554},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P74, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71036743538747393}]
[null,null,null,null,null,null,null,69,0.20699999999999999,0.12604286274509804,0.27018175825221069,0.14410369328595046,0.7103004737147609,0.7103004737147609,1,0.7103004737147609,1.1916590660742589E-6,5.1502457493695794E-2,795947.07035711675,1.2563649484272001E-6,0,6.6E-4,0.21015511779287699,7.5080795008714606E-3,0,7.5171097500907344E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,4.6486104011169677E-2,6.4828735984118566E-6,6.4828735984118566E-6,4.7692923716881122E-2,4.2080376994288477E-3,2.3878412110713504E-3,42.5,40.320599925881247,0.46024458688579239,0.29443674026650463,0.75706916836336835,0.76190971430921228,0.20191281319553275,3.057658809940058E-2,6.4471712698926462E-3,1.0923811071388373E-2,1.8974713771101317E-3,1.926845371839115E-2,5.0147539261658186E-2,4.4899065126050422E-2,0.15622022238619676,8.8350124809639975E-3,0.97711248843803111,0.98463937149555658,0.68309999999999993,0.40959637439477448,2.9024594781276525E-3,1.8515534304125714E-2,7.2047330533043352E-2,0.45394932883575295,6.5500708672437055E-3,1.1377505439645293E-3,1.155363604632781E-2,4.5019501423286179E-3,0,3.8872222537975433E-6,1.9729904399836036E-6,9.3671844088027506E-2,0.66483576505163555,0.40959637439477448,40.959637439477447,207,71.94908925319227,0.71949089253192267,795.94707035711679,null,0.17654841355844858,null,0.97711248843803111,0.15622022238619676,7.5171097500907344E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR75, IF(MODE_ILIM=4,#REF!,#REF!))","v":40.959637439477447},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ75, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.97711248843803111},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA75, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15622022238619676},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB75, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.5171097500907344E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S75, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":795.94707035711679},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P75, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.7103004737147609}]
[null,null,null,null,null,null,null,70,0.21,0.12603098039215688,0.27318178178392927,0.14710963450902309,0.71023351204204777,0.71023351204204777,1,0.71023351204204777,1.1906052768067038E-6,5.1545691983060089E-2,796615.23973820137,1.255311159159645E-6,0,6.6E-4,0.21311070722640379,7.7207495008714596E-3,0,7.7302988930827172E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,4.7157568091407656E-2,6.6715086848872485E-6,6.6715086848872485E-6,4.838396523705453E-2,4.3308649703119274E-3,2.3898457192146044E-3,42.5,39.8772521146701,0.46408427298349053,0.29468390948395545,0.76115802818666056,0.76614348081565176,0.20483840731933656,3.1469079834841825E-2,6.4525834418794319E-3,1.1160494536439962E-2,1.9272257011278492E-3,1.9540303679447243E-2,5.1328039277878379E-2,4.4899065126050422E-2,0.15631367255583528,8.8424291610940363E-3,0.98262762181045937,0.99036788264606335,0.69299999999999995,0.41167471896320285,2.9615942423438825E-3,1.8883415756076098E-2,7.1438357491915835E-2,0.45216380568590059,6.6298606807781851E-3,1.1448630575620043E-3,1.1607862951936627E-2,4.586489727210024E-3,0,3.963191144172475E-6,1.9546730517234346E-6,9.2857701615482832E-2,0.66227986907340186,0.41167471896320285,41.167471896320286,210,71.978028730187987,0.71978028730187982,796.61523973820135,null,0.17505615529550544,null,0.98262762181045937,0.15631367255583528,7.7302988930827172E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR76, IF(MODE_ILIM=4,#REF!,#REF!))","v":41.167471896320286},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ76, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.98262762181045937},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA76, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15631367255583528},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB76, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.7302988930827172E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S76, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":796.61523973820135},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P76, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71023351204204777}]
[null,null,null,null,null,null,null,71,0.21299999999999999,0.12601909803921568,0.27618180531564784,0.15011557573209569,0.71016655036933451,0.71016655036933451,1,0.71016655036933451,1.189553151435977E-6,5.1588930683221741E-2,797283.47419524507,1.2542590337889182E-6,0,6.6E-4,0.2160675207765804,7.9364795008714604E-3,0,7.9465703476981394E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,4.7829826663327586E-2,6.8630769559318869E-6,6.8630769559318869E-6,4.9075841117676822E-2,4.4556106356037992E-3,2.3918504225857351E-3,42.5,39.44354798581147,0.4679297903031393,0.29493110277430501,0.76525274350003003,0.7703855252203754,0.20776753379243507,3.2375511073642983E-2,6.4579961409814857E-3,1.1397560590134963E-2,1.9570475178719393E-3,1.9812604248988386E-2,5.2523585608165536E-2,4.4899065126050422E-2,0.15640713182699739,8.8498465635672204E-3,0.98816608921910554,0.99612281307759598,0.70289999999999997,0.41370839437215834,3.0210198949876905E-3,1.925282056685557E-2,7.0839492170501742E-2,0.45040757405361587,6.7083034450193847E-3,1.1518665334027856E-3,1.1661176116346548E-2,4.6712024345896726E-3,0,4.0394260177708657E-6,1.9366625397952913E-6,9.205711107768047E-2,0.65977654238155725,0.41370839437215834,41.370839437215835,213,72.003632642003467,0.72003632642003468,797.28347419524505,null,0.1735886654988871,null,0.98816608921910554,0.15640713182699739,7.9465703476981394E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR77, IF(MODE_ILIM=4,#REF!,#REF!))","v":41.370839437215835},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ77, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.98816608921910554},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA77, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15640713182699739},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB77, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.9465703476981394E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S77, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":797.28347419524505},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P77, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71016655036933451}]
[null,null,null,null,null,null,null,72,0.216,0.12600721568627452,0.27918182884736642,0.15312151695516832,0.71009958869662149,0.71009958869662149,1,0.71009958869662149,1.1885026860243346E-6,5.1632173594795924E-2,797951.77373775514,1.2532085683772758E-6,0,6.6E-4,0.21902550886720479,8.1552695008714621E-3,0,8.1659247516031683E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,4.8502868279964591E-2,7.0575846941507868E-6,7.0575846941507868E-6,4.9768540180066975E-2,4.5822790445616416E-3,2.3938553212132655E-3,42.5,39.019176271210277,0.47178113969667262,0.29517832014107037,0.76935331515895622,0.77463585883049124,0.21070014528875222,3.3295913418525974E-2,6.4634093672758172E-3,1.1635009288369089E-2,1.9869368847911005E-3,2.0085355540436004E-2,5.3734228569168062E-2,4.4899065126050422E-2,0.15650060020101286,8.8572646884890818E-3,0.99372795228916133,1.0019042250592949,0.71279999999999999,0.41569851498753446,3.0807317054067159E-3,1.9623718503153781E-2,7.0250482854724419E-2,0.44867989704309019,6.7854322152654323E-3,1.1587636256756711E-3,1.1713597742923533E-2,4.7560794343930951E-3,0,4.1159195801869174E-6,1.9189512618313009E-6,9.1269734986277898E-2,0.65732447298175267,0.41569851498753446,41.569851498753444,216,72.026192211331946,0.72026192211331941,797.95177373775516,null,0.17214532735572108,null,0.99372795228916133,0.15650060020101286,8.1659247516031683E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR78, IF(MODE_ILIM=4,#REF!,#REF!))","v":41.569851498753444},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ78, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.99372795228916133},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA78, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15650060020101286},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB78, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.1659247516031683E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S78, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":797.95177373775516},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P78, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71009958869662149}]
[null,null,null,null,null,null,null,73,0.219,0.12599533333333332,0.282181852379085,0.15612745817824092,0.71003262702390824,0.71003262702390824,1,0.71003262702390824,1.1874538766464467E-6,5.1675420718397966E-2,798620.13837524131,1.2521597589993879E-6,0,6.6E-4,0.22198462454534548,8.3771195008714595E-3,0,8.3883627516213779E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,4.9176682083255499E-2,7.2550381821527478E-6,7.2550381821527478E-6,5.046205182323403E-2,4.7108745472899003E-3,2.3958604151257238E-3,42.5,38.603838955870792,0.47563832201619072,0.29542556158776923,0.77345974401908568,0.77889449298884628,0.21363619692792135,3.4230318478369194E-2,6.4688231208394559E-3,1.1872840687048943E-2,2.0168938593452231E-3,2.0358557667233622E-2,5.4960018801899761E-2,4.4899065126050422E-2,0.15659407767921169,8.8646835359651802E-3,0.99931327300592288,1.0077121812295629,0.72270000000000001,0.41764615843519887,3.140725099322218E-3,1.9996080419452264E-2,6.9671086112825131E-2,0.44698006198124174,6.8612789576022112E-3,1.1655569009645422E-3,1.1765149302617387E-2,4.8411121880331471E-3,0,4.1926647655690932E-6,1.9015318269471175E-6,9.0495246957832953E-2,0.65492239211648429,0.41764615843519887,41.764615843519884,219,72.045963869077937,0.72045963869077934,798.62013837524125,null,0.17072554434854442,null,0.99931327300592288,0.15659407767921169,8.3883627516213779E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR79, IF(MODE_ILIM=4,#REF!,#REF!))","v":41.764615843519884},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ79, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.99931327300592288},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA79, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15659407767921169},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB79, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.3883627516213779E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S79, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":798.62013837524125},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P79, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71003262702390824}]
[null,null,null,null,null,null,null,74,0.222,0.12598345098039215,0.28518187591080357,0.15913339940131355,0.7099656653511951,0.7099656653511951,1,0.7099656653511951,1.1864067193893517E-6,5.1718672054643283E-2,799288.56811721437,1.2511126017422929E-6,0,6.6E-4,0.22494482331126894,8.6020295008714612E-3,0,8.6138850037385459E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,4.9851257765978346E-2,7.4554437025500489E-6,7.4554437025500489E-6,5.1156365986461658E-2,4.8414014947405007E-3,2.3978657043516429E-3,42.5,38.197250579966543,0.4795013381139594,0.29567282711791992,0.77757203093623095,0.78316143907414693,0.21657564611688293,3.5178757868208982E-2,6.4742374017494374E-3,1.211105484209201E-2,2.0469184990053874E-3,2.0632210742846834E-2,5.6201007274401894E-2,4.4899065126050422E-2,0.15668756426292402,8.8721031061010803E-3,1.0049221137175739,1.0135467445988513,0.73259999999999992,0.41955236709976679,3.2009956524015112E-3,2.0369878214174041E-2,6.9101066457443988E-2,0.44530737942925036,6.9358745933316892E-3,1.1722488418209282E-3,1.181585156383105E-2,4.9262924364627996E-3,0,4.2696547272507816E-6,1.88439708548145E-6,8.9733331260724275E-2,0.65256907250125318,0.41955236709976679,41.955236709976681,222,72.063171902227168,0.72063171902227163,799.28856811721437,null,0.1693287394272501,null,1.0049221137175739,0.15668756426292402,8.6138850037385459E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR80, IF(MODE_ILIM=4,#REF!,#REF!))","v":41.955236709976681},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ80, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0049221137175739},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA80, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15668756426292402},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB80, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.6138850037385459E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S80, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":799.28856811721437},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P80, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.7099656653511951}]
[null,null,null,null,null,null,null,75,0.22499999999999998,0.12597156862745099,0.28818189944252209,0.16213934062438615,0.70989870367848207,0.70989870367848207,1,0.70989870367848207,1.1853612103524047E-6,5.176192760414744E-2,799957.06297318765,1.2500670927053459E-6,0,6.6E-4,0.22790606296133939,8.8299995008714605E-3,0,8.8424921731074611E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,5.0526585536587114E-2,7.6588075379581628E-6,7.6588075379581628E-6,5.1851473114745882E-2,4.9738642387130482E-3,2.3998711889195632E-3,42.5,37.799137584555545,0.4833701888424109,0.29592011673504154,0.78169017676637198,0.78743670850108338,0.21951845240356183,3.6141263209241131E-2,6.4796522100828216E-3,1.2349651809426685E-2,2.0770108612538757E-3,2.0906314880763381E-2,5.7457245284428728E-2,4.4899065126050422E-2,0.15678105995348046,8.8795233990023852E-3,1.0105545371379951,1.019407978552477,0.74249999999999994,0.42141814955058687,3.2615390841424959E-3,2.0745084787966245E-2,6.854019602411128E-2,0.44366118224209516,7.0092490412426278E-3,1.1788418501630696E-3,1.1865724620839331E-2,5.0116121888078881E-3,0,4.3468828288355766E-6,1.8675401192338686E-6,8.8983682384074558E-2,0.65026332664639064,0.42141814955058687,42.141814955058685,224.99999999999997,72.078010752951272,0.72078010752951271,799.9570629731877,null,0.16795435422124561,null,1.0105545371379951,0.15678105995348046,8.8424921731074611E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR81, IF(MODE_ILIM=4,#REF!,#REF!))","v":42.141814955058685},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ81, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0105545371379951},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA81, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15678105995348046},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB81, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.8424921731074611E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S81, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":799.9570629731877},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P81, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70989870367848207}]
[null,null,null,null,null,null,null,76,0.22799999999999998,0.12595968627450979,0.29118192297424067,0.16514528184745877,0.70983174200576882,0.70983174200576882,1,0.70983174200576882,1.1843173456472303E-6,5.1805187367526109E-2,800625.62295267626,1.2490232280001715E-6,0,6.6E-4,0.2308683034427593,9.0610295008714571E-3,0,9.0741849340528688E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,5.1202656086689634E-2,7.8651359709954443E-6,7.8651359709954443E-6,5.2547364126837005E-2,5.1082671318550344E-3,2.4018768688580288E-3,42.5,37.409237697789344,0.48724487505414349,0.29616743044265398,0.78581418236565548,0.79172031272045396,0.22246457734156963,3.711786612882241E-2,6.4850675459166788E-3,1.258863164499225E-2,2.1071710035841687E-3,2.1180870194493096E-2,5.8728784462156416E-2,4.4899065126050422E-2,0.15687456475221173,8.8869444147747084E-3,1.0162106063495968,1.025295946853457,0.75239999999999985,0.42324448189903163,3.3223512520531976E-3,2.1121674003995779E-2,6.7988254265226838E-2,0.44204082467339589,7.0814312578448965E-3,1.1853382505112229E-3,1.1914787920838481E-2,5.0970637115472905E-3,0,4.4243426357115957E-6,1.8509542321728889E-6,8.8246004627440131E-2,0.64800400525972168,0.42324448189903163,42.324448189903165,227.99999999999997,72.090646982404948,0.72090646982404949,800.62562295267628,null,0.16660184828956484,null,1.0162106063495968,0.15687456475221173,9.0741849340528688E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR82, IF(MODE_ILIM=4,#REF!,#REF!))","v":42.324448189903165},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ82, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0162106063495968},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA82, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15687456475221173},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB82, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0741849340528688E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S82, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":800.62562295267628},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P82, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70983174200576882}]
[null,null,null,null,null,null,null,77,0.23099999999999998,0.12594780392156862,0.29418194650595925,0.16815122307053137,0.70976478033305579,0.70976478033305579,1,0.70976478033305579,1.1832751213976761E-6,5.1848451345395064E-2,801294.24806519644,1.2479810037506173E-6,0,6.6E-4,0.23383150671912883,9.2951195008714599E-3,0,9.3089639700764462E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,5.1879460560941476E-2,8.074435284282847E-6,8.074435284282847E-6,5.3244030385661223E-2,5.2446145276620485E-3,2.4038827441955892E-3,42.5,37.027299358721976,0.49112539760192114,0.29641476824427743,0.78994404859039413,0.79601226321928631,0.22541398436498125,3.8108598260472012E-2,6.4904834093280914E-3,1.282799440473888E-2,2.1373989835009456E-3,2.1455876797567917E-2,6.0015676772915728E-2,4.4899065126050422E-2,0.15696807866044882,8.8943661535236807E-3,1.0218903848061744,1.0312107136453714,0.76229999999999987,0.42503230909092221,3.3834281461069867E-3,2.149962065014583E-2,6.7445027658663892E-2,0.44044568152303154,7.1524492756809615E-3,1.1917402930683419E-3,1.1963060289703049E-2,5.1826395182099664E-3,0,4.502027906970951E-6,1.8346329415881097E-6,8.7520011710108994E-2,0.64578999572556806,0.42503230909092221,42.503230909092224,230.99999999999997,72.101220909974245,0.7210122090997424,801.29424806519648,null,0.16527069840681596,null,1.0218903848061744,0.15696807866044882,9.3089639700764462E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR83, IF(MODE_ILIM=4,#REF!,#REF!))","v":42.503230909092224},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ83, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0218903848061744},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA83, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15696807866044882},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB83, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.3089639700764462E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S83, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":801.29424806519648},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P83, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70976478033305579}]
[null,null,null,null,null,null,null,78,0.23399999999999999,0.12593592156862746,0.29718197003767782,0.171157164293604,0.70969781866034276,0.70969781866034276,1,0.70969781866034276,1.182234533739761E-6,5.1891719538370226E-2,801962.93832026713,1.2469404160927022E-6,0,6.6E-4,0.23679563664590189,9.5322695008714601E-3,0,9.5468299738618347E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,5.2556990529150402E-2,8.286711760443615E-6,8.286711760443615E-6,5.3941463670918968E-2,5.3829107804779812E-3,2.4058888149608012E-3,42.5,36.653081176058713,0.49501175733867464,0.29666213014343318,0.79407977629706861,0.80031257152096547,0.22836663867232768,3.9113491243873102E-2,6.4958998003941653E-3,1.3067740144627665E-2,2.1676948585200957E-3,2.1731334803541929E-2,6.1317974519948866E-2,4.4899065126050422E-2,0.15706160167952299,8.9017886153549657E-3,1.0275939363357924,1.037152343455251,0.77219999999999989,0.42678254613767436,3.4447658834621054E-3,2.187890040300821E-2,6.6910309430188511E-2,0.43887514732517208,7.2223302398208974E-3,1.1980501566546909E-3,1.2010559956521475E-2,5.2683323595602441E-3,0,4.5799325877119097E-6,1.8185699696618413E-6,8.6805426398922636E-2,0.6436202206558681,0.42678254613767436,42.678254613767436,234,72.109847935853821,0.72109847935853821,801.96293832026709,null,0.16396039788298439,null,1.0275939363357924,0.15706160167952299,9.5468299738618347E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR84, IF(MODE_ILIM=4,#REF!,#REF!))","v":42.678254613767436},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ84, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0275939363357924},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA84, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15706160167952299},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB84, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.5468299738618347E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S84, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":801.96293832026709},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P84, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70969781866034276}]
[null,null,null,null,null,null,null,79,0.23699999999999999,0.12592403921568626,0.3001819935693964,0.17416310551667663,0.7096308569876294,0.7096308569876294,1,0.7096308569876294,1.1811955788216299E-6,5.193499194706766E-2,802631.69372740923,1.2459014611745711E-6,0,6.6E-4,0.23976065885490472,9.7724795008714595E-3,0,9.7877836472797797E-3,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,5.3235237960405538E-2,8.5019716821030082E-6,8.5019716821030082E-6,5.4639656153676677E-2,5.5231602454952327E-3,2.4078950811822278E-3,42.5,36.286351419397448,0.49890395511750052,0.29690951614364319,0.79822136634232588,0.80462124918535582,0.23132250711902733,4.0132576724874337E-2,6.5013167191920159E-3,1.3307868920630603E-2,2.1980586861687144E-3,2.2007244325991333E-2,6.2635730347190555E-2,4.4899065126050422E-2,0.1571551338107659,8.9092118003742428E-3,1.0333213251436866,1.0431209011964848,0.78209999999999991,0.42849607928953193,3.5063607034275354E-3,2.2259489793572975E-2,6.638389928893669E-2,0.4373286355745043,7.2911004426406212E-3,1.2042699515044035E-3,1.2057304576977478E-2,5.3541352142446527E-3,0,4.6580508017028079E-6,1.8027592354372138E-6,8.6101980153605623E-2,0.64149363650945135,0.42849607928953193,42.849607928953191,237,72.116619551864289,0.72116619551864292,802.63169372740924,null,0.16267045591523221,null,1.0333213251436866,0.1571551338107659,9.7877836472797797E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR85, IF(MODE_ILIM=4,#REF!,#REF!))","v":42.849607928953191},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ85, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0333213251436866},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA85, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1571551338107659},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB85, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.7877836472797797E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S85, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":802.63169372740924},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P85, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.7096308569876294}]
[null,null,null,null,null,null,null,80,0.24,0.12591215686274507,0.30318201710111492,0.17716904673974926,0.70956389531491615,0.70956389531491615,1,0.70956389531491615,1.180158252803507E-6,5.197826857210347E-2,803300.51429614448,1.2448641351564482E-6,0,6.6E-4,0.2427265406471612,1.001574950087146E-2,0,1.0031825701393309E-2,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,5.3914195199062896E-2,8.7202213318879704E-6,8.7202213318879704E-6,5.5338600372785637E-2,5.6653672787549117E-3,2.4099015428884333E-3,42.5,35.926887540709757,0.50280199179166174,0.29715692624842976,0.8023688195829799,0.80893830780892795,0.234281558117553,4.1165886355491274E-2,6.5067341657987707E-3,1.3548380788730578E-2,2.2284905239851062E-3,2.2283605478514455E-2,6.3968997242073694E-2,4.4899065126050422E-2,0.15724867505550921,8.9166357086872036E-3,1.0390726158151979,1.0491164521717595,0.79199999999999993,0.43017376715403632,3.5682089626643434E-3,2.2641366174522875E-2,6.5865603175237347E-2,0.43580557798857045,7.3587853569767768E-3,1.2104017219314968E-3,1.2103311255640008E-2,5.4400412798750446E-3,0,4.7363768443879245E-6,1.7871948471611557E-6,8.5409412788648165E-2,0.63940923227575808,0.43017376715403632,43.017376715403636,240,72.121604042494241,0.72121604042494236,803.30051429614446,null,0.16140039696995098,null,1.0390726158151979,0.15724867505550921,1.0031825701393309E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR86, IF(MODE_ILIM=4,#REF!,#REF!))","v":43.017376715403636},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ86, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0390726158151979},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA86, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15724867505550921},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB86, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0031825701393309E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S86, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":803.30051429614446},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P86, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70956389531491615}]
[null,null,null,null,null,null,null,81,0.24299999999999999,0.12590027450980393,0.3061820406328335,0.18017498796282189,0.70949693364220323,0.70949693364220323,1,0.70949693364220323,1.1791225518576469E-6,5.2021549414093919E-2,803969.40003599692,1.2438284342105881E-6,0,6.6E-4,0.24569325089334057,1.0262079500871461E-2,0,1.027895685646299E-2,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,5.4593854942434836E-2,8.9414669924268499E-6,8.9414669924268499E-6,5.6038289212977613E-2,5.8095362371470482E-3,2.4119082001079909E-3,42.5,35.574475723984939,0.5067058682145873,0.29740436046131596,0.80652213687601115,0.81326375902488368,0.23724376154469737,4.2213451793907925E-2,6.5121521402915755E-3,1.3789275804921399E-2,2.2589904295187892E-3,2.2560418374731765E-2,6.5317828538359962E-2,4.4899065126050422E-2,0.15734222541508497,8.9240603403995672E-3,1.0448478733187281,1.0551390620760199,0.80189999999999995,0.43181644176269535,3.6303071306081946E-3,2.3024507689046059E-2,6.5355233020115019E-2,0.43430542380427073,7.425409667746085E-3,1.2164474488724111E-3,1.2148596567220853E-2,5.526043964524518E-3,0,4.8149051762169247E-6,1.7718710949820073E-6,8.4727472150849137E-2,0.63736602821952415,0.43181644176269535,43.181644176269536,243,72.124846875437001,0.72124846875436999,803.96940003599696,null,0.16014976019343496,null,1.0448478733187281,0.15734222541508497,1.027895685646299E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR87, IF(MODE_ILIM=4,#REF!,#REF!))","v":43.181644176269536},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ87, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0448478733187281},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA87, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15734222541508497},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB87, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.027895685646299E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S87, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":803.96940003599696},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P87, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70949693364220323}]
[null,null,null,null,null,"Eff (%)","Iout (mA)",82,0.24599999999999997,0.12588839215686273,0.30918206416455207,0.18318092918589446,0.70942997196949009,0.70942997196949009,1,0.70942997196949009,1.1780884721682863E-6,5.2064834473655452E-2,804638.35095649329,1.2427943545212275E-6,0,6.6E-4,0.24866075994120582,1.0511469500871458E-2,0,1.0529177841952246E-2,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,5.5274210220044813E-2,9.1657149463491199E-6,9.1657149463491199E-6,5.6738715884500412E-2,5.9556714784108102E-3,2.4139150528694796E-3,42.5,35.228910461122354,0.51061558523987283,0.29765181878582597,0.81068131907856822,0.8175976145032835,0.24020908865535834,4.3275304704478351E-2,6.5175706427475968E-3,1.4030554025207793E-2,2.2895584603305004E-3,2.283768312828589E-2,6.6682277918995586E-2,4.4899065126050422E-2,0.1574357848908256,8.9314856956170773E-3,1.0506471630087217,1.0611887969994567,0.81179999999999986,0.43342490958862656,3.692651785101567E-3,2.3408893241085634E-2,6.4852606515845318E-2,0.43282763910669747,7.4909973021113933E-3,1.2224090523116806E-3,1.2193176576855156E-2,5.6121368786139665E-3,0,4.8936304162804766E-6,1.7567824439827399E-6,8.4055913811678443E-2,0.63536307468316078,0.43342490958862656,43.342490958862655,245.99999999999997,72.126370778645395,0.72126370778645399,804.63835095649324,null,0.15891809884963895,null,1.0506471630087217,0.1574357848908256,1.0529177841952246E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR88, IF(MODE_ILIM=4,#REF!,#REF!))","v":43.342490958862655},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ88, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0506471630087217},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA88, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1574357848908256},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB88, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0529177841952246E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S88, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":804.63835095649324},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P88, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70942997196949009}]
[null,null,null,null,null,{"$f":"BT51","v":68.427867006324419},{"$f":"I56*1000","v":150},83,0.24899999999999997,0.12587650980392159,0.31218208769627065,0.18618687040896709,0.70936301029677706,0.70936301029677706,1,0.70936301029677706,1.1770560099316004E-6,5.2108123751404542E-2,805307.36706716113,1.2417618922845416E-6,0,6.6E-4,0.25162903952949861,1.0763919500871456E-2,0,1.0782489396532782E-2,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,5.5955254374321424E-2,9.3929714762850511E-6,9.3929714762850511E-6,5.7439873904169235E-2,6.1037773611346945E-3,2.4159221012014834E-3,42.5,34.889994152304176,0.51453114372128039,0.29789930122548419,0.81484636704796598,0.82193988595117196,0.24317751200231766,4.4351476757728013E-2,6.5229896732440064E-3,1.4272215505605394E-2,2.3201946739921922E-3,2.3115399852841594E-2,6.8062399418992461E-2,4.4899065126050422E-2,0.15752935348406361,8.9389117744454894E-3,1.0564705506286733,1.0672657234305187,0.82169999999999987,0.43499995251778545,3.7552396082251591E-3,2.3794502466949682E-2,6.4357546896975398E-2,0.43137170618857884,7.5555714582718134E-3,1.2282883935969605E-3,1.2237066859456882E-2,5.6983138271684908E-3,0,4.9725473362357445E-6,1.7419235275319321E-6,8.3394500773670582E-2,0.6333994509437576,0.43499995251778545,43.499995251778543,248.99999999999997,72.126175499523185,0.72126175499523182,805.30736706716118,null,0.15770497978357931,null,1.0564705506286733,0.15752935348406361,1.0782489396532782E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR89, IF(MODE_ILIM=4,#REF!,#REF!))","v":43.499995251778543},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ89, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0564705506286733},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA89, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15752935348406361},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB89, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0782489396532782E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S89, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":805.30736706716118},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P89, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70936301029677706}]
[null,null,null,null,null,{"$f":"BT81","v":72.078010752951272},{"$f":"I81*1000","v":224.99999999999997},84,0.252,0.1258646274509804,0.31518211122798923,0.18919281163203974,0.70929604862406381,0.70929604862406381,1,0.70929604862406381,1.1760251613556543E-6,5.215141724795784E-2,805976.44837753021,1.2407310437085955E-6,0,6.6E-4,0.25459806270774726,1.1019429500871461E-2,0,1.103889226809001E-2,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,5.6636981042617454E-2,9.6232428648654281E-6,9.6232428648654281E-6,5.8141757077721047E-2,6.2538582447567428E-3,2.4179293451325906E-3,42.5,34.557536729215833,0.51845254451273814,0.29814680778381597,0.81901728164168675,0.82629058511270581,0.24614900536153675,4.5441999630355383E-2,6.5284092318579953E-3,1.4514260302140754E-2,2.3508991280870397E-3,2.3393568662085789E-2,6.945824742833509E-2,4.4899065126050422E-2,0.1576229311961318,8.9463385769905854E-3,1.0623181023141632,1.0733699082589545,0.83160000000000001,0.43654232877622723,3.8180673823170752E-3,2.4181315708209829E-2,6.3869882731256558E-2,0.42993712293871705,7.619154632949582E-3,1.2340872776492526E-3,1.2280282518198052E-2,5.7845688024241067E-3,0,5.0516508545064529E-6,1.7272891409357147E-6,8.2743003190108716E-2,0.63147426412182572,0.43654232877622723,43.654232877622725,252,72.124237241864293,0.72124237241864297,805.97644837753023,null,0.15650998290902504,null,1.0623181023141632,0.1576229311961318,1.103889226809001E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR90, IF(MODE_ILIM=4,#REF!,#REF!))","v":43.654232877622725},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ90, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0623181023141632},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA90, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1576229311961318},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB90, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.103889226809001E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S90, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":805.97644837753023},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P90, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70929604862406381}]
[null,null,null,null,null,{"$f":"BT106","v":71.049894896969974},{"$f":"I106*1000","v":300},85,0.255,0.1258527450980392,0.3181821347597078,0.19219875285511237,0.70922908695135067,0.70922908695135067,1,0.70922908695135067,1.174995922660356E-6,5.2194714963932104E-2,806645.59489713248,1.2397018050132972E-6,0,6.600000000000001E-4,0.25756780376152993,1.1277999500871461E-2,0,1.1298387213728594E-2,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,5.7319384140449514E-2,9.8565353947212467E-6,9.8565353947212467E-6,5.8844359483369066E-2,6.4059184895647386E-3,2.4199367846913975E-3,42.5,34.231355299604552,0.52237978846834099,0.29839433846434721,0.82319406371737958,0.83064972376928059,0.24912354366253267,4.6546905005233369E-2,6.5338293186667732E-3,1.4756688470851351E-2,2.3816718802094428E-3,2.3672189669727568E-2,7.0869876694913431E-2,4.4899065126050429E-2,0.15771651802836337,8.9537661033581711E-3,1.0681898845959155,1.0795014187788752,0.84149999999999991,0.43805277381570967,3.8811319861701932E-3,2.4569313985821031E-2,6.338944771996971E-2,0.42852340225790159,7.6817686476419941E-3,1.2398074550738242E-3,1.2322838202157755E-2,5.8708959767664092E-3,0,5.1309360307431527E-6,1.7128742353749173E-6,8.2101198097302389E-2,0.62958664813907095,0.43805277381570967,43.805277381570967,255,72.120507778355574,0.72120507778355569,806.64559489713247,null,0.15533270071920502,null,1.0681898845959155,0.15771651802836337,1.1298387213728594E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR91, IF(MODE_ILIM=4,#REF!,#REF!))","v":43.805277381570967},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ91, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0681898845959155},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA91, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15771651802836337},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB91, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1298387213728594E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S91, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":806.64559489713247},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P91, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70922908695135067}]
[null,null,null,null,null,null,null,86,0.25800000000000001,0.12584086274509806,0.32118215829142638,0.195204694078185,0.70916212527863776,0.70916212527863776,1,0.70916212527863776,1.1739682900774127E-6,5.2238016899944159E-2,807314.80663550063,1.2386741724303539E-6,0,6.5999999999999989E-4,0.26053823814276861,1.1539629500871463E-2,0,1.1560974999778068E-2,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,5.8002457845863213E-2,1.0092855348483418E-5,1.0092855348483418E-5,5.9547675456463778E-2,6.5599624566964262E-3,2.4219444199065016E-3,42.5,33.911273811779225,0.5263128764423497,0.29864189327060436,0.82737671413286051,0.83501731373965926,0.25210110292343918,4.7666224571410856E-2,6.5392499337475554E-3,1.4999500067785573E-2,2.4125129879650265E-3,2.3951262989498158E-2,7.2297342327482195E-2,4.4899065126050408E-2,0.15781011398209155,8.9611943536540561E-3,1.0740859644028871,1.08566032269185,0.85139999999999993,0.43953200115980168,3.9444303913989285E-3,2.4958478975398948E-2,6.291608050715454E-2,0.42713007150086607,7.7434346737025768E-3,1.2454506241769798E-3,1.2364748123183954E-2,5.9572896959839295E-3,0,5.2103980605300972E-6,1.6986739121125675E-6,8.1468869158803262E-2,0.62773576272264187,0.43953200115980168,43.953200115980167,258,72.229662267470047,0.72229662267470052,807.31480663550064,null,0.15417273781933363,null,1.0740859644028871,0.15781011398209155,1.1560974999778068E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR92, IF(MODE_ILIM=4,#REF!,#REF!))","v":43.953200115980167},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ92, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0740859644028871},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA92, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15781011398209155},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB92, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1560974999778068E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S92, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":807.31480663550064},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P92, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70916212527863776}]
[null,null,null,null,null,null,null,87,0.26100000000000001,0.12582898039215687,0.32418218182314495,0.1982106353012576,0.70909516360592451,0.70909516360592451,1,0.70909516360592451,1.172942259850281E-6,5.2281323056611068E-2,807984.08360217104,1.2376481422032222E-6,0,6.6E-4,0.26350934240466317,1.1804319500871463E-2,0,1.182665640179848E-2,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,5.8686196584837202E-2,1.0332209008782473E-5,1.0332209008782473E-5,6.0251699575175018E-2,6.7159945081397198E-3,2.4239522508065132E-3,42.5,33.597122737758617,0.53025180928919269,0.29888947220611506,0.83156523374611424,0.83939336688010247,0.25508166019039025,4.8799990024114295E-2,6.5446710771775857E-3,1.5242695149002759E-2,2.4434225089706488E-3,2.4230788735150992E-2,7.3740699798646753E-2,4.4899065126050422E-2,0.15790371905865008,8.9686233279840984E-3,1.0800064090653834,1.0918466881100271,0.86129999999999995,0.44098070321253829,4.0079596589660963E-3,2.5348792983595256E-2,6.2449624497283335E-2,0.42575667194294703,7.8041732563120672E-3,1.251018432893558E-3,1.2406026072008983E-2,6.0437444728198971E-3,0,5.2900322703260405E-6,1.684683416957793E-6,8.0845806420943467E-2,0.62592079245345711,0.44098070321253829,44.098070321253829,261,72.361493645121143,0.72361493645121144,807.98408360217104,null,0.15302971047982938,null,1.0800064090653834,0.15790371905865008,1.182665640179848E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR93, IF(MODE_ILIM=4,#REF!,#REF!))","v":44.098070321253829},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ93, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0800064090653834},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA93, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15790371905865008},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB93, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.182665640179848E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S93, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":807.98408360217104},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P93, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70909516360592451}]
[null,null,null,null,null,null,null,88,0.26400000000000001,0.12581709803921567,0.32718220535486353,0.20121657652433023,0.70902820193321126,0.70902820193321126,1,0.70902820193321126,1.1719178282341254E-6,5.2324633434549891E-2,808653.42580668011,1.2366237105870667E-6,0,6.6E-4,0.26648109414091276,1.2072069500871462E-2,0,1.2095432204586157E-2,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,5.9370595017646743E-2,1.0574602658248261E-5,1.0574602658248261E-5,6.0956426647116924E-2,6.8740190067328906E-3,2.4259602774200405E-3,42.5,33.288738773869582,0.53419658786346391,0.29913707527440708,0.83575962341529109,0.84377789508449419,0.25806519348089546,4.9948233064749006E-2,6.5500927490341095E-3,1.5486273770573149E-2,2.474400500854396E-3,2.4510767020461656E-2,7.5200004947875806E-2,4.4899065126050422E-2,0.15799733325937271,8.9760530264541491E-3,1.085951286318197,1.0980605835592778,0.87119999999999997,0.44239955203154324,4.0717169358616481E-3,2.5740238925514615E-2,6.198992768094564E-2,0.4244027582701746,7.8640043373960043E-3,1.256512480629719E-3,1.244668543365675E-2,6.1302549808071524E-3,0,5.3698341126269483E-6,1.6708981349729789E-6,8.023180607911494E-2,0.62414094585634861,0.44239955203154324,44.239955203154324,264,72.477313046906502,0.724773130469065,808.65342580668016,null,0.15190324620916407,null,1.085951286318197,0.15799733325937271,1.2095432204586157E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR94, IF(MODE_ILIM=4,#REF!,#REF!))","v":44.239955203154324},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ94, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.085951286318197},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA94, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15799733325937271},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB94, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.2095432204586157E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S94, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":808.65342580668016},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P94, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70902820193321126}]
[null,null,null,null,null,null,null,89,0.26700000000000002,0.12580521568627451,0.33018222888658211,0.20422251774740285,0.70896124026049812,0.70896124026049812,1,0.70896124026049812,1.1708949914957693E-6,5.2367948034377894E-2,809322.83325856738,1.2356008738487105E-6,0,6.6E-4,0.26945347192889907,1.234287950087146E-2,0,1.2367303202179498E-2,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,6.0055648026114482E-2,1.0820042579509645E-5,1.0820042579509645E-5,6.1661851696844752E-2,7.034040316164801E-3,2.4279684997757021E-3,42.5,32.985964557684412,0.5381472130199243,0.29938470247900922,0.83995988399870924,0.84817091028447389,0.26105168173090659,5.1110985400900914E-2,6.5555149493943966E-3,1.573023598857794E-2,2.5054470212555937E-3,2.4791197959227934E-2,7.667531398454154E-2,4.4899065126050422E-2,0.15809095658559366,8.9834834491700991E-3,1.0919206643037791,1.1043020779823745,0.88109999999999999,0.44378920006742434,4.1356994519260995E-3,2.613280030312037E-2,6.1536842468137058E-2,0.42306789809160561,7.9229472775426326E-3,1.2619343200253445E-3,1.2486739202177877E-2,6.2168160483717571E-3,0,5.4497991613392991E-6,1.6573135854117951E-6,7.962667025424415E-2,0.62239545452989764,0.44378920006742434,44.378920006742433,267,72.230234640211876,0.72230234640211877,809.32283325856736,null,0.15079298334534483,null,1.0919206643037791,0.15809095658559366,1.2367303202179498E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR95, IF(MODE_ILIM=4,#REF!,#REF!))","v":44.378920006742433},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ95, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0919206643037791},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA95, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15809095658559366},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB95, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.2367303202179498E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S95, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":809.32283325856736},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P95, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70896124026049812}]
[null,null,null,null,null,null,null,90,0.27,0.12579333333333334,0.33318225241830068,0.20722845897047548,0.70889427858778509,0.70889427858778509,1,0.70889427858778509,1.1698737459136514E-6,5.24112668567124E-2,809992.30596737342,1.2345796282665926E-6,0,6.600000000000001E-4,0.27242645527653514,1.2616749500871462E-2,0,1.2642270197864871E-2,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,6.0741350701682101E-2,1.106853505519421E-5,1.106853505519421E-5,6.2367969954157942E-2,7.1960628009750845E-3,2.4299769179021201E-3,42.5,32.688648400266274,0.54210368561350164,0.29963235382345077,0.84416601635485455,0.8525724244495656,0.26404110474529752,5.2288278746337881E-2,6.5609376783357255E-3,1.5974581859109237E-2,2.5365621278248011E-3,2.5072081665269762E-2,7.8166683490986988E-2,4.4899065126050429E-2,0.15818458903864729,8.9909145962378464E-3,1.0979146115754379,1.1105712407421944,0.89100000000000001,0.445150280871148,4.1999045168104546E-3,2.6526461184578888E-2,6.1090225528767035E-2,0.42175167147277398,7.9810208769715181E-3,1.2672854586400976E-3,1.2526199994746572E-2,6.3034226531917485E-3,0,5.5299231073533672E-6,1.6439254168764359E-6,7.903020677894608E-2,0.62068357231395055,0.445150280871148,44.5150280871148,270,72.8349974854723,0.72834997485472297,809.99230596737345,null,0.14969857066508677,null,1.0979146115754379,0.15818458903864729,1.2642270197864871E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR96, IF(MODE_ILIM=4,#REF!,#REF!))","v":44.5150280871148},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ96, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0979146115754379},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA96, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15818458903864729},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB96, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.2642270197864871E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S96, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":809.99230596737345},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P96, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70889427858778509}]
[null,null,null,null,null,null,null,91,0.27300000000000002,0.12578145098039215,0.33618227595001926,0.21023440019354811,0.70882731691507184,0.70882731691507184,1,0.70882731691507184,1.1688540877777799E-6,5.2454589902170917E-2,810661.8439426414,1.2335599701307211E-6,0,6.6E-4,0.27540002457250801,1.2893679500871462E-2,0,1.2920334004182524E-2,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,6.1427698334242178E-2,1.1320086367927978E-5,1.1320086367927978E-5,6.3074776843150049E-2,7.3600908265543793E-3,2.4319855318279239E-3,42.5,32.396644032765629,0.54606600649929027,0.2998800293112619,0.84837802134238005,0.85698244958730885,0.26703344315150568,5.3480144821011308E-2,6.5663609359353963E-3,1.6219311438270104E-2,2.5677458782238224E-3,2.5353418252429323E-2,7.9674170425621707E-2,4.4899065126050422E-2,0.15827823061986829,8.9983464677633202E-3,1.1039331971005624,1.1168681416249491,0.90090000000000003,0.44648340977099932,4.2643295170670488E-3,2.6921206184495901E-2,6.064993764002443E-2,0.42045367048919907,8.0382433956006291E-3,1.2725673605669902E-3,1.2565080065151443E-2,6.3900699167982319E-3,0,5.6102017543064611E-6,1.6307294026830777E-6,7.8442228992873106E-2,0.619004574492934,0.44648340977099932,44.648340977099934,273,73.305168165960453,0.73305168165960455,810.66184394264144,null,0.14861966700978957,null,1.1039331971005624,0.15827823061986829,1.2920334004182524E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR97, IF(MODE_ILIM=4,#REF!,#REF!))","v":44.648340977099934},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ97, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1039331971005624},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA97, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15827823061986829},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB97, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.2920334004182524E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S97, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":810.66184394264144},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P97, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70882731691507184}]
[null,null,null,null,null,null,null,92,0.27600000000000002,0.12576956862745098,0.33918229948173784,0.21324034141662074,0.70876035524235881,0.70876035524235881,1,0.70876035524235881,1.1678360133896889E-6,5.2497917171370999E-2,811331.44719391537,1.2325418957426301E-6,0,6.6E-4,0.27837416103966617,1.317366950087146E-2,0,1.3201495442932653E-2,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,6.2114686401674377E-2,1.1574702800335055E-5,1.1574702800335055E-5,6.3782267971950357E-2,7.5261287591445163E-3,2.433994341581746E-3,42.5,32.1098103664782,0.55003417653255082,0.30012772894597317,0.85259589982010575,0.86140099774338807,0.2700286783561025,5.4686615351057594E-2,6.5717847222707144E-3,1.6464424782174532E-2,2.5989983301257001E-3,2.5635207834570944E-2,8.1197832126045033E-2,4.4899065126050422E-2,0.15837188133059144,9.00577906385246E-3,1.1099764902638769,1.1231928508434463,0.91080000000000005,0.4477891845206407,4.3289719133629539E-3,2.7317020444999913E-2,6.0215843540258579E-2,0.41917349879895366,8.0946325722566544E-3,1.2777814479770467E-3,1.2603391316710214E-2,6.4767530994067485E-3,0,5.6906310145265812E-6,1.6177214364251752E-6,7.7862555546799758E-2,0.61735775703317652,0.4477891845206407,44.778918452064069,276,73.638455592594738,0.73638455592594743,811.33144719391532,null,0.14755594092748048,null,1.1099764902638769,0.15837188133059144,1.3201495442932653E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR98, IF(MODE_ILIM=4,#REF!,#REF!))","v":44.778918452064069},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ98, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1099764902638769},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA98, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15837188133059144},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB98, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.3201495442932653E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S98, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":811.33144719391532},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P98, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70876035524235881}]
[null,null,null,null,null,null,null,93,0.27900000000000003,0.12575768627450981,0.34218232301345641,0.21624628263969334,0.70869339356964567,0.70869339356964567,1,0.70869339356964567,1.1668195190623907E-6,5.2541248664930394E-2,812001.11573074246,1.2315254014153319E-6,0,6.6E-4,0.28134884669132382,1.3456719500871466E-2,0,1.3485755345181464E-2,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,6.2802310560035421E-2,1.183239063503741E-5,1.183239063503741E-5,6.4490439123107299E-2,7.6941809658387355E-3,2.4360033471922272E-3,42.5,31.82801126553743,0.55400819656871159,0.30037545273111621,0.85681965264701998,0.865828081001767,0.27302679250408052,5.5907722068799674E-2,6.5772090374190146E-3,1.6709921946947461E-2,2.6303195412147283E-3,2.5917450525581202E-2,8.2737726312198473E-2,4.4899065126050422E-2,0.15846554117215206,9.0132123846112418E-3,1.1160445608707286,1.1295454390403814,0.92070000000000007,0.4490681859196986,4.3938292378123385E-3,2.7713889617631361E-2,5.9787811789054089E-2,0.41791077123334802,8.1502056430709825E-3,1.2829291025984923E-3,1.2641145314637003E-2,6.5634675949675049E-3,0,5.7712069051476928E-6,1.6048975277248206E-6,7.7291010215012085E-2,0.61574243585256483,0.4490681859196986,44.906818591969859,279,73.832411821820315,0.73832411821820321,812.00111573074241,null,0.14650707032993432,null,1.1160445608707286,0.15846554117215206,1.3485755345181464E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR99, IF(MODE_ILIM=4,#REF!,#REF!))","v":44.906818591969859},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ99, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1160445608707286},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA99, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15846554117215206},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB99, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.3485755345181464E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S99, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":812.00111573074241},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P99, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70869339356964567}]
[null,null,null,null,null,null,null,94,0.28199999999999997,0.12574580392156862,0.34518234654517488,0.21925222386276591,0.70862643189693253,0.70862643189693253,1,0.70862643189693253,1.1658046011203348E-6,5.2584584383466935E-2,812670.8495626708,1.230510483473276E-6,0,6.6E-4,0.28432406429027068,1.3742829500871455E-2,0,1.37731145512673E-2,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,6.3490566634355247E-2,1.2093156154654512E-5,1.2093156154654512E-5,6.5199286244567306E-2,7.8642518145818942E-3,2.4380125486880124E-3,42.5,31.551115331472079,0.55798806746336693,0.30062320067022313,0.86104928068227804,0.8702637114848174,0.27602776844066129,5.7143496712748501E-2,6.5826338814576344E-3,1.6955802988724768E-2,2.6617095691864466E-3,2.6200146439368847E-2,8.4293911089546383E-2,4.4899065126050422E-2,0.15855921014588559,9.0206464301456468E-3,1.1221374791503951,1.1359259772916535,0.93059999999999987,0.45032097840822943,4.4588990914189277E-3,2.8111799845997598E-2,5.9365714633195045E-2,0.41666511340484169,8.204979359101354E-3,1.288011667133664E-3,1.2678353297888963E-2,6.6502089264237202E-3,0,5.8519255443880531E-6,1.5922537981629307E-6,7.672742171559345E-2,0.61415794612093688,0.45032097840822943,45.032097840822942,282,73.8844086186851,0.73884408618685105,812.67084956267081,null,0.14547274216422565,null,1.1221374791503951,0.15855921014588559,1.37731145512673E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR100, IF(MODE_ILIM=4,#REF!,#REF!))","v":45.032097840822942},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ100, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1221374791503951},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA100, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15855921014588559},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB100, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.37731145512673E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S100, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":812.67084956267081},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P100, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70862643189693253}]
[null,null,null,null,null,null,null,95,0.28499999999999998,0.12573392156862745,0.34818237007689345,0.22225816508583854,0.70855947022421939,0.70855947022421939,1,0.70855947022421939,1.1647912558993616E-6,5.2627924327598566E-2,813340.64869925054,1.2294971382523028E-6,0,6.600000000000001E-4,0.28729979731029742,1.4031999500871457E-2,0,1.4063573910806962E-2,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,6.4179450609996788E-2,1.2357005641803052E-5,1.2357005641803052E-5,6.5908805441206766E-2,8.0363456741706658E-3,2.4400219460977515E-3,42.5,31.278995698912606,0.56197379007227832,0.30087097276682673,0.86528478478520277,0.87470790135345333,0.27903158967544545,5.8393971027604616E-2,6.5880592544639311E-3,1.7202067963653284E-2,2.6931684717476471E-3,2.648329568986486E-2,8.5866444952286222E-2,4.4899065126050429E-2,0.15865288825312762,9.0280812005616821E-3,1.1282553157594288,1.142334537109714,0.94049999999999989,0.45154811063633649,4.524179141626266E-3,2.8510737749156752E-2,5.8949427878231542E-2,0.41543616133134226,8.2589700032168981E-3,1.2930304466166932E-3,1.2715026190517717E-2,6.736972741168021E-3,0,5.9327831479837527E-6,1.5797864773795386E-6,7.6171623538221808E-2,0.61260364158972325,0.45154811063633649,45.154811063633652,285,73.791636151568156,0.73791636151568152,813.34064869925055,null,0.14445265209800881,null,1.1282553157594288,0.15865288825312762,1.4063573910806962E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR101, IF(MODE_ILIM=4,#REF!,#REF!))","v":45.154811063633652},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ101, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1282553157594288},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA101, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15865288825312762},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB101, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.4063573910806962E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S101, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":813.34064869925055},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P101, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70855947022421939}]
[null,null,null,null,null,null,null,96,{"$f":"IF(PLOT_TYPE=1, H102/100*Iout, min_I*EXP(H102*rr/100))","v":0.28799999999999998},{"$f":"IF(I102<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I102-Vout)/L*OnTime)","v":0.12572203921568625},{"$f":"IF(I102<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I102+((Vin-(Rdcr+RdsonTop)*J102-Vout)/L*OnTime)/2)","v":0.35118239360861203},{"$f":"IF(I102<Icrit, 0, I102-((Vin-(Rdcr+RdsonTop)*K102-Vout)/L*OnTime)/2)","v":0.22526410630891114},0.70849250855150614,{"$f":"IF(I102<Icrit, 1000*SQRT((J102*CoutEsr)^2+(((J102/2)-I102)*(OnTime+OffTime)/Cout)^2), 1000*J102*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":0.70849250855150614},1,{"$f":"IF(I102<Icrit, 1000*((N102/1000)*O102), 1000*J102*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":0.70849250855150614},1.1637794797466585E-6,5.2671268497943353E-2,814010.51315003366,1.2284853620995997E-6,0,{"$f":"S102*(T102*Iq_active+U102*Iq_sleep)","v":6.6E-4},0.29027602990005563,{"$f":"W102^2*Rdcr","v":1.432422950087146E-2},{"$f":"Core_Loss/1000*S102/$S$106","v":0},{"$f":"(Y102+X102*(1+Ltc*(Ta-25)))/(1-X102*Ltc*ThetaCa)","v":1.4357134282701899E-2},3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,6.4868958624539522E-2,1.2623945379096661E-5,1.2623945379096661E-5,6.6618992966878079E-2,8.2104669142537591E-3,2.4420315394501008E-3,42.5,31.011529841779044,{"$f":"IF(I102<Icrit, Vin*(I102+Iripple/2)*AK102/1000000000/2*S102, Vin*(I102-Iripple/2)*AJ102/1000000000/2*S102 + Vin*(I102+Iripple/2)*AK102/1000000000/2*S102)","v":0.56596536525137431},0.30111876902446044,0.86952616581528486,{"$f":"(AI102+AL102+AM102+AH102*(1+RdsonTopTc*(Ta-25)))/(1-AH102*RdsonTopTc*ThetaJA)","v":0.87916066280726379},0.28203824034873842,5.965917676425956E-2,6.5934851565152735E-3,{"$f":"IF(I102<Icrit, Vin*Idss*R102, QrrBot*(I102-Iripple/2)/1*S102*Vin+Vin*Idss*R102)","v":1.7448716927890788E-2},2.7246963066163755E-3,2.6766898391022437E-2,{"$f":"(AR102+AS102+AT102+AQ102*(1+RdsonBotTc*(Ta-25)))/(1-AQ102*RdsonBotTc*ThetaJA)","v":8.7455386786587874E-2},{"$f":"Vin*V102+Vout*Ifb/0.8","v":4.4899065126050422E-2},{"$f":"(Vin-Vdd)*(S102*QgBot+S102*QgTop)+AW102","v":0.15874657549521415},9.0355166959653743E-3,1.1343981417850313,{"$f":"SUM(Z102,AC102,AF102,AZ102)","v":1.1487711904469486},0.95039999999999991,0.45275011601014015,4.5896671199682345E-3,2.8910690405694758E-2,5.8538830765377102E-2,0.41422356107609698,8.3121934062822499E-3,1.2979867097148196E-3,1.2751174612549498E-2,6.8237548066871065E-3,0,6.0137760257698713E-6,1.5674918993359512E-6,7.562345377911478E-2,0.61107889394941051,0.45275011601014015,45.275011601014015,288,73.551124384272143,0.73551124384272137,814.0105131500336,null,0.14344650421786098,null,1.1343981417850313,0.15874657549521415,1.4357134282701899E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR102, IF(MODE_ILIM=4,#REF!,#REF!))","v":45.275011601014015},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ102, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1343981417850313},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA102, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15874657549521415},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB102, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.4357134282701899E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S102, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":814.0105131500336},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P102, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70849250855150614}]
[null,null,null,null,null,null,null,97,{"$f":"IF(PLOT_TYPE=1, H103/100*Iout, min_I*EXP(H103*rr/100))","v":0.29099999999999998},0.12571015686274511,0.35418241714033061,0.22827004753198377,0.70842554687879311,0.70842554687879311,1,0.70842554687879311,1.162769269020716E-6,5.2714616895119519E-2,814680.44292457437,{"$f":"IF(1/S103-OnTime-Q103>Tsleep, OnTime+Q103+Tsleep, 1/S103)","v":1.2274751513736572E-6},0,6.6E-4,0.29325274684909258,1.4619519500871458E-2,0,1.4653796535144634E-2,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,6.5559086960150087E-2,1.2893981649145565E-5,1.2893981649145565E-5,6.7329845216933942E-2,{"$f":"RdsonTop*AG103^2","v":8.3866199053321232E-3},2.4440413287737228E-3,42.5,30.748599389328206,0.56996279385674986,0.30136658944665851,0.87377342463218211,0.88362200808464531,0.28504770519990141,{"$f":"RdsonBot*AP103^2","v":6.0939145679797427E-2},6.5989115876890526E-3,1.7695749937606017E-2,2.7562931315219356E-3,2.7050954656817006E-2,8.9060795873863244E-2,4.4899065126050422E-2,0.15884027187348138,9.0429529164627754E-3,1.1405660287484529,1.155236009699083,0.96029999999999993,0.45392751321524161,4.6553608198160986E-3,2.9311645338462762E-2,5.81338058534807E-2,0.41302696840242814,8.364664962674441E-3,1.3028816899760525E-3,1.2786808890416747E-2,6.9105510063858285E-3,0,6.0949005784021722E-6,1.5553664987309922E-6,7.5082754982778596E-2,0.60958309221349649,0.45392751321524161,45.392751321524159,291,73.159788011658193,0.73159788011658189,814.68044292457432,null,0.14245401074006078,null,1.1405660287484529,0.15884027187348138,1.4653796535144634E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR103, IF(MODE_ILIM=4,#REF!,#REF!))","v":45.392751321524159},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ103, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1405660287484529},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA103, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15884027187348138},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB103, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.4653796535144634E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S103, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":814.68044292457432},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P103, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70842554687879311}]
[null,null,null,null,null,null,null,98,{"$f":"IF(PLOT_TYPE=1, H104/100*Iout, min_I*EXP(H104*rr/100))","v":0.29399999999999998},0.12569827450980392,0.35718244067204918,0.23127598875505639,0.70835858520607997,0.70835858520607997,1,0.70835858520607997,1.1617606200912847E-6,5.2757969519745367E-2,815350.43803242838,{"$f":"IF(1/S104-OnTime-Q104>Tsleep, OnTime+Q104+Tsleep, 1/S104)","v":1.2264665024442259E-6},0,6.6E-4,0.29622993355590854,1.4917869500871459E-2,0,1.4953561545625202E-2,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,6.6249832036406789E-2,1.3167120734556334E-5,1.3167120734556334E-5,6.804135872119664E-2,{"$f":"RdsonTop*AG104^2","v":8.5648090187591414E-3},2.4460513140972854E-3,42.5,30.490089951480048,0.57396607674466749,0.30161443403695587,0.87802656209572061,0.88809194946293724,0.28805996953758645,{"$f":"RdsonBot*AP104^2","v":6.2233909537496426E-2},6.6043385480626712E-3,1.794316704897865E-2,2.7879590042048908E-3,2.7335464601246213E-2,9.0682731894065713E-2,4.4899065126050422E-2,0.15893397738926587,9.050389862159957E-3,1.1467590486084287,1.1617290677086247,0.97019999999999984,0.45508080671875301,4.7212580942173664E-3,2.9713590499943085E-2,5.7734238905831056E-2,0.41184604844260347,8.4163996451644529E-3,1.3077165870257403E-3,1.2821939066962528E-2,6.9973573355820102E-3,0,6.1761532942126549E-6,1.5434068075639691E-6,7.4549373990236215E-2,0.60811564212766778,0.45508080671875301,45.508080671875298,294,72.614496083320674,0.72614496083320679,815.35043803242843,null,0.1414748917332076,null,1.1467590486084287,0.15893397738926587,1.4953561545625202E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR104, IF(MODE_ILIM=4,#REF!,#REF!))","v":45.508080671875298},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ104, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1467590486084287},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA104, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15893397738926587},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB104, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.4953561545625202E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S104, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":815.35043803242843},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P104, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70835858520607997}]
[null,null,null,null,null,null,null,99,{"$f":"IF(PLOT_TYPE=1, H105/100*Iout, min_I*EXP(H105*rr/100))","v":0.29699999999999999},0.12568639215686273,0.36018246420376776,0.23428192997812902,0.70829162353336672,0.70829162353336672,1,0.70829162353336672,1.1607535293393308E-6,5.2801326372439353E-2,816020.49848315364,{"$f":"IF(1/S105-OnTime-Q105>Tsleep, OnTime+Q105+Tsleep, 1/S105)","v":1.225459411692272E-6},0,6.6E-4,0.29920757599789816,1.5219279500871461E-2,0,1.5256430200937638E-2,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,6.6941190403546402E-2,1.344336891793156E-5,1.344336891793156E-5,6.8753530137342117E-2,{"$f":"RdsonTop*AG105^2","v":8.7450386267408607E-3},2.448061495449461E-3,42.5,30.23589095288175,0.57797521477155689,0.30186230279888815,0.88228557906589455,0.89257049925855514,0.29107501921172674,{"$f":"RdsonBot*AP105^2","v":6.3543500106830325E-2},6.6097660377135454E-3,1.8190968318199351E-2,2.8196939824170677E-3,2.7620428338329964E-2,9.2321254929020213E-2,4.4899065126050422E-2,0.1590276920439043,9.057827533163006E-3,1.1529772737646427,1.1682504377683345,0.98009999999999986,0.45621048725091107,4.7873568538214671E-3,3.0116514258213965E-2,5.7340018781563695E-2,0.41068047538016939,8.4674120191935657E-3,1.3124925677144704E-3,1.2856574911038044E-2,7.0841698976638846E-3,0,6.2575307461925426E-6,1.5316094518374002E-6,7.4023161793426606E-2,0.60667596560300319,0.45621048725091107,45.621048725091107,297,71.912167665597565,0.71912167665597559,816.02049848315369,null,0.14050887485212002,null,1.1529772737646427,0.1590276920439043,1.5256430200937638E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR105, IF(MODE_ILIM=4,#REF!,#REF!))","v":45.621048725091107},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ105, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1529772737646427},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA105, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1590276920439043},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB105, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.5256430200937638E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S105, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":816.02049848315369},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P105, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70829162353336672}]
[null,null,null,null,null,null,null,100,{"$f":"IF(PLOT_TYPE=1, H106/100*Iout, min_I*EXP(H106*rr/100))","v":0.3},0.12567450980392159,0.36318248773548634,0.23728787120120165,0.7082246618606538,0.7082246618606538,1,0.7082246618606538,1.1597479931569948E-6,5.284468745381999E-2,816690.62428630888,{"$f":"IF(1/S106-OnTime-Q106>Tsleep, OnTime+Q106+Tsleep, 1/S106)","v":1.224453875509936E-6},0,6.6E-4,0.30218566070304859,1.5523749500871461E-2,0,1.5562403397186571E-2,3.6279106032784197E-2,3.2904338363449972E-6,3.2904338363449972E-6,6.7633158736105009E-2,1.3722732481869531E-5,1.3722732481869531E-5,6.9466356244670333E-2,{"$f":"RdsonTop*AG106^2","v":8.9273131023361822E-3},2.4500718728589269E-3,42.5,29.985895475203591,0.58199020879401342,0.30211019573599135,0.88655047640286377,0.89705766982712454,0.29409284058716312,{"$f":"RdsonBot*AP106^2","v":6.4867949163469912E-2},6.615194056719103E-3,1.8439153801469692E-2,2.8514981239215549E-3,2.790584598211035E-2,9.397642546578415E-2,4.4899065126050422E-2,0.1591214158387336,9.0652659295780303E-3,1.1592207770612202,1.174800193624725,0.98999999999999988,0.45731703226723736,4.8536550648896606E-3,3.0520405383485175E-2,5.6951037331454304E-2,0.40952993214511429,8.5177162565729988E-3,1.3172107672195965E-3,1.289072592671244E-2,7.1709849004025694E-3,0,6.3390295890967628E-6,1.519971148392924E-6,7.3503973395485492E-2,{"$f":"SUM(BD106:BO106)","v":0.6052635001720742},0.45731703226723736,45.731703226723738,300,71.049894896969974,0.71049894896969978,816.69062428630889,null,0.13955569508248258,null,1.1592207770612202,0.1591214158387336,1.5562403397186571E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR106, IF(MODE_ILIM=4,#REF!,#REF!))","v":45.731703226723738},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ106, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1592207770612202},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA106, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1591214158387336},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB106, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.5562403397186571E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S106, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":816.69062428630889},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P106, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.7082246618606538}]
[null,null,null,null,null,null,null,null,{"$f":"Losses!$E$5/1000","v":0.5},0.12488235294117646,0.56318405651672432,0.43768395273937627,0.7037605503464448,0.7037605503464448,1,0.7037605503464448,{"$f":"IF(I107<Icrit, L*J107/(Vout+J107/2*(RdsonBot+Rdcr)), L*J107/(Vout+I107*(RdsonBot+Rdcr)))","v":1.0960419274092617E-6},{"$f":"OnTime*S107","v":5.5744996293550772E-2},{"$f":"IF(I107<Icrit,I107/((OnTime+Q107)*J107/2),1/(OnTime+Q107))","v":861513.57908214827},{"$f":"IF(1/S107-OnTime-Q107>Tsleep, OnTime+Q107+Tsleep, 1/S107)","v":1.1607478097622029E-6},{"$f":"IF(1/S107-OnTime-Q107>Tsleep, 1/S107-OnTime-Q107-Tsleep, 0)","v":0},6.6E-4,{"$f":"IF(I107<Icrit,Iripple*SQRT((OnTime+OffTime)*S107/3), SQRT(I107^2+Iripple^2/12))","v":0.50131444576686401},4.2723749500871475E-2,0,4.301781064745995E-2,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q107)*S107)","v":3.6279106032784197E-2},{"$f":"RCoutEsr*AA107^2","v":3.2904338363449972E-6},{"$f":"AB107","v":3.2904338363449972E-6},{"$f":"SQRT($R107)*SQRT($I107^2*(1-R107)+(Iripple^2)/12)","v":0.11503366033144466},{"$f":"RCinEsr*AD107^2","v":3.9698229027750553E-5},{"$f":"AE107","v":3.9698229027750553E-5},{"$f":"IF(I107<Icrit,Iripple*SQRT((OnTime)*S107/3), SQRT(OnTime*S107*(I107^2+Iripple^2/12)))","v":0.11836223706145547},{"$f":"RdsonTop*AG107^2","v":2.5917795450055542E-2},{"$f":"QgTop*S107*Vdd","v":2.5845407372464446E-3},42.5,{"$f":"IF(I107<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I107+Iripple/2)*1000000000)","v":19.33063226579619},0.86290937466585771,{"$f":"IF(I107<Icrit, Csw*(Vin)^2*S107/2, Csw*Vin^2*S107/2)","v":0.31869110317406824},1.1841850185771725,1.216321944375649,{"$f":"IF(I107<Icrit,Iripple*SQRT((OffTime)*S107/3), SQRT(OffTime*S107*(I107^2+Iripple^2/12)))","v":0.50109849425599207},{"$f":"RdsonBot*AP107^2","v":0.18832477570921688},{"$f":"QgBot*S107*Vdd","v":6.978259990565402E-3},3.5854380239459076E-2,{"$f":"IF(I107<Icrit, dead1*S107*(I107+Iripple/2)*((I107+Iripple/2)*BDserR+VSD), dead1*S107*(I107+Iripple/2)*((I107+Iripple/2)*BDserR+VSD)+dead2*S107*(I107-Iripple/2)*((I107-Iripple/2)*BDserR+VSD))","v":5.1307681813030012E-3},4.7963408411327478E-2,0.24540567024961357,4.4899065126050422E-2,0.16539035429647969,{"$f":"AI107+AR107","v":9.562800727811847E-3},{"$f":"AO107+AV107+AX107+AY107","v":1.636680769649554},1.679741568959878,{"$f":"Vout*I107","v":1.65},{"$f":"BB107/(BB107+BA107)","v":0.49553395235877595},9.6514774894422839E-3,5.9296572346292258E-2,{"$f":"Vin*S107*(QgBot+QgTop)/($BB107+$BA107)","v":3.9058313447090286E-2},0.35563871671490715,{"$f":"AS107/(BA107+BB107)","v":1.0767916817838516E-2},{"$f":"AT107/($BB107+$BA107)","v":1.5408908094046818E-3},1.44045438416141E-2,{"$f":"X107/($BB107+$BA107)","v":1.2830950575607954E-2},{"$f":"Y107/($BB107+$BA107)","v":0},{"$f":"(AF107)/($BB107+$BA107)","v":1.192231535258492E-5},{"$f":"(AC107)/($BB107+$BA107)","v":9.8819495993884025E-7},4.9670627846395664E-2,{"$f":"SUM(BD107:BO107)","v":0.55287292039890545},{"$f":"BC107","v":0.49553395235877595},{"$f":"100*BQ107","v":49.553395235877595},{"$f":"I107*1000","v":500},72.049894896970002,{"$f":"BT107/100","v":0.72049894896970001},{"$f":"S107/1000","v":861.51357908214823},null,{"$f":"AM107/($BB107+$BA107)","v":9.5710461780257258E-2},null,1.636680769649554,0.16539035429647969,4.301781064745995E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR107, IF(MODE_ILIM=4,#REF!,#REF!))","v":49.553395235877595},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ107, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.636680769649554},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA107, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16539035429647969},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB107, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.301781064745995E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S107, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":861.51357908214823},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P107, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.7037605503464448}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BD107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":9.6514774894422839E-3},{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BE107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":5.9296572346292258E-2},null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BG107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":0.35563871671490715},null,null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BJ107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":1.44045438416141E-2},{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BK107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":1.2830950575607954E-2},{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BL107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":0},null,null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BO107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":4.9670627846395664E-2}]
[null,null,null,null,null,null,null,1.0000000000000001E-5,"A","min_I",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Load (A)","High-side MOSFET Rdson %","Low-side MOSFET Rdson %","Gate Drive (Qg) Loss from Vin %","High-side MOSFET Switching Loss %","Reverse Recovery & Leakage Loss %","Deadtime Loss %",null,"Inductor Cu Loss %","Inductor Core Loss %","Cin ESR %","Cout ESR %","Quiescent Current Loss %","Total Loss %","Overall Eff %"]
[null,null,null,null,null,null,null,{"$f":"Iout","v":0.3},"A","max_I",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"I107","v":0.5},{"$f":"BD107","v":9.6514774894422839E-3},{"$f":"BE107","v":5.9296572346292258E-2},3.9058313447090286E-2,0.35563871671490715,1.0767916817838516E-2,1.5408908094046818E-3,null,1.2830950575607954E-2,0,1.192231535258492E-5,9.8819495993884025E-7,4.9670627846395664E-2,0.55287292039890545,0.49553395235877595]
[null,null,null,null,null,null,null,{"$f":"LOG(max_I/min_I,EXP(1))","v":10.308952660644293},null,"rr",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10mA",{"$f":"BD70","v":2.6113263840268474E-3},{"$f":"BE70","v":1.6700117754916838E-2},7.5253247650108171E-2,0.46334393990481237,6.1296767845237642E-3,1.10045289053448E-3,null,4.0821801511671555E-3,0,3.5116401386103263E-6,2.0694670206723219E-6,9.7958487067140693E-2,0.6784529726098153,0.39849283392808638]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"50ma",{"$f":"BD85","v":3.5063607034275354E-3},{"$f":"BE85","v":2.2259489793572975E-2},6.638389928893669E-2,0.4373286355745043,7.2911004426406212E-3,1.2042699515044035E-3,null,5.3541352142446527E-3,0,4.6580508017028079E-6,1.8027592354372138E-6,8.6101980153605623E-2,0.64149363650945135,0.42849607928953193]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"100mA",{"$f":"BD91","v":3.8811319861701932E-3},{"$f":"BE91","v":2.4569313985821031E-2},6.338944771996971E-2,0.42852340225790159,7.6817686476419941E-3,1.2398074550738242E-3,null,5.8708959767664092E-3,0,5.1309360307431527E-6,1.7128742353749173E-6,8.2101198097302389E-2,0.62958664813907095,0.43805277381570967]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"500mA",{"$f":"BD106","v":4.8536550648896606E-3},{"$f":"BE106","v":3.0520405383485175E-2},5.6951037331454304E-2,0.40952993214511429,8.5177162565729988E-3,1.3172107672195965E-3,null,7.1709849004025694E-3,0,6.3390295890967628E-6,1.519971148392924E-6,7.3503973395485492E-2,0.6052635001720742,0.45731703226723736]

{"sheet":"Design EMI Filter","index":7,"n_rows":33,"n_cols":15,"rows_kept":33,"cut":false,"hidden":false,"merged":[[0,0,0,22],[32,10,32,12],[29,10,29,12],[31,10,31,12]]}
["                         LM5168/9 100V, Low IQ DC/DC Converter Design Tool  "]
[]
[]
[]
[]
[]
["Step 7: EMI Filter (Optional)"]
[null,null,null,"Desired Maximum Noise Level, Vnoise(MAX)",50,"dBmV"]
[null,null,null,"EMI Filter Inductance, LF(EMI)",22,"mH"]
[null,null,null,"Minimum EMI Filter Capacitance",{"$f":"'Variable Mgmt'!M164","v":2.1475737064492679E-3},"mF"]
[null,null,null,"EMI Filter Capacitance, CF(EMI)",4.7,"mF"]
[null,null,null,"Minimum EMI Filter Damping Capacitance",{"$f":"'Variable Mgmt'!M168","v":160},"mF"]
[null,null,null,"EMI Filter Damping Capacitance, CD(EMI)",10,"mF"]
[null,null,null,"Minimum Damping Capacitor ESR",{"$f":"'Variable Mgmt'!M169","v":0.74161984870956621},"Ω"]
[null,null,null,"Damping Capacitor ESR, ESR CD(EMI)",3.3,"Ω"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"EMI Filter BOM"]
[null,null,null,null,null,null,null,"Count","Ref Des","Value","Description",null,null,"Part Number","MFR"]
[null,null,null,null,null,null,null,1,"LF(EMI)",{"$f":"'Variable Mgmt'!B298","v":"22µH"},{"$f":"\"Inductor, \"&Lf_emi*1000000&\" µH, \"&ROUNDUP(Isat_min,2)&\"A\"","v":"Inductor, 22 µH, 0.51A"},null,null,"Std","Std"]
[null,null,null,null,null,null,null,1,"CF(EMI)",{"$f":"'Variable Mgmt'!B299","v":"4.7µF"},{"$f":"IF(VIN_max>35, \"Capacitor, Ceramic, \"&'Variable Mgmt'!B299&\", 120V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B299&\", 50V, X7R, 10%\")","v":"Capacitor, Ceramic, 4.7µF, 120V, X7R, 10%"},null,null,"Std","Std"]
[null,null,null,null,null,null,null,1,"CD(EMI)",{"$f":"'Variable Mgmt'!B300","v":"10µF"},{"$f":"IF(VIN_max>35, \"Capacitor, Electrolytic, \"&'Variable Mgmt'!B300&\", 120V, ESR>\"&ESR_Cd&ohm, \"Capacitor, Electrolytic, \"&'Variable Mgmt'!B300&\", 50V, ESR>\"&ESR_Cd&ohm)","v":"Capacitor, Electrolytic, 10µF, 120V, ESR>3.3Ω"},null,null,"Std","Std"]

{"sheet":"EVM","index":8,"n_rows":85,"n_cols":15,"rows_kept":85,"cut":false,"hidden":true,"merged":[[0,0,0,16]]}
["LM5163/4 100V, Low IQ DC/DC Converter Design Tool  "]
[]
[null,"LM5164-Q1EVM-041 PCB Layout"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Top"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer 2"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer 3"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bottom"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer"]

{"sheet":"BOM & Schematic","index":9,"n_rows":53,"n_cols":13,"rows_kept":53,"cut":false,"hidden":true,"merged":[[33,3,33,5],[0,0,0,16],[29,3,29,5],[41,3,41,5],[47,7,47,9],[30,3,30,5],[43,3,43,5],[44,3,44,5],[42,3,42,5],[39,3,39,5],[40,3,40,5],[38,3,38,5],[37,3,37,5],[36,3,36,5],[31,3,31,5],[34,3,34,5],[32,3,32,5]]}
["                         LM5163/4 100V Low IQ DC/DC Converter Design Tool  "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[{"$f":"\"VIN = \"&Vin&\" V, VOUT = \"&Vout&\" V, IOUT = \"&Iout&\" A \"&'Variable Mgmt'!B35&\" Converter\"","v":"VIN = 68 V, VOUT = 3.3 V, IOUT = 0.3 A COT Converter"}]
["Low IQ, High Efficiency, Synchronous Buck Converter BOM"]
["Count","Ref Des","Value","Description",null,null,"Size","Part Number","MFR","Footprint (mm)","Area (mm2)"]
[{"$f":"ROUNDUP('Design Converter'!E37/10,0)","v":4},"CIN",{"$f":"Cin*1000000","v":40},{"$f":"IF(VIN_max>35, \"Capacitor, Ceramic, \"&'Variable Mgmt'!B257&\", 100V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B257&\", 50V, X7R, 10%\")","v":"Capacitor, Ceramic, 40µF, 100V, X7R, 10%"},null,null,5,"Std","Std",{"$f":"CHOOSE(G31,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)","v":"3.2 x 2.5"},{"$f":"CHOOSE(G31,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45)","v":8}]
[{"$f":"'Variable Mgmt'!D252","v":1},"COUT",{"$f":"'Variable Mgmt'!F253","v":"100µF"},{"$f":"CHOOSE(Cout_Voltage_Rating, \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 6.3V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 10V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 16V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 25V, X7R, 10%\",  \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 50V, X7R, 10%\")","v":"Capacitor, Ceramic, 100µF, 6.3V, X7R, 10%"},null,null,5,"Std","Std",{"$f":"CHOOSE(G32,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)","v":"3.2 x 2.5"},{"$f":"(CHOOSE(G32,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45))*A32","v":8}]
[{"$f":"CHOOSE(MODE, \"-\", \"-\", \"1\",\"-\")","v":"1"},{"$f":"CHOOSE(MODE,\"-\",\"-\",\"Ca\",\"-\")","v":"Ca"},{"$f":"CHOOSE(MODE, \"-\",\"-\",'Variable Mgmt'!B293, \"-\")","v":"3300pF"},{"$f":"CHOOSE(MODE,\"-\",\"-\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B293&\", 16V, X7R, 10%\", \"-\")","v":"Capacitor, Ceramic, 3300pF, 16V, X7R, 10%"},null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"-\", \"Std\", \"-\")","v":"Std"},{"$f":"H33","v":"Std"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G33,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G33,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[{"$f":"CHOOSE(MODE, \"-\", \"1\", \"1\",\"-\")","v":"1"},{"$f":"CHOOSE(MODE,\"-\",\"Cff\",\"Cb\",\"-\")","v":"Cb"},{"$f":"CHOOSE(MODE, \"-\",'Variable Mgmt'!B290,'Variable Mgmt'!B290, \"-\")","v":"56pF"},{"$f":"CHOOSE(MODE,\"-\",\"Capacitor, Ceramic, \"&'Variable Mgmt'!B290&\", 50V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B290&\", 50V, X7R, 10%\", \"-\")","v":"Capacitor, Ceramic, 56pF, 50V, X7R, 10%"},null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"Std\", \"Std\", \"-\")","v":"Std"},{"$f":"H34","v":"Std"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G34,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G34,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G34,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G34,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"CBST","2.2nF","Capacitor, Ceramic, 2.2nF, 25V, X7R, 10%",null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"Std\", \"Std\", \"-\")","v":"Std"},{"$f":"H35","v":"Std"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G35,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G35,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G35,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G35,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[]
[1,"LF",{"$f":"'Design Converter'!E17","v":33},{"$f":"\"Inductor, \"&Lf*1000000&\" µH, \"&Rdcr*1000&\" mΩ, >\"&ROUNDUP(Isat_min,2)&\"A\"","v":"Inductor, 33 µH, 170 mΩ, >0.51A"},null,null,4,"Various","Various",{"$f":"CHOOSE(G37,'Variable Mgmt'!T50,'Variable Mgmt'!T51,'Variable Mgmt'!T52,'Variable Mgmt'!T53,'Variable Mgmt'!T54,'Variable Mgmt'!T55,'Variable Mgmt'!T56)","v":"6.0 x 6.0"},{"$f":"CHOOSE(G37,'Variable Mgmt'!U50,'Variable Mgmt'!U51,'Variable Mgmt'!U52,'Variable Mgmt'!U53,'Variable Mgmt'!U54,'Variable Mgmt'!U55,'Variable Mgmt'!U56)","v":36}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(MODE_RSET=2,CHOOSE(G38,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":""}]
[{"$f":"CHOOSE(MODE, \"1\",\"1\",\"1\", \"-\")","v":"1"},"RT",{"$f":"CHOOSE(MODE, 'Design Converter'!E13, 'Design Converter'!E13,'Design Converter'!E13,\"-\")","v":11},{"$f":"C39","v":11},null,null,1,{"$f":"CHOOSE(MODE, \"Std\",\"Std\",\"Std\",\"-\")","v":"Std"},{"$f":"H39","v":"Std"},{"$f":"CHOOSE(MODE,CHOOSE(G39,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G39,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G39,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,CHOOSE(G39,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G39,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G39,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"RFB1",{"$f":"Rfb1_/1000","v":453},453,null,null,1,{"$f":"CHOOSE(MODE_VOUT,\"-\",\"Std\")","v":"Std"},{"$f":"H40","v":"Std"},{"$f":"(CHOOSE(MODE_VOUT,\"\",CHOOSE(G40,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)))","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE_VOUT,\"\",CHOOSE(G40,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45))","v":0.5}]
[1,"RFB2",{"$f":"Rfb2_u/1000","v":261},261,null,null,1,{"$f":"CHOOSE(MODE_VOUT,\"-\",\"Std\")","v":"Std"},{"$f":"H41","v":"Std"},{"$f":"CHOOSE(MODE_VOUT,\"\",CHOOSE(G41,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45))","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE_VOUT,\"\",CHOOSE(G41,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45))","v":0.5}]
[{"$f":"IF(MODE=3,\"1\",\"-\")","v":"1"},{"$f":"CHOOSE(MODE,\"-\",\"-\",\"Ra\",\"-\")","v":"Ra"},{"$f":"'Variable Mgmt'!F296","v":"31.6k"},{"$f":"\"Resistor, Chip, \"&'Variable Mgmt'!B296&\", 1/16W, 1%\"","v":"Resistor, Chip, 31.6kΩ, 1/16W, 1%"},null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"-\", \"Std\", \"-\")","v":"Std"},{"$f":"H42","v":"Std"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G42,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G42,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"RPGOOD",100,100,null,null,1,"Std","Std",{"$f":"CHOOSE(G43,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)","v":"1.0 x 0.5"},{"$f":"CHOOSE(G43,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45)","v":0.5}]
[{"$f":"CHOOSE(MODE_UVLO, \"1\", \"-\")","v":"1"},"RUV1",{"$f":"CHOOSE(MODE_UVLO, 'Variable Mgmt'!H275, \"-\")","v":"1M"},{"$f":"CHOOSE(MODE_UVLO, \"Resistor, Chip, \"&'Variable Mgmt'!C275&\", 1/16W, 1%\", \"-\")","v":"Resistor, Chip, 1MΩ, 1/16W, 1%"},null,null,2,{"$f":"CHOOSE(MODE_UVLO,\"Std\",\"-\")","v":"Std"},{"$f":"H44","v":"Std"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G44,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.6 x 0.8"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G44,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":1.3}]
[{"$f":"CHOOSE(MODE_UVLO, \"1\", \"-\")","v":"1"},"RUV2",{"$f":"CHOOSE(MODE_UVLO, 'Variable Mgmt'!H276, \"-\")","v":"332k"},{"$f":"CHOOSE(MODE_UVLO, \"Resistor, Chip, \"&'Variable Mgmt'!C276&\", 1/16W, 1%\", \"-\")","v":"Resistor, Chip, 332kΩ, 1/16W, 1%"},null,null,1,{"$f":"CHOOSE(MODE_UVLO,\"Std\",\"-\")","v":"Std"},{"$f":"H45","v":"Std"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G45,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G45,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"U1",{"$f":"CHOOSE(VARIANT, \"LM5163-Q1\", \"LM5164-Q1\")","v":"LM5163-Q1"},{"$f":"CHOOSE(VARIANT, \"IC, LM51643-Q1, Buck Converter, 6V–100V Input\", \"IC, LM5164-Q1, Buck Converter, 6V–100V Input\")","v":"IC, LM51643-Q1, Buck Converter, 6V–100V Input"},null,null,"SOIC-8",{"$f":"CHOOSE(VARIANT, \"LM5163QDDATQ1\", \"LM5164QDDATQ1\")","v":"LM5163QDDATQ1"},"TI","5.0 x 6.0",30]
[]
[null,{"$f":"\"Total Solution Size (padded by 15%) = \"&ROUND(K48,1)&\" mm^2 = \"&ROUND(M48,3)&\" in^2\"","v":"Total Solution Size (padded by 15%) = 101 mm^2 = 0.157 in^2"},null,null,null,null,null,null,null,null,{"$f":"SUM(K31:K46)*1.15","v":100.96999999999998},null,{"$f":"K48/25.4/25.4","v":0.156503813007626}]
[]
["NOTES:"]
["* Inductor saturation current should be higher than the peak inductor current setting for all operating temperatures *"]
["** Effective input and output capacitances should be appropriately derated for applied voltage and temperature, particularly with ceramics **"]
["***Estimated total solution size does not include EMI filter***"]

{"sheet":"Schematic Mgmt","index":10,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
[]
[{"$f":"'Variable Mgmt'!K27","v":"SCH_COT3_LM5168"}]

{"sheet":"sch_frank","index":11,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
[]
[{"$f":"CHOOSE(MODE,\"cot1_sch\",\"cot2_sch\",\"cot3_sch\")","v":"cot3_sch"}]

{"sheet":"Efficiency Plots","index":12,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
[]
[{"$f":"IF(PLOT_TYPE=1, \"EFF_LINEAR\", \"EFF_LOG\")","v":"EFF_LINEAR"}]