
**** 06/19/18 15:47:13 ****** PSpice 17.2.0 (March 2016) ****** ID# 0 ********

 ** Profile: "SCHEMATIC1-TesteDiodeB"  [ C:\Users\Workstation2\Desktop\SymbiotrackerGF 6-6-18\Symbiotracker pSpice Simul\KiCad Sym Pr


 ****     CIRCUIT DESCRIPTION


******************************************************************************




** Creating circuit file "TesteDiodeB.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
.LIB "E:/Cadence/SPB_17.2/tools/pspice/library/ti_spice_models/BQ25570/bq25570_trans.lib" 
.LIB "../../../spicemodels/sllm126/csd17308q3.lib" 
* From [PSPICE NETLIST] section of C:\SPB_DATA\cdssetup\OrCAD_PSpice\17.2.0\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.TRAN  0 2.5 0 0.05 
.OPTIONS ADVCONV
.AUTOCONVERGE ITL1=1000 ITL2=1000 ITL4=1000 RELTOL=0.05 ABSTOL=1.0E-6 VNTOL=.001 PIVTOL=1.0E-10 
.PROBE64 V(alias(*)) I(alias(*)) W(alias(*)) D(alias(*)) NOISE(alias(*)) 
.INC "..\SCHEMATIC1.net" 



**** INCLUDING SCHEMATIC1.net ****
* source TESTE1
X_U5         N40374 N39432 N39302 N39523 N40150 N39511 N387176 N43287 N44647
+  VBAT VOC_SAMP N39530 VOC_SAMP VOC_SAMP N44957 N39944 DC N39506 BQ25570 PARAMS:
+   FAST=1 UV_SEL=2
L_L1         N40150 DC  10uH  
L_L2         N387176 N39944  10uH  
R_R4         N39432 N39506  7.5M TC=0,0 
R_R5         0 N39432  5.6M TC=0,0 
R_ROUT2         N39530 N39506  8.2M TC=0,0 
R_ROUT1         0 N39530  4.3M TC=0,0 
C_C7         VOC_SAMP 0  4.7u IC=0 TC=0,0 
C_C8         VOC_SAMP 0  10nF IC=0 TC=0,0 
V_V1         DC 0 5Vdc
C_CRef         0 N39302  10n IC=0 TC=0,0 
R_R13         N44957 0  3k TC=0,0 
R_R14         N39511 N39506  1.2M TC=0,0 
R_R15         N39523 N39511  7.5M TC=0,0 
R_R16         0 N39523  4.7M TC=0,0 
C_C12         VBAT 0  1 IC=0 TC=0,0 
C_C15         0 N39944  20u IC=0 TC=0,0 
R_R19         0 N39944  0 TC=0,0 
------------------------$
ERROR(ORPSIM-16144): Value may not be 0
R_R20         N43287 0  3k TC=0,0 
R_R22         0 N44647  3k TC=0,0 
C_C16         0 DC  4.7u IC=0 TC=0,0 
C_C17         N39944 N43287  22u  TC=0,0 

**** RESUMING TesteDiodeB.cir ****
.END
