** Profile: "SCHEMATIC1-TestePspice"  [ C:\Users\GFonseca\Desktop\WavEC\Estudos e Projectos\Symbiotracker\KiCad Sym Project\teste1-pspicefiles\schematic1\testepspice.sim ] 

** Creating circuit file "TestePspice.cir" 
** WARNING: THIS AUTOMATICALLY GENERATED FILE MAY BE OVERWRITTEN BY SUBSEQUENT SIMULATIONS

*Libraries: 
* Profile Libraries :
* Local Libraries :
.LIB "C:/Cadence/SPB_17.2/tools/pspice/library/ti_pspice_models/LM74670-Q1_PSPICE_TRANS/LM74670-Q1_TRANS.LIB" 
.LIB "../../../spicemodels/sllm126/csd17308q3.lib" 
.INC "C:/Cadence/SPB_17.2/tools/pspice/library/ti_pspice_models/LM74670-Q1_PSPICE_TRANS/LM74670-Q1_TRANS-PSpiceFiles/LM74670-Q1_Tra"
+ "ns/trans.sim" 
* From [PSPICE NETLIST] section of C:\SPB_Data\cdssetup\OrCAD_PSpice\17.2.0\PSpice.ini file:
.lib "nom.lib" 

*Analysis directives: 
.TRAN  0 3ms 1ms 100u SKIPBP 
.OPTIONS ADVCONV
.AUTOCONVERGE ITL1=1000 ITL2=1000 ITL4=1000 RELTOL=0.05 ABSTOL=1.0E-6 VNTOL=.001 PIVTOL=1.0E-10 
.PROBE64 V(alias(*)) I(alias(*)) W(alias(*)) D(alias(*)) NOISE(alias(*)) 
.INC "..\SCHEMATIC1.net" 


.END
