### High pin count component to design outline

This constraint defines the rule for minimum allowable distance between edge of a high pin count component instance to the design outline.
A high pin count component is defined as a symbol having pin count greater than the value specified in the attribute DFA_MIN_PINCOUNT_HIGHPNCNT. This can be defined through "Design for Assembly" options page in Analysis Mode dialog.
This rule is applicable if the high pin count component criteria is satisfied.

#### DRC Code: %2