# Test Via Spacing

#### This group consists of Test Via Spacing constraints.
The rules are as follows:

- Test Via to Line: Defines the minimum test via to line spacing.
- Test Via to Thru Pin: Defines the minimum test via to thru pin spacing.
- Test Via to SMD Via: Defines the minimum test via to SMD via spacing.
- Test Via to Test Via: Defines the minimum test via to test via spacing.
- Test Via to Thru Via: Defines the minimum test via to thru via spacing.
- Test Via to BB Via: Defines the minimum test via to blind/buried via spacing.
- Test Via to Test Via: Defines the minimum test via to test via spacing.
- Test Via to Microvia : Defines the minimum microvia to test via spacing.
- Test Via to Shape: Defines the minimum test via to shape spacing.
- Test Via to Bond Finger : Defines the minimum test via to bond finger spacing.