### Outline to Non signal geometry fabrication checks

The Outline to non-signal geometry category consists of a group of fabrication checks for outermost edge of various non-signal geometry objects to outer edge of design outline geometry. A non-signal geometry can be one of the following:

- A filled shape which is not on any net in a conducting(ETCH) layer. This includes rectangles and polygons as well.
- Text line in conducting layer
- Line or arc in conducting layer

#### Example checks

- Design outline to non signal shape
- Design outline to text
- Design outline to line