### Maximum Stub Length

Checks the maximum stub length in design units for daisy chain routing.

Note: When a pin is routed to a connect line, the stub is the line of etch between the pin and the connect line.

The stub length constraint is validated only if NET_SCHEDULE is enabled and RATSNEST_SCHEDULE is set to either MIN_DAISY_CHAIN or MIN_SOURCE_LOAD_DAISY.

>

This check ignores pins at the end of clines, dangling clines, and test points. The chosen net schedule impacts the rule check.

#### DRC Code: %2