### Total Etch

The Total Etch constraint is used to specify the minimum and maximum etch requirements for Xnet or Net. The constraint consists of two portions, which are defined as follows:

- Total Etch Length Minimum:
Specifies the minimum allowable total etch length for the Net or Xnet.
- Total Etch Length Maximum
Specifies the maximum allowable total etch length for the Net or Xnet.

DRC Code:

#### DRC Code: %2