### Silkscreen object to pin object fabrication checks

The Silkscreen to pin object category consists of a group of fabrication checks for defining minimum allowable distance between various types of pin objects to any silkscreen geometry in the design. A silkscreen object can be any line, shape or text in a silkscreen subclass.

#### Example checks

- Silkscreen object to thru pin pad
- Silkscreen object to smd pin pad
- Silkscreen object to slot pad