# Same Net Test Via Spacing

#### This group consists of Same Net Test Via Spacing constraints.
The rules are as follows:

- Test Via to Line: Defines the minimum same net test via to line spacing.
- Test Via to Thru Pin: Defines the minimum same net test via to thru pin spacing.
- Test Via to SMD Via: Defines the minimum same net test via to SMD via spacing.
- Test Via to Test Pin: Defines the minimum same net test via to test pin spacing.
- Test Via to Thru Via: Defines the minimum same net test via to thru via spacing.
- Test Via to BB Via: Defines the minimum same net test via to blind/buried via spacing.
- Test Via to Test Via: Defines the minimum same net test via to test via spacing.
- Test Via to Microvia : Defines the minimum same net microvia to test via spacing.
- Test Via to Shape: Defines the minimum same net test via to shape spacing.
- Test Via to Bond Finger : Defines the minimum same net test via to bond finger spacing.