### Wire To Die Pin Spacing

This rule applies only to the space between a bond wire and die pad. The die pad to which the wire connects is excluded from the check. The distance is measured as the minimum 2D separation between the wire and die pad edge, ignoring any possible height difference between the wire and pad.
To run this online rule, choose Setup - Constraints - Modes and set Wire to Pin to On.

#### DRC Code: %2