### Design Outline Cutout checks

The design outline cutout category consists of a group of fabrication checks to ensure correctness from manufacturing point of view for outer edge of any object to the outer edge of any cutout geometry in the design.
Any object too close to a cutout geometry may create problems during manufacturing process. So it is advisable to set correct constraints for various types of objects and enable the checks, in order to avoid manufacturing problems down the line.