# Same Net Line Spacing

#### This group consists of Same Net Line Spacing constraints.
The rules are as follows:

- Line to Line: Defines the minimum same net line to line spacing.
- Line to Thru Pin: Defines the minimum same net line to thru pin spacing.
- Line to SMD Pin: Defines the minimum same net line to SMD pin spacing.
- Line to Test Pin: Defines the minimum same net line to test pin spacing.
- Line to Thru Via: Defines the minimum same net line to thru via spacing.
- Line to BB Via: Defines the minimum same net line to blind/buried via spacing.
- Line to Test Via: Defines the minimum same net line to test via spacing.
- Line to Microvia : Defines the minimum same net line to microvia spacing.
- Line to Shape: Defines the minimum same net line to shape spacing.
- Line to Bond Finger : Defines the minimum same net line to bond finger spacing.