# Shape Spacing

#### This group consists of Shape Spacing constraints.
The rules are as follows:

- Shape to Line: Defines the minimum shape to line spacing.
- Shape to Thru Pin: Defines the minimum shape to thru pin spacing.
- Shape to SMD Pin: Defines the minimum shape to SMD pin spacing.
- Shape to Test Pin: Defines the minimum shape to test pin spacing.
- Shape to Thru Via: Defines the minimum shape to thru via spacing.
- Shape to BB Via: Defines the minimum shape to blind/buried via spacing.
- Shape to Test Via: Defines the minimum shape to test via spacing.
- Shape to Microvia : Defines the minimum microvia to shape spacing.
- Shape to Shape: Defines the minimum shape to shape spacing.
- Shape to Bond Finger : Defines the minimum shape to bond finger spacing.