# Same Net Shape Spacing

#### This group consists of Same Net Shape Spacing constraints.
The rules are as follows:

- Shape to Line: Defines the minimum same net shape to line spacing.
- Shape to Thru Pin: Defines the minimum same net shape to thru pin spacing.
- Shape to SMD Pin: Defines the minimum same net shape to SMD pin spacing.
- Shape to Test Pin: Defines the minimum same net shape to test pin spacing.
- Shape to Thru Via: Defines the minimum same net shape to thru via spacing.
- Shape to BB Via: Defines the minimum same net shape to blind/buried via spacing.
- Shape to Test Via: Defines the minimum same net shape to test via spacing.
- Shape to Microvia : Defines the minimum same net microvia to shape spacing.
- Shape to Shape: Defines the minimum same net shape to shape spacing.
- Shape to Bond Finger : Defines the minimum same net shape to bond finger spacing.