### Package to cavity

Verifies the clearance between the edges of a package placebound shape to edge of cavity outline. Packages that do not maintain this distance are flagged.
The clearance value or the minimum distance between the edge of the placebound shape to the cavity outline is specified in the Package to cavity spacing field, available in the Design Options page of the Analysis Modes dialog box. The default clearance value is 0.

#### DRC Code: %2