# Same Net Microvia Spacing

#### This group consists of Same Net Microvia Spacing constraints.
The rules are as follows:

- Microvia to Line: Defines the minimum same net microvia to line spacing.
- Microvia to Thru Pin: Defines the minimum same net microvia to thru pin spacing.
- Microvia to SMD Pin: Defines the minimum same net microvia to SMD pin spacing.
- Microvia to Test Pin: Defines the minimum same net microvia to test pin spacing.
- Microvia to Thru Via: Defines the minimum same net microvia to thru via spacing.
- Microvia to BB Via: Defines the minimum same net microvia to blind/buried via spacing.
- Microvia to Test Via: Defines the minimum same net microvia to test via spacing.
- Microvia to Microvia : Defines the minimum same net microvia to microvia spacing.
- Microvia to Shape: Defines the minimum same net microvia to shape spacing.
- Microvia to Bond Finger : Defines the minimum same net microvia to bond finger spacing.