# Test Pin Spacing

#### This group consists of Test Pin Spacing constraints.
The rules are as follows:

- Test Pin to Line: Defines the minimum test pin to line spacing.
- Test Pin to Thru Pin: Defines the minimum test pin to thru pin spacing.
- Test Pin to SMD Pin: Defines the minimum test pin to SMD pin spacing.
- Test Pin to Test Pin: Defines the minimum test pin to test pin spacing.
- Test Pin to Thru Via: Defines the minimum test pin to thru via spacing.
- Test Pin to BB Via: Defines the minimum test pin to blind/buried via spacing.
- Test Pin to Test Via: Defines the minimum test pin to test via spacing.
- Test Pin to Microvia : Defines the minimum microvia to test pin spacing.
- Test Pin to Shape: Defines the minimum test pin to shape spacing.
- Test Pin to Bond Finger : Defines the minimum test pin to bond finger spacing.