# Same Net SMD Pin Spacing

#### This group consists of Same Net SMD Pin Spacing constraints.
The rules are as follows:

- SMD Pin to Line: Defines the minimum same net SMD pin to line spacing.
- SMD Pin to Thru Pin: Defines the minimum same net SMD pin to thru pin spacing.
- SMD Pin to SMD Pin: Defines the minimum same net SMD pin to SMD pin spacing.
- SMD Pin to Test Pin: Defines the minimum same net SMD pin to test pin spacing.
- SMD Pin to Thru Via: Defines the minimum same net SMD pin to thru via spacing.
- SMD Pin to BB Via: Defines the minimum same net SMD pin to blind/buried via spacing.
- SMD Pin to Test Via: Defines the minimum same net SMD pin to test via spacing.
- SMD Pin to Microvia : Defines the minimum same net microvia to SMD pin spacing.
- SMD Pin to Shape: Defines the minimum same net SMD pin to shape spacing.
- SMD Pin to Bond Finger : Defines the minimum same net SMD pin to bond finger spacing.