{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["TICSPro"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"TICSPro","index":0,"n_rows":22,"n_cols":4,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["Step 1",null,"Launch TICSPro"]
[null,null,"TICSPro Path","C:\\Program Files (x86)\\Texas Instruments\\TICS Pro"]
[null,null,"Selected Device","LMX2572"]
[]
[]
[]
["Step 2",null,"Run Commands","See Code for More Details"]
[null,null,"FirstLine","MASH_ORDER"]
[null,null,"CmdName","SETTEXT"]
[null,null,"Parameter","Integer Mode"]
[]
[]
[null,null,"Return Value"]
[]
[]
[]
[]
[]
[]
[]
["Note that if you have an error in your program, the link to TICSPro is broken"]
["In this case, close whole Excel and restart"]