/*
 *  ======== ti_utils_build_linker.cmd.genmap ========
 *  SysConfig-generated linker definitions.
 *
 *  This file provides "more portable" definitions for linker command files.
 *  The intent is to enable easier porting to different devices by leveraging
 *  these definitions.
 *
 *  DO NOT EDIT - This file is generated by the SysConfig tool for the
 *                CC2340R5RKP device, ticlang C/C++ toolchain
 */
/* symbols provided by /ti/devices/CCFG */
ti_utils_build_GenMap_sym_CRC_CCFG_BOOT_CFG_begin = 0x4e020000;
ti_utils_build_GenMap_sym_CRC_CCFG_BOOT_CFG_end = 0x4e02000b;
ti_utils_build_GenMap_sym_CRC_CCFG_begin = 0x4e020010;
ti_utils_build_GenMap_sym_CRC_CCFG_end = 0x4e02074b;
ti_utils_build_GenMap_sym_CRC_CCFG_DEBUG_begin = 0x4e0207d0;
ti_utils_build_GenMap_sym_CRC_CCFG_DEBUG_end = 0x4e0207fb;

/* definitions provided by /ti/drivers/Board */
#define ti_utils_build_GenMap_NVS_CONFIG_NVSINTERNAL_BASE 0x7c000
#define ti_utils_build_GenMap_NVS_CONFIG_NVSINTERNAL_SIZE 0x4000

/* definitions provided by /ti/devices/DriverLib */
#define ti_utils_build_GenMap_FLASH0_SIZE 0x80000
#define ti_utils_build_GenMap_RAM0_SIZE 0x9000
#define ti_utils_build_GenMap_S2RRAM_BASE 0x40098000
#define ti_utils_build_GenMap_S2RRAM_SIZE 0x1000
#define ti_utils_build_GenMap_CCFG_BASE 0x4e020000
#define ti_utils_build_GenMap_CCFG_SIZE 0x800
#define ti_utils_build_GenMap_FLASH0_BASE 0x0
#define ti_utils_build_GenMap_RAM0_BASE 0x20000000
