**USB Test for CC2544**

**Company Information:**

**Company**

Company Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Company Address: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Technical Contact**

Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Phone Number: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

E-Mail: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Windows WHQL test**

**Inf Verif** **(InfVerif.exe) □Pass ■Fail**

**Fail Description**

The CC2544 driver INF file(ccxxx\_usb\_cdc.inf) test fail while running InfVerif.exe. The Error Code is 1203 (Section not found).

**Fail Log (UniversalLog.txt):**

InfVerif failed for Driver. Partial Log:Error 1203 in ccxxxx\_usb\_cdc.inf, line 49 : Section [fakemodemcopyfilesection] not found.

**INF file (ccxxx\_usb\_cdc.inf):**

;

; Texas Instruments CCxxxx USB Serial Port Setup File

;

; Based on Windows USB CDC ACM Setup File

; Copyright (c) 2000 Microsoft Corporation

; Copyright (c) 2013 Texas Instruments Inc

[Version]

Signature="$Windows NT$"

Class=Ports

ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}

Provider=%PROVIDER%

DriverVer=04/05/2013,1.2.0.0

CatalogFile=ccxxxx\_usb\_cdc.cat

[Manufacturer]

%MFGNAME%=DeviceList,NTx86,NTamd64

[DeviceList.NTx86]

%DESC\_SRFEB% = DriverInstall, USB\VID\_0451&PID\_16B6

%DESC\_CC2511% = DriverInstall, USB\VID\_0451&PID\_16A4

%DESC\_CC1111% = DriverInstall, USB\VID\_0451&PID\_16A6

%DESC\_CC2531% = DriverInstall, USB\VID\_0451&PID\_16A8

%DESC\_CC2540% = DriverInstall, USB\VID\_0451&PID\_16AA

%DESC\_CC2544% = DriverInstall, USB\VID\_0451&PID\_16C5

%DESC\_CC2538% = DriverInstall, USB\VID\_0451&PID\_16C8

%DESC\_CCXXXXBL% = DriverInstall, USB\VID\_0451&PID\_16C7

%DESC\_REMOTINP% = DriverInstall, USB\VID\_0451&PID\_16B1

[DeviceList.NTamd64]

%DESC\_SRFEB% = DriverInstall, USB\VID\_0451&PID\_16B6

%DESC\_CC2511% = DriverInstall, USB\VID\_0451&PID\_16A4

%DESC\_CC1111% = DriverInstall, USB\VID\_0451&PID\_16A6

%DESC\_CC2531% = DriverInstall, USB\VID\_0451&PID\_16A8

%DESC\_CC2540% = DriverInstall, USB\VID\_0451&PID\_16AA

%DESC\_CC2544% = DriverInstall, USB\VID\_0451&PID\_16C5

%DESC\_CC2538% = DriverInstall, USB\VID\_0451&PID\_16C8

%DESC\_CCXXXXBL% = DriverInstall, USB\VID\_0451&PID\_16C7

%DESC\_REMOTINP% = DriverInstall, USB\VID\_0451&PID\_16B1

;------------------------------------------------------------------------------

; Windows 32-bit sections

;------------------------------------------------------------------------------

[DriverInstall.NTx86]

include=mdmcpq.inf

CopyFiles=FakeModemCopyFileSection

AddReg=DriverRegistryKeys

[DriverInstall.NTx86.Services]

AddService=usbser, 0x00000002, DriverService

;------------------------------------------------------------------------------

; Windows 64-bit sections

;------------------------------------------------------------------------------

[DriverInstall.NTamd64]

include=mdmcpq.inf

CopyFiles=FakeModemCopyFileSection

AddReg=DriverRegistryKeys

[DriverInstall.NTamd64.Services]

AddService=usbser, 0x00000002, DriverService

;------------------------------------------------------------------------------

;

;------------------------------------------------------------------------------

[DriverRegistryKeys]

HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[DriverService]

DisplayName = %SERVICE%

ServiceType = 1

StartType = 3

ErrorControl = 1

ServiceBinary = %12%\usbser.sys

;------------------------------------------------------------------------------

; String Definitions

;------------------------------------------------------------------------------

[Strings]

PROVIDER = "Texas Instruments"

MFGNAME = "Texas Instruments"

SERVICE = "TI USB CDC Driver"

DESC\_SRFEB = "TI SmartRFEB USB CDC Serial Port"

DESC\_CC1111 = "TI CC1111 USB CDC Serial Port"

DESC\_CC2511 = "TI CC2511 USB CDC Serial Port"

DESC\_CC2531 = "TI CC2531 USB CDC Serial Port"

DESC\_CC2538 = "TI CC2538 USB CDC Serial Port"

DESC\_CC2540 = "TI CC2540 USB CDC Serial Port"

DESC\_CC2544 = "TI CC2544 USB CDC Serial Port"

DESC\_CCXXXXBL = "TI CCxxxx Generic USB CDC Boot Loader"

DESC\_REMOTINP = "RemoTI Network Processor"