[IBIS Ver]   5.1
|
[Disclaimer]
             THIS IBIS MODEL HAS BEEN CREATED BY THE ALTERA
             SPICE CONVERSION PROCESS.
             THESE IBIS MODELS ARE PROVIDED "AS IS" WITH NO
             WARRANTY WHATSOEVER AND ALTERA
             SPECIFICALLY DISCLAIMS ANY IMPLIED WARRANTIES OF
             MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE,
             OR AGAINST INFRINGEMENT.
|
[File Name]  a10_rx_5p1.ibs
[Date]       July 6, 2016
[File Rev]   2.0
[Source]     Intel PSG High-Speed Technology Group
|
[Notes]
  This model is distributed in two versions:
   - "a10_rx_5p1.ibs" supports those IBIS-AMI simulators, which are
     compliant to version 5.1 of the IBIS specification.
   - "a10_rx_5p1_ads.ibs" supports Keysight ADS

  Note: SiSoft QCD users should ensure that they are using QCD v2014.05,
        or later, and use the v5.1 IBIS model, in order to avoid errors
        during model importing. The automatic CTLE optimization will work,
        despite the warning, above.
|
[Component]    Arria10_Rx
|
[Manufacturer] Intel Corporation
|
[Package]
R_pkg        0.001m  NA  NA
L_pkg        0.001nH  NA  NA
C_pkg        0.001pF  NA  NA
|
[Pin] signal_name model_name R_pin L_pin C_pin
  20   a10_rx_1P     a10_rx    NA    NA     NA
  21   a10_rx_1N     a10_rx    NA    NA     NA
  22   a10_rx_2P     a10_rx    NA    NA     NA
  23   a10_rx_2N     a10_rx    NA    NA     NA
  24   a10_rx_3P     a10_rx    NA    NA     NA
  25   a10_rx_3N     a10_rx    NA    NA     NA
|
[Diff Pin] inv_pin  vdiff tdelay_typ tdelay_min tdelay_max
     20       21    0.05      NA         NA         NA
     22       23    0.05      NA         NA         NA
     24       25    0.05      NA         NA         NA
|
[Model Selector] a10_rx
a10_rx_qcd  For SiSoft QCD users, only!
a10_rx_100  100 Ohms differential termination.
a10_rx_85   85 Ohms differential termination.
|
| ------------------------------------
|
|   model   a10_rx_qcd
|
[Model] a10_rx_qcd
Model_type Input
C_comp 1.2pF 1.1pF 1.3pF
Vinl = 0.025
Vinh = 0.025
[Temperature Range] 85 100 -40
[Voltage Range] 1.1 1.02 1.13
[Algorithmic Model]
Executable Windows_VisualStudio9.0.21022.8_32 a10gx_ami_rx_x86.dll a10_rx_5p1_qcd.ami
Executable Windows_VisualStudio9.0.21022.8_64 a10gx_ami_rx_x64.dll a10_rx_5p1_qcd.ami
Executable Linux_GCC4.8.2_32                  a10gx_ami_rx_x86.so  a10_rx_5p1_qcd.ami
Executable Linux_GCC4.8.2_64                  a10gx_ami_rx_x64.so  a10_rx_5p1_qcd.ami
[End Algorithmic Model]
[GND Clamp]
-1.0     -1.0      -1.0      -1.0
-0.5     -0.0240   -0.0216   -0.0264
 2.3      0.0320    0.0288    0.0352
 2.8      1.0       1.0       1.0
|
| ------------------------------------
|
|   model   a10_rx_85
|
[Model] a10_rx_85
Model_type Input
C_comp 1.2pF 1.1pF 1.3pF
Vinl = 0.025
Vinh = 0.025
[Temperature Range] 85 100 -40
[Voltage Range] 1.1 1.02 1.13
[Algorithmic Model]
Executable Windows_VisualStudio9.0.21022.8_32 a10gx_ami_rx_x86.dll a10_rx_85_5p1.ami
Executable Windows_VisualStudio9.0.21022.8_64 a10gx_ami_rx_x64.dll a10_rx_85_5p1.ami
Executable Linux_GCC4.8.2_32                  a10gx_ami_rx_x86.so  a10_rx_85_5p1.ami
Executable Linux_GCC4.8.2_64                  a10gx_ami_rx_x64.so  a10_rx_85_5p1.ami
[End Algorithmic Model]
[GND Clamp]
-1.0     -1.0      -1.0      -1.0
-0.5     -0.0282   -0.0264   -0.0300
 2.3      0.0376    0.0352    0.0400
 2.8      1.0       1.0       1.0
|
| ------------------------------------
|
|   model   a10_rx_100
|
[Model] a10_rx_100
Model_type Input
C_comp 1.2pF 1.1pF 1.3pF
Vinl = 0.025
Vinh = 0.025
[Temperature Range] 85 100 -40
[Voltage Range] 1.1 1.02 1.13
[Algorithmic Model]
Executable Windows_VisualStudio9.0.21022.8_32 a10gx_ami_rx_x86.dll a10_rx_5p1.ami
Executable Windows_VisualStudio9.0.21022.8_64 a10gx_ami_rx_x64.dll a10_rx_5p1.ami
Executable Linux_GCC4.8.2_32                  a10gx_ami_rx_x86.so  a10_rx_5p1.ami
Executable Linux_GCC4.8.2_64                  a10gx_ami_rx_x64.so  a10_rx_5p1.ami
[End Algorithmic Model]
[GND Clamp]
-1.0     -1.0      -1.0      -1.0
-0.5     -0.0240   -0.0231   -0.0261
 2.3      0.0320    0.0308    0.0348
 2.8      1.0       1.0       1.0
[End]
