DRC Rules Export File for PCB: E:\PCB\Current Boards\ADC12QJ_LIDAR_E2_Final\ADC12QJ_LIDAR_E2\ADC12QJ_LIDAR_RevE2.PcbDoc
RuleKind=Clearance|RuleName=Clearance_SigPour|Scope=Board|Minimum=5.00
RuleKind=Clearance|RuleName=Clearance_FID|Scope=Board|Minimum=0.00
RuleKind=Clearance|RuleName=serdes_1|Scope=Board|Minimum=5.00
RuleKind=MinimumAnnularRing|RuleName=MinimumAnnularRing|Scope=Board|Minimum=3.50
RuleKind=MinimumAnnularRing|RuleName=MinimumAnnularRing_ThermalPadVias|Scope=Board|Minimum=3.50
RuleKind=ShortCircuit|RuleName=ShortCircuit|Scope=Board|Allowed=0
RuleKind=SolderMaskExpansion|RuleName=SolderMaskExpansion|Scope=Board|Minimum=0.00
RuleKind=Width|RuleName=Width|Scope=Board|Minimum=3.25
RuleKind=Clearance|RuleName=Clearance|Scope=Board|Minimum=5.00
