[IBIS Ver] 6.0
[File Name]  ADC12xJ_17p16.ibs
[File Rev]   1.1
[Source]     Developed by: John Baprawski; John Baprawski Inc.; www.serdesdesign.com
[Notes]      v1.0   initial version, May 2021
             v1.1   reduced slope on Ramp statement, since this triggered memory warning in HyperLynx, 2/14/2022
[Component]    ADC12xJ_17p16
[Manufacturer] Texas Instruments Deutschland GmbH 
[Pin]    signal_name              model_name        R_pin L_pin  C_pin
2p       ADC12xJ_17p16_2p           ADC12xJ_17p16
2n       ADC12xJ_17p16_2n           ADC12xJ_17p16
[Diff_Pin] inv_pin vdiff tdelay_typ tdelay_min tdelay_max
2p       2n           NA    NA    NA    NA
[Package]
R_pkg  0.0    0.0      0.0
L_pkg  0.0    0.0      0.0
C_pkg  0.0    0.0      0.0

[Model Selector] ADC12xJ_17p16
ADC12xJ_17p16_typ          typical 
ADC12xJ_17p16_slow         slow 
ADC12xJ_17p16_fast         fast 
ADC12xJ_17p16_leakage      leakage 
ADC12xJ_17p16_tempinv      tempinv 

[Model] ADC12xJ_17p16_typ
Model_type Output
C_comp   0   0   0
Cref = 0
Vref = 0.5
Rref = 50
Vmeas = 0.5
[Temperature_Range] 25 125 0
[Voltage Range]  1  1  1
[Pulldown]
-5.05846572093478    -0.1    -0.1    -0.1
0.0      0.0     0.0     0.0
5.05846572093478      0.1     0.1     0.1
[Pullup]
-5.05846572093478     0.1     0.1     0.1
0.0      0.0     0.0     0.0
5.05846572093478     -0.1    -0.1    -0.1
[Ramp]
dV/dt_r 0.2/1p 0.2/1p 0.2/1p
dV/dt_f 0.2/1p 0.2/1p 0.2/1p
[Algorithmic Model]
Executable Windows_cl19.00.24215.1_64 ADC12xJ_17p16_x64.dll ADC12xJ_17p16_typ.ami
Executable Linux_gcc4.7.4_64 ADC12xJ_17p16_x64.so ADC12xJ_17p16_typ.ami
[End Algorithmic Model]

[Model] ADC12xJ_17p16_slow
Model_type Output
C_comp   0   0   0
Cref = 0
Vref = 0.5
Rref = 50
Vmeas = 0.5
[Temperature_Range] 25 125 0
[Voltage Range]  1  1  1
[Pulldown]
-5.9365899875812    -0.1    -0.1    -0.1
0.0      0.0     0.0     0.0
5.9365899875812      0.1     0.1     0.1
[Pullup]
-5.9365899875812     0.1     0.1     0.1
0.0      0.0     0.0     0.0
5.9365899875812     -0.1    -0.1    -0.1
[Ramp]
dV/dt_r 0.2/1p 0.2/1p 0.2/1p
dV/dt_f 0.2/1p 0.2/1p 0.2/1p
[Algorithmic Model]
Executable Windows_cl19.00.24215.1_64 ADC12xJ_17p16_x64.dll ADC12xJ_17p16_slow.ami
Executable Linux_gcc4.7.4_64 ADC12xJ_17p16_x64.so ADC12xJ_17p16_slow.ami
[End Algorithmic Model]

[Model] ADC12xJ_17p16_fast
Model_type Output
C_comp   0   0   0
Cref = 0
Vref = 0.5
Rref = 50
Vmeas = 0.5
[Temperature_Range] 25 125 0
[Voltage Range]  1  1  1
[Pulldown]
-4.26708554490087    -0.1    -0.1    -0.1
0.0      0.0     0.0     0.0
4.26708554490087      0.1     0.1     0.1
[Pullup]
-4.26708554490087     0.1     0.1     0.1
0.0      0.0     0.0     0.0
4.26708554490087     -0.1    -0.1    -0.1
[Ramp]
dV/dt_r 0.2/1p 0.2/1p 0.2/1p
dV/dt_f 0.2/1p 0.2/1p 0.2/1p
[Algorithmic Model]
Executable Windows_cl19.00.24215.1_64 ADC12xJ_17p16_x64.dll ADC12xJ_17p16_fast.ami
Executable Linux_gcc4.7.4_64 ADC12xJ_17p16_x64.so ADC12xJ_17p16_fast.ami
[End Algorithmic Model]

[Model] ADC12xJ_17p16_leakage
Model_type Output
C_comp   0   0   0
Cref = 0
Vref = 0.5
Rref = 50
Vmeas = 0.5
[Temperature_Range] 25 125 0
[Voltage Range]  1  1  1
[Pulldown]
-4.28985934122288    -0.1    -0.1    -0.1
0.0      0.0     0.0     0.0
4.28985934122288      0.1     0.1     0.1
[Pullup]
-4.28985934122288     0.1     0.1     0.1
0.0      0.0     0.0     0.0
4.28985934122288     -0.1    -0.1    -0.1
[Ramp]
dV/dt_r 0.2/1p 0.2/1p 0.2/1p
dV/dt_f 0.2/1p 0.2/1p 0.2/1p
[Algorithmic Model]
Executable Windows_cl19.00.24215.1_64 ADC12xJ_17p16_x64.dll ADC12xJ_17p16_leakage.ami
Executable Linux_gcc4.7.4_64 ADC12xJ_17p16_x64.so ADC12xJ_17p16_leakage.ami
[End Algorithmic Model]

[Model] ADC12xJ_17p16_tempinv
Model_type Output
C_comp   0   0   0
Cref = 0
Vref = 0.5
Rref = 50
Vmeas = 0.5
[Temperature_Range] 25 125 0
[Voltage Range]  1  1  1
[Pulldown]
-5.91307895912606    -0.1    -0.1    -0.1
0.0      0.0     0.0     0.0
5.91307895912606      0.1     0.1     0.1
[Pullup]
-5.91307895912606     0.1     0.1     0.1
0.0      0.0     0.0     0.0
5.91307895912606     -0.1    -0.1    -0.1
[Ramp]
dV/dt_r 0.2/1p 0.2/1p 0.2/1p
dV/dt_f 0.2/1p 0.2/1p 0.2/1p
[Algorithmic Model]
Executable Windows_cl19.00.24215.1_64 ADC12xJ_17p16_x64.dll ADC12xJ_17p16_tempinv.ami
Executable Linux_gcc4.7.4_64 ADC12xJ_17p16_x64.so ADC12xJ_17p16_tempinv.ami
[End Algorithmic Model]


[END]
