\*\*\* Errors \*\*\*

117 1> \*\*\* FAILURE: (TCP) Vendor ID should be 9876, but is 806.

118 2> \*\*\* FAILURE: (TCP) Product Name should be Communications Adapter Example, but is TMDS64EVM Discrete I/O Device.

119 3> \*\*\* FAILURE: (TCP) Product Code should be 100, but is 6402.

120 4> \*\*\* FAILURE: (TCP) Device Type should be 12, but is 7.

121 5> \*\*\* FAILURE: (TCP) Major Revision should be 1, but is 3.

122 6> \*\*\* FAILURE: (TCP) Minvor Revision should be 1, but is 7.

131 7> \*\*\* FAILURE: (UDP) Vendor ID should be 9876, but is 806.

132 8> \*\*\* FAILURE: (UDP) Product Name should be Communications Adapter Example, but is TMDS64EVM Discrete I/O Device.

133 9> \*\*\* FAILURE: (UDP) Product Code should be 100, but is 6402.

134 10> \*\*\* FAILURE: (UDP) Device Type should be 12, but is 7.

135 11> \*\*\* FAILURE: (UDP) Major Revision should be 1, but is 3.

136 12> \*\*\* FAILURE: (UDP) Minvor Revision should be 1, but is 7.

163 13> \*\*\* FAILURE: (UDP Directed Broadcast) Vendor ID should be 9876, but is 806.

164 14> \*\*\* FAILURE: (UDP Directed Broadcast) Product Name should be Communications Adapter Example, but is TMDS64EVM Discrete I/O Device.

165 15> \*\*\* FAILURE: (UDP Directed Broadcast) Product Code should be 100, but is 6402.

166 16> \*\*\* FAILURE: (UDP Directed Broadcast) Device Type should be 12, but is 7.

167 17> \*\*\* FAILURE: (UDP Directed Broadcast) Major Revision should be 1, but is 3.

168 18> \*\*\* FAILURE: (UDP Directed Broadcast) Minvor Revision should be 1, but is 7.

177 19> \*\*\* FAILURE: (UDP Global Broadcast) Vendor ID should be 9876, but is 806.

178 20> \*\*\* FAILURE: (UDP Global Broadcast) Product Name should be Communications Adapter Example, but is TMDS64EVM Discrete I/O Device.

179 21> \*\*\* FAILURE: (UDP Global Broadcast) Product Code should be 100, but is 6402.

180 22> \*\*\* FAILURE: (UDP Global Broadcast) Device Type should be 12, but is 7.

181 23> \*\*\* FAILURE: (UDP Global Broadcast) Major Revision should be 1, but is 3.

182 24> \*\*\* FAILURE: (UDP Global Broadcast) Minvor Revision should be 1, but is 7.

183 25> \*\*\* ListIdentity Failed

449 1> \*\*\* Class code 8 is undefined or is not in profile

453 2> \*\*\* Class code 9 is undefined or is not in profile

457 3> \*\*\* Class code 30 is undefined or is not in profile

461 4> \*\*\* Class code 67 is undefined or is not in profile

465 5> \*\*\* Class code 71 is undefined or is not in profile

469 6> \*\*\* Class code 72 is undefined or is not in profile

475 7> \*\*\* Class code 265 is undefined or is not in profile

479 8> \*\*\* Class code 266 is undefined or is not in profile

481 9> \*\*\* Found unexpected class

528 1> \*\*\* Expected attribute is not implemented!

537 2> \*\*\* Expected attribute is not implemented!

546 3> \*\*\* Expected attribute is not implemented!

555 4> \*\*\* Expected attribute is not implemented!

564 5> \*\*\* Expected attribute is not implemented!

573 6> \*\*\* Expected attribute is not implemented!

1049 1> \*\*\* Attribute data value incorrect attr 1, Srv Code x0E

1058 2> \*\*\* Attribute data value incorrect attr 2, Srv Code x0E

1067 3> \*\*\* Attribute data value incorrect attr 3, Srv Code x0E

1076 4> \*\*\* Attribute data value incorrect attr 4, Srv Code x0E

1101 5> \*\*\* Attribute data value incorrect attr 7, Srv Code x0E

2340 1> \*\*\* User skipped Identity Instance "Return to Factory Defaults" (Type 1) Reset service. This test is required and must be run at least once in order to pass the conformance test.

2366 2> \*\*\* Unexpected success response, Srv Code x05, Expected x20

2511 1> \*\*\* Expected attribute is not implemented!

2520 2> \*\*\* Expected attribute is not implemented!

2529 3> \*\*\* Expected attribute is not implemented!

2538 4> \*\*\* Expected attribute is not implemented!

2547 5> \*\*\* Expected attribute is not implemented!

2556 6> \*\*\* Expected attribute is not implemented!

3052 1> \*\*\* GetAttrTest was skipped due to Get\_Attribute\_Single service is not supported!

3191 1> \*\*\* STC Error: Unexpected fail to the implemented service!

3545 1> \*\*\* GetAttrTest was skipped due to Get\_Attribute\_Single service is not supported!

4001 1> \*\*\* STC error: Unexpected success for not implemented attribute 4.

4536 1> \*\*\* STC error: Unexpected success for not implemented attribute 4.

4674 1> \*\*\* Unexpected success response attr 3, Srv Code x10

5000 1> \*\*\* STC Error: Assembly Object Instance 103 is not defined in the stc file! Please update the stc file and rerun the test.

5002 2> \*\*\* STC Error: Assembly Object Instance 254 is not defined in the stc file! Please update the stc file and rerun the test.

5004 3> \*\*\* STC Error: Assembly Object Instance 255 is not defined in the stc file! Please update the stc file and rerun the test.

5075 1> \*\*\* Expected attribute is not implemented!

5084 2> \*\*\* Expected attribute is not implemented!

5093 3> \*\*\* Expected attribute is not implemented!

5102 4> \*\*\* Expected attribute is not implemented!

5111 5> \*\*\* Expected attribute is not implemented!

5120 6> \*\*\* Expected attribute is not implemented!

5591 1> \*\*\* GetAttrTest was skipped due to Get\_Attribute\_Single service is not supported!

6261 1> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0127 and 0x0004; expected Status = 0x0

6285 2> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0127 and 0x0004; expected Status = 0x0

6295 3> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0127 and 0x0004; expected Status = 0x0

6305 4> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0127 and 0x0004; expected Status = 0x0

6315 5> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0127 and 0x0004; expected Status = 0x0

6325 6> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0127 and 0x0004; expected Status = 0x0

6335 7> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0127 and 0x0004; expected Status = 0x0

6351 8> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0127 and 0x0004; expected Status = 0x0

6352 9> \*\*\* Forward Close IP Address Verification was interrupted.

6369 10> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0127 and 0x0004; expected Status = 0x0

6393 11> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0127 and 0x0004; expected Status = 0x0

6403 12> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0127 and 0x0004; expected Status = 0x0

6413 13> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0127 and 0x0004; expected Status = 0x0

6423 14> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0127 and 0x0004; expected Status = 0x0

6433 15> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0127 and 0x0004; expected Status = 0x0

6443 16> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0127 and 0x0004; expected Status = 0x0

6459 17> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0127 and 0x0004; expected Status = 0x0

6460 18> \*\*\* Forward Close IP Address Verification was interrupted.

6842 19> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0114; expected Status = 0x0

6852 20> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0114; expected Status = 0x0

6862 21> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0114; expected Status = 0x0

6872 22> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0114; expected Status = 0x0

6891 23> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0114; expected Status = 0x1, Extended Status = 0x0115;

6928 24> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0114; expected Status = 0x0

6938 25> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0114; expected Status = 0x0

6948 26> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0114; expected Status = 0x0

6958 27> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0114; expected Status = 0x1, Extended Status = 0x0116;

7103 28> \*\*\* The DUT does not support required Electronic Key Format 4.

7113 29> \*\*\* Unexpected fail to UCMM service with an valid Electronic Key in Format 4.

7192 30> \*\*\* Unexpected fail or status to ForwardOpen request with a valid Electronic Key in format 4.

7230 31> \*\*\* Returned Max Size 4 bytes does not match calculated connection size 22 (includes class 1 sequence count +2, 32-bit RT header +4, or both +6, as applicable)

7240 32> \*\*\* Returned Max Size 4 bytes does not match calculated connection size 22 (includes class 1 sequence count +2, 32-bit RT header +4, or both +6, as applicable)

7250 33> \*\*\* Returned Max Size 4 bytes does not match calculated connection size 22 (includes class 1 sequence count +2, 32-bit RT header +4, or both +6, as applicable)

7260 34> \*\*\* Returned Max Size 4 bytes does not match calculated connection size 22 (includes class 1 sequence count +2, 32-bit RT header +4, or both +6, as applicable)

7270 35> \*\*\* Returned Max Size 4 bytes does not match calculated connection size 22 (includes class 1 sequence count +2, 32-bit RT header +4, or both +6, as applicable)

7280 36> \*\*\* Returned Max Size 4 bytes does not match calculated connection size 22 (includes class 1 sequence count +2, 32-bit RT header +4, or both +6, as applicable)

7290 37> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0127 and 0x0004; expected Status = 0x1, Extended Status = 0x0128;

7300 38> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0127 and 0x0004; expected Status = 0x1, Extended Status = 0x0128;

7310 39> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0127 and 0x0004; expected Status = 0x1, Extended Status = 0x0128;

7320 40> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0127 and 0x0004; expected Status = 0x1, Extended Status = 0x0128;

7330 41> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0127 and 0x0004; expected Status = 0x1, Extended Status = 0x0128;

7340 42> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0127 and 0x0004; expected Status = 0x1, Extended Status = 0x0128;

7350 43> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0117; expected Status = 0x1, Extended Status = 0x0127;

7360 44> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0117; expected Status = 0x1, Extended Status = 0x0127;

7370 45> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0117; expected Status = 0x1, Extended Status = 0x0127;

7380 46> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0117; expected Status = 0x1, Extended Status = 0x0128;

7390 47> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0117; expected Status = 0x1, Extended Status = 0x0128;

7400 48> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0117; expected Status = 0x1, Extended Status = 0x0128;

7410 49> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0117; expected Status = 0x1, Extended Status = 0x0128;

7420 50> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0117; expected Status = 0x1, Extended Status = 0x0128;

7430 51> \*\*\* ForwardOpen returned unexpected Status = 0x1, Extended Status = 0x0117; expected Status = 0x1, Extended Status = 0x0128;

7467 52> \*\*\* Expected Successful ForwardOpen: Received General Status 0x01, Extended Status 0x0127.

7468 53> \*\*\* Unexpected failure in GetTargetConnIDsFromOpen; test case aborted.

7507 54> \*\*\* Expected Successful ForwardOpen: Received General Status 0x01, Extended Status 0x0117.

7508 55> \*\*\* Unexpected failure in GetTargetConnIDsFromOpen; test case aborted.

7549 56> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

7560 57> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

7571 58> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

7582 59> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

7593 60> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

7604 61> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

7615 62> \*\*\* Expected Successful ForwardOpen or Extended status 0x11D (T->O Production Trigger not supported): Received General Status 01, Extended Status 0x0117

7626 63> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

7866 64> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0127

7883 65> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0127

7900 66> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0127

7901 67> \*\*\* Failed to open IO connection.

7918 68> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0127

7919 69> \*\*\* Failed to open IO connection

7936 70> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0127

7937 71> \*\*\* Failed to open IO connection

7954 72> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0127

7955 73> \*\*\* Failed to open IO connection

7972 74> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0127

7973 75> \*\*\* Failed to open IO connection

7990 76> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0127

7991 77> \*\*\* Failed to open IO connection

8008 78> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0127

8044 79> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0127

8062 80> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0127

8079 81> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0127

8096 82> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0127

8097 83> \*\*\* Failed to open IO connection.

8114 84> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0127

8115 85> \*\*\* Failed to open IO connection

8132 86> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0127

8133 87> \*\*\* Failed to open IO connection

8150 88> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0127

8151 89> \*\*\* Failed to open IO connection

8168 90> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0127

8169 91> \*\*\* Failed to open IO connection

8186 92> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0127

8187 93> \*\*\* Failed to open IO connection

8204 94> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0127

8261 95> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

8279 96> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

8296 97> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

8313 98> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

8314 99> \*\*\* Failed to open IO connection.

8331 100> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

8332 101> \*\*\* Failed to open IO connection

8349 102> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

8350 103> \*\*\* Failed to open IO connection

8367 104> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

8368 105> \*\*\* Failed to open IO connection

8385 106> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

8386 107> \*\*\* Failed to open IO connection

8403 108> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

8404 109> \*\*\* Failed to open IO connection

8421 110> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

8457 111> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

8475 112> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

8492 113> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

8509 114> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

8510 115> \*\*\* Failed to open IO connection.

8527 116> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

8528 117> \*\*\* Failed to open IO connection

8545 118> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

8546 119> \*\*\* Failed to open IO connection

8563 120> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

8564 121> \*\*\* Failed to open IO connection

8581 122> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

8582 123> \*\*\* Failed to open IO connection

8599 124> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

8600 125> \*\*\* Failed to open IO connection

8617 126> \*\*\* Expected Successful ForwardOpen: Received General Status 01, Extended Status 0x0117

8653 127> \*\*\* Expected general status 1, extended status 0x0119, Received 1 0x0117

8709 1> \*\*\* The expected CIP Object 0x37 instance 0 does not exist! Get Attributes Test was skipped. When an instance does not exist, DUT should return status 0x16 (Object instance does not exist) to services accessing this instance.

8730 1> \*\*\* Incorrect error code, Srv Code x10, Expected x08

8739 2> \*\*\* The declared CIP Object 55 instance 0 does not exist! Set Attributes Test was skipped.

8743 3> \*\*\* The declared CIP Object 55 instance 0 does not exist! Set Attributes Test was skipped.

8756 1> \*\*\* Unexpected status code 0x05, expect 0x08!

8765 2> \*\*\* Unexpected status code 0x05, expect 0x08!

8774 3> \*\*\* Unexpected status code 0x05, expect 0x08!

8783 4> \*\*\* Received unexpected Status 0x05 for Get\_Attribute\_List request!

8873 5> \*\*\* Unexpected status code 0x05, expect 0x08!

8882 6> \*\*\* Unexpected status code 0x05, expect 0x08!

8891 7> \*\*\* Unexpected status code 0x05, expect 0x08!

8900 8> \*\*\* Received unexpected status for service 0x08. Manual verification may waive this error.

8909 9> \*\*\* Unexpected status code 0x05, expect 0x08!

8918 10> \*\*\* Unexpected status code 0x05, expect 0x08!

8927 11> \*\*\* Unexpected status code 0x05, expect 0x08!

8936 12> \*\*\* Unexpected status code 0x05, expect 0x08!

8945 13> \*\*\* Unexpected status code 0x05, expect 0x08!

8954 14> \*\*\* Unexpected status code 0x05, expect 0x08!

8963 15> \*\*\* Received unexpected status 0x05, expected status 0x08.

8980 16> \*\*\* Unexpected status code 0x05, expect 0x08!

8989 17> \*\*\* Unexpected status code 0x05, expect 0x08!

8998 18> \*\*\* Unexpected status code 0x05, expect 0x08!

9007 19> \*\*\* Unexpected status code 0x05, expect 0x08!

9016 20> \*\*\* Unexpected status code 0x05, expect 0x08!

9025 21> \*\*\* Received unexpected status for service 0x17. Manual verification may waive this error.

9034 22> \*\*\* Expected status 0x08 as DUT claims not support such service.

9043 23> \*\*\* Expected status 0x08 as DUT claims not support such service.

9052 24> \*\*\* Expected status 0x08 as DUT claims not support such service.

9061 25> \*\*\* Expected status 0x08 as DUT claims not support such service.

9070 26> \*\*\* Unexpected status code 0x05, expect 0x08!

9082 27> \*\*\* Unexpected status code 0x05, expect 0x08!

9086 28> \*\*\* Unexpected status code 0x05, expect 0x08!

9090 29> \*\*\* Unexpected status code 0x05, expect 0x08!

9094 30> \*\*\* Unexpected status code 0x05, expect 0x08!

9098 31> \*\*\* Unexpected status code 0x05, expect 0x08!

9102 32> \*\*\* Unexpected status code 0x05, expect 0x08!

9106 33> \*\*\* Unexpected status code 0x05, expect 0x08!

9110 34> \*\*\* Unexpected status code 0x05, expect 0x08!

9114 35> \*\*\* Unexpected status code 0x05, expect 0x08!

9118 36> \*\*\* Unexpected status code 0x05, expect 0x08!

9122 37> \*\*\* Unexpected status code 0x05, expect 0x08!

9126 38> \*\*\* Unexpected status code 0x05, expect 0x08!

9130 39> \*\*\* Unexpected status code 0x05, expect 0x08!

9134 40> \*\*\* Unexpected status code 0x05, expect 0x08!

9138 41> \*\*\* Unexpected status code 0x05, expect 0x08!

9142 42> \*\*\* Unexpected status code 0x05, expect 0x08!

9146 43> \*\*\* Unexpected status code 0x05, expect 0x08!

9150 44> \*\*\* Unexpected status code 0x05, expect 0x08!

9154 45> \*\*\* Unexpected status code 0x05, expect 0x08!

9158 46> \*\*\* Unexpected status code 0x05, expect 0x08!

9172 1> \*\*\* The object does not exist. Object Specific Services Test was skipped.

9187 1> \*\*\* The object does not exist. Unused Services Test was skipped.

9200 1> \*\*\* Missing required File Object Class attribute 3 (Number\_of\_Instances)

9209 2> \*\*\* Missing required File Object Class attribute 32 (Directory)

9218 3> \*\*\* Failed to Get File Object Number of Instances attribute.

9284 1> \*\*\* Expected attribute is not implemented!

9293 2> \*\*\* Expected attribute is not implemented!

9302 3> \*\*\* Expected attribute is not implemented!

9311 4> \*\*\* Expected attribute is not implemented!

9745 1> \*\*\* Attribute data value incorrect attr 2, Srv Code x0E

9796 2> \*\*\* STC error: Unexpected success for not implemented attribute 8.

9818 3> \*\*\* STC error: Unexpected success for not implemented attribute 9.

9827 4> \*\*\* STC error: Unexpected success for not implemented attribute 10.

9836 5> \*\*\* STC error: Unexpected success for not implemented attribute 11.

10061 1> \*\*\* Unexpected success response attr 5, Srv Code x10

10070 2> \*\*\* Unexpected success response attr 6, Srv Code x10

10087 3> \*\*\* Unexpected success response attr 8, Srv Code x10

10096 4> \*\*\* Incorrect error code attr 9, Srv Code x10, Expected x0E

10105 5> \*\*\* Unexpected success response attr 10, Srv Code x10

10122 6> \*\*\* Unexpected success response attr 11, Srv Code x10

11049 1> \*\*\* After Type 0 Reset, no DUT response at new address 192.168.1.11. Is Reset timer not long enough?. (NV value not maintained ?)

11073 2> \*\*\* After Type 0 Reset, DUT responds at prior address 192.168.1.10

11129 3> \*\*\* E.Int.F5.5 Change IP Address - failure logged

11568 1> \*\*\* Expected attribute is not implemented!

11577 2> \*\*\* Expected attribute is not implemented!

11586 3> \*\*\* Expected attribute is not implemented!

11595 4> \*\*\* Expected attribute is not implemented!

11690 1> \*\*\* Incorrect error code attr 4, Srv Code x10, Expected x08

11699 2> \*\*\* Incorrect error code attr 5, Srv Code x10, Expected x08

11716 3> \*\*\* Incorrect error code attr 7, Srv Code x10, Expected x08

12057 1> \*\*\* STC error: Unexpected success for not implemented attribute 4.

12068 2> \*\*\* STC error: Unexpected success for not implemented attribute 5.

12080 3> \*\*\* STC error: Unexpected success for not implemented attribute 6.

12092 4> \*\*\* STC error: Unexpected success for not implemented attribute 7.

12104 5> \*\*\* STC error: Unexpected success for not implemented attribute 8.

12116 6> \*\*\* STC error: Unexpected success for not implemented attribute 9.

12335 1> \*\*\* Unexpected success response attr 6, Srv Code x10

12360 2> \*\*\* Unexpected success response attr 9, Srv Code x10

12818 1> \*\*\* Incorrect error code, Srv Code x4C, Expected x08

12847 1> \*\*\* STC FILE ERROR: The Set\_Attribute\_Single service shall be implemented if the Interface Control attribute is implemented.

12848 2> \*\*\* Get\_and\_Clear service shall be supported if the Interface Counters, Media Counters, HC Interface Counters, HC Media Counters or Link\_Down Counter are implemented.

12986 3> \*\*\* Test skipped: Interface Control attribute not implemented or not settable.

\*\* Warnings \*\*

\* Reminders \*

10875 1> \* Reminder: Device support of EtherNet/IP ACD (Address Conflict Detection) requires manual verification. Please contact ODVA for assistance.