Easy measurement points:

-0-
The AM62 EVM has INA231 ADCs which can be controlled via I2C. This allow high side measurements.
	 VDD_CORE           .01 ohms   (core to core)
	 VDD_CORE           .01 ohms   (core to vcc_0v85)
	 SOC_DVDD1V8        .01 ohms
	 VDDA_1V8           .01 ohms
	 VDD_DDR4           .01 ohms
	 SOC_DVD3V3         .01 ohms
Using the pi_analog probe or mixed signal probe voltage and current can be measuring the drop across the sense resistors.

