These scripts launch TI PDK unit tests for FreeRTOS using JTAG.
A script can be cloned and adapted to support the launch of a custom AutoSAR OS

 1: Set up paths to test in script
 2: Run script to:
	a: Initialize all system power, clocks, ddr
	b: launch test case

NOTES: 
1: Scripts assume NOBOOT mode. Scripts can work in other modes however any target
  code which runs ahead of the script (like DDR init) may result in failure.
2: A power on reset is needed between script executions as the DDR script assumes
  first init
