|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| equipment | serial number | phenomenon | 官方答复 | test results |
| 设备一 | SB45058 | After power on, the two indicators are not on | This probe could be dead | Can't electricity test |
| 设备二 | SB46011 | USB MODE red light / green light flashing | There is some issue with the boot up  建议进入安全模式尝试 | The system returns to normal. After 20 seconds of power-on, the green light is on, and the COMPUTER can identify it and debug can pass |
| 设备三 | SB45959 | USE MODE red light / green light flashing | Operation as above, as before USB MODE red light / green light flashing |
| 设备四 | SB46012 | USE MODE green light/MODE Red blinking | This probe looks good, the issue is elsewhere | computer recognized it, but the connection test failed |

 