C:\PROCESSOR_SDK_VISION_03_06_00_00\vision_sdk\build>gmake -s showconfig
#
# Build Config is [ tda2xx_evm_bios_all ]
# Build Config file is @ C:/PROCESSOR_SDK_VISION_03_06_00_00/vision_sdk/configs/tda2xx_evm_bios_all/cfg.mk
# Build Config .h file is @ C:/PROCESSOR_SDK_VISION_03_06_00_00/vision_sdk/links_fw/include/config/apps/tda2xx_evm_bios_all/system_cfg.h
# Build CPUs is @ ipu1_0 ipu1_1 ipu2 a15_0 dsp1 dsp2 eve1 eve2 eve3 eve4
#
# CPUs included in application,
# PROC_IPU1_0_INCLUDE=yes
# PROC_IPU1_1_INCLUDE=yes
# PROC_IPU2_INCLUDE=yes
# PROC_DSP1_INCLUDE=yes
# PROC_DSP2_INCLUDE=yes
# PROC_EVE1_INCLUDE=yes
# PROC_EVE2_INCLUDE=yes
# PROC_EVE3_INCLUDE=yes
# PROC_EVE4_INCLUDE=yes
# PROC_A15_0_INCLUDE=yes
#
# Platform config,
# VSDK_BOARD_TYPE=TDA2XX_EVM [options: TDA2XX_EVM TDA2EX_EVM TDA3XX_EVM TDA3XX_RVP TDA2XX_RVP]
# PLATFORM=tda2xx-evm
# DUAL_A15_SMP_BIOS=no
# IPU1_SMP_BIOS=no
# DDR_MEM=DDR_MEM_512M [options: DDR_MEM_128M DDR_MEM_512M DDR_MEM_1024M]
# EMIFMODE=SINGLE_EMIF_512MB [options: SINGLE_EMIF_512MB SINGLE_EMIF_1GB ref build_pdk.mk]
# NDK_PROC_TO_USE=ipu1_1 [options: a15_0 ipu1_0 ipu1_1 ipu2 none]
# NSP_TFDTP_INCLUDE=no [options: yes no]
# TDA2EX_ETHSRV_BOARD=no [options: yes no]
# FATFS_PROC_TO_USE=ipu1_0 [options: ipu1_0 none]
# RADAR_BOARD=none [options: TDA3XX_AR12_ALPS TDA3XX_AR12_VIB_DAB_BOOSTER TDA3XX_RADAR_RVP none]
#
# Build config,
# BUILD_OS=Windows_NT [options: Windows_NT Linux]
# BUILD_DEPENDENCY_ALWAYS=no
# BUILD_ALGORITHMS=no
# BUILD_INFOADAS=no
# PROFILE=release [options: debug release]
# KW_BUILD=no
# CPLUSPLUS_BUILD=no
# IPU_PRIMARY_CORE=ipu1_0 [options: ipu1_0 ipu2]
# IPU_SECONDARY_CORE=ipu2 [options: ipu1_0 ipu2]
# A15_TARGET_OS=Bios [options: Bios Linux Qnx]
# BSP_STW_PACKAGE_SELECT=all [options: all vps-iss-dss-only vps-vip-vpe]
#
# Safety Module config,
# RTI_INCLUDE=no
# ECC_FFI_INCLUDE=no
# DCC_ESM_INCLUDE=no
#
# Video Module config,
# IVAHD_INCLUDE=yes
# VPE_INCLUDE=yes
# CAL_INCLUDE=no
# ISS_INCLUDE=no
# ISS_ENABLE_DEBUG_TAPS=no
# WDR_LDC_INCLUDE=no
# DSS_INCLUDE=yes
#
# Open Compute config,
# OPENCL_INCLUDE=no
# TARGET_ROOTDIR=C:/PROCESSOR_SDK_VISION_03_06_00_00/vision_sdk/apps/src/rtos/opencl
# ENABLE_OPENCV=no
# ENABLE_OPENCV_TESTS=no
# OPENVX_INCLUDE=yes
#
# Log config,
# ENABLE_UART_LOG=yes
# ENABLE_NETWORK_LOG=no
# ENABLE_CCS_LOG=no
# CIO_REDIRECT=yes
#
# IPC config,
# WORKQ_INCLUDE=no
# IPC_LIB_INCLUDE=no
#
# AUTOSAR_APP=no
#
# Surround View config,
# SRV_FAST_BOOT_INCLUDE=no
#
# Other Module config,
# AVB_INCLUDE=no
# DCAN_INCLUDE=no
# RADAR_ONLY=no
# CPU_IDLE_ENABLED=yes
# FAST_BOOT_INCLUDE=no
# DATA_VIS_INCLUDE=no
# HS_DEVICE=no
# ULTRASONIC_INCLUDE=no
# PGA450=
# PGA460=
# ENABLE_ALL_DEPTH=
#
# Linux config,
# DEFAULT_UBOOT_CONFIG=dra7xx_evm_vision_config
# DEFAULT_KERNEL_CONFIG=ti_sdk_dra7x_release_defconfig
# DEFAULT_DTB=dra7-evm-infoadas.dtb
# CMEM_INCLUDE=no
# IPUMM_INCLUDE=no
# IPU1_EVELOADER_INCLUDE=no
# ROBUST_RVC_INCLUDE=no
# BUILD_ADAM_CAR=no
#
# Alg plugins included in build,
# ALG_autocalibration ALG_autoremap ALG_census ALG_clr ALG_denseopticalflow ALG_disparityhamdist ALG_dmaSwMs ALG_vpeSwMs ALG_edgedetection ALG_framecopy ALG_lanedetection ALG_objectdetection ALG_remapmerge ALG_safe_framecopy ALG_sfm ALG_sparseopticalflow ALG_stereo_postprocessing ALG_subframecopy ALG_surroundview ALG_openvx ALG_tidl ALG_tiop
#
# Use-cases included in build,
# UC_srv_calibration UC_lvds_vip_dual_cam_dual_display UC_lvds_vip_multi_cam_view UC_lvds_vip_sv_analytics_us UC_lvds_vip_sv_standalone UC_lvds_vip_single_stereo UC_lvds_vip_single_stereo_auto_calib UC_lvds_vip_single_stereo_calibration UC_network_rx_tx UC_network_stereo_display UC_null_src_dec_display UC_null_src_display UC_ov490_vip_sv_standalone UC_saveDisFrame UC_vip_single_cam_analytics2 UC_vip_single_cam_dense_optical_flow UC_vip_single_cam_dual_display UC_vip_single_cam_edge_detection UC_vip_single_cam_frame_copy UC_vip_single_cam_frame_copy_safety UC_vip_single_cam_lane_detection UC_vip_single_cam_object_detection2 UC_vip_single_cam_sfm UC_vip_single_cam_sparse_optical_flow UC_vip_single_cam_subframe_copy UC_vip_single_cam_tlr UC_vip_single_cam_view UC_vip_single_cam_view_encdec UC_vip_single_cam_openvx UC_tidl UC_semSeg UC_tidl_OD
#
#
# CPUs that are NOT required but included in config [ tda2xx_evm_bios_all ],
#
# WARNING: IPU1_1 can be excluded from application
# WARNING: IPU2 can be excluded from application
#
# CPUs that are required but not included in config [ tda2xx_evm_bios_all ],
#
#
# Edit C:/PROCESSOR_SDK_VISION_03_06_00_00/vision_sdk/apps/configs/tda2xx_evm_bios_all/cfg.mk to include or exclude CPUs in an application
#

C:\PROCESSOR_SDK_VISION_03_06_00_00\vision_sdk\build>