# Size of L2 Aux SRAM  Memory in KB which can be used by TIDL, Recommended value is
# 224KB considering that 32KB of L2 is used for other purpose.
L2MEMSIZE_KB           = 224
# Size of L2 main SRAM Memory in KB which can be used by TIDL
MSMCSIZE_KB            = 1024
#ID for a Device, TDA4VMID = 0, TIDL_TDA4AEP = 1,  TIDL_TDA4AM = 2, TIDL_TDA4AMPlus = 3, TIDL_AM62A = 4
DEVICE_NAME            = 4
ENABLE_PERSIT_WT_ALLOC = 1
DDRFREQ_MHZ            = 3200
MATPANELSIZE           = 32


FILENAME_NET     = /home/root/model-artifacts/Seg4/tempDir/subgraph_0_tidl_net.bin
FILEFORMAT_NET     = -1
DEVICE_NAME     = 260
PACKETIZE_MODE     = 0
OUTPUT_DIR     = /home/root/model-artifacts/Seg4/tempDir/subgraph_0_tidl_net.bin
