quinn.carver@CTSI-ASSET1876 MINGW64 ~
$ mkdir bugfix

quinn.carver@CTSI-ASSET1876 MINGW64 ~
$ git clone https://git.ti.com/cgit/processor-sdk/rtos-template-app
Cloning into 'rtos-template-app'...

quinn.carver@CTSI-ASSET1876 MINGW64 ~/rtos-template-app (master)
$ git branch bugfix/i2c-task-start-typo

..edits...

quinn.carver@CTSI-ASSET1876 MINGW64 ~/rtos-template-app (master)
$ git status
On branch master
Your branch is up-to-date with 'origin/master'.
Changes not staged for commit:
        modified:   am335x/evmAM335x/A8/template_app/rtos/app.c
        modified:   am437x/evmAM437x/A9/template_app/rtos/app.c
        modified:   am572x/evmAM572X/A15/template_app/rtos/app.c
        modified:   am572x/evmAM572X/M4/template_app/rtos/app.c
        modified:   am65xx/evmAM65xx/A53/template_app/rtos/app.c

no changes added to commit
quinn.carver@CTSI-ASSET1876 MINGW64 ~/rtos-template-app (master)
$ git add */*/*/template_app/rtos/app.c

quinn.carver@CTSI-ASSET1876 MINGW64 ~/rtos-template-app (master)
$ git commit -m "fixed typo where block was declared to start a task for spi, but was actually i2c"
[master b95cccd] fixed typo where block was declared to start a task for spi, but was actually i2c
 5 files changed, 5 insertions(+), 5 deletions(-)

quinn.carver@CTSI-ASSET1876 MINGW64 ~/rtos-template-app (master)
$ git diff bugfix/i2c-task-start-typo master
diff --git a/am335x/evmAM335x/A8/template_app/rtos/app.c b/am335x/evmAM335x/A8/template_app/rtos/app.c
index 1809e5a..b6122d9 100644
--- a/am335x/evmAM335x/A8/template_app/rtos/app.c
+++ b/am335x/evmAM335x/A8/template_app/rtos/app.c
@@ -92,7 +92,7 @@ void appTasksCreate(void)
                    "spi_test_task",
                    6, 4096);

-    /* Create task to test spi interface */
+    /* Create task to test i2c interface */
     biosTaskCreate(i2c_eeprom_read_and_display_task,
                    "i2c_eeprom_read_and_display_task",
                    7, 4096);
diff --git a/am437x/evmAM437x/A9/template_app/rtos/app.c b/am437x/evmAM437x/A9/template_app/rtos/app.c
index 9b0ec65..503161f 100644
--- a/am437x/evmAM437x/A9/template_app/rtos/app.c
+++ b/am437x/evmAM437x/A9/template_app/rtos/app.c
@@ -97,7 +97,7 @@ void appTasksCreate(void)
                    "spi_test_task",
                    6, 4096);

-    /* Create task to test spi interface */
+    /* Create task to test i2c interface */
     biosTaskCreate(i2c_eeprom_read_and_display_task,
                    "i2c_eeprom_read_and_display_task",
                    7, 4096);
diff --git a/am572x/evmAM572X/A15/template_app/rtos/app.c b/am572x/evmAM572X/A15/template_app/rtos/app.c
index dc2cc8c..ce69a2b 100644
--- a/am572x/evmAM572X/A15/template_app/rtos/app.c
+++ b/am572x/evmAM572X/A15/template_app/rtos/app.c
@@ -97,7 +97,7 @@ void appTasksCreate(void)
                    "spi_test_task",
                    6, 4096);

-    /* Create task to test spi interface */
+    /* Create task to test i2c interface */
     biosTaskCreate(i2c_eeprom_read_and_display_task,
                    "i2c_eeprom_read_and_display_task",
                    7, 4096);
quinn.carver@CTSI-ASSET1876 MINGW64 ~/rtos-template-app (master)
$ git push
error: Cannot access URL https://git.ti.com/cgit/processor-sdk/rtos-template-app/, return code 22
fatal: git-http-push failed
error: failed to push some refs to 'https://git.ti.com/cgit/processor-sdk/rtos-template-app'