Connection Diagram:

LM4F232H5QD Evaluation Board

GND

3.3v

CANH

60 ohms termination resistor

CANL

EN

Rs

R

D

GND

GND

GND

3.3v

Vcc

SN65HVD234D

PB4 (CAN0RX)

PB5 (CAN0TX)