XXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXX
X   Artwork and documentation done by: Texas Instruments Norway 			X
X   Company: Texas Instruments Norway AS                                               		X
X   Address: Gaustadalléen 21    0349 OSLO                           			X
X                                                                     					X
XXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXX

PCB NAME : SmartRFCC2510 
REVISION: 1.1 (PCB 1.1, Schematic 1.1)
DATE: 2009-03-13


Manufacturers marking: Two letter + year + week
The two letter code shall identify the manufaturer and is decided by the manufacturer. 
No logos or other identifyers are allowed.
The marking shall be in silk screen print at secondary side of the PCB, or in solder 
resist if no silk print at secondary side.

FILE: SmartRFCC2510_1_1.ZIP PACKED WITH WinZIP 

PCB DESCRIPTION:	2 LAYER PCB 0.8 MM
		Copper	35 um
		DE104iML or equivalent substrate (Resin contents around 45%, which gives Er=4.42@2.4GHz, TanD=0.016)
  		Dimensions in mil (0.001 inch)
               		DOUBLE SIDE SOLDER MASK,
                	DOUBLE SIDE SILKSCREEN,
                	8 MIL MIN TRACE WIDTH AND 8 MIL MIN ISOLATION.

                 
FILE NAME            				DESCRIPTION                               		FILE TYPE
------------------------------------------------------------------------------------------------------------------------------------
***PCB MANUFACTURING FILES:
l1.SPL                  			LAYER 1 COMPONENT SIDE/POSITIV             		EXT. GERBER
l2.SPL                  			LAYER 2 SOLDER SIDE/POSITIV                 		EXT. GERBER

STOPCOMP.SPL            		SOLDER MASK COMPONENT SIDE/NEGATIVE         		EXT. GERBER
STOPSOLD.SPL            		SOLDER MASK SOLDER SIDE/NEGATIVE            		EXT. GERBER

SILKCOMP.SPL            		SILKSCREEN COMPONENT SIDE/POSITIVE          		EXT. GERBER
SILKSOLD.SPL           		SILKSCREEN SOLDER SIDE/POSITIVE             		EXT. GERBER

PASTCOMP.SPL            		SOLDER PAST COMPONENT SIDE/POSITIVE         		EXT. GERBER
PATSOLD.SPL             		SOLDER PAST SOLDER SIDE/POSITIVE            		EXT. GERBER

ASSYCOMP.SPL            		ASSEMBLY DRAWING COMPONENT SIDE/NEGATIVE    	EXT. GERBER
ASSYSOLD.SPL            		ASSEMBLY DRAWING SOLDER SIDE/NEGATIVE       		EXT. GERBER

NCDRILL.SPL             		NC DRILL THROUGH HOLE                       			EXCELLON
DRILL.SPL               			DRILL/MECHANICAL DRAWING                    		EXT. GERBER

GERBER.REP             		 DRILL/NC DRILL REPORT                       			ASCII

P&PCOMP.REP             		PICK AND PLACE FILE COMPONENT SIDE          		ASCII
P&PSOLD.REP             		PICK AND PLACE FILE SOLDER SIDE             		ASCII

EXT_GERBER.USR          		EXTENDED GERBER APERTURE TABLE              		ASCII
CNC.USR                 			NC DRILL DEVICE FILE                        			ASCII

SmartRFCC2510_PARTLIST_1_1.xls			PART LIST			XLS

***PDF FILES
SmartRFCC2510_Schematic1_1.PDF		SCHEMATIC FILE			PDF
SmartRFCC2510_Layout1_1.pdf    			ASSEMBLY DRAWING		PDF

***CADSTAR FILES
CC2510DEMO_1_1.scm								Cadstar Schematic file
SmartRFCC2510_1_1.csa								Cadstar Shematic archive
CC2510DEMO_1_1.pcb								Cadstar layout file
SmartRFCC2510_1_1.cpa								Cadstar PCB 

	
README.TXT              			THIS FILE                                   		ASCII							
